  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GW023B
 Exp. Code:  GW023B  


Schedule Version:       3.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Di Wen

Address:  Kapteyn Astronomical Institute
          Landleven 12
          9747 AD Groningen
          the Netherlands

Phone:    +31 503 638 324
EMAIL:    wen@astro.rug.nl
Fax:
Phone during observation: +31 685 842 225

Observing mode:

Notes:
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

 Next scan frequencies:  4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

16 00 00  J0132+4325   19 28 15  19.6  50.3 -6.1     -65.9     0        0   16 00 00
16 03 00  =0129+431    19 31 15  20.1  50.5 -6.0     -66.3   180       46   16 00 01

16 03 00  B0128+437    19 31 15  20.5  50.1 -6.0     -66.8    -9       46   16 03 09
16 06 30  ---          19 34 46  21.1  50.3 -6.0     -67.3   201       98   16 03 01

16 06 30  J0132+4325   19 34 46  20.7  50.8 -6.0     -66.9    -9       98   16 06 39
16 08 00  =0129+431    19 36 16  20.9  50.9 -6.0     -67.1    81      119   16 06 31

16 08 30  B0128+437    19 36 46  21.5  50.5 -5.9     -67.6    21      119   16 08 30
16 12 00  ---          19 40 17  22.0  50.7 -5.9     -68.1   210      173   16 08 31

 ---------- Scan set 10 ----------

16 12 36  J0132+4325   19 40 53  21.7  51.2 -5.9     -67.7    27      173   16 12 36
16 14 06  =0129+431    19 42 23  21.9  51.3 -5.9     -68.0    90      196   16 12 37

16 14 06  B0128+437    19 42 23  22.4  50.9 -5.8     -68.4    -9      196   16 14 15
16 17 36  ---          19 45 54  23.0  51.1 -5.8     -68.9   201      248   16 14 07

16 18 06  J0132+4325   19 46 24  22.6  51.6 -5.8     -68.5    21      248   16 18 06
16 19 36  =0129+431    19 47 54  22.9  51.7 -5.8     -68.8    90      271   16 18 07

16 19 36  B0128+437    19 47 54  23.3  51.3 -5.7     -69.2    -9      271   16 19 45
16 23 06  ---          19 51 24  23.9  51.5 -5.7     -69.7   201      323   16 19 37

16 23 06  J0132+4325   19 51 24  23.5  52.0 -5.7     -69.3    -9      323   16 23 15
16 24 36  =0129+431    19 52 55  23.7  52.1 -5.7     -69.5    81      344   16 23 07

16 24 36  B0128+437    19 52 55  24.2  51.6 -5.7     -69.9    -9      344   16 24 45
16 28 06  ---          19 56 25  24.7  51.9 -5.6     -70.4   201      396   16 24 37

16 28 36  J0132+4325   19 56 55  24.4  52.4 -5.6     -70.1    21      396   16 28 36
16 30 06  =0129+431    19 58 26  24.6  52.5 -5.6     -70.3    90      419   16 28 37

16 30 06  B0128+437    19 58 26  25.1  52.0 -5.6     -70.7    -9      419   16 30 15
16 33 36  ---          20 01 56  25.7  52.2 -5.5     -71.3   201      471   16 30 07

16 33 36  J0132+4325   20 01 56  25.2  52.7 -5.5     -70.8    -9      471   16 33 45
16 35 06  =0129+431    20 03 26  25.5  52.8 -5.5     -71.0    81      492   16 33 37
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

16 35 06  B0128+437    20 03 26  25.9  52.3 -5.5     -71.5    -9      492   16 35 15
16 36 06  ---          20 04 27  26.1  52.4 -5.5     -71.6    51      505   16 35 07

 ---------- Scan set 11 ----------

16 36 06  B0128+437    20 04 27  26.1  52.4 -5.5     -71.6    -6      505   16 36 12
16 39 36  ---          20 07 57  26.7  52.6 -5.4     -72.1   204      557   16 36 07

16 40 06  J0132+4325   20 08 27  26.4  53.1 -5.4     -71.7    21      557   16 40 06
16 41 36  =0129+431    20 09 58  26.6  53.2 -5.4     -71.9    90      580   16 40 07

16 41 36  B0128+437    20 09 58  27.1  52.7 -5.4     -72.4    -9      580   16 41 45
16 45 06  ---          20 13 28  27.7  52.9 -5.3     -72.9   201      632   16 41 37

16 45 06  J0132+4325   20 13 28  27.2  53.4 -5.3     -72.5    -9      632   16 45 15
16 46 36  =0129+431    20 14 58  27.5  53.5 -5.3     -72.7    81      653   16 45 07

 ---------- Scan set 11 ----------

16 46 36  B0128+437    20 14 58  27.9  53.0 -5.3     -73.2    -9      653   16 46 45
16 50 06  ---          20 18 29  28.5  53.2 -5.2     -73.7   201      705   16 46 37

16 50 36  J0132+4325   20 18 59  28.2  53.8 -5.3     -73.2    21      705   16 50 36
16 52 06  =0129+431    20 20 29  28.4  53.9 -5.2     -73.5    90      728   16 50 37

16 52 06  B0128+437    20 20 29  28.9  53.3 -5.2     -74.0    -9      728   16 52 15
16 55 36  ---          20 24 00  29.5  53.5 -5.1     -74.5   201      780   16 52 07

16 55 36  J0132+4325   20 24 00  29.1  54.1 -5.2     -74.0    -9      780   16 55 45
16 57 06  =0129+431    20 25 30  29.3  54.1 -5.1     -74.2    81      801   16 55 37

16 57 06  B0128+437    20 25 30  29.7  53.6 -5.1     -74.7    -9      801   16 57 15
16 58 06  ---          20 26 30  29.9  53.7 -5.1     -74.9    51      814   16 57 07

 ---------- Scan set 12 ----------

16 58 06  B0128+437    20 26 30  29.9  53.7 -5.1     -74.9    -6      814   16 58 12
17 01 36  ---          20 30 01  30.5  53.9 -5.0     -75.4   204      866   16 58 07

17 02 06  J0132+4325   20 30 31  30.2  54.4 -5.1     -74.9    21      866   17 02 06
17 03 36  =0129+431    20 32 01  30.5  54.5 -5.0     -75.1    90      890   17 02 07

17 03 36  B0128+437    20 32 01  30.9  54.0 -5.0     -75.7    -9      890   17 03 45
17 07 06  ---          20 35 32  31.5  54.1 -5.0     -76.2   201      941   17 03 37
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

17 07 06  J0132+4325   20 35 32  31.1  54.7 -5.0     -75.6    -8      941   17 07 14
17 08 36  =0129+431    20 37 02  31.3  54.8 -5.0     -75.9    82      963   17 07 07

 ---------- Scan set 12 ----------

17 08 36  B0128+437    20 37 02  31.7  54.2 -4.9     -76.4    -9      963   17 08 45
17 12 06  ---          20 40 33  32.3  54.4 -4.9     -76.9   201     1014   17 08 37

17 12 36  J0132+4325   20 41 03  32.0  55.0 -4.9     -76.4    22     1014   17 12 36
17 14 06  =0129+431    20 42 33  32.3  55.0 -4.9     -76.7    90     1038   17 12 37

17 14 06  B0128+437    20 42 33  32.7  54.5 -4.8     -77.2    -9     1038   17 14 15
17 17 36  ---          20 46 03  33.3  54.7 -4.8     -77.7   201     1089   17 14 07

17 17 36  J0132+4325   20 46 03  32.9  55.2 -4.8     -77.2    -8     1089   17 17 44
17 19 06  =0129+431    20 47 34  33.2  55.3 -4.8     -77.4    82     1110   17 17 37

17 19 06  B0128+437    20 47 34  33.6  54.7 -4.8     -78.0    -8     1110   17 19 14
17 20 06  ---          20 48 34  33.8  54.8 -4.7     -78.1    52     1124   17 19 07

 ---------- Scan set 13 ----------

17 20 06  B0128+437    20 48 34  33.8  54.8 -4.7     -78.1    -6     1124   17 20 12
17 23 36  ---          20 52 04  34.4  54.9 -4.7     -78.6   204     1176   17 20 07

17 24 06  J0132+4325   20 52 34  34.1  55.5 -4.7     -78.1    22     1176   17 24 06
17 25 36  =0129+431    20 54 05  34.3  55.6 -4.7     -78.4    90     1200   17 24 07

17 25 36  B0128+437    20 54 05  34.7  55.0 -4.6     -78.9    -8     1200   17 25 44
17 29 06  ---          20 57 35  35.3  55.1 -4.6     -79.5   202     1252   17 25 37

17 29 06  J0132+4325   20 57 35  35.0  55.7 -4.6     -78.9    -8     1252   17 29 14
17 30 36  =0129+431    20 59 06  35.2  55.8 -4.6     -79.1    82     1273   17 29 07

 ---------- Scan set 13 ----------

17 30 36  B0128+437    20 59 06  35.6  55.2 -4.6     -79.7    -8     1273   17 30 44
17 34 06  ---          21 02 36  36.2  55.3 -4.5     -80.2   202     1325   17 30 37

17 34 36  J0132+4325   21 03 06  36.0  56.0 -4.5     -79.7    22     1325   17 34 36
17 36 06  =0129+431    21 04 36  36.2  56.0 -4.5     -79.9    90     1348   17 34 37

17 36 06  B0128+437    21 04 36  36.6  55.4 -4.5     -80.5    -8     1348   17 36 14
17 39 36  ---          21 08 07  37.2  55.5 -4.4     -81.1   202     1400   17 36 07
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

17 39 36  J0132+4325   21 08 07  36.8  56.2 -4.4     -80.4    -8     1400   17 39 44
17 41 06  =0129+431    21 09 37  37.1  56.2 -4.4     -80.7    82     1421   17 39 37

17 41 06  B0128+437    21 09 37  37.5  55.6 -4.4     -81.3    -8     1421   17 41 14
17 42 06  ---          21 10 37  37.6  55.6 -4.4     -81.5    52     1435   17 41 07

 ---------- Scan set 14 ----------

17 42 06  B0128+437    21 10 37  37.6  55.6 -4.4     -81.5    -6     1435   17 42 12
17 45 36  ---          21 14 08  38.3  55.7 -4.3     -82.0   204     1487   17 42 07

17 46 06  J0132+4325   21 14 38  38.0  56.4 -4.3     -81.4    22     1487   17 46 06
17 47 36  =0129+431    21 16 08  38.3  56.4 -4.3     -81.6    90     1510   17 46 07

17 47 36  B0128+437    21 16 08  38.6  55.8 -4.3     -82.3    -8     1510   17 47 44
17 51 06  ---          21 19 39  39.3  55.9 -4.2     -82.8   202     1562   17 47 37

17 51 06  J0132+4325   21 19 39  38.9  56.6 -4.2     -82.2    -8     1562   17 51 14
17 52 36  =0129+431    21 21 09  39.2  56.6 -4.2     -82.4    82     1583   17 51 07

 ---------- Scan set 14 ----------

17 52 36  B0128+437    21 21 09  39.5  56.0 -4.2     -83.1    -8     1583   17 52 44
17 56 06  ---          21 24 40  40.1  56.0 -4.1     -83.6   202     1635   17 52 37

17 56 36  J0132+4325   21 25 10  39.9  56.7 -4.1     -83.0    22     1635   17 56 36
17 58 06  =0129+431    21 26 40  40.2  56.8 -4.1     -83.3    90     1659   17 56 37

17 58 06  B0128+437    21 26 40  40.5  56.1 -4.1     -83.9    -8     1659   17 58 14
18 01 36  ---          21 30 11  41.1  56.2 -4.0     -84.5   202     1711   17 58 07

18 01 36  J0132+4325   21 30 11  40.8  56.9 -4.1     -83.8    -8     1711   18 01 44
18 03 06  =0129+431    21 31 41  41.1  56.9 -4.0     -84.0    82     1732   18 01 37

18 03 06  B0128+437    21 31 41  41.4  56.2 -4.0     -84.7    -8     1732   18 03 14
18 04 06  ---          21 32 41  41.6  56.2 -4.0     -84.9    52     1745   18 03 07

 ---------- Scan set 15 ----------

18 04 06  B0128+437    21 32 41  41.6  56.2 -4.0     -84.9    -6     1745   18 04 12
18 07 36  ---          21 36 12  42.2  56.3 -3.9     -85.5   204     1798   18 04 07

18 08 06  J0132+4325   21 36 42  42.0  57.0 -4.0     -84.8    22     1798   18 08 06
18 09 36  =0129+431    21 38 12  42.3  57.1 -3.9     -85.1    90     1821   18 08 07
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

18 09 36  B0128+437    21 38 12  42.6  56.3 -3.9     -85.8    -8     1821   18 09 44
18 13 06  ---          21 41 43  43.2  56.4 -3.8     -86.4   202     1873   18 09 37

18 13 06  J0132+4325   21 41 43  42.9  57.1 -3.9     -85.6    -8     1873   18 13 14
18 14 36  =0129+431    21 43 13  43.2  57.2 -3.8     -85.8    82     1894   18 13 07

 ---------- Scan set 15 ----------

18 14 36  B0128+437    21 43 13  43.5  56.4 -3.8     -86.6    -8     1894   18 14 44
18 18 06  ---          21 46 43  44.1  56.5 -3.8     -87.2   202     1946   18 14 37

18 18 36  J0132+4325   21 47 13  43.9  57.2 -3.8     -86.5    22     1946   18 18 36
18 20 06  =0129+431    21 48 44  44.2  57.2 -3.8     -86.7    90     1969   18 18 37

18 20 06  B0128+437    21 48 44  44.5  56.5 -3.7     -87.5    -8     1969   18 20 14
18 23 36  ---          21 52 14  45.1  56.5 -3.7     -88.1   202     2021   18 20 07

18 23 36  J0132+4325   21 52 14  44.8  57.3 -3.7     -87.3    -8     2021   18 23 44
18 25 06  =0129+431    21 53 45  45.1  57.3 -3.7     -87.6    82     2043   18 23 37

18 25 06  B0128+437    21 53 45  45.4  56.5 -3.6     -88.4    -8     2043   18 25 14
18 26 06  ---          21 54 45  45.5  56.6 -3.6     -88.5    52     2056   18 25 07

 ---------- Scan set 16 ----------

18 26 06  B0128+437    21 54 45  45.5  56.6 -3.6     -88.5    -6     2056   18 26 12
18 29 36  ---          21 58 15  46.2  56.6 -3.6     -89.1   204     2109   18 26 07

18 30 06  J0132+4325   21 58 45  46.0  57.4 -3.6     -88.4    22     2109   18 30 06
18 31 36  =0129+431    22 00 16  46.2  57.4 -3.6     -88.6    90     2132   18 30 07

18 31 36  B0128+437    22 00 16  46.5  56.6 -3.5     -89.5    -8     2132   18 31 44
18 35 06  ---          22 03 46  47.2  56.6 -3.5     -90.1   202     2184   18 31 37

18 35 06  J0132+4325   22 03 46  46.9  57.4 -3.5     -89.2    -8     2184   18 35 14
18 36 36  =0129+431    22 05 16  47.2  57.4 -3.5     -89.5    82     2205   18 35 07

 ---------- Scan set 16 ----------

18 36 36  B0128+437    22 05 16  47.4  56.6 -3.5     -90.3    -8     2205   18 36 44
18 40 06  ---          22 08 47  48.1  56.6 -3.4     -91.0   202     2257   18 36 37

18 40 36  J0132+4325   22 09 17  47.9  57.4 -3.4     -90.2    22     2257   18 40 36
18 42 06  =0129+431    22 10 47  48.2  57.4 -3.4     -90.4    90     2280   18 40 37
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

18 42 06  B0128+437    22 10 47  48.4  56.6 -3.4     -91.3    -8     2280   18 42 14
18 45 36  ---          22 14 18  49.0  56.5 -3.3     -91.9   202     2332   18 42 07

18 45 36  J0132+4325   22 14 18  48.8  57.4 -3.3     -91.0    -8     2332   18 45 44
18 47 06  =0129+431    22 15 48  49.1  57.4 -3.3     -91.3    82     2353   18 45 37

18 47 06  B0128+437    22 15 48  49.3  56.5 -3.3     -92.2    -8     2353   18 47 14
18 48 06  ---          22 16 48  49.5  56.5 -3.3     -92.4    52     2367   18 47 07

 ---------- Scan set 17 ----------

18 48 06  B0128+437    22 16 48  49.5  56.5 -3.3     -92.4    -6     2367   18 48 12
18 51 36  ---          22 20 19  50.1  56.5 -3.2     -93.0   204     2419   18 48 07

18 52 06  J0132+4325   22 20 49  50.0  57.3 -3.2     -92.2    22     2419   18 52 06
18 53 36  =0129+431    22 22 19  50.2  57.3 -3.2     -92.5    90     2442   18 52 07

18 53 36  B0128+437    22 22 19  50.5  56.4 -3.2     -93.4    -8     2442   18 53 44
18 57 06  ---          22 25 50  51.1  56.4 -3.1     -94.1   202     2494   18 53 37

18 57 06  J0132+4325   22 25 50  50.9  57.3 -3.1     -93.1    -8     2494   18 57 14
18 58 36  =0129+431    22 27 20  51.1  57.2 -3.1     -93.4    82     2516   18 57 07

 ---------- Scan set 17 ----------

18 58 36  B0128+437    22 27 20  51.4  56.3 -3.1     -94.4    -8     2516   18 58 44
19 02 06  ---          22 30 51  52.0  56.2 -3.0     -95.0   202     2568   18 58 37

19 02 36  J0132+4325   22 31 21  51.9  57.2 -3.0     -94.2    22     2568   19 02 36
19 04 06  =0129+431    22 32 51  52.1  57.1 -3.0     -94.4    90     2591   19 02 37

19 04 06  B0128+437    22 32 51  52.4  56.2 -3.0     -95.4    -8     2591   19 04 14
19 07 36  ---          22 36 21  53.0  56.1 -2.9     -96.1   202     2643   19 04 07

19 07 36  J0132+4325   22 36 21  52.8  57.0 -3.0     -95.1    -8     2643   19 07 44
19 09 06  =0129+431    22 37 52  53.0  57.0 -2.9     -95.4    82     2664   19 07 37

19 09 06  B0128+437    22 37 52  53.3  56.0 -2.9     -96.4    -8     2664   19 09 14
19 10 06  ---          22 38 52  53.4  56.0 -2.9     -96.6    52     2677   19 09 07

 ---------- Scan set 18 ----------

19 10 06  B0128+437    22 38 52  53.4  56.0 -2.9     -96.6    -6     2677   19 10 12
19 13 06  ---          22 41 52  54.0  55.9 -2.8     -97.2   174     2722   19 10 07
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

19 13 36  J0132+4325   22 42 22  53.9  56.9 -2.9     -96.3    22     2722   19 13 36
19 15 06  =0129+431    22 43 53  54.1  56.8 -2.8     -96.6    90     2745   19 13 37

 ---------- Scan set 19 FF ----------

19 17 06  3C84         22 45 53  34.8  58.1 -4.6     -77.7    73     2745   19 17 06
19 20 06  ---          22 48 54  35.3  58.3 -4.5     -78.1   180     2792   19 17 07

19 22 06  J0132+4325   22 50 54  55.4  56.5 -2.7     -98.0    73     2792   19 22 06
19 23 36  =0129+431    22 52 24  55.7  56.4 -2.7     -98.4    90     2815   19 22 07

19 23 36  B0128+437    22 52 24  55.8  55.4 -2.7     -99.5    -8     2815   19 23 44
19 27 06  ---          22 55 55  56.5  55.2 -2.6    -100.2   202     2867   19 23 37

19 27 06  J0132+4325   22 55 55  56.3  56.3 -2.6     -99.1    -8     2867   19 27 14
19 28 36  =0129+431    22 57 25  56.6  56.2 -2.6     -99.4    82     2888   19 27 07

19 29 06  B0128+437    22 57 55  56.8  55.1 -2.6    -100.7    22     2888   19 29 06
19 31 06  ---          22 59 55  57.2  55.0 -2.5    -101.1   120     2919   19 29 07

19 31 06  B0128+437    22 59 55  57.2  55.0 -2.5    -101.1    -6     2919   19 31 12
19 32 06  ---          23 00 56  57.4  54.9 -2.5    -101.4    54     2933   19 31 07

 ---------- Scan set 21 ----------

19 34 06  J0132+4325   23 02 56  57.5  55.9 -2.5    -100.6   112     2933   19 34 06
19 36 36  =0129+431    23 05 26  58.0  55.7 -2.5    -101.2   150     2972   19 34 07

19 36 36  B0128+437    23 05 26  58.1  54.6 -2.5    -102.4    -8     2972   19 36 44
19 40 06  ---          23 08 57  58.8  54.3 -2.4    -103.3   202     3024   19 36 37

19 40 36  J0132+4325   23 09 27  58.7  55.4 -2.4    -102.1    22     3024   19 40 36
19 42 06  =0129+431    23 10 57  59.0  55.3 -2.4    -102.5    90     3047   19 40 37

19 42 06  B0128+437    23 10 57  59.1  54.2 -2.4    -103.7    -8     3047   19 42 14
19 45 36  ---          23 14 28  59.7  53.9 -2.3    -104.6   202     3099   19 42 07

19 45 36  J0132+4325   23 14 28  59.6  55.0 -2.3    -103.3    -9     3099   19 45 45
19 47 06  =0129+431    23 15 58  59.9  54.9 -2.3    -103.7    81     3120   19 45 37

19 47 06  B0128+437    23 15 58  60.0  53.7 -2.3    -105.0    -9     3120   19 47 15
19 48 06  ---          23 16 58  60.2  53.6 -2.3    -105.3    51     3133   19 47 07
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

 ---------- Scan set 22 ----------

19 48 06  B0128+437    23 16 58  60.2  53.6 -2.3    -105.3    -6     3133   19 48 12
19 51 36  ---          23 20 29  60.8  53.3 -2.2    -106.2   204     3185   19 48 07

19 52 06  J0132+4325   23 20 59  60.7  54.5 -2.2    -105.0    21     3185   19 52 06
19 53 36  =0129+431    23 22 29  61.0  54.3 -2.2    -105.4    90     3209   19 52 07

19 53 36  B0128+437    23 22 29  61.1  53.1 -2.2    -106.7    -9     3209   19 53 45
19 57 06  ---          23 26 00  61.7  52.7 -2.1    -107.6   201     3260   19 53 37

19 57 06  J0132+4325   23 26 00  61.6  54.0 -2.1    -106.3    -9     3260   19 57 15
20 00 00  =0129+431    23 28 54  62.1  53.6 -2.1    -107.1   165     3303   19 57 07

20 00 00  B0128+437    23 28 54  62.2  52.3 -2.1    -108.5    -9     3303   20 00 09
20 01 00  ---          23 29 54  62.4  52.2 -2.0    -108.7    51     3316   20 00 01

20 01 00  B0128+437    23 29 54  62.4  52.2 -2.0    -108.7    -6     3316   20 01 06
20 04 30  ---          23 33 25  63.0  51.8 -2.0    -109.8   204     3369   20 01 01

20 04 45  J0132+4325   23 33 40  62.9  53.1 -2.0    -108.4     6     3369   20 04 45
20 06 15  =0129+431    23 35 10  63.2  52.9 -2.0    -108.8    90     3392   20 04 46

20 06 15  B0128+437    23 35 10  63.3  51.5 -2.0    -110.3    -9     3392   20 06 24
20 09 45  ---          23 38 41  63.9  51.0 -1.9    -111.3   201     3444   20 06 16

20 09 45  J0132+4325   23 38 41  63.8  52.4 -1.9    -109.8    -9     3444   20 09 54
20 11 15  =0129+431    23 40 11  64.1  52.2 -1.9    -110.3    81     3464   20 09 46

20 11 15  B0128+437    23 40 11  64.1  50.8 -1.9    -111.8    -9     3464   20 11 24
20 14 45  ---          23 43 42  64.7  50.2 -1.8    -112.9   201     3516   20 11 16

20 15 00  J0132+4325   23 43 57  64.7  51.6 -1.8    -111.4     6     3516   20 15 00
20 16 30  =0129+431    23 45 27  64.9  51.4 -1.8    -111.9    90     3539   20 15 01

20 16 30  B0128+437    23 45 27  65.0  50.0 -1.8    -113.5    -9     3539   20 16 39
20 20 00  ---          23 48 57  65.6  49.3 -1.7    -114.6   201     3591   20 16 31

20 20 00  J0132+4325   23 48 57  65.5  50.8 -1.8    -113.0    -9     3591   20 20 09
20 21 30  =0129+431    23 50 28  65.8  50.6 -1.7    -113.5    81     3612   20 20 01

20 21 30  B0128+437    23 50 28  65.8  49.1 -1.7    -115.2    -9     3612   20 21 39
20 22 30  ---          23 51 28  66.0  48.9 -1.7    -115.5    51     3625   20 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

20 22 30  B0128+437    23 51 28  66.0  48.9 -1.7    -115.5    -6     3625   20 22 36
20 26 00  ---          23 54 58  66.5  48.2 -1.6    -116.7   204     3678   20 22 31

20 26 15  J0132+4325   23 55 13  66.6  49.7 -1.6    -115.2     6     3678   20 26 15
20 27 45  =0129+431    23 56 44  66.8  49.4 -1.6    -115.7    90     3701   20 26 16

20 27 45  B0128+437    23 56 44  66.8  47.8 -1.6    -117.4    -9     3701   20 27 54
20 31 15  ---          00 00 14  67.4  47.1 -1.5    -118.7   201     3753   20 27 46

20 31 15  J0132+4325   00 00 14  67.4  48.7 -1.6    -117.0    -9     3753   20 31 24
20 32 45  =0129+431    00 01 44  67.6  48.3 -1.5    -117.5    81     3774   20 31 16

20 32 45  B0128+437    00 01 44  67.6  46.7 -1.5    -119.3    -9     3774   20 32 54
20 36 15  ---          00 05 15  68.1  45.9 -1.5    -120.7   201     3825   20 32 46

20 36 30  J0132+4325   00 05 30  68.2  47.5 -1.5    -119.0     6     3825   20 36 30
20 38 00  =0129+431    00 07 00  68.5  47.1 -1.5    -119.6    90     3849   20 36 31

20 38 00  B0128+437    00 07 00  68.4  45.5 -1.4    -121.4    -9     3849   20 38 09
20 41 30  ---          00 10 31  69.0  44.5 -1.4    -122.8   201     3900   20 38 01

20 41 30  J0132+4325   00 10 31  69.0  46.2 -1.4    -121.0    -9     3900   20 41 39
20 43 00  =0129+431    00 12 01  69.2  45.8 -1.4    -121.6    81     3921   20 41 31

20 43 00  B0128+437    00 12 01  69.2  44.1 -1.3    -123.5    -9     3921   20 43 09
20 44 00  ---          00 13 01  69.3  43.8 -1.3    -123.9    51     3934   20 43 01

20 44 00  B0128+437    00 13 01  69.3  43.8 -1.3    -123.9    -6     3934   20 44 06
20 47 30  ---          00 16 32  69.8  42.8 -1.3    -125.5   204     3987   20 44 01

20 47 45  J0132+4325   00 16 47  70.0  44.5 -1.3    -123.7     6     3987   20 47 45
20 49 15  =0129+431    00 18 17  70.2  44.0 -1.3    -124.4    90     4010   20 47 46

20 49 15  B0128+437    00 18 17  70.1  42.3 -1.2    -126.3    -9     4010   20 49 24
20 52 45  ---          00 21 48  70.6  41.1 -1.2    -128.0   201     4062   20 49 16

20 52 45  J0132+4325   00 21 48  70.7  42.9 -1.2    -126.0    -9     4062   20 52 54
20 54 15  =0129+431    00 23 18  70.9  42.5 -1.2    -126.7    81     4083   20 52 46

20 54 15  B0128+437    00 23 18  70.8  40.6 -1.2    -128.7    -9     4083   20 54 24
20 57 45  ---          00 26 49  71.3  39.4 -1.1    -130.5   201     4135   20 54 16

20 58 00  J0132+4325   00 27 04  71.5  41.2 -1.1    -128.6     6     4135   20 58 00
20 59 30  =0129+431    00 28 34  71.7  40.6 -1.1    -129.4    90     4158   20 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

20 59 30  B0128+437    00 28 34  71.5  38.7 -1.1    -131.4    -9     4158   20 59 39
21 03 00  ---          00 32 04  72.0  37.4 -1.0    -133.3   201     4210   20 59 31

21 03 00  J0132+4325   00 32 04  72.2  39.3 -1.0    -131.3    -9     4210   21 03 09
21 04 30  =0129+431    00 33 35  72.4  38.7 -1.0    -132.1    81     4230   21 03 01

21 04 30  B0128+437    00 33 35  72.2  36.8 -1.0    -134.2    -9     4230   21 04 39
21 05 30  ---          00 34 35  72.3  36.4 -1.0    -134.7    51     4244   21 04 31

21 05 30  B0128+437    00 34 35  72.3  36.4 -1.0    -134.7    -6     4244   21 05 36
21 09 00  ---          00 38 05  72.8  34.9 -0.9    -136.8   204     4296   21 05 31

21 09 15  J0132+4325   00 38 20  73.0  36.7 -0.9    -134.8     6     4296   21 09 15
21 10 45  =0129+431    00 39 51  73.2  36.0 -0.9    -135.7    90     4319   21 09 16

21 10 45  B0128+437    00 39 51  73.0  34.1 -0.9    -137.8    -9     4319   21 10 54
21 14 15  ---          00 43 21  73.4  32.4 -0.8    -140.0   201     4371   21 10 46

21 14 15  J0132+4325   00 43 21  73.6  34.4 -0.8    -137.9    -9     4371   21 14 24
21 15 45  =0129+431    00 44 52  73.8  33.7 -0.8    -138.8    81     4392   21 14 16

21 15 45  B0128+437    00 44 52  73.6  31.7 -0.8    -141.0    -9     4392   21 15 54
21 19 15  ---          00 48 22  74.0  29.9 -0.7    -143.3   201     4444   21 15 46

21 19 30  J0132+4325   00 48 37  74.2  31.8 -0.8    -141.3     6     4444   21 19 30
21 21 00  =0129+431    00 50 07  74.4  31.0 -0.7    -142.3    90     4467   21 19 31

21 21 00  B0128+437    00 50 07  74.1  29.0 -0.7    -144.5    -9     4467   21 21 09
21 24 30  ---          00 53 38  74.5  27.1 -0.6    -147.0   201     4519   21 21 01

21 24 30  J0132+4325   00 53 38  74.8  29.1 -0.7    -144.8    -9     4519   21 24 39
21 26 00  =0129+431    00 55 08  74.9  28.2 -0.7    -145.9    81     4540   21 24 31

21 26 00  B0128+437    00 55 08  74.6  26.2 -0.6    -148.1    -9     4540   21 26 09
21 27 00  ---          00 56 08  74.7  25.6 -0.6    -148.8    51     4553   21 26 01

21 27 00  B0128+437    00 56 08  74.7  25.6 -0.6    -148.8    -6     4553   21 27 06
21 30 30  ---          00 59 39  75.0  23.5 -0.5    -151.4   204     4605   21 27 01

21 30 45  J0132+4325   00 59 54  75.4  25.4 -0.6    -149.4     6     4605   21 30 45
21 32 15  =0129+431    01 01 24  75.5  24.4 -0.5    -150.6    90     4628   21 30 46

21 32 15  B0128+437    01 01 24  75.2  22.4 -0.5    -152.8    -9     4628   21 32 24
21 35 45  ---          01 04 55  75.5  20.2 -0.5    -155.6   201     4680   21 32 16
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

21 35 45  J0132+4325   01 04 55  75.8  22.1 -0.5    -153.4    -9     4680   21 35 54
21 37 15  =0129+431    01 06 25  76.0  21.1 -0.5    -154.7    81     4701   21 35 46

21 37 15  B0128+437    01 06 25  75.6  19.2 -0.4    -156.8    -9     4701   21 37 24
21 40 45  ---          01 09 56  75.8  16.8 -0.4    -159.7   201     4753   21 37 16

21 41 00  J0132+4325   01 10 11  76.2  18.5 -0.4    -157.8     6     4753   21 41 00
21 42 30  =0129+431    01 11 41  76.3  17.5 -0.4    -159.1    90     4776   21 41 01

21 42 30  B0128+437    01 11 41  75.9  15.6 -0.3    -161.2    -9     4776   21 42 39
21 46 00  ---          01 15 12  76.1  13.1 -0.3    -164.2   201     4828   21 42 31

21 46 00  J0132+4325   01 15 12  76.5  14.9 -0.3    -162.2    -9     4828   21 46 09
21 47 30  =0129+431    01 16 42  76.6  13.8 -0.3    -163.6    81     4849   21 46 01

21 47 30  B0128+437    01 16 42  76.2  12.1 -0.3    -165.5    -9     4849   21 47 39
21 48 30  ---          01 17 42  76.2  11.3 -0.2    -166.4    51     4862   21 47 31

21 48 30  B0128+437    01 17 42  76.2  11.3 -0.2    -166.4    -6     4862   21 48 36
21 52 00  ---          01 21 13  76.4   8.7 -0.2    -169.5   204     4914   21 48 31

21 52 15  J0132+4325   01 21 28  76.8  10.1 -0.2    -167.9     6     4914   21 52 15
21 53 45  =0129+431    01 22 58  76.9   9.0 -0.2    -169.3    90     4938   21 52 16

21 53 45  B0128+437    01 22 58  76.4   7.4 -0.2    -171.1    -9     4938   21 53 54
21 57 15  ---          01 26 28  76.5   4.7 -0.1    -174.3   201     4989   21 53 46

21 57 15  J0132+4325   01 26 28  77.0   6.2 -0.1    -172.7    -9     4989   21 57 24
21 58 45  =0129+431    01 27 59  77.0   5.0 -0.1    -174.1    81     5010   21 57 16

21 58 45  B0128+437    01 27 59  76.5   3.6 -0.1    -175.7    -9     5010   21 58 54
22 02 15  ---          01 31 29  76.5   0.9 -0.0    -178.9   201     5062   21 58 46

22 02 30  J0132+4325   01 31 44  77.1   1.9 -0.0    -177.7     6     5062   22 02 30
22 04 00  =0129+431    01 33 14  77.1   0.7 -0.0    -179.1    90     5085   22 02 31

22 04 00  B0128+437    01 33 14  76.5  -0.5  0.0     179.4    -9     5085   22 04 09
22 07 30  ---          01 36 45  76.5  -3.2  0.1     176.2   201     5137   22 04 01

22 07 30  J0132+4325   01 36 45  77.1  -2.1  0.0     177.5    -9     5137   22 07 39
22 09 00  =0129+431    01 38 15  77.1  -3.3  0.1     176.0    81     5158   22 07 31

22 09 00  B0128+437    01 38 15  76.5  -4.3  0.1     174.8    -9     5158   22 09 09
22 10 00  ---          01 39 15  76.5  -5.1  0.1     173.9    51     5171   22 09 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

22 10 00  B0128+437    01 39 15  76.5  -5.1  0.1     173.9    -6     5171   22 10 06
22 13 30  ---          01 42 46  76.4  -7.8  0.2     170.7   204     5224   22 10 01

22 13 45  J0132+4325   01 43 01  77.0  -7.1  0.1     171.5     6     5224   22 13 45
22 15 15  =0129+431    01 44 31  76.9  -8.3  0.2     170.1    90     5247   22 13 46

22 15 15  B0128+437    01 44 31  76.3  -9.1  0.2     169.1    -9     5247   22 15 24
22 18 45  ---          01 48 02  76.2 -11.7  0.3     166.0   201     5299   22 15 16

22 18 45  J0132+4325   01 48 02  76.8 -11.1  0.2     166.8    -9     5299   22 18 54
22 20 15  =0129+431    01 49 32  76.7 -12.2  0.3     165.4    81     5319   22 18 46

22 20 15  B0128+437    01 49 32  76.1 -12.8  0.3     164.7    -9     5319   22 20 24
22 23 45  ---          01 53 03  75.9 -15.3  0.3     161.6   201     5371   22 20 16

22 24 00  J0132+4325   01 53 18  76.5 -15.1  0.3     162.0     6     5371   22 24 00
22 25 30  =0129+431    01 54 48  76.5 -16.2  0.3     160.7    90     5394   22 24 01

22 25 30  B0128+437    01 54 48  75.8 -16.5  0.4     160.1    -9     5394   22 25 39
22 29 00  ---          01 58 19  75.6 -18.9  0.4     157.2   201     5446   22 25 31

22 29 00  J0132+4325   01 58 19  76.2 -18.7  0.4     157.6    -9     5446   22 29 09
22 30 30  =0129+431    01 59 49  76.1 -19.7  0.4     156.4    81     5467   22 29 01

22 30 30  B0128+437    01 59 49  75.5 -19.9  0.5     156.0    -9     5467   22 30 39
22 31 30  ---          02 00 49  75.4 -20.5  0.5     155.2    51     5480   22 30 31

22 31 30  B0128+437    02 00 49  75.4 -20.5  0.5     155.2    -6     5480   22 31 36
22 35 00  ---          02 04 20  75.2 -22.7  0.5     152.4   204     5533   22 31 31

22 35 15  J0132+4325   02 04 35  75.7 -22.9  0.5     152.4     6     5533   22 35 15
22 36 45  =0129+431    02 06 05  75.6 -23.9  0.5     151.2    90     5556   22 35 16

22 36 45  B0128+437    02 06 05  75.0 -23.8  0.6     151.1    -9     5556   22 36 54
22 40 15  ---          02 09 35  74.7 -25.9  0.6     148.5   201     5608   22 36 46

22 40 15  J0132+4325   02 09 35  75.3 -26.1  0.6     148.5    -9     5608   22 40 24
22 41 45  =0129+431    02 11 06  75.2 -27.0  0.6     147.4    81     5629   22 40 16

22 41 45  B0128+437    02 11 06  74.5 -26.8  0.6     147.4    -9     5629   22 41 54
22 45 15  ---          02 14 36  74.2 -28.7  0.7     144.9   201     5680   22 41 46

22 45 30  J0132+4325   02 14 51  74.8 -29.2  0.7     144.6     6     5680   22 45 30
22 47 00  =0129+431    02 16 22  74.6 -30.0  0.7     143.6    90     5704   22 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

22 47 00  B0128+437    02 16 22  74.0 -29.6  0.7     143.7    -9     5704   22 47 09
22 50 30  ---          02 19 52  73.6 -31.4  0.8     141.3   201     5755   22 47 01

22 50 30  J0132+4325   02 19 52  74.2 -31.9  0.8     141.2    -9     5755   22 50 39
22 52 00  =0129+431    02 21 22  74.1 -32.7  0.8     140.2    81     5776   22 50 31

22 52 00  B0128+437    02 21 22  73.5 -32.2  0.8     140.4    -9     5776   22 52 09
22 53 00  ---          02 22 23  73.3 -32.6  0.8     139.7    51     5789   22 52 01

22 53 00  B0128+437    02 22 23  73.3 -32.6  0.8     139.7    -6     5789   22 53 06
22 56 30  ---          02 25 53  72.9 -34.3  0.9     137.6   204     5842   22 53 01

22 56 45  J0132+4325   02 26 08  73.5 -35.0  0.9     137.1     6     5842   22 56 45
22 58 15  =0129+431    02 27 38  73.3 -35.7  0.9     136.2    90     5865   22 56 46

22 58 15  B0128+437    02 27 38  72.7 -35.1  0.9     136.5    -9     5865   22 58 24
23 01 45  ---          02 31 09  72.3 -36.6  1.0     134.5   201     5917   22 58 16

23 01 45  J0132+4325   02 31 09  72.8 -37.2  1.0     134.1    -9     5917   23 01 54
23 03 15  =0129+431    02 32 39  72.6 -37.9  1.0     133.2    81     5938   23 01 46

23 03 15  B0128+437    02 32 39  72.1 -37.2  1.0     133.6    -9     5938   23 03 24
23 06 45  ---          02 36 10  71.6 -38.5  1.1     131.7   201     5990   23 03 16

23 07 00  J0132+4325   02 36 25  72.1 -39.4  1.0     131.1     6     5990   23 07 00
23 08 30  =0129+431    02 37 55  71.9 -39.9  1.1     130.3    90     6013   23 07 01

23 08 30  B0128+437    02 37 55  71.4 -39.2  1.1     130.8    -9     6013   23 08 39
23 12 00  ---          02 41 26  70.9 -40.4  1.1     129.0   201     6065   23 08 31

23 12 00  J0132+4325   02 41 26  71.4 -41.2  1.1     128.5    -9     6065   23 12 09
23 13 30  =0129+431    02 42 56  71.2 -41.8  1.1     127.8    81     6085   23 12 01

23 13 30  B0128+437    02 42 56  70.7 -41.0  1.2     128.3    -9     6085   23 13 39
23 14 30  ---          02 43 56  70.5 -41.3  1.2     127.8    51     6099   23 13 31

23 14 30  B0128+437    02 43 56  70.5 -41.3  1.2     127.8    -6     6099   23 14 36
23 18 00  ---          02 47 27  70.0 -42.4  1.2     126.1   204     6151   23 14 31

23 18 15  J0132+4325   02 47 42  70.5 -43.3  1.2     125.5     6     6151   23 18 15
23 19 45  =0129+431    02 49 12  70.3 -43.8  1.3     124.8    90     6174   23 18 16

23 19 45  B0128+437    02 49 12  69.8 -42.9  1.3     125.3    -9     6174   23 19 54
23 23 15  ---          02 52 42  69.3 -44.0  1.3     123.7   201     6226   23 19 46
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

23 23 15  J0132+4325   02 52 42  69.8 -44.8  1.3     123.2    -9     6226   23 23 24
23 24 45  =0129+431    02 54 13  69.6 -45.3  1.3     122.5    81     6247   23 23 16

23 24 45  B0128+437    02 54 13  69.0 -44.4  1.4     123.1    -9     6247   23 24 54
23 28 15  ---          02 57 43  68.5 -45.3  1.4     121.6   201     6299   23 24 46

23 28 30  J0132+4325   02 57 58  69.0 -46.3  1.4     120.9     6     6299   23 28 30
23 30 00  =0129+431    02 59 29  68.7 -46.7  1.4     120.3    90     6322   23 28 31

23 30 00  B0128+437    02 59 29  68.2 -45.8  1.4     120.9    -9     6322   23 30 09
23 33 30  ---          03 02 59  67.7 -46.6  1.5     119.5   201     6374   23 30 01

23 33 30  J0132+4325   03 02 59  68.2 -47.5  1.5     118.9    -9     6374   23 33 39
23 35 00  =0129+431    03 04 29  68.0 -47.9  1.5     118.3    81     6395   23 33 31

23 35 00  B0128+437    03 04 29  67.5 -46.9  1.5     118.9    -9     6395   23 35 09
23 36 00  ---          03 05 30  67.3 -47.2  1.5     118.5    51     6408   23 35 01

23 36 00  B0128+437    03 05 30  67.3 -47.2  1.5     118.5    -6     6408   23 36 06
23 39 30  ---          03 09 00  66.7 -47.9  1.6     117.2   204     6460   23 36 01

23 39 45  J0132+4325   03 09 15  67.2 -48.9  1.6     116.5     6     6460   23 39 45
23 41 15  =0129+431    03 10 45  66.9 -49.2  1.6     116.0    90     6483   23 39 46

23 41 15  B0128+437    03 10 45  66.5 -48.3  1.6     116.6    -9     6483   23 41 24
23 44 45  ---          03 14 16  65.9 -49.0  1.7     115.3   201     6535   23 41 16

23 44 45  J0132+4325   03 14 16  66.4 -49.9  1.7     114.8    -9     6535   23 44 54
23 46 15  =0129+431    03 15 46  66.1 -50.2  1.7     114.2    81     6556   23 44 46

 ---------- Scan set 34 FF ----------

23 47 45  3C84         03 17 17  79.0   4.0 -0.1    -175.4    43     6556   23 47 45
23 50 45  ---          03 20 17  79.0   1.1 -0.0    -178.8   180     6602   23 47 46

23 52 15  J0132+4325   03 21 47  65.1 -51.2  1.8     112.2    45     6602   23 52 15
23 53 45  =0129+431    03 23 18  64.9 -51.5  1.8     111.8    90     6626   23 52 16

23 53 45  B0128+437    03 23 18  64.4 -50.5  1.8     112.4    -9     6626   23 53 54
23 56 45  ---          03 26 18  63.9 -51.0  1.9     111.4   171     6670   23 53 46

23 56 45  J0132+4325   03 26 18  64.4 -51.9  1.9     110.8    -9     6670   23 56 54
23 58 15  =0129+431    03 27 48  64.1 -52.1  1.9     110.4    81     6691   23 56 46
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  26 Feb 2024   Day  57 ---

23 58 15  B0128+437    03 27 48  63.7 -51.2  1.9     111.0    -9     6691   23 58 24
23 59 15  ---          03 28 48  63.5 -51.4  1.9     110.7    51     6704   23 58 16

 --- Start: Mon  26 Feb 2024   Day  57 -- Stop: Tue  27 Feb 2024   Day  58 ---

23 59 15  B0128+437    03 28 48  63.5 -51.4  1.9     110.7    -6     6704   23 59 21
00 02 45  ---          03 32 19  62.9 -51.8  2.0     109.6   204     6756   23 59 16

00 03 00  J0132+4325   03 32 34  63.3 -52.8  2.0     109.0     6     6756   00 03 00
00 04 30  =0129+431    03 34 04  63.0 -53.0  2.0     108.5    90     6779   00 03 01

00 04 30  B0128+437    03 34 04  62.6 -52.1  2.0     109.1    -9     6779   00 04 39
00 08 00  ---          03 37 35  62.0 -52.5  2.1     108.1   201     6831   00 04 31

00 08 00  J0132+4325   03 37 35  62.4 -53.4  2.1     107.6    -9     6831   00 08 09
00 09 30  =0129+431    03 39 05  62.2 -53.6  2.1     107.1    81     6852   00 08 01

00 09 30  B0128+437    03 39 05  61.7 -52.7  2.1     107.7    -9     6852   00 09 39
00 13 00  ---          03 42 36  61.1 -53.1  2.2     106.7   201     6904   00 09 31

00 13 15  J0132+4325   03 42 51  61.5 -54.0  2.1     106.1     6     6904   00 13 15
00 14 45  =0129+431    03 44 21  61.3 -54.2  2.2     105.7    90     6927   00 13 16

00 14 45  B0128+437    03 44 21  60.8 -53.2  2.2     106.3    -9     6927   00 14 54
00 18 15  ---          03 47 52  60.2 -53.6  2.3     105.4   201     6979   00 14 46

00 18 15  J0132+4325   03 47 52  60.6 -54.5  2.2     104.8    -9     6979   00 18 24
00 19 45  =0129+431    03 49 22  60.4 -54.7  2.3     104.4    81     7000   00 18 16

00 19 45  B0128+437    03 49 22  60.0 -53.7  2.3     105.0    -9     7000   00 19 54
00 20 45  ---          03 50 22  59.8 -53.8  2.3     104.7    51     7013   00 19 46

00 20 45  B0128+437    03 50 22  59.8 -53.8  2.3     104.7    -6     7013   00 20 51
00 24 15  ---          03 53 53  59.2 -54.1  2.4     103.9   204     7065   00 20 46

00 24 30  J0132+4325   03 54 08  59.5 -55.1  2.3     103.3     7     7065   00 24 30
00 26 00  =0129+431    03 55 38  59.3 -55.2  2.4     102.9    90     7089   00 24 31

00 26 00  B0128+437    03 55 38  58.9 -54.3  2.4     103.4    -9     7089   00 26 09
00 29 30  ---          03 59 08  58.3 -54.6  2.4     102.6   201     7140   00 26 01

00 29 30  J0132+4325   03 59 08  58.6 -55.5  2.4     102.1    -8     7140   00 29 38
00 31 00  =0129+431    04 00 39  58.4 -55.6  2.4     101.7    82     7162   00 29 31
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

00 31 00  B0128+437    04 00 39  58.0 -54.7  2.5     102.2    -8     7162   00 31 08
00 34 30  ---          04 04 09  57.4 -54.9  2.5     101.4   202     7214   00 31 01

00 34 45  J0132+4325   04 04 24  57.7 -55.8  2.5     100.9     7     7214   00 34 45
00 36 15  =0129+431    04 05 54  57.4 -55.9  2.5     100.5    90     7237   00 34 46

00 36 15  B0128+437    04 05 54  57.1 -55.0  2.6     101.0    -8     7237   00 36 23
00 39 45  ---          04 09 25  56.5 -55.2  2.6     100.2   202     7289   00 36 16

00 39 45  J0132+4325   04 09 25  56.8 -56.1  2.6      99.7    -8     7289   00 39 53
00 41 15  =0129+431    04 10 55  56.6 -56.2  2.6      99.4    82     7310   00 39 46

00 41 15  B0128+437    04 10 55  56.2 -55.3  2.6      99.9    -8     7310   00 41 23
00 42 15  ---          04 11 55  56.0 -55.4  2.7      99.7    52     7323   00 41 16

00 42 15  B0128+437    04 11 55  56.0 -55.4  2.7      99.7    -6     7323   00 42 21
00 45 45  ---          04 15 26  55.4 -55.5  2.7      98.9   204     7376   00 42 16

00 46 00  J0132+4325   04 15 41  55.7 -56.4  2.7      98.4     7     7376   00 46 00
00 47 30  =0129+431    04 17 11  55.4 -56.5  2.7      98.1    90     7399   00 46 01

00 47 30  B0128+437    04 17 11  55.1 -55.6  2.7      98.5    -8     7399   00 47 38
00 51 00  ---          04 20 42  54.5 -55.8  2.8      97.8   202     7451   00 47 31

00 51 00  J0132+4325   04 20 42  54.8 -56.7  2.8      97.3    -8     7451   00 51 08
00 52 30  =0129+431    04 22 12  54.5 -56.7  2.8      97.0    82     7472   00 51 01

00 52 30  B0128+437    04 22 12  54.2 -55.8  2.8      97.5    -8     7472   00 52 38
00 56 00  ---          04 25 43  53.6 -56.0  2.9      96.8   202     7524   00 52 31

00 56 15  J0132+4325   04 25 58  53.9 -56.9  2.9      96.3     7     7524   00 56 15
00 57 45  =0129+431    04 27 28  53.6 -56.9  2.9      96.0    90     7548   00 56 16

00 57 45  B0128+437    04 27 28  53.3 -56.0  2.9      96.4    -8     7548   00 57 53
01 01 15  ---          04 30 59  52.6 -56.2  3.0      95.7   202     7600   00 57 46

01 01 15  J0132+4325   04 30 59  52.9 -57.0  2.9      95.3    -8     7600   01 01 23
01 02 45  =0129+431    04 32 29  52.7 -57.0  3.0      95.0    82     7621   01 01 16

01 02 45  B0128+437    04 32 29  52.4 -56.2  3.0      95.4    -8     7621   01 02 53
01 03 45  ---          04 33 29  52.2 -56.2  3.0      95.2    52     7634   01 02 46

01 03 45  B0128+437    04 33 29  52.2 -56.2  3.0      95.2    -6     7634   01 03 51
01 07 15  ---          04 37 00  51.5 -56.3  3.1      94.5   204     7687   01 03 46
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

01 07 30  J0132+4325   04 37 15  51.8 -57.2  3.1      94.1     7     7687   01 07 30
01 09 00  =0129+431    04 38 45  51.5 -57.2  3.1      93.8    90     7710   01 07 31

01 09 00  B0128+437    04 38 45  51.2 -56.3  3.1      94.2    -8     7710   01 09 08
01 12 30  ---          04 42 15  50.6 -56.4  3.2      93.5   202     7762   01 09 01

01 12 30  J0132+4325   04 42 15  50.9 -57.3  3.1      93.2    -8     7762   01 12 38
01 14 00  =0129+431    04 43 46  50.6 -57.3  3.2      92.9    82     7783   01 12 31

01 14 00  B0128+437    04 43 46  50.3 -56.4  3.2      93.3    -8     7783   01 14 08
01 17 30  ---          04 47 16  49.7 -56.5  3.2      92.6   202     7835   01 14 01

01 17 45  J0132+4325   04 47 31  50.0 -57.3  3.2      92.2     7     7835   01 17 45
01 19 15  =0129+431    04 49 02  49.7 -57.3  3.2      91.9    90     7858   01 17 46

01 19 15  B0128+437    04 49 02  49.4 -56.5  3.3      92.3    -8     7858   01 19 23
01 22 45  ---          04 52 32  48.8 -56.5  3.3      91.7   202     7910   01 19 16

01 22 45  J0132+4325   04 52 32  49.0 -57.4  3.3      91.3    -8     7910   01 22 53
01 24 15  =0129+431    04 54 02  48.8 -57.4  3.3      91.0    82     7931   01 22 46

01 24 15  B0128+437    04 54 02  48.5 -56.6  3.4      91.4    -8     7931   01 24 23
01 25 15  ---          04 55 03  48.3 -56.6  3.4      91.2    52     7945   01 24 16

01 25 15  B0128+437    04 55 03  48.3 -56.6  3.4      91.2    -6     7945   01 25 21
01 28 45  ---          04 58 33  47.7 -56.6  3.4      90.6   204     7997   01 25 16

01 29 00  J0132+4325   04 58 48  47.9 -57.4  3.4      90.2     7     7997   01 29 00
01 30 30  =0129+431    05 00 18  47.6 -57.4  3.4      89.9    90     8021   01 29 01

01 30 30  B0128+437    05 00 18  47.4 -56.6  3.5      90.3    -8     8021   01 30 38
01 34 00  ---          05 03 49  46.7 -56.6  3.5      89.7   202     8073   01 30 31

01 34 00  J0132+4325   05 03 49  47.0 -57.4  3.5      89.3    -8     8073   01 34 08
01 35 30  =0129+431    05 05 19  46.7 -57.4  3.5      89.1    82     8094   01 34 01

01 35 30  B0128+437    05 05 19  46.5 -56.6  3.5      89.4    -8     8094   01 35 38
01 39 00  ---          05 08 50  45.8 -56.6  3.6      88.8   202     8146   01 35 31

01 39 15  J0132+4325   05 09 05  46.1 -57.4  3.6      88.5     7     8146   01 39 15
01 40 45  =0129+431    05 10 35  45.8 -57.3  3.6      88.2    90     8169   01 39 16

01 40 45  B0128+437    05 10 35  45.5 -56.6  3.6      88.5    -8     8169   01 40 53
01 44 15  ---          05 14 06  44.9 -56.5  3.7      87.9   202     8221   01 40 46
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

01 44 15  J0132+4325   05 14 06  45.1 -57.3  3.7      87.6    -8     8221   01 44 23
01 45 45  =0129+431    05 15 36  44.9 -57.3  3.7      87.4    82     8242   01 44 16

01 45 45  B0128+437    05 15 36  44.6 -56.5  3.7      87.7    -8     8242   01 45 53
01 46 45  ---          05 16 36  44.4 -56.5  3.7      87.5    52     8256   01 45 46

01 46 45  B0128+437    05 16 36  44.4 -56.5  3.7      87.5    -6     8256   01 46 51
01 50 15  ---          05 20 07  43.8 -56.5  3.8      86.9   204     8308   01 46 46

01 50 30  J0132+4325   05 20 22  44.0 -57.2  3.8      86.6     7     8308   01 50 30
01 52 00  =0129+431    05 21 52  43.7 -57.2  3.8      86.4    90     8331   01 50 31

01 52 00  B0128+437    05 21 52  43.5 -56.4  3.8      86.6    -8     8331   01 52 08
01 55 30  ---          05 25 23  42.9 -56.4  3.9      86.1   202     8383   01 52 01

01 55 30  J0132+4325   05 25 23  43.1 -57.1  3.9      85.8    -8     8383   01 55 38
01 57 00  =0129+431    05 26 53  42.8 -57.1  3.9      85.6    82     8404   01 55 31

01 57 00  B0128+437    05 26 53  42.6 -56.4  3.9      85.8    -8     8404   01 57 08
02 00 30  ---          05 30 23  42.0 -56.3  4.0      85.3   202     8456   01 57 01

02 00 45  J0132+4325   05 30 38  42.2 -57.0  3.9      85.0     7     8456   02 00 45
02 02 15  =0129+431    05 32 09  41.9 -57.0  4.0      84.7    90     8480   02 00 46

02 02 15  B0128+437    05 32 09  41.7 -56.2  4.0      85.0    -8     8480   02 02 23
02 05 45  ---          05 35 39  41.0 -56.2  4.1      84.4   202     8532   02 02 16

02 05 45  J0132+4325   05 35 39  41.2 -56.9  4.0      84.2    -8     8532   02 05 53
02 07 15  =0129+431    05 37 09  41.0 -56.9  4.1      83.9    82     8553   02 05 46

02 07 15  B0128+437    05 37 09  40.8 -56.1  4.1      84.2    -8     8553   02 07 23
02 08 15  ---          05 38 10  40.6 -56.1  4.1      84.0    52     8566   02 07 16

02 08 15  B0128+437    05 38 10  40.6 -56.1  4.1      84.0    -6     8566   02 08 21
02 11 45  ---          05 41 40  40.0 -56.0  4.2      83.5   204     8619   02 08 16

02 12 00  J0132+4325   05 41 55  40.1 -56.8  4.1      83.2     7     8619   02 12 00
02 13 30  =0129+431    05 43 25  39.8 -56.7  4.2      83.0    90     8642   02 12 01

02 13 30  B0128+437    05 43 25  39.6 -56.0  4.2      83.2    -8     8642   02 13 38
02 17 00  ---          05 46 56  39.0 -55.9  4.2      82.6   202     8694   02 13 31

02 17 00  J0132+4325   05 46 56  39.2 -56.6  4.2      82.4    -8     8694   02 17 08
02 18 30  =0129+431    05 48 26  38.9 -56.6  4.2      82.2    82     8715   02 17 01
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

02 18 30  B0128+437    05 48 26  38.8 -55.8  4.3      82.4    -8     8715   02 18 38
02 22 00  ---          05 51 57  38.1 -55.7  4.3      81.9   202     8767   02 18 31

02 22 15  J0132+4325   05 52 12  38.3 -56.4  4.3      81.6     7     8767   02 22 15
02 23 45  =0129+431    05 53 42  38.0 -56.4  4.3      81.4    90     8790   02 22 16

02 23 45  B0128+437    05 53 42  37.8 -55.7  4.4      81.6    -8     8790   02 23 53
02 27 15  ---          05 57 13  37.2 -55.5  4.4      81.1   202     8842   02 23 46

02 27 15  J0132+4325   05 57 13  37.4 -56.3  4.4      80.9    -8     8842   02 27 23
02 28 45  =0129+431    05 58 43  37.1 -56.2  4.4      80.7    82     8864   02 27 16

02 28 45  B0128+437    05 58 43  36.9 -55.5  4.4      80.8    -8     8864   02 28 53
02 29 45  ---          05 59 43  36.7 -55.5  4.5      80.7    52     8877   02 28 46

02 29 45  B0128+437    05 59 43  36.7 -55.5  4.5      80.7    -6     8877   02 29 51
02 33 15  ---          06 03 14  36.1 -55.3  4.5      80.1   204     8929   02 29 46

02 33 30  J0132+4325   06 03 29  36.3 -56.0  4.5      79.9     7     8929   02 33 30
02 35 00  =0129+431    06 04 59  36.0 -56.0  4.5      79.7    90     8953   02 33 31

02 35 00  B0128+437    06 04 59  35.8 -55.3  4.5      79.9    -8     8953   02 35 08
02 38 30  ---          06 08 30  35.2 -55.1  4.6      79.3   202     9005   02 35 01

02 38 30  J0132+4325   06 08 30  35.4 -55.8  4.6      79.2    -8     9005   02 38 38
02 40 00  =0129+431    06 10 00  35.1 -55.8  4.6      79.0    82     9026   02 38 31

02 40 00  B0128+437    06 10 00  34.9 -55.1  4.6      79.1    -8     9026   02 40 08
02 43 30  ---          06 13 30  34.3 -54.9  4.7      78.6   202     9078   02 40 01

02 43 45  J0132+4325   06 13 45  34.4 -55.6  4.7      78.4     7     9078   02 43 45
02 45 15  =0129+431    06 15 16  34.2 -55.5  4.7      78.2    90     9101   02 43 46

02 45 15  B0128+437    06 15 16  34.0 -54.8  4.7      78.3    -8     9101   02 45 23
02 48 45  ---          06 18 46  33.4 -54.7  4.8      77.8   202     9153   02 45 16

02 48 45  J0132+4325   06 18 46  33.5 -55.4  4.7      77.7    -8     9153   02 48 53
02 50 15  =0129+431    06 20 16  33.3 -55.3  4.8      77.5    82     9174   02 48 46

02 50 15  B0128+437    06 20 16  33.1 -54.6  4.8      77.6    -8     9174   02 50 23
02 51 15  ---          06 21 17  32.9 -54.6  4.8      77.4    52     9188   02 50 16

02 51 15  B0128+437    06 21 17  32.9 -54.6  4.8      77.4    -6     9188   02 51 21
02 54 45  ---          06 24 47  32.3 -54.4  4.9      76.9   204     9240   02 51 16
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

02 55 00  J0132+4325   06 25 02  32.4 -55.1  4.8      76.8     7     9240   02 55 00
02 56 30  =0129+431    06 26 33  32.2 -55.0  4.9      76.5    90     9263   02 55 01

02 56 30  B0128+437    06 26 33  32.0 -54.3  4.9      76.7    -8     9263   02 56 38
03 00 00  ---          06 30 03  31.4 -54.1  5.0      76.1   202     9315   02 56 31

03 00 00  J0132+4325   06 30 03  31.5 -54.8  4.9      76.0    -8     9315   03 00 08
03 01 30  =0129+431    06 31 33  31.3 -54.7  5.0      75.8    82     9337   03 00 01

03 01 30  B0128+437    06 31 33  31.2 -54.1  5.0      75.9    -8     9337   03 01 38
03 05 00  ---          06 35 04  30.5 -53.9  5.0      75.4   202     9389   03 01 31

03 05 15  J0132+4325   06 35 19  30.6 -54.6  5.0      75.3     7     9389   03 05 15
03 06 45  =0129+431    06 36 49  30.4 -54.5  5.0      75.1    90     9412   03 05 16

03 06 45  B0128+437    06 36 49  30.2 -53.8  5.1      75.1    -8     9412   03 06 53
03 10 15  ---          06 40 20  29.6 -53.6  5.1      74.6   202     9464   03 06 46

03 10 15  J0132+4325   06 40 20  29.7 -54.3  5.1      74.5    -8     9464   03 10 23
03 11 45  =0129+431    06 41 50  29.5 -54.2  5.1      74.3    82     9485   03 10 16

03 11 45  B0128+437    06 41 50  29.4 -53.5  5.2      74.4    -8     9485   03 11 53
03 12 45  ---          06 42 50  29.2 -53.5  5.2      74.3    52     9498   03 11 46

03 12 45  B0128+437    06 42 50  29.2 -53.5  5.2      74.3    -6     9498   03 12 51
03 16 15  ---          06 46 21  28.6 -53.3  5.2      73.7   204     9551   03 12 46

03 16 30  J0132+4325   06 46 36  28.7 -53.9  5.2      73.6     7     9551   03 16 30
03 18 00  =0129+431    06 48 06  28.4 -53.8  5.2      73.4    90     9574   03 16 31

03 18 00  B0128+437    06 48 06  28.3 -53.2  5.3      73.5    -8     9574   03 18 08
03 21 30  ---          06 51 37  27.7 -52.9  5.3      73.0   202     9626   03 18 01

03 21 30  J0132+4325   06 51 37  27.8 -53.6  5.3      72.9    -8     9626   03 21 38
03 23 00  =0129+431    06 53 07  27.5 -53.5  5.3      72.7    82     9647   03 21 31

03 23 00  B0128+437    06 53 07  27.4 -52.9  5.3      72.7    -8     9647   03 23 08
03 26 30  ---          06 56 37  26.8 -52.6  5.4      72.2   202     9699   03 23 01

03 26 45  J0132+4325   06 56 52  26.9 -53.3  5.4      72.2     7     9699   03 26 45
03 28 15  =0129+431    06 58 23  26.6 -53.2  5.4      71.9    90     9722   03 26 46

03 28 15  B0128+437    06 58 23  26.5 -52.5  5.4      72.0    -8     9722   03 28 23
03 31 45  ---          07 01 53  25.9 -52.3  5.5      71.5   202     9775   03 28 16
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GW023B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  27 Feb 2024   Day  58 ---

03 31 45  J0132+4325   07 01 53  26.0 -53.0  5.5      71.4    -8     9775   03 31 53
03 33 15  =0129+431    07 03 24  25.8 -52.9  5.5      71.2    82     9796   03 31 46

03 33 15  B0128+437    07 03 24  25.7 -52.2  5.5      71.2    -8     9796   03 33 23
03 34 15  ---          07 04 24  25.5 -52.2  5.5      71.1    52     9809   03 33 16

03 34 15  B0128+437    07 04 24  25.5 -52.2  5.5      71.1    -6     9809   03 34 21
03 37 45  ---          07 07 54  24.9 -51.9  5.6      70.6   204     9862   03 34 16

03 38 00  J0132+4325   07 08 09  24.9 -52.6  5.6      70.5     7     9862   03 38 00
03 39 30  =0129+431    07 09 40  24.7 -52.5  5.6      70.3    90     9885   03 38 01

03 39 30  B0128+437    07 09 40  24.6 -51.8  5.6      70.3    -8     9885   03 39 38
03 43 00  ---          07 13 10  24.0 -51.6  5.7      69.8   202     9937   03 39 31

03 43 00  J0132+4325   07 13 10  24.1 -52.2  5.7      69.8    -8     9937   03 43 08
03 44 30  =0129+431    07 14 40  23.8 -52.1  5.7      69.6    82     9958   03 43 01

03 44 30  B0128+437    07 14 40  23.8 -51.5  5.7      69.6    -8     9958   03 44 38
03 48 00  ---          07 18 11  23.2 -51.2  5.8      69.1   202    10010   03 44 31

03 48 15  J0132+4325   07 18 26  23.2 -51.9  5.7      69.0     7    10010   03 48 15
03 49 45  =0129+431    07 19 56  22.9 -51.8  5.8      68.8    90    10033   03 48 16

03 49 45  B0128+437    07 19 56  22.9 -51.1  5.8      68.8    -8    10033   03 49 53
03 53 15  ---          07 23 27  22.3 -50.9  5.8      68.3   202    10085   03 49 46

03 53 15  J0132+4325   07 23 27  22.3 -51.5  5.8      68.3    -8    10085   03 53 23
03 54 45  =0129+431    07 24 57  22.1 -51.4  5.8      68.1    82    10106   03 53 16

 ---------- Scan set 47 ----------

03 54 45  B0128+437    07 24 57  22.0 -50.7  5.9      68.1    -8    10106   03 54 53
03 57 45  ---          07 27 58  21.5 -50.5  5.9      67.6   172    10151   03 54 46

03 57 45  J0132+4325   07 27 58  21.6 -51.2  5.9      67.7    -8    10151   03 57 53
03 59 27  =0129+431    07 29 40  21.3 -51.1  5.9      67.4    94    10175   03 57 46


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess124.C2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    5         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  20  Setup file default.  Used with PCAL = off
   LO sum=   4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  20  21  22  23  24  25  26  27  28  29

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * B0128+437         01 28 15.245932   * 01 31 13.491000     01 32 37.920649       0.00
                     43 42 46.77735    * 43 58 12.85100      44 05 45.20346        0.00
                     From catalog imbedded in main SCHED input file.

   0129+431          01 29 45.959987   * 01 32 44.126798     01 34 08.543723       0.20
 * J0132+4325        43 10 09.12650    * 43 25 32.66097      43 33 03.72690        0.19
                     /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,     94 observations.

 * 3C84              03 16 29.567265   * 03 19 48.160096     03 21 23.294230       1.50
   J0319+4130        41 19 51.91692    * 41 30 42.10404      41 36 05.04981        2.86
   0316+413          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0319+41          GSFC 2016a X/S astro solution,  10291 observations.

 * 3C147             05 38 43.517517   * 05 42 36.137894     05 44 28.872436       0.04
   J0542+4951        49 49 42.83709    * 49 51 07.23372      49 51 59.86927        0.03
   0538+498          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0542+49          GSFC 2016a X/S astro solution,   1444 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  B0128+437  sess124.C2048glob     1 2 3 4 5 6 7 8 9 11 16 17  +    13.075  1643.802
  J0132+4325 sess124.C2048glob     1 2 3 4 5 6 7 8 9 11 16 17  +     5.652   698.416
  3C84       sess124.C2048glob     1 2 3 4 5 6 7 8 9 11 16 17  +     0.200    32.455
  3C147      sess124.C2048glob     18                                0.054     0.000

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   0133+476          01 33 55.103060   * 01 36 58.594805     01 38 25.490847       0.00
 * J0136+4751        47 36 12.85364    * 47 51 29.10003      47 58 58.06347        0.00
   J0136+47          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution, 193511 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   B0128+437           66.0
   J0132+4325          65.8
   J0136+4751          69.3
   3C84                82.0
   3C147              107.5

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

