  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Global 7mm VLBI observations of Cygnus A
 Exp. Code:  GB075A  


Schedule Version:       5.00
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Biagina Boccardi

Address:  Max Planck Institute for Radioastronomy
          Auf dem Huegel 69
          Bonn, 53121
           Germany

Phone:    +49 (0)228 525 366
EMAIL:    bboccardi@mpifr-bonn.mpg.de
Fax:      +49-2257-301-106
Phone during observation: +49-2257-301-155

Observing mode: 1024-32-2

Notes:
 
 
 


COVER LETTER:

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

 Next scan frequencies:  43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
 Next BBC frequencies:     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

02 12 00  CYG-A        12 21 47   3.6  43.6 -7.6     -51.6     0        0   02 12 00
02 21 00  ---          12 30 49   4.9  44.7 -7.5     -53.0   540       70   02 12 01

02 41 00  2013+370     12 50 52   3.4  48.0 -7.4     -53.4  1187       70   02 41 00
02 44 00  ---          12 53 52   3.9  48.4 -7.4     -53.9   180       93   02 41 01

02 46 00  CYG-A        12 55 53   8.8  47.4 -7.1     -56.8   103       93   02 46 00
02 55 00  ---          13 04 54  10.2  48.4 -6.9     -58.1   540      162   02 46 01

03 01 00  2013+370     13 10 55   6.7  50.3 -7.1     -56.3   343      162   03 01 00
03 04 00  ---          13 13 56   7.2  50.6 -7.0     -56.7   180      185   03 01 01

03 06 00  CYG-A        13 15 56  12.0  49.5 -6.7     -59.7   103      185   03 06 00
03 15 00  ---          13 24 57  13.5  50.3 -6.6     -61.0   540      255   03 06 01

03 16 00  CYG-A        13 25 58  13.7  50.4 -6.6     -61.1    54      255   03 16 00
03 19 00  ---          13 28 58  14.2  50.7 -6.5     -61.6   180      278   03 16 01

03 24 00  2013+370     13 33 59  10.6  52.8 -6.7     -59.4   283      278   03 24 00
03 26 00  ---          13 35 59  10.9  53.0 -6.7     -59.6   120      294   03 24 01

03 28 00  CYG-A        13 38 00  15.7  51.5 -6.4     -62.8   103      294   03 28 00
03 37 00  ---          13 47 01  17.2  52.3 -6.2     -64.1   540      363   03 28 01

03 43 00  2013+370     13 53 02  13.9  54.7 -6.4     -61.9   343      363   03 43 00
03 46 00  ---          13 56 03  14.4  55.0 -6.3     -62.2   180      386   03 43 01

03 48 00  CYG-A        13 58 03  19.1  53.3 -6.0     -65.6   103      386   03 48 00
03 57 00  ---          14 07 04  20.7  54.0 -5.9     -66.8   540      456   03 48 01

03 58 00  CYG-A        14 08 05  20.8  54.1 -5.9     -66.9    54      456   03 58 00
04 01 00  ---          14 11 05  21.4  54.3 -5.8     -67.3   180      479   03 58 01

04 06 00  2013+370     14 16 06  18.0  56.8 -6.0     -64.8   284      479   04 06 00
04 08 00  ---          14 18 06  18.3  57.0 -6.0     -65.0   120      495   04 06 01

04 10 00  CYG-A        14 20 06  22.9  55.0 -5.7     -68.6   104      495   04 10 00
04 19 00  ---          14 29 08  24.5  55.7 -5.5     -69.8   540      564   04 10 01

04 28 00  BLLAC        14 38 09   6.4  43.9 -7.4     -53.8   494      564   04 28 00
04 30 00  ---          14 40 10   6.7  44.1 -7.4     -54.1   120      580   04 28 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

04 39 00  2013+370     14 49 11  24.0  59.6 -5.4     -68.8   501      580   04 39 00
04 42 00  ---          14 52 12  24.6  59.8 -5.4     -69.1   180      603   04 39 01

04 44 00  CYG-A        14 54 12  29.0  57.4 -5.1     -73.1   104      603   04 44 00
04 53 00  ---          15 03 14  30.7  57.9 -4.9     -74.3   540      672   04 44 01

04 59 00  2013+370     15 09 15  27.8  61.1 -5.1     -71.1   344      672   04 59 00
05 02 00  ---          15 12 15  28.3  61.3 -5.1     -71.5   180      696   04 59 01

05 03 00  CYG-A        15 13 15  32.5  58.5 -4.8     -75.6    44      696   05 03 00
05 12 00  ---          15 22 17  34.2  59.0 -4.6     -76.8   540      765   05 03 01

05 13 00  CYG-A        15 23 17  34.4  59.0 -4.6     -77.0    54      765   05 13 00
05 16 00  ---          15 26 17  34.9  59.2 -4.6     -77.4   180      788   05 13 01

05 21 00  2013+370     15 31 18  32.0  62.7 -4.7     -73.7   284      788   05 21 00
05 23 00  ---          15 33 18  32.3  62.8 -4.7     -74.0   120      804   05 21 01

05 24 00  CYG-A        15 34 19  36.4  59.6 -4.4     -78.5    44      804   05 24 00
05 33 00  ---          15 43 20  38.1  60.0 -4.3     -79.7   540      873   05 24 01

05 39 00  2013+370     15 49 21  35.4  63.8 -4.4     -75.8   345      873   05 39 00
05 42 00  ---          15 52 22  36.0  64.0 -4.4     -76.2   180      897   05 39 01

05 43 00  CYG-A        15 53 22  39.9  60.4 -4.1     -81.1    45      897   05 43 00
05 52 00  ---          16 02 23  41.6  60.7 -4.0     -82.3   540      966   05 43 01

05 53 00  CYG-A        16 03 23  41.8  60.8 -3.9     -82.5    54      966   05 53 00
05 56 00  ---          16 06 24  42.4  60.9 -3.9     -82.9   180      989   05 53 01

06 01 00  2013+370     16 11 25  39.7  65.0 -4.1     -78.4   285      989   06 01 00
06 03 00  ---          16 13 25  40.1  65.1 -4.0     -78.6   120     1005   06 01 01

06 04 00  CYG-A        16 14 25  43.9  61.1 -3.8     -84.0    45     1005   06 04 00
06 13 00  ---          16 23 27  45.6  61.3 -3.6     -85.4   540     1074   06 04 01

06 22 00  BLLAC        16 32 28  25.1  54.0 -5.5     -70.4   489     1074   06 22 00
06 24 00  ---          16 34 28  25.4  54.2 -5.5     -70.7   120     1090   06 22 01

06 33 00  2013+370     16 43 30  46.0  66.5 -3.5     -82.3   495     1090   06 33 00
06 35 00  ---          16 45 30  46.4  66.6 -3.5     -82.5   120     1105   06 33 01

06 36 00  CYG-A        16 46 30  50.0  61.6 -3.2     -88.9    45     1105   06 36 00
06 45 00  ---          16 55 32  51.7  61.7 -3.1     -90.3   540     1175   06 36 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

06 51 00  2013+370     17 01 33  49.6  67.1 -3.2     -84.5   346     1175   06 51 00
06 54 00  ---          17 04 33  50.2  67.2 -3.2     -84.9   180     1198   06 51 01

06 55 00  CYG-A        17 05 34  53.6  61.6 -2.9     -92.0    46     1198   06 55 00
07 04 00  ---          17 14 35  55.3  61.4 -2.8     -93.6   540     1268   06 55 01

07 05 00  CYG-A        17 15 35  55.5  61.4 -2.7     -93.8    54     1268   07 05 00
07 08 00  ---          17 18 36  56.0  61.4 -2.7     -94.3   180     1291   07 05 01

07 13 00  2013+370     17 23 37  53.9  67.6 -2.9     -87.5   286     1291   07 13 00
07 15 00  ---          17 25 37  54.3  67.6 -2.8     -87.8   120     1306   07 13 01

07 17 00  CYG-A        17 27 37  57.7  61.1 -2.5     -96.1   106     1306   07 17 00
07 26 00  ---          17 36 39  59.4  60.7 -2.4     -97.9   540     1376   07 17 01

07 32 00  2013+370     17 42 40  57.7  67.7 -2.6     -90.3   346     1376   07 32 00
07 35 00  ---          17 45 40  58.3  67.7 -2.5     -90.7   180     1399   07 32 01

07 37 00  CYG-A        17 47 40  61.5  60.0 -2.2    -100.3   106     1399   07 37 00
07 46 00  ---          17 56 42  63.2  59.3 -2.1    -102.4   540     1469   07 37 01

07 47 00  CYG-A        17 57 42  63.4  59.2 -2.0    -102.6    54     1469   07 47 00
07 50 00  ---          18 00 43  63.9  58.9 -2.0    -103.4   180     1492   07 47 01

07 55 00  2013+370     18 05 43  62.3  67.4 -2.2     -94.1   286     1492   07 55 00
07 57 00  ---          18 07 44  62.7  67.3 -2.1     -94.4   120     1507   07 55 01

07 59 00  CYG-A        18 09 44  65.6  57.9 -1.8    -105.7   106     1507   07 59 00
08 08 00  ---          18 18 46  67.2  56.7 -1.7    -108.4   540     1577   07 59 01

08 14 00  2013+370     18 24 47  66.1  66.5 -1.9     -97.8   345     1577   08 14 00
08 17 00  ---          18 27 47  66.7  66.3 -1.8     -98.4   180     1600   08 14 01

08 18 00  CYG-A        18 28 47  69.0  54.9 -1.5    -111.6    44     1600   08 18 00
08 27 00  ---          18 37 49  70.5  53.0 -1.4    -114.9   540     1669   08 18 01

08 28 00  CYG-A        18 38 49  70.7  52.7 -1.4    -115.3    54     1669   08 28 00
08 31 00  ---          18 41 49  71.2  52.0 -1.3    -116.5   180     1693   08 28 01

08 38 00  BLLAC        18 48 51  49.8  59.2 -3.2     -90.6   367     1693   08 38 00
08 40 00  ---          18 50 51  50.2  59.2 -3.2     -90.9   120     1708   08 38 01

08 47 00  2013+370     18 57 52  72.5  62.6 -1.3    -106.4   370     1708   08 47 00
08 50 00  ---          19 00 52  73.1  62.0 -1.3    -107.4   180     1731   08 47 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

08 52 00  CYG-A        19 02 53  74.6  44.8 -1.0    -126.8   100     1731   08 52 00
09 01 00  ---          19 11 54  76.0  40.5 -0.8    -132.4   540     1801   08 52 01

09 02 00  CYG-A        19 12 54  76.1  40.0 -0.8    -133.1    54     1801   09 02 00
09 05 00  ---          19 15 55  76.5  38.3 -0.7    -135.2   180     1824   09 02 01

09 10 00  2013+370     19 20 56  76.8  56.3 -0.9    -116.0   278     1824   09 10 00
09 13 00  ---          19 23 56  77.4  55.1 -0.9    -117.6   180     1847   09 10 01

09 15 00  CYG-A        19 25 57  77.7  31.9 -0.6    -143.1    96     1847   09 15 00
09 24 00  ---          19 34 58  78.7  24.8 -0.4    -151.5   540     1917   09 15 01

09 30 00  2013+370     19 40 59  80.2  45.4 -0.6    -129.7   335     1917   09 30 00
09 33 00  ---          19 44 00  80.6  43.1 -0.5    -132.5   180     1940   09 30 01

09 34 00  CYG-A        19 45 00  79.4  15.7 -0.3    -162.1    33     1940   09 34 00
09 43 00  ---          19 54 01  79.8   6.4 -0.1    -172.7   540     2010   09 34 01

09 44 00  CYG-A        19 55 01  79.8   5.3 -0.1    -173.9    54     2010   09 44 00
09 47 00  ---          19 58 02  79.9   2.1 -0.0    -177.6   180     2033   09 44 01

09 52 00  2013+370     20 03 03  82.9  21.4 -0.2    -156.8   274     2033   09 52 00
09 55 00  ---          20 06 03  83.1  16.8 -0.2    -161.8   180     2056   09 52 01

09 56 00  CYG-A        20 07 03  79.8  -7.5  0.1     171.4    35     2056   09 56 00
10 05 00  ---          20 16 05  79.4 -16.7  0.3     160.9   540     2126   09 56 01

10 06 00  2013+370     20 17 05  83.4  -1.8  0.0     178.1    41     2126   10 06 00
10 09 00  ---          20 20 05  83.4  -7.0  0.1     172.5   180     2149   10 06 01

10 10 00  CYG-A        20 21 06  79.0 -21.4  0.4     155.5    42     2149   10 10 00
10 19 00  ---          20 30 07  78.2 -29.0  0.5     146.6   540     2218   10 10 01

10 25 00  BLLAC        20 36 08  69.0  50.1 -1.5    -116.8   295     2218   10 25 00
10 28 00  ---          20 39 09  69.5  49.3 -1.4    -118.0   180     2241   10 25 01

10 29 00  BLLAC        20 40 09  69.7  49.1 -1.4    -118.4    54     2241   10 29 00
10 31 00  ---          20 42 09  70.0  48.6 -1.4    -119.2   120     2257   10 29 01

10 40 00  2013+370     20 51 11  80.2 -45.5  0.6     129.6   470     2257   10 40 00
10 43 00  ---          20 54 11  79.7 -47.6  0.6     127.1   180     2280   10 40 01

10 45 00  CYG-A        20 56 11  74.8 -44.4  0.9     127.3   103     2280   10 45 00
10 54 00  ---          21 05 13  73.4 -48.0  1.1     122.4   540     2350   10 45 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

10 56 00  2013+370     21 07 13  77.5 -54.7  0.9     118.1   103     2350   10 56 00
10 59 00  ---          21 10 14  77.0 -55.9  0.9     116.5   180     2373   10 56 01

11 00 00  CYG-A        21 11 14  72.4 -50.0  1.2     119.5    43     2373   11 00 00
11 09 00  ---          21 20 15  70.9 -52.5  1.3     115.7   540     2442   11 00 01

11 10 00  CYG-A        21 21 15  70.7 -52.7  1.4     115.3    54     2442   11 10 00
11 19 00  ---          21 30 17  69.1 -54.7  1.5     111.9   540     2512   11 10 01

11 20 00  2013+370     21 31 17  73.1 -62.0  1.3     107.4    44     2512   11 20 00
11 23 00  ---          21 34 18  72.5 -62.6  1.3     106.4   180     2535   11 20 01

11 24 00  CYG-A        21 35 18  68.3 -55.7  1.6     110.2    44     2535   11 24 00
11 33 00  ---          21 44 19  66.6 -57.1  1.7     107.4   540     2605   11 24 01

11 34 00  2013+370     21 45 19  70.4 -64.3  1.5     103.1    44     2605   11 34 00
11 37 00  ---          21 48 20  69.8 -64.7  1.5     102.2   180     2628   11 34 01

11 38 00  CYG-A        21 49 20  65.7 -57.8  1.8     106.0    44     2628   11 38 00
11 47 00  ---          21 58 22  64.1 -58.8  2.0     103.6   540     2697   11 38 01

11 48 00  2013+370     21 59 22  67.7 -65.9  1.7      99.5    45     2697   11 48 00
11 51 00  ---          22 02 22  67.1 -66.1  1.8      98.8   180     2721   11 48 01

11 52 00  CYG-A        22 03 22  63.2 -59.3  2.1     102.3    45     2721   11 52 00
12 00 00  ---          22 11 24  61.7 -59.9  2.2     100.5   480     2782   11 52 01

12 01 00  CYG-A        22 12 24  61.5 -60.0  2.2     100.2    54     2782   12 01 00
12 07 00  ---          22 18 25  60.4 -60.4  2.3      98.9   360     2829   12 01 01

12 08 00  2013+370     22 19 25  63.7 -67.1  2.1      95.3    45     2829   12 08 00
12 11 00  ---          22 22 25  63.1 -67.2  2.1      94.8   180     2852   12 08 01

12 12 00  CYG-A        22 23 26  59.4 -60.7  2.4      97.9    45     2852   12 12 00
12 21 00  ---          22 32 27  57.7 -61.1  2.5      96.0   540     2922   12 12 01

12 22 00  CYG-A        22 33 27  57.5 -61.1  2.6      95.8    54     2922   12 22 00
12 28 00  ---          22 39 28  56.4 -61.3  2.7      94.7   360     2968   12 22 01

12 30 00  BLLAC        22 41 29  76.0 -30.5  0.6     143.8    73     2968   12 30 00
12 32 00  ---          22 43 29  75.8 -31.7  0.7     142.3   120     2983   12 30 01

12 33 00  BLLAC        22 44 29  75.7 -32.3  0.7     141.6    54     2983   12 33 00
12 35 00  ---          22 46 29  75.5 -33.4  0.7     140.1   120     2999   12 33 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

12 36 00  BLLAC        22 47 30  75.3 -34.0  0.7     139.4    54     2999   12 36 00
12 38 00  ---          22 49 30  75.1 -35.1  0.8     138.0   120     3014   12 36 01

12 41 00  2013+370     22 52 30  57.1 -67.7  2.6      89.8   138     3014   12 41 00
12 44 00  ---          22 55 31  56.5 -67.7  2.7      89.4   180     3038   12 41 01

12 45 00  CYG-A        22 56 31  53.2 -61.6  2.9      91.7    46     3038   12 45 00
12 54 00  ---          23 05 33  51.5 -61.7  3.1      90.2   540     3107   12 45 01

12 55 00  2013+370     23 06 33  54.3 -67.6  2.8      87.8    46     3107   12 55 00
12 58 00  ---          23 09 33  53.7 -67.6  2.9      87.3   180     3130   12 55 01

13 00 00  CYG-A        23 11 34  50.3 -61.6  3.2      89.2   106     3130   13 00 00
13 09 00  ---          23 20 35  48.6 -61.6  3.3      87.8   540     3200   13 00 01

13 10 00  CYG-A        23 21 35  48.4 -61.6  3.4      87.6    54     3200   13 10 00
13 16 00  ---          23 27 36  47.3 -61.5  3.5      86.7   360     3246   13 10 01

13 17 00  2013+370     23 28 36  49.9 -67.2  3.2      84.8    46     3246   13 17 00
13 20 00  ---          23 31 37  49.4 -67.1  3.3      84.4   180     3269   13 17 01

13 21 00  CYG-A        23 32 37  46.3 -61.4  3.5      85.9    46     3269   13 21 00
13 30 00  ---          23 41 38  44.6 -61.2  3.7      84.6   540     3339   13 21 01

13 31 00  2013+370     23 42 39  47.2 -66.7  3.4      83.0    47     3339   13 31 00
13 34 00  ---          23 45 39  46.6 -66.6  3.5      82.6   180     3362   13 31 01

13 35 00  CYG-A        23 46 39  43.7 -61.1  3.8      83.9    47     3362   13 35 00
13 44 00  ---          23 55 41  42.0 -60.8  3.9      82.6   540     3432   13 35 01

13 45 00  CYG-A        23 56 41  41.8 -60.8  3.9      82.5    54     3432   13 45 00
13 51 00  ---          00 02 42  40.7 -60.5  4.0      81.6   360     3478   13 45 01

13 52 00  2013+370     00 03 42  43.0 -65.9  3.8      80.4    47     3478   13 52 00
13 55 00  ---          00 06 43  42.4 -65.7  3.8      80.1   180     3501   13 52 01

13 56 00  CYG-A        00 07 43  39.7 -60.4  4.1      80.9    47     3501   13 56 00
14 05 00  ---          00 16 44  38.1 -60.0  4.3      79.7   540     3571   13 56 01

14 06 00  2013+370     00 17 44  40.3 -65.2  4.0      78.8    47     3571   14 06 00
14 09 00  ---          00 20 45  39.7 -65.0  4.1      78.4   180     3594   14 06 01

14 10 00  CYG-A        00 21 45  37.1 -59.8  4.4      79.0    47     3594   14 10 00
14 19 00  ---          00 30 47  35.5 -59.3  4.5      77.8   540     3664   14 10 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

14 20 00  CYG-A        00 31 47  35.3 -59.3  4.5      77.6    54     3664   14 20 00
14 26 00  ---          00 37 48  34.2 -59.0  4.6      76.8   360     3710   14 20 01

14 28 00  BLLAC        00 39 48  56.8 -58.4  2.6      97.7    67     3710   14 28 00
14 30 00  ---          00 41 48  56.4 -58.4  2.6      97.3   120     3725   14 28 01

14 31 00  BLLAC        00 42 48  56.2 -58.5  2.7      97.1    54     3725   14 31 00
14 33 00  ---          00 44 49  55.9 -58.6  2.7      96.6   120     3741   14 31 01

14 39 00  2013+370     00 50 50  33.9 -63.3  4.6      74.9   311     3741   14 39 00
14 42 00  ---          00 53 50  33.3 -63.1  4.6      74.5   180     3764   14 39 01

14 43 00  CYG-A        00 54 50  31.0 -58.0  4.9      74.5    48     3764   14 43 00
14 52 00  ---          01 03 52  29.4 -57.5  5.1      73.4   540     3834   14 43 01

14 53 00  2013+370     01 04 52  31.2 -62.4  4.8      73.2    48     3834   14 53 00
14 56 00  ---          01 07 53  30.6 -62.2  4.9      72.9   180     3857   14 53 01

14 57 00  CYG-A        01 08 53  28.5 -57.2  5.1      72.7    48     3857   14 57 00
15 06 00  ---          01 17 54  26.9 -56.6  5.3      71.5   540     3926   14 57 01

15 07 00  2013+370     01 18 54  28.5 -61.4  5.0      71.6    48     3926   15 07 00
15 10 00  ---          01 21 55  27.9 -61.2  5.1      71.3   180     3950   15 07 01

15 11 00  CYG-A        01 22 55  26.0 -56.2  5.4      70.8    48     3950   15 11 00
15 20 00  ---          01 31 57  24.4 -55.6  5.5      69.6   540     4019   15 11 01

15 21 00  CYG-A        01 32 57  24.2 -55.5  5.5      69.5    54     4019   15 21 00
15 27 00  ---          01 38 58  23.1 -55.1  5.6      68.7   360     4066   15 21 01

15 28 00  2013+370     01 39 58  24.6 -59.8  5.4      69.1    49     4066   15 28 00
15 31 00  ---          01 42 58  24.0 -59.6  5.4      68.8   180     4089   15 28 01

15 32 00  CYG-A        01 43 59  22.2 -54.7  5.7      68.0    49     4089   15 32 00
15 41 00  ---          01 53 00  20.7 -54.0  5.9      66.8   540     4158   15 32 01

15 42 00  2013+370     01 54 00  22.0 -58.7  5.6      67.4    49     4158   15 42 00
15 45 00  ---          01 57 01  21.4 -58.5  5.7      67.1   180     4181   15 42 01

15 46 00  CYG-A        01 58 01  19.8 -53.6  6.0      66.1    49     4181   15 46 00
15 55 00  ---          02 07 02  18.2 -52.8  6.1      64.9   540     4251   15 46 01

15 56 00  CYG-A        02 08 02  18.1 -52.8  6.1      64.7    54     4251   15 56 00
16 02 00  ---          02 14 03  17.0 -52.2  6.2      63.9   360     4297   15 56 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Jun 2014   Day 159 ---

16 03 00  2013+370     02 15 04  18.1 -56.9  6.0      64.9    49     4297   16 03 00
16 06 00  ---          02 18 04  17.6 -56.6  6.0      64.5   180     4321   16 03 01

16 07 00  CYG-A        02 19 04  16.2 -51.8  6.3      63.2    49     4321   16 07 00
16 16 00  ---          02 28 06  14.7 -51.0  6.5      62.0   540     4390   16 07 01

16 18 00  BLLAC        02 30 06  36.5 -57.6  4.4      79.4    69     4390   16 18 00
16 20 00  ---          02 32 06  36.1 -57.5  4.5      79.2   120     4406   16 18 01

16 22 00  2013+370     02 34 07  14.7 -55.2  6.3      62.5    70     4406   16 22 00
16 25 00  ---          02 37 07  14.2 -54.9  6.4      62.1   180     4429   16 22 01

16 26 00  CYG-A        02 38 07  13.0 -50.0  6.6      60.6    49     4429   16 26 00
16 35 00  ---          02 47 09  11.5 -49.2  6.8      59.3   540     4498   16 26 01

16 36 00  2013+370     02 48 09  12.3 -53.8  6.5      60.7    49     4498   16 36 00
16 39 00  ---          02 51 10  11.8 -53.5  6.6      60.3   180     4522   16 36 01

16 40 00  CYG-A        02 52 10  10.7 -48.7  6.9      58.5    49     4522   16 40 00
16 49 00  ---          03 01 11   9.3 -47.7  7.0      57.2   540     4591   16 40 01

16 50 00  2013+370     03 02 11   9.9 -52.4  6.8      58.8    49     4591   16 50 00
16 53 00  ---          03 05 12   9.4 -52.0  6.8      58.4   180     4614   16 50 01

16 54 00  CYG-A        03 06 12   8.5 -47.2  7.1      56.5    49     4614   16 54 00
17 00 00  ---          03 12 13   7.5 -46.6  7.2      55.6   360     4661   16 54 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ./sess214.Q1024
   Matching groups in /aux/vlb056a/p459kri/sched-11.3/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:    7         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   9  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
   BBC fr=     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.25    754.25    786.25    786.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   9  10  11  12  13  14  15  16  17  18

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J1959+4044        19 57 44.453094   * 19 59 28.368821     20 00 00.195809     167.68
 * CYG-A             40 35 46.31273    * 40 44 02.04732      40 46 25.12046      120.15
   CYGNUS-A          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J1959+40          rfc_2012b Petrov, 2012, unpublished 3 observations
   1957+405
   1957+404

   J2015+3710        20 13 37.014489   * 20 15 28.729775     20 16 02.683977       0.16
 * 2013+370          37 01 44.45943    * 37 10 59.51531      37 13 39.55603        0.16
                     /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 282 observations

   J2202+4216        22 00 39.362504   * 22 02 43.291371     22 03 20.430294       0.14
 * BLLAC             42 02 08.59073    * 42 16 39.97987      42 20 44.72528        0.10
   2200+420          /aux/vlb056a/p459kri/sched-11.3/catalogs/sources.vlba
   J2202+42          rfc_2012b Petrov, 2012, unpublished 59418 observations
   VR422201



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  CYG-A      ./sess214.Q1024       1 2 3 4 5 8 9                     9.983   678.351
  2013+370   ./sess214.Q1024       1 2 3 4 5 8 9                     2.783   179.750
  BLLAC      ./sess214.Q1024       1 2 3 4 5 8 9                     0.483    31.313


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   CYG-A              104.6
   2013+370           105.0
   BLLAC               85.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

