  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Tracing the Evolution of Fast Jet-Driven Outflows
 Exp. Code:  GN002B  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Kristina Nyland

Address:  ASTRON, Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands
 

Phone:    0521-595-766
EMAIL:    nyland@astron.nl
Fax:
Phone during observation: 0521-595-766

Observing mode: 21cm spectral line

Notes:    Target: 3C236
          Phase calibrator: J1001+3424
          Bandpass Calibrators: J0927+3902=4C39.25 (J0958+3224 for Arecibo scans)
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

 Next scan frequencies:  1300.75  1300.75  1316.75  1316.75  1332.75  1332.75  1348.75  1348.75
 Next BBC frequencies:    799.25   799.25   783.25   783.25   767.25   767.25   751.25   751.25
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

17 30 00  3C236        04 01 03  15.8  58.5 -6.1     -63.4     0        0   17 30 00
17 33 40  ---          04 04 44  16.5  58.9 -6.0     -63.8   220       14   17 30 01

17 34 40  J1001+3424   04 05 44  17.4  59.9 -5.9     -64.4    51       14   17 34 40
17 35 40  =0958+346    04 06 44  17.6  60.0 -5.9     -64.5    60       18   17 34 41

17 35 40  3C236        04 06 44  16.9  59.1 -6.0     -64.1    -9       18   17 35 49
17 39 20  ---          04 10 25  17.6  59.4 -5.9     -64.5   211       32   17 35 41

17 39 20  J1001+3424   04 10 25  18.3  60.3 -5.9     -64.9    -9       32   17 39 29
17 41 20  =0958+346    04 12 25  18.6  60.5 -5.8     -65.1   111       39   17 39 21

17 41 20  3C236        04 12 25  17.9  59.6 -5.9     -64.7    -9       39   17 41 29
17 45 00  ---          04 16 06  18.6  59.9 -5.8     -65.1   211       52   17 41 21

17 46 00  J1001+3424   04 17 06  19.5  60.9 -5.7     -65.6    51       52   17 46 00
17 47 00  =0958+346    04 18 06  19.7  61.0 -5.7     -65.7    60       56   17 46 01

17 47 00  3C236        04 18 06  19.0  60.1 -5.8     -65.4    -9       56   17 47 09
17 50 40  ---          04 21 47  19.7  60.5 -5.8     -65.8   211       70   17 47 01

17 50 40  J1001+3424   04 21 47  20.4  61.4 -5.7     -66.1    -9       70   17 50 49
17 52 40  =0958+346    04 23 47  20.8  61.5 -5.6     -66.4   111       77   17 50 41

17 52 40  3C236        04 23 47  20.1  60.6 -5.7     -66.0    -9       77   17 52 49
17 56 20  ---          04 27 28  20.7  61.0 -5.7     -66.4   211       91   17 52 41

17 57 20  J1001+3424   04 28 28  21.7  61.9 -5.6     -66.9    51       91   17 57 20
17 58 20  =0958+346    04 29 28  21.8  62.0 -5.5     -67.0    60       94   17 57 21

17 58 20  3C236        04 29 28  21.1  61.1 -5.6     -66.6    -9       94   17 58 29
18 02 00  ---          04 33 09  21.8  61.5 -5.6     -67.0   211      108   17 58 21

18 02 00  J1001+3424   04 33 09  22.5  62.4 -5.5     -67.4    -9      108   18 02 09
18 04 00  =0958+346    04 35 09  22.9  62.5 -5.4     -67.6   111      115   18 02 01

18 04 00  3C236        04 35 09  22.2  61.6 -5.5     -67.3    -9      115   18 04 09
18 07 40  ---          04 38 50  22.9  61.9 -5.5     -67.7   211      129   18 04 01

18 08 40  J1001+3424   04 39 50  23.8  62.9 -5.4     -68.1    51      129   18 08 40
18 09 40  =0958+346    04 40 50  24.0  63.0 -5.4     -68.2    60      133   18 08 41
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

18 09 40  3C236        04 40 50  23.3  62.1 -5.4     -67.9    -9      133   18 09 49
18 13 20  ---          04 44 31  24.0  62.4 -5.4     -68.3   211      146   18 09 41

18 13 20  J1001+3424   04 44 31  24.7  63.3 -5.3     -68.6    -9      146   18 13 29
18 15 20  =0958+346    04 46 31  25.1  63.5 -5.3     -68.8   111      153   18 13 21

18 15 20  3C236        04 46 31  24.4  62.6 -5.3     -68.5    -9      153   18 15 29
18 18 50  ---          04 50 01  25.0  62.9 -5.3     -68.9   201      166   18 15 21

18 19 50  J1001+3424   04 51 02  26.0  63.8 -5.2     -69.3    50      166   18 19 50
18 20 50  =0958+346    04 52 02  26.2  63.9 -5.2     -69.4    60      170   18 19 51

18 21 50  J0927+3902   04 53 02  34.3  61.2 -4.6     -76.0    36      170   18 21 50
18 26 50  =0923+392    04 58 03  35.2  61.5 -4.5     -76.6   300      189   18 21 51

18 26 50  J1001+3424   04 58 03  27.3  64.4 -5.1     -70.0   -23      189   18 27 13
18 29 50  =0958+346    05 01 03  27.9  64.6 -5.0     -70.3   157      200   18 26 51

18 29 50  3C236        05 01 03  27.1  63.8 -5.1     -70.1    -9      200   18 29 59
18 33 20  ---          05 04 34  27.8  64.0 -5.0     -70.4   201      213   18 29 51

18 34 20  J1001+3424   05 05 34  28.8  65.0 -4.9     -70.8    50      213   18 34 20
18 35 20  =0958+346    05 06 34  29.0  65.1 -4.9     -70.9    60      216   18 34 21

18 35 20  3C236        05 06 34  28.2  64.2 -5.0     -70.7   -10      216   18 35 30
18 38 50  ---          05 10 05  28.9  64.5 -4.9     -71.0   200      229   18 35 21

18 38 50  J1001+3424   05 10 05  29.7  65.3 -4.9     -71.3   -10      229   18 39 00
18 40 50  =0958+346    05 12 05  30.1  65.5 -4.8     -71.5   110      236   18 38 51

18 40 50  3C236        05 12 05  29.3  64.6 -4.9     -71.2   -10      236   18 41 00
18 44 20  ---          05 15 36  30.0  64.9 -4.9     -71.6   200      249   18 40 51

18 45 20  J1001+3424   05 16 36  31.0  65.8 -4.8     -71.9    50      249   18 45 20
18 46 20  =0958+346    05 17 36  31.2  65.9 -4.7     -72.1    60      253   18 45 21

18 46 20  3C236        05 17 36  30.4  65.0 -4.8     -71.8   -10      253   18 46 30
18 49 50  ---          05 21 07  31.0  65.3 -4.8     -72.2   200      266   18 46 21

18 49 50  J1001+3424   05 21 07  31.8  66.2 -4.7     -72.4   -10      266   18 50 00
18 51 50  =0958+346    05 23 07  32.2  66.3 -4.6     -72.6   110      273   18 49 51

18 51 50  3C236        05 23 07  31.4  65.4 -4.7     -72.4   -10      273   18 52 00
18 55 20  ---          05 26 37  32.1  65.7 -4.7     -72.8   200      286   18 51 51
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

18 56 20  J1001+3424   05 27 38  33.1  66.6 -4.6     -73.1    50      286   18 56 20
18 57 20  =0958+346    05 28 38  33.3  66.7 -4.6     -73.2    60      290   18 56 21

18 57 20  3C236        05 28 38  32.5  65.8 -4.6     -73.0   -10      290   18 57 30
19 00 50  ---          05 32 08  33.2  66.1 -4.6     -73.3   200      303   18 57 21

19 00 50  J1001+3424   05 32 08  34.0  67.0 -4.5     -73.5   -10      303   19 01 00
19 02 50  =0958+346    05 34 09  34.4  67.1 -4.5     -73.7   110      310   19 00 51

19 02 50  3C236        05 34 09  33.6  66.2 -4.5     -73.6   -10      310   19 03 00
19 06 20  ---          05 37 39  34.3  66.4 -4.5     -73.9   200      323   19 02 51

19 07 20  J1001+3424   05 38 39  35.3  67.4 -4.4     -74.2    50      323   19 07 20
19 08 20  =0958+346    05 39 40  35.5  67.5 -4.4     -74.3    60      327   19 07 21

19 08 20  3C236        05 39 40  34.7  66.6 -4.5     -74.1   -10      327   19 08 30
19 11 50  ---          05 43 10  35.4  66.8 -4.4     -74.5   200      339   19 08 21

19 11 50  J1001+3424   05 43 10  36.2  67.7 -4.3     -74.7   -10      339   19 12 00
19 13 50  =0958+346    05 45 10  36.6  67.9 -4.3     -74.9   110      347   19 11 51

19 13 50  3C236        05 45 10  35.8  67.0 -4.4     -74.7   -10      347   19 14 00
19 17 20  ---          05 48 41  36.5  67.2 -4.3     -75.1   200      359   19 13 51

19 18 20  J1001+3424   05 49 41  37.5  68.2 -4.2     -75.3    50      359   19 18 20
19 19 20  =0958+346    05 50 41  37.7  68.2 -4.2     -75.4    60      363   19 18 21

19 19 20  3C236        05 50 41  36.9  67.3 -4.3     -75.3   -10      363   19 19 30
19 22 50  ---          05 54 12  37.6  67.6 -4.2     -75.6   200      376   19 19 21

19 22 50  J1001+3424   05 54 12  38.4  68.5 -4.1     -75.8   -10      376   19 23 00
19 24 50  =0958+346    05 56 12  38.8  68.6 -4.1     -76.0   110      383   19 22 51

19 24 50  3C236        05 56 12  38.0  67.7 -4.2     -75.8   -10      383   19 25 00
19 28 20  ---          05 59 43  38.7  67.9 -4.1     -76.2   200      396   19 24 51

19 29 20  J1001+3424   06 00 43  39.7  68.9 -4.0     -76.4    50      396   19 29 20
19 30 20  =0958+346    06 01 43  39.9  68.9 -4.0     -76.5    60      400   19 29 21

19 31 20  J0927+3902   06 02 43  47.6  64.2 -3.4     -85.1    37      400   19 31 20
19 36 20  =0923+392    06 07 44  48.6  64.3 -3.3     -85.8   300      419   19 31 21

19 36 20  J1001+3424   06 07 44  41.1  69.3 -3.9     -77.1   -23      419   19 36 43
19 39 20  =0958+346    06 10 45  41.7  69.5 -3.9     -77.4   157      429   19 36 21
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

19 39 20  3C236        06 10 45  40.9  68.6 -3.9     -77.4   -10      429   19 39 30
19 43 00  ---          06 14 25  41.6  68.8 -3.9     -77.7   210      443   19 39 21

19 44 00  J1001+3424   06 15 25  42.7  69.8 -3.8     -77.9    50      443   19 44 00
19 45 00  =0958+346    06 16 26  42.9  69.8 -3.8     -78.0    60      447   19 44 01

19 45 00  3C236        06 16 26  42.0  68.9 -3.8     -77.9   -10      447   19 45 10
19 48 40  ---          06 20 06  42.7  69.1 -3.8     -78.3   210      460   19 45 01

19 48 40  J1001+3424   06 20 06  43.6  70.0 -3.7     -78.4   -10      460   19 48 50
19 50 40  =0958+346    06 22 06  44.0  70.2 -3.7     -78.6   110      467   19 48 41

19 50 40  3C236        06 22 06  43.1  69.2 -3.7     -78.5   -10      467   19 50 50
19 54 20  ---          06 25 47  43.9  69.4 -3.7     -78.9   210      481   19 50 41

19 55 20  J1001+3424   06 26 47  45.0  70.4 -3.6     -79.1    50      481   19 55 20
19 56 20  =0958+346    06 27 47  45.2  70.5 -3.6     -79.2    60      485   19 55 21

19 56 20  3C236        06 27 47  44.3  69.5 -3.7     -79.1   -10      485   19 56 30
20 00 00  ---          06 31 28  45.0  69.7 -3.6     -79.5   210      498   19 56 21

20 00 00  J1001+3424   06 31 28  45.9  70.7 -3.5     -79.5   -10      498   20 00 10
20 02 00  =0958+346    06 33 28  46.3  70.8 -3.5     -79.7   110      505   20 00 01

20 02 00  3C236        06 33 28  45.4  69.8 -3.6     -79.7   -10      505   20 02 10
20 05 40  ---          06 37 09  46.2  70.0 -3.5     -80.1   210      519   20 02 01

20 06 40  J1001+3424   06 38 09  47.3  71.0 -3.4     -80.2    50      519   20 06 40
20 07 40  =0958+346    06 39 09  47.5  71.1 -3.4     -80.3    60      523   20 06 41

20 07 40  3C236        06 39 09  46.6  70.1 -3.5     -80.3   -10      523   20 07 50
20 11 20  ---          06 42 50  47.3  70.3 -3.4     -80.7   210      536   20 07 41

20 11 20  J1001+3424   06 42 50  48.2  71.3 -3.3     -80.7   -10      536   20 11 30
20 13 20  =0958+346    06 44 50  48.6  71.4 -3.3     -80.9   110      543   20 11 21

20 13 20  3C236        06 44 50  47.7  70.4 -3.4     -80.9   -10      543   20 13 30
20 17 00  ---          06 48 31  48.5  70.6 -3.3     -81.3   210      557   20 13 21

20 18 00  J1001+3424   06 49 31  49.6  71.6 -3.2     -81.4    50      557   20 18 00
20 19 00  =0958+346    06 50 31  49.8  71.6 -3.2     -81.5    60      561   20 18 01

20 19 00  3C236        06 50 31  48.9  70.7 -3.3     -81.6   -10      561   20 19 10
20 22 40  ---          06 54 12  49.6  70.8 -3.2     -82.0   210      574   20 19 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

20 22 40  J1001+3424   06 54 12  50.6  71.8 -3.1     -81.9   -10      574   20 22 50
20 24 40  =0958+346    06 56 12  51.0  71.9 -3.1     -82.1   110      581   20 22 41

20 24 40  3C236        06 56 12  50.0  70.9 -3.2     -82.2   -10      581   20 24 50
20 28 00  ---          06 59 33  50.7  71.1 -3.1     -82.5   190      594   20 24 41

20 29 00  J1001+3424   07 00 33  51.9  72.1 -3.0     -82.6    50      594   20 29 00
20 30 00  =0958+346    07 01 33  52.1  72.1 -3.0     -82.7    60      598   20 29 01

20 30 00  J0958+3224   07 01 33  52.4  75.5 -3.0     -80.4   -10      598   20 30 10
20 37 00  =0955+326    07 08 34  53.8  75.9 -2.8     -81.0   410      624   20 30 01

20 38 00  J1001+3424   07 09 34  53.7  72.5 -2.9     -83.5    50      624   20 38 00
20 40 30  =0958+346    07 12 05  54.2  72.6 -2.8     -83.8   150      634   20 38 01

20 40 30  3C236        07 12 05  53.3  71.6 -2.9     -83.9   -10      634   20 40 40
20 43 50  ---          07 15 25  54.0  71.7 -2.9     -84.3   190      646   20 40 31

20 44 50  J1001+3424   07 16 25  55.1  72.7 -2.8     -84.3    50      646   20 44 50
20 45 50  =0958+346    07 17 26  55.3  72.8 -2.7     -84.4    60      650   20 44 51

20 45 50  3C236        07 17 26  54.4  71.8 -2.8     -84.6   -10      650   20 46 00
20 49 10  ---          07 20 46  55.1  71.9 -2.8     -84.9   190      662   20 45 51

20 49 10  J1001+3424   07 20 46  56.0  72.9 -2.7     -84.8   -10      662   20 49 20
20 51 10  =0958+346    07 22 46  56.4  72.9 -2.7     -85.0   110      669   20 49 11

20 51 10  3C236        07 22 46  55.5  71.9 -2.7     -85.2   -10      669   20 51 20
20 54 30  ---          07 26 07  56.1  72.0 -2.7     -85.6   190      681   20 51 11

20 55 30  J1001+3424   07 27 07  57.3  73.1 -2.6     -85.5    50      681   20 55 30
20 56 30  =0958+346    07 28 07  57.5  73.1 -2.6     -85.6    60      685   20 55 31

20 56 30  3C236        07 28 07  56.6  72.1 -2.6     -85.8   -10      685   20 56 40
20 59 50  ---          07 31 28  57.2  72.2 -2.6     -86.2   190      697   20 56 31

20 59 50  J1001+3424   07 31 28  58.2  73.2 -2.5     -86.0   -10      697   21 00 00
21 01 50  =0958+346    07 33 28  58.6  73.3 -2.5     -86.3   110      704   20 59 51

21 01 50  3C236        07 33 28  57.7  72.2 -2.6     -86.5   -10      704   21 02 00
21 05 10  ---          07 36 49  58.3  72.3 -2.5     -86.9   190      717   21 01 51

21 06 10  J1001+3424   07 37 49  59.5  73.4 -2.4     -86.8    50      717   21 06 10
21 07 10  =0958+346    07 38 49  59.7  73.4 -2.4     -86.9    60      721   21 06 11
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

21 07 10  3C236        07 38 49  58.7  72.3 -2.5     -87.1   -10      721   21 07 20
21 10 30  ---          07 42 10  59.4  72.4 -2.4     -87.6   190      733   21 07 11

21 10 30  J1001+3424   07 42 10  60.4  73.5 -2.3     -87.3   -10      733   21 10 40
21 12 30  =0958+346    07 44 10  60.8  73.5 -2.3     -87.6   110      740   21 10 31

21 12 30  3C236        07 44 10  59.8  72.4 -2.4     -87.8   -10      740   21 12 40
21 15 50  ---          07 47 30  60.5  72.5 -2.3     -88.3   190      752   21 12 31

21 16 50  J1001+3424   07 48 31  61.7  73.6 -2.2     -88.1    50      752   21 16 50
21 17 50  =0958+346    07 49 31  61.9  73.6 -2.2     -88.3    60      756   21 16 51

21 17 50  3C236        07 49 31  60.9  72.5 -2.3     -88.5   -10      756   21 18 00
21 21 10  ---          07 52 51  61.6  72.5 -2.2     -89.0   190      768   21 17 51

21 21 10  J1001+3424   07 52 51  62.6  73.6 -2.2     -88.7   -10      768   21 21 20
21 23 10  =0958+346    07 54 52  63.0  73.6 -2.1     -89.0   110      775   21 21 11

21 23 10  3C236        07 54 52  62.0  72.5 -2.2     -89.2   -10      775   21 23 20
21 26 30  ---          07 58 12  62.7  72.6 -2.1     -89.7   190      788   21 23 11

21 27 30  J1001+3424   07 59 12  63.9  73.7 -2.0     -89.5    50      788   21 27 30
21 28 30  =0958+346    08 00 13  64.1  73.7 -2.0     -89.7    60      791   21 27 31

21 28 30  3C236        08 00 13  63.1  72.6 -2.1     -90.0   -10      791   21 28 40
21 31 50  ---          08 03 33  63.8  72.6 -2.1     -90.5   190      804   21 28 31

21 31 50  J1001+3424   08 03 33  64.8  73.7 -2.0     -90.2   -10      804   21 32 00
21 33 50  =0958+346    08 05 33  65.2  73.7 -1.9     -90.4   110      811   21 31 51

21 33 50  3C236        08 05 33  64.2  72.5 -2.0     -90.8   -10      811   21 34 00
21 37 10  ---          08 08 54  64.9  72.5 -2.0     -91.3   190      823   21 33 51

21 38 10  J1001+3424   08 09 54  66.1  73.6 -1.9     -91.1    50      823   21 38 10
21 39 10  =0958+346    08 10 54  66.3  73.6 -1.9     -91.2    60      827   21 38 11

21 39 10  3C236        08 10 54  65.3  72.5 -1.9     -91.6   -10      827   21 39 20
21 42 30  ---          08 14 15  66.0  72.4 -1.9     -92.1   190      839   21 39 11

21 42 30  J1001+3424   08 14 15  67.0  73.6 -1.8     -91.7   -10      839   21 42 40
21 44 30  =0958+346    08 16 15  67.4  73.5 -1.8     -92.1   110      846   21 42 31

21 44 30  3C236        08 16 15  66.4  72.4 -1.8     -92.4   -10      846   21 44 40
21 47 50  ---          08 19 36  67.1  72.3 -1.8     -93.0   190      858   21 44 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

21 48 50  J1001+3424   08 20 36  68.3  73.4 -1.7     -92.8    50      858   21 48 50
21 50 00  =0958+346    08 21 46  68.6  73.4 -1.7     -93.0    70      863   21 48 51

21 51 00  J0958+3224   08 22 46  69.4  79.0 -1.6     -88.3    48      863   21 51 00
21 58 00  =0955+326    08 29 47  70.9  79.1 -1.5     -89.1   420      890   21 51 01

21 58 00  J1001+3424   08 29 47  70.2  73.1 -1.5     -94.4   -12      890   21 58 12
22 00 00  =0958+346    08 31 48  70.6  73.0 -1.5     -94.7   108      897   21 58 01

22 00 00  3C236        08 31 48  69.6  71.8 -1.6     -95.2   -10      897   22 00 10
22 03 30  ---          08 35 18  70.3  71.6 -1.5     -95.9   200      910   22 00 01

22 04 30  J1001+3424   08 36 18  71.6  72.7 -1.4     -95.6    50      910   22 04 30
22 05 30  =0958+346    08 37 19  71.8  72.7 -1.4     -95.8    60      914   22 04 31

22 05 30  3C236        08 37 19  70.7  71.5 -1.5     -96.3   -10      914   22 05 40
22 09 00  ---          08 40 49  71.5  71.2 -1.4     -97.0   200      927   22 05 31

22 09 00  J1001+3424   08 40 49  72.5  72.4 -1.4     -96.6   -10      927   22 09 10
22 11 00  =0958+346    08 42 50  72.9  72.3 -1.3     -97.0   110      934   22 09 01

22 11 00  3C236        08 42 50  71.9  71.1 -1.4     -97.5   -10      934   22 11 10
22 14 30  ---          08 46 20  72.6  70.8 -1.3     -98.3   200      946   22 11 01

22 15 30  J1001+3424   08 47 20  73.8  71.8 -1.2     -98.1    50      946   22 15 30
22 16 30  =0958+346    08 48 20  74.0  71.7 -1.2     -98.3    60      950   22 15 31

22 16 30  3C236        08 48 20  73.0  70.5 -1.3     -98.8   -10      950   22 16 40
22 20 00  ---          08 51 51  73.7  70.1 -1.3     -99.6   200      963   22 16 31

22 20 00  J1001+3424   08 51 51  74.8  71.3 -1.2     -99.2   -10      963   22 20 10
22 22 00  =0958+346    08 53 51  75.2  71.1 -1.1     -99.7   110      970   22 20 01

22 22 00  3C236        08 53 51  74.1  69.9 -1.2    -100.2   -10      970   22 22 10
22 25 30  ---          08 57 22  74.8  69.4 -1.2    -101.1   200      983   22 22 01

22 26 30  J1001+3424   08 58 22  76.1  70.4 -1.1    -101.0    50      983   22 26 30
22 27 30  =0958+346    08 59 22  76.3  70.2 -1.0    -101.3    60      987   22 26 31

22 27 30  3C236        08 59 22  75.2  69.1 -1.1    -101.7   -10      987   22 27 40
22 31 00  ---          09 02 53  75.9  68.5 -1.1    -102.8   200     1000   22 27 31

22 31 00  J1001+3424   09 02 53  77.0  69.6 -1.0    -102.4   -10     1000   22 31 10
22 33 00  =0958+346    09 04 53  77.4  69.2 -1.0    -103.1   110     1007   22 31 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

22 33 00  3C236        09 04 53  76.3  68.1 -1.0    -103.5   -10     1007   22 33 10
22 36 30  ---          09 08 24  77.0  67.3 -1.0    -104.7   200     1020   22 33 01

22 37 30  J1001+3424   09 09 24  78.3  68.1 -0.9    -104.8    50     1020   22 37 30
22 38 30  =0958+346    09 10 24  78.5  67.8 -0.9    -105.2    60     1024   22 37 31

22 38 30  3C236        09 10 24  77.4  66.8 -0.9    -105.5   -10     1024   22 38 40
22 42 00  ---          09 13 55  78.1  65.9 -0.9    -106.9   200     1037   22 38 31

22 42 00  J1001+3424   09 13 55  79.2  66.8 -0.8    -106.7   -10     1037   22 42 10
22 44 00  =0958+346    09 15 55  79.6  66.1 -0.8    -107.7   110     1044   22 42 01

22 44 00  3C236        09 15 55  78.5  65.3 -0.9    -107.8   -10     1044   22 44 10
22 47 30  ---          09 19 26  79.2  64.1 -0.8    -109.5   200     1057   22 44 01

22 48 30  J1001+3424   09 20 26  80.5  64.4 -0.7    -110.0    50     1057   22 48 30
22 49 30  =0958+346    09 21 26  80.7  64.0 -0.7    -110.6    60     1061   22 48 31

22 49 30  3C236        09 21 26  79.6  63.3 -0.8    -110.5   -10     1061   22 49 40
22 53 00  ---          09 24 56  80.2  61.8 -0.7    -112.5   200     1073   22 49 31

22 53 00  J1001+3424   09 24 56  81.3  62.2 -0.6    -112.8   -10     1073   22 53 10
22 55 00  =0958+346    09 26 57  81.7  61.1 -0.6    -114.2   110     1080   22 53 01

22 55 00  3C236        09 26 57  80.6  60.8 -0.7    -113.7   -10     1080   22 55 10
22 58 30  ---          09 30 27  81.3  58.9 -0.6    -116.1   200     1093   22 55 01

22 59 30  J1001+3424   09 31 28  82.6  58.1 -0.5    -117.7    50     1093   22 59 30
23 00 30  =0958+346    09 32 28  82.7  57.4 -0.5    -118.6    60     1097   22 59 31

23 01 30  J0927+3902   09 33 28  81.6  -7.3  0.1     171.9     6     1097   23 01 30
23 06 30  =0923+392    09 38 29  81.4 -13.7  0.2     164.8   300     1117   23 01 31

23 06 30  J1001+3424   09 38 29  83.8  51.8 -0.4    -125.0   -54     1117   23 07 24
23 08 30  =0958+346    09 40 29  84.1  49.5 -0.4    -127.6    66     1121   23 06 31

23 08 30  3C236        09 40 29  83.0  51.2 -0.4    -125.2   -10     1121   23 08 40
23 12 00  ---          09 44 00  83.6  47.5 -0.4    -129.4   200     1134   23 08 31

23 13 00  J1001+3424   09 45 00  84.8  43.1 -0.3    -134.6    50     1134   23 13 00
23 14 00  =0958+346    09 46 00  85.0  41.4 -0.3    -136.4    60     1138   23 13 01

23 14 00  3C236        09 46 00  83.9  45.0 -0.3    -132.2   -10     1138   23 14 10
23 17 30  ---          09 49 30  84.4  40.0 -0.3    -137.7   200     1150   23 14 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  13 Jun 2015   Day 164 ---

23 17 30  J1001+3424   09 49 30  85.4  34.8 -0.2    -143.5   -12     1150   23 17 42
23 19 30  =0958+346    09 51 31  85.7  30.3 -0.2    -148.2   108     1157   23 17 31

23 19 30  3C236        09 51 31  84.7  36.7 -0.3    -141.3   -12     1157   23 19 42
23 23 00  ---          09 55 01  85.1  30.0 -0.2    -148.4   198     1170   23 19 31

23 24 00  J1001+3424   09 56 02  86.1  18.6 -0.1    -160.5    46     1170   23 24 00
23 25 00  =0958+346    09 57 02  86.1  15.7 -0.1    -163.6    60     1174   23 24 01

23 25 00  3C236        09 57 02  85.3  25.7 -0.2    -152.9   -15     1174   23 25 15
23 28 30  ---          10 00 32  85.6  17.3 -0.1    -161.8   195     1187   23 25 01

23 28 30  J1001+3424   10 00 32  86.3   5.0  0.0    -174.8   -17     1187   23 28 47
23 30 30  =0958+346    10 02 33  86.3  -1.4  0.0     178.5   103     1193   23 28 31

23 30 30  3C236        10 02 33  85.7  12.1 -0.1    -167.3   -17     1193   23 30 47
23 34 00  ---          10 06 03  85.8   2.4  0.0    -177.5   193     1206   23 30 31

23 35 00  J1001+3424   10 07 03  86.1 -15.4  0.1     163.9    41     1206   23 35 00
23 36 00  =0958+346    10 08 04  86.1 -18.4  0.1     160.8    60     1209   23 35 01

23 36 00  3C236        10 08 04  85.8  -3.2  0.0     176.7   -18     1209   23 36 18
23 39 30  ---          10 11 34  85.7 -12.8  0.1     166.6   192     1222   23 36 01

23 39 30  J1001+3424   10 11 34  85.8 -27.7  0.2     151.0   -19     1222   23 39 49
23 41 30  =0958+346    10 13 34  85.6 -32.4  0.2     146.1   101     1228   23 39 31

23 41 30  3C236        10 13 34  85.6 -18.0  0.1     161.1   -18     1228   23 41 48
23 45 00  ---          10 17 05  85.3 -26.3  0.2     152.3   192     1241   23 41 31

23 46 00  J1001+3424   10 18 05  85.0 -41.3  0.3     136.6    42     1241   23 46 00
23 47 00  =0958+346    10 19 05  84.8 -42.9  0.3     134.8    60     1245   23 46 01

23 47 00  3C236        10 19 05  85.1 -30.6  0.2     147.8   -16     1245   23 47 16
23 50 30  ---          10 22 36  84.7 -37.1  0.3     140.7   194     1257   23 47 01

23 50 30  J1001+3424   10 22 36  84.3 -48.1  0.3     129.2   -16     1257   23 50 46
23 52 30  =0958+346    10 24 36  84.0 -50.5  0.4     126.4   104     1264   23 50 31

23 52 30  3C236        10 24 36  84.4 -40.4  0.3     137.2   -15     1264   23 52 45
23 56 00  ---          10 28 07  83.9 -45.3  0.4     131.8   195     1276   23 52 31

23 57 00  J1001+3424   10 29 07  83.2 -55.2  0.5     121.2    46     1276   23 57 00
23 58 00  =0958+346    10 30 07  83.0 -56.1  0.5     120.2    60     1280   23 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Start: Sat  13 Jun 2015   Day 164 -- Stop: Sun  14 Jun 2015   Day 165 ---

23 58 00  3C236        10 30 07  83.6 -47.8  0.4     129.1   -14     1280   23 58 14
00 01 30  ---          10 33 38  83.0 -51.5  0.4     124.9   196     1293   23 58 01

00 01 30  J1001+3424   10 33 38  82.4 -58.8  0.5     117.0   -13     1293   00 01 43
00 03 30  =0958+346    10 35 38  82.0 -60.1  0.6     115.3   107     1300   00 01 31

00 03 30  3C236        10 35 38  82.7 -53.3  0.5     122.8   -13     1300   00 03 43
00 07 00  ---          10 39 09  82.0 -56.1  0.5     119.5   197     1312   00 03 31

00 08 00  J1001+3424   10 40 09  81.2 -62.7  0.6     112.2    48     1312   00 08 00
00 09 00  =0958+346    10 41 09  81.0 -63.2  0.7     111.5    60     1316   00 08 01

00 09 00  3C236        10 41 09  81.7 -57.5  0.6     117.9   -12     1316   00 09 12
00 12 30  ---          10 44 40  81.0 -59.7  0.6     115.2   198     1329   00 09 01

00 12 30  J1001+3424   10 44 40  80.3 -64.8  0.7     109.5   -12     1329   00 12 42
00 14 30  =0958+346    10 46 40  79.9 -65.5  0.7     108.4   108     1336   00 12 31

00 14 30  3C236        10 46 40  80.7 -60.7  0.7     113.9   -11     1336   00 14 41
00 18 00  ---          10 50 10  80.0 -62.4  0.7     111.7   199     1349   00 14 31

00 19 00  J1001+3424   10 51 11  79.0 -67.1  0.8     106.3    49     1349   00 19 00
00 20 00  =0958+346    10 52 11  78.8 -67.4  0.8     105.9    60     1353   00 19 01

00 20 00  3C236        10 52 11  79.6 -63.2  0.8     110.6   -11     1353   00 20 11
00 23 30  ---          10 55 41  78.9 -64.5  0.8     108.9   199     1365   00 20 01

00 23 30  J1001+3424   10 55 41  78.1 -68.3  0.9     104.5   -11     1365   00 23 41
00 25 30  =0958+346    10 57 42  77.7 -68.8  0.9     103.7   109     1373   00 23 31

00 25 30  3C236        10 57 42  78.5 -65.2  0.8     107.9   -10     1373   00 25 40
00 28 50  ---          11 01 02  77.9 -66.2  0.9     106.5   190     1385   00 25 31

00 29 50  J1001+3424   11 02 02  76.8 -69.7  1.0     102.2    50     1385   00 29 50
00 30 50  =0958+346    11 03 03  76.6 -69.9  1.0     101.9    60     1389   00 29 51

00 31 50  J0927+3902   11 04 03  68.7 -60.5  1.6     105.7    37     1389   00 31 50
00 36 50  =0923+392    11 09 04  67.7 -61.1  1.7     104.2   300     1408   00 31 51

00 36 50  J1001+3424   11 09 04  75.4 -70.9  1.1     100.1   -23     1408   00 37 13
00 38 50  =0958+346    11 11 04  75.0 -71.2  1.1      99.5    97     1414   00 36 51

00 38 50  3C236        11 11 04  75.9 -68.5  1.1     102.8   -10     1414   00 39 00
00 42 20  ---          11 14 34  75.2 -69.1  1.1     101.7   200     1427   00 38 51
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

00 43 20  J1001+3424   11 15 35  74.1 -71.7  1.2      98.4    50     1427   00 43 20
00 44 20  =0958+346    11 16 35  73.9 -71.8  1.2      98.1    60     1431   00 43 21

00 44 20  3C236        11 16 35  74.8 -69.4  1.2     101.1   -10     1431   00 44 30
00 47 40  ---          11 19 55  74.1 -69.9  1.2     100.2   190     1443   00 44 21

00 47 40  J1001+3424   11 19 55  73.2 -72.1  1.3      97.3   -10     1443   00 47 50
00 49 40  =0958+346    11 21 56  72.8 -72.3  1.3      96.9   110     1450   00 47 41

00 49 40  3C236        11 21 56  73.7 -70.1  1.3      99.7   -10     1450   00 49 50
00 53 10  ---          11 25 26  73.0 -70.5  1.3      98.8   200     1463   00 49 41

00 54 10  J1001+3424   11 26 26  71.9 -72.7  1.4      95.9    50     1463   00 54 10
00 55 10  =0958+346    11 27 27  71.7 -72.7  1.4      95.7    60     1467   00 54 11

00 55 10  3C236        11 27 27  72.6 -70.7  1.3      98.3   -10     1467   00 55 20
00 58 30  ---          11 30 47  71.9 -71.1  1.4      97.5   190     1479   00 55 11

00 58 30  J1001+3424   11 30 47  71.0 -72.9  1.5      95.1   -10     1479   00 58 40
01 00 30  =0958+346    11 32 47  70.6 -73.0  1.5      94.7   110     1486   00 58 31

01 00 30  3C236        11 32 47  71.5 -71.2  1.4      97.1   -10     1486   01 00 40
01 04 00  ---          11 36 18  70.8 -71.5  1.5      96.3   200     1499   01 00 31

01 05 00  J1001+3424   11 37 18  69.6 -73.2  1.6      93.8    50     1499   01 05 00
01 06 00  =0958+346    11 38 18  69.4 -73.3  1.6      93.7    60     1503   01 05 01

01 06 00  3C236        11 38 18  70.4 -71.6  1.5      95.9   -10     1503   01 06 10
01 09 20  ---          11 41 39  69.7 -71.8  1.6      95.2   190     1515   01 06 01

01 09 20  J1001+3424   11 41 39  68.7 -73.4  1.7      93.1   -10     1515   01 09 30
01 11 20  =0958+346    11 43 39  68.3 -73.4  1.7      92.8   110     1522   01 09 21

01 11 20  3C236        11 43 39  69.3 -71.9  1.6      94.9   -10     1522   01 11 30
01 14 50  ---          11 47 10  68.6 -72.1  1.7      94.2   200     1535   01 11 21

01 15 50  J1001+3424   11 48 10  67.4 -73.5  1.8      92.0    50     1535   01 15 50
01 16 50  =0958+346    11 49 10  67.2 -73.6  1.8      91.9    60     1539   01 15 51

01 16 50  3C236        11 49 10  68.2 -72.1  1.7      93.9   -10     1539   01 17 00
01 20 10  ---          11 52 31  67.5 -72.3  1.8      93.3   190     1551   01 16 51

01 20 10  J1001+3424   11 52 31  66.5 -73.6  1.8      91.3   -10     1551   01 20 20
01 22 10  =0958+346    11 54 31  66.1 -73.6  1.9      91.0   110     1558   01 20 11
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

01 22 10  3C236        11 54 31  67.1 -72.3  1.8      92.9   -10     1558   01 22 20
01 25 40  ---          11 58 02  66.3 -72.4  1.9      92.4   200     1571   01 22 11

01 26 40  J1001+3424   11 59 02  65.2 -73.7  1.9      90.4    50     1571   01 26 40
01 27 40  =0958+346    12 00 02  64.9 -73.7  2.0      90.2    60     1575   01 26 41

01 27 40  3C236        12 00 02  65.9 -72.4  1.9      92.0   -10     1575   01 27 50
01 31 00  ---          12 03 22  65.2 -72.5  1.9      91.5   190     1587   01 27 41

01 31 00  J1001+3424   12 03 22  64.3 -73.7  2.0      89.8   -10     1587   01 31 10
01 33 00  =0958+346    12 05 23  63.8 -73.7  2.1      89.5   110     1595   01 31 01

01 33 00  3C236        12 05 23  64.8 -72.5  2.0      91.2   -10     1595   01 33 10
01 36 30  ---          12 08 53  64.1 -72.5  2.0      90.7   200     1607   01 33 01

01 37 30  J1001+3424   12 09 53  62.9 -73.6  2.1      88.9    50     1607   01 37 30
01 38 30  =0958+346    12 10 54  62.7 -73.6  2.1      88.7    60     1611   01 37 31

01 38 30  3C236        12 10 54  63.7 -72.6  2.1      90.4   -10     1611   01 38 40
01 41 50  ---          12 14 14  63.0 -72.6  2.1      89.9   190     1624   01 38 31

01 41 50  J1001+3424   12 14 14  62.0 -73.6  2.2      88.3   -10     1624   01 42 00
01 43 50  =0958+346    12 16 15  61.6 -73.6  2.2      88.1   110     1631   01 41 51

01 43 50  3C236        12 16 15  62.6 -72.6  2.2      89.6   -10     1631   01 44 00
01 47 20  ---          12 19 45  61.9 -72.5  2.2      89.1   200     1643   01 43 51

01 48 20  J1001+3424   12 20 45  60.7 -73.5  2.3      87.5    50     1643   01 48 20
01 49 20  =0958+346    12 21 45  60.5 -73.5  2.3      87.4    60     1647   01 48 21

01 49 20  3C236        12 21 45  61.5 -72.5  2.2      88.9   -10     1647   01 49 30
01 52 40  ---          12 25 06  60.8 -72.5  2.3      88.4   190     1660   01 49 21

01 52 40  J1001+3424   12 25 06  59.8 -73.4  2.4      86.9   -10     1660   01 52 50
01 54 40  =0958+346    12 27 06  59.4 -73.3  2.4      86.7   110     1667   01 52 41

01 54 40  3C236        12 27 06  60.4 -72.5  2.3      88.1   -10     1667   01 54 50
01 58 00  ---          12 30 27  59.7 -72.4  2.4      87.7   190     1679   01 54 41

01 59 00  J1001+3424   12 31 27  58.5 -73.2  2.5      86.2    50     1679   01 59 00
02 00 00  =0958+346    12 32 27  58.3 -73.2  2.5      86.1    60     1683   01 59 01

02 01 00  J0927+3902   12 33 27  51.5 -64.5  3.1      87.9    39     1683   02 01 00
02 06 00  =0923+392    12 38 28  50.5 -64.5  3.2      87.2   300     1702   02 01 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

02 06 00  J1001+3424   12 38 28  57.0 -73.0  2.6      85.4   -21     1702   02 06 21
02 08 00  =0958+346    12 40 28  56.6 -73.0  2.6      85.1    99     1708   02 06 01

02 08 00  3C236        12 40 28  57.6 -72.2  2.6      86.5   -10     1708   02 08 10
02 11 30  ---          12 43 59  56.9 -72.1  2.6      86.0   200     1721   02 08 01

02 12 30  J1001+3424   12 44 59  55.7 -72.8  2.7      84.6    50     1721   02 12 30
02 13 30  =0958+346    12 45 59  55.5 -72.8  2.7      84.5    60     1725   02 12 31

02 13 30  3C236        12 45 59  56.5 -72.1  2.7      85.8   -10     1725   02 13 40
02 17 00  ---          12 49 30  55.8 -72.0  2.7      85.4   200     1738   02 13 31

02 17 00  J1001+3424   12 49 30  54.8 -72.7  2.8      84.1   -10     1738   02 17 10
02 19 00  =0958+346    12 51 30  54.3 -72.6  2.8      83.9   110     1745   02 17 01

02 19 00  3C236        12 51 30  55.4 -71.9  2.7      85.1   -10     1745   02 19 10
02 22 30  ---          12 55 01  54.7 -71.8  2.8      84.7   200     1758   02 19 01

02 23 30  J1001+3424   12 56 01  53.4 -72.4  2.9      83.4    50     1758   02 23 30
02 24 30  =0958+346    12 57 01  53.2 -72.4  2.9      83.3    60     1762   02 23 31

02 24 30  3C236        12 57 01  54.2 -71.7  2.8      84.5   -10     1762   02 24 40
02 28 00  ---          13 00 32  53.5 -71.6  2.9      84.1   200     1775   02 24 31

02 28 00  J1001+3424   13 00 32  52.5 -72.2  3.0      82.9   -10     1775   02 28 10
02 30 00  =0958+346    13 02 32  52.1 -72.1  3.0      82.7   110     1782   02 28 01

02 30 00  3C236        13 02 32  53.1 -71.5  2.9      83.9   -10     1782   02 30 10
02 33 30  ---          13 06 03  52.4 -71.4  3.0      83.5   200     1795   02 30 01

02 34 30  J1001+3424   13 07 03  51.2 -71.9  3.1      82.2    50     1795   02 34 30
02 35 30  =0958+346    13 08 03  50.9 -71.9  3.1      82.1    60     1799   02 34 31

02 35 30  3C236        13 08 03  52.0 -71.3  3.0      83.2   -10     1799   02 35 40
02 39 00  ---          13 11 34  51.3 -71.2  3.1      82.8   200     1812   02 35 31

02 39 00  J1001+3424   13 11 34  50.2 -71.7  3.2      81.7   -10     1812   02 39 10
02 41 00  =0958+346    13 13 34  49.8 -71.6  3.2      81.5   110     1819   02 39 01

02 41 00  3C236        13 13 34  50.9 -71.1  3.1      82.6   -10     1819   02 41 10
02 44 30  ---          13 17 04  50.2 -71.0  3.2      82.2   200     1831   02 41 01

02 45 30  J1001+3424   13 18 05  48.9 -71.4  3.3      81.0    50     1831   02 45 30
02 46 30  =0958+346    13 19 05  48.7 -71.4  3.3      80.9    60     1835   02 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

02 46 30  3C236        13 19 05  49.8 -70.9  3.2      82.0   -10     1835   02 46 40
02 50 00  ---          13 22 35  49.0 -70.7  3.3      81.6   200     1848   02 46 31

02 50 00  J1001+3424   13 22 35  48.0 -71.2  3.3      80.6   -10     1848   02 50 10
02 52 00  =0958+346    13 24 36  47.6 -71.1  3.4      80.4   110     1855   02 50 01

02 52 00  3C236        13 24 36  48.6 -70.6  3.3      81.4   -10     1855   02 52 10
02 55 30  ---          13 28 06  47.9 -70.5  3.4      81.0   200     1868   02 52 01

02 56 30  J1001+3424   13 29 06  46.7 -70.9  3.5      79.9    50     1868   02 56 30
02 57 30  =0958+346    13 30 07  46.5 -70.8  3.5      79.8    60     1872   02 56 31

02 57 30  3C236        13 30 07  47.5 -70.4  3.4      80.8   -10     1872   02 57 40
03 01 00  ---          13 33 37  46.8 -70.2  3.4      80.5   200     1885   02 57 31

03 01 00  J1001+3424   13 33 37  45.7 -70.6  3.5      79.4   -10     1885   03 01 10
03 03 00  =0958+346    13 35 38  45.3 -70.5  3.6      79.2   110     1892   03 01 01

03 03 00  3C236        13 35 38  46.4 -70.1  3.5      80.2   -10     1892   03 03 10
03 06 30  ---          13 39 08  45.7 -69.9  3.5      79.9   200     1905   03 03 01

03 07 30  J1001+3424   13 40 08  44.4 -70.3  3.6      78.8    50     1905   03 07 30
03 08 30  =0958+346    13 41 08  44.2 -70.2  3.7      78.7    60     1909   03 07 31

03 08 30  3C236        13 41 08  45.3 -69.8  3.6      79.7   -10     1909   03 08 40
03 12 00  ---          13 44 39  44.6 -69.6  3.6      79.3   200     1922   03 08 31

03 12 00  J1001+3424   13 44 39  43.5 -70.0  3.7      78.3   -10     1922   03 12 10
03 14 00  =0958+346    13 46 39  43.1 -69.9  3.7      78.1   110     1929   03 12 01

03 14 00  3C236        13 46 39  44.2 -69.5  3.7      79.1   -10     1929   03 14 10
03 17 30  ---          13 50 10  43.5 -69.3  3.7      78.7   200     1942   03 14 01

03 18 30  J1001+3424   13 51 10  42.2 -69.6  3.8      77.7    50     1942   03 18 30
03 19 30  =0958+346    13 52 10  42.0 -69.6  3.8      77.6    60     1945   03 18 31

03 19 30  3C236        13 52 10  43.1 -69.2  3.8      78.5   -10     1945   03 19 40
03 23 00  ---          13 55 41  42.4 -69.0  3.8      78.1   200     1958   03 19 31

03 23 00  J1001+3424   13 55 41  41.3 -69.4  3.9      77.2   -10     1958   03 23 10
03 25 00  =0958+346    13 57 41  40.9 -69.2  3.9      77.0   110     1965   03 23 01

03 26 00  J0927+3902   13 58 41  35.1 -61.5  4.5      76.5    41     1965   03 26 00
03 31 20  =0923+392    14 04 02  34.1 -61.2  4.6      75.9   320     1986   03 26 01
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

03 31 20  J1001+3424   14 04 02  39.6 -68.8  4.0      76.4   -19     1986   03 31 39
03 33 20  =0958+346    14 06 03  39.2 -68.7  4.1      76.2   101     1993   03 31 21

03 33 20  3C236        14 06 03  40.3 -68.4  4.0      77.1   -10     1993   03 33 30
03 36 50  ---          14 09 33  39.6 -68.2  4.0      76.7   200     2005   03 33 21

03 37 50  J1001+3424   14 10 33  38.3 -68.4  4.1      75.7    50     2005   03 37 50
03 38 50  =0958+346    14 11 33  38.1 -68.4  4.2      75.6    60     2009   03 37 51

03 38 50  3C236        14 11 33  39.2 -68.1  4.1      76.5   -10     2009   03 39 00
03 42 20  ---          14 15 04  38.5 -67.8  4.1      76.1   200     2022   03 38 51

03 42 20  J1001+3424   14 15 04  37.4 -68.1  4.2      75.3   -10     2022   03 42 30
03 44 20  =0958+346    14 17 04  37.0 -68.0  4.2      75.1   110     2029   03 42 21

03 44 20  3C236        14 17 04  38.1 -67.7  4.2      75.9   -10     2029   03 44 30
03 47 50  ---          14 20 35  37.4 -67.5  4.2      75.5   200     2042   03 44 21

03 48 50  J1001+3424   14 21 35  36.1 -67.7  4.3      74.6    50     2042   03 48 50
03 49 50  =0958+346    14 22 35  35.9 -67.6  4.3      74.5    60     2046   03 48 51

03 49 50  3C236        14 22 35  37.0 -67.4  4.3      75.3   -10     2046   03 50 00
03 53 20  ---          14 26 06  36.3 -67.1  4.3      75.0   200     2059   03 49 51

03 53 20  J1001+3424   14 26 06  35.2 -67.4  4.4      74.1   -10     2059   03 53 30
03 55 20  =0958+346    14 28 06  34.8 -67.2  4.4      73.9   110     2066   03 53 21

03 55 20  3C236        14 28 06  35.9 -67.0  4.4      74.8   -10     2066   03 55 30
03 58 50  ---          14 31 37  35.2 -66.8  4.4      74.4   200     2079   03 55 21

03 59 50  J1001+3424   14 32 37  33.9 -66.9  4.5      73.5    50     2079   03 59 50
04 00 50  =0958+346    14 33 37  33.7 -66.9  4.5      73.4    60     2083   03 59 51

04 00 50  3C236        14 33 37  34.8 -66.6  4.4      74.2   -10     2083   04 01 00
04 04 20  ---          14 37 08  34.1 -66.4  4.5      73.8   200     2096   04 00 51

04 04 20  J1001+3424   14 37 08  33.0 -66.6  4.6      73.0   -10     2096   04 04 30
04 06 20  =0958+346    14 39 08  32.6 -66.5  4.6      72.8   110     2103   04 04 21

04 06 20  3C236        14 39 08  33.7 -66.2  4.5      73.6   -10     2103   04 06 30
04 09 50  ---          14 42 38  33.0 -66.0  4.6      73.3   200     2116   04 06 21

04 10 50  J1001+3424   14 43 39  31.7 -66.1  4.7      72.4    50     2116   04 10 50
04 11 50  =0958+346    14 44 39  31.5 -66.1  4.7      72.3    60     2119   04 10 51
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

04 11 50  3C236        14 44 39  32.6 -65.9  4.6      73.0   -10     2119   04 12 00
04 15 20  ---          14 48 09  31.9 -65.6  4.7      72.7   200     2132   04 11 51

04 15 20  J1001+3424   14 48 09  30.8 -65.8  4.8      71.9   -10     2132   04 15 30
04 17 20  =0958+346    14 50 10  30.5 -65.6  4.8      71.7   110     2139   04 15 21

04 17 20  3C236        14 50 10  31.5 -65.5  4.7      72.5   -10     2139   04 17 30
04 20 50  ---          14 53 40  30.9 -65.2  4.8      72.1   200     2152   04 17 21

04 21 50  J1001+3424   14 54 40  29.6 -65.3  4.9      71.2    50     2152   04 21 50
04 22 50  =0958+346    14 55 41  29.4 -65.2  4.9      71.1    60     2156   04 21 51

04 22 50  3C236        14 55 41  30.5 -65.1  4.8      71.9   -10     2156   04 23 00
04 26 20  ---          14 59 11  29.8 -64.8  4.9      71.5   200     2169   04 22 51

04 26 20  J1001+3424   14 59 11  28.7 -65.0  5.0      70.8   -10     2169   04 26 30
04 28 20  =0958+346    15 01 12  28.3 -64.8  5.0      70.5   110     2176   04 26 21

04 29 20  J0927+3902   15 02 12  23.3 -57.3  5.6      68.6    42     2176   04 29 20
04 34 40  =0923+392    15 07 33  22.3 -56.8  5.7      67.9   320     2197   04 29 21

04 34 40  J1001+3424   15 07 33  27.1 -64.3  5.1      69.9   -17     2197   04 34 57
04 36 40  =0958+346    15 09 33  26.7 -64.1  5.1      69.7   103     2203   04 34 41

04 36 40  3C236        15 09 33  27.8 -64.0  5.0      70.4   -10     2203   04 36 50
04 40 00  ---          15 12 53  27.1 -63.7  5.1      70.1   190     2216   04 36 41

04 41 00  J1001+3424   15 13 54  25.8 -63.8  5.2      69.2    50     2216   04 41 00
04 42 00  =0958+346    15 14 54  25.6 -63.7  5.2      69.1    60     2219   04 41 01

04 42 00  3C236        15 14 54  26.7 -63.6  5.1      69.8   -10     2219   04 42 10
04 45 20  ---          15 18 14  26.1 -63.3  5.2      69.5   190     2232   04 42 01

04 45 20  J1001+3424   15 18 14  25.0 -63.4  5.3      68.8   -10     2232   04 45 30
04 47 20  =0958+346    15 20 15  24.6 -63.3  5.3      68.5   110     2239   04 45 21

04 47 20  3C236        15 20 15  25.7 -63.2  5.2      69.3   -10     2239   04 47 30
04 50 40  ---          15 23 35  25.1 -62.9  5.3      68.9   190     2251   04 47 21

04 51 40  J1001+3424   15 24 35  23.8 -62.9  5.4      68.1    50     2251   04 51 40
04 52 40  =0958+346    15 25 36  23.6 -62.8  5.4      68.0    60     2255   04 51 41

04 52 40  3C236        15 25 36  24.7 -62.7  5.3      68.7   -10     2255   04 52 50
04 56 00  ---          15 28 56  24.1 -62.4  5.4      68.3   190     2267   04 52 41
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Jun 2015   Day 165 ---

04 56 00  J1001+3424   15 28 56  22.9 -62.5  5.4      67.6   -10     2267   04 56 10
04 58 00  =0958+346    15 30 56  22.6 -62.4  5.5      67.4   110     2274   04 56 01

04 58 00  3C236        15 30 56  23.7 -62.3  5.4      68.1   -10     2274   04 58 10
05 01 20  ---          15 34 17  23.0 -62.0  5.5      67.7   190     2286   04 58 01

05 02 20  J1001+3424   15 35 17  21.7 -62.0  5.6      66.9    50     2286   05 02 20
05 03 20  =0958+346    15 36 17  21.5 -61.9  5.6      66.8    60     2290   05 02 21

05 03 20  3C236        15 36 17  22.7 -61.8  5.5      67.5   -10     2290   05 03 30
05 06 40  ---          15 39 38  22.0 -61.5  5.5      67.2   190     2303   05 03 21

05 06 40  J1001+3424   15 39 38  20.9 -61.6  5.6      66.4   -10     2303   05 06 50
05 08 40  =0958+346    15 41 38  20.5 -61.4  5.7      66.2   110     2310   05 06 41

05 08 40  3C236        15 41 38  21.6 -61.4  5.6      66.9   -10     2310   05 08 50
05 12 00  ---          15 44 59  21.0 -61.1  5.6      66.6   190     2322   05 08 41

05 13 00  J1001+3424   15 45 59  19.7 -61.0  5.7      65.7    50     2322   05 13 00
05 14 00  =0958+346    15 46 59  19.5 -60.9  5.7      65.6    60     2326   05 13 01

05 14 00  3C236        15 46 59  20.6 -60.9  5.7      66.3   -10     2326   05 14 10
05 17 20  ---          15 50 20  20.0 -60.6  5.7      66.0   190     2338   05 14 01

05 17 20  J1001+3424   15 50 20  18.9 -60.6  5.8      65.3   -10     2338   05 17 30
05 19 20  =0958+346    15 52 20  18.5 -60.5  5.8      65.0   110     2345   05 17 21

05 19 20  3C236        15 52 20  19.6 -60.4  5.8      65.7   -10     2345   05 19 30
05 22 40  ---          15 55 40  19.0 -60.1  5.8      65.4   190     2357   05 19 21

05 23 40  J1001+3424   15 56 41  17.7 -60.1  5.9      64.6    50     2357   05 23 40
05 24 40  =0958+346    15 57 41  17.5 -60.0  5.9      64.4    60     2361   05 23 41

05 24 40  3C236        15 57 41  18.6 -59.9  5.8      65.1   -10     2361   05 24 50
05 28 00  ---          16 01 01  18.0 -59.6  5.9      64.8   190     2373   05 24 41

05 28 00  J1001+3424   16 01 01  16.9 -59.7  6.0      64.1   -10     2373   05 28 10
05 30 00  =0958+346    16 03 02  16.5 -59.5  6.0      63.8   110     2381   05 28 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: 3C236globHI.set
   Matching groups in /usr/local/sched/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         L         L         L         L         L         L         L         L
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

  Frequency Set:   7  Based on FREQ, BW, and/or DOPPLER in schedule.  Used with PCAL = off
   LO sum=   1300.75  1300.75  1316.75  1316.75  1332.75  1332.75  1348.75  1348.75
   BBC fr=    799.25   799.25   783.25   783.25   767.25   767.25   751.25   751.25
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     783.25    783.25    767.25    767.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   7   8   9  10  11  12  13  14  15  16

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 3C236             10 03 05.383878   * 10 06 01.731500     10 06 55.181395       0.00
                     35 08 47.92723    * 34 54 10.43400      34 49 42.75248        0.00
                     From catalog imbedded in main SCHED input file.
                     Doppler based on heliocentric frame and optical definition.  Velocities:
                      29600.00 29600.00 29600.00 29600.00 29600.00 29600.00 29600.00 29600.00

   0923+392          09 23 55.319219   * 09 27 03.013940     09 27 59.641320       0.13
 * J0927+3902        39 15 23.56641    * 39 02 20.85181      38 58 20.84761        0.10
                     /usr/local/sched/catalogs/sources.rfc
                     rfc_2015a Petrov, 2015, unpublished.  252917 observations
                     Doppler based on other sources.

   0955+326          09 55 25.405783   * 09 58 20.949640     09 59 14.173570       0.12
 * J0958+3224        32 38 23.03247    * 32 24 02.20952      32 19 38.48830        0.10
                     /usr/local/sched/catalogs/sources.rfc
                     rfc_2015a Petrov, 2015, unpublished.  4018 observations
                     Doppler based on other sources.

   0958+346          09 58 15.166820   * 10 01 11.949214     10 02 05.519375       0.13
 * J1001+3424        34 39 17.56149    * 34 24 50.45927      34 20 25.53804        0.11
                     /usr/local/sched/catalogs/sources.rfc
                     rfc_2015a Petrov, 2015, unpublished.  843 observations
                     Doppler based on other sources.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  3C236      3C236globHI.set       1 2 3 4 5 6 7 17                  8.461   512.328
  J0927+3902 3C236globHI.set       1 2 3 4 5 6 7                     0.761    46.616
  J0958+3224 3C236globHI.set       1 2 3 4 5 7 17                    0.233    27.415
  J1001+3424 3C236globHI.set       1 2 3 4 5 6 7 17                  4.061   219.192


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   3C236               60.9
   J0927+3902          52.8
   J0958+3224          59.8
   J1001+3424          60.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

