  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Resolving the jets in Cygnus A
 Exp. Code:  GB065A  


Schedule Version:       1.00                                              
Processed by SCHED version:   8.00  2008 December Release                 

PI:       Uwe Bach                                                        

Address:  Max-Planck-Institut fuer Radioastronomie                        
          Auf dem Huegel 69                                               
          53121 Bonn                                                      
          Germany                                                         

Phone:    0049-2257-301-168                                               
EMAIL:    ubach@mpifr-bonn.mpg.de                                         
Fax:      0049-2257-301-106                                               
Phone during observation: 0049-2257-301-155                               

Observing mode: 512-8-2                                                   

Notes:    Use 2013+370 as fring tracer and 0836+71,                       
          1749+096 and BL Lac as polarization calibrators                 
          Do not point on CygA, it is extended                            
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

 ---------- Back to VLBI ----------

 Next scan frequencies: 43170.49 43170.49 43186.49 43186.49 43202.49 43202.49
                        43218.49 43218.49
 Next BBC frequencies:    770.49   770.49   786.49   786.49   802.49   802.49
                          818.49   818.49
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00

06 36 22  3C345        11 28 22  27.1  57.8 -5.2     -71.4     0   1  1      0  06 36 22
06 51 22  ---          11 43 24  29.8  58.8 -5.0     -73.3   900   F  1     58  06 36 23

06 59 52  0836+710     11 51 56  42.3 -19.0  3.2     121.2   452   1  1     58  06 59 52
07 14 52  ---          12 06 58  41.2 -19.8  3.4     117.1   900   F  1    116  06 59 53

07 15 40  0716+714     12 07 46  34.9 -21.7  4.7      97.0    29   1  1    116  07 15 40
07 30 40  ---          12 22 49  33.7 -21.8  5.0      93.3   900   F  1    174  07 15 41

07 49 34  CYG-A        12 41 45   6.6  46.0 -7.3     -54.7  1073   1  1    174  07 49 34
07 59 34  ---          12 51 47   8.2  47.0 -7.1     -56.2   600   F  1    213  07 49 35

07 59 56  CYG-A        12 52 09   8.2  47.1 -7.1     -56.3    17   1  1    213  07 59 56
08 09 56  ---          13 02 11   9.8  48.1 -7.0     -57.8   600   F  1    252  07 59 57

 ---------- Back to VLBI ----------

08 18 15  1749+096     13 10 31  21.7  91.5 -4.7     -60.7   464   1  1    252  08 18 15
08 22 15  ---          13 14 32  22.6  92.0 -4.6     -60.7   240   F  1    267  08 18 16

08 30 15  2013+370     13 22 33   8.6  51.6 -6.9     -57.9   446   1  1    267  08 30 15
08 34 15  ---          13 26 34   9.3  52.1 -6.8     -58.4   240   F  1    283  08 30 16

08 35 32  CYG-A        13 27 51  14.0  50.6 -6.5     -61.4    61   1  1    283  08 35 32
08 45 32  ---          13 37 53  15.7  51.6 -6.4     -62.8   600   F  1    321  08 35 33

08 45 54  CYG-A        13 38 15  15.8  51.6 -6.4     -62.9    17   1  1    321  08 45 54
08 55 54  ---          13 48 16  17.5  52.5 -6.2     -64.3   600   F  1    360  08 45 55

09 03 54  1749+096     13 56 18  31.5  97.8 -3.9     -59.9   444   1  1    360  09 03 54
09 07 54  ---          14 00 18  32.4  98.4 -3.9     -59.7   240   F  1    375  09 03 55
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

 ---------- Back to VLBI ----------

09 22 16  2013+370     14 14 43  17.7  56.7 -6.0     -64.6   827   1  1    375  09 22 16
09 26 16  ---          14 18 44  18.5  57.1 -6.0     -65.1   240   F  1    391  09 22 17

09 27 20  CYG-A        14 19 47  22.9  55.0 -5.7     -68.5    49   1  1    391  09 27 20
09 37 20  ---          14 29 49  24.7  55.8 -5.5     -69.9   600   F  1    430  09 27 21

09 37 42  CYG-A        14 30 11  24.8  55.8 -5.5     -69.9    17   1  1    430  09 37 42
09 47 42  ---          14 40 13  26.6  56.5 -5.3     -71.3   600   F  1    468  09 37 43

09 48 39  2013+370     14 41 11  22.6  59.0 -5.6     -67.8    44   1  1    468  09 48 39
09 52 39  ---          14 45 11  23.3  59.3 -5.5     -68.3   240   F  1    484  09 48 40

09 53 38  CYG-A        14 46 09  27.6  56.9 -5.2     -72.0    43   1  1    484  09 53 38
10 03 38  ---          14 56 11  29.4  57.5 -5.1     -73.4   600   F  1    523  09 53 39

10 04 00  CYG-A        14 56 33  29.5  57.5 -5.1     -73.4    17   1  1    523  10 04 00
10 14 00  ---          15 06 35  31.3  58.1 -4.9     -74.8   600   F  1    561  10 04 01

10 16 29  BLLAC        15 09 04  11.2  47.1 -6.9     -58.5   103   1  1    561  10 16 29
10 20 29  ---          15 13 05  11.9  47.5 -6.8     -59.1   240   F  1    577  10 16 30

10 29 09  1749+096     15 21 46  49.3 112.9 -2.5     -53.5   439   1  1    577  10 29 09
10 33 09  ---          15 25 47  50.1 113.8 -2.4     -53.0   240   F  1    592  10 29 10

 ---------- Back to VLBI ----------

10 48 11  2013+370     15 40 52  33.8  63.3 -4.6     -74.8   863   1  1    592  10 48 11
10 52 11  ---          15 44 52  34.6  63.6 -4.5     -75.3   240   F  1    608  10 48 12

10 53 01  CYG-A        15 45 43  38.6  60.1 -4.2     -80.0    37   1  1    608  10 53 01
11 03 01  ---          15 55 45  40.4  60.5 -4.1     -81.4   600   F  1    646  10 53 02

11 03 24  CYG-A        15 56 07  40.5  60.5 -4.1     -81.5    17   1  1    646  11 03 24
11 13 24  ---          16 06 09  42.4  60.9 -3.9     -82.9   600   F  1    685  11 03 25

11 16 47  1749+096     16 09 33  58.2 125.9 -1.7     -45.0   154   1  1    685  11 16 47
11 20 47  ---          16 13 33  58.9 127.3 -1.6     -44.0   240   F  1    701  11 16 48

 ---------- Back to VLBI ----------

11 30 24  2013+370     16 23 12  42.0  65.7 -3.9     -79.8   530   1  1    701  11 30 24
11 34 24  ---          16 27 13  42.8  65.8 -3.8     -80.3   240   F  1    716  11 30 25
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

11 35 12  CYG-A        16 28 00  46.5  61.4 -3.5     -86.0    34   1  1    716  11 35 12
11 45 12  ---          16 38 02  48.4  61.6 -3.4     -87.6   600   F  1    755  11 35 13

11 45 34  CYG-A        16 38 24  48.5  61.6 -3.4     -87.6    17   1  1    755  11 45 34
11 55 34  ---          16 48 26  50.4  61.7 -3.2     -89.2   600   F  1    793  11 45 35

 ---------- Back to VLBI ----------

12 03 37  BLLAC        16 56 30  29.3  55.6 -5.1     -73.8   435   1  1    793  12 03 37
12 07 37  ---          17 00 31  30.1  55.9 -5.0     -74.4   240   F  1    809  12 03 38

 ---------- Back to VLBI ----------

12 15 31  2013+370     17 08 26  51.0  67.3 -3.1     -85.4   426   1  1    809  12 15 31
12 19 31  ---          17 12 26  51.8  67.4 -3.1     -86.0   240   F  1    824  12 15 32

12 20 24  CYG-A        17 13 19  55.1  61.5 -2.8     -93.4    40   1  1    824  12 20 24
12 30 24  ---          17 23 21  57.0  61.2 -2.6     -95.2   600   F  1    863  12 20 25

12 30 46  CYG-A        17 23 43  57.0  61.2 -2.6     -95.3    17   1  1    863  12 30 46
12 40 46  ---          17 33 45  58.9  60.8 -2.4     -97.3   600   F  1    902  12 30 47

 ---------- Back to VLBI ----------

12 55 48  2013+370     17 48 50  59.0  67.7 -2.4     -91.2   892   1  1    902  12 55 48
12 59 48  ---          17 52 51  59.8  67.7 -2.4     -91.9   240   F  1    917  12 55 49

13 01 08  CYG-A        17 54 11  62.7  59.5 -2.1    -101.8    68   1  1    917  13 01 08
13 11 08  ---          18 04 12  64.6  58.6 -1.9    -104.3   600   F  1    956  13 01 09

13 11 34  CYG-A        18 04 38  64.7  58.5 -1.9    -104.4    21   1  1    956  13 11 34
13 21 34  ---          18 14 40  66.5  57.3 -1.8    -107.2   600   F  1    995  13 11 35

13 27 35  1749+096     18 20 42  68.0 199.2  0.5      16.6   260   1  1    995  13 27 35
13 31 35  ---          18 24 42  67.7 201.7  0.5      18.8   240   F  1   1010  13 27 36

 ---------- Back to VLBI ----------

13 41 50  2013+370     18 35 00  68.2  65.7 -1.7    -100.0   519   1  1   1010  13 41 50
13 45 50  ---          18 39 00  68.9  65.3 -1.6    -101.0   240   F  1   1026  13 41 51

13 49 53  CYG-A        18 43 04  71.5  51.6 -1.3    -117.1   228   1  1   1026  13 49 53
13 59 53  ---          18 53 05  73.1  48.6 -1.1    -121.6   600   F  1   1064  13 49 54
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

14 00 17  CYG-A        18 53 29  73.2  48.4 -1.1    -121.8    19   1  1   1064  14 00 17
14 10 17  ---          19 03 31  74.8  44.5 -0.9    -127.2   600   F  1   1103  14 00 18

 ---------- Back to VLBI ----------

14 21 03  BLLAC        19 14 19  54.5  58.9 -2.8     -95.2   600   1  1   1103  14 21 03
14 25 03  ---          19 18 20  55.3  58.7 -2.7     -96.0   240   F  1   1119  14 21 04

 ---------- Back to VLBI ----------

14 36 29  2013+370     19 29 47  78.4  52.3 -0.8    -121.2   633   1  1   1119  14 36 29
14 40 29  ---          19 33 48  79.1  50.1 -0.7    -124.0   240   F  1   1134  14 36 30

14 41 30  CYG-A        19 34 49  78.7  24.8 -0.4    -151.5    38   1  1   1134  14 41 30
14 51 30  ---          19 44 51  79.4  15.6 -0.2    -162.2   600   F  1   1173  14 41 31

14 51 52  CYG-A        19 45 13  79.5  15.3 -0.2    -162.6    17   1  1   1173  14 51 52
15 01 52  ---          19 55 15  79.8   4.9 -0.1    -174.5   600   F  1   1212  14 51 53

15 05 55  BLLAC        19 59 18  62.7  56.0 -2.1    -105.2   202   1  1   1212  15 05 55
15 09 55  ---          20 03 18  63.4  55.6 -2.0    -106.3   240   F  1   1227  15 05 56

 ---------- Back to VLBI ----------

15 20 32  2013+370     20 13 58  83.4   3.2  0.0    -176.5   592   1  1   1227  15 20 32
15 24 32  ---          20 17 59  83.4  -3.8  0.0     175.9   240   F  1   1243  15 20 33

15 25 57  CYG-A        20 19 23  79.1 -20.1  0.3     157.1    68   1  1   1243  15 25 57
15 35 57  ---          20 29 25  78.2 -28.6  0.5     147.0   600   F  1   1281  15 25 58

15 36 19  CYG-A        20 29 47  78.2 -28.9  0.5     146.7    17   1  1   1281  15 36 19
15 46 19  ---          20 39 49  77.0 -35.9  0.7     138.2   600   F  1   1320  15 36 20

15 53 36  1749+096     20 47 07  44.3 252.2  2.9      56.2   239   1  1   1320  15 53 36
15 57 36  ---          20 51 08  43.4 253.0  3.0      56.6   240   F  1   1335  15 53 37

 ---------- Back to VLBI ----------

16 06 41  2013+370     21 00 14  78.7 308.5  0.7     122.3   469   1  1   1335  16 06 41
16 10 41  ---          21 04 15  78.0 306.5  0.8     119.7   240   F  1   1351  16 06 42

16 12 04  CYG-A        21 05 38  73.3 311.7  1.1     122.1    67   1  1   1351  16 12 04
16 22 04  ---          21 15 39  71.6 308.6  1.3     117.4   600   F  1   1390  16 12 05
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

16 22 26  CYG-A        21 16 01  71.6 308.5  1.3     117.3    17   1  1   1390  16 22 26
16 32 26  ---          21 26 03  69.9 306.1  1.4     113.3   600   F  1   1428  16 22 27

 ---------- Back to VLBI ----------

16 40 29  BLLAC        21 34 08  77.0 384.4 -0.5    -151.3   425   1  1   1428  16 40 29
16 44 29  ---          21 38 09  77.3 381.4 -0.4    -154.9   240   F  1   1444  16 40 30

 ---------- Back to VLBI ----------

16 52 28  2013+370     21 46 09  70.2 295.5  1.5     102.7   415   1  1   1444  16 52 28
16 56 28  ---          21 50 09  69.4 295.0  1.6     101.7   240   F  1   1459  16 52 29

16 57 12  CYG-A        21 50 53  65.4 302.0  1.9     105.5    30   1  1   1459  16 57 12
17 07 12  ---          22 00 55  63.6 300.9  2.0     102.9   600   F  1   1498  16 57 13

17 07 34  CYG-A        22 01 17  63.5 300.8  2.0     102.8    17   1  1   1498  17 07 34
17 17 34  ---          22 11 19  61.6 300.0  2.2     100.4   600   F  1   1537  17 07 35

17 21 15  1749+096     22 15 01  25.7 266.0  4.4      60.5   144   1  1   1537  17 21 15
17 25 15  ---          22 19 01  24.8 266.6  4.5      60.6   240   F  1   1552  17 21 16

17 28 00  2013+370     22 21 46  63.2 292.7  2.1      94.8    81   1  1   1552  17 28 00
17 32 00  ---          22 25 47  62.4 292.6  2.2      94.1   240   F  1   1568  17 28 01

17 32 42  CYG-A        22 26 29  58.8 299.1  2.4      97.2    29   1  1   1568  17 32 42
17 42 42  ---          22 36 31  56.9 298.7  2.6      95.2   600   F  1   1606  17 32 43

17 43 04  CYG-A        22 36 53  56.8 298.7  2.6      95.1    17   1  1   1606  17 43 04
17 53 04  ---          22 46 55  55.0 298.5  2.8      93.3   600   F  1   1645  17 43 05

 ---------- Back to VLBI ----------

18 01 07  BLLAC        22 54 59  74.4 322.0  0.9     134.2   438   1  1   1645  18 01 07
18 05 07  ---          22 59 00  73.8 320.1  0.9     131.7   240   F  1   1661  18 01 08

 ---------- Back to VLBI ----------

18 13 07  2013+370     23 07 01  54.2 292.4  2.9      87.6   434   1  1   1661  18 13 07
18 17 07  ---          23 11 01  53.4 292.4  2.9      87.1   240   F  1   1676  18 13 08

18 17 48  CYG-A        23 11 43  50.3 298.3  3.2      89.1    29   1  1   1676  18 17 48
18 27 48  ---          23 21 44  48.4 298.4  3.4      87.5   600   F  1   1715  18 17 49
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

18 28 10  CYG-A        23 22 07  48.3 298.4  3.4      87.5    17   1  1   1715  18 28 10
18 38 10  ---          23 32 08  46.4 298.6  3.5      86.0   600   F  1   1753  18 28 11

18 38 51  2013+370     23 32 49  49.1 292.9  3.3      84.2    29   1  1   1753  18 38 51
18 42 51  ---          23 36 50  48.3 293.1  3.4      83.7   240   F  1   1769  18 38 52

18 43 32  CYG-A        23 37 31  45.4 298.7  3.6      85.2    29   1  1   1769  18 43 32
18 53 32  ---          23 47 32  43.5 298.9  3.8      83.7   600   F  1   1808  18 43 33

18 53 54  CYG-A        23 47 55  43.4 299.0  3.8      83.6    17   1  1   1808  18 53 54
19 03 54  ---          23 57 56  41.5 299.3  4.0      82.2   600   F  1   1846  18 53 55

 ---------- Back to VLBI ----------

19 11 55  BLLAC        00 05 58  62.9 304.1  2.0     105.4   432   1  1   1846  19 11 55
19 15 55  ---          00 09 59  62.2 303.7  2.1     104.4   240   F  1   1862  19 11 56

 ---------- Back to VLBI ----------

19 23 54  2013+370     00 17 59  40.2 294.8  4.0      78.7   429   1  1   1862  19 23 54
19 27 54  ---          00 22 00  39.4 295.0  4.1      78.2   240   F  1   1877  19 23 55

19 28 34  CYG-A        00 22 40  36.9 300.3  4.4      78.8    29   1  1   1877  19 28 34
19 38 34  ---          00 32 42  35.1 300.8  4.5      77.5   600   F  1   1916  19 28 35

19 38 56  CYG-A        00 33 04  35.0 300.8  4.6      77.4    17   1  1   1916  19 38 56
19 48 56  ---          00 43 06  33.1 301.3  4.7      76.1   600   F  1   1955  19 38 57

19 49 36  2013+370     00 43 46  35.2 296.3  4.5      75.7    30   1  1   1955  19 49 36
19 53 36  ---          00 47 46  34.4 296.5  4.5      75.2   240   F  1   1970  19 49 37

19 54 16  CYG-A        00 48 27  32.2 301.6  4.8      75.4    30   1  1   1970  19 54 16
20 04 16  ---          00 58 28  30.3 302.2  5.0      74.0   600   F  1   2009  19 54 17

20 04 38  CYG-A        00 58 50  30.3 302.2  5.0      74.0    17   1  1   2009  20 04 38
20 14 38  ---          01 08 52  28.4 302.8  5.2      72.6   600   F  1   2048  20 04 39

 ---------- Back to VLBI ----------

20 22 35  BLLAC        01 16 50  49.9 300.8  3.2      90.7   428   1  1   2048  20 22 35
20 26 35  ---          01 20 51  49.2 300.8  3.3      90.0   240   F  1   2063  20 22 36
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Resolving the jets in Cygnus A
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Thu  19 Mar 2009   Day  78 ---

 ---------- Back to VLBI ----------

20 34 32  2013+370     01 28 49  26.6 299.3  5.2      70.4   426   1  1   2063  20 34 32
20 38 32  ---          01 32 50  25.8 299.6  5.3      69.9   240   F  1   2079  20 34 33

20 39 12  CYG-A        01 33 30  24.0 304.5  5.6      69.4    30   1  1   2079  20 39 12
20 49 12  ---          01 43 31  22.3 305.3  5.7      68.0   600   F  1   2117  20 39 13

20 49 34  CYG-A        01 43 53  22.2 305.3  5.7      68.0    17   1  1   2117  20 49 34
20 59 34  ---          01 53 55  20.4 306.1  5.9      66.6   600   F  1   2156  20 49 35

20 59 56  2013+370     01 54 18  21.9 301.3  5.6      67.4    14   1  1   2156  20 59 56
21 03 56  ---          01 58 18  21.1 301.6  5.7      66.9   240   F  1   2171  20 59 57

21 04 19  CYG-A        01 58 41  19.6 306.5  6.0      66.0    14   1  1   2171  21 04 19
21 14 19  ---          02 08 43  17.9 307.3  6.1      64.6   600   F  1   2210  21 04 20

21 14 34  CYG-A        02 08 58  17.9 307.3  6.2      64.6    10   1  1   2210  21 14 34
21 24 34  ---          02 19 00  16.1 308.2  6.3      63.2   600   F  1   2249  21 14 35

21 25 55  BLLAC        02 20 21  38.2 302.0  4.3      80.8    31   1  1   2249  21 25 55
21 29 55  ---          02 24 22  37.5 302.1  4.4      80.2   240   F  1   2264  21 25 56

21 31 14  2013+370     02 25 41  16.2 304.1  6.2      63.5    30   1  1   2264  21 31 14
21 35 14  ---          02 29 41  15.5 304.4  6.2      63.0   240   F  1   2280  21 31 15

21 35 37  CYG-A        02 30 04  14.3 309.2  6.5      61.7    13   1  1   2280  21 35 37
21 45 37  ---          02 40 06  12.6 310.2  6.7      60.2   600   F  1   2319  21 35 38

21 45 52  CYG-A        02 40 21  12.6 310.2  6.7      60.2    10   1  1   2319  21 45 52
21 55 52  ---          02 50 23  10.9 311.2  6.8      58.8   600   F  1   2357  21 45 53

21 56 15  2013+370     02 50 45  11.8 306.5  6.6      60.3    13   1  1   2357  21 56 15
22 00 15  ---          02 54 46  11.1 306.9  6.6      59.8   240   F  1   2373  21 56 16

22 00 37  CYG-A        02 55 09  10.2 311.6  6.9      58.1    13   1  1   2373  22 00 37
22 10 37  ---          03 05 10   8.6 312.7  7.1      56.6   600   F  1   2411  22 00 38

22 10 53  CYG-A        03 05 26   8.5 312.7  7.1      56.6    10   1  1   2411  22 10 53
22 20 53  ---          03 15 27   7.0 313.8  7.3      55.1   600   F  1   2450  22 10 54

22 22 11  BLLAC        03 16 46  28.1 304.8  5.2      72.8    30   1  1   2450  22 22 11
22 26 11  ---          03 20 46  27.4 305.1  5.3      72.3   240   F  1   2466  22 22 12


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: 7mmpol.set
   Matches group v7mm_c8 in ./7mmfreq.dat

   Setup group:    2         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.4      7.6     11.6

  The following frequency sets based on this setup were used.

   Frequency Set:   2  Setup file default.  Used pcal sets:   1
   LO sum=   43170.49  43170.49  43186.49  43186.49  43202.49  43202.49  43218.49  43218.49
   BBC fr=     770.49    770.49    786.49    786.49    802.49    802.49    818.49    818.49
   Bandwd=     16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510 13510 13510 13510 13510
    PCALFR2=   510   510   510   510 13510 13510 13510 13510

   Track assignments are: 
    track1=   2, 18,  3, 19, 66, 82, 67, 83
    barrel=roll_off 
 SOURCE LIST -- Resolving the jets in Cygnus A
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 2013+370          20 13 37.018003   * 20 15 28.733300     20 15 48.816844       0.00
                     37 01 44.44891    * 37 10 59.50500      37 12 24.88186        0.00
                     From catalog imbedded in main SCHED input file.
                        1.483 scan hours,    108.181 baseline hours above horizon.

   J0721+7120        07 16 13.029732   * 07 21 53.448467     07 22 59.712579       0.63
 * 0716+714          71 26 15.17408    * 71 20 36.36342      71 19 48.91200        0.40
   J0721+71          /home/ubach/data/progs/sched/catalogs/sources.vlba
                     VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
                        0.250 scan hours,     22.750 baseline hours above horizon.

   J0841+7053        08 36 21.556634   * 08 41 24.365272     08 42 24.725856       0.61
 * 0836+710          71 04 22.42737    * 70 53 42.17300      70 51 53.70649        0.40
   J0841+70          /home/ubach/data/progs/sched/catalogs/sources.vlba
                     VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
                        0.250 scan hours,     22.750 baseline hours above horizon.

   J1642+3948        16 41 17.606227   * 16 42 58.809964     16 43 18.595081       0.26
 * 3C345             39 54 10.81495    * 39 48 36.99401      39 47 10.86448        0.40
   1641+399          /home/ubach/data/progs/sched/catalogs/sources.vlba
   J1642+39          VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
                        0.250 scan hours,     19.500 baseline hours above horizon.

   J1751+0939        17 49 10.387930   * 17 51 32.818573     17 51 59.834092       0.30
 * 1749+096          09 39 42.82589    * 09 39 00.72844      09 38 36.65235        0.20
   J1751+09          /home/ubach/data/progs/sched/catalogs/sources.vlba
                     VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
                        0.467 scan hours,     35.266 baseline hours above horizon.

   J1959+4044        19 57 44.440774   * 19 59 28.356451     19 59 47.002836       1.23
 * CYG-A             40 35 46.36296    * 40 44 02.09677      40 45 15.07111        0.88
   CYGNUS-A          /home/ubach/data/progs/sched/catalogs/sources.vlba
   J1959+40          VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
                        7.333 scan hours,    552.153 baseline hours above horizon.

   J2202+4216        22 00 39.362505   * 22 02 43.291372     22 03 04.987739       0.27
 * BLLAC             42 02 08.59080    * 42 16 39.97994      42 19 11.11740        0.40
   2200+420          /home/ubach/data/progs/sched/catalogs/sources.vlba
   J2202+42          VLBA Calib Survey - GSFC sols. - created L.Petrov 2008a_astro
   VR42220              0.667 scan hours,     51.463 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   2013+370            63.2
   0716+714            97.1
   0836+710           102.9
   3C345              104.2
   1749+096            91.2
   CYG-A               67.5
   BLLAC               49.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

