  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Tracing the Evolution of Fast Jet-Driven Outflows
 Exp. Code:  GN002A  


Schedule Version:       1.00
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Kristina Nyland

Address:  ASTRON, Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands
 

Phone:    0521-595-766
EMAIL:    nyland@astron.nl
Fax:
Phone during observation: 0521-595-766

Observing mode: 21cm spectral line

Notes:    Target: 3C293
          Phase calibrator: J1350+3034
          Bandpass Calibrator: J1407+2827
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

 Next scan frequencies:  1364.50  1364.50  1379.75  1379.75  1395.00  1395.00  1410.25  1410.25
 Next BBC frequencies:    735.50   735.50   720.25   720.25   705.00   705.00   689.75   689.75
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

03 30 00  J1407+2827   07 16 37   4.3  59.4 -6.9     -57.3     0        0   03 30 00
03 35 30  =1404+286    07 22 08   5.3  60.0 -6.8     -57.9   330       21   03 30 01

03 35 45  J1350+3034   07 22 23   9.5  60.0 -6.5     -59.9    -1       21   03 35 46
03 37 45  =1348+308    07 24 23   9.8  60.3 -6.5     -60.1   119       29   03 35 46

03 37 45  3C293        07 24 23  10.0  59.3 -6.5     -60.1    -8       29   03 37 53
03 41 30  ---          07 28 09  10.7  59.8 -6.4     -60.5   217       43   03 37 46

03 42 00  J1350+3034   07 28 39  10.6  60.7 -6.4     -60.6    22       43   03 42 00
03 43 45  =1348+308    07 30 24  11.0  60.9 -6.4     -60.8   105       50   03 42 01

03 43 45  3C293        07 30 24  11.1  60.0 -6.4     -60.8    -8       50   03 43 53
03 47 30  ---          07 34 10  11.8  60.4 -6.3     -61.2   217       64   03 43 46

03 47 30  J1350+3034   07 34 10  11.7  61.3 -6.3     -61.2    -8       64   03 47 38
03 49 30  =1348+308    07 36 10  12.1  61.5 -6.3     -61.4   112       71   03 47 31

03 49 30  3C293        07 36 10  12.2  60.6 -6.3     -61.4    -8       71   03 49 38
03 53 15  ---          07 39 56  12.9  61.0 -6.2     -61.8   217       85   03 49 31

03 53 45  J1350+3034   07 40 26  12.9  62.0 -6.2     -61.8    22       85   03 53 45
03 55 30  =1348+308    07 42 11  13.2  62.2 -6.2     -62.0   105       92   03 53 46

03 55 30  3C293        07 42 11  13.3  61.2 -6.2     -62.0    -8       92   03 55 38
03 59 15  ---          07 45 57  14.0  61.6 -6.1     -62.4   217      106   03 55 31

03 59 15  J1350+3034   07 45 57  13.9  62.5 -6.1     -62.4    -8      106   03 59 23
04 01 15  =1348+308    07 47 57  14.3  62.7 -6.1     -62.6   112      113   03 59 16

04 01 15  3C293        07 47 57  14.4  61.8 -6.1     -62.7    -8      113   04 01 23
04 05 00  ---          07 51 43  15.1  62.2 -6.0     -63.0   217      127   04 01 16

04 05 30  J1350+3034   07 52 13  15.1  63.2 -6.0     -63.0    22      127   04 05 30
04 07 15  =1348+308    07 53 58  15.4  63.4 -6.0     -63.2   105      134   04 05 31

04 07 15  3C293        07 53 58  15.6  62.4 -6.0     -63.3    -8      134   04 07 23
04 11 00  ---          07 57 43  16.3  62.8 -5.9     -63.7   217      147   04 07 16

04 11 00  J1350+3034   07 57 43  16.2  63.7 -5.9     -63.6    -8      147   04 11 08
04 13 00  =1348+308    07 59 44  16.6  63.9 -5.9     -63.8   112      155   04 11 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

04 13 00  3C293        07 59 44  16.7  63.0 -5.9     -63.9    -8      155   04 13 08
04 16 45  ---          08 03 29  17.4  63.4 -5.8     -64.3   217      169   04 13 01

04 17 15  J1350+3034   08 04 00  17.4  64.4 -5.8     -64.2    22      169   04 17 15
04 19 00  =1348+308    08 05 45  17.7  64.5 -5.8     -64.4   105      175   04 17 16

04 19 00  3C293        08 05 45  17.8  63.6 -5.8     -64.5    -8      175   04 19 08
04 22 45  ---          08 09 30  18.6  63.9 -5.7     -64.9   217      189   04 19 01

04 22 45  J1350+3034   08 09 30  18.5  64.9 -5.7     -64.7    -8      189   04 22 53
04 24 45  =1348+308    08 11 31  18.8  65.1 -5.7     -64.9   112      197   04 22 46

04 24 45  3C293        08 11 31  18.9  64.1 -5.7     -65.1    -8      197   04 24 53
04 28 30  ---          08 15 16  19.7  64.5 -5.6     -65.4   217      211   04 24 46

04 29 00  J1350+3034   08 15 46  19.7  65.5 -5.6     -65.3    22      211   04 29 00
04 30 45  =1348+308    08 17 32  20.0  65.7 -5.6     -65.5   105      217   04 29 01

04 30 45  3C293        08 17 32  20.1  64.7 -5.6     -65.6    -8      217   04 30 53
04 34 30  ---          08 21 17  20.8  65.0 -5.5     -66.0   217      231   04 30 46

04 34 30  J1350+3034   08 21 17  20.8  66.0 -5.5     -65.8    -8      231   04 34 38
04 36 30  =1348+308    08 23 18  21.2  66.2 -5.5     -66.0   112      239   04 34 31

04 36 30  3C293        08 23 18  21.2  65.2 -5.5     -66.2    -8      239   04 36 38
04 40 15  ---          08 27 03  22.0  65.6 -5.4     -66.6   217      253   04 36 31

04 40 45  J1350+3034   08 27 33  22.0  66.6 -5.4     -66.4    22      253   04 40 45
04 42 30  =1348+308    08 29 19  22.3  66.8 -5.4     -66.6   105      259   04 40 46

04 42 30  3C293        08 29 19  22.4  65.8 -5.4     -66.8    -8      259   04 42 38
04 46 15  ---          08 33 04  23.1  66.1 -5.3     -67.1   217      273   04 42 31

04 46 15  J1350+3034   08 33 04  23.1  67.1 -5.3     -66.9    -8      273   04 46 23
04 48 15  =1348+308    08 35 05  23.5  67.3 -5.3     -67.1   112      281   04 46 16

04 48 15  3C293        08 35 05  23.5  66.3 -5.3     -67.3    -8      281   04 48 23
04 52 00  ---          08 38 50  24.3  66.6 -5.2     -67.7   217      294   04 48 16

04 52 30  J1350+3034   08 39 20  24.3  67.7 -5.2     -67.5    22      294   04 52 30
04 54 15  =1348+308    08 41 06  24.7  67.8 -5.2     -67.7   105      301   04 52 31

04 54 15  3C293        08 41 06  24.7  66.8 -5.2     -67.9    -8      301   04 54 23
04 58 00  ---          08 44 51  25.5  67.2 -5.1     -68.2   217      315   04 54 16
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

04 58 00  J1350+3034   08 44 51  25.4  68.2 -5.1     -68.0    -8      315   04 58 08
05 00 00  =1348+308    08 46 52  25.8  68.4 -5.1     -68.2   112      322   04 58 01

05 00 00  3C293        08 46 52  25.9  67.3 -5.1     -68.4    -8      322   05 00 08
05 03 25  ---          08 50 17  26.6  67.6 -5.0     -68.7   197      335   05 00 01

05 03 55  J1350+3034   08 50 47  26.6  68.7 -5.0     -68.5    22      335   05 03 55
05 05 40  =1348+308    08 52 32  27.0  68.9 -5.0     -68.7   105      342   05 03 56

05 05 55  J1407+2827   08 52 48  23.0  69.6 -5.2     -66.4    -1      342   05 05 56
05 11 25  =1404+286    08 58 18  24.1  70.1 -5.2     -66.9   329      363   05 05 56

05 11 40  J1350+3034   08 58 33  28.2  69.4 -4.9     -69.2    -1      363   05 11 41
05 13 40  =1348+308    09 00 34  28.6  69.6 -4.9     -69.4   119      371   05 11 41

05 13 40  3C293        09 00 34  28.6  68.5 -4.9     -69.7    -8      371   05 13 48
05 17 25  ---          09 04 19  29.4  68.8 -4.8     -70.0   217      385   05 13 41

05 17 55  J1350+3034   09 04 49  29.4  69.9 -4.8     -69.7    22      385   05 17 55
05 19 40  =1348+308    09 06 35  29.8  70.1 -4.7     -69.9   105      391   05 17 56

05 19 40  3C293        09 06 35  29.8  69.0 -4.8     -70.2    -8      391   05 19 48
05 23 25  ---          09 10 20  30.6  69.3 -4.7     -70.5   217      405   05 19 41

05 23 25  J1350+3034   09 10 20  30.6  70.4 -4.7     -70.2    -8      405   05 23 33
05 25 25  =1348+308    09 12 21  31.0  70.6 -4.7     -70.4   112      413   05 23 26

05 25 25  3C293        09 12 21  31.0  69.5 -4.7     -70.7    -8      413   05 25 33
05 29 10  ---          09 16 06  31.7  69.8 -4.6     -71.1   217      427   05 25 26

05 29 40  J1350+3034   09 16 36  31.8  70.9 -4.6     -70.7    22      427   05 29 40
05 31 25  =1348+308    09 18 22  32.2  71.1 -4.6     -70.9   105      433   05 29 41

05 31 25  3C293        09 18 22  32.2  70.0 -4.6     -71.2    -8      433   05 31 33
05 35 10  ---          09 22 07  32.9  70.3 -4.5     -71.6   217      447   05 31 26

05 35 10  J1350+3034   09 22 07  33.0  71.4 -4.5     -71.2    -8      447   05 35 18
05 37 10  =1348+308    09 24 08  33.4  71.6 -4.5     -71.3   112      455   05 35 11

05 37 10  3C293        09 24 08  33.4  70.5 -4.5     -71.7    -8      455   05 37 18
05 40 55  ---          09 27 53  34.1  70.8 -4.4     -72.1   217      469   05 37 11

05 41 25  J1350+3034   09 28 23  34.2  71.9 -4.4     -71.7    22      469   05 41 25
05 43 10  =1348+308    09 30 09  34.6  72.1 -4.4     -71.8   105      475   05 41 26
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

05 43 10  3C293        09 30 09  34.6  70.9 -4.4     -72.3    -8      475   05 43 18
05 46 55  ---          09 33 54  35.3  71.2 -4.3     -72.6   217      489   05 43 11

05 46 55  J1350+3034   09 33 54  35.4  72.4 -4.3     -72.1    -8      489   05 47 03
05 48 55  =1348+308    09 35 55  35.8  72.5 -4.3     -72.3   112      497   05 46 56

05 48 55  3C293        09 35 55  35.7  71.4 -4.3     -72.8    -8      497   05 49 03
05 52 40  ---          09 39 40  36.5  71.7 -4.2     -73.1   217      511   05 48 56

05 53 10  J1350+3034   09 40 10  36.6  72.9 -4.2     -72.6    22      511   05 53 10
05 54 55  =1348+308    09 41 56  37.0  73.0 -4.2     -72.8   105      517   05 53 11

05 54 55  3C293        09 41 56  37.0  71.9 -4.2     -73.3    -8      517   05 55 03
05 58 40  ---          09 45 41  37.7  72.1 -4.1     -73.6   217      531   05 54 56

05 58 40  J1350+3034   09 45 41  37.8  73.3 -4.1     -73.0    -8      531   05 58 48
06 00 40  =1348+308    09 47 42  38.2  73.5 -4.1     -73.2   112      538   05 58 41

06 00 40  3C293        09 47 42  38.2  72.3 -4.1     -73.7    -8      538   06 00 48
06 04 25  ---          09 51 27  38.9  72.6 -4.0     -74.1   217      552   06 00 41

06 04 55  J1350+3034   09 51 57  39.1  73.8 -4.0     -73.5    21      552   06 04 55
06 06 40  =1348+308    09 53 42  39.4  73.9 -4.0     -73.7   105      559   06 04 56

06 06 40  3C293        09 53 42  39.4  72.8 -4.0     -74.2    -9      559   06 06 49
06 10 25  ---          09 57 28  40.2  73.0 -3.9     -74.5   216      573   06 06 41

06 10 25  J1350+3034   09 57 28  40.2  74.2 -3.9     -74.0    -9      573   06 10 34
06 12 25  =1348+308    09 59 28  40.6  74.4 -3.9     -74.1   111      580   06 10 26

06 12 25  3C293        09 59 28  40.6  73.2 -3.9     -74.7    -9      580   06 12 34
06 16 10  ---          10 03 14  41.3  73.5 -3.8     -75.0   216      594   06 12 26

06 16 40  J1350+3034   10 03 44  41.5  74.7 -3.8     -74.4    21      594   06 16 40
06 18 25  =1348+308    10 05 29  41.9  74.9 -3.8     -74.6   105      601   06 16 41

06 18 25  3C293        10 05 29  41.8  73.6 -3.8     -75.2    -9      601   06 18 34
06 22 10  ---          10 09 15  42.6  73.9 -3.7     -75.5   216      615   06 18 26

06 22 10  J1350+3034   10 09 15  42.7  75.1 -3.7     -74.9    -9      615   06 22 19
06 24 10  =1348+308    10 11 15  43.1  75.3 -3.7     -75.0   111      622   06 22 11

06 24 10  3C293        10 11 15  43.0  74.0 -3.7     -75.7    -9      622   06 24 19
06 27 40  ---          10 14 46  43.7  74.3 -3.6     -76.0   201      635   06 24 11
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

06 28 10  J1350+3034   10 15 16  43.9  75.6 -3.6     -75.3    21      635   06 28 10
06 29 55  =1348+308    10 17 01  44.3  75.7 -3.6     -75.4   105      642   06 28 11

06 30 00  3C293        10 17 06  44.2  74.5 -3.6     -76.1    -4      642   06 30 04
06 33 22  ---          10 20 29  44.9  74.7 -3.5     -76.4   198      654   06 29 56

06 33 52  J1350+3034   10 20 59  45.1  76.0 -3.5     -75.7    21      654   06 33 52
06 35 47  =1348+308    10 22 54  45.5  76.2 -3.5     -75.9   115      662   06 33 53

06 35 52  3C293        10 22 59  45.4  74.9 -3.5     -76.6    -4      662   06 35 56
06 39 14  ---          10 26 22  46.1  75.1 -3.4     -76.9   198      675   06 35 48

06 39 19  J1350+3034   10 26 27  46.2  76.4 -3.4     -76.1    -4      675   06 39 23
06 41 15  =1348+308    10 28 23  46.7  76.6 -3.4     -76.3   112      682   06 39 15

06 41 20  3C293        10 28 28  46.6  75.3 -3.4     -77.1    -4      682   06 41 24
06 44 42  ---          10 31 51  47.3  75.5 -3.4     -77.3   198      695   06 41 16

06 45 12  J1350+3034   10 32 21  47.5  76.9 -3.3     -76.6    21      695   06 45 12
06 47 07  =1348+308    10 34 16  47.9  77.0 -3.3     -76.7   115      702   06 45 13

06 47 12  3C293        10 34 21  47.8  75.7 -3.3     -77.5    -4      702   06 47 16
06 50 34  ---          10 37 44  48.5  75.9 -3.3     -77.8   198      715   06 47 08

06 50 39  J1350+3034   10 37 49  48.6  77.3 -3.2     -76.9    -4      715   06 50 43
06 52 35  =1348+308    10 39 45  49.0  77.4 -3.2     -77.1   112      722   06 50 35

06 52 40  3C293        10 39 50  48.9  76.0 -3.2     -78.0    -4      722   06 52 44
06 56 02  ---          10 43 13  49.6  76.3 -3.2     -78.2   198      735   06 52 36

06 56 32  J1350+3034   10 43 43  49.9  77.7 -3.1     -77.4    21      735   06 56 32
06 58 27  =1348+308    10 45 38  50.3  77.9 -3.1     -77.5   115      742   06 56 33

06 58 32  3C293        10 45 43  50.2  76.4 -3.1     -78.4    -4      742   06 58 36
07 01 54  ---          10 49 06  50.9  76.7 -3.1     -78.7   198      755   06 58 28

07 01 59  J1350+3034   10 49 11  51.0  78.1 -3.0     -77.8    -4      755   07 02 03
07 03 55  =1348+308    10 51 07  51.4  78.3 -3.0     -77.9   112      762   07 01 55

07 04 00  3C293        10 51 12  51.3  76.8 -3.0     -78.8    -4      762   07 04 04
07 07 22  ---          10 54 34  52.0  77.0 -3.0     -79.1   198      775   07 03 56

07 07 52  J1350+3034   10 55 05  52.3  78.5 -2.9     -78.2    21      775   07 07 52
07 09 47  =1348+308    10 57 00  52.7  78.7 -2.9     -78.3   115      782   07 07 53
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

07 09 52  3C293        10 57 05  52.6  77.2 -2.9     -79.3    -4      782   07 09 56
07 13 14  ---          11 00 27  53.3  77.4 -2.9     -79.6   198      795   07 09 48

07 13 19  J1350+3034   11 00 32  53.4  78.9 -2.9     -78.5    -4      795   07 13 23
07 15 15  =1348+308    11 02 29  53.8  79.1 -2.8     -78.7   112      802   07 13 15

07 15 20  3C293        11 02 34  53.7  77.5 -2.8     -79.7    -4      802   07 15 24
07 18 54  ---          11 06 08  54.5  77.8 -2.8     -80.0   210      816   07 15 16

07 19 24  J1350+3034   11 06 38  54.7  79.4 -2.7     -79.0    21      816   07 19 24
07 21 19  =1348+308    11 08 34  55.1  79.5 -2.7     -79.1   115      823   07 19 25

07 21 34  J1407+2827   11 08 49  51.3  81.7 -3.0     -75.4    -1      823   07 21 35
07 27 04  =1404+286    11 14 20  52.4  82.2 -2.9     -75.7   329      844   07 21 35

07 27 19  J1350+3034   11 14 35  56.4  79.9 -2.6     -79.5    -1      844   07 27 20
07 29 59  =1348+308    11 17 15  56.9  80.1 -2.6     -79.7   159      855   07 27 20

07 30 04  3C293        11 17 20  56.8  78.5 -2.6     -80.9    -4      855   07 30 08
07 33 26  ---          11 20 43  57.5  78.7 -2.5     -81.2   198      867   07 30 00

07 33 56  J1350+3034   11 21 13  57.8  80.4 -2.5     -80.0    21      867   07 33 56
07 35 51  =1348+308    11 23 08  58.2  80.5 -2.5     -80.1   115      875   07 33 57

07 35 56  3C293        11 23 13  58.1  78.8 -2.5     -81.4    -4      875   07 36 00
07 39 18  ---          11 26 36  58.8  79.0 -2.4     -81.6   198      887   07 35 52

07 39 23  J1350+3034   11 26 41  58.9  80.8 -2.4     -80.3    -4      887   07 39 27
07 41 18  =1348+308    11 28 36  59.4  80.9 -2.4     -80.5   111      895   07 39 19

07 41 23  3C293        11 28 41  59.2  79.2 -2.4     -81.8    -4      895   07 41 27
07 44 45  ---          11 32 04  59.9  79.4 -2.3     -82.1   198      907   07 41 19

07 45 15  J1350+3034   11 32 34  60.2  81.2 -2.3     -80.7    21      907   07 45 15
07 47 10  =1348+308    11 34 29  60.6  81.3 -2.3     -80.8   115      915   07 45 16

07 47 15  3C293        11 34 34  60.5  79.5 -2.3     -82.3    -4      915   07 47 19
07 50 37  ---          11 37 57  61.2  79.7 -2.3     -82.5   198      928   07 47 11

07 50 42  J1350+3034   11 38 02  61.4  81.6 -2.2     -81.1    -4      928   07 50 46
07 52 37  =1348+308    11 39 57  61.8  81.7 -2.2     -81.2   111      935   07 50 38

07 52 42  3C293        11 40 02  61.6  79.8 -2.2     -82.7    -4      935   07 52 46
07 56 04  ---          11 43 24  62.3  80.0 -2.2     -83.0   198      947   07 52 38
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

07 56 34  J1350+3034   11 43 55  62.6  82.0 -2.1     -81.5    21      947   07 56 34
07 58 29  =1348+308    11 45 50  63.0  82.1 -2.1     -81.6   115      955   07 56 35

07 58 34  3C293        11 45 55  62.9  80.2 -2.1     -83.2    -4      955   07 58 38
08 01 56  ---          11 49 17  63.6  80.3 -2.1     -83.4   198      968   07 58 30

08 02 01  J1350+3034   11 49 22  63.8  82.4 -2.0     -81.8    -4      968   08 02 05
08 03 56  =1348+308    11 51 18  64.2  82.5 -2.0     -81.9   111      975   08 01 57

08 04 01  3C293        11 51 23  64.0  80.5 -2.0     -83.6    -4      975   08 04 05
08 07 23  ---          11 54 45  64.7  80.6 -2.0     -83.9   198      988   08 03 57

08 07 53  J1350+3034   11 55 15  65.0  82.8 -1.9     -82.2    21      988   08 07 53
08 09 48  =1348+308    11 57 11  65.4  82.9 -1.9     -82.3   115      995   08 07 54

08 09 53  3C293        11 57 16  65.3  80.8 -1.9     -84.1    -4      995   08 09 57
08 13 15  ---          12 00 38  66.0  80.9 -1.9     -84.4   198     1008   08 09 49

08 13 20  J1350+3034   12 00 43  66.2  83.2 -1.8     -82.5    -4     1008   08 13 24
08 15 15  =1348+308    12 02 39  66.6  83.3 -1.8     -82.7   111     1015   08 13 16

08 15 20  3C293        12 02 44  66.4  81.1 -1.8     -84.5    -4     1015   08 15 24
08 18 54  ---          12 06 18  67.2  81.2 -1.8     -84.8   210     1028   08 15 16

08 19 24  J1350+3034   12 06 48  67.5  83.6 -1.7     -82.9    20     1028   08 19 24
08 21 20  =1348+308    12 08 45  67.9  83.7 -1.7     -83.0   116     1036   08 19 25

08 21 35  J1407+2827   12 09 00  64.1  87.4 -2.0     -77.7     0     1036   08 21 35
08 27 05  =1404+286    12 14 31  65.3  88.0 -1.9     -77.8   330     1057   08 21 36

08 27 20  J1350+3034   12 14 46  69.2  84.1 -1.6     -83.4    -1     1057   08 27 21
08 30 00  =1348+308    12 17 26  69.8  84.3 -1.6     -83.6   159     1067   08 27 21

08 30 00  3C293        12 17 26  69.6  81.8 -1.6     -85.8   -10     1067   08 30 10
08 33 30  ---          12 20 57  70.3  81.9 -1.5     -86.1   200     1080   08 30 01

08 34 00  J1350+3034   12 21 27  70.6  84.6 -1.5     -83.8    20     1080   08 34 00
08 35 45  =1348+308    12 23 12  71.0  84.7 -1.5     -83.9   105     1087   08 34 01

08 35 45  3C293        12 23 12  70.8  82.0 -1.5     -86.3   -10     1087   08 35 55
08 39 15  ---          12 26 43  71.5  82.2 -1.4     -86.6   200     1100   08 35 46

08 39 15  J1350+3034   12 26 43  71.8  85.0 -1.4     -84.2   -10     1100   08 39 25
08 41 15  =1348+308    12 28 43  72.2  85.1 -1.4     -84.3   110     1107   08 39 16
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

08 41 15  3C293        12 28 43  72.0  82.2 -1.4     -86.8   -10     1107   08 41 25
08 44 45  ---          12 32 13  72.7  82.4 -1.3     -87.2   200     1120   08 41 16

08 45 15  J1350+3034   12 32 44  73.0  85.4 -1.3     -84.5    20     1120   08 45 15
08 47 00  =1348+308    12 34 29  73.4  85.5 -1.3     -84.6   105     1127   08 45 16

08 47 00  3C293        12 34 29  73.2  82.4 -1.3     -87.4   -10     1127   08 47 10
08 50 30  ---          12 37 59  73.9  82.5 -1.3     -87.7   200     1139   08 47 01

08 50 30  J1350+3034   12 37 59  74.2  85.8 -1.2     -84.8   -10     1139   08 50 40
08 52 30  =1348+308    12 40 00  74.6  85.9 -1.2     -84.9   110     1147   08 50 31

08 52 30  3C293        12 40 00  74.4  82.6 -1.2     -87.9   -10     1147   08 52 40
08 56 00  ---          12 43 30  75.1  82.7 -1.2     -88.3   200     1159   08 52 31

08 56 30  J1350+3034   12 44 00  75.5  86.2 -1.1     -85.2    20     1159   08 56 30
08 58 15  =1348+308    12 45 46  75.8  86.3 -1.1     -85.3   105     1166   08 56 31

08 58 15  3C293        12 45 46  75.6  82.8 -1.1     -88.5   -10     1166   08 58 25
09 01 45  ---          12 49 16  76.3  82.8 -1.1     -88.9   200     1179   08 58 16

09 01 45  J1350+3034   12 49 16  76.6  86.6 -1.0     -85.5   -11     1179   09 01 56
09 03 45  =1348+308    12 51 17  77.0  86.7 -1.0     -85.6   109     1186   09 01 46

09 03 45  3C293        12 51 17  76.8  82.9 -1.0     -89.2   -11     1186   09 03 56
09 07 15  ---          12 54 47  77.5  82.9 -1.0     -89.6   199     1199   09 03 46

09 07 45  J1350+3034   12 55 17  77.9  87.0 -0.9     -85.8    19     1199   09 07 45
09 09 30  =1348+308    12 57 03  78.3  87.2 -0.9     -85.9   105     1206   09 07 46

09 09 30  3C293        12 57 03  78.0  82.9 -0.9     -89.9   -11     1206   09 09 41
09 13 00  ---          13 00 33  78.7  82.9 -0.9     -90.3   199     1219   09 09 31

09 13 00  J1350+3034   13 00 33  79.0  87.4 -0.9     -86.1   -11     1219   09 13 11
09 15 00  =1348+308    13 02 33  79.5  87.6 -0.8     -86.2   109     1226   09 13 01

09 15 00  3C293        13 02 33  79.2  82.9 -0.8     -90.6   -11     1226   09 15 11
09 18 30  ---          13 06 04  79.9  82.8 -0.8     -91.1   199     1238   09 15 01

09 19 00  J1350+3034   13 06 34  80.3  87.9 -0.8     -86.4    19     1238   09 19 00
09 20 45  =1348+308    13 08 19  80.7  88.0 -0.7     -86.4   105     1245   09 19 01

09 21 00  J1407+2827   13 08 34  76.9  96.2 -1.0     -76.5     0     1245   09 21 00
09 26 30  =1404+286    13 14 05  78.1  97.6 -0.9     -75.8   330     1266   09 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

09 26 45  J1350+3034   13 14 20  82.0  88.6 -0.6     -86.7    -1     1266   09 26 46
09 28 45  =1348+308    13 16 21  82.4  88.7 -0.6     -86.8   119     1274   09 26 46

09 28 45  3C293        13 16 21  82.1  82.3 -0.6     -93.0   -12     1274   09 28 57
09 32 11  ---          13 19 47  82.8  82.0 -0.6     -93.7   194     1287   09 28 46

09 32 41  J1350+3034   13 20 17  83.3  89.1 -0.5     -86.9    17     1287   09 32 41
09 34 26  =1348+308    13 22 03  83.6  89.3 -0.5     -86.9   105     1293   09 32 42

09 34 26  3C293        13 22 03  83.3  81.7 -0.5     -94.3   -13     1293   09 34 39
09 37 51  ---          13 25 28  84.1  81.1 -0.5     -95.3   192     1306   09 34 27

09 37 51  J1350+3034   13 25 28  84.4  89.7 -0.4     -87.0   -14     1306   09 38 05
09 39 51  =1348+308    13 27 29  84.8  89.9 -0.4     -87.0   106     1312   09 37 52

09 39 51  3C293        13 27 29  84.5  80.7 -0.4     -96.0   -14     1312   09 40 05
09 43 17  ---          13 30 55  85.2  79.8 -0.4     -97.4   192     1325   09 39 52

09 43 47  J1350+3034   13 31 25  85.7  90.5 -0.3     -87.0    15     1325   09 43 47
09 45 32  =1348+308    13 33 10  86.0  90.7 -0.3     -86.9   105     1332   09 43 48

09 45 32  3C293        13 33 10  85.7  78.9 -0.3     -98.5   -16     1332   09 45 48
09 48 57  ---          13 36 36  86.4  77.2 -0.3    -100.7   189     1344   09 45 33

09 48 57  J1350+3034   13 36 36  86.8  91.4 -0.2     -86.7   -18     1344   09 49 15
09 50 57  =1348+308    13 38 36  87.2  91.9 -0.2     -86.5   102     1350   09 48 58

09 50 57  3C293        13 38 36  86.8  75.7 -0.2    -102.5   -20     1350   09 51 17
09 54 23  ---          13 42 03  87.5  71.9 -0.2    -106.7   186     1362   09 50 58

09 54 53  J1350+3034   13 42 33  88.1  93.3 -0.2     -85.6     7     1362   09 54 53
09 56 38  =1348+308    13 44 18  88.4  94.3 -0.1     -84.7   105     1369   09 54 54

09 56 38  3C293        13 44 18  88.0  67.9 -0.1    -110.9   -27     1369   09 57 05
10 00 03  ---          13 47 44  88.7  56.6 -0.1    -122.7   178     1381   09 56 39

10 00 03  J1350+3034   13 47 44  89.2  98.8 -0.1     -80.7   -39     1381   10 00 42
10 02 03  =1348+308    13 49 44  89.6 108.2 -0.0     -71.6    81     1386   10 00 04

10 02 03  3C293        13 49 44  89.0  43.4 -0.1    -136.2   -60     1386   10 03 03
10 05 29  ---          13 53 11  89.3  -3.1  0.0     176.9   146     1395   10 02 04

10 07 44  3C293        13 55 26  89.1 -35.4  0.0     144.3   122     1395   10 07 44
10 11 09  ---          13 58 52  88.5 -59.4  0.1     119.9   205     1408   10 07 45
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

10 11 09  J1350+3034   13 58 52  88.4 265.7  0.1  W   84.7  -241     1408   10 15 10
10 13 09  =1348+308    14 00 52  88.0 266.8  0.2  W   85.7     0     1401   10 11 10

10 13 09  3C293        14 00 52  88.2 294.0  0.1     113.0   -27     1401   10 13 36
10 16 35  ---          14 04 19  87.5 287.6  0.2     106.1   179     1412   10 13 10

10 17 05  J1350+3034   14 04 49  87.1 268.2  0.2      86.5     8     1412   10 17 05
10 18 50  =1348+308    14 06 34  86.8 268.6  0.2      86.7   105     1419   10 17 06

10 18 50  3C293        14 06 34  87.0 285.0  0.2     103.3   -19     1419   10 19 09
10 22 15  ---          14 09 59  86.3 282.5  0.3     100.3   186     1431   10 18 51

10 22 15  J1350+3034   14 09 59  86.0 269.3  0.3      86.9   -17     1431   10 22 32
10 24 15  =1348+308    14 12 00  85.6 269.6  0.3      87.0   103     1437   10 22 16

10 24 15  3C293        14 12 00  85.9 281.4  0.3      99.0   -16     1437   10 24 31
10 27 45  ---          14 15 30  85.1 280.1  0.4      97.2   194     1450   10 24 16

10 28 15  J1350+3034   14 16 00  84.7 270.1  0.4      87.0    15     1450   10 28 15
10 30 00  =1348+308    14 17 46  84.4 270.3  0.4      87.0   105     1457   10 28 16

10 30 00  3C293        14 17 46  84.6 279.5  0.4      96.3   -14     1457   10 30 14
10 33 30  ---          14 21 16  83.9 278.7  0.5      95.1   196     1469   10 30 01

10 33 30  J1350+3034   14 21 16  83.6 270.7  0.5      86.9   -14     1469   10 33 44
10 35 30  =1348+308    14 23 17  83.2 270.9  0.5      86.9   106     1476   10 33 31

10 35 30  3C293        14 23 17  83.5 278.4  0.5      94.5   -13     1476   10 35 43
10 39 00  ---          14 26 47  82.7 278.0  0.6      93.6   197     1489   10 35 31

10 39 00  J1350+3034   14 26 47  82.4 271.3  0.6      86.8   -13     1489   10 39 13
10 41 00  =1348+308    14 28 48  82.0 271.4  0.6      86.7   107     1496   10 39 01

10 41 00  3C293        14 28 48  82.3 277.8  0.6      93.1   -12     1496   10 41 12
10 44 30  ---          14 32 18  81.5 277.5  0.7      92.4   198     1509   10 41 01

10 44 30  J1350+3034   14 32 18  81.2 271.7  0.7      86.5   -12     1509   10 44 42
10 46 30  =1348+308    14 34 18  80.8 271.9  0.7      86.5   108     1515   10 44 31

10 46 30  3C293        14 34 18  81.1 277.4  0.7      92.1   -12     1515   10 46 42
10 50 00  ---          14 37 49  80.4 277.2  0.7      91.5   198     1528   10 46 31

10 50 00  J1350+3034   14 37 49  80.1 272.2  0.8      86.3   -11     1528   10 50 11
10 52 00  =1348+308    14 39 49  79.6 272.4  0.8      86.2   109     1535   10 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

10 52 00  3C293        14 39 49  79.9 277.2  0.8      91.1   -11     1535   10 52 11
10 55 30  ---          14 43 20  79.2 277.1  0.8      90.6   199     1548   10 52 01

10 55 30  J1350+3034   14 43 20  78.9 272.6  0.9      86.0   -11     1548   10 55 41
10 57 30  =1348+308    14 45 20  78.4 272.8  0.9      85.9   109     1555   10 55 31

10 57 30  3C293        14 45 20  78.8 277.1  0.9      90.3   -11     1555   10 57 41
11 01 00  ---          14 48 51  78.0 277.1  0.9      89.9   199     1568   10 57 31

11 01 00  J1350+3034   14 48 51  77.7 273.0  1.0      85.7   -11     1568   11 01 11
11 03 00  =1348+308    14 50 51  77.2 273.2  1.0      85.6   109     1575   11 01 01

11 03 15  J1407+2827   14 51 06  80.3 259.3  0.7      73.9    -3     1575   11 03 18
11 08 15  =1404+286    14 56 07  79.2 260.9  0.8      75.0   297     1594   11 03 16

11 08 30  J1350+3034   14 56 22  76.1 273.6  1.1      85.3    -2     1594   11 08 32
11 10 30  =1348+308    14 58 22  75.6 273.7  1.1      85.2   118     1602   11 08 31

11 10 30  3C293        14 58 22  76.0 277.2  1.1      88.7   -10     1602   11 10 40
11 14 00  ---          15 01 53  75.2 277.3  1.1      88.4   200     1615   11 10 31

11 14 00  J1350+3034   15 01 53  74.9 274.0  1.2      85.0   -10     1615   11 14 10
11 16 00  =1348+308    15 03 53  74.5 274.1  1.2      84.9   110     1622   11 14 01

11 16 00  3C293        15 03 53  74.8 277.3  1.2      88.2   -10     1622   11 16 10
11 19 30  ---          15 07 24  74.1 277.4  1.2      87.8   200     1635   11 16 01

11 19 30  J1350+3034   15 07 24  73.7 274.4  1.3      84.7   -10     1635   11 19 40
11 21 30  =1348+308    15 09 24  73.3 274.5  1.3      84.6   110     1642   11 19 31

11 21 30  3C293        15 09 24  73.6 277.5  1.3      87.6   -10     1642   11 21 40
11 25 00  ---          15 12 55  72.9 277.6  1.3      87.2   200     1654   11 21 31

11 25 00  J1350+3034   15 12 55  72.5 274.8  1.4      84.4   -10     1654   11 25 10
11 27 00  =1348+308    15 14 55  72.1 274.9  1.4      84.2   110     1662   11 25 01

11 27 00  3C293        15 14 55  72.5 277.7  1.4      87.1   -10     1662   11 27 10
11 30 30  ---          15 18 26  71.7 277.8  1.4      86.7   200     1674   11 27 01

11 30 30  J1350+3034   15 18 26  71.3 275.2  1.4      84.0   -10     1674   11 30 40
11 32 30  =1348+308    15 20 26  70.9 275.3  1.5      83.9   110     1682   11 30 31

11 32 30  3C293        15 20 26  71.3 277.9  1.5      86.5   -10     1682   11 32 40
11 36 00  ---          15 23 57  70.5 278.0  1.5      86.2   200     1694   11 32 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

11 36 00  J1350+3034   15 23 57  70.2 275.6  1.5      83.7   -10     1694   11 36 10
11 38 00  =1348+308    15 25 57  69.7 275.7  1.6      83.6   110     1702   11 36 01

11 38 00  3C293        15 25 57  70.1 278.1  1.5      86.0   -10     1702   11 38 10
11 41 30  ---          15 29 27  69.4 278.3  1.6      85.7   200     1714   11 38 01

11 41 30  J1350+3034   15 29 27  69.0 275.9  1.6      83.4   -10     1714   11 41 40
11 43 30  =1348+308    15 31 28  68.5 276.1  1.7      83.2   110     1721   11 41 31

11 43 30  3C293        15 31 28  68.9 278.4  1.6      85.5    -9     1721   11 43 39
11 47 00  ---          15 34 58  68.2 278.5  1.7      85.2   201     1734   11 43 31

11 47 00  J1350+3034   15 34 58  67.8 276.3  1.7      83.0    -9     1734   11 47 09
11 49 00  =1348+308    15 36 59  67.4 276.5  1.8      82.9   111     1742   11 47 01

11 49 00  3C293        15 36 59  67.8 278.6  1.7      85.1    -9     1742   11 49 09
11 52 30  ---          15 40 29  67.0 278.8  1.8      84.8   201     1755   11 49 01

11 52 30  J1350+3034   15 40 29  66.6 276.7  1.8      82.7    -9     1755   11 52 39
11 54 30  =1348+308    15 42 30  66.2 276.8  1.8      82.5   111     1762   11 52 31

11 54 30  3C293        15 42 30  66.6 278.9  1.8      84.6    -9     1762   11 54 39
11 58 00  ---          15 46 00  65.8 279.1  1.9      84.3   201     1775   11 54 31

11 58 00  J1350+3034   15 46 00  65.4 277.1  1.9      82.3    -9     1775   11 58 09
12 00 00  =1348+308    15 48 01  65.0 277.2  1.9      82.2   111     1782   11 58 01

12 00 00  3C293        15 48 01  65.4 279.2  1.9      84.1    -9     1782   12 00 09
12 03 30  ---          15 51 31  64.7 279.4  2.0      83.9   201     1795   12 00 01

12 03 30  J1350+3034   15 51 31  64.3 277.5  2.0      82.0    -9     1795   12 03 39
12 05 30  =1348+308    15 53 31  63.8 277.6  2.0      81.8   111     1802   12 03 31

12 05 30  3C293        15 53 31  64.2 279.5  2.0      83.7    -9     1802   12 05 39
12 09 00  ---          15 57 02  63.5 279.7  2.1      83.4   201     1815   12 05 31

12 09 00  J1350+3034   15 57 02  63.1 277.9  2.1      81.6    -9     1815   12 09 09
12 11 00  =1348+308    15 59 02  62.7 278.0  2.1      81.5   111     1822   12 09 01

12 11 00  3C293        15 59 02  63.1 279.8  2.1      83.2    -9     1822   12 11 09
12 14 30  ---          16 02 33  62.3 280.0  2.2      83.0   201     1835   12 11 01

12 14 30  J1350+3034   16 02 33  61.9 278.2  2.2      81.2    -9     1835   12 14 39
12 16 30  =1348+308    16 04 33  61.5 278.4  2.2      81.1   111     1842   12 14 31
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

12 16 30  3C293        16 04 33  61.9 280.1  2.2      82.8    -9     1842   12 16 39
12 20 00  ---          16 08 04  61.2 280.3  2.3      82.5   201     1855   12 16 31

12 20 00  J1350+3034   16 08 04  60.7 278.6  2.3      80.9    -9     1855   12 20 09
12 22 00  =1348+308    16 10 04  60.3 278.8  2.3      80.7   111     1862   12 20 01

12 22 00  3C293        16 10 04  60.7 280.4  2.3      82.4    -9     1862   12 22 09
12 25 30  ---          16 13 35  60.0 280.6  2.3      82.1   201     1875   12 22 01

12 25 30  J1350+3034   16 13 35  59.6 279.0  2.4      80.5    -9     1875   12 25 39
12 27 30  =1348+308    16 15 35  59.1 279.1  2.4      80.4   111     1882   12 25 31

12 27 30  3C293        16 15 35  59.6 280.7  2.4      81.9    -9     1882   12 27 39
12 31 00  ---          16 19 06  58.8 280.9  2.4      81.6   201     1895   12 27 31

12 31 00  J1350+3034   16 19 06  58.4 279.4  2.5      80.1    -9     1895   12 31 09
12 33 00  =1348+308    16 21 06  58.0 279.5  2.5      80.0   111     1902   12 31 01

12 33 15  J1407+2827   16 21 21  60.9 274.1  2.2      77.3     1     1902   12 33 15
12 38 15  =1404+286    16 26 22  59.9 274.6  2.3      77.1   300     1922   12 33 16

12 38 30  J1350+3034   16 26 37  56.8 279.9  2.6      79.6     1     1922   12 38 30
12 40 30  =1348+308    16 28 37  56.4 280.1  2.6      79.5   120     1929   12 38 31

12 40 30  3C293        16 28 37  56.8 281.5  2.6      80.9    -9     1929   12 40 39
12 44 00  ---          16 32 08  56.1 281.7  2.7      80.6   201     1942   12 40 31

12 44 00  J1350+3034   16 32 08  55.6 280.3  2.7      79.3    -9     1942   12 44 09
12 46 00  =1348+308    16 34 08  55.2 280.5  2.7      79.1   111     1949   12 44 01

12 46 00  3C293        16 34 08  55.7 281.9  2.7      80.5    -9     1949   12 46 09
12 49 30  ---          16 37 39  54.9 282.1  2.7      80.2   201     1962   12 46 01

12 49 30  J1350+3034   16 37 39  54.5 280.7  2.8      78.9    -9     1962   12 49 39
12 51 30  =1348+308    16 39 39  54.0 280.9  2.8      78.7   111     1970   12 49 31

12 51 30  3C293        16 39 39  54.5 282.2  2.8      80.0    -9     1970   12 51 39
12 55 00  ---          16 43 10  53.8 282.4  2.8      79.8   201     1983   12 51 31

12 55 00  J1350+3034   16 43 10  53.3 281.1  2.9      78.5    -9     1983   12 55 09
12 57 00  =1348+308    16 45 10  52.9 281.2  2.9      78.4   111     1990   12 55 01

12 57 00  3C293        16 45 10  53.3 282.6  2.9      79.6    -9     1990   12 57 09
13 00 30  ---          16 48 40  52.6 282.8  2.9      79.3   201     2003   12 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

13 00 30  J1350+3034   16 48 40  52.1 281.5  3.0      78.1    -9     2003   13 00 39
13 02 30  =1348+308    16 50 41  51.7 281.6  3.0      78.0   111     2010   13 00 31

13 02 30  3C293        16 50 41  52.2 282.9  3.0      79.2    -9     2010   13 02 39
13 06 00  ---          16 54 11  51.4 283.2  3.0      78.9   201     2023   13 02 31

13 06 00  J1350+3034   16 54 11  51.0 281.9  3.0      77.7    -9     2023   13 06 09
13 08 00  =1348+308    16 56 12  50.6 282.0  3.1      77.6   111     2030   13 06 01

13 08 00  3C293        16 56 12  51.0 283.3  3.1      78.7    -9     2030   13 08 09
13 11 30  ---          16 59 42  50.3 283.5  3.1      78.5   201     2043   13 08 01

13 11 30  J1350+3034   16 59 42  49.8 282.3  3.1      77.3    -9     2043   13 11 39
13 13 30  =1348+308    17 01 43  49.4 282.5  3.2      77.2   111     2050   13 11 31

13 13 30  3C293        17 01 43  49.9 283.7  3.1      78.3    -9     2050   13 13 39
13 17 00  ---          17 05 13  49.1 283.9  3.2      78.0   201     2063   13 13 31

13 17 00  J1350+3034   17 05 13  48.7 282.7  3.2      77.0    -9     2063   13 17 09
13 19 00  =1348+308    17 07 14  48.2 282.9  3.3      76.8   111     2070   13 17 01

13 19 00  3C293        17 07 14  48.7 284.0  3.2      77.9    -9     2070   13 19 09
13 22 30  ---          17 10 44  48.0 284.3  3.3      77.6   201     2083   13 19 01

13 22 30  J1350+3034   17 10 44  47.5 283.1  3.3      76.6    -9     2083   13 22 39
13 24 30  =1348+308    17 12 44  47.1 283.3  3.4      76.4   111     2090   13 22 31

13 24 30  3C293        17 12 44  47.6 284.4  3.3      77.4    -9     2090   13 24 39
13 28 00  ---          17 16 15  46.8 284.6  3.4      77.2   201     2103   13 24 31

13 28 00  J1350+3034   17 16 15  46.3 283.5  3.4      76.2    -9     2103   13 28 09
13 30 00  =1348+308    17 18 15  45.9 283.7  3.4      76.0   111     2110   13 28 01

13 30 00  3C293        17 18 15  46.4 284.8  3.4      77.0    -9     2110   13 30 09
13 33 30  ---          17 21 46  45.7 285.0  3.5      76.7   201     2123   13 30 01

13 33 30  J1350+3034   17 21 46  45.2 283.9  3.5      75.8    -9     2123   13 33 39
13 35 30  =1348+308    17 23 46  44.8 284.1  3.5      75.6   111     2130   13 33 31

13 35 30  3C293        17 23 46  45.3 285.2  3.5      76.6    -9     2130   13 35 39
13 39 00  ---          17 27 17  44.5 285.4  3.6      76.3   201     2143   13 35 31

13 39 00  J1350+3034   17 27 17  44.0 284.4  3.6      75.3    -9     2143   13 39 09
13 41 00  =1348+308    17 29 17  43.6 284.5  3.6      75.2   111     2150   13 39 01
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

13 41 00  3C293        17 29 17  44.1 285.6  3.6      76.1    -9     2150   13 41 09
13 44 30  ---          17 32 48  43.4 285.8  3.7      75.8   201     2163   13 41 01

13 44 30  J1350+3034   17 32 48  42.9 284.8  3.7      74.9    -9     2163   13 44 39
13 46 30  =1348+308    17 34 48  42.5 284.9  3.7      74.8   111     2171   13 44 31

13 46 30  3C293        17 34 48  43.0 286.0  3.7      75.7    -9     2171   13 46 39
13 50 00  ---          17 38 19  42.3 286.2  3.8      75.4   201     2183   13 46 31

13 50 00  J1350+3034   17 38 19  41.7 285.2  3.8      74.5    -9     2183   13 50 09
13 52 00  =1348+308    17 40 19  41.3 285.4  3.8      74.4   111     2191   13 50 01

13 52 00  3C293        17 40 19  41.9 286.4  3.8      75.2    -9     2191   13 52 09
13 55 30  ---          17 43 50  41.1 286.6  3.8      74.9   201     2204   13 52 01

13 55 30  J1350+3034   17 43 50  40.6 285.6  3.9      74.1    -9     2204   13 55 39
13 57 30  =1348+308    17 45 50  40.2 285.8  3.9      73.9   111     2211   13 55 31

13 57 30  3C293        17 45 50  40.7 286.8  3.9      74.8    -9     2211   13 57 39
14 01 00  ---          17 49 20  40.0 287.0  3.9      74.5   201     2224   13 57 31

14 01 00  J1350+3034   17 49 20  39.5 286.1  4.0      73.7    -9     2224   14 01 09
14 03 00  =1348+308    17 51 21  39.0 286.2  4.0      73.5   111     2231   14 01 01

14 03 15  J1407+2827   17 51 36  41.7 282.2  3.7      72.9     2     2231   14 03 15
14 08 15  =1404+286    17 56 37  40.7 282.7  3.8      72.6   300     2250   14 03 16

14 08 30  J1350+3034   17 56 52  37.9 286.6  4.1      73.1     2     2250   14 08 30
14 10 30  =1348+308    17 58 52  37.5 286.8  4.1      72.9   120     2258   14 08 31

14 10 30  3C293        17 58 52  38.0 287.7  4.1      73.7    -9     2258   14 10 39
14 14 00  ---          18 02 23  37.3 288.0  4.2      73.4   201     2271   14 10 31

14 14 00  J1350+3034   18 02 23  36.8 287.1  4.2      72.7    -9     2271   14 14 09
14 16 00  =1348+308    18 04 23  36.4 287.3  4.2      72.5   111     2278   14 14 01

14 16 00  3C293        18 04 23  36.9 288.2  4.2      73.2    -9     2278   14 16 09
14 19 30  ---          18 07 53  36.2 288.4  4.2      72.9   201     2291   14 16 01

14 19 30  J1350+3034   18 07 53  35.6 287.5  4.3      72.2    -9     2291   14 19 39
14 21 30  =1348+308    18 09 54  35.2 287.7  4.3      72.1   111     2298   14 19 31

14 21 30  3C293        18 09 54  35.8 288.6  4.3      72.8    -9     2298   14 21 39
14 25 00  ---          18 13 24  35.1 288.9  4.3      72.5   201     2311   14 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

14 25 00  J1350+3034   18 13 24  34.5 288.0  4.4      71.8    -9     2311   14 25 09
14 27 00  =1348+308    18 15 25  34.1 288.1  4.4      71.6   111     2318   14 25 01

14 27 00  3C293        18 15 25  34.7 289.0  4.4      72.3    -9     2318   14 27 09
14 30 30  ---          18 18 55  33.9 289.3  4.4      72.0   201     2331   14 27 01

14 30 30  J1350+3034   18 18 55  33.4 288.4  4.5      71.3    -9     2331   14 30 39
14 32 30  =1348+308    18 20 56  33.0 288.6  4.5      71.2   111     2338   14 30 31

14 32 30  3C293        18 20 56  33.5 289.5  4.5      71.8    -9     2338   14 32 39
14 36 00  ---          18 24 26  32.8 289.7  4.5      71.5   201     2351   14 32 31

14 36 00  J1350+3034   18 24 26  32.3 288.9  4.5      70.9    -9     2351   14 36 09
14 38 00  =1348+308    18 26 26  31.9 289.1  4.6      70.7   111     2358   14 36 01

14 38 00  3C293        18 26 26  32.4 289.9  4.6      71.4    -9     2358   14 38 09
14 41 30  ---          18 29 57  31.7 290.2  4.6      71.0   201     2371   14 38 01

14 41 30  J1350+3034   18 29 57  31.1 289.4  4.6      70.4    -9     2371   14 41 39
14 43 30  =1348+308    18 31 57  30.7 289.5  4.7      70.3   111     2378   14 41 31

14 43 30  3C293        18 31 57  31.3 290.4  4.6      70.9    -9     2378   14 43 39
14 47 00  ---          18 35 28  30.6 290.6  4.7      70.6   201     2391   14 43 31

14 47 00  J1350+3034   18 35 28  30.0 289.8  4.7      70.0    -9     2391   14 47 09
14 49 00  =1348+308    18 37 28  29.6 290.0  4.8      69.8   111     2399   14 47 01

14 49 00  3C293        18 37 28  30.2 290.8  4.7      70.4    -9     2399   14 49 09
14 52 30  ---          18 40 59  29.5 291.1  4.8      70.1   201     2411   14 49 01

14 52 30  J1350+3034   18 40 59  28.9 290.3  4.8      69.5    -9     2411   14 52 39
14 54 30  =1348+308    18 42 59  28.5 290.5  4.9      69.3   111     2419   14 52 31

14 54 30  3C293        18 42 59  29.1 291.3  4.8      69.9    -9     2419   14 54 39
14 58 00  ---          18 46 30  28.4 291.6  4.9      69.6   201     2432   14 54 31

14 58 00  J1350+3034   18 46 30  27.8 290.8  4.9      69.0    -9     2432   14 58 09
15 00 00  =1348+308    18 48 30  27.4 290.9  4.9      68.8   111     2439   14 58 01

15 00 00  3C293        18 48 30  28.0 291.7  4.9      69.4    -9     2439   15 00 09
15 03 30  ---          18 52 01  27.3 292.0  5.0      69.1   201     2452   15 00 01

15 03 30  J1350+3034   18 52 01  26.7 291.3  5.0      68.5    -9     2452   15 03 39
15 05 30  =1348+308    18 54 01  26.3 291.4  5.0      68.4   111     2459   15 03 31
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

15 05 30  3C293        18 54 01  26.9 292.2  5.0      68.9    -9     2459   15 05 39
15 09 00  ---          18 57 32  26.2 292.5  5.1      68.6   201     2472   15 05 31

15 09 00  J1350+3034   18 57 32  25.6 291.7  5.1      68.1    -9     2472   15 09 09
15 11 00  =1348+308    18 59 32  25.2 291.9  5.1      67.9   111     2479   15 09 01

15 11 00  3C293        18 59 32  25.8 292.7  5.1      68.4    -9     2479   15 11 09
15 14 30  ---          19 03 02  25.1 293.0  5.2      68.1   201     2492   15 11 01

15 14 30  J1350+3034   19 03 02  24.5 292.2  5.2      67.6    -9     2492   15 14 39
15 16 30  =1348+308    19 05 03  24.1 292.4  5.2      67.4   111     2499   15 14 31

15 16 30  3C293        19 05 03  24.7 293.2  5.2      67.9    -9     2499   15 16 39
15 20 00  ---          19 08 33  24.0 293.5  5.3      67.6   201     2512   15 16 31

15 20 00  J1350+3034   19 08 33  23.4 292.7  5.3      67.1    -9     2512   15 20 09
15 22 00  =1348+308    19 10 34  23.0 292.9  5.3      66.9   111     2519   15 20 01

15 22 00  3C293        19 10 34  23.6 293.7  5.3      67.4    -9     2519   15 22 09
15 25 30  ---          19 14 04  22.9 294.0  5.4      67.0   201     2532   15 22 01

15 25 30  J1350+3034   19 14 04  22.3 293.2  5.4      66.6    -9     2532   15 25 39
15 27 30  =1348+308    19 16 05  21.9 293.4  5.4      66.4   111     2539   15 25 31

15 27 30  3C293        19 16 05  22.5 294.2  5.4      66.8    -9     2539   15 27 39
15 31 00  ---          19 19 35  21.8 294.5  5.4      66.5   201     2552   15 27 31

15 31 00  J1350+3034   19 19 35  21.2 293.8  5.5      66.1    -9     2552   15 31 09
15 33 00  =1348+308    19 21 36  20.8 294.0  5.5      65.9   111     2559   15 31 01

15 33 15  J1407+2827   19 21 51  23.1 290.4  5.2      66.5     2     2559   15 33 15
15 38 15  =1404+286    19 26 51  22.1 290.8  5.3      66.1   300     2579   15 33 16

15 38 30  J1350+3034   19 27 06  19.7 294.5  5.6      65.4     2     2579   15 38 30
15 40 30  =1348+308    19 29 07  19.3 294.7  5.6      65.2   120     2586   15 38 31

15 40 30  3C293        19 29 07  20.0 295.4  5.6      65.6    -9     2586   15 40 39
15 44 00  ---          19 32 37  19.3 295.7  5.7      65.2   201     2599   15 40 31

15 44 00  J1350+3034   19 32 37  18.7 295.0  5.7      64.8    -9     2599   15 44 09
15 46 00  =1348+308    19 34 38  18.3 295.2  5.7      64.6   111     2606   15 44 01

15 46 00  3C293        19 34 38  18.9 295.9  5.7      65.0    -9     2606   15 46 09
15 49 30  ---          19 38 08  18.2 296.2  5.8      64.7   201     2619   15 46 01
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               Tracing the Evolution of Fast Jet-Driven Outflows
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   3 Mar 2015   Day  62 ---

15 49 30  J1350+3034   19 38 08  17.6 295.5  5.8      64.3    -9     2619   15 49 39
15 51 30  =1348+308    19 40 09  17.2 295.7  5.8      64.1   111     2627   15 49 31

15 51 30  3C293        19 40 09  17.8 296.4  5.8      64.5    -9     2627   15 51 39
15 55 00  ---          19 43 39  17.2 296.8  5.8      64.1   201     2640   15 51 31

15 55 00  J1350+3034   19 43 39  16.5 296.1  5.9      63.8    -9     2640   15 55 09
15 57 00  =1348+308    19 45 39  16.1 296.3  5.9      63.6   111     2647   15 55 01

15 57 00  3C293        19 45 39  16.8 297.0  5.9      63.9    -9     2647   15 57 09
16 00 30  ---          19 49 10  16.1 297.3  5.9      63.6   201     2660   15 57 01

16 00 30  J1350+3034   19 49 10  15.5 296.6  6.0      63.2    -9     2660   16 00 39
16 02 30  =1348+308    19 51 10  15.1 296.8  6.0      63.0   111     2667   16 00 31

16 02 30  3C293        19 51 10  15.7 297.5  6.0      63.4    -9     2667   16 02 39
16 06 00  ---          19 54 41  15.1 297.8  6.0      63.0   201     2680   16 02 31

16 06 00  J1350+3034   19 54 41  14.4 297.2  6.1      62.7    -9     2680   16 06 09
16 08 00  =1348+308    19 56 41  14.0 297.4  6.1      62.4   111     2687   16 06 01

16 08 00  3C293        19 56 41  14.7 298.1  6.1      62.8    -9     2687   16 08 09
16 11 30  ---          20 00 12  14.0 298.4  6.1      62.4   201     2700   16 08 01

16 11 30  J1350+3034   20 00 12  13.3 297.8  6.1      62.1    -9     2700   16 11 39
16 13 30  =1348+308    20 02 12  13.0 298.0  6.2      61.9   111     2707   16 11 31

16 13 30  3C293        20 02 12  13.6 298.6  6.2      62.2    -9     2707   16 13 39
16 17 00  ---          20 05 43  13.0 299.0  6.2      61.8   201     2720   16 13 31

16 17 00  J1350+3034   20 05 43  12.3 298.3  6.2      61.5    -9     2720   16 17 09
16 19 00  =1348+308    20 07 43  11.9 298.6  6.3      61.3   111     2727   16 17 01

16 19 00  3C293        20 07 43  12.6 299.2  6.2      61.6    -9     2727   16 19 09
16 22 30  ---          20 11 14  11.9 299.5  6.3      61.2   201     2740   16 19 01

16 22 30  J1350+3034   20 11 14  11.3 298.9  6.3      60.9    -9     2740   16 22 39
16 24 30  =1348+308    20 13 14  10.9 299.1  6.4      60.7   111     2747   16 22 31

16 24 30  3C293        20 13 14  11.6 299.8  6.3      61.0    -9     2747   16 24 39
16 28 00  ---          20 16 45  10.9 300.1  6.4      60.6   201     2760   16 24 31

16 28 00  J1350+3034   20 16 45  10.2 299.5  6.4      60.3    -9     2760   16 28 09
16 30 00  =1348+308    20 18 45   9.8 299.7  6.5      60.1   111     2767   16 28 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: 3C293globHI.set
   Matching groups in /home/guest/rmc/SCHED/sched11.3u1/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         L         L         L         L         L         L         L         L
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.1      2.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

  Frequency Set:   8  Based on FREQ, BW, and/or DOPPLER in schedule.  Used with PCAL = off
   LO sum=   1364.50  1364.50  1379.75  1379.75  1395.00  1395.00  1410.25  1410.25
   BBC fr=    735.50   735.50   720.25   720.25   705.00   705.00   689.75   689.75
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     720.25    720.25    705.00    705.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   8   9  10  11  12  13  14  15  16  18

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 3C293             13 50 03.134041   * 13 52 17.765000     13 52 59.488926       0.00
                     31 41 32.42285    * 31 26 46.10000      31 22 06.46058        0.00
                     From catalog imbedded in main SCHED input file.
                     target
                     Doppler based on heliocentric frame and radio definition.  Velocities:
                      13500.00 13500.00 13500.00 13500.00 13500.00 13500.00 13500.00 13500.00

 * J1350+3034        13 48 37.245632   * 13 50 52.736222     13 51 34.730633       0.13
   1348+308          30 49 42.80390    * 30 34 53.59050      30 30 13.18355        0.11
   J1350+30          /home/guest/rmc/SCHED/sched11.3u1/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 722 observations
                     Doppler based on other sources.

 * J1407+2827        14 04 45.615156   * 14 07 00.394414     14 07 42.118209       0.24
   1404+286          28 41 29.23519    * 28 27 14.69022      28 22 45.41879        0.34
   J1407+28          /home/guest/rmc/SCHED/sched11.3u1/catalogs/sources.vlba
   OQ208             GSFC 2011B astro solution     66461 Observations
                     Doppler based on other sources.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  3C293      3C293globHI.set       1 2 3 4 5 6 7 8 17               10.878   649.233
  J1350+3034 3C293globHI.set       1 2 3 4 5 6 7 8 17                6.361   359.330
  J1407+2827 3C293globHI.set       1 2 3 4 5 6 7 8 17                1.067    75.055


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   3C293              131.9
   J1350+3034         132.4
   J1407+2827         129.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

