  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg081c  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band,Q-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   7 Mar 2017   Day  66 ---

 ---------- K-band VLBI scans. Space segment 03: Target down, observing calibrator with rest of VLBA ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

21 00 00  0716+714     01 07 17  27.6  21.1 -6.3     -75.5     0        0   21 00 00
21 10 00  ---          01 17 19  28.3  21.3 -6.1     -77.8   600       77   20 59 50

 ---------- K-band  VLBI scans.  Ground segment 03: target source  with EVN+VLBA+HH ----------

21 10 30  0716+714     01 17 49  28.4  21.4 -6.1     -77.9    24       77   21 10 19
21 18 30  ---          01 25 50  29.0  21.5 -6.0     -79.7   480      141   21 10 20

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

21 18 30  0716+714     01 25 50  29.0  21.5 -6.0     -79.7    -6      141   21 18 36
21 26 00  ---          01 33 22  29.6  21.6 -5.8     -81.4   444      198   21 18 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

21 26 30  0716+714     01 33 52  29.7  21.6 -5.8     -81.6    24      198   21 26 19
21 32 00  ---          01 39 23  30.1  21.7 -5.7     -82.8   330      242   21 26 20

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

21 32 30  0716+714     01 39 53  30.1  21.7 -5.7     -82.9    24      242   21 32 19
21 40 00  ---          01 47 24  30.7  21.8 -5.6     -84.7   450      301   21 32 20

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

21 40 30  0716+714     01 47 54  30.8  21.8 -5.6     -84.8    24      301   21 40 19
21 46 00  ---          01 53 25  31.2  21.8 -5.5     -86.1   330      345   21 40 20

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

21 46 30  0716+714     01 53 55  31.3  21.8 -5.5     -86.2    24      345   21 46 19
21 54 00  ---          02 01 26  31.9  21.8 -5.4     -88.0   450      404   21 46 20

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

21 54 30  0716+714     02 01 56  31.9  21.9 -5.4     -88.1    24      404   21 54 19
22 00 00  ---          02 07 27  32.3  21.9 -5.3     -89.4   330      448   21 54 20
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   7 Mar 2017   Day  66 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

22 09 00  0851+202     02 16 29   2.1  67.9 -6.7  D  -58.0   473      448   22 08 49
22 18 30  ---          02 26 00   4.0  69.0 -6.5  H  -58.8     0      523   22 08 50

22 19 00  0851+202     02 26 30   4.1  69.1 -6.5  H  -58.8    24      523   22 18 49
22 28 30  ---          02 36 02   6.0  70.2 -6.3     -59.5     0      598   22 18 50

22 29 00  0851+202     02 36 32   6.1  70.3 -6.3     -59.6    24      598   22 28 49
22 38 30  ---          02 46 04   8.1  71.4 -6.2     -60.3   570      673   22 28 50

22 39 00  0851+202     02 46 34   8.2  71.5 -6.2     -60.3    24      673   22 38 49
22 48 30  ---          02 56 05  10.1  72.6 -6.0     -60.9   570      748   22 38 50

22 49 00  0851+202     02 56 35  10.2  72.7 -6.0     -61.0    24      748   22 48 49
22 58 30  ---          03 06 07  12.2  73.8 -5.8     -61.6   570      823   22 48 50

22 59 00  0851+202     03 06 37  12.3  73.8 -5.8     -61.6    24      823   22 58 49
23 08 30  ---          03 16 09  14.3  74.9 -5.7     -62.2   570      897   22 58 50

23 09 00  0851+202     03 16 39  14.4  75.0 -5.7     -62.2    24      897   23 08 49
23 18 30  ---          03 26 10  16.3  76.0 -5.5     -62.7   570      972   23 08 50

23 19 00  0851+202     03 26 40  16.4  76.1 -5.5     -62.8    24      972   23 18 49
23 28 30  ---          03 36 12  18.4  77.2 -5.3     -63.2   570     1047   23 18 50

23 28 30  0851+202     03 36 12  18.4  77.2 -5.3     -63.2    -6     1047   23 28 36
23 30 00  ---          03 37 42  18.8  77.3 -5.3     -63.3    84     1058   23 28 31

23 30 30  0851+202     03 38 12  18.9  77.4 -5.3     -63.3    24     1058   23 30 19
23 38 30  ---          03 46 13  20.5  78.3 -5.2     -63.7   480     1121   23 30 20

23 39 00  0851+202     03 46 44  20.7  78.3 -5.2     -63.8    24     1121   23 38 49
23 44 30  ---          03 52 14  21.8  78.9 -5.1     -64.0   330     1165   23 38 50

 ---------- K-band VLBI scans. Space segment 04: 0851+202 with EVN ----------

23 45 00  0851+202     03 52 45  21.9  79.0 -5.1     -64.0    24     1165   23 44 49
23 55 00  ---          04 02 46  24.0  80.1 -4.9     -64.5   600     1244   23 44 50

 --- Start: Tue   7 Mar 2017   Day  66 -- Stop: Wed   8 Mar 2017   Day  67 ---

23 55 30  0851+202     04 03 16  24.2  80.2 -4.9     -64.5    24     1244   23 55 19
00 05 00  ---          04 12 48  26.2  81.2 -4.7     -64.8   570     1319   23 55 20
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

00 05 30  0851+202     04 13 18  26.3  81.3 -4.7     -64.9    24     1319   00 05 19
00 15 00  ---          04 22 49  28.3  82.3 -4.5     -65.2   570     1393   00 05 20

00 15 30  0851+202     04 23 20  28.4  82.4 -4.5     -65.2    24     1393   00 15 19
00 16 30  ---          04 24 20  28.6  82.5 -4.5     -65.2    60     1403   00 15 20

00 16 40  0851+202     04 24 30  28.7  82.5 -4.5     -65.2     4     1403   00 16 36
00 25 00  ---          04 32 51  30.4  83.5 -4.4     -65.5   500     1468   00 16 31

00 25 30  0851+202     04 33 21  30.6  83.5 -4.4     -65.5    24     1468   00 25 19
00 26 30  ---          04 34 21  30.8  83.6 -4.4     -65.5    60     1477   00 25 20

00 26 40  0851+202     04 34 31  30.8  83.7 -4.4     -65.5     4     1477   00 26 36
00 35 00  ---          04 42 53  32.6  84.6 -4.2     -65.8   500     1542   00 26 31

00 35 30  0851+202     04 43 23  32.7  84.7 -4.2     -65.8    24     1542   00 35 19
00 36 30  ---          04 44 23  32.9  84.8 -4.2     -65.8    60     1551   00 35 20

00 36 40  0851+202     04 44 33  33.0  84.8 -4.2     -65.8     4     1551   00 36 36
00 45 00  ---          04 52 54  34.7  85.8 -4.0     -66.0   500     1616   00 36 31

 ---------- K-band  VLBI scans.  Ground segment 04: target source  with EVN+VLBA+GBT ----------

00 45 30  0851+202     04 53 24  34.9  85.8 -4.0     -66.0    24     1616   00 45 19
00 46 30  ---          04 54 25  35.1  85.9 -4.0     -66.0    60     1625   00 45 20

00 46 40  0851+202     04 54 35  35.1  86.0 -4.0     -66.0     4     1625   00 46 36
00 57 00  ---          05 04 56  37.3  87.2 -3.8     -66.2   620     1705   00 46 31

 ---------- Ground-only VLBA+Ef U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

00 58 00  0851+202     05 05 57  37.5  87.3 -3.8     -66.2    54     1705   00 57 49
01 06 00  ---          05 13 58  39.3  88.3 -3.7     -66.3   480     1768   00 57 50

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

01 07 00  0851+202     05 14 58  39.5  88.4 -3.7     -66.3    54     1768   01 06 49
01 08 00  ---          05 15 58  39.7  88.5 -3.7     -66.3    60     1778   01 06 50

01 08 10  0851+202     05 16 08  39.7  88.5 -3.7     -66.3     4     1778   01 08 06
01 17 00  ---          05 25 00  41.6  89.6 -3.5     -66.3   530     1846   01 08 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 18 00  0851+202     05 26 00  41.9  89.8 -3.5     -66.3    54     1846   01 17 49
01 19 00  ---          05 27 00  42.1  89.9 -3.5     -66.3    60     1856   01 17 50

01 19 10  0851+202     05 27 10  42.1  89.9 -3.5     -66.3     4     1856   01 19 06
01 26 10  ---          05 34 11  43.6  90.8 -3.4     -66.3   420     1910   01 19 01

01 26 40  0851+202     05 34 41  43.7  90.9 -3.4     -66.3    24     1910   01 26 29
01 27 40  ---          05 35 41  43.9  91.0 -3.3     -66.3    60     1919   01 26 30

01 27 50  0851+202     05 35 51  44.0  91.0 -3.3     -66.3     4     1919   01 27 46
01 36 10  ---          05 44 13  45.8  92.1 -3.2     -66.2   500     1984   01 27 41

01 36 40  0851+202     05 44 43  45.9  92.2 -3.2     -66.2    24     1984   01 36 29
01 37 40  ---          05 45 43  46.1  92.3 -3.2     -66.2    60     1993   01 36 30

01 37 50  0851+202     05 45 53  46.1  92.4 -3.2     -66.2     4     1993   01 37 46
01 46 10  ---          05 54 14  47.9  93.5 -3.0     -66.1   500     2058   01 37 41

01 46 40  0851+202     05 54 45  48.0  93.6 -3.0     -66.1    24     2058   01 46 29
01 47 40  ---          05 55 45  48.2  93.8 -3.0     -66.1    60     2067   01 46 30

01 47 50  0851+202     05 55 55  48.3  93.8 -3.0     -66.0     4     2067   01 47 46
01 56 10  ---          06 04 16  50.1  95.0 -2.9     -65.8   500     2132   01 47 41

01 56 40  0851+202     06 04 46  50.2  95.1 -2.9     -65.8    24     2132   01 56 29
01 57 40  ---          06 05 46  50.4  95.2 -2.8     -65.8    60     2141   01 56 30

01 57 50  0851+202     06 05 56  50.4  95.3 -2.8     -65.8     4     2141   01 57 46
02 06 10  ---          06 14 18  52.2  96.5 -2.7     -65.5   500     2206   01 57 41

02 06 40  0851+202     06 14 48  52.3  96.6 -2.7     -65.5    24     2206   02 06 29
02 15 40  ---          06 23 49  54.3  98.1 -2.5     -65.1   540     2277   02 06 30

 ---------- Ground-only VLBA+Ef U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

02 17 00  0851+202     06 25 10  54.5  98.3 -2.5     -65.0    74     2277   02 16 49
02 26 30  ---          06 34 41  56.6 100.0 -2.4     -64.4   570     2352   02 16 50
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

 ---------- Ground-only VLBA+VLA27+Ef+Yb Q-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

02 27 30  0851+202     06 35 41  56.8 100.2 -2.3     -64.3    54     2352   02 27 19
02 28 30  ---          06 36 41  57.0 100.4 -2.3     -64.3    60     2361   02 27 20

02 28 40  0851+202     06 36 51  57.0 100.4 -2.3     -64.3     4     2361   02 28 36
02 37 30  ---          06 45 43  58.9 102.2 -2.2     -63.6   530     2430   02 28 31

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

02 38 00  0851+202     06 46 13  59.0 102.3 -2.2     -63.5    24     2430   02 37 49
02 39 00  ---          06 47 13  59.2 102.5 -2.1     -63.4    60     2439   02 37 50

02 39 10  0851+202     06 47 23  59.2 102.5 -2.1     -63.4     4     2439   02 39 06
02 49 30  ---          06 57 45  61.4 104.7 -2.0     -62.3   620     2520   02 39 01

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

02 51 00  0716+714     06 59 15  49.2   3.0 -0.4    -171.9    10     2520   02 50 50
02 56 30  ---          07 04 46  49.2   2.3 -0.3    -173.7   330     2564   02 50 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

02 57 30  0716+714     07 05 46  49.2   2.2 -0.3    -174.0    54     2564   02 57 19
02 58 30  ---          07 06 46  49.3   2.1 -0.3    -174.4    60     2573   02 57 20

02 58 40  0716+714     07 06 56  49.3   2.1 -0.3    -174.4     4     2573   02 58 36
03 01 30  ---          07 09 47  49.3   1.7 -0.2    -175.4   170     2595   02 58 31

03 02 00  0716+714     07 10 17  49.3   1.7 -0.2    -175.5    24     2595   03 01 49
03 03 00  ---          07 11 17  49.3   1.5 -0.2    -175.9    60     2604   03 01 50

03 03 10  0716+714     07 11 27  49.3   1.5 -0.2    -175.9     4     2604   03 03 06
03 08 00  ---          07 16 18  49.3   0.9 -0.1    -177.5   290     2642   03 03 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

03 09 00  0716+714     07 17 18  49.3   0.8 -0.1    -177.8    54     2642   03 08 49
03 16 00  ---          07 24 19  49.3  -0.1  0.0     179.8   420     2698   03 08 50

 ---------- K-band VLBI scans. Space segment 05: 0851+202 with EVN+VLBA+VLA27+GBT ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 20 00  0851+202     07 28 20  67.6 113.1 -1.5     -57.4   152     2698   03 19 49
03 21 00  ---          07 29 20  67.8 113.5 -1.4     -57.2    60     2707   03 19 50

03 21 10  0851+202     07 29 30  67.9 113.5 -1.4     -57.1     4     2707   03 21 06
03 30 00  ---          07 38 22  69.6 116.7 -1.3     -54.9   530     2776   03 21 01

03 30 30  0851+202     07 38 52  69.7 116.9 -1.3     -54.8    24     2776   03 30 19
03 31 30  ---          07 39 52  69.9 117.3 -1.3     -54.5    60     2785   03 30 20

03 31 40  0851+202     07 40 02  69.9 117.4 -1.3     -54.4     4     2785   03 31 36
03 40 00  ---          07 48 23  71.5 120.9 -1.1     -51.8   500     2850   03 31 31

03 40 30  0851+202     07 48 53  71.6 121.2 -1.1     -51.6    24     2850   03 40 19
03 41 30  ---          07 49 53  71.8 121.6 -1.1     -51.2    60     2859   03 40 20

03 41 40  0851+202     07 50 03  71.8 121.7 -1.1     -51.2     4     2859   03 41 36
03 50 00  ---          07 58 25  73.3 126.0 -1.0     -47.8   500     2924   03 41 31

03 50 30  0851+202     07 58 55  73.4 126.2 -0.9     -47.6    24     2924   03 50 19
03 51 30  ---          07 59 55  73.5 126.8 -0.9     -47.2    60     2933   03 50 20

03 51 40  0851+202     08 00 05  73.6 126.9 -0.9     -47.1     4     2933   03 51 36
04 00 00  ---          08 08 26  75.0 132.0 -0.8     -42.9   500     2998   03 51 31

04 00 30  0851+202     08 08 57  75.0 132.4 -0.8     -42.6    24     2998   04 00 19
04 01 30  ---          08 09 57  75.2 133.0 -0.8     -42.0    60     3007   04 00 20

04 01 40  0851+202     08 10 07  75.2 133.1 -0.8     -41.9     4     3007   04 01 36
04 10 00  ---          08 18 28  76.5 139.4 -0.6     -36.6   500     3072   04 01 31

04 10 30  0851+202     08 18 58  76.5 139.8 -0.6     -36.3    24     3072   04 10 19
04 11 30  ---          08 19 58  76.7 140.6 -0.6     -35.6    60     3081   04 10 20
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

04 11 40  0851+202     08 20 08  76.7 140.7 -0.6     -35.4     4     3081   04 11 36
04 20 00  ---          08 28 30  77.7 148.2 -0.5     -28.8   500     3146   04 11 31

 ---------- K-band  VLBI scans.  Ground segment 04: target source  with VLBA+GBT ----------

04 20 30  0851+202     08 29 00  77.8 148.7 -0.4     -28.4    24     3146   04 20 19
04 21 30  ---          08 30 00  77.9 149.7 -0.4     -27.5    60     3155   04 20 20

04 21 40  0851+202     08 30 10  77.9 149.9 -0.4     -27.3     4     3155   04 21 36
04 30 30  ---          08 39 01  78.8 159.4 -0.3     -18.8   530     3224   04 21 31

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

04 31 00  0851+202     08 39 32  78.8 159.9 -0.3     -18.3    24     3224   04 30 49
04 41 00  ---          08 49 33  79.3 172.1 -0.1      -7.3   600     3303   04 30 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 41 30  0851+202     08 50 03  79.3 172.7 -0.1      -6.7    24     3303   04 41 19
04 42 30  ---          08 51 03  79.4 174.0 -0.1      -5.5    60     3312   04 41 20

04 42 40  0851+202     08 51 13  79.4 174.2 -0.1      -5.3     4     3312   04 42 36
04 51 00  ---          08 59 35  79.4 184.8  0.1       4.4   500     3377   04 42 31

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

04 51 30  0851+202     09 00 05  79.4 185.4  0.1       5.0    24     3377   04 51 19
04 52 30  ---          09 01 05  79.3 186.7  0.1       6.1    60     3386   04 51 20

04 52 40  0851+202     09 01 15  79.3 186.9  0.1       6.3     4     3386   04 52 36
05 01 00  ---          09 09 36  79.0 197.2  0.2      15.7   500     3451   04 52 31

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 02 30  0851+202     09 11 07  78.9 198.9  0.3      17.3    83     3451   05 02 19
05 03 30  ---          09 12 07  78.8 200.1  0.3      18.3    60     3460   05 02 20

05 03 40  0851+202     09 12 17  78.8 200.3  0.3      18.5     4     3460   05 03 36
05 12 00  ---          09 20 38  78.0 209.3  0.4      26.6   500     3525   05 03 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

05 12 30  0851+202     09 21 08  78.0 209.8  0.4      27.1    24     3525   05 12 19
05 13 30  ---          09 22 09  77.9 210.8  0.4      28.0    60     3534   05 12 20

05 13 40  0851+202     09 22 19  77.8 211.0  0.4      28.1     4     3534   05 13 36
05 22 00  ---          09 30 40  76.8 218.6  0.6      34.8   500     3599   05 13 31

05 22 30  0851+202     09 31 10  76.7 219.0  0.6      35.2    24     3599   05 22 19
05 23 30  ---          09 32 10  76.6 219.8  0.6      35.9    60     3608   05 22 20

05 23 40  0851+202     09 32 20  76.6 220.0  0.6      36.1     4     3608   05 23 36
05 32 00  ---          09 40 42  75.4 226.3  0.7      41.5   500     3673   05 23 31

05 32 30  0851+202     09 41 12  75.3 226.6  0.8      41.8    24     3673   05 32 19
05 42 00  ---          09 50 43  73.7 232.6  0.9      46.7   570     3748   05 32 20

05 42 30  0851+202     09 51 13  73.6 232.9  0.9      47.0    24     3748   05 42 19
05 43 30  ---          09 52 13  73.5 233.5  0.9      47.4    60     3757   05 42 20

05 43 40  0851+202     09 52 23  73.4 233.6  0.9      47.5     4     3757   05 43 36
05 52 00  ---          10 00 45  71.9 237.9  1.1      50.9   500     3822   05 43 31

05 52 30  0851+202     10 01 15  71.8 238.1  1.1      51.1    24     3822   05 52 19
05 53 30  ---          10 02 15  71.7 238.6  1.1      51.4    60     3831   05 52 20

05 53 40  0851+202     10 02 25  71.6 238.7  1.1      51.5     4     3831   05 53 36
06 02 00  ---          10 10 46  70.1 242.3  1.2      54.2   500     3896   05 53 31

06 02 30  0851+202     10 11 17  70.0 242.5  1.3      54.3    24     3896   06 02 19
06 03 30  ---          10 12 17  69.8 242.9  1.3      54.6    60     3905   06 02 20

06 03 40  0851+202     10 12 27  69.7 243.0  1.3      54.7     4     3905   06 03 36
06 12 00  ---          10 20 48  68.1 246.0  1.4      56.8   500     3970   06 03 31

06 12 30  0851+202     10 21 18  68.0 246.2  1.4      56.9    24     3970   06 12 19
06 13 30  ---          10 22 18  67.8 246.6  1.4      57.2    60     3979   06 12 20

06 13 40  0851+202     10 22 28  67.8 246.6  1.4      57.2     4     3979   06 13 36
06 22 00  ---          10 30 50  66.1 249.3  1.6      58.9   500     4044   06 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

 ---------- Ground-only VLBA Q-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

06 22 30  0851+202     10 31 20  66.0 249.4  1.6      59.0    24     4044   06 22 19
06 23 30  ---          10 32 20  65.8 249.7  1.6      59.2    60     4053   06 22 20

06 23 40  0851+202     10 32 30  65.8 249.8  1.6      59.2     4     4053   06 23 36
06 29 40  ---          10 38 31  64.6 251.5  1.7      60.3   360     4100   06 23 31

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 30 10  0851+202     10 39 01  64.5 251.6  1.7      60.3    24     4100   06 29 59
06 36 30  ---          10 45 22  63.2 253.2  1.8      61.3   380     4150   06 30 00

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

06 37 00  0851+202     10 45 52  63.1 253.4  1.8      61.3    24     4150   06 36 49
06 46 30  ---          10 55 24  61.1 255.6  2.0      62.5   570     4225   06 36 50

06 47 00  0851+202     10 55 54  61.0 255.7  2.0      62.6    24     4225   06 46 49
06 56 30  ---          11 05 25  59.0 257.7  2.2      63.5   570     4300   06 46 50

06 57 00  0851+202     11 05 56  58.9 257.9  2.2      63.6    24     4300   06 56 49
06 59 30  ---          11 08 26  58.4 258.4  2.2      63.8   150     4321   06 56 50

 ---------- K-band VLBI scans. Space segment 06: 0851+202 with VLBA+VLA27+GBT ----------

07 00 00  0851+202     11 08 56  58.3 258.5  2.2      63.8    24     4321   06 59 49
07 01 00  ---          11 09 56  58.0 258.6  2.2      63.9    60     4330   06 59 50

07 01 10  0851+202     11 10 06  58.0 258.7  2.2      63.9     4     4330   07 01 06
07 10 00  ---          11 18 58  56.1 260.3  2.4      64.5   530     4399   07 01 01

07 10 30  0851+202     11 19 28  56.0 260.4  2.4      64.6    24     4399   07 10 19
07 11 30  ---          11 20 28  55.8 260.6  2.4      64.6    60     4408   07 10 20

07 11 40  0851+202     11 20 38  55.8 260.6  2.4      64.6     4     4408   07 11 36
07 20 00  ---          11 28 59  54.0 262.1  2.6      65.1   500     4473   07 11 31

07 20 30  0851+202     11 29 29  53.9 262.2  2.6      65.1    24     4473   07 20 19
07 21 30  ---          11 30 30  53.7 262.3  2.6      65.2    60     4482   07 20 20
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

07 21 40  0851+202     11 30 40  53.6 262.4  2.6      65.2     4     4482   07 21 36
07 30 00  ---          11 39 01  51.9 263.7  2.7      65.6   500     4547   07 21 31

07 30 30  0851+202     11 39 31  51.8 263.8  2.7      65.6    24     4547   07 30 19
07 31 30  ---          11 40 31  51.5 264.0  2.7      65.6    60     4556   07 30 20

07 31 40  0851+202     11 40 41  51.5 264.0  2.7      65.6     4     4556   07 31 36
07 40 00  ---          11 49 03  49.7 265.3  2.9      65.9   500     4621   07 31 31

07 40 30  0851+202     11 49 33  49.6 265.3  2.9      65.9    24     4621   07 40 19
07 41 30  ---          11 50 33  49.4 265.5  2.9      65.9    60     4630   07 40 20

07 41 40  0851+202     11 50 43  49.4 265.5  2.9      65.9     4     4630   07 41 36
07 50 00  ---          11 59 04  47.6 266.7  3.1      66.1   500     4695   07 41 31

07 50 30  0851+202     11 59 34  47.5 266.8  3.1      66.1    24     4695   07 50 19
07 51 30  ---          12 00 34  47.2 266.9  3.1      66.1    60     4704   07 50 20

07 51 40  0851+202     12 00 44  47.2 266.9  3.1      66.1     4     4704   07 51 36
08 00 00  ---          12 09 06  45.4 268.1  3.2      66.3   500     4769   07 51 31

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

08 00 30  0851+202     12 09 36  45.3 268.2  3.2      66.3    24     4769   08 00 19
08 09 30  ---          12 18 37  43.4 269.3  3.4      66.3   540     4840   08 00 20

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

08 10 00  0851+202     12 19 07  43.2 269.4  3.4      66.3    24     4840   08 09 49
08 11 00  ---          12 20 08  43.0 269.5  3.4      66.3    60     4849   08 09 50

08 11 10  0851+202     12 20 18  43.0 269.6  3.4      66.3     4     4849   08 11 06
08 19 30  ---          12 28 39  41.2 270.6  3.5      66.3   500     4914   08 11 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

08 20 00  0851+202     12 29 09  41.1 270.7  3.6      66.3    24     4914   08 19 49
08 21 00  ---          12 30 09  40.9 270.8  3.6      66.3    60     4923   08 19 50

08 21 10  0851+202     12 30 19  40.8 270.8  3.6      66.3     4     4923   08 21 06
08 29 30  ---          12 38 41  39.0 271.9  3.7      66.3   500     4988   08 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

08 30 00  0851+202     12 39 11  38.9 271.9  3.7      66.3    24     4988   08 29 49
08 31 00  ---          12 40 11  38.7 272.0  3.7      66.2    60     4997   08 29 50

08 31 10  0851+202     12 40 21  38.7 272.1  3.7      66.2     4     4997   08 31 06
08 39 30  ---          12 48 42  36.9 273.1  3.9      66.1   500     5062   08 31 01

08 40 00  0851+202     12 49 12  36.8 273.1  3.9      66.1    24     5062   08 39 49
08 48 00  ---          12 57 14  35.1 274.1  4.0      66.0   480     5126   08 39 50

08 48 30  0851+202     12 57 44  35.0 274.1  4.0      66.0    24     5126   08 48 19
08 58 00  ---          13 07 15  32.9 275.2  4.2      65.8   570     5200   08 48 20

08 58 30  0851+202     13 07 45  32.8 275.3  4.2      65.8    24     5200   08 58 19
09 08 00  ---          13 17 17  30.8 276.4  4.4      65.5   570     5275   08 58 20

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

09 08 30  0851+202     13 17 47  30.7 276.4  4.4      65.5    24     5275   09 08 19
09 17 30  ---          13 26 49  28.7 277.4  4.5      65.3   540     5346   09 08 20

 ---------- Ground-only VLBA U-band on target source ----------

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

09 18 00  0851+202     13 27 19  28.6 277.5  4.5      65.2    24     5346   09 17 49
09 19 00  ---          13 28 19  28.4 277.6  4.5      65.2    60     5355   09 17 50

09 19 10  0851+202     13 28 29  28.4 277.6  4.5      65.2     4     5355   09 19 06
09 27 30  ---          13 36 50  26.6 278.6  4.7      64.9   500     5420   09 19 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

09 28 00  0851+202     13 37 20  26.5 278.6  4.7      64.9    24     5420   09 27 49
09 29 00  ---          13 38 20  26.3 278.7  4.7      64.9    60     5429   09 27 50

09 29 10  0851+202     13 38 31  26.2 278.7  4.7      64.9     4     5429   09 29 06
09 39 00  ---          13 48 22  24.1 279.8  4.9      64.5   590     5506   09 29 01

09 39 10  0716+714     13 48 32  26.9 339.1  6.4      73.7   -40     5506   09 39 50
09 46 40  ---          13 56 03  26.4 339.3  6.5      72.0   410     5559   09 39 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 Mar 2017   Day  67 ---

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

09 46 50  0716+714     13 56 13  26.4 339.3  6.5      71.9     4     5559   09 46 46
09 51 50  ---          14 01 14  26.0 339.4  6.6      70.8   300     5598   09 46 41

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

09 52 00  0716+714     14 01 24  26.0 339.4  6.6      70.8     4     5598   09 51 56
10 00 00  ---          14 09 26  25.4 339.7  6.8      69.0   480     5660   09 51 51


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg081c_freq.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  26  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
   BBC fr=     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     759.99    759.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  26  27  28  29  30  31  32  33  34  35

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg081c_freq.dat:
     v7mm_c8

   Setup group:   54         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  36  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
   BBC fr=     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     767.25    767.25    799.25    799.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  36  37  38  39  40  41  42  61  62  63

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg081c_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   43         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  43  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
   BBC fr=     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     776.99    776.99    808.99    808.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  43  44  45  46  47  48  49  56  57  58

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 59.861040       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 12.96182        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 1814-637          18 14 45.949299   * 18 19 35.002600     18 21 12.288328       0.00
                    -63 47 03.20742    *-63 45 48.20500     -63 44 57.59250        0.00
                     From catalog imbedded in main SCHED input file.
                     possble calibrator source for LBA??

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 56.345486       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 08.66218        0.00
 * 3C286             ./gg081c_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati

 * 0716+714          07 16 13.029739   * 07 21 53.448474     07 23 50.595719       0.00
   J0721+7120        71 26 15.17406    * 71 20 36.36340      71 18 40.38874        0.00
                     ./gg081c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 42370 observations, RA-AO3-04, RA-AO2-1

 * 0851+202          08 51 57.250618   * 08 54 48.874930     08 55 48.283390       0.00
   J0854+2006        20 17 58.41733    * 20 06 30.64078      20 02 24.49441        0.00
   OJ287             ./gg081c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 213710 observations, RA-AO3-04, RA-AO3-



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            21                                5.750     0.000
  1814-637   ra1cm2.set            9 10 11 12 13                     2.639    20.990
  3C286      ra1cm2.set            51                                0.267     0.000
             ra7mm2.set            52                                0.367     0.000
  0716+714   ra1cm2.set            1 2 5 6 14 15 16 17 18 19 2 +    12.436   152.486
             ra2cm2.set            43 55                             0.450    14.171
             ra7mm2.set            23 36 59 60                       4.575    33.390
  0851+202   ra1cm2.set            1 2 5 6 9 10 11 12 13 14 15 +    17.411  1982.713
             ra2cm2.set            43 55                             0.864    39.108
             ra7mm2.set            36 52 59 60                       0.911    54.094


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              99.9
   1814-637            78.3
   3C286              138.8
   0716+714           104.6
   0851+202           143.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

