  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Probing the inner jet collimation profile of Mrk 501 with global VLBI at
 Exp. Code:  GK050   


Schedule Version:       3.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Shoko Koyama

Address:  Max Planck Institute for Radio Astronomy
          Auf dem Huegel 69
          53121 Bonn
          Germany

Phone:    +49-228-525-473
EMAIL:    skoyama@mpifr-bonn.mpg.de
Fax:      +49-228-525-229
Phone during observation: 555 1000

Observing mode: continuum global VLBI at 7mm

Notes:
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  10 Mar 2017   Day  69 ---

 Next scan frequencies:  43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
 Next BBC frequencies:     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

14 00 00  3C345        18 17 58  68.7 -58.1  1.6     108.1     0        0   14 00 00
14 04 00  ---          18 21 59  68.0 -58.7  1.6     106.9   240       31   14 00 01

14 04 20  DA426        18 22 19  69.9 -57.0  1.5     110.2     8       31   14 04 20
14 12 00  ---          18 30 00  68.5 -58.4  1.6     107.7   460       90   14 04 21

14 12 00  3C345        18 30 00  66.5 -59.8  1.8     104.6   -12       90   14 12 12
14 16 00  ---          18 34 01  65.8 -60.3  1.8     103.6   228      120   14 12 01

14 16 20  DA426        18 34 21  67.8 -59.1  1.7     106.4     8      120   14 16 20
14 24 00  ---          18 42 02  66.3 -60.0  1.8     104.2   460      179   14 16 21

14 24 00  3C345        18 42 02  64.3 -61.1  2.0     101.6   -12      179   14 24 12
14 28 00  ---          18 46 03  63.5 -61.4  2.0     100.6   228      208   14 24 01

14 28 20  DA426        18 46 23  65.5 -60.5  1.9     103.1     8      208   14 28 20
14 36 00  ---          18 54 04  64.1 -61.3  2.0     101.2   460      267   14 28 21

14 36 00  3C345        18 54 04  62.0 -62.0  2.2      98.8   -12      267   14 36 12
14 40 00  ---          18 58 05  61.2 -62.2  2.2      98.0   228      297   14 36 01

14 40 20  DA426        18 58 25  63.2 -61.6  2.1     100.2     8      297   14 40 20
14 48 00  ---          19 06 06  61.8 -62.1  2.2      98.5   460      356   14 40 21

14 48 00  3C345        19 06 06  59.7 -62.6  2.4      96.3   -12      356   14 48 12
14 52 00  ---          19 10 07  58.9 -62.7  2.4      95.6   228      385   14 48 01

14 52 20  DA426        19 10 27  61.0 -62.4  2.3      97.6     8      385   14 52 20
15 00 00  ---          19 18 08  59.5 -62.7  2.4      96.0   460      445   14 52 21

15 00 00  3C345        19 18 08  57.4 -63.0  2.6      94.1   -12      445   15 00 12
15 04 00  ---          19 22 09  56.6 -63.1  2.6      93.4   228      474   15 00 01

15 04 20  DA426        19 22 29  58.7 -62.9  2.5      95.2     8      474   15 04 20
15 12 00  ---          19 30 10  57.2 -63.1  2.6      93.8   460      533   15 04 21

15 12 00  3C345        19 30 10  55.1 -63.2  2.8      92.0   -12      533   15 12 12
15 16 00  ---          19 34 11  54.3 -63.3  2.8      91.3   228      563   15 12 01

15 16 20  DA426        19 34 31  56.4 -63.2  2.7      93.0     8      563   15 16 20
15 24 00  ---          19 42 12  54.9 -63.3  2.8      91.7   460      622   15 16 21
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  10 Mar 2017   Day  69 ---

15 24 00  3C345        19 42 12  52.8 -63.3  3.0      90.0   -12      622   15 24 12
15 28 00  ---          19 46 13  52.0 -63.3  3.0      89.4   228      651   15 24 01

15 28 20  DA426        19 46 33  54.0 -63.3  2.9      91.0     8      651   15 28 20
15 36 00  ---          19 54 14  52.6 -63.4  3.0      89.8   460      711   15 28 21

15 36 00  3C345        19 54 14  50.5 -63.2  3.2      88.1   -12      711   15 36 12
15 40 00  ---          19 58 15  49.7 -63.2  3.2      87.5   228      740   15 36 01

15 40 20  DA426        19 58 35  51.7 -63.3  3.1      89.1     8      740   15 40 20
15 48 00  ---          20 06 16  50.3 -63.3  3.2      87.9   460      799   15 40 21

15 48 00  3C345        20 06 16  48.2 -63.0  3.4      86.3   -12      799   15 48 12
15 52 00  ---          20 10 17  47.4 -63.0  3.4      85.7   228      829   15 48 01

15 52 20  DA426        20 10 37  49.4 -63.2  3.3      87.2     8      829   15 52 20
16 00 00  ---          20 18 18  47.9 -63.1  3.4      86.1   460      888   15 52 21

16 00 00  3C345        20 18 18  45.9 -62.8  3.6      84.6   -12      888   16 00 12
16 04 00  ---          20 22 18  45.1 -62.7  3.6      84.0   228      917   16 00 01

16 04 20  DA426        20 22 39  47.1 -63.0  3.5      85.5     8      917   16 04 20
16 12 00  ---          20 30 20  45.6 -62.8  3.6      84.4   460      976   16 04 21

16 12 00  3C345        20 30 20  43.6 -62.4  3.8      82.9   -12      976   16 12 12
16 16 00  ---          20 34 20  42.8 -62.3  3.8      82.4   228     1006   16 12 01

16 16 20  DA426        20 34 41  44.8 -62.7  3.7      83.8     8     1006   16 16 20
16 24 00  ---          20 42 22  43.3 -62.4  3.8      82.7   460     1065   16 16 21

16 24 00  3C345        20 42 22  41.3 -62.0  4.0      81.3   -12     1065   16 24 12
16 28 00  ---          20 46 22  40.5 -61.8  4.0      80.7   228     1094   16 24 01

16 28 20  DA426        20 46 42  42.5 -62.3  3.9      82.1     8     1094   16 28 20
16 36 00  ---          20 54 24  41.0 -62.0  4.0      81.1   460     1154   16 28 21

16 36 00  3C345        20 54 24  39.0 -61.5  4.2      79.7   -12     1154   16 36 12
16 40 00  ---          20 58 24  38.2 -61.3  4.2      79.2   228     1183   16 36 01

16 40 20  DA426        20 58 44  40.2 -61.8  4.1      80.5     8     1183   16 40 20
16 48 00  ---          21 06 26  38.8 -61.5  4.2      79.5   460     1242   16 40 21

16 48 00  3C345        21 06 26  36.7 -60.9  4.4      78.1   -12     1242   16 48 12
16 52 00  ---          21 10 26  36.0 -60.7  4.4      77.6   228     1272   16 48 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  10 Mar 2017   Day  69 ---

16 52 20  DA426        21 10 46  37.9 -61.3  4.3      78.9     8     1272   16 52 20
17 00 00  ---          21 18 28  36.5 -60.9  4.4      77.9   460     1331   16 52 21

17 00 00  3C345        21 18 28  34.5 -60.3  4.6      76.5   -12     1331   17 00 12
17 04 00  ---          21 22 28  33.7 -60.1  4.6      76.0   228     1360   17 00 01

17 04 20  DA426        21 22 48  35.7 -60.7  4.5      77.4     8     1360   17 04 20
17 12 00  ---          21 30 30  34.2 -60.3  4.6      76.4   460     1420   17 04 21

17 12 00  3C345        21 30 30  32.2 -59.6  4.8      75.0   -12     1420   17 12 12
17 16 00  ---          21 34 30  31.5 -59.4  4.8      74.5   228     1449   17 12 01

17 16 20  DA426        21 34 50  33.4 -60.1  4.7      75.8     8     1449   17 16 20
17 24 00  ---          21 42 32  32.0 -59.6  4.8      74.8   460     1508   17 16 21

17 24 00  3C345        21 42 32  30.0 -58.9  5.0      73.4   -12     1508   17 24 12
17 28 00  ---          21 46 32  29.3 -58.6  5.0      72.9   228     1538   17 24 01

17 28 20  DA426        21 46 52  31.2 -59.3  4.9      74.3     8     1538   17 28 20
17 36 00  ---          21 54 34  29.8 -58.9  5.0      73.3   460     1597   17 28 21

17 36 00  3C345        21 54 34  27.8 -58.1  5.2      71.9   -12     1597   17 36 12
17 40 00  ---          21 58 34  27.1 -57.8  5.3      71.4   228     1626   17 36 01

17 40 20  DA426        21 58 54  29.0 -58.6  5.1      72.7     8     1626   17 40 20
17 48 00  ---          22 06 36  27.6 -58.1  5.2      71.7   460     1685   17 40 21

17 48 00  3C345        22 06 36  25.6 -57.3  5.4      70.4   -12     1685   17 48 12
17 52 00  ---          22 10 36  24.9 -57.0  5.5      69.8   228     1715   17 48 01

17 52 20  DA426        22 10 56  26.8 -57.8  5.3      71.2     8     1715   17 52 20
18 00 00  ---          22 18 38  25.4 -57.2  5.4      70.2   460     1774   17 52 21

18 00 00  3C345        22 18 38  23.4 -56.4  5.6      68.8   -12     1774   18 00 12
18 04 00  ---          22 22 38  22.7 -56.1  5.7      68.3   228     1803   18 00 01

18 04 20  DA426        22 22 58  24.6 -56.9  5.5      69.6     8     1803   18 04 20
18 12 00  ---          22 30 40  23.2 -56.3  5.6      68.6   460     1863   18 04 21

18 12 00  3C345        22 30 40  21.3 -55.4  5.8      67.2   -12     1863   18 12 12
18 16 00  ---          22 34 40  20.6 -55.1  5.9      66.7   228     1892   18 12 01

18 16 20  DA426        22 35 00  22.4 -56.0  5.7      68.1     8     1892   18 16 20
18 24 00  ---          22 42 41  21.1 -55.4  5.8      67.1   460     1951   18 16 21
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  10 Mar 2017   Day  69 ---

18 24 00  3C345        22 42 41  19.2 -54.5  6.0      65.6   -12     1951   18 24 12
18 28 00  ---          22 46 42  18.5 -54.1  6.1      65.1   228     1981   18 24 01

18 28 20  DA426        22 47 02  20.3 -55.0  5.9      66.5     8     1981   18 28 20
18 36 00  ---          22 54 43  19.0 -54.4  6.0      65.5   460     2040   18 28 21

18 36 00  3C345        22 54 43  17.1 -53.4  6.2      64.0   -12     2040   18 36 12
18 40 00  ---          22 58 44  16.4 -53.1  6.3      63.5   228     2069   18 36 01

18 40 20  DA426        22 59 04  18.2 -54.0  6.1      64.9     8     2069   18 40 20
18 48 00  ---          23 06 45  16.9 -53.4  6.2      63.9   460     2129   18 40 21

18 48 00  3C345        23 06 45  15.0 -52.3  6.4      62.4   -12     2129   18 48 12
18 52 00  ---          23 10 46  14.3 -52.0  6.5      61.9   228     2158   18 48 01

18 52 20  DA426        23 11 06  16.1 -53.0  6.3      63.3     8     2158   18 52 20
19 00 00  ---          23 18 47  14.8 -52.3  6.4      62.2   460     2217   18 52 21

19 00 30  0716+714     23 19 17  19.9  17.0 -8.1     -51.6   -27     2217   19 00 57
19 06 00  ---          23 24 48  20.2  17.2 -8.0     -52.8   303     2256   19 00 31

19 06 00  3C345        23 24 48  12.0 -50.6  6.7      59.9   -56     2256   19 06 56
19 10 00  ---          23 28 49  11.3 -50.2  6.8      59.4   184     2280   19 06 01

19 10 20  DA426        23 29 09  13.1 -51.3  6.6      60.8     8     2280   19 10 20
19 18 00  ---          23 36 50  11.8 -50.5  6.7      59.8   460     2339   19 10 21

19 18 00  3C345        23 36 50  10.0 -49.4  6.9      58.2   -12     2339   19 18 12
19 22 00  ---          23 40 51   9.3 -49.0  7.0      57.7   228     2369   19 18 01

19 22 20  DA426        23 41 11  11.1 -50.1  6.8      59.2     9     2369   19 22 20
19 30 00  ---          23 48 52   9.8 -49.3  6.9      58.1   460     2428   19 22 21

19 30 00  3C345        23 48 52   8.1 -48.2  7.1      56.5   -11     2428   19 30 11
19 34 00  ---          23 52 53   7.4 -47.7  7.2      55.9   229     2457   19 30 01

19 34 20  DA426        23 53 13   9.1 -48.9  7.0      57.4     9     2457   19 34 20
19 42 00  ---          00 00 54   7.8 -48.1  7.1      56.3   460     2517   19 34 21

19 42 00  3C345        00 00 54   6.1 -46.8  7.3      54.7   -11     2517   19 42 11
19 46 00  ---          00 04 55   5.5 -46.4  7.4      54.1   229     2546   19 42 01

19 46 20  DA426        00 05 15   7.2 -47.6  7.2      55.7     9     2546   19 46 20
19 54 00  ---          00 12 56   5.9 -46.7  7.3      54.6   460     2605   19 46 21
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  10 Mar 2017   Day  69 ---

19 54 00  3C345        00 12 56   4.3 -45.5  7.5      52.9   -11     2605   19 54 11
19 58 00  ---          00 16 57   3.7 -45.0  7.6  H   52.3     0     2635   19 54 01

19 58 20  DA426        00 17 17   5.3 -46.3  7.4      53.9     9     2635   19 58 20
20 06 00  ---          00 24 58   4.1 -45.4  7.5      52.8   460     2694   19 58 21

20 06 00  3C345        00 24 58   2.5 -44.0  7.7  H   51.1   -11     2694   20 06 11
20 10 00  ---          00 28 59   1.9 -43.6  7.8  D   50.5     0     2724   20 06 01

20 10 20  DA426        00 29 19   3.4 -44.9  7.6  H   52.1    10     2724   20 10 20
20 18 00  ---          00 37 00   2.3 -43.9  7.7  H   50.9     0     2783   20 10 21

 --- Sat  11 Mar 2017   Day  70 ---

06 01 00  0716+714     10 21 36  42.8 -17.8  3.0     124.8 34926     2783   06 01 00
06 06 00  ---          10 26 37  42.5 -18.1  3.0     123.4   300     2822   06 01 01

06 06 00  3C345        10 26 37  16.1  52.9 -6.3     -63.3   -60     2822   06 07 00
06 08 00  ---          10 28 37  16.4  53.1 -6.2     -63.5    60     2829   06 06 01

06 08 20  DA426        10 28 57  14.6  52.2 -6.4     -62.1     8     2829   06 08 20
06 18 00  ---          10 38 39  16.3  53.1 -6.3     -63.4   580     2904   06 08 21

06 18 00  3C345        10 38 39  18.2  54.0 -6.1     -64.9   -12     2904   06 18 12
06 20 00  ---          10 40 39  18.5  54.1 -6.0     -65.1   108     2918   06 18 01

06 20 20  DA426        10 40 59  16.7  53.3 -6.2     -63.7     8     2918   06 20 20
06 30 00  ---          10 50 41  18.4  54.1 -6.1     -65.0   580     2993   06 20 21

06 30 00  3C345        10 50 41  20.3  55.0 -5.9     -66.5   -12     2993   06 30 12
06 32 00  ---          10 52 41  20.6  55.1 -5.8     -66.7   108     3007   06 30 01

06 32 20  DA426        10 53 01  18.8  54.3 -6.0     -65.3     8     3007   06 32 20
06 42 00  ---          11 02 43  20.5  55.1 -5.9     -66.6   580     3081   06 32 21

06 42 00  3C345        11 02 43  22.4  55.9 -5.7     -68.0   -12     3081   06 42 12
06 44 00  ---          11 04 43  22.8  56.1 -5.6     -68.3   108     3095   06 42 01

06 44 20  DA426        11 05 03  20.9  55.3 -5.8     -66.9     8     3095   06 44 20
06 54 00  ---          11 14 45  22.6  56.1 -5.7     -68.2   580     3170   06 44 21

06 54 00  3C345        11 14 45  24.6  56.8 -5.5     -69.6   -12     3170   06 54 12
06 56 00  ---          11 16 45  24.9  57.0 -5.4     -69.9   108     3184   06 54 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Mar 2017   Day  70 ---

06 56 20  DA426        11 17 05  23.0  56.3 -5.6     -68.5     8     3184   06 56 20
07 06 00  ---          11 26 47  24.8  57.0 -5.5     -69.7   580     3258   06 56 21

07 06 20  3C345        11 27 07  26.8  57.7 -5.3     -71.2     8     3258   07 06 20
07 14 00  ---          11 34 48  28.2  58.3 -5.1     -72.2   460     3318   07 06 21

07 14 20  DA426        11 35 08  26.3  57.6 -5.3     -70.8     8     3318   07 14 20
07 24 00  ---          11 44 50  28.0  58.2 -5.2     -72.1   580     3392   07 14 21

07 24 00  3C345        11 44 50  30.0  58.9 -5.0     -73.5   -12     3392   07 24 12
07 26 00  ---          11 46 50  30.4  59.0 -4.9     -73.7   108     3406   07 24 01

07 26 20  DA426        11 47 10  28.5  58.4 -5.1     -72.4     8     3406   07 26 20
07 36 00  ---          11 56 52  30.2  59.0 -5.0     -73.6   580     3481   07 26 21

07 36 00  3C345        11 56 52  32.3  59.6 -4.8     -75.0   -12     3481   07 36 12
07 38 00  ---          11 58 52  32.6  59.8 -4.7     -75.3   108     3495   07 36 01

07 38 20  DA426        11 59 12  30.7  59.2 -4.9     -73.9     8     3495   07 38 20
07 48 00  ---          12 08 54  32.5  59.8 -4.8     -75.1   580     3570   07 38 21

07 48 00  3C345        12 08 54  34.5  60.3 -4.6     -76.6   -12     3570   07 48 12
07 50 00  ---          12 10 54  34.9  60.4 -4.5     -76.8   108     3584   07 48 01

07 50 20  DA426        12 11 14  32.9  59.9 -4.7     -75.4     8     3584   07 50 20
08 00 00  ---          12 20 56  34.7  60.4 -4.6     -76.7   580     3658   07 50 21

08 00 00  3C345        12 20 56  36.8  60.9 -4.4     -78.1   -12     3658   08 00 12
08 02 00  ---          12 22 56  37.1  61.0 -4.3     -78.4   108     3672   08 00 01

08 02 30  0716+714     12 23 26  33.7 -21.8  5.0      93.4   -37     3672   08 03 07
08 08 00  ---          12 28 57  33.2 -21.8  5.1      92.1   293     3710   08 02 31

08 08 00  3C345        12 28 57  38.3  61.3 -4.2     -79.2   -67     3710   08 09 07
08 10 00  ---          12 30 57  38.7  61.4 -4.2     -79.4    53     3717   08 08 01

08 10 20  DA426        12 31 17  36.7  61.0 -4.4     -78.0     8     3717   08 10 20
08 20 00  ---          12 40 59  38.5  61.4 -4.2     -79.3   580     3792   08 10 21

08 20 00  3C345        12 40 59  40.6  61.8 -4.0     -80.8   -12     3792   08 20 12
08 22 00  ---          12 42 59  40.9  61.9 -4.0     -81.0   108     3805   08 20 01

08 22 20  DA426        12 43 19  38.9  61.5 -4.2     -79.6     8     3805   08 22 20
08 32 00  ---          12 53 01  40.8  62.0 -4.0     -80.9   580     3880   08 22 21
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Mar 2017   Day  70 ---

08 32 00  3C345        12 53 01  42.8  62.3 -3.8     -82.4   -12     3880   08 32 12
08 34 00  ---          12 55 01  43.2  62.4 -3.8     -82.7   108     3894   08 32 01

08 34 20  DA426        12 55 21  41.2  62.0 -4.0     -81.2     8     3894   08 34 20
08 44 00  ---          13 05 03  43.1  62.4 -3.8     -82.5   580     3969   08 34 21

08 44 00  3C345        13 05 03  45.1  62.7 -3.6     -84.1   -12     3969   08 44 12
08 46 00  ---          13 07 03  45.5  62.7 -3.6     -84.3   108     3983   08 44 01

08 46 20  DA426        13 07 23  43.5  62.5 -3.8     -82.8     8     3983   08 46 20
08 56 00  ---          13 17 05  45.4  62.8 -3.6     -84.2   580     4057   08 46 21

08 56 00  3C345        13 17 05  47.4  63.0 -3.4     -85.8   -12     4057   08 56 12
08 58 00  ---          13 19 05  47.8  63.0 -3.4     -86.1   108     4071   08 56 01

08 58 20  DA426        13 19 25  45.8  62.8 -3.6     -84.5     8     4071   08 58 20
09 08 00  ---          13 29 07  47.7  63.1 -3.4     -85.9   580     4146   08 58 21

09 08 00  3C345        13 29 07  49.8  63.2 -3.2     -87.5   -12     4146   09 08 12
09 10 00  ---          13 31 07  50.1  63.2 -3.2     -87.8   108     4160   09 08 01

09 10 20  DA426        13 31 27  48.1  63.1 -3.4     -86.2     8     4160   09 10 20
09 20 00  ---          13 41 09  50.0  63.3 -3.2     -87.7   580     4235   09 10 21

09 20 00  3C345        13 41 09  52.1  63.3 -3.0     -89.4   -12     4235   09 20 12
09 22 00  ---          13 43 09  52.4  63.3 -3.0     -89.7   108     4249   09 20 01

09 22 20  DA426        13 43 29  50.4  63.3 -3.2     -88.0     8     4249   09 22 20
09 32 00  ---          13 53 11  52.3  63.4 -3.0     -89.5   580     4323   09 22 21

09 32 00  3C345        13 53 11  54.4  63.2 -2.8     -91.3   -12     4323   09 32 12
09 34 00  ---          13 55 11  54.8  63.2 -2.8     -91.7   108     4337   09 32 01

09 34 20  DA426        13 55 31  52.7  63.4 -3.0     -89.9     8     4337   09 34 20
09 44 00  ---          14 05 13  54.6  63.3 -2.8     -91.5   580     4412   09 34 21

09 44 00  3C345        14 05 13  56.7  63.1 -2.6     -93.4   -12     4412   09 44 12
09 46 00  ---          14 07 13  57.1  63.0 -2.6     -93.8   108     4426   09 44 01

09 46 20  DA426        14 07 33  55.0  63.3 -2.8     -91.9     8     4426   09 46 20
09 56 00  ---          14 17 15  56.9  63.1 -2.6     -93.5   580     4501   09 46 21

09 56 20  3C345        14 17 35  59.1  62.7 -2.4     -95.7     8     4501   09 56 20
10 04 00  ---          14 25 16  60.5  62.4 -2.3     -97.2   460     4560   09 56 21
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Mar 2017   Day  70 ---

10 04 20  DA426        14 25 36  58.5  62.9 -2.5     -95.1     8     4560   10 04 20
10 14 00  ---          14 35 18  60.4  62.5 -2.3     -96.9   580     4635   10 04 21

10 14 00  3C345        14 35 18  62.4  61.8 -2.1     -99.3   -12     4635   10 14 12
10 16 00  ---          14 37 18  62.8  61.7 -2.1     -99.8   108     4648   10 14 01

10 16 20  DA426        14 37 38  60.8  62.4 -2.3     -97.4     8     4648   10 16 20
10 26 00  ---          14 47 20  62.7  61.8 -2.1     -99.5   580     4723   10 16 21

10 26 00  3C345        14 47 20  64.7  60.9 -1.9    -102.1   -12     4723   10 26 12
10 28 00  ---          14 49 20  65.1  60.7 -1.9    -102.6   108     4737   10 26 01

10 28 20  DA426        14 49 40  63.1  61.7 -2.1    -100.0     8     4737   10 28 20
10 38 00  ---          14 59 21  64.9  60.8 -1.9    -102.3   580     4812   10 28 21

10 38 00  3C345        14 59 21  66.9  59.5 -1.7    -105.2   -12     4812   10 38 12
10 40 00  ---          15 01 22  67.3  59.3 -1.7    -105.8   108     4826   10 38 01

10 40 20  DA426        15 01 42  65.4  60.6 -1.9    -102.9     8     4826   10 40 20
10 50 00  ---          15 11 23  67.2  59.5 -1.7    -105.5   580     4900   10 40 21

10 50 00  3C345        15 11 23  69.2  57.7 -1.5    -108.8   -12     4900   10 50 12
10 52 00  ---          15 13 24  69.5  57.3 -1.5    -109.5   108     4914   10 50 01

10 52 20  DA426        15 13 44  67.6  59.2 -1.7    -106.1     8     4914   10 52 20
11 02 00  ---          15 23 25  69.4  57.6 -1.5    -109.1   580     4989   10 52 21

11 02 00  3C345        15 23 25  71.3  55.3 -1.3    -113.1   -12     4989   11 02 12
11 04 00  ---          15 25 26  71.7  54.8 -1.3    -113.9   108     5003   11 02 01

11 04 20  DA426        15 25 46  69.8  57.2 -1.5    -109.9     8     5003   11 04 20
11 14 00  ---          15 35 27  71.5  55.1 -1.3    -113.4   580     5078   11 04 21

11 14 00  3C345        15 35 27  73.4  52.0 -1.1    -118.1   -12     5078   11 14 12
11 16 00  ---          15 37 28  73.7  51.3 -1.1    -119.1   108     5092   11 14 01

11 16 20  DA426        15 37 48  71.9  54.5 -1.3    -114.3     8     5092   11 16 20
11 26 00  ---          15 47 29  73.6  51.7 -1.1    -118.5   580     5166   11 16 21

11 26 00  3C345        15 47 29  75.4  47.5 -0.9    -124.4   -12     5166   11 26 12
11 28 00  ---          15 49 30  75.7  46.6 -0.9    -125.5   108     5180   11 26 01

11 28 20  DA426        15 49 50  74.0  51.0 -1.1    -119.7     9     5180   11 28 20
11 38 00  ---          15 59 31  75.6  47.2 -0.9    -124.9   580     5255   11 28 21
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Probing the inner jet collimation profile of Mrk 501 with global VLBI at
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Mar 2017   Day  70 ---

11 38 00  3C345        15 59 31  77.2  41.5 -0.7    -132.2   -12     5255   11 38 12
11 40 00  ---          16 01 32  77.5  40.3 -0.7    -133.6   108     5269   11 38 01

11 40 20  DA426        16 01 52  76.0  46.1 -0.9    -126.3     8     5269   11 40 20
11 50 00  ---          16 11 33  77.4  40.9 -0.7    -132.8   580     5344   11 40 21

11 50 00  3C345        16 11 33  78.8  33.3 -0.5    -142.0   -13     5344   11 50 13
11 52 00  ---          16 13 34  79.0  31.7 -0.5    -143.9   107     5357   11 50 01

11 52 20  DA426        16 13 54  77.7  39.5 -0.7    -134.6     7     5357   11 52 20
12 02 00  ---          16 23 35  78.9  32.6 -0.5    -143.0   580     5432   11 52 21

12 02 00  3C345        16 23 35  80.0  22.6 -0.3    -154.5   -15     5432   12 02 15
12 04 00  ---          16 25 36  80.2  20.6 -0.3    -156.8   105     5446   12 02 01

12 04 20  DA426        16 25 56  79.2  30.6 -0.5    -145.2     5     5446   12 04 20
12 14 00  ---          16 35 37  80.1  21.6 -0.3    -155.7   580     5520   12 04 21

12 14 00  3C345        16 35 37  80.7   9.5 -0.1    -169.4   -17     5520   12 14 17
12 16 00  ---          16 37 38  80.8   7.1 -0.1    -172.0   103     5534   12 14 01

12 16 20  DA426        16 37 58  80.3  19.2 -0.3    -158.5     3     5534   12 16 20
12 26 00  ---          16 47 39  80.8   8.2 -0.1    -170.8   580     5608   12 16 21

12 26 00  3C345        16 47 39  80.8  -4.9  0.1     174.5   -17     5608   12 26 17
12 28 00  ---          16 49 40  80.8  -7.3  0.1     171.8   103     5622   12 26 01

12 28 00  3C345        16 49 40  80.8  -7.3  0.1     171.8    -6     5622   12 28 06
12 30 00  ---          16 51 40  80.7  -9.7  0.1     169.1   114     5636   12 28 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess117.Q1024glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:    2         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   4  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
   BBC fr=     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.25    754.25    786.25    786.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   4   5   6   7   8   9  10  11  12  13

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0716+714          07 16 13.029731   * 07 21 53.448466     07 23 50.463513       0.01
   J0721+7120        71 26 15.17408    * 71 20 36.36342      71 18 40.96255        0.00
   J0721+71          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished  63527 observations.

 * 3C345             16 41 17.606228   * 16 42 58.809966     16 43 33.375579       0.76
   J1642+3948        39 54 10.81496    * 39 48 36.99402      39 46 33.76781        0.52
   1641+399          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J1642+39          GSFC 2015a astro solution, unpublished  53430 observations.

 * DA426             16 52 11.729420   * 16 53 52.216685     16 54 26.479049       0.01
   J1653+3945        39 50 25.15738    * 39 45 36.60895      39 43 48.88682        0.01
   1652+398          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J1653+39          GSFC 2015a astro solution, unpublished   6336 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  0716+714   sess117.Q1024glob     1 4 14 15 16 17 18                0.358    22.312
  3C345      sess117.Q1024glob     1 4 14 15 16 17 18                5.378   308.567
  DA426      sess117.Q1024glob     1 4 14 15 16 17 18               16.100   952.224


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0716+714           102.6
   3C345              100.5
   DA426               98.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

