  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: BNS merger counterpart
 Exp. Code:  gg084a  


Schedule Version:       3.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Giancarlo Ghirlanda

Address:  JIVE
          Oude Hoogeveensedijk 4
          Dwingeloo
          Netherlands

Phone:    +31 521 596 536
EMAIL:    zparagi@jive.eu
Fax:      +31 521 596 539
Phone during observation: +31 521 596 530

Observing mode:

Notes:    v3 - includes one-hour before start for LBA fringe checks
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

 Next scan frequencies:  4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

04 55 50  J1337-1257   09 19 15  14.0 114.7 -4.3     -53.4     0        0   04 55 50
04 58 50  =1334-127    09 22 15  14.5 115.1 -4.3     -53.1   180       46   04 55 51

05 00 00  J1311-2329   09 23 25  12.8 127.7 -3.8     -48.0    53       46   05 00 00
05 02 00  ---          09 25 26  13.2 128.0 -3.8     -47.7   120       77   05 00 01

05 02 00  EM170817     09 25 26  13.6 128.2 -3.8     -47.5    -9       77   05 02 09
05 04 30  ---          09 27 56  14.0 128.6 -3.7     -47.1   141      114   05 02 01

05 04 30  J1311-2329   09 27 56  13.6 128.4 -3.7     -47.3    -8      114   05 04 38
05 06 00  ---          09 29 26  13.8 128.7 -3.7     -47.1    82      135   05 04 31

05 06 00  EM170817     09 29 26  14.2 128.9 -3.7     -46.9    -9      135   05 06 09
05 08 30  ---          09 31 57  14.6 129.3 -3.6     -46.5   141      171   05 06 01

05 09 00  J1311-2329   09 32 27  14.3 129.2 -3.7     -46.7    22      171   05 09 00
05 10 00  ---          09 33 27  14.5 129.3 -3.7     -46.6    60      187   05 09 01

05 10 00  EM170817     09 33 27  14.9 129.5 -3.6     -46.3    -9      187   05 10 09
05 12 30  ---          09 35 57  15.3 130.0 -3.6     -46.0   141      223   05 10 01

05 12 30  J1311-2329   09 35 57  14.9 129.7 -3.6     -46.2    -8      223   05 12 38
05 14 00  ---          09 37 28  15.2 130.0 -3.6     -46.0    82      244   05 12 31

05 14 00  J1312-2350   09 37 28  14.7 130.1 -3.6     -46.1    -9      244   05 14 09
05 16 30  ---          09 39 58  15.2 130.5 -3.6     -45.7   141      280   05 14 01

05 17 10  J1311-2329   09 40 38  15.7 130.5 -3.5     -45.5    31      280   05 17 10
05 18 10  ---          09 41 38  15.9 130.7 -3.5     -45.4    60      296   05 17 11

05 18 10  EM170817     09 41 38  16.2 130.9 -3.5     -45.2    -8      296   05 18 18
05 20 40  ---          09 44 09  16.6 131.3 -3.4     -44.8   142      332   05 18 11

05 20 40  J1311-2329   09 44 09  16.3 131.1 -3.5     -45.0    -8      332   05 20 48
05 22 10  ---          09 45 39  16.5 131.4 -3.4     -44.8    82      353   05 20 41

05 22 10  EM170817     09 45 39  16.9 131.6 -3.4     -44.6    -8      353   05 22 18
05 24 40  ---          09 48 09  17.3 132.0 -3.4     -44.2   142      390   05 22 11

05 25 10  J1311-2329   09 48 39  17.0 131.9 -3.4     -44.4    22      390   05 25 10
05 26 10  ---          09 49 40  17.2 132.0 -3.4     -44.2    60      406   05 25 11
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

05 26 10  EM170817     09 49 40  17.5 132.3 -3.4     -44.0    -8      406   05 26 18
05 28 40  ---          09 52 10  17.9 132.7 -3.3     -43.6   142      442   05 26 11

05 28 40  J1311-2329   09 52 10  17.6 132.5 -3.3     -43.8    -8      442   05 28 48
05 30 10  ---          09 53 40  17.8 132.7 -3.3     -43.6    82      463   05 28 41

05 30 10  J1312-2350   09 53 40  17.4 132.8 -3.3     -43.7    -9      463   05 30 19
05 32 40  ---          09 56 11  17.8 133.2 -3.3     -43.3   141      500   05 30 11

05 32 40  J1311-2329   09 56 11  18.2 133.2 -3.3     -43.2    -9      500   05 32 49
05 34 10  ---          09 57 41  18.4 133.4 -3.2     -43.0    81      520   05 32 41

05 34 10  J1303-2405   09 57 41  19.3 135.3 -3.1     -41.5   -10      520   05 34 20
05 36 40  ---          10 00 11  19.6 135.8 -3.1     -41.1   140      556   05 34 11

05 37 20  J1311-2329   10 00 51  18.9 134.0 -3.2     -42.5    30      556   05 37 20
05 38 20  ---          10 01 52  19.1 134.2 -3.2     -42.3    60      572   05 37 21

05 39 00  J1337-1257   10 02 32  22.2 121.6 -3.6     -48.8    23      572   05 39 00
05 42 00  =1334-127    10 05 32  22.7 122.2 -3.6     -48.4   180      618   05 39 01

05 42 30  J1259-2310   10 06 02  21.8 137.0 -2.9     -39.7    12      618   05 42 30
05 43 30  =1256-229    10 07 02  22.0 137.2 -2.9     -39.5    60      634   05 42 31

05 43 30  J1311-2329   10 07 02  19.9 135.1 -3.1     -41.5   -12      634   05 43 42
05 45 00  ---          10 08 33  20.1 135.4 -3.1     -41.2    78      654   05 43 31

05 45 00  EM170817     10 08 33  20.5 135.7 -3.0     -41.0    -8      654   05 45 08
05 47 30  ---          10 11 03  20.8 136.1 -3.0     -40.6   142      690   05 45 01

05 47 30  J1311-2329   10 11 03  20.5 135.9 -3.0     -40.8    -8      690   05 47 38
05 49 00  ---          10 12 33  20.7 136.1 -3.0     -40.6    82      712   05 47 31

05 49 00  EM170817     10 12 33  21.1 136.4 -3.0     -40.3    -8      712   05 49 08
05 51 30  ---          10 15 04  21.4 136.9 -2.9     -39.9   142      748   05 49 01

05 52 00  J1259-2310   10 15 34  23.2 138.9 -2.7     -38.0    19      748   05 52 00
05 53 00  =1256-229    10 16 34  23.3 139.1 -2.7     -37.8    60      764   05 52 01

05 53 00  J1311-2329   10 16 34  21.3 136.9 -2.9     -39.9   -12      764   05 53 12
05 54 30  ---          10 18 04  21.5 137.2 -2.9     -39.7    78      784   05 53 01

05 54 30  EM170817     10 18 04  21.9 137.4 -2.9     -39.4    -8      784   05 54 38
05 57 00  ---          10 20 35  22.2 137.9 -2.8     -38.9   142      820   05 54 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

05 57 00  J1311-2329   10 20 35  21.9 137.7 -2.9     -39.2    -8      820   05 57 08
05 58 30  ---          10 22 05  22.1 137.9 -2.8     -39.0    82      841   05 57 01

05 58 30  EM170817     10 22 05  22.4 138.2 -2.8     -38.7    -8      841   05 58 38
06 01 00  ---          10 24 35  22.8 138.7 -2.8     -38.3   142      878   05 58 31

06 01 30  J1259-2310   10 25 05  24.5 140.8 -2.6     -36.3    19      878   06 01 30
06 02 30  =1256-229    10 26 05  24.7 141.0 -2.6     -36.1    60      893   06 01 31

06 02 30  J1311-2329   10 26 05  22.7 138.7 -2.8     -38.3   -12      893   06 02 42
06 04 00  ---          10 27 36  22.9 139.0 -2.8     -38.0    78      914   06 02 31

06 04 00  EM170817     10 27 36  23.2 139.3 -2.7     -37.7    -8      914   06 04 08
06 06 30  ---          10 30 06  23.6 139.8 -2.7     -37.3   142      950   06 04 01

06 06 30  J1311-2329   10 30 06  23.2 139.5 -2.7     -37.6    -8      950   06 06 38
06 08 00  ---          10 31 36  23.4 139.8 -2.7     -37.3    82      971   06 06 31

06 08 00  EM170817     10 31 36  23.8 140.1 -2.7     -37.0    -8      971   06 08 08
06 10 30  ---          10 34 07  24.1 140.6 -2.6     -36.5   142     1008   06 08 01

06 11 00  J1259-2310   10 34 37  25.8 142.8 -2.4     -34.5    19     1008   06 11 00
06 12 00  =1256-229    10 35 37  25.9 143.0 -2.4     -34.3    60     1023   06 11 01

06 12 00  J1311-2329   10 35 37  24.0 140.6 -2.6     -36.6   -12     1023   06 12 12
06 13 30  ---          10 37 07  24.2 140.9 -2.6     -36.3    78     1043   06 12 01

06 13 30  EM170817     10 37 07  24.5 141.2 -2.6     -36.0    -8     1043   06 13 38
06 16 00  ---          10 39 38  24.9 141.7 -2.5     -35.5   142     1080   06 13 31

06 16 00  J1311-2329   10 39 38  24.5 141.4 -2.5     -35.8    -8     1080   06 16 08
06 17 30  ---          10 41 08  24.7 141.7 -2.5     -35.6    82     1101   06 16 01

06 17 30  J1312-2350   10 41 08  24.3 141.7 -2.5     -35.7    -9     1101   06 17 39
06 18 30  ---          10 42 08  24.4 141.9 -2.5     -35.5    51     1114   06 17 31

06 19 00  J1259-2310   10 42 38  26.8 144.5 -2.3     -33.0    17     1114   06 19 00
06 20 00  =1256-229    10 43 38  26.9 144.7 -2.3     -32.8    60     1130   06 19 01

06 20 00  J1311-2329   10 43 38  25.1 142.2 -2.5     -35.1   -12     1130   06 20 12
06 21 30  ---          10 45 09  25.3 142.6 -2.5     -34.8    78     1150   06 20 01

06 21 30  EM170817     10 45 09  25.6 142.9 -2.4     -34.5    -8     1150   06 21 38
06 24 00  ---          10 47 39  25.9 143.4 -2.4     -34.0   142     1186   06 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

06 24 00  J1311-2329   10 47 39  25.6 143.1 -2.4     -34.3    -8     1186   06 24 08
06 25 30  ---          10 49 09  25.8 143.4 -2.4     -34.0    82     1208   06 24 01

06 25 30  EM170817     10 49 09  26.1 143.7 -2.4     -33.7    -8     1208   06 25 38
06 28 00  ---          10 51 40  26.4 144.2 -2.3     -33.2   142     1244   06 25 31

06 28 30  J1259-2310   10 52 10  28.0 146.6 -2.1     -31.1    19     1244   06 28 30
06 29 30  =1256-229    10 53 10  28.1 146.8 -2.1     -30.9    60     1260   06 28 31

06 29 30  J1311-2329   10 53 10  26.3 144.2 -2.3     -33.3   -12     1260   06 29 42
06 31 00  ---          10 54 40  26.5 144.6 -2.3     -33.0    78     1280   06 29 31

06 31 00  EM170817     10 54 40  26.8 144.9 -2.3     -32.7    -8     1280   06 31 08
06 33 30  ---          10 57 11  27.1 145.4 -2.2     -32.2   142     1316   06 31 01

06 33 30  J1311-2329   10 57 11  26.8 145.1 -2.3     -32.5    -8     1316   06 33 38
06 35 00  ---          10 58 41  27.0 145.4 -2.2     -32.2    82     1337   06 33 31

06 35 00  EM170817     10 58 41  27.3 145.8 -2.2     -31.9    -8     1337   06 35 08
06 37 30  ---          11 01 11  27.6 146.3 -2.2     -31.4   142     1374   06 35 01

06 38 00  J1259-2310   11 01 41  29.1 148.7 -2.0     -29.1    19     1374   06 38 00
06 39 00  =1256-229    11 02 41  29.2 148.9 -2.0     -28.9    60     1389   06 38 01

06 39 00  J1311-2329   11 02 41  27.5 146.3 -2.2     -31.4   -11     1389   06 39 11
06 40 30  ---          11 04 12  27.6 146.6 -2.1     -31.1    79     1410   06 39 01

06 40 30  EM170817     11 04 12  28.0 147.0 -2.1     -30.7    -8     1410   06 40 38
06 43 00  ---          11 06 42  28.2 147.5 -2.1     -30.2   142     1446   06 40 31

06 43 00  J1311-2329   11 06 42  27.9 147.2 -2.1     -30.6    -8     1446   06 43 08
06 44 30  ---          11 08 12  28.1 147.5 -2.1     -30.3    82     1468   06 43 01

06 44 30  EM170817     11 08 12  28.4 147.9 -2.0     -29.9    -8     1468   06 44 38
06 47 00  ---          11 10 43  28.7 148.5 -2.0     -29.4   142     1504   06 44 31

06 47 30  J1259-2310   11 11 13  30.1 150.9 -1.8     -27.1    19     1504   06 47 30
06 48 30  =1256-229    11 12 13  30.2 151.2 -1.8     -26.8    60     1520   06 47 31

06 48 30  J1311-2329   11 12 13  28.6 148.4 -2.0     -29.4   -11     1520   06 48 41
06 50 00  ---          11 13 43  28.7 148.8 -2.0     -29.1    79     1540   06 48 31

06 50 00  EM170817     11 13 43  29.0 149.1 -2.0     -28.8    -8     1540   06 50 08
06 52 30  ---          11 16 14  29.3 149.7 -1.9     -28.2   142     1576   06 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

06 52 30  J1311-2329   11 16 14  29.0 149.4 -1.9     -28.6    -8     1576   06 52 38
06 54 00  ---          11 17 44  29.2 149.7 -1.9     -28.3    82     1598   06 52 31

06 54 00  J1312-2350   11 17 44  28.7 149.6 -1.9     -28.4    -9     1598   06 54 09
06 55 00  ---          11 18 44  28.9 149.9 -1.9     -28.2    51     1611   06 54 01

06 55 30  J1259-2310   11 19 14  30.9 152.9 -1.7     -25.3    18     1611   06 55 30
06 56 30  =1256-229    11 20 14  31.0 153.1 -1.7     -25.1    60     1626   06 55 31

06 56 30  J1311-2329   11 20 14  29.4 150.3 -1.9     -27.7   -11     1626   06 56 41
06 58 00  ---          11 21 45  29.6 150.6 -1.8     -27.4    79     1647   06 56 31

06 58 00  EM170817     11 21 45  29.9 151.0 -1.8     -27.0    -8     1647   06 58 08
07 00 30  ---          11 24 15  30.2 151.6 -1.8     -26.5   142     1683   06 58 01

07 00 30  J1311-2329   11 24 15  29.9 151.2 -1.8     -26.9    -8     1683   07 00 38
07 02 00  ---          11 25 45  30.0 151.6 -1.8     -26.5    82     1704   07 00 31

07 02 00  EM170817     11 25 45  30.3 152.0 -1.8     -26.2    -8     1704   07 02 08
07 04 30  ---          11 28 16  30.6 152.6 -1.7     -25.6   142     1741   07 02 01

07 05 00  J1259-2310   11 28 46  31.8 155.2 -1.5     -23.1    20     1741   07 05 00
07 06 00  =1256-229    11 29 46  31.9 155.4 -1.5     -22.9    60     1756   07 05 01

07 06 00  J1311-2329   11 29 46  30.4 152.5 -1.7     -25.7   -11     1756   07 06 11
07 07 30  ---          11 31 16  30.6 152.9 -1.7     -25.3    79     1777   07 06 01

07 07 30  EM170817     11 31 16  30.9 153.3 -1.7     -24.9    -8     1777   07 07 38
07 10 00  ---          11 33 47  31.1 153.9 -1.6     -24.4   142     1813   07 07 31

07 10 00  J1311-2329   11 33 47  30.8 153.5 -1.6     -24.8    -8     1813   07 10 08
07 11 30  ---          11 35 17  31.0 153.9 -1.6     -24.4    82     1834   07 10 01

07 11 30  EM170817     11 35 17  31.2 154.3 -1.6     -24.0    -8     1834   07 11 38
07 14 00  ---          11 37 47  31.5 154.9 -1.6     -23.5   142     1871   07 11 31

07 14 30  J1259-2310   11 38 17  32.6 157.6 -1.4     -20.9    20     1871   07 14 30
07 15 30  =1256-229    11 39 17  32.7 157.8 -1.3     -20.7    60     1886   07 14 31

07 15 30  J1311-2329   11 39 17  31.3 154.9 -1.6     -23.5   -11     1886   07 15 41
07 17 00  ---          11 40 48  31.5 155.2 -1.5     -23.2    79     1907   07 15 31

07 17 00  EM170817     11 40 48  31.7 155.6 -1.5     -22.8    -8     1907   07 17 08
07 19 30  ---          11 43 18  32.0 156.2 -1.5     -22.2   142     1943   07 17 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

07 19 30  J1311-2329   11 43 18  31.7 155.8 -1.5     -22.6    -8     1943   07 19 38
07 21 00  ---          11 44 48  31.8 156.2 -1.5     -22.2    82     1964   07 19 31

07 21 00  EM170817     11 44 48  32.1 156.6 -1.4     -21.9    -8     1964   07 21 08
07 23 30  ---          11 47 19  32.3 157.3 -1.4     -21.3   142     2001   07 21 01

07 24 00  J1259-2310   11 47 49  33.4 160.0 -1.2     -18.6    20     2001   07 24 00
07 25 00  =1256-229    11 48 49  33.4 160.3 -1.2     -18.4    60     2017   07 24 01

07 25 00  J1311-2329   11 48 49  32.2 157.2 -1.4     -21.3   -11     2017   07 25 11
07 26 30  ---          11 50 19  32.3 157.6 -1.4     -21.0    79     2037   07 25 01

07 26 30  EM170817     11 50 19  32.6 158.0 -1.3     -20.6    -8     2037   07 26 38
07 29 00  ---          11 52 50  32.7 158.7 -1.3     -20.0   142     2073   07 26 31

07 29 00  J1311-2329   11 52 50  32.5 158.2 -1.3     -20.4    -8     2073   07 29 08
07 30 30  ---          11 54 20  32.6 158.6 -1.3     -20.0    82     2095   07 29 01

07 30 30  J1312-2350   11 54 20  32.2 158.5 -1.3     -20.2    -9     2095   07 30 39
07 31 30  ---          11 55 20  32.3 158.7 -1.3     -20.0    51     2108   07 30 31

07 32 00  J1259-2310   11 55 50  33.9 162.2 -1.1     -16.7    19     2108   07 32 00
07 33 00  =1256-229    11 56 50  34.0 162.4 -1.1     -16.4    60     2123   07 32 01

07 33 00  J1311-2329   11 56 50  32.8 159.3 -1.3     -19.4   -10     2123   07 33 10
07 34 30  ---          11 58 21  32.9 159.7 -1.2     -19.1    80     2144   07 33 01

07 34 30  EM170817     11 58 21  33.2 160.1 -1.2     -18.6    -8     2144   07 34 38
07 37 00  ---          12 00 51  33.3 160.7 -1.2     -18.0   142     2180   07 34 31

07 37 00  J1311-2329   12 00 51  33.1 160.3 -1.2     -18.4    -8     2180   07 37 08
07 38 30  ---          12 02 21  33.2 160.7 -1.2     -18.1    82     2202   07 37 01

07 38 30  EM170817     12 02 21  33.5 161.1 -1.1     -17.7    -8     2202   07 38 38
07 41 00  ---          12 04 52  33.6 161.8 -1.1     -17.0   142     2238   07 38 31

07 41 30  J1259-2310   12 05 22  34.5 164.7 -0.9     -14.3    20     2238   07 41 30
07 42 30  =1256-229    12 06 22  34.6 165.0 -0.9     -14.1    60     2254   07 41 31

07 42 30  J1311-2329   12 06 22  33.5 161.7 -1.1     -17.1   -10     2254   07 42 40
07 44 00  ---          12 07 52  33.6 162.1 -1.1     -16.7    80     2274   07 42 31

07 44 00  EM170817     12 07 52  33.8 162.6 -1.0     -16.3    -8     2274   07 44 08
07 46 30  ---          12 10 23  34.0 163.2 -1.0     -15.7   142     2311   07 44 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

07 46 30  J1311-2329   12 10 23  33.8 162.8 -1.0     -16.1    -8     2311   07 46 38
07 48 00  ---          12 11 53  33.8 163.2 -1.0     -15.7    82     2332   07 46 31

07 48 00  EM170817     12 11 53  34.1 163.6 -1.0     -15.3    -8     2332   07 48 08
07 50 30  ---          12 14 23  34.2 164.3 -0.9     -14.7   142     2368   07 48 01

07 51 00  J1259-2310   12 14 53  35.0 167.3 -0.8     -11.9    20     2368   07 51 00
07 52 00  =1256-229    12 15 53  35.1 167.6 -0.7     -11.6    60     2384   07 51 01

07 52 00  J1311-2329   12 15 53  34.1 164.3 -0.9     -14.7   -10     2384   07 52 10
07 53 30  ---          12 17 24  34.2 164.7 -0.9     -14.4    80     2405   07 52 01

07 53 30  EM170817     12 17 24  34.4 165.1 -0.9     -13.9    -8     2405   07 53 38
07 56 00  ---          12 19 54  34.5 165.8 -0.8     -13.3   142     2441   07 53 31

07 56 00  J1311-2329   12 19 54  34.3 165.3 -0.9     -13.7    -8     2441   07 56 08
07 57 30  ---          12 21 24  34.4 165.8 -0.9     -13.4    82     2462   07 56 01

07 57 30  EM170817     12 21 24  34.6 166.2 -0.8     -12.9    -8     2462   07 57 38
08 00 00  ---          12 23 55  34.7 166.9 -0.8     -12.3   142     2499   07 57 31

08 00 30  J1259-2310   12 24 25  35.4 169.9 -0.6      -9.4    20     2499   08 00 30
08 01 30  =1256-229    12 25 25  35.5 170.2 -0.6      -9.2    60     2514   08 00 31

08 01 30  J1311-2329   12 25 25  34.6 166.8 -0.8     -12.3   -10     2514   08 01 40
08 03 00  ---          12 26 55  34.7 167.2 -0.8     -12.0    80     2535   08 01 31

08 03 00  EM170817     12 26 55  34.9 167.7 -0.7     -11.5    -8     2535   08 03 08
08 05 30  ---          12 29 26  35.0 168.4 -0.7     -10.9   142     2571   08 03 01

08 05 30  J1311-2329   12 29 26  34.8 167.9 -0.7     -11.3    -8     2571   08 05 38
08 07 00  ---          12 30 56  34.9 168.3 -0.7     -10.9    82     2593   08 05 31

08 07 00  J1312-2350   12 30 56  34.5 168.1 -0.7     -11.2    -9     2593   08 07 09
08 08 00  ---          12 31 56  34.5 168.4 -0.7     -10.9    51     2606   08 07 01

08 08 30  J1259-2310   12 32 26  35.7 172.2 -0.5      -7.3    20     2606   08 08 30
08 09 30  =1256-229    12 33 26  35.7 172.4 -0.4      -7.1    60     2621   08 08 31

08 09 30  J1311-2329   12 33 26  35.0 169.0 -0.7     -10.3   -10     2621   08 09 40
08 11 00  ---          12 34 57  35.0 169.4 -0.6      -9.9    80     2642   08 09 31

08 11 00  EM170817     12 34 57  35.2 169.9 -0.6      -9.4    -8     2642   08 11 08
08 13 30  ---          12 37 27  35.3 170.6 -0.6      -8.8   142     2678   08 11 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

08 13 30  J1311-2329   12 37 27  35.1 170.1 -0.6      -9.3    -8     2678   08 13 38
08 15 00  ---          12 38 57  35.2 170.6 -0.6      -8.9    82     2700   08 13 31

08 15 00  EM170817     12 38 57  35.4 171.0 -0.5      -8.4    -8     2700   08 15 08
08 17 30  ---          12 41 28  35.4 171.7 -0.5      -7.7   142     2736   08 15 01

08 18 00  J1259-2310   12 41 58  35.9 174.8 -0.3      -4.8    20     2736   08 18 00
08 19 00  =1256-229    12 42 58  35.9 175.1 -0.3      -4.6    60     2752   08 18 01

08 19 00  J1311-2329   12 42 58  35.3 171.7 -0.5      -7.8   -10     2752   08 19 10
08 20 30  ---          12 44 28  35.4 172.1 -0.5      -7.4    80     2772   08 19 01

08 20 30  EM170817     12 44 28  35.5 172.6 -0.4      -7.0    -8     2772   08 20 38
08 23 00  ---          12 46 59  35.6 173.3 -0.4      -6.3   142     2809   08 20 31

08 23 00  J1311-2329   12 46 59  35.4 172.8 -0.4      -6.8    -8     2809   08 23 08
08 24 30  ---          12 48 29  35.5 173.2 -0.4      -6.4    82     2830   08 23 01

08 24 30  EM170817     12 48 29  35.6 173.7 -0.4      -5.9    -8     2830   08 24 38
08 27 00  ---          12 50 59  35.7 174.4 -0.3      -5.2   142     2866   08 24 31

08 27 30  J1259-2310   12 51 29  36.1 177.5 -0.1      -2.3    20     2866   08 27 30
08 28 30  =1256-229    12 52 29  36.1 177.8 -0.1      -2.0    60     2882   08 27 31

08 28 30  J1311-2329   12 52 29  35.6 174.3 -0.3      -5.3   -10     2882   08 28 40
08 30 00  ---          12 54 00  35.6 174.8 -0.3      -4.9    80     2903   08 28 31

08 30 00  EM170817     12 54 00  35.7 175.3 -0.3      -4.5    -8     2903   08 30 08
08 32 30  ---          12 56 30  35.8 176.0 -0.2      -3.8   142     2939   08 30 01

08 32 30  J1311-2329   12 56 30  35.6 175.5 -0.3      -4.3    -8     2939   08 32 38
08 34 00  ---          12 58 00  35.7 175.9 -0.2      -3.9    82     2960   08 32 31

08 34 00  EM170817     12 58 00  35.8 176.4 -0.2      -3.4    -8     2960   08 34 08
08 36 30  ---          13 00 31  35.8 177.1 -0.2      -2.7   142     2997   08 34 01

08 37 00  J1259-2310   13 01 01  36.1 180.3  0.0       0.2    20     2997   08 37 00
08 38 00  =1256-229    13 02 01  36.1 180.5  0.0       0.5    60     3012   08 37 01

08 38 00  J1311-2329   13 02 01  35.7 177.0 -0.2      -2.8   -10     3012   08 38 10
08 39 30  ---          13 03 31  35.7 177.4 -0.2      -2.4    80     3033   08 38 01

08 39 30  EM170817     13 03 31  35.9 177.9 -0.1      -1.9    -8     3033   08 39 38
08 42 00  ---          13 06 02  35.9 178.7 -0.1      -1.3   142     3070   08 39 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

08 42 00  J1311-2329   13 06 02  35.7 178.1 -0.1      -1.7    -8     3070   08 42 08
08 43 30  ---          13 07 32  35.8 178.6 -0.1      -1.3    82     3091   08 42 01

08 43 30  J1312-2350   13 07 32  35.4 178.2 -0.1      -1.7    -8     3091   08 43 38
08 44 30  ---          13 08 32  35.4 178.5 -0.1      -1.4    52     3104   08 43 31

08 45 00  J1259-2310   13 09 02  36.0 182.5  0.1       2.4    19     3104   08 45 00
08 46 00  =1256-229    13 10 02  36.0 182.8  0.2       2.6    60     3119   08 45 01

08 46 00  J1311-2329   13 10 02  35.8 179.3 -0.0      -0.7   -10     3119   08 46 10
08 47 30  ---          13 11 33  35.8 179.7 -0.0      -0.3    80     3140   08 46 01

08 47 30  EM170817     13 11 33  35.9 180.2  0.0       0.2    -8     3140   08 47 38
08 50 00  ---          13 14 03  35.9 180.9  0.1       0.9   142     3177   08 47 31

08 50 00  J1311-2329   13 14 03  35.8 180.4  0.0       0.4    -8     3177   08 50 08
08 51 30  ---          13 15 33  35.8 180.8  0.0       0.8    82     3198   08 50 01

08 51 30  EM170817     13 15 33  35.9 181.3  0.1       1.3    -8     3198   08 51 38
08 54 00  ---          13 18 04  35.9 182.1  0.1       1.9   142     3234   08 51 31

08 54 30  J1259-2310   13 18 34  35.9 185.2  0.3       4.9    20     3234   08 54 30
08 55 30  =1256-229    13 19 34  35.9 185.5  0.3       5.2    60     3250   08 54 31

08 55 30  J1311-2329   13 19 34  35.7 182.0  0.1       1.8   -10     3250   08 55 40
08 57 00  ---          13 21 04  35.7 182.4  0.1       2.2    80     3270   08 55 31

08 57 00  EM170817     13 21 04  35.8 182.9  0.2       2.7    -8     3270   08 57 08
08 59 30  ---          13 23 35  35.8 183.6  0.2       3.4   142     3307   08 57 01

08 59 30  J1311-2329   13 23 35  35.7 183.1  0.2       2.9    -8     3307   08 59 38
09 01 00  ---          13 25 05  35.7 183.5  0.2       3.3    82     3328   08 59 31

09 01 00  EM170817     13 25 05  35.8 184.0  0.2       3.8    -8     3328   09 01 08
09 03 30  ---          13 27 35  35.7 184.7  0.3       4.5   142     3365   09 01 01

09 04 00  J1259-2310   13 28 05  35.7 187.9  0.5       7.4    20     3365   09 04 00
09 05 00  =1256-229    13 29 05  35.6 188.2  0.5       7.7    60     3380   09 04 01

09 05 00  J1311-2329   13 29 05  35.6 184.6  0.3       4.4   -10     3380   09 05 10
09 06 30  ---          13 30 36  35.6 185.1  0.3       4.8    80     3401   09 05 01

09 06 30  EM170817     13 30 36  35.7 185.6  0.3       5.2    -8     3401   09 06 38
09 09 00  ---          13 33 06  35.6 186.3  0.4       5.9   142     3437   09 06 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

09 09 00  J1311-2329   13 33 06  35.5 185.8  0.3       5.4    -8     3437   09 09 08
09 10 30  ---          13 34 36  35.5 186.2  0.4       5.8    82     3459   09 09 01

09 10 30  EM170817     13 34 36  35.6 186.7  0.4       6.3    -8     3459   09 10 38
09 13 00  ---          13 37 07  35.5 187.4  0.4       7.0   142     3495   09 10 31

09 13 30  J1259-2310   13 37 37  35.3 190.6  0.6       9.9    20     3495   09 13 30
09 14 30  =1256-229    13 38 37  35.3 190.8  0.6      10.2    60     3511   09 13 31

09 14 30  J1311-2329   13 38 37  35.4 187.3  0.4       6.9   -10     3511   09 14 40
09 16 00  ---          13 40 07  35.4 187.7  0.5       7.3    80     3531   09 14 31

09 16 00  EM170817     13 40 07  35.4 188.3  0.5       7.7    -8     3531   09 16 08
09 18 30  ---          13 42 38  35.4 189.0  0.5       8.4   142     3568   09 16 01

09 18 30  J1311-2329   13 42 38  35.3 188.4  0.5       7.9    -8     3568   09 18 38
09 20 00  ---          13 44 08  35.2 188.8  0.5       8.3    82     3589   09 18 31

09 20 00  J1312-2350   13 44 08  34.9 188.5  0.5       8.0    -8     3589   09 20 08
09 21 00  ---          13 45 08  34.9 188.7  0.5       8.2    52     3602   09 20 01

09 21 30  J1259-2310   13 45 38  35.0 192.8  0.8      12.0    19     3602   09 21 30
09 22 30  =1256-229    13 46 38  34.9 193.1  0.8      12.2    60     3618   09 21 31

09 22 30  J1311-2329   13 46 38  35.2 189.5  0.6       9.0   -10     3618   09 22 40
09 24 00  ---          13 48 09  35.1 190.0  0.6       9.3    80     3638   09 22 31

09 24 00  EM170817     13 48 09  35.2 190.5  0.6       9.8    -8     3638   09 24 08
09 26 30  ---          13 50 39  35.1 191.2  0.7      10.5   142     3675   09 24 01

09 26 30  J1311-2329   13 50 39  35.0 190.6  0.6      10.0    -8     3675   09 26 38
09 28 00  ---          13 52 09  34.9 191.1  0.7      10.4    82     3696   09 26 31

09 28 00  EM170817     13 52 09  35.0 191.6  0.7      10.9    -8     3696   09 28 08
09 30 30  ---          13 54 40  34.9 192.3  0.7      11.5   142     3733   09 28 01

09 31 00  J1259-2310   13 55 10  34.5 195.4  0.9      14.4    20     3733   09 31 00
09 32 00  =1256-229    13 56 10  34.4 195.6  0.9      14.6    60     3748   09 31 01

09 32 00  J1311-2329   13 56 10  34.8 192.2  0.7      11.4   -10     3748   09 32 10
09 33 30  ---          13 57 40  34.7 192.6  0.8      11.8    80     3769   09 32 01

09 33 30  EM170817     13 57 40  34.7 193.1  0.8      12.3    -8     3769   09 33 38
09 36 00  ---          14 00 11  34.6 193.8  0.8      12.9   142     3805   09 33 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

09 36 00  J1311-2329   14 00 11  34.6 193.3  0.8      12.4    -8     3805   09 36 08
09 37 30  ---          14 01 41  34.5 193.7  0.8      12.8    82     3826   09 36 01

09 37 30  EM170817     14 01 41  34.5 194.2  0.8      13.3    -8     3826   09 37 38
09 40 00  ---          14 04 11  34.4 194.9  0.9      13.9   142     3863   09 37 31

09 40 30  J1259-2310   14 04 41  33.9 197.9  1.1      16.8    20     3863   09 40 30
09 41 30  =1256-229    14 05 41  33.8 198.2  1.1      17.0    60     3878   09 40 31

09 41 30  J1311-2329   14 05 41  34.3 194.7  0.9      13.8   -10     3878   09 41 40
09 43 00  ---          14 07 12  34.2 195.2  0.9      14.2    80     3899   09 41 31

09 43 00  EM170817     14 07 12  34.2 195.7  0.9      14.7    -8     3899   09 43 08
09 45 30  ---          14 09 42  34.1 196.3  1.0      15.3   142     3936   09 43 01

09 45 30  J1311-2329   14 09 42  34.1 195.8  1.0      14.8    -8     3936   09 45 38
09 47 00  ---          14 11 12  34.0 196.2  1.0      15.2    82     3957   09 45 31

09 47 00  EM170817     14 11 12  34.0 196.8  1.0      15.7    -8     3957   09 47 08
09 49 30  ---          14 13 43  33.8 197.4  1.0      16.3   142     3993   09 47 01

09 50 00  J1259-2310   14 14 13  33.2 200.4  1.2      19.1    20     3993   09 50 00
09 51 00  =1256-229    14 15 13  33.2 200.7  1.3      19.3    60     4009   09 50 01

09 51 00  J1311-2329   14 15 13  33.7 197.3  1.0      16.2   -10     4009   09 51 10
09 52 30  ---          14 16 43  33.6 197.7  1.1      16.6    80     4029   09 51 01

09 52 30  EM170817     14 16 43  33.6 198.2  1.1      17.0    -8     4029   09 52 38
09 55 00  ---          14 19 14  33.5 198.9  1.1      17.7   142     4066   09 52 31

09 55 00  J1311-2329   14 19 14  33.5 198.3  1.1      17.2    -8     4066   09 55 08
09 56 30  ---          14 20 44  33.4 198.7  1.1      17.6    82     4087   09 55 01

09 56 30  J1312-2350   14 20 44  33.1 198.3  1.1      17.2    -8     4087   09 56 38
09 57 30  ---          14 21 44  33.0 198.6  1.1      17.4    52     4101   09 56 31

09 58 00  J1259-2310   14 22 14  32.6 202.5  1.4      21.0    19     4101   09 58 00
09 59 00  =1256-229    14 23 14  32.5 202.7  1.4      21.2    60     4116   09 58 01

09 59 00  J1311-2329   14 23 14  33.2 199.4  1.2      18.2   -10     4116   09 59 10
10 00 30  ---          14 24 45  33.1 199.8  1.2      18.5    80     4137   09 59 01

10 00 30  EM170817     14 24 45  33.1 200.3  1.2      19.0    -8     4137   10 00 38
10 03 00  ---          14 27 15  32.9 201.0  1.3      19.6   142     4173   10 00 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

10 03 00  J1311-2329   14 27 15  32.9 200.4  1.2      19.1    -8     4173   10 03 08
10 04 30  ---          14 28 45  32.8 200.8  1.3      19.5    82     4194   10 03 01

10 04 30  EM170817     14 28 45  32.8 201.3  1.3      20.0    -8     4194   10 04 38
10 07 00  ---          14 31 16  32.6 202.0  1.3      20.6   142     4231   10 04 31

10 07 30  J1259-2310   14 31 46  31.8 204.9  1.5      23.2    20     4231   10 07 30
10 08 30  =1256-229    14 32 46  31.7 205.1  1.5      23.4    60     4246   10 07 31

10 08 30  J1311-2329   14 32 46  32.5 201.8  1.3      20.5   -10     4246   10 08 40
10 10 00  ---          14 34 16  32.3 202.2  1.4      20.8    80     4267   10 08 31

10 10 00  EM170817     14 34 16  32.3 202.7  1.4      21.3    -8     4267   10 10 08
10 12 30  ---          14 36 47  32.1 203.4  1.4      21.8   142     4304   10 10 01

10 12 30  J1311-2329   14 36 47  32.1 202.9  1.4      21.4    -8     4304   10 12 38
10 14 00  ---          14 38 17  32.0 203.2  1.4      21.7    82     4325   10 12 31

10 14 00  EM170817     14 38 17  32.0 203.7  1.5      22.2    -8     4325   10 14 08
10 16 30  ---          14 40 47  31.7 204.4  1.5      22.8   142     4361   10 14 01

10 17 00  J1259-2310   14 41 17  30.9 207.2  1.7      25.4    20     4361   10 17 00
10 18 00  =1256-229    14 42 17  30.8 207.5  1.7      25.6    60     4377   10 17 01

10 18 00  J1311-2329   14 42 17  31.7 204.2  1.5      22.7   -10     4377   10 18 10
10 19 30  ---          14 43 48  31.5 204.6  1.5      23.0    80     4397   10 18 01

10 19 30  EM170817     14 43 48  31.5 205.1  1.5      23.5    -8     4397   10 19 38
10 22 00  ---          14 46 18  31.2 205.7  1.6      24.0   142     4434   10 19 31

10 22 00  J1311-2329   14 46 18  31.3 205.2  1.6      23.6    -8     4434   10 22 08
10 23 30  ---          14 47 48  31.2 205.6  1.6      23.9    82     4455   10 22 01

10 23 30  EM170817     14 47 48  31.1 206.1  1.6      24.4    -8     4455   10 23 38
10 26 00  ---          14 50 19  30.9 206.7  1.7      24.9   142     4492   10 23 31

10 26 30  J1259-2310   14 50 49  29.9 209.5  1.8      27.5    20     4492   10 26 30
10 27 30  =1256-229    14 51 49  29.8 209.7  1.9      27.7    60     4507   10 26 31

10 27 30  J1311-2329   14 51 49  30.8 206.6  1.7      24.8   -10     4507   10 27 40
10 29 00  ---          14 53 19  30.6 206.9  1.7      25.2    80     4528   10 27 31

10 29 00  EM170817     14 53 19  30.6 207.4  1.7      25.6    -8     4528   10 29 08
10 31 30  ---          14 55 50  30.3 208.0  1.8      26.2   142     4564   10 29 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

10 31 30  J1311-2329   14 55 50  30.4 207.5  1.7      25.7    -8     4564   10 31 38
10 33 00  ---          14 57 20  30.2 207.9  1.7      26.1    82     4585   10 31 31

10 33 00  J1312-2350   14 57 20  30.0 207.4  1.7      25.7    -8     4585   10 33 08
10 34 00  ---          14 58 20  29.9 207.7  1.7      25.9    52     4599   10 33 01

10 34 30  J1259-2310   14 58 50  29.0 211.3  2.0      29.2    20     4599   10 34 30
10 35 30  =1256-229    14 59 50  28.9 211.6  2.0      29.4    60     4614   10 34 31

10 35 30  J1311-2329   14 59 50  30.0 208.5  1.8      26.6   -10     4614   10 35 40
10 37 00  ---          15 01 21  29.8 208.9  1.8      26.9    80     4635   10 35 31

10 37 00  EM170817     15 01 21  29.7 209.3  1.8      27.4    -8     4635   10 37 08
10 39 30  ---          15 03 51  29.5 209.9  1.9      27.9   142     4671   10 37 01

10 39 30  J1311-2329   15 03 51  29.6 209.4  1.9      27.5    -8     4671   10 39 38
10 41 00  ---          15 05 21  29.4 209.8  1.9      27.8    82     4693   10 39 31

10 41 00  EM170817     15 05 21  29.3 210.3  1.9      28.2    -8     4693   10 41 08
10 43 30  ---          15 07 52  29.0 210.9  2.0      28.8   142     4729   10 41 01

10 44 00  J1259-2310   15 08 22  27.9 213.5  2.1      31.1    20     4729   10 44 00
10 45 00  =1256-229    15 09 22  27.8 213.7  2.2      31.3    60     4745   10 44 01

10 45 00  J1311-2329   15 09 22  29.0 210.7  1.9      28.7   -10     4745   10 45 10
10 46 30  ---          15 10 52  28.8 211.1  2.0      29.0    80     4765   10 45 01

10 46 30  EM170817     15 10 52  28.7 211.5  2.0      29.4    -8     4765   10 46 38
10 49 00  ---          15 13 23  28.4 212.1  2.0      29.9   142     4802   10 46 31

10 49 00  J1311-2329   15 13 23  28.5 211.6  2.0      29.5    -8     4802   10 49 08
10 50 30  ---          15 14 53  28.4 212.0  2.0      29.8    82     4823   10 49 01

10 50 30  EM170817     15 14 53  28.3 212.5  2.1      30.2    -8     4823   10 50 38
10 53 00  ---          15 17 23  28.0 213.0  2.1      30.7   142     4860   10 50 31

10 53 30  J1259-2310   15 17 53  26.8 215.6  2.3      33.0    20     4860   10 53 30
10 54 30  =1256-229    15 18 53  26.7 215.8  2.3      33.2    60     4875   10 53 31

10 54 30  J1311-2329   15 18 53  27.9 212.9  2.1      30.6   -10     4875   10 54 40
10 56 00  ---          15 20 24  27.7 213.2  2.1      30.9    80     4896   10 54 31

10 56 00  EM170817     15 20 24  27.6 213.7  2.2      31.3    -8     4896   10 56 08
10 58 30  ---          15 22 54  27.3 214.2  2.2      31.9   142     4932   10 56 01
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

10 58 30  J1311-2329   15 22 54  27.4 213.8  2.2      31.5    -8     4932   10 58 38
11 00 00  ---          15 24 24  27.2 214.1  2.2      31.8    82     4953   10 58 31

11 00 00  EM170817     15 24 24  27.1 214.6  2.2      32.2    -8     4953   11 00 08
11 02 30  ---          15 26 55  26.8 215.1  2.3      32.7   142     4990   11 00 01

11 03 00  J1259-2310   15 27 25  25.6 217.6  2.5      34.9    20     4990   11 03 00
11 04 00  =1256-229    15 28 25  25.4 217.8  2.5      35.1    60     5005   11 03 01

11 04 00  J1311-2329   15 28 25  26.8 215.0  2.3      32.6   -11     5005   11 04 11
11 05 30  ---          15 29 55  26.6 215.3  2.3      32.9    79     5026   11 04 01

11 05 30  EM170817     15 29 55  26.4 215.8  2.3      33.2    -8     5026   11 05 38
11 08 00  ---          15 32 26  26.1 216.3  2.4      33.7   142     5062   11 05 31

11 08 00  J1311-2329   15 32 26  26.3 215.8  2.3      33.3    -8     5062   11 08 08
11 09 30  ---          15 33 56  26.1 216.1  2.4      33.6    82     5083   11 08 01

11 09 30  J1312-2350   15 33 56  25.9 215.7  2.3      33.3    -8     5083   11 09 38
11 10 30  ---          15 34 56  25.8 215.9  2.4      33.5    52     5097   11 09 31

11 11 00  J1259-2310   15 35 26  24.5 219.3  2.6      36.4    19     5097   11 11 00
11 12 00  =1256-229    15 36 26  24.3 219.5  2.6      36.5    60     5112   11 11 01

11 12 00  J1311-2329   15 36 26  25.7 216.7  2.4      34.1   -11     5112   11 12 11
11 13 30  ---          15 37 57  25.5 217.0  2.4      34.4    79     5133   11 12 01

11 13 30  EM170817     15 37 57  25.4 217.5  2.5      34.8    -8     5133   11 13 38
11 16 00  ---          15 40 27  25.1 218.0  2.5      35.3   142     5169   11 13 31

11 16 00  J1311-2329   15 40 27  25.2 217.5  2.5      34.9    -8     5169   11 16 08
11 17 30  ---          15 41 57  25.0 217.8  2.5      35.2    82     5190   11 16 01

11 17 30  EM170817     15 41 57  24.9 218.3  2.5      35.5    -8     5190   11 17 38
11 20 00  ---          15 44 28  24.5 218.8  2.6      36.0   142     5227   11 17 31

11 20 30  J1259-2310   15 44 58  23.2 221.2  2.7      38.1    19     5227   11 20 30
11 21 30  =1256-229    15 45 58  23.0 221.4  2.8      38.2    60     5242   11 20 31

11 21 30  J1311-2329   15 45 58  24.5 218.7  2.6      35.9   -11     5242   11 21 41
11 23 00  ---          15 47 28  24.3 219.0  2.6      36.2    79     5263   11 21 31

11 23 00  EM170817     15 47 28  24.1 219.4  2.6      36.5    -8     5263   11 23 08
11 25 30  ---          15 49 59  23.8 219.9  2.7      37.0   142     5299   11 23 01
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

11 25 30  J1311-2329   15 49 59  23.9 219.5  2.6      36.6    -8     5299   11 25 38
11 27 00  ---          15 51 29  23.7 219.8  2.6      36.9    82     5320   11 25 31

11 27 00  EM170817     15 51 29  23.6 220.2  2.7      37.3    -8     5320   11 27 08
11 29 30  ---          15 53 59  23.2 220.7  2.7      37.7   142     5357   11 27 01

11 30 00  J1259-2310   15 54 29  21.8 223.0  2.9      39.7    19     5357   11 30 00
11 31 00  =1256-229    15 55 29  21.6 223.2  2.9      39.9    60     5373   11 30 01

11 31 00  J1311-2329   15 55 29  23.2 220.6  2.7      37.6   -11     5373   11 31 11
11 32 30  ---          15 57 00  23.0 220.9  2.7      37.9    79     5393   11 31 01

11 32 30  EM170817     15 57 00  22.8 221.3  2.8      38.3    -8     5393   11 32 38
11 35 00  ---          15 59 30  22.4 221.8  2.8      38.7   142     5429   11 32 31

11 35 00  J1311-2329   15 59 30  22.6 221.4  2.8      38.3    -8     5429   11 35 08
11 36 30  ---          16 01 00  22.4 221.6  2.8      38.6    82     5451   11 35 01

11 36 30  EM170817     16 01 00  22.2 222.1  2.8      38.9    -8     5451   11 36 38
11 39 00  ---          16 03 31  21.9 222.6  2.9      39.4   142     5487   11 36 31

11 39 30  J1259-2310   16 04 01  20.4 224.8  3.1      41.3    19     5487   11 39 30
11 40 30  =1256-229    16 05 01  20.2 225.0  3.1      41.5    60     5503   11 39 31

11 40 30  J1311-2329   16 05 01  21.8 222.4  2.9      39.3   -11     5503   11 40 41
11 42 00  ---          16 06 31  21.6 222.7  2.9      39.6    79     5523   11 40 31

11 42 00  EM170817     16 06 31  21.4 223.1  2.9      39.9    -8     5523   11 42 08
11 44 30  ---          16 09 02  21.1 223.6  3.0      40.3   142     5560   11 42 01

11 44 30  J1311-2329   16 09 02  21.2 223.2  2.9      40.0    -8     5560   11 44 38
11 46 00  ---          16 10 32  21.0 223.5  3.0      40.2    82     5581   11 44 31

11 46 00  J1312-2350   16 10 32  20.9 223.0  2.9      39.9    -8     5581   11 46 08
11 47 00  ---          16 11 32  20.8 223.2  3.0      40.1    52     5594   11 46 01

11 47 30  J1259-2310   16 12 02  19.1 226.2  3.2      42.6    19     5594   11 47 30
11 48 30  =1256-229    16 13 02  19.0 226.4  3.2      42.7    60     5610   11 47 31

11 48 30  J1311-2329   16 13 02  20.6 223.9  3.0      40.6   -11     5610   11 48 41
11 50 00  ---          16 14 33  20.4 224.2  3.0      40.9    79     5630   11 48 31

11 50 00  EM170817     16 14 33  20.2 224.6  3.1      41.2    -8     5630   11 50 08
11 52 30  ---          16 17 03  19.9 225.1  3.1      41.6   142     5666   11 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

11 52 30  J1311-2329   16 17 03  20.0 224.7  3.1      41.3    -8     5666   11 52 38
11 54 00  ---          16 18 33  19.8 224.9  3.1      41.5    82     5688   11 52 31

11 54 00  EM170817     16 18 33  19.6 225.4  3.1      41.9    -8     5688   11 54 08
11 56 30  ---          16 21 04  19.2 225.8  3.2      42.3   142     5724   11 54 01

11 57 00  J1259-2310   16 21 34  17.6 227.9  3.4      44.0    19     5724   11 57 00
11 58 00  =1256-229    16 22 34  17.5 228.1  3.4      44.2    60     5740   11 57 01

11 58 00  J1311-2329   16 22 34  19.2 225.7  3.2      42.2   -11     5740   11 58 11
11 59 30  ---          16 24 04  19.0 225.9  3.2      42.4    79     5760   11 58 01

11 59 30  EM170817     16 24 04  18.8 226.3  3.2      42.7    -8     5760   11 59 38
12 02 00  ---          16 26 35  18.4 226.8  3.3      43.1   142     5797   11 59 31

12 02 00  J1311-2329   16 26 35  18.6 226.4  3.2      42.8    -8     5797   12 02 08
12 03 30  ---          16 28 05  18.3 226.6  3.3      43.1    82     5818   12 02 01

12 03 30  EM170817     16 28 05  18.1 227.1  3.3      43.4    -8     5818   12 03 38
12 06 00  ---          16 30 35  17.7 227.5  3.3      43.8   142     5854   12 03 31

12 06 30  J1259-2310   16 31 05  16.1 229.5  3.5      45.5    19     5854   12 06 30
12 07 30  =1256-229    16 32 05  15.9 229.7  3.5      45.6    60     5870   12 06 31

12 07 30  J1311-2329   16 32 05  17.7 227.4  3.3      43.7   -12     5870   12 07 42
12 09 00  ---          16 33 36  17.5 227.6  3.3      43.9    78     5890   12 07 31

12 09 00  EM170817     16 33 36  17.3 228.0  3.4      44.2    -8     5890   12 09 08
12 11 30  ---          16 36 06  16.9 228.4  3.4      44.6   142     5926   12 09 01

12 11 30  J1311-2329   16 36 06  17.1 228.0  3.4      44.3    -8     5926   12 11 38
12 13 00  ---          16 37 36  16.8 228.3  3.4      44.5    82     5948   12 11 31

12 13 00  EM170817     16 37 36  16.6 228.7  3.4      44.8    -8     5948   12 13 08
12 15 30  ---          16 40 07  16.2 229.1  3.5      45.2   142     5984   12 13 01

12 16 00  J1259-2310   16 40 37  14.5 231.1  3.7      46.8    19     5984   12 16 00
12 17 00  =1256-229    16 41 37  14.3 231.3  3.7      47.0    60     6000   12 16 01

12 17 00  J1311-2329   16 41 37  16.2 229.0  3.5      45.1   -12     6000   12 17 12
12 18 30  ---          16 43 07  15.9 229.2  3.5      45.3    78     6020   12 17 01

12 18 30  EM170817     16 43 07  15.7 229.6  3.5      45.6    -8     6020   12 18 38
12 21 00  ---          16 45 38  15.3 230.0  3.6      46.0   142     6056   12 18 31
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               BNS merger counterpart
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  12 Mar 2018   Day  71 ---

12 21 00  J1311-2329   16 45 38  15.5 229.7  3.6      45.7    -8     6056   12 21 08
12 22 30  ---          16 47 08  15.3 229.9  3.6      45.9    82     6077   12 21 01

12 22 30  J1312-2350   16 47 08  15.2 229.4  3.6      45.7    -8     6077   12 22 38
12 23 30  ---          16 48 08  15.1 229.6  3.6      45.8    52     6091   12 22 31

12 23 50  J1259-2310   16 48 28  13.2 232.4  3.8      47.9     8     6091   12 23 50
12 24 50  =1256-229    16 49 28  13.0 232.5  3.8      48.0    60     6106   12 23 51

12 25 10  J1259-2310   16 49 48  13.0 232.6  3.8      48.1    14     6106   12 25 10
12 26 10  =1256-229    16 50 49  12.8 232.7  3.8      48.2    60     6122   12 25 11

12 27 00  J1337-1257   16 51 39  26.3 234.2  3.2      45.7    15     6122   12 27 00
12 30 00  =1334-127    16 54 39  25.8 234.7  3.3      46.1   180     6168   12 27 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess118.C2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  21  Setup file default.  Used with PCAL = off
   LO sum=   4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  21  22  24  25  27  28  29  30  31  32

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * EM170817          13 07 05.876058   * 13 09 48.089000     13 10 47.788605       0.00
                    -23 06 55.47686    *-23 22 53.35000     -23 28 38.30163        0.00
                     From catalog imbedded in main SCHED input file.

 * J1303-2405        13 00 37.951987   * 13 03 19.646900     13 04 19.193675       0.00
                    -23 48 57.23719    *-24 05 03.05600     -24 10 51.14860        0.00
                     From catalog imbedded in main SCHED input file.

 * J1312-2350        13 10 05.987814   * 13 12 48.758100     13 13 48.658933       0.00
                    -23 34 53.02797    *-23 50 46.95300     -23 56 30.19216        0.00
                     From catalog imbedded in main SCHED input file.

 * J1311-2329        13 08 54.934098   * 13 11 37.413987     13 12 37.206648       0.00
                    -23 14 01.14446    *-23 29 56.64651     -23 35 40.60279        0.00
                     From catalog imbedded in main SCHED input file.

   1256-229          12 56 27.604314   * 12 59 08.462031     13 00 07.699580       0.09
 * J1259-2310       -22 54 28.11906    *-23 10 38.65427     -23 16 28.89761        0.21
                     /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished    244 observations.

 * 3C286             13 28 49.657758   * 13 31 08.288051     13 31 59.000385       0.18
   J1331+3030        30 45 58.64059    * 30 30 32.95924      30 24 51.51461        0.17
   1328+307          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J1331+30          GSFC 2015a astro solution, unpublished    225 observations.

   1334-127          13 34 59.803873   * 13 37 39.782778     13 38 38.411011       0.00
 * J1337-1257       -12 42 09.74301    *-12 57 24.69328     -13 02 54.87645        0.00
   J1337-12          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished  91811 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  EM170817   sess118.C2048glob     1 2 3 4 6 7 8 9 10 12 13 14 +     9.708   320.723
  J1303-2405 sess118.C2048glob     1 2 3 4 6 7 8 9 10 12 13 14 +     0.875    21.342
  J1312-2350 sess118.C2048glob     1 2 3 4 6 7 8 9 10 12 13 14 +     1.892    56.087
  J1311-2329 sess118.C2048glob     1 2 3 4 6 7 8 9 10 12 13 14 +     7.117   226.084
  J1259-2310 sess118.C2048glob     21 23 26                          0.800    35.448
  3C286      sess118.C2048glob     26                                0.106     0.000
  J1337-1257 sess118.C2048glob     1 2 3 4 6 7 8 9 10 12 13 14 +     1.250    28.401


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   EM170817           143.3
   J1303-2405         143.9
   J1312-2350         142.5
   J1311-2329         142.9
   J1259-2310         145.2
   3C286              140.2
   J1337-1257         143.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

