  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GM080 - FRB121102
 Exp. Code:  GM080   


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Marcote

Address:  JIVE
          Oude Hoogeveensedijk 4
          Dwingeloo
          Netherlands

Phone:    +31 521 596 536
EMAIL:    marcote@jive.eu
Fax:      +31 521 596 539
Phone during observation: +31 521 596 508

Observing mode: evn

Notes:    ###########################################################
          ########## Please, make sure PHASE CAL is OFF. ############
          ###########################################################
          base (vla D-config) version -- use by all stations besides VLA

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

 Next scan frequencies:  8240.00  8240.00  8304.00  8304.00  8368.00  8368.00  8432.00  8432.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

17 41 20  FRB121102    22 15 48   2.3  52.2 -7.3  H  -54.3     0        0   17 41 20
17 43 50  ---          22 18 18   2.7  52.5 -7.3     -54.6     0       39   17 41 21

17 43 50  J0529+3209   22 18 18   2.6  53.6 -7.2  H  -54.9    -8       39   17 43 58
17 45 20  ---          22 19 49   2.8  53.8 -7.2     -55.1     0       60   17 43 51

17 45 20  FRB121102    22 19 49   3.0  52.7 -7.2     -54.8    -8       60   17 45 28
17 47 50  ---          22 22 19   3.4  53.0 -7.2     -55.2   142       96   17 45 21

17 48 30  J0529+3209   22 22 59   3.4  54.2 -7.1     -55.5    32       96   17 48 30
17 49 30  ---          22 23 59   3.6  54.3 -7.1     -55.7    60      112   17 48 31

17 49 30  FRB121102    22 23 59   3.7  53.2 -7.2     -55.4    -8      112   17 49 38
17 52 00  ---          22 26 30   4.1  53.5 -7.1     -55.7   142      148   17 49 31

17 52 00  J0529+3209   22 26 30   4.0  54.6 -7.1     -56.0    -8      148   17 52 08
17 53 30  ---          22 28 00   4.3  54.8 -7.0     -56.2    82      170   17 52 01

17 53 30  INBEAM       22 28 00   4.4  53.7 -7.1     -55.9    -8      170   17 53 38
17 56 00  ---          22 30 30   4.8  54.0 -7.0     -56.2   142      206   17 53 31

17 56 40  J0529+3209   22 31 11   4.8  55.2 -7.0     -56.6    32      206   17 56 40
17 57 40  ---          22 32 11   5.0  55.3 -7.0     -56.7    60      222   17 56 41

17 57 40  FRB121102    22 32 11   5.1  54.2 -7.0     -56.4    -8      222   17 57 48
18 00 10  ---          22 34 41   5.5  54.5 -7.0     -56.8   142      258   17 57 41

18 00 10  J0529+3209   22 34 41   5.4  55.6 -6.9     -57.0    -8      258   18 00 18
18 01 40  ---          22 36 11   5.7  55.7 -6.9     -57.2    82      279   18 00 11

18 01 40  FRB121102    22 36 11   5.8  54.6 -7.0     -56.9    -8      279   18 01 48
18 04 10  ---          22 38 42   6.2  54.9 -6.9     -57.3   142      316   18 01 41

18 04 50  J0529+3209   22 39 22   6.3  56.1 -6.9     -57.6    32      316   18 04 50
18 05 50  ---          22 40 22   6.4  56.2 -6.8     -57.7    60      331   18 04 51

18 05 50  FRB121102    22 40 22   6.5  55.1 -6.9     -57.5    -8      331   18 05 58
18 08 20  ---          22 42 53   7.0  55.4 -6.8     -57.8   142      368   18 05 51

18 08 20  J0529+3209   22 42 53   6.9  56.5 -6.8     -58.0    -8      368   18 08 28
18 09 50  ---          22 44 23   7.2  56.7 -6.8     -58.2    82      389   18 08 21
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

18 09 50  INBEAM       22 44 23   7.3  55.5 -6.8     -58.0    -8      389   18 09 58
18 12 20  ---          22 46 53   7.7  55.8 -6.8     -58.3   142      426   18 09 51

18 13 00  J0529+3209   22 47 33   7.7  57.0 -6.7     -58.5    32      426   18 13 00
18 14 00  ---          22 48 33   7.9  57.1 -6.7     -58.6    60      441   18 13 01

18 14 00  FRB121102    22 48 33   8.0  56.0 -6.7     -58.5    -8      441   18 14 08
18 16 30  ---          22 51 04   8.4  56.3 -6.7     -58.8   142      478   18 14 01

18 16 30  J0529+3209   22 51 04   8.4  57.4 -6.7     -58.9    -8      478   18 16 38
18 18 00  ---          22 52 34   8.6  57.6 -6.6     -59.1    82      499   18 16 31

18 18 00  FRB121102    22 52 34   8.7  56.5 -6.7     -58.9    -8      499   18 18 08
18 20 30  ---          22 55 05   9.1  56.7 -6.6     -59.2   142      535   18 18 01

18 21 10  J0529+3209   22 55 45   9.2  57.9 -6.6     -59.5    32      535   18 21 10
18 22 10  ---          22 56 45   9.4  58.0 -6.6     -59.6    60      551   18 21 11

18 22 10  FRB121102    22 56 45   9.5  56.9 -6.6     -59.4    -8      551   18 22 18
18 24 40  ---          22 59 15   9.9  57.2 -6.6     -59.7   142      587   18 22 11

18 24 40  J0529+3209   22 59 15   9.9  58.3 -6.5     -59.9    -8      587   18 24 48
18 26 10  ---          23 00 45  10.1  58.5 -6.5     -60.1    82      609   18 24 41

18 26 10  INBEAM       23 00 45  10.2  57.3 -6.5     -59.9    -8      609   18 26 18
18 28 40  ---          23 03 16  10.7  57.6 -6.5     -60.2   142      645   18 26 11

18 29 20  J0529+3209   23 03 56  10.7  58.8 -6.4     -60.4    32      645   18 29 20
18 30 20  ---          23 04 56  10.9  58.9 -6.4     -60.5    60      661   18 29 21

18 30 20  FRB121102    23 04 56  10.9  57.8 -6.5     -60.4    -8      661   18 30 28
18 32 50  ---          23 07 27  11.4  58.0 -6.4     -60.7   142      697   18 30 21

18 32 50  J0529+3209   23 07 27  11.4  59.2 -6.4     -60.8    -8      697   18 32 58
18 34 20  ---          23 08 57  11.7  59.3 -6.4     -61.0    82      718   18 32 51

18 34 20  FRB121102    23 08 57  11.7  58.2 -6.4     -60.9    -8      718   18 34 28
18 36 50  ---          23 11 27  12.1  58.5 -6.4     -61.2   142      755   18 34 21

18 37 30  J0529+3209   23 12 07  12.2  59.7 -6.3     -61.3    32      755   18 37 30
18 38 50  ---          23 13 28  12.5  59.8 -6.3     -61.5    80      775   18 37 31

18 46 50  DA193        23 21 29  13.0  51.1 -6.6     -60.7   465      775   18 46 50
18 49 50  ---          23 24 29  13.5  51.4 -6.5     -61.2   180      822   18 46 51
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

18 50 50  J0403+2600   23 25 29  29.5  75.4 -4.6     -68.0    21      822   18 50 50
18 52 50  =0400+258    23 27 30  29.9  75.6 -4.6     -68.1   120      853   18 50 51

18 53 50  J0529+3209   23 28 30  15.3  61.3 -6.0     -63.1    23      853   18 53 50
18 55 50  ---          23 30 30  15.7  61.5 -6.0     -63.3   120      884   18 53 51

18 55 50  FRB121102    23 30 30  15.7  60.4 -6.0     -63.3    -8      884   18 55 58
18 58 20  ---          23 33 01  16.1  60.6 -6.0     -63.6   142      920   18 55 51

18 58 20  J0529+3209   23 33 01  16.2  61.8 -6.0     -63.6    -8      920   18 58 28
18 59 50  ---          23 34 31  16.4  61.9 -5.9     -63.8    82      941   18 58 21

18 59 50  FRB121102    23 34 31  16.4  60.8 -6.0     -63.8    -8      941   18 59 58
19 02 20  ---          23 37 01  16.9  61.0 -5.9     -64.0   142      978   18 59 51

19 03 00  J0529+3209   23 37 41  17.0  62.2 -5.9     -64.1    32      978   19 03 00
19 04 00  ---          23 38 42  17.2  62.3 -5.9     -64.2    60      993   19 03 01

19 04 00  FRB121102    23 38 42  17.2  61.2 -5.9     -64.2    -8      993   19 04 08
19 06 30  ---          23 41 12  17.7  61.4 -5.9     -64.5   142     1030   19 04 01

19 06 30  J0529+3209   23 41 12  17.7  62.6 -5.8     -64.5    -9     1030   19 06 39
19 08 00  ---          23 42 42  18.0  62.7 -5.8     -64.6    81     1051   19 06 31

19 08 00  INBEAM       23 42 42  18.0  61.5 -5.8     -64.7    -9     1051   19 08 09
19 10 30  ---          23 45 13  18.4  61.8 -5.8     -64.9   141     1087   19 08 01

19 11 10  J0529+3209   23 45 53  18.6  63.0 -5.7     -65.0    31     1087   19 11 10
19 12 10  ---          23 46 53  18.8  63.1 -5.7     -65.1    60     1103   19 11 11

19 12 10  FRB121102    23 46 53  18.7  61.9 -5.8     -65.1    -9     1103   19 12 19
19 14 40  ---          23 49 23  19.2  62.2 -5.7     -65.4   141     1139   19 12 11

19 14 40  J0529+3209   23 49 23  19.3  63.4 -5.7     -65.3    -9     1139   19 14 49
19 16 10  ---          23 50 54  19.6  63.5 -5.7     -65.5    81     1160   19 14 41

19 17 10  J0403+2600   23 51 54  35.0  78.0 -4.2     -69.5    22     1160   19 17 10
19 19 10  =0400+258    23 53 54  35.4  78.1 -4.2     -69.6   120     1191   19 17 11

19 20 10  J0529+3209   23 54 54  20.3  63.9 -5.6     -65.9    22     1191   19 20 10
19 21 40  ---          23 56 25  20.6  64.0 -5.6     -66.0    90     1214   19 20 11

19 21 40  FRB121102    23 56 25  20.6  62.8 -5.6     -66.1    -9     1214   19 21 49
19 24 10  ---          23 58 55  21.0  63.0 -5.6     -66.4   141     1250   19 21 41
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

19 24 10  J0529+3209   23 58 55  21.1  64.2 -5.5     -66.3    -9     1250   19 24 19
19 25 40  ---          00 00 25  21.4  64.4 -5.5     -66.4    81     1271   19 24 11

19 25 40  FRB121102    00 00 25  21.3  63.2 -5.5     -66.5    -9     1271   19 25 49
19 28 10  ---          00 02 56  21.8  63.4 -5.5     -66.8   141     1308   19 25 41

19 28 50  J0529+3209   00 03 36  22.0  64.7 -5.5     -66.7    31     1308   19 28 50
19 29 50  ---          00 04 36  22.2  64.7 -5.4     -66.8    60     1323   19 28 51

19 29 50  FRB121102    00 04 36  22.1  63.5 -5.5     -67.0    -9     1323   19 29 59
19 32 20  ---          00 07 06  22.6  63.8 -5.4     -67.2   141     1359   19 29 51

19 32 20  J0529+3209   00 07 06  22.7  65.0 -5.4     -67.1    -9     1359   19 32 29
19 33 50  ---          00 08 37  23.0  65.1 -5.4     -67.2    81     1380   19 32 21

19 33 50  INBEAM       00 08 37  22.9  63.9 -5.4     -67.4    -9     1380   19 33 59
19 36 20  ---          00 11 07  23.4  64.1 -5.4     -67.6   141     1416   19 33 51

19 37 00  J0529+3209   00 11 47  23.6  65.4 -5.3     -67.6    31     1416   19 37 00
19 38 00  ---          00 12 47  23.8  65.5 -5.3     -67.6    60     1432   19 37 01

19 38 00  FRB121102    00 12 47  23.7  64.3 -5.3     -67.8    -9     1432   19 38 09
19 40 30  ---          00 15 18  24.2  64.5 -5.3     -68.1   141     1468   19 38 01

19 40 30  J0529+3209   00 15 18  24.3  65.7 -5.3     -67.9    -9     1468   19 40 39
19 42 00  ---          00 16 48  24.6  65.8 -5.2     -68.0    81     1489   19 40 31

19 43 00  J0403+2600   00 17 48  40.5  80.5 -3.8     -70.8    21     1489   19 43 00
19 45 00  =0400+258    00 19 48  40.9  80.6 -3.7     -70.9   120     1520   19 43 01

19 46 00  J0529+3209   00 20 49  25.4  66.2 -5.2     -68.4    21     1520   19 46 00
19 47 30  ---          00 22 19  25.7  66.3 -5.1     -68.6    90     1543   19 46 01

19 47 30  FRB121102    00 22 19  25.6  65.1 -5.2     -68.8    -9     1543   19 47 39
19 50 00  ---          00 24 49  26.0  65.3 -5.1     -69.0   141     1580   19 47 31

19 50 00  J0529+3209   00 24 49  26.2  66.5 -5.1     -68.8    -9     1580   19 50 09
19 51 30  ---          00 26 19  26.5  66.6 -5.1     -69.0    81     1600   19 50 01

19 51 30  FRB121102    00 26 19  26.3  65.4 -5.1     -69.2    -9     1600   19 51 39
19 54 00  ---          00 28 50  26.8  65.6 -5.1     -69.4   141     1637   19 51 31

19 54 40  J0529+3209   00 29 30  27.1  66.9 -5.0     -69.3    31     1637   19 54 40
19 55 40  ---          00 30 30  27.3  67.0 -5.0     -69.4    60     1652   19 54 41
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

19 55 40  FRB121102    00 30 30  27.2  65.8 -5.0     -69.6    -9     1652   19 55 49
19 58 10  ---          00 33 01  27.7  66.0 -5.0     -69.8   141     1689   19 55 41

19 58 10  J0529+3209   00 33 01  27.8  67.2 -5.0     -69.6    -9     1689   19 58 19
19 59 40  ---          00 34 31  28.1  67.3 -4.9     -69.7    81     1709   19 58 11

19 59 40  INBEAM       00 34 31  28.0  66.1 -5.0     -70.0    -9     1709   19 59 49
20 02 10  ---          00 37 01  28.5  66.3 -4.9     -70.2   141     1746   19 59 41

20 02 50  J0529+3209   00 37 41  28.7  67.6 -4.9     -70.0    31     1746   20 02 50
20 03 50  ---          00 38 41  28.9  67.7 -4.9     -70.1    60     1761   20 02 51

20 03 50  FRB121102    00 38 41  28.8  66.4 -4.9     -70.4    -9     1761   20 03 59
20 06 20  ---          00 41 12  29.3  66.6 -4.9     -70.6   141     1798   20 03 51

20 06 20  J0529+3209   00 41 12  29.4  67.9 -4.8     -70.4    -9     1798   20 06 29
20 07 50  ---          00 42 42  29.7  68.0 -4.8     -70.5    81     1818   20 06 21

20 08 50  J0403+2600   00 43 42  46.0  83.0 -3.3     -71.9    20     1818   20 08 50
20 10 50  =0400+258    00 45 43  46.4  83.2 -3.3     -72.0   120     1849   20 08 51

20 11 50  J0529+3209   00 46 43  30.5  68.3 -4.7     -70.9    21     1849   20 11 50
20 13 20  ---          00 48 13  30.8  68.5 -4.7     -71.0    90     1873   20 11 51

20 13 20  FRB121102    00 48 13  30.7  67.2 -4.8     -71.3    -9     1873   20 13 29
20 15 50  ---          00 50 43  31.2  67.4 -4.7     -71.6   141     1909   20 13 21

20 15 50  J0529+3209   00 50 43  31.3  68.7 -4.7     -71.2    -9     1909   20 15 59
20 17 20  ---          00 52 14  31.6  68.8 -4.6     -71.4    81     1930   20 15 51

20 17 20  FRB121102    00 52 14  31.5  67.5 -4.7     -71.7    -9     1930   20 17 29
20 19 50  ---          00 54 44  32.0  67.7 -4.6     -71.9   141     1966   20 17 21

20 20 30  J0529+3209   00 55 24  32.3  69.0 -4.6     -71.7    31     1966   20 20 30
20 21 30  ---          00 56 24  32.5  69.1 -4.6     -71.8    60     1981   20 20 31

20 21 30  FRB121102    00 56 24  32.3  67.8 -4.6     -72.1    -9     1981   20 21 39
20 24 00  ---          00 58 55  32.8  68.0 -4.6     -72.4   141     2018   20 21 31

20 24 00  J0529+3209   00 58 55  33.0  69.3 -4.5     -72.0    -9     2018   20 24 09
20 25 30  ---          01 00 25  33.3  69.4 -4.5     -72.1    81     2039   20 24 01

20 25 30  INBEAM       01 00 25  33.1  68.1 -4.5     -72.5    -9     2039   20 25 39
20 28 00  ---          01 02 55  33.6  68.3 -4.5     -72.8   141     2075   20 25 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

20 28 40  J0529+3209   01 03 36  33.9  69.7 -4.5     -72.4    31     2075   20 28 40
20 29 40  ---          01 04 36  34.1  69.7 -4.4     -72.5    60     2090   20 28 41

20 29 40  FRB121102    01 04 36  33.9  68.4 -4.5     -72.9    -9     2090   20 29 49
20 32 10  ---          01 07 06  34.4  68.6 -4.4     -73.1   141     2127   20 29 41

20 32 10  J0529+3209   01 07 06  34.6  69.9 -4.4     -72.7    -9     2127   20 32 19
20 33 40  ---          01 08 36  34.9  70.0 -4.4     -72.9    81     2148   20 32 11

20 34 40  J0403+2600   01 09 37  51.5  85.7 -2.9     -72.8    20     2148   20 34 40
20 36 40  =0400+258    01 11 37  51.9  85.9 -2.9     -72.8   120     2179   20 34 41

20 37 40  J0529+3209   01 12 37  35.8  70.3 -4.3     -73.2    20     2179   20 37 40
20 39 10  ---          01 14 07  36.1  70.5 -4.3     -73.3    90     2202   20 37 41

20 39 10  FRB121102    01 14 07  35.8  69.1 -4.3     -73.8    -9     2202   20 39 19
20 41 40  ---          01 16 38  36.3  69.3 -4.3     -74.0   141     2238   20 39 11

20 41 40  J0529+3209   01 16 38  36.6  70.6 -4.2     -73.6    -9     2238   20 41 49
20 43 10  ---          01 18 08  36.9  70.8 -4.2     -73.7    81     2259   20 41 41

20 43 10  FRB121102    01 18 08  36.6  69.4 -4.3     -74.2    -9     2259   20 43 19
20 45 40  ---          01 20 38  37.1  69.6 -4.2     -74.4   141     2295   20 43 11

20 46 20  J0529+3209   01 21 18  37.5  71.0 -4.2     -74.0    31     2295   20 46 20
20 47 20  ---          01 22 19  37.7  71.1 -4.1     -74.1    60     2311   20 46 21

20 47 20  FRB121102    01 22 19  37.5  69.7 -4.2     -74.6    -9     2311   20 47 29
20 49 50  ---          01 24 49  38.0  69.9 -4.1     -74.8   141     2347   20 47 21

20 49 50  J0529+3209   01 24 49  38.2  71.3 -4.1     -74.3    -9     2347   20 49 59
20 51 20  ---          01 26 19  38.5  71.4 -4.1     -74.4    81     2368   20 49 51

20 51 20  INBEAM       01 26 19  38.3  69.9 -4.1     -75.0    -9     2368   20 51 29
20 53 50  ---          01 28 50  38.8  70.1 -4.1     -75.2   141     2404   20 51 21

20 54 30  J0529+3209   01 29 30  39.2  71.6 -4.0     -74.7    31     2404   20 54 30
20 55 30  ---          01 30 30  39.4  71.7 -4.0     -74.8    60     2420   20 54 31

20 55 30  FRB121102    01 30 30  39.1  70.3 -4.0     -75.3    -9     2420   20 55 39
20 58 00  ---          01 33 00  39.6  70.4 -4.0     -75.6   141     2456   20 55 31

20 58 00  J0529+3209   01 33 00  39.9  71.8 -4.0     -75.0    -9     2456   20 58 09
20 59 30  ---          01 34 31  40.2  71.9 -3.9     -75.1    81     2477   20 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

21 00 30  J0403+2600   01 35 31  57.1  88.6 -2.5     -73.2    19     2477   21 00 30
21 02 30  =0400+258    01 37 31  57.5  88.8 -2.4     -73.3   120     2508   21 00 31

21 03 30  J0529+3209   01 38 31  41.0  72.2 -3.9     -75.5    19     2508   21 03 30
21 05 00  ---          01 40 02  41.3  72.3 -3.8     -75.6    90     2531   21 03 31

21 05 00  FRB121102    01 40 02  41.1  70.9 -3.9     -76.2    -9     2531   21 05 09
21 07 30  ---          01 42 32  41.6  71.1 -3.8     -76.5   141     2567   21 05 01

21 07 30  J0529+3209   01 42 32  41.9  72.5 -3.8     -75.8    -9     2567   21 07 39
21 09 00  ---          01 44 02  42.2  72.6 -3.8     -76.0    81     2588   21 07 31

21 09 00  FRB121102    01 44 02  41.9  71.2 -3.8     -76.6    -9     2588   21 09 09
21 11 30  ---          01 46 33  42.4  71.3 -3.8     -76.8   141     2625   21 09 01

21 12 10  J0529+3209   01 47 13  42.8  72.8 -3.7     -76.2    31     2625   21 12 10
21 13 10  ---          01 48 13  43.0  72.9 -3.7     -76.3    60     2640   21 12 11

21 13 10  FRB121102    01 48 13  42.7  71.4 -3.8     -77.0    -9     2640   21 13 19
21 15 40  ---          01 50 43  43.2  71.6 -3.7     -77.2   141     2676   21 13 11

21 15 40  J0529+3209   01 50 43  43.5  73.1 -3.7     -76.5    -9     2676   21 15 49
21 17 10  ---          01 52 14  43.8  73.2 -3.6     -76.7    81     2697   21 15 41

21 17 10  INBEAM       01 52 14  43.6  71.7 -3.7     -77.4    -9     2697   21 17 19
21 19 40  ---          01 54 44  44.1  71.8 -3.6     -77.6   141     2734   21 17 11

21 20 20  J0529+3209   01 55 24  44.5  73.4 -3.6     -77.0    31     2734   21 20 20
21 21 20  ---          01 56 24  44.7  73.5 -3.6     -77.0    60     2749   21 20 21

21 21 20  FRB121102    01 56 24  44.4  71.9 -3.6     -77.8    -9     2749   21 21 29
21 23 50  ---          01 58 55  44.9  72.1 -3.6     -78.0   141     2785   21 21 21

21 23 50  J0529+3209   01 58 55  45.2  73.6 -3.5     -77.3    -9     2785   21 23 59
21 25 20  ---          02 00 25  45.5  73.7 -3.5     -77.4    81     2806   21 23 51

21 26 20  J0403+2600   02 01 25  62.7  91.9 -2.0     -73.2    18     2806   21 26 20
21 28 20  =0400+258    02 03 25  63.1  92.2 -2.0     -73.2   120     2837   21 26 21

21 29 20  J0529+3209   02 04 26  46.4  74.0 -3.4     -77.7    19     2837   21 29 20
21 30 50  ---          02 05 56  46.7  74.1 -3.4     -77.9    90     2860   21 29 21

21 30 50  FRB121102    02 05 56  46.4  72.5 -3.5     -78.6    -9     2860   21 30 59
21 33 20  ---          02 08 26  46.9  72.7 -3.4     -78.9   141     2897   21 30 51
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

21 33 20  J0529+3209   02 08 26  47.2  74.2 -3.4     -78.1    -9     2897   21 33 29
21 34 50  ---          02 09 56  47.5  74.3 -3.3     -78.2    81     2917   21 33 21

21 34 50  FRB121102    02 09 56  47.2  72.8 -3.4     -79.0    -9     2917   21 34 59
21 37 20  ---          02 12 27  47.7  72.9 -3.3     -79.3   141     2954   21 34 51

21 38 00  J0529+3209   02 13 07  48.2  74.5 -3.3     -78.5    31     2954   21 38 00
21 39 00  ---          02 14 07  48.4  74.6 -3.3     -78.6    60     2969   21 38 01

21 39 00  FRB121102    02 14 07  48.0  73.0 -3.3     -79.4    -9     2969   21 39 09
21 41 30  ---          02 16 38  48.6  73.2 -3.3     -79.7   141     3006   21 39 01

21 41 30  J0529+3209   02 16 38  48.9  74.8 -3.2     -78.8    -9     3006   21 41 39
21 43 00  ---          02 18 08  49.2  74.9 -3.2     -78.9    81     3026   21 41 31

21 43 00  INBEAM       02 18 08  48.9  73.2 -3.3     -79.8    -9     3026   21 43 09
21 45 30  ---          02 20 38  49.4  73.3 -3.2     -80.1   141     3063   21 43 01

21 46 10  J0529+3209   02 21 18  49.9  75.1 -3.2     -79.2    31     3063   21 46 10
21 47 10  ---          02 22 18  50.1  75.1 -3.1     -79.3    60     3078   21 46 11

21 47 10  FRB121102    02 22 18  49.7  73.5 -3.2     -80.2    -9     3078   21 47 19
21 49 40  ---          02 24 49  50.2  73.6 -3.1     -80.4   141     3115   21 47 11

21 49 40  J0529+3209   02 24 49  50.6  75.3 -3.1     -79.5    -9     3115   21 49 49
21 51 10  ---          02 26 19  50.9  75.4 -3.1     -79.6    81     3135   21 49 41

21 52 10  J0403+2600   02 27 19  68.2  96.1 -1.6     -72.2    18     3135   21 52 10
21 54 10  =0400+258    02 29 20  68.6  96.5 -1.6     -72.1   120     3166   21 52 11

21 55 10  J0529+3209   02 30 20  51.7  75.6 -3.0     -80.0    19     3166   21 55 10
21 56 40  ---          02 31 50  52.1  75.7 -3.0     -80.1    90     3190   21 55 11

22 05 40  DA193        02 40 52  49.4  63.1 -3.3     -87.3   523     3190   22 05 40
22 08 40  ---          02 43 52  50.0  63.1 -3.2     -87.8   180     3236   22 05 41

22 09 40  J0403+2600   02 44 52  72.0  99.8 -1.3     -70.7     9     3236   22 09 40
22 11 40  =0400+258    02 46 52  72.4 100.3 -1.3     -70.5   120     3267   22 09 41

22 12 40  J0529+3209   02 47 53  55.4  76.6 -2.7     -81.5    18     3267   22 12 40
22 14 40  ---          02 49 53  55.8  76.7 -2.7     -81.7   120     3298   22 12 41

22 14 40  FRB121102    02 49 53  55.4  74.9 -2.7     -82.9    -9     3298   22 14 49
22 17 10  ---          02 52 23  56.0  75.0 -2.7     -83.1   141     3334   22 14 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

22 17 10  J0529+3209   02 52 23  56.3  76.9 -2.6     -81.9    -9     3334   22 17 19
22 18 40  ---          02 53 54  56.7  76.9 -2.6     -82.0    81     3355   22 17 11

22 18 40  FRB121102    02 53 54  56.3  75.1 -2.7     -83.2    -9     3355   22 18 49
22 21 10  ---          02 56 24  56.8  75.2 -2.6     -83.5   141     3391   22 18 41

22 21 50  J0529+3209   02 57 04  57.3  77.1 -2.6     -82.3    31     3391   22 21 50
22 22 50  ---          02 58 04  57.5  77.2 -2.5     -82.4    60     3407   22 21 51

22 22 50  FRB121102    02 58 04  57.1  75.2 -2.6     -83.7    -9     3407   22 22 59
22 25 20  ---          03 00 35  57.7  75.3 -2.5     -83.9   141     3443   22 22 51

22 25 20  J0529+3209   03 00 35  58.1  77.3 -2.5     -82.6    -9     3443   22 25 29
22 26 50  ---          03 02 05  58.4  77.4 -2.5     -82.7    81     3464   22 25 21

22 26 50  INBEAM       03 02 05  58.0  75.4 -2.5     -84.1    -9     3464   22 26 59
22 29 20  ---          03 04 35  58.5  75.5 -2.5     -84.4   141     3500   22 26 51

22 30 00  J0529+3209   03 05 16  59.0  77.5 -2.4     -83.0    31     3500   22 30 00
22 31 00  ---          03 06 16  59.3  77.6 -2.4     -83.1    60     3516   22 30 01

22 31 00  FRB121102    03 06 16  58.8  75.6 -2.5     -84.5    -9     3516   22 31 09
22 33 30  ---          03 08 46  59.4  75.7 -2.4     -84.8   141     3552   22 31 01

22 33 30  J0529+3209   03 08 46  59.8  77.7 -2.4     -83.3    -9     3552   22 33 39
22 35 00  ---          03 10 16  60.1  77.8 -2.3     -83.5    81     3573   22 33 31

22 36 00  J0403+2600   03 11 16  77.5 108.1 -0.9     -65.5    18     3573   22 36 00
22 38 00  =0400+258    03 13 17  77.9 109.0 -0.9     -64.9   120     3604   22 36 01

22 39 00  J0529+3209   03 14 17  60.9  78.0 -2.3     -83.9    18     3604   22 39 00
22 40 30  ---          03 15 47  61.3  78.0 -2.3     -84.0    90     3627   22 39 01

22 40 30  FRB121102    03 15 47  60.8  75.9 -2.3     -85.5    -9     3627   22 40 39
22 43 00  ---          03 18 18  61.3  76.0 -2.3     -85.8   141     3663   22 40 31

22 43 00  J0529+3209   03 18 18  61.8  78.1 -2.2     -84.2    -9     3663   22 43 09
22 44 30  ---          03 19 48  62.1  78.2 -2.2     -84.4    81     3684   22 43 01

22 44 30  FRB121102    03 19 48  61.7  76.0 -2.2     -85.9    -9     3684   22 44 39
22 47 00  ---          03 22 18  62.2  76.1 -2.2     -86.2   141     3721   22 44 31

22 47 40  J0529+3209   03 22 58  62.8  78.4 -2.1     -84.7    31     3721   22 47 40
22 48 40  ---          03 23 59  63.0  78.4 -2.1     -84.8    60     3736   22 47 41
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

22 48 40  FRB121102    03 23 59  62.5  76.2 -2.2     -86.4    -9     3736   22 48 49
22 51 10  ---          03 26 29  63.1  76.2 -2.1     -86.7   141     3772   22 48 41

22 51 10  J0529+3209   03 26 29  63.5  78.5 -2.1     -85.0    -9     3772   22 51 19
22 52 40  ---          03 27 59  63.8  78.6 -2.0     -85.1    81     3793   22 51 11

22 52 40  INBEAM       03 27 59  63.4  76.2 -2.1     -86.9   -10     3793   22 52 50
22 55 10  ---          03 30 30  63.9  76.3 -2.0     -87.2   140     3829   22 52 41

22 55 50  J0529+3209   03 31 10  64.5  78.7 -2.0     -85.5    30     3829   22 55 50
22 56 50  ---          03 32 10  64.7  78.7 -2.0     -85.6    60     3845   22 55 51

22 56 50  FRB121102    03 32 10  64.2  76.4 -2.0     -87.3   -10     3845   22 57 00
22 59 20  ---          03 34 40  64.8  76.4 -2.0     -87.6   140     3881   22 56 51

22 59 20  J0529+3209   03 34 40  65.2  78.8 -1.9     -85.8   -10     3881   22 59 30
23 00 50  ---          03 36 11  65.6  78.9 -1.9     -86.0    80     3901   22 59 21

23 01 50  J0403+2600   03 37 11  82.5 125.8 -0.5     -51.0    19     3901   23 01 50
23 03 50  =0400+258    03 39 11  82.8 128.0 -0.4     -49.0   120     3932   23 01 51

23 04 50  J0529+3209   03 40 11  66.4  79.0 -1.8     -86.4    17     3932   23 04 50
23 06 20  ---          03 41 41  66.7  79.1 -1.8     -86.5    90     3956   23 04 51

23 06 20  FRB121102    03 41 41  66.2  76.5 -1.9     -88.5   -10     3956   23 06 30
23 08 50  ---          03 44 12  66.8  76.6 -1.8     -88.8   140     3992   23 06 21

23 08 50  J0529+3209   03 44 12  67.3  79.1 -1.8     -86.8   -10     3992   23 09 00
23 10 20  ---          03 45 42  67.6  79.2 -1.8     -86.9    80     4012   23 08 51

23 10 20  FRB121102    03 45 42  67.1  76.6 -1.8     -89.0   -10     4012   23 10 30
23 12 50  ---          03 48 13  67.6  76.6 -1.8     -89.3   140     4048   23 10 21

23 13 30  J0529+3209   03 48 53  68.2  79.3 -1.7     -87.3    30     4048   23 13 30
23 14 30  ---          03 49 53  68.5  79.3 -1.7     -87.4    60     4064   23 13 31

23 14 30  FRB121102    03 49 53  68.0  76.6 -1.7     -89.5   -10     4064   23 14 40
23 17 00  ---          03 52 23  68.5  76.6 -1.7     -89.9   140     4100   23 14 31

23 17 00  J0529+3209   03 52 23  69.0  79.4 -1.6     -87.7   -10     4100   23 17 10
23 18 30  ---          03 53 53  69.3  79.4 -1.6     -87.8    80     4120   23 17 01

23 18 30  INBEAM       03 53 53  68.8  76.6 -1.7     -90.2   -10     4120   23 18 40
23 21 00  ---          03 56 24  69.3  76.6 -1.6     -90.5   140     4156   23 18 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

23 21 40  J0529+3209   03 57 04  70.0  79.5 -1.6     -88.2    30     4156   23 21 40
23 22 40  ---          03 58 04  70.2  79.5 -1.5     -88.3    60     4172   23 21 41

23 22 40  FRB121102    03 58 04  69.7  76.6 -1.6     -90.7   -10     4172   23 22 50
23 25 10  ---          04 00 35  70.2  76.6 -1.5     -91.0   140     4208   23 22 41

23 25 10  J0529+3209   04 00 35  70.7  79.5 -1.5     -88.6   -10     4208   23 25 20
23 26 40  ---          04 02 05  71.0  79.6 -1.5     -88.8    80     4229   23 25 11

23 27 40  J0403+2600   04 03 05  85.4 176.4 -0.0      -3.4   -17     4229   23 27 57
23 29 40  =0400+258    04 05 05  85.4 182.1  0.0       2.0   103     4255   23 27 41

23 30 40  J0529+3209   04 06 05  71.9  79.6 -1.4     -89.3   -21     4255   23 31 01
23 32 10  ---          04 07 36  72.2  79.6 -1.4     -89.5    69     4273   23 30 41

23 32 10  FRB121102    04 07 36  71.7  76.5 -1.4     -92.1   -10     4273   23 32 20
23 34 40  ---          04 10 06  72.2  76.4 -1.4     -92.5   140     4309   23 32 11

23 34 40  J0529+3209   04 10 06  72.7  79.6 -1.3     -89.8   -10     4309   23 34 50
23 36 10  ---          04 11 36  73.0  79.6 -1.3     -90.0    80     4330   23 34 41

23 36 10  FRB121102    04 11 36  72.5  76.4 -1.4     -92.8   -10     4330   23 36 20
23 38 40  ---          04 14 07  73.0  76.3 -1.3     -93.2   140     4366   23 36 11

23 39 20  J0529+3209   04 14 47  73.7  79.6 -1.3     -90.4    30     4366   23 39 20
23 40 20  ---          04 15 47  73.9  79.6 -1.3     -90.5    60     4381   23 39 21

23 40 20  FRB121102    04 15 47  73.4  76.2 -1.3     -93.5   -10     4381   23 40 30
23 42 50  ---          04 18 17  73.9  76.1 -1.3     -93.9   140     4417   23 40 21

23 42 50  J0529+3209   04 18 17  74.5  79.6 -1.2     -90.9   -10     4417   23 43 00
23 44 20  ---          04 19 48  74.8  79.6 -1.2     -91.1    80     4438   23 42 51

23 44 20  INBEAM       04 19 48  74.2  75.9 -1.2     -94.3   -10     4438   23 44 30
23 46 50  ---          04 22 18  74.7  75.7 -1.2     -94.8   140     4474   23 44 21

23 47 30  J0529+3209   04 22 58  75.5  79.5 -1.1     -91.6    29     4474   23 47 30
23 48 30  ---          04 23 58  75.7  79.5 -1.1     -91.8    60     4489   23 47 31

23 48 30  FRB121102    04 23 58  75.1  75.7 -1.2     -95.1   -11     4489   23 48 41
23 51 00  ---          04 26 29  75.6  75.5 -1.1     -95.6   139     4525   23 48 31

23 51 00  J0529+3209   04 26 29  76.2  79.4 -1.1     -92.2   -11     4525   23 51 11
23 52 30  ---          04 27 59  76.5  79.4 -1.0     -92.4    79     4546   23 51 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  14 Mar 2021   Day  73 ---

23 54 30  J0403+2600   04 29 59  82.7 232.5  0.4      49.5     3     4546   23 54 30
23 56 30  =0400+258    04 32 00  82.4 234.7  0.5      51.4   120     4576   23 54 31

23 58 30  J0529+3209   04 34 00  77.8  79.1 -0.9     -93.5     1     4576   23 58 30
23 59 59  ---          04 35 30  78.1  79.0 -0.9     -93.8    89     4600   23 58 31

 --- Mon  15 Mar 2021   Day  74 ---

00 00 00  FRB121102    04 35 30  77.5  74.6 -1.0     -97.7   -11     4600   00 00 11
00 02 30  ---          04 38 01  78.0  74.2 -0.9     -98.4   139     4635   00 00 00

00 03 10  J0529+3209   04 38 41  78.8  78.7 -0.9     -94.5    29     4635   00 03 10
00 04 10  ---          04 39 41  79.0  78.6 -0.9     -94.7    60     4651   00 03 11

00 04 10  FRB121102    04 39 41  78.3  74.0 -0.9     -98.9   -11     4651   00 04 21
00 06 40  ---          04 42 11  78.9  73.6 -0.9     -99.7   139     4687   00 04 11

00 06 40  J0529+3209   04 42 11  79.5  78.4 -0.8     -95.3   -11     4687   00 06 51
00 08 10  ---          04 43 42  79.8  78.2 -0.8     -95.6    79     4707   00 06 41

00 08 10  INBEAM       04 43 42  79.2  73.1 -0.8    -100.3   -12     4707   00 08 22
00 10 40  ---          04 46 12  79.7  72.6 -0.8    -101.2   138     4743   00 08 11

00 11 20  J0529+3209   04 46 52  80.5  77.8 -0.7     -96.5    28     4743   00 11 20
00 12 20  ---          04 47 52  80.7  77.7 -0.7     -96.7    60     4758   00 11 21

00 12 20  FRB121102    04 47 52  80.0  72.4 -0.8    -101.6   -12     4758   00 12 32
00 14 50  ---          04 50 23  80.5  71.7 -0.7    -102.6   138     4794   00 12 21

00 14 50  J0529+3209   04 50 23  81.2  77.2 -0.7     -97.5   -12     4794   00 15 02
00 16 20  ---          04 51 53  81.6  77.0 -0.6     -98.0    78     4814   00 14 51

00 19 20  J0403+2600   04 54 53  78.0 250.7  0.8      64.7    49     4814   00 19 20
00 21 20  =0400+258    04 56 54  77.6 251.6  0.9      65.4   120     4845   00 19 21

00 24 20  J0529+3209   04 59 54  83.2  74.8 -0.5    -101.1    47     4845   00 24 20
00 25 50  ---          05 01 25  83.5  74.3 -0.5    -101.9    90     4868   00 24 21

00 25 50  FRB121102    05 01 25  82.8  67.5 -0.5    -108.3   -13     4868   00 26 03
00 28 20  ---          05 03 55  83.3  66.0 -0.5    -110.1   137     4903   00 25 51

00 28 20  J0529+3209   05 03 55  84.1  73.2 -0.4    -103.3   -13     4903   00 28 33
00 29 50  ---          05 05 25  84.4  72.5 -0.4    -104.2    77     4923   00 28 21
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

00 29 50  FRB121102    05 05 25  83.6  65.1 -0.5    -111.2   -13     4923   00 30 03
00 32 20  ---          05 07 56  84.0  63.2 -0.4    -113.4   137     4958   00 29 51

00 32 20  J0529+3209   05 07 56  84.9  71.0 -0.4    -106.0   -13     4958   00 32 33
00 33 50  ---          05 09 26  85.2  69.9 -0.4    -107.3    77     4978   00 32 21

00 33 50  FRB121102    05 09 26  84.3  62.0 -0.4    -114.9   -14     4978   00 34 04
00 36 20  ---          05 11 56  84.8  59.5 -0.4    -117.7   136     5013   00 33 51

00 36 20  J0529+3209   05 11 56  85.7  67.8 -0.3    -109.7   -14     5013   00 36 34
00 37 50  ---          05 13 27  86.0  66.3 -0.3    -111.5    76     5033   00 36 21

00 37 50  INBEAM       05 13 27  85.1  57.5 -0.3    -119.9   -14     5033   00 38 04
00 40 20  ---          05 15 57  85.5  54.1 -0.3    -123.6   136     5068   00 37 51

00 40 20  J0529+3209   05 15 57  86.5  63.1 -0.2    -115.0   -14     5068   00 40 34
00 41 50  ---          05 17 27  86.8  60.7 -0.2    -117.5    76     5087   00 40 21

00 41 50  FRB121102    05 17 27  85.8  52.1 -0.3    -125.8   -14     5087   00 42 04
00 44 20  ---          05 19 58  86.2  47.5 -0.2    -130.8   136     5122   00 41 51

00 44 20  J0529+3209   05 19 58  87.2  55.6 -0.2    -123.0   -13     5122   00 44 33
00 45 50  ---          05 21 28  87.5  51.7 -0.2    -127.1    77     5142   00 44 21

00 48 50  J0403+2600   05 24 28  71.8 260.4  1.3      70.8    24     5142   00 48 50
00 50 50  =0400+258    05 26 29  71.4 260.9  1.4      71.0   120     5173   00 48 51

00 53 50  J0529+3209   05 29 29  88.4 370.4 -0.0    -169.4    86     5173   00 53 50
00 55 20  ---          05 30 59  88.5 358.7  0.0     178.7    90     5196   00 53 51

00 55 20  FRB121102    05 30 59  87.4 371.1 -0.0    -168.6   -16     5196   00 55 36
00 57 50  ---          05 33 30  87.5 359.3  0.0     179.3   134     5231   00 55 21

00 57 50  J0529+3209   05 33 30  88.4 340.0  0.0     159.6   -23     5231   00 58 13
00 59 20  ---          05 35 00  88.2 330.3  0.1     149.8    67     5248   00 57 51

00 59 20  FRB121102    05 35 00  87.4 352.2  0.0     172.0   -22     5248   00 59 42
01 01 50  ---          05 37 30  87.3 341.0  0.1     160.5   128     5281   00 59 21

01 02 30  J0529+3209   05 38 11  87.8 315.1  0.1     134.1    15     5281   01 02 30
01 03 30  ---          05 39 11  87.6 311.5  0.1     130.4    60     5297   01 02 31

01 03 30  FRB121102    05 39 11  87.2 334.3  0.1     153.5   -23     5297   01 03 53
01 06 00  ---          05 41 41  86.9 325.6  0.1     144.5   127     5329   01 03 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

01 06 00  J0529+3209   05 41 41  87.2 304.4  0.2     123.0   -23     5329   01 06 23
01 07 30  ---          05 43 11  86.9 301.2  0.2     119.5    67     5347   01 06 01

01 07 30  INBEAM       05 43 11  86.7 321.1  0.2     139.8   -22     5347   01 07 52
01 10 00  ---          05 45 42  86.3 314.9  0.2     133.2   128     5379   01 07 31

01 10 40  J0529+3209   05 46 22  86.3 296.0  0.3     114.0    19     5379   01 10 40
01 11 40  ---          05 47 22  86.1 294.7  0.3     112.6    60     5395   01 10 41

01 11 40  FRB121102    05 47 22  86.1 311.3  0.2     129.4   -19     5395   01 11 59
01 14 10  ---          05 49 52  85.7 306.9  0.3     124.7   131     5429   01 11 41

01 14 10  J0529+3209   05 49 52  85.7 292.0  0.3     109.6   -19     5429   01 14 29
01 15 40  ---          05 51 23  85.4 290.7  0.3     108.1    71     5447   01 14 11

01 16 40  J0403+2600   05 52 23  65.9 265.8  1.8      72.8    14     5447   01 16 40
01 18 40  =0400+258    05 54 23  65.4 266.1  1.8      72.9   120     5478   01 16 41

01 19 40  J0529+3209   05 55 23  84.5 288.0  0.4     104.8    14     5478   01 19 40
01 21 10  ---          05 56 54  84.2 287.2  0.4     103.8    90     5501   01 19 41

01 21 10  FRB121102    05 56 54  84.4 298.4  0.4     115.3   -16     5501   01 21 26
01 23 40  ---          05 59 24  83.9 296.3  0.4     112.8   134     5536   01 21 11

01 23 40  J0529+3209   05 59 24  83.7 286.1  0.5     102.3   -15     5536   01 23 55
01 25 10  ---          06 00 54  83.4 285.5  0.5     101.6    75     5555   01 23 41

01 25 10  FRB121102    06 00 54  83.6 295.2  0.5     111.5   -15     5555   01 25 25
01 27 40  ---          06 03 25  83.1 293.6  0.5     109.6   135     5590   01 25 11

01 28 20  J0529+3209   06 04 05  82.7 284.4  0.6     100.1    26     5590   01 28 20
01 29 20  ---          06 05 05  82.5 284.1  0.6      99.7    60     5605   01 28 21

01 29 20  FRB121102    06 05 05  82.8 292.6  0.5     108.4   -14     5605   01 29 34
01 31 50  ---          06 07 35  82.3 291.4  0.6     106.9   136     5640   01 29 21

01 31 50  J0529+3209   06 07 35  82.0 283.5  0.6      98.7   -14     5640   01 32 04
01 33 20  ---          06 09 06  81.7 283.2  0.6      98.2    76     5660   01 31 51

01 33 20  INBEAM       06 09 06  82.0 290.9  0.6     106.2   -13     5660   01 33 33
01 35 50  ---          06 11 36  81.5 289.9  0.6     104.8   137     5695   01 33 21

01 36 30  J0529+3209   06 12 16  81.0 282.6  0.7      97.2    27     5695   01 36 30
01 37 30  ---          06 13 16  80.8 282.4  0.7      96.9    60     5711   01 36 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

01 37 30  FRB121102    06 13 16  81.2 289.2  0.7     103.9   -13     5711   01 37 43
01 40 00  ---          06 15 47  80.7 288.4  0.7     102.8   137     5746   01 37 31

01 40 00  J0529+3209   06 15 47  80.3 282.1  0.7      96.2   -12     5746   01 40 12
01 41 30  ---          06 17 17  80.0 281.9  0.8      95.8    78     5766   01 40 01

01 42 30  J0403+2600   06 18 17  60.3 269.6  2.2      73.3    13     5766   01 42 30
01 44 30  =0400+258    06 20 17  59.9 269.8  2.3      73.3   120     5797   01 42 31

01 45 30  J0529+3209   06 21 18  79.1 281.4  0.8      94.8    14     5797   01 45 30
01 47 00  ---          06 22 48  78.8 281.3  0.9      94.5    90     5820   01 45 31

01 47 00  FRB121102    06 22 48  79.2 286.8  0.8     100.2   -12     5820   01 47 12
01 49 30  ---          06 25 18  78.7 286.3  0.9      99.4   138     5856   01 47 01

01 49 30  J0529+3209   06 25 18  78.3 281.1  0.9      94.0   -12     5856   01 49 42
01 51 00  ---          06 26 49  78.0 281.0  0.9      93.7    78     5876   01 49 31

01 51 00  FRB121102    06 26 49  78.4 286.1  0.9      99.0   -11     5876   01 51 11
01 53 30  ---          06 29 19  77.9 285.7  0.9      98.2   139     5912   01 51 01

01 54 10  J0529+3209   06 29 59  77.3 280.8  1.0      93.1    29     5912   01 54 10
01 55 10  ---          06 30 59  77.1 280.8  1.0      92.9    60     5927   01 54 11

01 55 10  FRB121102    06 30 59  77.5 285.4  1.0      97.8   -11     5927   01 55 21
01 57 40  ---          06 33 30  77.0 285.1  1.0      97.2   139     5963   01 55 11

01 57 40  J0529+3209   06 33 30  76.6 280.7  1.0      92.4   -11     5963   01 57 51
01 59 10  ---          06 35 00  76.2 280.6  1.1      92.2    79     5983   01 57 41

01 59 10  INBEAM       06 35 00  76.7 285.1  1.0      96.9   -11     5983   01 59 21
02 01 40  ---          06 37 30  76.1 284.8  1.1      96.3   139     6019   01 59 11

02 02 20  J0529+3209   06 38 10  75.6 280.5  1.1      91.7    29     6019   02 02 20
02 03 20  ---          06 39 11  75.4 280.5  1.1      91.5    60     6034   02 02 21

02 03 20  FRB121102    06 39 11  75.8 284.6  1.1      95.8   -11     6034   02 03 31
02 05 50  ---          06 41 41  75.3 284.4  1.1      95.3   139     6070   02 03 21

02 05 50  J0529+3209   06 41 41  74.8 280.4  1.2      91.1   -11     6070   02 06 01
02 07 20  ---          06 43 11  74.5 280.4  1.2      90.9    79     6091   02 05 51

02 08 20  J0403+2600   06 44 11  54.7 272.7  2.7      73.1    13     6091   02 08 20
02 10 20  =0400+258    06 46 12  54.3 272.9  2.7      73.0   120     6121   02 08 21
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

02 11 20  J0529+3209   06 47 12  73.7 280.4  1.3      90.4    14     6121   02 11 20
02 12 50  ---          06 48 42  73.3 280.4  1.3      90.2    90     6145   02 11 21

02 20 50  DA193        06 56 43  74.8 311.1  1.0     122.4   448     6145   02 20 50
02 23 50  ---          06 59 44  74.3 310.0  1.0     120.9   180     6191   02 20 51

02 24 50  J0403+2600   07 00 44  51.2 274.5  2.9      72.7     7     6191   02 24 50
02 26 50  =0400+258    07 02 44  50.7 274.7  3.0      72.7   120     6222   02 24 51

02 27 50  J0529+3209   07 03 45  70.2 280.5  1.5      88.3    14     6222   02 27 50
02 29 50  ---          07 05 45  69.7 280.5  1.6      88.1   120     6253   02 27 51

02 29 50  FRB121102    07 05 45  70.3 283.4  1.5      91.1   -10     6253   02 30 00
02 32 20  ---          07 08 15  69.7 283.4  1.6      90.7   140     6289   02 29 51

02 32 20  J0529+3209   07 08 15  69.2 280.6  1.6      87.8   -10     6289   02 32 30
02 33 50  ---          07 09 46  68.9 280.6  1.6      87.6    80     6310   02 32 21

02 33 50  FRB121102    07 09 46  69.4 283.4  1.6      90.5   -10     6310   02 34 00
02 36 20  ---          07 12 16  68.9 283.4  1.6      90.2   140     6346   02 33 51

02 36 20  J0529+3209   07 12 16  68.4 280.7  1.7      87.3   -10     6346   02 36 30
02 37 50  ---          07 13 46  68.0 280.7  1.7      87.2    80     6366   02 36 21

02 37 50  FRB121102    07 13 46  68.6 283.4  1.7      89.9   -10     6366   02 38 00
02 40 20  ---          07 16 17  68.1 283.4  1.7      89.6   140     6402   02 37 51

02 40 20  J0529+3209   07 16 17  67.5 280.8  1.8      86.9   -10     6402   02 40 30
02 41 50  ---          07 17 47  67.2 280.9  1.8      86.7    80     6423   02 40 21

02 41 50  INBEAM       07 17 47  67.7 283.4  1.7      89.5   -10     6423   02 42 00
02 44 20  ---          07 20 17  67.2 283.5  1.8      89.1   140     6459   02 41 51

02 44 20  J0529+3209   07 20 17  66.7 280.9  1.8      86.5   -10     6459   02 44 30
02 45 50  ---          07 21 48  66.3 281.0  1.8      86.3    80     6480   02 44 21

02 45 50  FRB121102    07 21 48  66.9 283.4  1.8      88.9   -10     6480   02 46 00
02 48 20  ---          07 24 18  66.4 283.4  1.8      88.6   140     6516   02 45 51

02 48 20  J0529+3209   07 24 18  65.8 281.1  1.9      86.1   -10     6516   02 48 30
02 49 50  ---          07 25 48  65.5 281.1  1.9      85.9    80     6536   02 48 21

02 50 50  J0403+2600   07 26 48  45.6 277.2  3.4      71.9    13     6536   02 50 50
02 53 30  =0400+258    07 29 29  45.0 277.4  3.4      71.8   160     6578   02 50 51
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

02 54 30  J0529+3209   07 30 29  64.5 281.3  2.0      85.5    13     6578   02 54 30
02 56 00  ---          07 31 59  64.2 281.4  2.0      85.3    90     6601   02 54 31

02 56 00  FRB121102    07 31 59  64.8 283.6  2.0      87.6    -9     6601   02 56 09
02 58 30  ---          07 34 30  64.3 283.6  2.0      87.3   141     6637   02 56 01

02 58 30  J0529+3209   07 34 30  63.7 281.5  2.1      85.1    -9     6637   02 58 39
03 00 00  ---          07 36 00  63.3 281.5  2.1      84.9    81     6658   02 58 31

03 00 00  FRB121102    07 36 00  63.9 283.7  2.0      87.2    -9     6658   03 00 09
03 02 30  ---          07 38 30  63.4 283.7  2.1      86.9   141     6694   03 00 01

03 02 30  J0529+3209   07 38 30  62.8 281.6  2.1      84.7    -9     6694   03 02 39
03 04 00  ---          07 40 01  62.5 281.7  2.2      84.5    81     6715   03 02 31

03 04 00  FRB121102    07 40 01  63.1 283.8  2.1      86.7    -9     6715   03 04 09
03 06 30  ---          07 42 31  62.6 283.8  2.2      86.4   141     6751   03 04 01

03 06 30  J0529+3209   07 42 31  62.0 281.8  2.2      84.3    -9     6751   03 06 39
03 08 00  ---          07 44 01  61.7 281.9  2.2      84.2    81     6772   03 06 31

03 08 00  INBEAM       07 44 01  62.2 283.9  2.2      86.3    -9     6772   03 08 09
03 10 30  ---          07 46 32  61.7 284.0  2.2      86.0   141     6809   03 08 01

03 10 30  J0529+3209   07 46 32  61.1 282.0  2.3      83.9    -9     6809   03 10 39
03 12 00  ---          07 48 02  60.8 282.1  2.3      83.8    81     6829   03 10 31

03 12 00  FRB121102    07 48 02  61.4 284.0  2.2      85.8    -9     6829   03 12 09
03 14 30  ---          07 50 32  60.9 284.1  2.3      85.6   141     6866   03 12 01

03 14 30  J0529+3209   07 50 32  60.3 282.2  2.3      83.6    -9     6866   03 14 39
03 16 00  ---          07 52 02  60.0 282.3  2.4      83.4    81     6887   03 14 31

03 17 00  J0403+2600   07 53 03  40.0 279.8  3.8      70.7    13     6887   03 17 00
03 19 40  =0400+258    07 55 43  39.4 280.0  3.9      70.6   160     6928   03 17 01

03 20 40  J0529+3209   07 56 43  59.0 282.5  2.4      83.0    13     6928   03 20 40
03 22 10  ---          07 58 13  58.7 282.6  2.5      82.9    90     6951   03 20 41

03 22 10  FRB121102    07 58 13  59.3 284.4  2.4      84.7    -9     6951   03 22 19
03 24 40  ---          08 00 44  58.8 284.4  2.5      84.5   141     6987   03 22 11

03 24 40  J0529+3209   08 00 44  58.1 282.7  2.5      82.6    -9     6987   03 24 49
03 26 10  ---          08 02 14  57.8 282.8  2.5      82.5    81     7008   03 24 41
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

03 26 10  FRB121102    08 02 14  58.5 284.5  2.5      84.3    -9     7008   03 26 19
03 28 40  ---          08 04 45  57.9 284.6  2.5      84.1   141     7045   03 26 11

03 28 40  J0529+3209   08 04 45  57.3 282.9  2.6      82.3    -9     7045   03 28 49
03 30 10  ---          08 06 15  57.0 283.0  2.6      82.1    81     7065   03 28 41

03 30 10  FRB121102    08 06 15  57.6 284.7  2.5      83.9    -9     7065   03 30 19
03 32 40  ---          08 08 45  57.1 284.8  2.6      83.7   141     7102   03 30 11

03 32 40  J0529+3209   08 08 45  56.5 283.1  2.6      81.9    -9     7102   03 32 49
03 34 10  ---          08 10 15  56.1 283.2  2.7      81.8    81     7123   03 32 41

03 34 10  INBEAM       08 10 15  56.8 284.9  2.6      83.5    -9     7123   03 34 19
03 36 40  ---          08 12 46  56.3 285.0  2.7      83.3   141     7159   03 34 11

03 36 40  J0529+3209   08 12 46  55.6 283.3  2.7      81.6    -9     7159   03 36 49
03 38 10  ---          08 14 16  55.3 283.4  2.7      81.4    81     7180   03 36 41

03 38 10  FRB121102    08 14 16  56.0 285.0  2.7      83.1    -9     7180   03 38 19
03 40 40  ---          08 16 47  55.4 285.1  2.7      82.9   141     7216   03 38 11

03 40 40  J0529+3209   08 16 47  54.8 283.6  2.8      81.2    -9     7216   03 40 49
03 42 10  ---          08 18 17  54.5 283.6  2.8      81.1    81     7237   03 40 41

03 43 10  J0403+2600   08 19 17  34.5 282.3  4.2      69.4    13     7237   03 43 10
03 45 50  =0400+258    08 21 57  33.9 282.5  4.3      69.2   160     7278   03 43 11

03 46 50  J0529+3209   08 22 58  53.5 283.9  2.9      80.7    13     7278   03 46 50
03 48 20  ---          08 24 28  53.2 284.0  2.9      80.6    90     7301   03 46 51

03 48 20  FRB121102    08 24 28  53.8 285.5  2.9      82.1    -9     7301   03 48 29
03 50 50  ---          08 26 58  53.3 285.6  2.9      81.9   141     7338   03 48 21

03 50 50  J0529+3209   08 26 58  52.6 284.1  2.9      80.3    -9     7338   03 50 59
03 52 20  ---          08 28 28  52.3 284.2  3.0      80.2    81     7359   03 50 51

03 52 20  FRB121102    08 28 28  53.0 285.7  2.9      81.7    -9     7359   03 52 29
03 54 50  ---          08 30 59  52.5 285.8  3.0      81.5   141     7395   03 52 21

03 54 50  J0529+3209   08 30 59  51.8 284.4  3.0      80.0    -9     7395   03 54 59
03 56 20  ---          08 32 29  51.5 284.5  3.0      79.9    81     7416   03 54 51

03 56 20  FRB121102    08 32 29  52.2 285.9  3.0      81.3    -9     7416   03 56 29
03 58 50  ---          08 35 00  51.7 286.0  3.0      81.1   141     7452   03 56 21
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

03 58 50  J0529+3209   08 35 00  51.0 284.6  3.1      79.6    -9     7452   03 58 59
04 00 20  ---          08 36 30  50.7 284.7  3.1      79.5    81     7473   03 58 51

04 00 20  INBEAM       08 36 30  51.3 286.1  3.1      81.0    -9     7473   04 00 29
04 02 50  ---          08 39 00  50.8 286.3  3.1      80.7   141     7509   04 00 21

04 02 50  J0529+3209   08 39 00  50.1 284.9  3.1      79.3    -9     7509   04 02 59
04 04 20  ---          08 40 30  49.8 285.0  3.2      79.2    81     7530   04 02 51

04 04 20  FRB121102    08 40 30  50.5 286.3  3.1      80.6    -9     7530   04 04 29
04 06 50  ---          08 43 01  50.0 286.5  3.2      80.3   141     7567   04 04 21

04 06 50  J0529+3209   08 43 01  49.3 285.1  3.2      79.0    -9     7567   04 06 59
04 08 20  ---          08 44 31  49.0 285.2  3.2      78.8    81     7587   04 06 51

04 09 20  J0403+2600   08 45 31  29.0 284.8  4.7      67.8    13     7587   04 09 20
04 12 00  =0400+258    08 48 12  28.4 285.1  4.7      67.6   160     7629   04 09 21

04 13 00  J0529+3209   08 49 12  48.0 285.5  3.3      78.4    13     7629   04 13 00
04 14 30  ---          08 50 42  47.7 285.6  3.3      78.3    90     7652   04 13 01

04 14 30  FRB121102    08 50 42  48.4 286.9  3.3      79.6    -9     7652   04 14 39
04 17 00  ---          08 53 13  47.9 287.0  3.3      79.4   141     7688   04 14 31

04 17 00  J0529+3209   08 53 13  47.2 285.8  3.4      78.1    -9     7688   04 17 09
04 18 30  ---          08 54 43  46.9 285.8  3.4      77.9    81     7709   04 17 01

04 18 30  FRB121102    08 54 43  47.6 287.1  3.4      79.2    -9     7709   04 18 39
04 21 00  ---          08 57 13  47.1 287.3  3.4      79.0   141     7745   04 18 31

04 21 00  J0529+3209   08 57 13  46.4 286.0  3.4      77.7    -9     7745   04 21 09
04 22 30  ---          08 58 43  46.1 286.1  3.5      77.6    81     7766   04 21 01

04 22 30  FRB121102    08 58 43  46.8 287.3  3.4      78.8    -9     7766   04 22 39
04 25 00  ---          09 01 14  46.3 287.5  3.5      78.6   141     7803   04 22 31

04 25 00  J0529+3209   09 01 14  45.5 286.3  3.5      77.4    -9     7803   04 25 09
04 26 30  ---          09 02 44  45.2 286.4  3.5      77.3    81     7823   04 25 01

04 26 30  INBEAM       09 02 44  45.9 287.6  3.5      78.5    -9     7823   04 26 39
04 29 00  ---          09 05 14  45.4 287.8  3.5      78.2   141     7860   04 26 31

04 29 00  J0529+3209   09 05 14  44.7 286.5  3.6      77.0    -9     7860   04 29 09
04 30 30  ---          09 06 45  44.4 286.6  3.6      76.9    81     7881   04 29 01
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

04 30 30  FRB121102    09 06 45  45.1 287.8  3.6      78.1    -9     7881   04 30 39
04 33 00  ---          09 09 15  44.6 288.0  3.6      77.9   141     7917   04 30 31

04 33 00  J0529+3209   09 09 15  43.9 286.8  3.6      76.7    -9     7917   04 33 09
04 34 30  ---          09 10 45  43.6 286.9  3.7      76.6    81     7938   04 33 01

04 35 30  J0403+2600   09 11 46  23.6 287.4  5.1      66.1    13     7938   04 35 30
04 38 10  =0400+258    09 14 26  23.0 287.6  5.2      65.9   160     7979   04 35 31

04 39 10  J0529+3209   09 15 26  42.6 287.2  3.7      76.2    13     7979   04 39 10
04 40 40  ---          09 16 56  42.3 287.3  3.8      76.0    90     8002   04 39 11

04 40 40  FRB121102    09 16 56  43.0 288.5  3.7      77.1    -9     8002   04 40 49
04 43 10  ---          09 19 27  42.5 288.6  3.8      76.9   141     8039   04 40 41

04 43 10  J0529+3209   09 19 27  41.8 287.5  3.8      75.8    -9     8039   04 43 19
04 44 40  ---          09 20 57  41.5 287.6  3.8      75.7    81     8059   04 43 11

04 44 40  FRB121102    09 20 57  42.2 288.7  3.8      76.8    -9     8059   04 44 49
04 47 10  ---          09 23 27  41.7 288.9  3.8      76.5   141     8096   04 44 41

04 47 10  J0529+3209   09 23 27  41.0 287.8  3.9      75.5    -9     8096   04 47 19
04 48 40  ---          09 24 58  40.7 287.9  3.9      75.3    81     8117   04 47 11

04 48 40  FRB121102    09 24 58  41.4 289.0  3.9      76.4    -9     8117   04 48 49
04 51 10  ---          09 27 28  40.9 289.2  3.9      76.2   141     8153   04 48 41

04 51 10  J0529+3209   09 27 28  40.1 288.1  3.9      75.1   -10     8153   04 51 20
04 52 40  ---          09 28 58  39.8 288.2  4.0      75.0    80     8174   04 51 11

04 52 40  INBEAM       09 28 58  40.6 289.3  3.9      76.0    -9     8174   04 52 49
04 55 10  ---          09 31 29  40.1 289.5  4.0      75.8   141     8210   04 52 41

04 55 10  J0529+3209   09 31 29  39.3 288.4  4.0      74.8    -9     8210   04 55 19
04 56 40  ---          09 32 59  39.0 288.5  4.0      74.6    81     8231   04 55 11

04 56 40  FRB121102    09 32 59  39.8 289.5  4.0      75.6    -9     8231   04 56 49
04 59 10  ---          09 35 29  39.3 289.7  4.0      75.4   141     8267   04 56 41

04 59 10  J0529+3209   09 35 29  38.5 288.7  4.1      74.4   -10     8267   04 59 20
05 00 40  ---          09 37 00  38.2 288.8  4.1      74.3    80     8288   04 59 11

05 01 40  J0403+2600   09 38 00  18.2 290.0  5.6      64.1    13     8288   05 01 40
05 04 20  =0400+258    09 40 40  17.7 290.3  5.6      63.9   160     8329   05 01 41
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

05 05 20  J0529+3209   09 41 40  37.2 289.1  4.2      73.9    13     8329   05 05 20
05 06 50  ---          09 43 11  36.9 289.2  4.2      73.7    90     8352   05 05 21

05 08 20  B0329+54     09 44 41  23.2 321.0  6.2      69.2    55     8352   05 08 20
05 12 20  ---          09 48 42  22.6 321.3  6.2      68.5   240     8414   05 08 21

05 13 20  DA193        09 49 42  42.4 297.8  3.9      82.1    13     8414   05 13 20
05 16 20  ---          09 52 42  41.9 297.9  3.9      81.7   180     8460   05 13 21

05 16 50  DA193        09 53 12  41.8 298.0  3.9      81.7    24     8460   05 16 50
05 18 20  ---          09 54 43  41.5 298.0  4.0      81.5    90     8484   05 16 51

05 19 20  J0529+3209   09 55 43  34.4 290.2  4.4      72.6    38     8484   05 19 20
05 20 50  ---          09 57 13  34.1 290.3  4.4      72.5    90     8507   05 19 21

05 20 50  FRB121102    09 57 13  34.9 291.2  4.4      73.4   -10     8507   05 21 00
05 23 20  ---          09 59 43  34.4 291.4  4.4      73.1   140     8543   05 20 51

05 23 20  J0529+3209   09 59 43  33.6 290.5  4.5      72.3   -10     8543   05 23 30
05 24 50  ---          10 01 14  33.3 290.6  4.5      72.1    80     8563   05 23 21

05 24 50  FRB121102    10 01 14  34.1 291.5  4.5      73.0   -10     8563   05 25 00
05 27 20  ---          10 03 44  33.6 291.7  4.5      72.7   140     8599   05 24 51

05 27 20  J0529+3209   10 03 44  32.8 290.8  4.5      71.9   -10     8599   05 27 30
05 28 50  ---          10 05 14  32.5 290.9  4.6      71.8    80     8620   05 27 21

05 28 50  FRB121102    10 05 14  33.3 291.8  4.5      72.6   -10     8620   05 29 00
05 31 20  ---          10 07 45  32.8 292.0  4.6      72.4   140     8656   05 28 51

05 31 20  J0529+3209   10 07 45  32.0 291.1  4.6      71.5   -10     8656   05 31 30
05 32 50  ---          10 09 15  31.7 291.2  4.6      71.4    80     8677   05 31 21

05 32 50  INBEAM       10 09 15  32.5 292.2  4.6      72.2   -10     8677   05 33 00
05 35 20  ---          10 11 45  32.0 292.3  4.6      72.0   140     8713   05 32 51

05 35 20  J0529+3209   10 11 45  31.2 291.4  4.7      71.2   -10     8713   05 35 30
05 36 50  ---          10 13 16  30.9 291.5  4.7      71.0    80     8733   05 35 21

05 36 50  FRB121102    10 13 16  31.7 292.4  4.7      71.8   -10     8733   05 37 00
05 39 20  ---          10 15 46  31.2 292.6  4.7      71.6   140     8769   05 36 51

05 39 20  J0529+3209   10 15 46  30.4 291.7  4.7      70.8   -10     8769   05 39 30
05 40 50  ---          10 17 16  30.1 291.9  4.8      70.7    80     8790   05 39 21
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

05 41 50  DA193        10 18 16  37.0 299.0  4.4      78.3    38     8790   05 41 50
05 43 50  ---          10 20 17  36.7 299.1  4.4      78.1   120     8821   05 41 51

05 44 50  J0529+3209   10 21 17  29.3 292.2  4.8      70.3    38     8821   05 44 50
05 46 20  ---          10 22 47  29.0 292.3  4.9      70.1    90     8844   05 44 51

05 46 20  FRB121102    10 22 47  29.8 293.2  4.8      70.9   -10     8844   05 46 30
05 48 50  ---          10 25 18  29.3 293.4  4.9      70.7   140     8880   05 46 21

05 48 50  J0529+3209   10 25 18  28.5 292.5  4.9      69.9   -10     8880   05 49 00
05 50 20  ---          10 26 48  28.2 292.6  4.9      69.8    80     8901   05 48 51

05 50 20  FRB121102    10 26 48  29.0 293.5  4.9      70.5   -10     8901   05 50 30
05 52 50  ---          10 29 18  28.5 293.7  4.9      70.3   140     8937   05 50 21

05 52 50  J0529+3209   10 29 18  27.7 292.8  5.0      69.5   -10     8937   05 53 00
05 54 20  ---          10 30 48  27.4 293.0  5.0      69.4    80     8958   05 52 51

05 54 20  FRB121102    10 30 48  28.2 293.8  5.0      70.1   -10     8958   05 54 30
05 56 50  ---          10 33 19  27.7 294.0  5.0      69.9   140     8994   05 54 21

05 56 50  J0529+3209   10 33 19  26.9 293.2  5.0      69.1   -10     8994   05 57 00
05 58 20  ---          10 34 49  26.6 293.3  5.1      69.0    80     9014   05 56 51

05 58 20  INBEAM       10 34 49  27.4 294.2  5.0      69.7   -10     9014   05 58 30
06 00 50  ---          10 37 20  26.9 294.4  5.1      69.5   140     9050   05 58 21

06 00 50  J0529+3209   10 37 20  26.1 293.5  5.1      68.8   -10     9050   06 01 00
06 02 20  ---          10 38 50  25.8 293.7  5.1      68.6    80     9071   06 00 51

06 02 20  FRB121102    10 38 50  26.6 294.5  5.1      69.3   -10     9071   06 02 30
06 04 50  ---          10 41 20  26.2 294.7  5.1      69.1   140     9107   06 02 21

06 04 50  J0529+3209   10 41 20  25.3 293.9  5.2      68.4   -10     9107   06 05 00
06 06 20  ---          10 42 50  25.0 294.0  5.2      68.2    80     9128   06 04 51

06 07 20  DA193        10 43 51  32.3 300.4  4.8      75.0    37     9128   06 07 20
06 09 20  ---          10 45 51  31.9 300.5  4.8      74.8   120     9159   06 07 21

06 10 20  J0529+3209   10 46 51  24.2 294.3  5.3      67.8    37     9159   06 10 20
06 11 50  ---          10 48 21  23.9 294.5  5.3      67.7    90     9182   06 10 21

06 11 50  FRB121102    10 48 21  24.8 295.3  5.3      68.4   -10     9182   06 12 00
06 14 20  ---          10 50 52  24.3 295.5  5.3      68.1   140     9218   06 11 51
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

06 14 20  J0529+3209   10 50 52  23.4 294.7  5.3      67.5   -10     9218   06 14 30
06 15 50  ---          10 52 22  23.1 294.8  5.4      67.3    80     9238   06 14 21

06 15 50  FRB121102    10 52 22  24.0 295.6  5.3      68.0   -10     9238   06 16 00
06 18 20  ---          10 54 52  23.5 295.8  5.4      67.7   140     9274   06 15 51

06 18 20  J0529+3209   10 54 52  22.7 295.1  5.4      67.1   -10     9274   06 18 30
06 19 50  ---          10 56 23  22.4 295.2  5.4      66.9    80     9295   06 18 21

06 19 50  J0529+3209   10 56 23  22.4 295.2  5.4      66.9    -6     9295   06 19 56
06 21 20  ---          10 57 53  22.1 295.3  5.5      66.8    84     9317   06 19 51

06 21 20  FRB121102    10 57 53  22.9 296.1  5.4      67.4   -10     9317   06 21 30
06 23 50  ---          11 00 23  22.5 296.3  5.5      67.1   140     9353   06 21 21

06 23 50  J0529+3209   11 00 23  21.6 295.6  5.5      66.5   -10     9353   06 24 00
06 25 20  ---          11 01 54  21.3 295.7  5.5      66.4    80     9373   06 23 51

06 26 20  DA193        11 02 54  28.7 301.6  5.1      72.6    37     9373   06 26 20
06 28 20  ---          11 04 54  28.4 301.7  5.1      72.3   120     9404   06 26 21

06 29 20  J0529+3209   11 05 54  20.5 296.1  5.6      66.0    37     9404   06 29 20
06 30 50  ---          11 07 24  20.2 296.2  5.6      65.8    90     9428   06 29 21

06 30 50  FRB121102    11 07 24  21.1 296.9  5.6      66.4   -10     9428   06 31 00
06 33 20  ---          11 09 55  20.6 297.2  5.6      66.1   140     9464   06 30 51

06 33 20  J0529+3209   11 09 55  19.7 296.4  5.7      65.6   -10     9464   06 33 30
06 34 50  ---          11 11 25  19.5 296.6  5.7      65.4    80     9484   06 33 21

06 34 50  FRB121102    11 11 25  20.3 297.3  5.6      66.0   -10     9484   06 35 00
06 37 20  ---          11 13 56  19.9 297.5  5.7      65.7   140     9520   06 34 51

06 37 20  J0529+3209   11 13 56  19.0 296.8  5.7      65.1   -10     9520   06 37 30
06 38 50  ---          11 15 26  18.7 296.9  5.7      65.0    80     9541   06 37 21

06 38 50  FRB121102    11 15 26  19.6 297.7  5.7      65.6   -10     9541   06 39 00
06 41 20  ---          11 17 56  19.1 297.9  5.7      65.3   140     9577   06 38 51

06 41 20  J0529+3209   11 17 56  18.2 297.2  5.8      64.7   -10     9577   06 41 30
06 42 50  ---          11 19 26  17.9 297.3  5.8      64.6    80     9598   06 41 21

06 42 50  INBEAM       11 19 26  18.8 298.1  5.8      65.1   -10     9598   06 43 00
06 45 20  ---          11 21 57  18.3 298.3  5.8      64.9   140     9634   06 42 51
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

06 45 20  J0529+3209   11 21 57  17.4 297.6  5.9      64.3   -10     9634   06 45 30
06 46 50  ---          11 23 27  17.1 297.7  5.9      64.2    80     9654   06 45 21

06 46 50  FRB121102    11 23 27  18.1 298.4  5.8      64.7   -10     9654   06 47 00
06 49 20  ---          11 25 58  17.6 298.6  5.9      64.4   140     9690   06 46 51

06 49 20  J0529+3209   11 25 58  16.7 298.0  5.9      63.9   -10     9690   06 49 30
06 50 50  ---          11 27 28  16.4 298.1  5.9      63.7    80     9711   06 49 21

06 51 50  DA193        11 28 28  24.1 303.4  5.5      69.3    37     9711   06 51 50
06 53 50  ---          11 30 28  23.7 303.5  5.6      69.0   120     9742   06 51 51

06 54 50  J0529+3209   11 31 28  15.6 298.5  6.0      63.3    36     9742   06 54 50
06 56 20  ---          11 32 59  15.3 298.6  6.0      63.1    90     9765   06 54 51

06 56 20  FRB121102    11 32 59  16.3 299.3  6.0      63.7   -10     9765   06 56 30
06 58 50  ---          11 35 29  15.8 299.6  6.0      63.4   140     9801   06 56 21

06 58 50  J0529+3209   11 35 29  14.9 298.9  6.1      62.9   -10     9801   06 59 00
07 00 20  ---          11 36 59  14.6 299.0  6.1      62.7    80     9822   06 58 51

07 00 20  FRB121102    11 36 59  15.5 299.7  6.1      63.2   -10     9822   07 00 30
07 02 50  ---          11 39 30  15.0 299.9  6.1      63.0   140     9858   07 00 21

07 02 50  J0529+3209   11 39 30  14.1 299.3  6.1      62.4   -10     9858   07 03 00
07 04 20  ---          11 41 00  13.8 299.4  6.2      62.3    80     9878   07 02 51

07 04 20  FRB121102    11 41 00  14.8 300.1  6.1      62.8   -10     9878   07 04 30
07 06 50  ---          11 43 30  14.3 300.3  6.2      62.5   140     9914   07 04 21

07 06 50  J0529+3209   11 43 30  13.4 299.7  6.2      62.0   -10     9914   07 07 00
07 08 20  ---          11 45 01  13.1 299.9  6.2      61.8    80     9935   07 06 51

07 08 20  INBEAM       11 45 01  14.0 300.5  6.2      62.3   -10     9935   07 08 30
07 10 50  ---          11 47 31  13.5 300.8  6.2      62.0   140     9971   07 08 21

07 10 50  J0529+3209   11 47 31  12.6 300.1  6.3      61.6   -10     9971   07 11 00
07 12 20  ---          11 49 01  12.3 300.3  6.3      61.4    80     9992   07 10 51

07 12 20  FRB121102    11 49 01  13.3 300.9  6.3      61.9   -10     9992   07 12 30
07 14 50  ---          11 51 32  12.8 301.2  6.3      61.6   140    10028   07 12 21

07 14 50  J0529+3209   11 51 32  11.9 300.5  6.3      61.1   -10    10028   07 15 00
07 16 20  ---          11 53 02  11.6 300.7  6.4      61.0    80    10048   07 14 51
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

07 17 20  DA193        11 54 02  19.6 305.4  6.0      65.9    36    10048   07 17 20
07 19 20  ---          11 56 02  19.2 305.6  6.0      65.7   120    10079   07 17 21

07 20 20  J0529+3209   11 57 03  10.9 301.1  6.4      60.5    36    10079   07 20 20
07 21 50  ---          11 58 33  10.6 301.3  6.5      60.3    90    10103   07 20 21

07 22 20  3C147        11 59 03  20.7 316.6  6.2      66.6     2    10103   07 22 20
07 25 30  ---          12 02 13  20.2 316.8  6.3      66.1   190    10151   07 22 21

07 26 00  DA193        12 02 44  18.0 306.1  6.1      64.8    15    10151   07 26 00
07 30 00  ---          12 06 44  17.3 306.5  6.2      64.2   240    10213   07 26 01

07 31 00  J0529+3209   12 07 44   8.9 302.3  6.6      59.3    36    10213   07 31 00
07 32 30  ---          12 09 15   8.6 302.4  6.6      59.1    90    10236   07 31 01

07 32 30  FRB121102    12 09 15   9.6 303.0  6.6      59.5   -10    10236   07 32 40
07 35 00  ---          12 11 45   9.1 303.3  6.6      59.2   140    10273   07 32 31

07 35 00  J0529+3209   12 11 45   8.2 302.7  6.7      58.8   -10    10273   07 35 10
07 36 30  ---          12 13 15   7.9 302.9  6.7      58.6    80    10293   07 35 01

07 36 30  FRB121102    12 13 15   8.9 303.4  6.7      59.1   -10    10293   07 36 40
07 39 00  ---          12 15 46   8.4 303.7  6.7      58.8   140    10329   07 36 31

07 39 00  J0529+3209   12 15 46   7.4 303.2  6.7      58.3   -10    10329   07 39 10
07 40 30  ---          12 17 16   7.2 303.3  6.8      58.2    80    10350   07 39 01

07 40 30  FRB121102    12 17 16   8.1 303.9  6.7      58.6   -10    10350   07 40 40
07 43 00  ---          12 19 46   7.7 304.2  6.8      58.3   140    10386   07 40 31

07 43 00  J0529+3209   12 19 46   6.7 303.6  6.8      57.9   -10    10386   07 43 10
07 44 30  ---          12 21 17   6.5 303.8  6.8      57.7    80    10407   07 43 01

07 44 30  INBEAM       12 21 17   7.4 304.4  6.8      58.1   -10    10407   07 44 40
07 47 00  ---          12 23 47   7.0 304.6  6.8      57.8   140    10443   07 44 31

07 47 00  J0529+3209   12 23 47   6.0 304.1  6.9      57.4   -10    10443   07 47 10
07 48 30  ---          12 25 17   5.7 304.2  6.9      57.2    80    10463   07 47 01

07 48 30  FRB121102    12 25 17   6.7 304.8  6.9      57.6   -10    10463   07 48 40
07 51 00  ---          12 27 48   6.3 305.1  6.9      57.3   140    10499   07 48 31

07 51 00  J0529+3209   12 27 48   5.3 304.5  6.9      56.9   -10    10499   07 51 10
07 52 30  ---          12 29 18   5.0 304.7  7.0      56.7    80    10520   07 51 01
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               GM080 - FRB121102
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  15 Mar 2021   Day  74 ---

07 52 30  FRB121102    12 29 18   6.0 305.2  6.9      57.1   -10    10520   07 52 40
07 55 00  ---          12 31 48   5.6 305.5  7.0      56.8   140    10556   07 52 31

07 55 00  J0529+3209   12 31 48   4.6 305.0  7.0      56.4   -10    10556   07 55 10
07 56 30  ---          12 33 19   4.3 305.2  7.0      56.2    80    10577   07 55 01

07 56 30  FRB121102    12 33 19   5.3 305.7  7.0      56.6   -10    10577   07 56 40
07 59 00  ---          12 35 49   4.9 306.0  7.0      56.3   140    10613   07 56 31

07 59 00  J0529+3209   12 35 49   3.9 305.5  7.1  H   55.9   -10    10613   07 59 10
08 00 30  ---          12 37 19   3.6 305.6  7.1  H   55.7     0    10633   07 59 01

08 00 30  FRB121102    12 37 19   4.6 306.2  7.1      56.1   -10    10633   08 00 40
08 03 00  ---          12 39 50   4.2 306.5  7.1  H   55.8     0    10669   08 00 31

08 03 00  J0529+3209   12 39 50   3.2 305.9  7.1  H   55.4   -10    10669   08 03 10
08 04 30  ---          12 41 20   2.9 306.1  7.2  H   55.2     0    10690   08 03 01

08 04 30  INBEAM       12 41 20   3.9 306.7  7.1  H   55.6   -10    10690   08 04 40
08 07 00  ---          12 43 50   3.5 307.0  7.2  H   55.2     0    10726   08 04 31

08 07 00  J0529+3209   12 43 50   2.5 306.4  7.2  H   54.9   -10    10726   08 07 10
08 08 30  ---          12 45 21   2.2 306.6  7.2  D   54.7     0    10747   08 07 01

08 08 30  FRB121102    12 45 21   3.2 307.1  7.2  H   55.0   -10    10747   08 08 40
08 11 00  ---          12 47 51   2.8 307.4  7.2  H   54.7     0    10783   08 08 31

08 12 30  FRB121102    12 49 21   2.5 307.6  7.3  H   54.5    84    10783   08 12 30
08 15 00  ---          12 51 52   2.1 307.9  7.3  D   54.2     0    10821   08 12 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess121.X2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  15  Setup file default.  Used with PCAL = off
   LO sum=   8240.00  8240.00  8304.00  8304.00  8368.00  8368.00  8432.00  8432.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  15  16  17  18  19  20  21  22  23  26

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FRB121102         05 28 41.724732   * 05 31 58.701590     05 33 21.007842       0.00
                     33 06 43.23988    * 33 08 52.54910      33 09 48.98090        0.00
                     From catalog imbedded in main SCHED input file.

 * INBEAM            05 28 36.907210   * 05 31 53.922113     05 33 16.243821       0.00
                     33 08 10.41555    * 33 10 20.07143      33 11 16.65597        0.00
                     From catalog imbedded in main SCHED input file.

 * J0529+3209        05 26 12.903667   * 05 29 28.211037     05 30 49.804396       0.00
                     32 07 26.83083    * 32 09 46.94745      32 10 47.58147        0.00
                     From catalog imbedded in main SCHED input file.

 * B0329+54          03 29 11.066308   * 03 32 59.368000     03 34 33.896560       0.00
                     54 24 37.47697    * 54 34 43.57000      54 39 04.14336        0.00
                     From catalog imbedded in main SCHED input file.

   0400+258          04 00 03.594851   * 04 03 05.586081     04 04 21.136232       0.02
 * J0403+2600        25 51 46.48888    * 26 00 01.50275      26 03 27.97338        0.03
   J0403+26          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,   2233 observations.

 * 3C147             05 38 43.517517   * 05 42 36.137894     05 44 13.439989       0.04
   J0542+4951        49 49 42.83709    * 49 51 07.23372      49 51 49.80700        0.03
   0538+498          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0542+49          GSFC 2016a X/S astro solution,   1444 observations.

   0552+398          05 52 01.407168   * 05 55 30.805611     05 56 58.454068       0.00
   J0555+3948        39 48 21.94581    * 39 48 49.16496      39 49 04.93001        0.00
 * DA193             /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0555+39          GSFC 2016a X/S astro solution, 415688 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FRB121102  sess121.X2048glob     1 2 3 4 6 7 8 9 11 12 14 15 +    11.792   839.991
  INBEAM     sess121.X2048glob     1 2 3 4 6 7 8 9 11 12 14 15 +     3.375   229.176
  J0529+3209 sess121.X2048glob     1 2 3 4 6 7 8 9 11 12 14 15 +     9.147   647.110
  B0329+54   sess121.X2048glob     1 2 3 4 6 7 8 9 15 24 25          0.150     7.417
  J0403+2600 sess121.X2048glob     1 4 6 8 9 11 12 14 15 24 25       0.933    87.889
  3C147      sess121.X2048glob     15 25                             0.103     2.335
  DA193      sess121.X2048glob     1 2 3 4 6 7 8 9 11 12 14 15 +     1.083    59.248


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FRB121102           89.9
   INBEAM              89.9
   J0529+3209          89.3
   B0329+54            74.4
   J0403+2600          69.8
   3C147               92.4
   DA193               94.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

