!*  Schedule for VLBA_FD   *!
!*  Experiment GP036B   *!
!* Schedule Version:       1.00 *!
!* Processed by SCHED version: Release of 02 July 2002 *!
!* PI:       Zsolt Paragi *!
!* Address:  JIVE *!
!*           Postbus 2 *!
!*           7990 AA Dwingeloo *!
!*           The Netherlands *!
!* Phone:    +31-521-596536 *!
!* EMAIL:    paragi@jive.nl *!
!* Fax:      +31-521-597332 *!
!* Phone during observation: +31-521-596536 *!
!* Observing mode: Continuum 18 cm; Recording mode: 256-4-2 (VLBA/MKIV). *!
!* Notes:    Global VLBI observations at 18cm. *!
!*  *!
!*           Send logs and calibration information to Zsolt Paragi. *!
!*  *!
!*  Start at 03h59m20s     Fri, 2003 May 30  Day of year  150   *!
program=GP036B  
autoallocate=off
autoreverse=off

!* The first scan is preceeded by a setup scan *!
!* that ends at the start time of the first scan  *!
!* ========= New tape starts at: 03h58m50s ========= *!

!* --- Scan from 03h58m50s to 04h09m50s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=999  calib='N'
maxcaltime= 120
fe=(1,20cm),(3,20cm)
fexfer=(2,norm)
noise=(1,low-s),(2,low-s),(3,low-s),(4,low-s)
synth=( 1,15.4),( 2, 2.4),( 3,15.4)
logging=STANDARD
nchan= 4
format=VLBA1:4
barrel=roll_off
ifdistr=(1,0),(2,0),(3,0),(4,0)
baseband=(1,1),(2,2),(3,3),(4,4)
ifchan=(1,A),(2,C),(3,A),(4,C)
sideband=(1,U),(2,U),(3,U),(4,U)
bits=(1,2),(2,2),(3,2),(4,2)
period=(1,1),(2,1),(3,1),(4,1)
level=(1,-1),(2,-1),(3,-1),(4,-1)
azcolim=   0.00  elcolim=   0.00
bbsynth=( 1,759.01),( 2,759.01),( 3,743.01),( 4,743.01)
bbfilter=(1,16M),(2,16M),(3,16M),(4,16M)
pcal=1MHZ
pcalxbit1=(1,S1),(2,S3),(3,S1),(4,S3),(5,S1),(6,S2),(7,S3),(8,S4)
pcalxbit2=(1,S2),(2,S4),(3,S2),(4,S4),(5,M1),(6,M2),(7,M3),(8,M4)
pcalxfreq1=(1,990),(2,990),(3,13990),(4,13990),(5,0),(6,0),(7,0),(8,0)
pcalxfreq2=(1,990),(2,990),(3,13990),(4,13990),(5,0),(6,0),(7,0),(8,0)
samplerate=32M
track=(1,2),(2,18),(3,3),(4,19)
tape=(2,STOP)    write=(2,off) 
tape=( 1,STOP)   write=( 1,off) head=( 1,-319)
  date = 2003May30
stop=03h58m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-319) 
stop=04h09m50s   !NEXT!

!* --- Scan from 04h10m20s to 04h15m50s   Fri, 2003 May 30 --- *!
sname='OQ208'  ra=14h07m00.394410s  dec= 28d27'14.68998"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-319)
stop=04h10m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-319) 
stop=04h15m50s   !NEXT!

!* --- Scan from 04h17m20s to 04h22m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-319)
stop=04h17m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-319) 
stop=04h22m50s   !NEXT!

!* --- Scan from 04h24m20s to 04h29m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,  31)
stop=04h24m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  31) 
stop=04h29m50s   !NEXT!

!* --- Scan from 04h30m20s to 04h46m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,  31)
stop=04h30m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  31) 
stop=04h46m50s   !NEXT!

!* --- Scan from 04h48m20s to 04h53m50s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,-271)
stop=04h48m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-271) 
stop=04h53m50s   !NEXT!

!* --- Scan from 04h55m20s to 05h11m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-271)
stop=04h55m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-271) 
stop=05h11m50s   !NEXT!

!* --- Scan from 05h13m20s to 05h18m50s   Fri, 2003 May 30 --- *!
sname='OQ208'  ra=14h07m00.394410s  dec= 28d27'14.68998"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,  79)
stop=05h13m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  79) 
stop=05h18m50s   !NEXT!

!* --- Scan from 05h20m20s to 05h25m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,  79)
stop=05h20m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  79) 
stop=05h25m50s   !NEXT!

!* --- Scan from 05h26m50s to 05h32m20s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,  79)
stop=05h26m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  79) 
stop=05h32m20s   !NEXT!

!* --- Scan from 05h34m20s to 05h39m50s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,  79)
stop=05h34m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  79) 
stop=05h39m50s   !NEXT!

!* --- Scan from 05h40m50s to 06h02m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-223)
stop=05h40m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-223) 
stop=06h02m50s   !NEXT!

!* --- Scan from 06h04m50s to 06h21m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 127)
stop=06h04m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 127) 
stop=06h21m20s   !NEXT!

!* --- Scan from 06h23m20s to 06h28m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1, 127)
stop=06h23m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 127) 
stop=06h28m50s   !NEXT!

!* --- Scan from 06h29m50s to 06h35m20s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-175)
stop=06h29m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-175) 
stop=06h35m20s   !NEXT!

!* --- Scan from 06h36m50s to 06h42m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,-175)
stop=06h36m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-175) 
stop=06h42m20s   !NEXT!

!* --- Scan from 06h43m50s to 06h54m50s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-175)
stop=06h43m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-175) 
stop=06h54m50s   !NEXT!

!* --- Scan from 06h57m20s to 07h02m50s   Fri, 2003 May 30 --- *!
sname='OQ208'  ra=14h07m00.394410s  dec= 28d27'14.68998"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 175)
stop=06h57m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 175) 
stop=07h02m50s   !NEXT!

!* --- Scan from 07h05m20s to 07h10m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1, 175)
stop=07h05m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 175) 
stop=07h10m50s   !NEXT!

!* --- Scan from 07h11m50s to 07h22m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 175)
stop=07h11m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 175) 
stop=07h22m50s   !NEXT!

!* --- Scan from 07h24m20s to 07h29m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-127)
stop=07h24m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-127) 
stop=07h29m50s   !NEXT!

!* --- Scan from 07h31m20s to 07h42m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1,-127)
stop=07h31m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-127) 
stop=07h42m20s   !NEXT!

!* --- Scan from 07h42m50s to 07h48m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1,-127)
stop=07h42m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-127) 
stop=07h48m20s   !NEXT!

!* --- Scan from 07h50m20s to 08h12m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 223)
stop=07h50m20s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 223) 
stop=08h12m20s   !NEXT!

!* --- Scan from 08h13m50s to 08h19m20s   Fri, 2003 May 30 --- *!
sname='OQ208'  ra=14h07m00.394410s  dec= 28d27'14.68998"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, -79)
stop=08h13m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -79) 
stop=08h19m20s   !NEXT!

!* --- Scan from 08h20m50s to 08h26m20s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1, -79)
stop=08h20m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -79) 
stop=08h26m20s   !NEXT!

!* --- Scan from 08h27m20s to 08h32m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, -79)
stop=08h27m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -79) 
stop=08h32m50s   !NEXT!

!* --- Scan from 08h34m50s to 08h40m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1, -79)
stop=08h34m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -79) 
stop=08h40m20s   !NEXT!

!* --- Scan from 08h41m50s to 08h47m20s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 271)
stop=08h41m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 271) 
stop=08h47m20s   !NEXT!

!* --- Scan from 08h48m50s to 09h05m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 271)
stop=08h48m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 271) 
stop=09h05m20s   !NEXT!

!* --- Scan from 09h07m20s to 09h12m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, -31)
stop=09h07m20s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -31) 
stop=09h12m50s   !NEXT!

!* --- Scan from 09h12m50s to 09h18m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=  0  calib='V'
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -31) 
stop=09h18m20s   !NEXT!

!* --- Scan from 09h18m20s to 09h23m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=  0  calib='N'
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -31) 
stop=09h23m50s   !NEXT!

!* --- Scan from 09h25m50s to 09h31m20s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 1,STOP)   write=( 1,off) head=( 1, -31)
stop=09h25m50s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -31) 
stop=09h31m20s   !NEXT!

!* --- Scan from 09h31m50s to 09h53m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 1,STOP)   write=( 1,off) head=( 1, 319)
stop=09h31m50s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 319) 
stop=09h53m50s   !NEXT!

!* ============= Change Tape ============ *!
!*   There were no scheduled tape stops in the last pass.  *!
!*   If it was not interrupted, a POSTPASS is not needed.  *!
 !* ======== UNLOADING DRIVE 1 ========= *! 
tape=(1,STOP)    write=(1,off) 
dur=0  stop=09h53m52s  !NEXT! 
tape=(1,UNLOAD)
!* ========= New tape starts at: 10h08m20s ========= *!

!* --- Scan from 10h08m20s to 10h13m50s   Fri, 2003 May 30 --- *!
sname='OQ208'  ra=14h07m00.394410s  dec= 28d27'14.68998"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-319)
stop=10h08m20s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-319) 
stop=10h13m50s   !NEXT!

!* --- Scan from 10h15m20s to 10h20m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 2,STOP)   write=( 2,off) head=( 2,-319)
stop=10h15m20s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-319) 
stop=10h20m50s   !NEXT!

!* --- Scan from 10h21m20s to 10h26m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-319)
stop=10h21m20s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-319) 
stop=10h26m50s   !NEXT!

!* --- Scan from 10h27m20s to 10h32m50s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 2,STOP)   write=( 2,off) head=( 2,-319)
stop=10h27m20s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-319) 
stop=10h32m50s   !NEXT!

!* --- Scan from 10h33m20s to 10h38m50s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,  31)
stop=10h33m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2,  31) 
stop=10h38m50s   !NEXT!

!* --- Scan from 10h39m20s to 10h55m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,  31)
stop=10h39m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2,  31) 
stop=10h55m50s   !NEXT!

!* --- Scan from 10h57m50s to 11h19m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-271)
stop=10h57m50s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-271) 
stop=11h19m50s   !NEXT!

!* --- Scan from 11h21m20s to 11h32m20s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=999  calib='V'
tape=( 2,STOP)   write=( 2,off) head=( 2,  79)
stop=11h21m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2,  79) 
stop=11h32m20s   !NEXT!

!* --- Scan from 11h33m20s to 11h38m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,  79)
stop=11h33m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2,  79) 
stop=11h38m50s   !NEXT!

!* --- Scan from 11h38m50s to 11h44m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=  0  calib='V'
tape=( 2,-RUN)   write=( 2,on)  head=( 2,  79) 
stop=11h44m20s   !NEXT!

!* --- Scan from 11h44m50s to 12h06m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-223)
stop=11h44m50s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-223) 
stop=12h06m50s   !NEXT!

!* --- Scan from 12h08m20s to 12h24m50s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2, 127)
stop=12h08m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2, 127) 
stop=12h24m50s   !NEXT!

!* --- Scan from 12h24m50s to 12h30m20s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=  0  calib='V'
tape=( 2,-RUN)   write=( 2,on)  head=( 2, 127) 
stop=12h30m20s   !NEXT!

!* --- Scan from 12h30m50s to 12h41m50s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-175)
stop=12h30m50s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-175) 
stop=12h41m50s   !NEXT!

!* --- Scan from 12h41m50s to 12h46m50s   Fri, 2003 May 30 --- *!
sname='J2002+4725'  ra=20h02m10.418290s  dec= 47d25'28.77340"  qual=  0  calib='V'
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-175) 
stop=12h46m50s   !NEXT!

!* --- Scan from 12h46m50s to 12h51m50s   Fri, 2003 May 30 --- *!
sname='NRAO512'  ra=16h40m29.632771s  dec= 39d46'46.02854"  qual=  0  calib='N'
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-175) 
stop=12h51m50s   !NEXT!

!* --- Scan from 12h52m20s to 13h14m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,+REWIND)   write=( 2,off) head=( 2, 175)
stop=12h52m20s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2, 175) 
stop=13h14m20s   !NEXT!

!* --- Scan from 13h16m20s to 13h38m20s   Fri, 2003 May 30 --- *!
sname='SS433'  ra=19h11m49.555000s  dec= 04d58'56.94900"  qual=999  calib='N'
tape=( 2,STOP)   write=( 2,off) head=( 2,-127)
stop=13h16m20s   !NEXT!        
qual=  0
tape=( 2,+RUN)   write=( 2,on)  head=( 2,-127) 
stop=13h38m20s   !NEXT!

!* --- Scan from 13h38m30s to 13h49m30s   Fri, 2003 May 30 --- *!
sname='J1832+1357'  ra=18h32m43.471123s  dec= 13d57'44.40030"  qual=999  calib='V'
tape=( 2,STOP)   write=( 2,off) head=( 2, 223)
stop=13h38m30s   !NEXT!        
qual=  0
tape=( 2,-RUN)   write=( 2,on)  head=( 2, 223) 
stop=13h49m30s   !NEXT!

!* --- Scan from 13h49m30s to 14h00m00s   Fri, 2003 May 30 --- *!
sname='3C345'  ra=16h42m58.809952s  dec= 39d48'36.99395"  qual=  0  calib='N'
tape=( 2,-RUN)   write=( 2,on)  head=( 2, 223) 
stop=14h00m00s   !NEXT!

!* =====  POSTPASSING DRIVE 2 ==== *!
tape=(2,STOP)    write=(2,off)   dur=0s 
stop=14h00m05s  !NEXT! 
tape=(2,POSTPASS)  stop=14h00m07s
  !NEXT! 
  stop=14h00m11s   !QUIT!
