  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron polarization imaging
 Exp. Code:  GG085G  


Schedule Version:       5.00
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es
Fax:
Phone during observation:

Observing mode: K-band dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 May 2019   Day 128 ---

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

10 00 00  1749+096     18 08 01  68.7 190.6  0.3       9.2     0        0   10 00 00
10 09 00  ---          18 17 02  68.2 196.5  0.4      14.4   540       70   10 00 01

10 09 30  1749+096     18 17 32  68.2 196.9  0.4      14.7    24       70   10 09 30
10 17 00  ---          18 25 04  67.7 201.6  0.5      18.7   450      128   10 09 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

10 17 30  1749+096     18 25 34  67.6 201.9  0.6      19.0    24      128   10 17 30
10 27 30  ---          18 35 35  66.7 207.8  0.7      24.0   600      205   10 17 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

10 28 00  1749+096     18 36 05  66.7 208.1  0.7      24.3    24      205   10 28 00
10 34 00  ---          18 42 06  66.0 211.4  0.8      27.1   360      251   10 28 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

10 35 00  1641+399     18 43 07  64.1 298.8  2.0     101.3   -10      251   10 35 10
10 44 00  ---          18 52 08  62.4 298.2  2.1      99.3   530      319   10 35 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

10 44 45  1641+399     18 52 53  62.2 298.1  2.2      99.1    39      319   10 44 45
10 54 30  ---          19 02 40  60.4 297.6  2.3      97.0   585      395   10 44 46

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

10 55 00  1641+399     19 03 10  60.3 297.5  2.3      96.9    24      395   10 55 00
11 02 00  ---          19 10 11  58.9 297.2  2.4      95.6   420      449   10 55 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

11 02 30  1641+399     19 10 41  58.8 297.2  2.5      95.5    24      449   11 02 30
11 05 15  ---          19 13 27  58.3 297.1  2.5      95.0   165      470   11 02 31

11 37 40  1641+399     19 45 57  52.1 296.7  3.0      89.4  1938      470   11 37 40
11 44 30  ---          19 52 48  50.8 296.8  3.2      88.3   410      523   11 37 41

11 45 00  1641+399     19 53 18  50.7 296.8  3.2      88.3    24      523   11 45 00
11 51 30  ---          19 59 49  49.4 296.8  3.3      87.3   390      573   11 45 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 May 2019   Day 128 ---

11 52 00  1641+399     20 00 19  49.3 296.9  3.3      87.2    24      573   11 52 00
12 00 00  ---          20 08 21  47.8 297.0  3.4      86.0   480      635   11 52 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

12 00 45  1641+399     20 09 06  47.6 297.0  3.4      85.9    39      635   12 00 45
12 10 45  ---          20 19 07  45.7 297.2  3.6      84.5   600      712   12 00 46

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

12 11 15  1641+399     20 19 37  45.6 297.3  3.6      84.4    24      712   12 11 15
12 18 15  ---          20 26 39  44.3 297.5  3.7      83.4   420      766   12 11 16

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

12 18 45  1641+399     20 27 09  44.2 297.5  3.7      83.4    24      766   12 18 45
12 29 00  ---          20 37 25  42.2 297.8  3.9      82.0   615      846   12 18 46

12 29 30  1641+399     20 37 55  42.1 297.8  3.9      81.9    24      846   12 29 30
12 39 45  ---          20 48 12  40.2 298.2  4.1      80.5   615      925   12 29 31

12 40 15  1641+399     20 48 42  40.1 298.3  4.1      80.4    24      925   12 40 15
12 50 30  ---          20 58 59  38.1 298.7  4.3      79.1   615     1004   12 40 16

12 51 00  1641+399     20 59 29  38.0 298.7  4.3      79.0    24     1004   12 51 00
13 01 15  ---          21 09 46  36.1 299.2  4.4      77.7   615     1083   12 51 01

13 01 45  1641+399     21 10 16  36.0 299.3  4.4      77.6    24     1083   13 01 45
13 04 45  ---          21 13 16  35.5 299.4  4.5      77.2   180     1107   13 01 46

13 05 15  1641+399     21 13 46  35.4 299.4  4.5      77.2    24     1107   13 05 15
13 10 45  ---          21 19 17  34.3 299.7  4.6      76.4   330     1149   13 05 16

13 11 15  1641+399     21 19 47  34.2 299.8  4.6      76.4    24     1149   13 11 15
13 21 30  ---          21 30 04  32.3 300.3  4.8      75.1   615     1228   13 11 16

13 22 00  1641+399     21 30 34  32.2 300.4  4.8      75.0    24     1228   13 22 00
13 32 15  ---          21 40 51  30.3 301.0  5.0      73.7   615     1308   13 22 01

13 32 45  1641+399     21 41 21  30.2 301.0  5.0      73.6    24     1308   13 32 45
13 43 00  ---          21 51 37  28.3 301.7  5.1      72.3   615     1387   13 32 46
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 May 2019   Day 128 ---

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

13 43 45  1641+399     21 52 23  28.2 301.7  5.1      72.2    39     1387   13 43 45
13 53 45  ---          22 02 24  26.4 302.4  5.3      70.9   600     1464   13 43 46

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

13 54 15  1641+399     22 02 54  26.3 302.5  5.3      70.8    24     1464   13 54 15
14 04 15  ---          22 12 56  24.5 303.2  5.5      69.5   600     1541   13 54 16

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

14 05 00  1641+399     22 13 41  24.3 303.2  5.5      69.4    39     1541   14 05 00
14 08 00  ---          22 16 42  23.8 303.5  5.6      69.1   180     1565   14 05 01

14 08 30  1641+399     22 17 12  23.7 303.5  5.6      69.0    24     1565   14 08 30
14 18 30  ---          22 27 13  21.9 304.3  5.7      67.7   600     1642   14 08 31

14 19 00  1641+399     22 27 43  21.8 304.3  5.7      67.6    24     1642   14 19 00
14 29 00  ---          22 37 45  20.1 305.1  5.9      66.3   600     1719   14 19 01

14 29 30  1749+096     22 38 15  20.8 269.0  4.8      60.8    -4     1719   14 29 34
14 35 00  ---          22 43 46  19.6 269.7  4.9      60.8   326     1761   14 29 31

14 35 30  1749+096     22 44 16  19.5 269.8  4.9      60.8    24     1761   14 35 30
14 40 30  ---          22 49 17  18.4 270.4  4.9      60.8   300     1800   14 35 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

14 41 15  1749+096     22 50 02  18.3 270.5  5.0      60.8    39     1800   14 41 15
14 51 15  ---          23 00 04  16.1 271.8  5.1      60.7   600     1877   14 41 16

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

14 51 45  1749+096     23 00 34  16.0 271.9  5.1      60.7    24     1877   14 51 45
14 57 45  ---          23 06 35  14.7 272.6  5.2      60.7   360     1923   14 51 46

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

14 58 30  1749+096     23 07 20  14.6 272.7  5.2      60.7    39     1923   14 58 30
15 06 30  ---          23 15 21  12.8 273.7  5.4      60.6   480     1985   14 58 31

15 07 00  2251+158     23 15 51  74.8 199.6  0.3      17.5  -100     1985   15 08 40
15 12 30  ---          23 21 22  74.4 204.3  0.4      21.6   230     2015   15 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   8 May 2019   Day 128 ---

15 13 00  2251+158     23 21 52  74.3 204.7  0.4      22.0    24     2015   15 13 00
15 16 00  ---          23 24 53  74.1 207.1  0.5      24.1   180     2038   15 13 01

15 16 30  2251+158     23 25 23  74.0 207.5  0.5      24.5    24     2038   15 16 30
15 24 30  ---          23 33 24  73.1 213.6  0.6      29.7   480     2100   15 16 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

15 25 00  2251+158     23 33 54  73.1 214.0  0.7      30.0    24     2100   15 25 00
15 35 00  ---          23 43 56  71.8 220.7  0.8      35.7   600     2177   15 25 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

15 35 30  2251+158     23 44 26  71.7 221.0  0.8      36.0    24     2177   15 35 30
15 41 30  ---          23 50 27  70.8 224.5  0.9      38.9   360     2224   15 35 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

15 42 30  1641+399     23 51 27   7.7 312.1  7.1      56.1   -73     2224   15 43 43
15 48 00  ---          23 56 58   6.8 312.7  7.2      55.3   257     2257   15 42 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

15 49 00  1641+399     23 57 58   6.6 312.8  7.2      55.2    54     2257   15 49 00
15 59 00  ---          00 08 00   5.1 314.0  7.4      53.7   600     2334   15 49 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

16 00 00  1641+399     00 09 00   4.9 314.1  7.4      53.6    54     2334   16 00 00
16 07 00  ---          00 16 01   3.8 314.9  7.5  H   52.5     0     2388   16 00 01

 --- Thu   9 May 2019   Day 129 ---

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

00 44 00  1641+399     08 54 26   1.3 403.1 -7.8  D  -49.9 31012     2388   00 44 00
00 54 00  ---          09 04 28   2.8 404.3 -7.7     -51.4     0     2465   00 44 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

00 55 00  1641+399     09 05 28   2.9 404.4 -7.6     -51.6    54     2465   00 55 00
01 03 30  ---          09 13 59   4.2 405.4 -7.5     -52.9   510     2531   00 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   9 May 2019   Day 129 ---

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

01 50 30  1641+399     10 01 07  11.8 410.5 -6.7     -59.7  2813     2531   01 50 30
02 00 30  ---          10 11 09  13.4 411.5 -6.5     -61.1   600     2608   01 50 31

02 01 00  1641+399     10 11 39  13.5 411.5 -6.5     -61.2    24     2608   02 01 00
02 07 00  ---          10 17 40  14.5 412.1 -6.4     -62.0   360     2655   02 01 01

02 07 30  1641+399     10 18 10  14.6 412.1 -6.4     -62.1    24     2655   02 07 30
02 17 30  ---          10 28 11  16.3 413.0 -6.3     -63.5   600     2732   02 07 31

02 18 00  1641+399     10 28 42  16.4 413.1 -6.2     -63.5    24     2732   02 18 00
02 28 00  ---          10 38 43  18.2 414.0 -6.1     -64.9   600     2809   02 18 01

02 28 30  1641+399     10 39 13  18.3 414.0 -6.1     -64.9    24     2809   02 28 30
02 31 30  ---          10 42 14  18.8 414.3 -6.0     -65.3   180     2832   02 28 31

02 32 00  1641+399     10 42 44  18.9 414.3 -6.0     -65.4    24     2832   02 32 00
02 38 30  ---          10 49 15  20.0 414.9 -5.9     -66.3   390     2883   02 32 01

02 39 00  1641+399     10 49 45  20.1 414.9 -5.9     -66.3    24     2883   02 39 00
02 49 00  ---          10 59 47  21.9 415.7 -5.7     -67.6   600     2960   02 39 01

02 49 30  1641+399     11 00 17  22.0 415.7 -5.7     -67.7    24     2960   02 49 30
02 59 30  ---          11 10 18  23.8 416.5 -5.6     -69.0   600     3037   02 49 31

03 00 00  1641+399     11 10 48  23.8 416.6 -5.5     -69.1    24     3037   03 00 00
03 10 00  ---          11 20 50  25.6 417.3 -5.4     -70.4   600     3115   03 00 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

03 11 00  1641+399     11 21 50  25.8 417.4 -5.4     -70.5    54     3115   03 11 00
03 21 00  ---          11 31 52  27.7 418.1 -5.2     -71.8   600     3192   03 11 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

03 22 00  1641+399     11 32 52  27.8 418.1 -5.2     -71.9    54     3192   03 22 00
03 30 30  ---          11 41 23  29.4 418.7 -5.0     -73.0   510     3258   03 22 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   9 May 2019   Day 129 ---

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

03 31 30  1641+399     11 42 24  29.6 418.7 -5.0     -73.2    54     3258   03 31 30
03 34 30  ---          11 45 24  30.1 418.9 -5.0     -73.5   180     3281   03 31 31

03 35 00  1641+399     11 45 54  30.2 419.0 -5.0     -73.6    24     3281   03 35 00
03 45 00  ---          11 55 56  32.1 419.6 -4.8     -74.9   600     3358   03 35 01

03 45 30  1641+399     11 56 26  32.2 419.6 -4.8     -75.0    24     3358   03 45 30
03 55 30  ---          12 06 28  34.0 420.2 -4.6     -76.2   600     3435   03 45 31

03 56 00  1641+399     12 06 58  34.1 420.2 -4.6     -76.3    24     3435   03 56 00
04 06 00  ---          12 16 59  36.0 420.7 -4.4     -77.6   600     3513   03 56 01

04 06 30  1641+399     12 17 29  36.1 420.8 -4.4     -77.7    24     3513   04 06 30
04 16 30  ---          12 27 31  38.0 421.3 -4.3     -79.0   600     3590   04 06 31

04 17 00  1641+399     12 28 01  38.1 421.3 -4.3     -79.0    24     3590   04 17 00
04 27 00  ---          12 38 03  40.0 421.7 -4.1     -80.4   600     3667   04 17 01

04 27 30  1641+399     12 38 33  40.1 421.7 -4.1     -80.4    24     3667   04 27 30
04 37 30  ---          12 48 34  42.0 422.1 -3.9     -81.8   600     3745   04 27 31

04 38 00  1641+399     12 49 05  42.1 422.2 -3.9     -81.9    24     3745   04 38 00
04 45 30  ---          12 56 36  43.5 422.4 -3.8     -82.9   450     3802   04 38 01

04 46 00  1641+399     12 57 06  43.6 422.4 -3.8     -82.9    24     3802   04 46 00
04 53 30  ---          13 04 37  45.0 422.7 -3.7     -84.0   450     3860   04 46 01

04 54 00  1641+399     13 05 07  45.1 422.7 -3.6     -84.1    24     3860   04 54 00
05 01 30  ---          13 12 38  46.6 422.9 -3.5     -85.1   450     3918   04 54 01

05 02 00  1749+096     13 13 08  22.2  91.8 -4.7     -60.7  -213     3918   05 05 33
05 06 00  ---          13 17 09  23.1  92.3 -4.6     -60.7    27     3922   05 02 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

05 07 00  1749+096     13 18 09  23.3  92.5 -4.6     -60.7    54     3922   05 07 00
05 17 00  ---          13 28 11  25.4  93.8 -4.4     -60.6   600     3999   05 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   9 May 2019   Day 129 ---

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

05 18 00  1749+096     13 29 11  25.6  93.9 -4.4     -60.5    54     3999   05 18 00
05 25 00  ---          13 36 12  27.2  94.9 -4.3     -60.4   420     4053   05 18 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

05 26 00  1749+096     13 37 12  27.4  95.0 -4.3     -60.4    54     4053   05 26 00
05 34 30  ---          13 45 44  29.2  96.2 -4.1     -60.2   510     4119   05 26 01

05 35 00  1641+399     13 46 14  53.0  63.3 -3.0     -90.2   -25     4119   05 35 25
05 38 00  ---          13 49 14  53.6  63.3 -2.9     -90.7   155     4139   05 35 01

05 38 30  1641+399     13 49 44  53.7  63.3 -2.9     -90.8    24     4139   05 38 30
05 44 30  ---          13 55 45  54.9  63.2 -2.8     -91.8   360     4185   05 38 31

05 45 00  1641+399     13 56 16  54.9  63.2 -2.8     -91.8    24     4185   05 45 00
05 51 00  ---          14 02 17  56.1  63.1 -2.7     -92.9   360     4232   05 45 01

05 51 30  1641+399     14 02 47  56.2  63.1 -2.7     -93.0    24     4232   05 51 30
06 01 30  ---          14 12 48  58.1  62.9 -2.5     -94.8   600     4309   05 51 31

06 02 00  1641+399     14 13 18  58.2  62.9 -2.5     -94.9    24     4309   06 02 00
06 12 00  ---          14 23 20  60.1  62.5 -2.3     -96.8   600     4386   06 02 01

06 12 30  1641+399     14 23 50  60.2  62.5 -2.3     -96.9    24     4386   06 12 30
06 22 30  ---          14 33 52  62.1  61.9 -2.2     -99.0   600     4464   06 12 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

06 23 30  1641+399     14 34 52  62.3  61.9 -2.1     -99.2    54     4464   06 23 30
06 33 30  ---          14 44 53  64.2  61.1 -2.0    -101.5   600     4541   06 23 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 34 30  1641+399     14 45 54  64.4  61.0 -2.0    -101.7    54     4541   06 34 30
06 43 00  ---          14 54 25  66.0  60.1 -1.8    -103.9   510     4607   06 34 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

06 44 00  1641+399     14 55 25  66.2  60.0 -1.8    -104.1    54     4607   06 44 00
06 54 00  ---          15 05 27  68.1  58.7 -1.6    -107.0   600     4684   06 44 01

06 54 30  1641+399     15 05 57  68.1  58.6 -1.6    -107.1    24     4684   06 54 30
07 04 30  ---          15 15 59  70.0  56.9 -1.5    -110.3   600     4761   06 54 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   9 May 2019   Day 129 ---

07 05 00  1641+399     15 16 29  70.1  56.8 -1.5    -110.5    24     4761   07 05 00
07 15 00  ---          15 26 30  71.8  54.5 -1.3    -114.2   600     4838   07 05 01

07 15 30  1641+399     15 27 00  71.9  54.4 -1.3    -114.4    24     4838   07 15 30
07 20 10  ---          15 31 41  72.7  53.1 -1.2    -116.4   280     4875   07 15 31

07 20 40  1641+399     15 32 11  72.8  53.0 -1.2    -116.6    24     4875   07 20 40
07 30 40  ---          15 42 13  74.5  49.7 -1.0    -121.4   600     4952   07 20 41

07 31 10  1641+399     15 42 43  74.6  49.5 -1.0    -121.7    24     4952   07 31 10
07 41 10  ---          15 52 45  76.2  45.1 -0.8    -127.5   600     5029   07 31 11

07 41 40  1641+399     15 53 15  76.3  44.9 -0.8    -127.8    24     5029   07 41 40
07 51 40  ---          16 03 16  77.7  39.2 -0.7    -134.9   600     5106   07 41 41

07 52 10  1641+399     16 03 46  77.8  38.9 -0.7    -135.3    24     5106   07 52 10
08 00 00  ---          16 11 38  78.8  33.3 -0.5    -142.0   470     5167   07 52 11


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    8         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   6  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
   BBC fr=     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     695.99    695.99    727.99    727.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   6   7   8   9  10  11  12  13  14  15

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:   48         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  16  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
   BBC fr=     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     767.25    767.25    799.25    799.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  16  17  18  19  20  21  22  23  24  25

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   36         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  26  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
   BBC fr=     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     776.99    776.99    808.99    808.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  26  27  28  29  30  31  32  33  34  35

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   1328+307          13 28 49.657783   * 13 31 08.288075     13 32 02.136734       0.18
   J1331+3030        30 45 58.64055    * 30 30 32.95919      30 24 43.07322        0.17
 * 3C286             From catalog imbedded in main SCHED input file.
                     rfc_2018a Petrov and Kovalev, in preparation  603 observations

 * 0355+508          03 55 45.261377   * 03 59 29.747278     04 00 53.430855       0.16
   J0359+5057        50 49 20.28597    * 50 57 50.16192      51 00 56.76709        0.10
   NRAO150           /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  27427 observations

 * 1641+399          16 41 17.606226   * 16 42 58.809963     16 43 38.773734       0.13
   J1642+3948        39 54 10.81487    * 39 48 36.99393      39 46 26.22766        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  52534 observations

 * 1749+096          17 49 10.387930   * 17 51 32.818573     17 52 27.954984       0.10
   J1751+0939        09 39 42.82586    * 09 39 00.72841      09 38 43.28918        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  217453 observations

 * 2200+420          22 00 39.362505   * 22 02 43.291372     22 03 30.249781       0.14
   J2202+4216        42 02 08.59082    * 42 16 39.97996      42 21 56.96920        0.10
   BLLAC             /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  60473 observations

 * 2251+158          22 51 29.519743   * 22 53 57.747942     22 54 53.589085       0.10
   J2253+1608        15 52 54.34805    * 16 08 53.56088      16 14 49.53006        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  41804 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  3C286      ra1cm2.set            1                                 0.583     0.000
             ra2cm2.set            3                                 0.525     0.000
             ra7mm2.set            2                                 0.658     0.000
  0355+508   ra1cm2.set            36 40                             6.584    39.501
  1641+399   ra1cm2.set            1 5 6 36 39 40 44 46 47 48  +    19.668  2404.375
             ra2cm2.set            3 26 58                           0.942    43.892
             ra7mm2.set            2 16 41 56 57                     1.804    85.688
  1749+096   ra1cm2.set            1 5 6 36 39 40 44 46 47 49  +     2.262   152.382
             ra2cm2.set            3 26 58                           0.317    13.945
             ra7mm2.set            2 16 41 56 57                     0.833    31.011
  2200+420   ra1cm2.set            1                                 0.233     0.000
             ra2cm2.set            3                                 0.233     0.000
             ra7mm2.set            2                                 0.233     0.000
  2251+158   ra1cm2.set            1 5 6 36 39 45 46 47 48 49  +     4.528   172.228
             ra2cm2.set            3 26                              0.100     5.500
             ra7mm2.set            2 16 41                           0.333     9.667


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   3C286              127.7
   0355+508            35.8
   1641+399           118.3
   1749+096           130.1
   2200+420            67.3
   2251+158            58.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

