  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GS045A
 Exp. Code:  GS045A  


Schedule Version:       2.00
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Robert Schulz

Address:  ASTRON
          Oude Hoogeveensedijk 4
          7991PD Dwingeloo
           The Netherlands

Phone:    0031 521 595 755
EMAIL:    schulz@astron.nl
Fax:
Phone during observation: 0031 521 595 755

Observing mode: Line

Notes:    Target              : OQ208
          Bandpass Calibrator : 3C345
          Phase Reference     : J1419+2706
          SCHED v11.5

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

 Next scan frequencies:  1295.25  1295.25  1311.25  1311.25  1327.25  1327.25  1343.25  1343.25
 Next BBC frequencies:    804.75   804.75   788.75   788.75   772.75   772.75   756.75   756.75
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

00 01 45  J1419+2706   09 11 12  23.5  71.4 -5.2     -66.3     0        0   00 01 45
00 03 00  =1417+273    09 12 28  23.7  71.6 -5.1     -66.4    75        5   00 01 46

00 03 00  OQ208        09 12 28  26.9  71.4 -4.9     -68.0   -14        5   00 03 14
00 09 50  ---          09 19 19  28.3  72.1 -4.8     -68.5   396       30   00 03 01

00 10 30  J1419+2706   09 19 59  25.3  72.3 -5.0     -66.9    26       30   00 10 30
00 11 45  =1417+273    09 21 14  25.5  72.4 -5.0     -67.0    75       35   00 10 31

00 11 45  OQ208        09 21 14  28.7  72.2 -4.8     -68.6   -14       35   00 11 59
00 18 35  ---          09 28 05  30.1  72.9 -4.7     -69.1   396       61   00 11 46

00 19 15  J1419+2706   09 28 45  27.1  73.1 -4.9     -67.6    26       61   00 19 15
00 20 30  =1417+273    09 30 01  27.3  73.2 -4.8     -67.7    75       66   00 19 16

00 20 30  OQ208        09 30 01  30.5  73.0 -4.6     -69.3   -14       66   00 20 44
00 27 20  ---          09 36 52  31.9  73.6 -4.5     -69.8   396       91   00 20 31

00 28 00  J1419+2706   09 37 32  28.9  74.0 -4.7     -68.2    26       91   00 28 00
00 29 15  =1417+273    09 38 47  29.2  74.1 -4.7     -68.3    75       96   00 28 01

00 29 15  OQ208        09 38 47  32.3  73.8 -4.5     -69.9   -14       96   00 29 29
00 36 05  ---          09 45 38  33.7  74.4 -4.4     -70.4   396      121   00 29 16

00 36 45  J1419+2706   09 46 18  30.7  74.8 -4.6     -68.8    26      121   00 36 45
00 38 00  =1417+273    09 47 33  31.0  74.9 -4.6     -68.8    75      126   00 36 46

00 38 00  OQ208        09 47 33  34.1  74.6 -4.3     -70.5   -14      126   00 38 14
00 44 50  ---          09 54 25  35.6  75.2 -4.2     -71.0   396      152   00 38 01

00 45 30  J1419+2706   09 55 05  32.5  75.6 -4.4     -69.3    26      152   00 45 30
00 46 45  =1417+273    09 56 20  32.8  75.7 -4.4     -69.4    75      157   00 45 31

00 46 45  OQ208        09 56 20  36.0  75.4 -4.2     -71.1   -14      157   00 46 59
00 53 35  ---          10 03 11  37.4  76.0 -4.1     -71.6   396      182   00 46 46

00 54 15  J1419+2706   10 03 51  34.4  76.4 -4.3     -69.9    26      182   00 54 15
00 55 30  =1417+273    10 05 06  34.6  76.5 -4.3     -69.9    75      187   00 54 16

00 55 30  OQ208        10 05 06  37.8  76.1 -4.0     -71.7   -14      187   00 55 44
01 02 20  ---          10 11 57  39.2  76.7 -3.9     -72.1   396      212   00 55 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

01 03 00  J1419+2706   10 12 38  36.2  77.2 -4.1     -70.4    26      212   01 03 00
01 04 15  =1417+273    10 13 53  36.5  77.4 -4.1     -70.5    75      217   01 03 01

01 04 15  OQ208        10 13 53  39.6  76.9 -3.9     -72.3   -14      217   01 04 29
01 11 05  ---          10 20 44  41.1  77.5 -3.8     -72.7   396      243   01 04 16

01 11 45  J1419+2706   10 21 24  38.0  78.1 -4.0     -70.9    26      243   01 11 45
01 13 00  =1417+273    10 22 39  38.3  78.2 -4.0     -71.0    75      248   01 11 46

01 13 00  OQ208        10 22 39  41.5  77.7 -3.8     -72.8   -14      248   01 13 14
01 19 50  ---          10 29 30  42.9  78.3 -3.6     -73.2   396      273   01 13 01

01 20 30  J1419+2706   10 30 10  39.9  78.9 -3.8     -71.4    26      273   01 20 30
01 21 45  =1417+273    10 31 26  40.2  79.0 -3.8     -71.5    75      278   01 20 31

01 21 45  OQ208        10 31 26  43.3  78.4 -3.6     -73.3   -14      278   01 21 59
01 28 35  ---          10 38 17  44.8  79.0 -3.5     -73.7   396      303   01 21 46

01 29 15  J1419+2706   10 38 57  41.8  79.7 -3.7     -71.8    26      303   01 29 15
01 30 30  =1417+273    10 40 12  42.0  79.8 -3.7     -71.9    75      308   01 29 16

01 30 30  OQ208        10 40 12  45.2  79.2 -3.5     -73.8   -14      308   01 30 44
01 37 20  ---          10 47 03  46.6  79.8 -3.3     -74.2   396      334   01 30 31

01 38 00  J1419+2706   10 47 43  43.6  80.5 -3.6     -72.3    26      334   01 38 00
01 39 15  =1417+273    10 48 58  43.9  80.6 -3.5     -72.4    75      339   01 38 01

01 39 15  OQ208        10 48 58  47.0  80.0 -3.3     -74.3   -14      339   01 39 29
01 46 05  ---          10 55 50  48.5  80.6 -3.2     -74.7   396      364   01 39 16

01 46 45  J1419+2706   10 56 30  45.5  81.3 -3.4     -72.7    26      364   01 46 45
01 48 00  =1417+273    10 57 45  45.7  81.4 -3.4     -72.8    75      369   01 46 46

01 48 00  OQ208        10 57 45  48.9  80.7 -3.2     -74.8   -14      369   01 48 14
01 54 50  ---          11 04 36  50.3  81.3 -3.1     -75.2   396      394   01 48 01

01 55 30  J1419+2706   11 05 16  47.3  82.2 -3.3     -73.1    26      394   01 55 30
01 56 45  =1417+273    11 06 31  47.6  82.3 -3.2     -73.2    75      399   01 55 31

01 56 45  OQ208        11 06 31  50.7  81.5 -3.0     -75.3   -14      399   01 56 59
02 03 35  ---          11 13 22  52.2  82.1 -2.9     -75.6   396      425   01 56 46

02 04 15  J1419+2706   11 14 03  49.2  83.0 -3.1     -73.5    26      425   02 04 15
02 05 30  =1417+273    11 15 18  49.5  83.1 -3.1     -73.5    75      430   02 04 16
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

02 05 30  OQ208        11 15 18  52.6  82.3 -2.9     -75.7   -14      430   02 05 44
02 12 20  ---          11 22 09  54.1  82.9 -2.8     -76.0   396      455   02 05 31

02 13 00  J1419+2706   11 22 49  51.1  83.9 -3.0     -73.8    26      455   02 13 00
02 14 15  =1417+273    11 24 04  51.4  84.0 -2.9     -73.9    75      460   02 13 01

02 14 15  OQ208        11 24 04  54.5  83.1 -2.7     -76.1   -14      460   02 14 29
02 21 05  ---          11 30 55  55.9  83.7 -2.6     -76.4   396      485   02 14 16

02 21 45  J1419+2706   11 31 35  53.0  84.7 -2.8     -74.1    26      485   02 21 45
02 23 00  =1417+273    11 32 51  53.2  84.9 -2.8     -74.2    75      490   02 21 46

02 23 00  OQ208        11 32 51  56.4  83.9 -2.6     -76.5   -14      490   02 23 14
02 29 50  ---          11 39 42  57.8  84.5 -2.5     -76.7   396      516   02 23 01

02 30 30  J1419+2706   11 40 22  54.8  85.6 -2.7     -74.4    26      516   02 30 30
02 31 45  =1417+273    11 41 37  55.1  85.8 -2.7     -74.4    75      521   02 30 31

02 34 05  3C345        11 43 57  29.9  58.8 -5.0     -73.4    82      521   02 34 05
02 39 05  ---          11 48 58  30.8  59.2 -4.9     -74.0   300      540   02 34 06

02 41 25  J1419+2706   11 51 19  57.2  86.8 -2.5     -74.7    81      540   02 41 25
02 42 40  =1417+273    11 52 34  57.5  86.9 -2.5     -74.7    75      545   02 41 26

02 42 40  OQ208        11 52 34  60.6  85.8 -2.3     -77.2   -14      545   02 42 54
02 49 30  ---          11 59 25  62.0  86.5 -2.1     -77.4   396      570   02 42 41

02 50 10  J1419+2706   12 00 05  59.1  87.8 -2.3     -74.8    26      570   02 50 10
02 51 25  =1417+273    12 01 20  59.4  87.9 -2.3     -74.8    75      575   02 50 11

02 51 25  OQ208        12 01 20  62.5  86.6 -2.1     -77.5   -14      575   02 51 39
02 58 15  ---          12 08 11  63.9  87.4 -2.0     -77.6   396      601   02 51 26

02 58 55  J1419+2706   12 08 52  61.0  88.8 -2.2     -74.9    26      601   02 58 55
03 00 10  =1417+273    12 10 07  61.2  88.9 -2.2     -75.0    75      605   02 58 56

03 00 10  OQ208        12 10 07  64.3  87.6 -2.0     -77.7   -14      605   03 00 24
03 06 55  ---          12 16 53  65.8  88.3 -1.8     -77.8   391      631   03 00 11

03 07 10  J1419+2706   12 17 08  62.7  89.8 -2.1     -75.0     1      631   03 07 10
03 08 10  =1417+273    12 18 08  63.0  89.9 -2.0     -75.0    60      634   03 07 11

03 08 10  OQ208        12 18 08  66.1  88.5 -1.8     -77.8   -14      634   03 08 24
03 14 55  ---          12 24 54  67.5  89.3 -1.7     -77.9   391      660   03 08 11
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

03 15 10  J1419+2706   12 25 09  64.5  90.9 -1.9     -75.0     1      660   03 15 10
03 16 10  =1417+273    12 26 09  64.7  91.0 -1.9     -75.0    60      663   03 15 11

03 16 10  OQ208        12 26 09  67.8  89.4 -1.7     -77.9   -14      663   03 16 24
03 22 55  ---          12 32 56  69.3  90.3 -1.6     -77.9   391      689   03 16 11

03 23 10  J1419+2706   12 33 11  66.2  92.0 -1.8     -74.9     1      689   03 23 10
03 24 10  =1417+273    12 34 11  66.4  92.1 -1.8     -74.8    60      693   03 23 11

03 24 10  OQ208        12 34 11  69.5  90.4 -1.6     -77.9   -14      693   03 24 24
03 30 55  ---          12 40 57  71.0  91.4 -1.4     -77.8   391      718   03 24 11

03 31 10  J1419+2706   12 41 12  67.9  93.2 -1.7     -74.7     1      718   03 31 10
03 32 10  =1417+273    12 42 12  68.1  93.3 -1.6     -74.6    60      722   03 31 11

03 32 10  OQ208        12 42 12  71.2  91.5 -1.4     -77.8   -14      722   03 32 24
03 38 55  ---          12 48 58  72.7  92.6 -1.3     -77.6   391      747   03 32 11

03 39 10  J1419+2706   12 49 13  69.6  94.5 -1.5     -74.3     1      747   03 39 10
03 40 10  =1417+273    12 50 13  69.9  94.7 -1.5     -74.3    60      751   03 39 11

03 40 10  OQ208        12 50 13  73.0  92.8 -1.3     -77.6   -14      751   03 40 24
03 46 55  ---          12 56 59  74.4  93.9 -1.2     -77.3   391      776   03 40 11

03 47 10  J1419+2706   12 57 15  71.4  96.0 -1.4     -73.9     1      776   03 47 10
03 48 10  =1417+273    12 58 15  71.6  96.1 -1.4     -73.8    60      780   03 47 11

03 48 10  OQ208        12 58 15  74.7  94.1 -1.2     -77.2   -14      780   03 48 24
03 54 55  ---          13 05 01  76.1  95.5 -1.0     -76.7   391      805   03 48 11

03 55 10  J1419+2706   13 05 16  73.1  97.6 -1.3     -73.2     1      805   03 55 10
03 56 10  =1417+273    13 06 16  73.3  97.8 -1.2     -73.1    60      809   03 55 11

03 56 10  OQ208        13 06 16  76.4  95.7 -1.0     -76.6   -14      809   03 56 24
04 02 55  ---          13 13 02  77.9  97.3 -0.9     -75.9   391      834   03 56 11

04 03 10  J1419+2706   13 13 17  74.8  99.5 -1.1     -72.3     1      834   04 03 10
04 04 10  =1417+273    13 14 17  75.0  99.8 -1.1     -72.1    60      838   04 03 11

04 04 10  OQ208        13 14 17  78.1  97.7 -0.9     -75.7   -14      838   04 04 24
04 10 55  ---          13 21 03  79.6  99.6 -0.8     -74.6   391      863   04 04 11

04 11 10  J1419+2706   13 21 18  76.5 101.8 -1.0     -71.0     1      863   04 11 10
04 12 10  =1417+273    13 22 19  76.7 102.1 -1.0     -70.8    60      867   04 11 11
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

04 12 10  OQ208        13 22 19  79.8 100.0 -0.8     -74.3   -14      867   04 12 24
04 18 55  ---          13 29 05  81.3 102.6 -0.6     -72.6   391      892   04 12 11

04 19 10  J1419+2706   13 29 20  78.2 104.6 -0.9     -69.2     1      892   04 19 10
04 20 10  =1417+273    13 30 20  78.4 105.0 -0.8     -68.9    60      896   04 19 11

04 22 10  3C345        13 32 20  50.4  63.2 -3.2     -88.0    56      896   04 22 10
04 27 10  ---          13 37 21  51.3  63.3 -3.1     -88.8   300      915   04 22 11

04 29 10  J1419+2706   13 39 21  80.2 109.1 -0.7     -65.9    56      915   04 29 10
04 30 10  =1417+273    13 40 22  80.4 109.7 -0.7     -65.4    60      919   04 29 11

04 30 10  OQ208        13 40 22  83.6 109.0 -0.5     -67.6   -14      919   04 30 24
04 36 55  ---          13 47 08  84.9 115.4 -0.3     -62.0   391      944   04 30 11

04 37 10  J1419+2706   13 47 23  81.8 114.2 -0.6     -61.8     1      944   04 37 10
04 38 10  =1417+273    13 48 23  82.0 114.9 -0.5     -61.1    60      948   04 37 11

04 38 10  OQ208        13 48 23  85.2 116.9 -0.3     -60.7   -14      948   04 38 24
04 44 55  ---          13 55 09  86.4 128.5 -0.2     -49.9   391      973   04 38 11

04 45 10  J1419+2706   13 55 24  83.4 121.4 -0.4     -55.5     1      973   04 45 10
04 46 10  =1417+273    13 56 24  83.5 122.5 -0.4     -54.5    60      977   04 45 11

04 46 10  OQ208        13 56 24  86.6 131.6 -0.2     -47.0   -15      977   04 46 25
04 52 55  ---          14 03 10  87.5 155.4 -0.1     -24.0   390     1002   04 46 11

04 53 10  J1419+2706   14 03 25  84.7 132.3 -0.3     -45.5    -9     1002   04 53 19
04 54 10  =1417+273    14 04 26  84.9 134.1 -0.3     -43.9    51     1006   04 53 11

04 54 10  OQ208        14 04 26  87.6 161.5 -0.1     -18.1   -29     1006   04 54 39
05 00 55  ---          14 11 12  87.6 197.8  0.1      17.4   376     1030   04 54 11

05 01 10  J1419+2706   14 11 27  85.8 149.7 -0.2     -29.2   -26     1030   05 01 36
05 02 10  =1417+273    14 12 27  85.9 152.5 -0.1     -26.5    34     1032   05 01 11

05 02 10  OQ208        14 12 27  87.5 203.9  0.1      23.4   -47     1032   05 02 57
05 08 55  ---          14 19 13  86.6 228.1  0.2      46.7   358     1055   05 02 11

05 09 10  J1419+2706   14 19 28  86.4 175.1 -0.0      -4.7   -30     1055   05 09 40
05 10 10  =1417+273    14 20 28  86.4 178.6 -0.0      -1.3    30     1057   05 09 11

05 10 10  OQ208        14 20 28  86.4 231.1  0.2      49.6   -46     1057   05 10 56
05 16 55  ---          14 27 14  85.2 242.9  0.3      60.5   359     1080   05 10 11
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

05 17 10  J1419+2706   14 27 29  86.1 202.3  0.1      21.5   -21     1080   05 17 31
05 18 10  =1417+273    14 28 29  86.0 205.3  0.1      24.4    39     1083   05 17 11

05 18 10  OQ208        14 28 29  85.0 244.4  0.3      61.9   -36     1083   05 18 46
05 24 55  ---          14 35 16  83.6 250.9  0.5      67.5   369     1106   05 18 11

05 25 10  J1419+2706   14 35 31  85.2 222.5  0.2      40.7   -13     1106   05 25 23
05 26 10  =1417+273    14 36 31  85.0 224.4  0.3      42.6    47     1109   05 25 11

05 26 10  OQ208        14 36 31  83.4 251.8  0.5      68.2   -27     1109   05 26 37
05 32 55  ---          14 43 17  82.0 255.8  0.6      71.4   378     1134   05 26 11

05 33 10  J1419+2706   14 43 32  83.9 235.3  0.4      52.6    -7     1134   05 33 17
05 34 10  =1417+273    14 44 32  83.7 236.6  0.4      53.7    53     1137   05 33 11

05 34 10  OQ208        14 44 32  81.7 256.4  0.6      71.9   -22     1137   05 34 32
05 40 55  ---          14 51 18  80.3 259.2  0.7      73.9   383     1162   05 34 11

05 41 10  J1419+2706   14 51 33  82.4 243.6  0.5      59.9    -4     1162   05 41 14
05 42 10  =1417+273    14 52 33  82.2 244.5  0.5      60.6    56     1165   05 41 11

05 42 10  OQ208        14 52 33  80.0 259.7  0.7      74.1   -19     1165   05 42 29
05 48 55  ---          14 59 20  78.6 261.8  0.9      75.4   386     1190   05 42 11

05 49 10  J1419+2706   14 59 35  80.8 249.3  0.6      64.6    -2     1190   05 49 12
05 50 10  =1417+273    15 00 35  80.6 249.9  0.7      65.1    58     1194   05 49 11

05 50 10  OQ208        15 00 35  78.3 262.1  0.9      75.6   -17     1194   05 50 27
05 56 55  ---          15 07 21  76.9 263.8  1.0      76.4   388     1219   05 50 11

05 57 10  J1419+2706   15 07 36  79.2 253.4  0.8      67.8     0     1219   05 57 10
05 58 10  =1417+273    15 08 36  78.9 253.9  0.8      68.1    60     1223   05 57 11

05 58 10  OQ208        15 08 36  76.6 264.1  1.0      76.6   -15     1223   05 58 25
06 04 55  ---          15 15 22  75.2 265.5  1.1      77.1   390     1248   05 58 11

06 05 10  J1419+2706   15 15 37  77.5 256.6  0.9      70.0     1     1248   06 05 10
06 06 10  =1417+273    15 16 37  77.3 257.0  0.9      70.2    60     1252   06 05 11

06 06 10  OQ208        15 16 37  74.9 265.7  1.1      77.2   -14     1252   06 06 24
06 12 55  ---          15 23 23  73.4 266.9  1.3      77.5   391     1277   06 06 11

06 13 10  J1419+2706   15 23 38  75.8 259.2  1.0      71.6     2     1277   06 13 10
06 14 10  =1417+273    15 24 39  75.6 259.5  1.1      71.7    60     1281   06 13 11
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

06 14 10  OQ208        15 24 39  73.2 267.1  1.3      77.6   -13     1281   06 14 23
06 20 55  ---          15 31 25  71.7 268.1  1.4      77.8   392     1306   06 14 11

06 21 10  J1419+2706   15 31 40  74.1 261.3  1.2      72.7     2     1306   06 21 10
06 22 10  =1417+273    15 32 40  73.9 261.5  1.2      72.8    60     1310   06 21 11

06 22 10  OQ208        15 32 40  71.4 268.3  1.4      77.8   -13     1310   06 22 23
06 28 55  ---          15 39 26  70.0 269.3  1.5      77.9   392     1335   06 22 11

06 29 10  J1419+2706   15 39 41  72.4 263.1  1.3      73.5     2     1335   06 29 10
06 30 10  =1417+273    15 40 41  72.2 263.3  1.3      73.6    60     1339   06 29 11

06 30 10  OQ208        15 40 41  69.7 269.4  1.5      77.9   -13     1339   06 30 23
06 36 55  ---          15 47 27  68.3 270.3  1.7      77.9   392     1364   06 30 11

06 37 10  J1419+2706   15 47 42  70.7 264.7  1.4      74.1     2     1364   06 37 10
06 38 10  =1417+273    15 48 43  70.5 264.8  1.5      74.1    60     1368   06 37 11

06 38 10  OQ208        15 48 43  68.0 270.5  1.7      77.9   -13     1368   06 38 23
06 44 55  ---          15 55 29  66.5 271.3  1.8      77.8   392     1394   06 38 11

06 45 10  J1419+2706   15 55 44  69.0 266.1  1.6      74.5     2     1394   06 45 10
06 46 10  =1417+273    15 56 44  68.7 266.2  1.6      74.5    60     1397   06 45 11

06 46 10  OQ208        15 56 44  66.3 271.4  1.8      77.8   -13     1397   06 46 23
06 52 55  ---          16 03 30  64.8 272.2  1.9      77.7   392     1423   06 46 11

06 53 10  J1419+2706   16 03 45  67.2 267.3  1.7      74.8     2     1423   06 53 10
06 54 10  =1417+273    16 04 45  67.0 267.5  1.7      74.8    60     1426   06 53 11

06 54 10  OQ208        16 04 45  64.5 272.3  1.9      77.7   -13     1426   06 54 23
07 00 55  ---          16 11 31  63.1 273.0  2.1      77.5   392     1452   06 54 11

07 01 10  J1419+2706   16 11 46  65.5 268.5  1.8      74.9     2     1452   07 01 10
07 02 10  =1417+273    16 12 47  65.3 268.6  1.9      74.9    60     1456   07 01 11

07 02 10  OQ208        16 12 47  62.8 273.2  2.1      77.5   -13     1456   07 02 23
07 08 55  ---          16 19 33  61.4 273.9  2.2      77.3   392     1481   07 02 11

07 09 10  J1419+2706   16 19 48  63.8 269.6  2.0      75.0     2     1481   07 09 10
07 10 10  =1417+273    16 20 48  63.6 269.7  2.0      75.0    60     1485   07 09 11

07 10 10  OQ208        16 20 48  61.1 274.0  2.2      77.3   -13     1485   07 10 23
07 16 55  ---          16 27 34  59.6 274.7  2.3      77.1   392     1510   07 10 11
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

07 17 10  J1419+2706   16 27 49  62.1 270.6  2.1      75.0     2     1510   07 17 10
07 18 10  =1417+273    16 28 49  61.8 270.7  2.1      75.0    60     1514   07 17 11

07 18 10  OQ208        16 28 49  59.4 274.8  2.3      77.0   -13     1514   07 18 23
07 24 55  ---          16 35 35  57.9 275.4  2.5      76.8   392     1539   07 18 11

07 25 10  J1419+2706   16 35 50  60.3 271.6  2.2      74.9     2     1539   07 25 10
07 26 10  =1417+273    16 36 50  60.1 271.7  2.3      74.9    60     1543   07 25 11

07 26 10  OQ208        16 36 50  57.7 275.6  2.5      76.7   -13     1543   07 26 23
07 32 55  ---          16 43 37  56.2 276.2  2.6      76.4   392     1568   07 26 11

07 33 10  J1419+2706   16 43 52  58.6 272.5  2.4      74.8     2     1568   07 33 10
07 34 10  =1417+273    16 44 52  58.4 272.6  2.4      74.8    60     1572   07 33 11

07 34 10  OQ208        16 44 52  55.9 276.3  2.6      76.4   -13     1572   07 34 23
07 40 55  ---          16 51 38  54.5 276.9  2.7      76.1   392     1597   07 34 11

07 41 10  J1419+2706   16 51 53  56.9 273.4  2.5      74.6     2     1597   07 41 10
07 42 10  =1417+273    16 52 53  56.7 273.5  2.5      74.6    60     1601   07 41 11

07 42 10  OQ208        16 52 53  54.2 277.0  2.8      76.0   -13     1601   07 42 23
07 48 55  ---          16 59 39  52.8 277.7  2.9      75.7   392     1626   07 42 11

07 49 10  J1419+2706   16 59 54  55.2 274.2  2.7      74.4     2     1626   07 49 10
07 50 10  =1417+273    17 00 54  54.9 274.3  2.7      74.4    60     1630   07 49 11

07 50 10  OQ208        17 00 54  52.5 277.8  2.9      75.7   -13     1630   07 50 23
07 56 55  ---          17 07 41  51.1 278.4  3.0      75.3   392     1656   07 50 11

07 57 10  J1419+2706   17 07 56  53.4 275.0  2.8      74.2     2     1656   07 57 10
07 58 10  =1417+273    17 08 56  53.2 275.1  2.8      74.1    60     1659   07 57 11

07 58 10  OQ208        17 08 56  50.8 278.5  3.0      75.3   -13     1659   07 58 23
08 04 55  ---          17 15 42  49.4 279.1  3.1      74.9   392     1685   07 58 11

08 05 10  J1419+2706   17 15 57  51.7 275.8  2.9      73.9     2     1685   08 05 10
08 06 10  =1417+273    17 16 57  51.5 275.9  2.9      73.9    60     1688   08 05 11

08 06 10  OQ208        17 16 57  49.1 279.2  3.2      74.9   -13     1688   08 06 23
08 12 55  ---          17 23 43  47.7 279.8  3.3      74.5   392     1714   08 06 11

08 13 10  J1419+2706   17 23 58  50.0 276.6  3.1      73.6     2     1714   08 13 10
08 14 10  =1417+273    17 24 58  49.8 276.7  3.1      73.6    60     1718   08 13 11
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

08 14 10  OQ208        17 24 58  47.4 279.9  3.3      74.4   -13     1718   08 14 23
08 20 55  ---          17 31 44  46.0 280.5  3.4      74.1   392     1743   08 14 11

08 21 10  J1419+2706   17 32 00  48.3 277.4  3.2      73.3     2     1743   08 21 10
08 22 10  =1417+273    17 33 00  48.1 277.5  3.2      73.3    60     1747   08 21 11

08 22 10  OQ208        17 33 00  45.7 280.6  3.4      74.0   -13     1747   08 22 23
08 28 55  ---          17 39 46  44.3 281.2  3.5      73.6   392     1772   08 22 11

08 29 10  J1419+2706   17 40 01  46.6 278.2  3.3      72.9     2     1772   08 29 10
08 30 10  =1417+273    17 41 01  46.4 278.3  3.3      72.9    60     1776   08 29 11

08 31 40  3C345        17 42 31  74.9 311.3  1.0     122.8    26     1776   08 31 40
08 37 00  ---          17 47 52  74.1 309.3  1.1     120.0   320     1796   08 31 41

08 39 00  J1419+2706   17 49 52  44.5 279.1  3.5      72.5    54     1796   08 39 00
08 40 00  =1417+273    17 50 53  44.3 279.2  3.5      72.4    60     1800   08 39 01

08 40 00  OQ208        17 50 53  41.9 282.1  3.7      72.9   -13     1800   08 40 13
08 46 45  ---          17 57 39  40.5 282.7  3.8      72.5   392     1826   08 40 01

08 47 00  J1419+2706   17 57 54  42.8 279.9  3.6      72.1     2     1826   08 47 00
08 48 00  =1417+273    17 58 54  42.6 280.0  3.6      72.0    60     1829   08 47 01

08 48 00  OQ208        17 58 54  40.2 282.8  3.9      72.4   -13     1829   08 48 13
08 54 45  ---          18 05 40  38.8 283.4  4.0      72.0   392     1855   08 48 01

08 55 00  J1419+2706   18 05 55  41.1 280.6  3.8      71.7     2     1855   08 55 00
08 56 00  =1417+273    18 06 55  40.9 280.7  3.8      71.6    60     1859   08 55 01

08 56 00  OQ208        18 06 55  38.6 283.5  4.0      71.9   -13     1859   08 56 13
09 02 45  ---          18 13 41  37.2 284.1  4.1      71.5   392     1884   08 56 01

09 03 00  J1419+2706   18 13 56  39.4 281.4  3.9      71.3     2     1884   09 03 00
09 04 00  =1417+273    18 14 57  39.2 281.4  3.9      71.2    60     1888   09 03 01

09 04 00  OQ208        18 14 57  36.9 284.2  4.1      71.4   -13     1888   09 04 13
09 10 45  ---          18 21 43  35.5 284.8  4.2      71.0   392     1913   09 04 01

09 11 00  J1419+2706   18 21 58  37.7 282.1  4.0      70.8     3     1913   09 11 00
09 12 00  =1417+273    18 22 58  37.5 282.2  4.0      70.7    60     1917   09 11 01

09 12 00  OQ208        18 22 58  35.2 284.9  4.3      70.9   -13     1917   09 12 13
09 18 45  ---          18 29 44  33.8 285.5  4.4      70.4   392     1942   09 12 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GS045A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  24 May 2019   Day 144 ---

09 19 00  J1419+2706   18 29 59  36.0 282.8  4.2      70.3     3     1942   09 19 00
09 20 00  =1417+273    18 30 59  35.8 282.9  4.2      70.3    60     1946   09 19 01

09 20 00  OQ208        18 30 59  33.6 285.6  4.4      70.3   -13     1946   09 20 13
09 26 45  ---          18 37 45  32.2 286.3  4.5      69.8   392     1971   09 20 01

09 27 00  J1419+2706   18 38 00  34.3 283.6  4.3      69.9     3     1971   09 27 00
09 28 00  =1417+273    18 39 00  34.1 283.7  4.3      69.8    60     1975   09 27 01

09 28 00  OQ208        18 39 00  31.9 286.4  4.5      69.8   -12     1975   09 28 12
09 34 45  ---          18 45 47  30.5 287.0  4.6      69.3   393     2000   09 28 01

09 35 00  J1419+2706   18 46 02  32.7 284.3  4.4      69.4     3     2000   09 35 00
09 36 00  =1417+273    18 47 02  32.5 284.4  4.4      69.3    60     2004   09 35 01

09 36 00  OQ208        18 47 02  30.2 287.1  4.7      69.2   -12     2004   09 36 12
09 42 45  ---          18 53 48  28.9 287.7  4.8      68.7   393     2029   09 36 01

09 43 00  J1419+2706   18 54 03  31.0 285.1  4.6      68.8     3     2029   09 43 00
09 44 00  =1417+273    18 55 03  30.8 285.2  4.6      68.8    60     2033   09 43 01

09 44 00  OQ208        18 55 03  28.6 287.8  4.8      68.6   -12     2033   09 44 12
09 50 45  ---          19 01 49  27.2 288.4  4.9      68.1   393     2059   09 44 01

09 51 00  J1419+2706   19 02 04  29.3 285.8  4.7      68.3     3     2059   09 51 00
09 52 00  =1417+273    19 03 04  29.1 285.9  4.7      68.2    60     2063   09 51 01

09 52 00  OQ208        19 03 04  27.0 288.6  4.9      68.0   -12     2063   09 52 12
09 58 45  ---          19 09 51  25.6 289.2  5.0      67.4   393     2088   09 52 01

09 59 00  J1419+2706   19 10 06  27.7 286.6  4.8      67.8     3     2088   09 59 00
10 00 00  =1417+273    19 11 06  27.5 286.7  4.8      67.7    60     2092   09 59 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess219.H512glob
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = off
   LO sum=   1295.25  1295.25  1311.25  1311.25  1327.25  1327.25  1343.25  1343.25
   BBC fr=    804.75   804.75   788.75   788.75   772.75   772.75   756.75   756.75
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     788.75    788.75    772.75    772.75
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20  21  22

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * OQ208             14 04 45.615157   * 14 07 00.394415     14 07 52.878233       0.00
                     28 41 29.23512    * 28 27 14.69015      28 21 53.84474        0.00
                     From catalog imbedded in main SCHED input file.

   1417+273          14 17 45.094593   * 14 19 59.297078     14 20 51.605388       0.03
 * J1419+2706        27 20 09.10604    * 27 06 25.55282      27 01 16.09780        0.04
   J1419+27          /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,   1160 observations.

 * 3C345             16 41 17.606229   * 16 42 58.809967     16 43 39.006767       0.79
   J1642+3948        39 54 10.81492    * 39 48 36.99399      39 46 30.32855        0.59
   1641+399          /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
   J1642+39          GSFC 2016a X/S astro solution,  53724 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  OQ208      sess219.H512glob      1 2 3 4 5 6 7 12 13              13.483  1013.735
  J1419+2706 sess219.H512glob      1 2 3 4 5 6 7 12 13               2.367   199.310
  3C345      sess219.H512glob      1 2 3 4 5 6 7 12 13               0.339    30.684


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   OQ208              123.7
   J1419+2706         126.4
   3C345              118.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

