  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Radio AGN feedback
 Exp. Code:  GM081E  


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Suma Murthy

Address:  JIVE
          Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands

Phone:    +31 521 596 508
EMAIL:    murthy@jive.eu
Fax:
Phone during observation: +31 521 596 508

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
          v2: fixed (mixed-BW) tunings, line at 1313.75 with DOPINCR 250kHz
            line centered in USB of 2nd DBBC BBC per pol
 


COVER LETTER:


Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

 Next scan frequencies:  1285.75  1285.75  1301.75  1301.75  1317.75  1317.75  1333.75  1333.75
 Next BBC frequencies:    814.25   814.25   798.25   798.25   782.25   782.25   766.25   766.25
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

09 00 00  4C39.25      04 58 36  35.2  61.6 -4.5     -76.6     0        0   09 00 00
09 06 00  ---          05 04 37  36.4  61.9 -4.4     -77.4   360       23   09 00 01

09 07 00  J1049+1429   05 05 37  10.4  79.3 -5.8     -60.8     1       23   09 07 00
09 12 00  ---          05 10 38  11.4  79.9 -5.7     -61.0   300       43   09 07 01

09 12 00  J1056+1419   05 10 38   9.9  79.3 -5.8     -60.7   -11       43   09 12 11
09 17 00  ---          05 15 38  10.9  79.9 -5.7     -60.9   289       61   09 12 01

09 17 30  J1049+1429   05 16 09  12.6  80.6 -5.6     -61.2    19       61   09 17 30
09 19 00  ---          05 17 39  12.9  80.8 -5.6     -61.3    90       67   09 17 31

09 19 00  J1056+1419   05 17 39  11.4  80.1 -5.7     -61.0   -11       67   09 19 11
09 24 00  ---          05 22 40  12.4  80.7 -5.6     -61.2   289       86   09 19 01

09 24 30  J1049+1429   05 23 10  14.1  81.4 -5.5     -61.4    19       86   09 24 30
09 26 00  ---          05 24 40  14.4  81.6 -5.4     -61.5    90       91   09 24 31

09 26 00  J1056+1419   05 24 40  12.9  80.9 -5.6     -61.2   -11       91   09 26 11
09 31 00  ---          05 29 41  13.9  81.5 -5.5     -61.4   289      110   09 26 01

09 31 30  J1049+1429   05 30 11  15.6  82.3 -5.3     -61.7    19      110   09 31 30
09 33 00  ---          05 31 41  15.9  82.5 -5.3     -61.7    90      116   09 31 31

09 33 00  J1056+1419   05 31 41  14.3  81.8 -5.4     -61.5   -11      116   09 33 11
09 38 00  ---          05 36 42  15.4  82.4 -5.4     -61.6   289      134   09 33 01

09 38 30  J1049+1429   05 37 12  17.1  83.1 -5.2     -61.9    19      134   09 38 30
09 40 00  ---          05 38 42  17.4  83.3 -5.2     -61.9    90      140   09 38 31

09 40 00  J1056+1419   05 38 42  15.8  82.6 -5.3     -61.7   -11      140   09 40 11
09 45 00  ---          05 43 43  16.9  83.2 -5.2     -61.8   289      159   09 40 01

09 45 30  J1049+1429   05 44 13  18.6  83.9 -5.1     -62.0    19      159   09 45 30
09 47 00  ---          05 45 43  18.9  84.1 -5.1     -62.1    90      165   09 45 31

09 47 00  J1056+1419   05 45 43  17.3  83.5 -5.2     -61.9   -11      165   09 47 11
09 52 00  ---          05 50 44  18.4  84.1 -5.1     -62.0   289      183   09 47 01

09 52 30  J1049+1429   05 51 14  20.1  84.8 -5.0     -62.2    19      183   09 52 30
09 54 00  ---          05 52 45  20.4  85.0 -5.0     -62.2    90      189   09 52 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

09 54 00  J1056+1419   05 52 45  18.8  84.3 -5.1     -62.0   -11      189   09 54 11
09 59 00  ---          05 57 45  19.9  84.9 -5.0     -62.1   289      208   09 54 01

09 59 30  J1049+1429   05 58 15  21.6  85.6 -4.9     -62.3    19      208   09 59 30
10 01 00  ---          05 59 46  21.9  85.8 -4.9     -62.4    90      213   09 59 31

10 01 00  J1056+1419   05 59 46  20.3  85.1 -5.0     -62.2   -11      213   10 01 11
10 06 00  ---          06 04 47  21.4  85.8 -4.9     -62.3   289      232   10 01 01

10 06 30  J1049+1429   06 05 17  23.1  86.5 -4.8     -62.4    19      232   10 06 30
10 08 00  ---          06 06 47  23.4  86.7 -4.7     -62.5    90      238   10 06 31

10 08 00  J1056+1419   06 06 47  21.9  86.0 -4.9     -62.3   -11      238   10 08 11
10 13 00  ---          06 11 48  22.9  86.6 -4.8     -62.4   289      256   10 08 01

10 13 30  J1049+1429   06 12 18  24.6  87.3 -4.6     -62.5    19      256   10 13 30
10 15 00  ---          06 13 48  24.9  87.5 -4.6     -62.6    90      262   10 13 31

10 15 00  J1056+1419   06 13 48  23.4  86.9 -4.7     -62.4   -11      262   10 15 11
10 20 00  ---          06 18 49  24.4  87.5 -4.7     -62.5   289      281   10 15 01

10 20 30  J1049+1429   06 19 19  26.1  88.2 -4.5     -62.6    19      281   10 20 30
10 22 00  ---          06 20 49  26.4  88.4 -4.5     -62.6    90      287   10 20 31

10 22 00  J1056+1419   06 20 49  24.9  87.7 -4.6     -62.5   -11      287   10 22 11
10 27 00  ---          06 25 50  25.9  88.3 -4.5     -62.5   289      305   10 22 01

10 27 30  J1049+1429   06 26 20  27.6  89.1 -4.4     -62.6    19      305   10 27 30
10 29 00  ---          06 27 50  27.9  89.3 -4.4     -62.6    90      311   10 27 31

10 29 00  J1056+1419   06 27 50  26.4  88.6 -4.5     -62.5   -11      311   10 29 11
10 34 00  ---          06 32 51  27.5  89.2 -4.4     -62.6   289      330   10 29 01

10 34 30  J1049+1429   06 33 21  29.1  90.0 -4.3     -62.7    19      330   10 34 30
10 36 00  ---          06 34 51  29.4  90.2 -4.3     -62.7    90      335   10 34 31

10 36 00  J1056+1419   06 34 51  27.9  89.5 -4.4     -62.6   -11      335   10 36 11
10 41 00  ---          06 39 52  29.0  90.1 -4.3     -62.6   289      354   10 36 01

10 41 30  J1049+1429   06 40 22  30.6  90.9 -4.2     -62.6    19      354   10 41 30
10 43 00  ---          06 41 53  31.0  91.1 -4.2     -62.6    90      360   10 41 31

10 43 00  J1056+1419   06 41 53  29.4  90.4 -4.3     -62.6   -11      360   10 43 11
10 48 00  ---          06 46 53  30.5  91.0 -4.2     -62.6   289      378   10 43 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

10 48 30  J1049+1429   06 47 23  32.1  91.8 -4.1     -62.6    19      378   10 48 30
10 50 00  ---          06 48 54  32.5  92.0 -4.0     -62.6    90      384   10 48 31

10 50 00  J1056+1419   06 48 54  30.9  91.3 -4.1     -62.5   -11      384   10 50 11
10 55 00  ---          06 53 55  32.0  91.9 -4.1     -62.5   289      403   10 50 01

10 55 30  J1049+1429   06 54 25  33.6  92.7 -3.9     -62.5    19      403   10 55 30
10 57 00  ---          06 55 55  34.0  92.9 -3.9     -62.5    90      409   10 55 31

10 57 00  J1056+1419   06 55 55  32.4  92.2 -4.0     -62.5   -11      409   10 57 11
11 02 00  ---          07 00 56  33.5  92.9 -3.9     -62.4   289      427   10 57 01

11 02 30  J1049+1429   07 01 26  35.2  93.7 -3.8     -62.4    19      427   11 02 30
11 04 00  ---          07 02 56  35.5  93.9 -3.8     -62.4    90      433   11 02 31

11 04 00  J1056+1419   07 02 56  33.9  93.1 -3.9     -62.4   -11      433   11 04 11
11 09 00  ---          07 07 57  35.0  93.8 -3.8     -62.3   289      452   11 04 01

11 09 30  J1049+1429   07 08 27  36.7  94.7 -3.7     -62.3    19      452   11 09 30
11 11 00  ---          07 09 57  37.0  94.9 -3.7     -62.3    90      458   11 09 31

11 11 00  J1056+1419   07 09 57  35.4  94.1 -3.8     -62.3   -11      458   11 11 11
11 16 00  ---          07 14 58  36.5  94.8 -3.7     -62.2   289      476   11 11 01

11 16 30  J1049+1429   07 15 28  38.2  95.6 -3.6     -62.1    19      476   11 16 30
11 18 00  ---          07 16 58  38.5  95.9 -3.6     -62.1    90      482   11 16 31

11 20 00  4C39.25      07 18 59  62.3  63.7 -2.2     -97.5    66      482   11 20 00
11 25 00  ---          07 23 59  63.3  63.4 -2.1     -98.5   300      501   11 20 01

11 27 00  J1049+1429   07 26 00  40.4  97.2 -3.4     -61.8    66      501   11 27 00
11 30 00  ---          07 29 00  41.1  97.7 -3.4     -61.7   180      513   11 27 01

11 30 00  J1056+1419   07 29 00  39.5  96.8 -3.5     -61.8   -11      513   11 30 11
11 35 00  ---          07 34 01  40.6  97.6 -3.4     -61.6   289      531   11 30 01

11 35 30  J1049+1429   07 34 31  42.2  98.5 -3.3     -61.5    19      531   11 35 30
11 37 00  ---          07 36 01  42.6  98.7 -3.2     -61.4    90      537   11 35 31

11 37 00  J1056+1419   07 36 01  41.0  97.9 -3.4     -61.5   -11      537   11 37 11
11 42 00  ---          07 41 02  42.1  98.7 -3.3     -61.3   289      556   11 37 01

11 42 30  J1049+1429   07 41 32  43.7  99.6 -3.2     -61.1    19      556   11 42 30
11 44 00  ---          07 43 03  44.0  99.9 -3.1     -61.1    90      562   11 42 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

11 44 00  J1056+1419   07 43 03  42.5  99.0 -3.2     -61.2   -11      562   11 44 11
11 49 00  ---          07 48 03  43.6  99.8 -3.2     -61.0   289      580   11 44 01

11 49 30  J1049+1429   07 48 34  45.2 100.8 -3.0     -60.8    19      580   11 49 30
11 51 00  ---          07 50 04  45.5 101.0 -3.0     -60.7    90      586   11 49 31

11 51 00  J1056+1419   07 50 04  44.0 100.1 -3.1     -60.9   -11      586   11 51 11
11 56 00  ---          07 55 05  45.1 100.9 -3.0     -60.6   289      605   11 51 01

11 56 30  J1049+1429   07 55 35  46.7 102.0 -2.9     -60.3    19      605   11 56 30
11 58 00  ---          07 57 05  47.0 102.2 -2.9     -60.2    90      610   11 56 31

11 58 00  J1056+1419   07 57 05  45.5 101.3 -3.0     -60.5   -11      610   11 58 11
12 03 00  ---          08 02 06  46.5 102.1 -2.9     -60.2   289      629   11 58 01

12 03 30  J1049+1429   08 02 36  48.2 103.2 -2.8     -59.8    19      629   12 03 30
12 05 00  ---          08 04 06  48.5 103.5 -2.8     -59.7    90      635   12 03 31

12 05 00  J1056+1419   08 04 06  47.0 102.5 -2.9     -60.1   -11      635   12 05 11
12 10 00  ---          08 09 07  48.0 103.4 -2.8     -59.7   289      654   12 05 01

12 10 30  J1049+1429   08 09 37  49.6 104.5 -2.7     -59.3    19      654   12 10 30
12 12 00  ---          08 11 07  49.9 104.8 -2.7     -59.2    90      659   12 10 31

12 12 00  J1056+1419   08 11 07  48.4 103.8 -2.8     -59.6   -11      659   12 12 11
12 17 00  ---          08 16 08  49.5 104.7 -2.7     -59.2   289      678   12 12 01

12 17 30  J1049+1429   08 16 38  51.1 105.9 -2.6     -58.7    19      678   12 17 30
12 19 00  ---          08 18 08  51.4 106.2 -2.5     -58.5    90      684   12 17 31

12 19 00  J1056+1419   08 18 08  49.9 105.1 -2.7     -59.0   -11      684   12 19 11
12 24 00  ---          08 23 09  50.9 106.1 -2.6     -58.5   289      702   12 19 01

12 24 30  J1049+1429   08 23 39  52.5 107.4 -2.5     -58.0    19      702   12 24 30
12 26 00  ---          08 25 10  52.8 107.7 -2.4     -57.8    90      708   12 24 31

12 26 00  J1056+1419   08 25 10  51.3 106.5 -2.5     -58.3   -11      708   12 26 11
12 31 00  ---          08 30 10  52.4 107.5 -2.5     -57.8   289      727   12 26 01

12 31 30  J1049+1429   08 30 40  54.0 108.9 -2.3     -57.2    19      727   12 31 30
12 33 00  ---          08 32 11  54.3 109.2 -2.3     -57.0    90      733   12 31 31

12 33 00  J1056+1419   08 32 11  52.8 107.9 -2.4     -57.6   -11      733   12 33 11
12 38 00  ---          08 37 11  53.8 109.0 -2.3     -57.0   289      751   12 33 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

12 38 30  J1049+1429   08 37 42  55.4 110.5 -2.2     -56.3    19      751   12 38 30
12 40 00  ---          08 39 12  55.7 110.9 -2.2     -56.1    90      757   12 38 31

12 40 00  J1056+1419   08 39 12  54.2 109.5 -2.3     -56.8   -11      757   12 40 11
12 45 00  ---          08 44 13  55.2 110.7 -2.2     -56.1   289      776   12 40 01

12 45 30  J1049+1429   08 44 43  56.8 112.2 -2.1     -55.3    19      776   12 45 30
12 47 00  ---          08 46 13  57.1 112.6 -2.1     -55.1    90      781   12 45 31

12 47 00  J1056+1419   08 46 13  55.6 111.1 -2.2     -55.9   -11      781   12 47 11
12 52 00  ---          08 51 14  56.6 112.4 -2.1     -55.2   289      800   12 47 01

12 52 30  J1049+1429   08 51 44  58.2 114.0 -2.0     -54.2    19      800   12 52 30
12 54 00  ---          08 53 14  58.5 114.4 -2.0     -54.0    90      806   12 52 31

12 54 00  J1056+1419   08 53 14  57.0 112.9 -2.1     -54.9   -11      806   12 54 11
12 59 00  ---          08 58 15  58.0 114.2 -2.0     -54.1   289      824   12 54 01

12 59 30  J1049+1429   08 58 45  59.6 116.0 -1.9     -53.0    19      824   12 59 30
13 01 00  ---          09 00 15  59.8 116.4 -1.8     -52.7    90      830   12 59 31

13 01 00  J1056+1419   09 00 15  58.4 114.7 -2.0     -53.7   -11      830   13 01 11
13 06 00  ---          09 05 16  59.4 116.1 -1.9     -52.8   289      849   13 01 01

13 06 30  J1049+1429   09 05 46  60.9 118.1 -1.8     -51.6    19      849   13 06 30
13 08 00  ---          09 07 16  61.2 118.5 -1.7     -51.3    90      855   13 06 31

13 08 00  J1056+1419   09 07 16  59.8 116.7 -1.8     -52.4   -11      855   13 08 11
13 13 00  ---          09 12 17  60.7 118.2 -1.8     -51.4   289      873   13 08 01

13 13 30  J1049+1429   09 12 47  62.2 120.3 -1.6     -50.1    19      873   13 13 30
13 15 00  ---          09 14 18  62.5 120.8 -1.6     -49.7    90      879   13 13 31

13 15 00  J1056+1419   09 14 18  61.1 118.9 -1.7     -51.0   -11      879   13 15 11
13 20 00  ---          09 19 18  62.0 120.5 -1.6     -49.9   289      898   13 15 01

13 20 30  J1049+1429   09 19 48  63.5 122.8 -1.5     -48.3    19      898   13 20 30
13 22 00  ---          09 21 19  63.8 123.3 -1.5     -47.9    90      903   13 20 31

13 22 00  J1056+1419   09 21 19  62.4 121.2 -1.6     -49.4   -11      903   13 22 11
13 27 00  ---          09 26 20  63.3 122.9 -1.5     -48.2   289      922   13 22 01

13 27 30  J1049+1429   09 26 50  64.8 125.4 -1.4     -46.4    19      922   13 27 30
13 29 00  ---          09 28 20  65.0 126.0 -1.4     -45.9    90      928   13 27 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

13 29 00  J1056+1419   09 28 20  63.7 123.7 -1.5     -47.6   -11      928   13 29 11
13 34 00  ---          09 33 21  64.6 125.6 -1.4     -46.2   289      946   13 29 01

13 34 30  J1049+1429   09 33 51  66.0 128.3 -1.3     -44.2    19      946   13 34 30
13 36 00  ---          09 35 21  66.2 128.9 -1.3     -43.7    90      952   13 34 31

13 38 00  4C39.25      09 37 21  81.5 -11.8  0.1     166.9    12      952   13 38 00
13 43 00  ---          09 42 22  81.2 -18.0  0.2     160.0   300      972   13 38 01

13 45 00  J1049+1429   09 44 22  67.7 133.1 -1.1     -40.5     5      972   13 45 00
13 48 00  ---          09 47 23  68.1 134.5 -1.1     -39.3   180      983   13 45 01

13 48 00  J1056+1419   09 47 23  66.9 131.5 -1.2     -41.6   -10      983   13 48 10
13 53 00  ---          09 52 24  67.7 133.9 -1.1     -39.7   290     1002   13 48 01

13 53 30  J1049+1429   09 52 54  69.0 137.4 -1.0     -36.9    20     1002   13 53 30
13 55 00  ---          09 54 24  69.2 138.2 -0.9     -36.3    90     1008   13 53 31

13 56 00  4C39.25      09 55 24  80.0 -31.8  0.4     144.3   -70     1008   13 57 10
14 00 00  ---          09 59 25  79.6 -35.3  0.5     140.3   170     1019   13 56 01

14 02 00  J1049+1429   10 01 25  70.2 142.3 -0.8     -32.9   -14     1019   14 02 14
14 05 00  ---          10 04 26  70.5 144.1 -0.8     -31.4   166     1029   14 02 01

14 05 00  J1056+1419   10 04 26  69.5 140.3 -0.9     -34.5   -11     1029   14 05 11
14 12 00  ---          10 11 27  70.4 144.5 -0.8     -31.1   409     1056   14 05 01

14 12 30  J1049+1429   10 11 57  71.4 149.0 -0.7     -27.2    19     1056   14 12 30
14 14 00  ---          10 13 27  71.6 150.0 -0.6     -26.4    90     1061   14 12 31

14 14 00  J1056+1419   10 13 27  70.7 145.7 -0.7     -30.0   -11     1061   14 14 11
14 21 00  ---          10 20 28  71.5 150.3 -0.6     -26.1   409     1088   14 14 01

14 21 30  J1049+1429   10 20 58  72.3 155.4 -0.5     -21.7    19     1088   14 21 30
14 23 00  ---          10 22 29  72.5 156.5 -0.5     -20.7    90     1094   14 21 31

14 23 00  J1056+1419   10 22 29  71.7 151.7 -0.6     -24.9   -11     1094   14 23 11
14 30 00  ---          10 29 30  72.3 156.8 -0.5     -20.5   409     1120   14 23 01

14 30 30  J1049+1429   10 30 00  73.0 162.3 -0.3     -15.6    18     1120   14 30 30
14 32 00  ---          10 31 30  73.1 163.6 -0.3     -14.6    90     1126   14 30 31

14 32 00  J1056+1419   10 31 30  72.5 158.3 -0.4     -19.1   -12     1126   14 32 12
14 39 00  ---          10 38 31  73.0 163.8 -0.3     -14.3   408     1152   14 32 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

14 39 30  J1049+1429   10 39 01  73.5 169.8 -0.2      -9.1    18     1152   14 39 30
14 41 00  ---          10 40 32  73.6 171.0 -0.2      -8.0    90     1158   14 39 31

14 41 00  J1056+1419   10 40 32  73.1 165.4 -0.3     -12.9   -12     1158   14 41 12
14 48 00  ---          10 47 33  73.4 171.2 -0.2      -7.8   408     1184   14 41 01

14 48 30  J1049+1429   10 48 03  73.7 177.5 -0.0      -2.2    18     1184   14 48 30
14 50 00  ---          10 49 33  73.7 178.8 -0.0      -1.1    90     1190   14 48 31

14 50 00  J1056+1419   10 49 33  73.5 172.9 -0.1      -6.3   -12     1190   14 50 12
14 57 00  ---          10 56 34  73.6 178.9 -0.0      -1.0   408     1216   14 50 01

14 57 30  J1049+1429   10 57 04  73.7 185.3  0.1       4.7    18     1216   14 57 30
14 59 00  ---          10 58 35  73.6 186.6  0.1       5.8    90     1222   14 57 31

14 59 00  J1056+1419   10 58 35  73.6 180.6  0.0       0.6   -12     1222   14 59 12
15 06 00  ---          11 05 36  73.5 186.6  0.1       5.9   408     1248   14 59 01

15 06 30  J1049+1429   11 06 06  73.4 192.9  0.3      11.4    18     1248   15 06 30
15 08 00  ---          11 07 36  73.3 194.2  0.3      12.5    90     1254   15 06 31

15 08 00  J1056+1419   11 07 36  73.4 188.3  0.2       7.4   -12     1254   15 08 12
15 15 00  ---          11 14 37  73.1 194.1  0.3      12.5   408     1280   15 08 01

15 15 30  J1049+1429   11 15 07  72.8 200.2  0.4      17.8    18     1280   15 15 30
15 17 00  ---          11 16 38  72.7 201.4  0.4      18.9    90     1286   15 15 31

15 17 00  J1056+1419   11 16 38  73.0 195.8  0.3      14.0   -12     1286   15 17 12
15 24 00  ---          11 23 39  72.5 201.3  0.4      18.8   408     1312   15 17 01

15 24 30  J1049+1429   11 24 09  72.0 207.0  0.6      23.7    18     1312   15 24 30
15 26 00  ---          11 25 39  71.9 208.0  0.6      24.7    90     1318   15 24 31

15 26 00  J1056+1419   11 25 39  72.4 202.8  0.5      20.1   -12     1318   15 26 12
15 33 00  ---          11 32 40  71.7 207.9  0.6      24.5   408     1344   15 26 01

15 33 30  J1049+1429   11 33 10  71.1 213.1  0.7      29.1    19     1344   15 33 30
15 35 00  ---          11 34 41  70.9 214.1  0.7      29.9    90     1350   15 33 31

15 35 00  J1056+1419   11 34 41  71.5 209.3  0.6      25.7   -11     1350   15 35 11
15 42 00  ---          11 41 42  70.7 214.0  0.7      29.7   409     1377   15 35 01

15 42 30  J1049+1429   11 42 12  69.9 218.7  0.9      33.8    19     1377   15 42 30
15 44 00  ---          11 43 42  69.7 219.6  0.9      34.5    90     1382   15 42 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

15 44 00  J1056+1419   11 43 42  70.5 215.2  0.8      30.8   -11     1382   15 44 11
15 51 00  ---          11 50 43  69.6 219.4  0.9      34.3   409     1409   15 44 01

15 51 30  J1049+1429   11 51 13  68.6 223.7  1.0      37.9    19     1409   15 51 30
15 53 00  ---          11 52 44  68.4 224.5  1.0      38.5    90     1415   15 51 31

15 53 00  J1056+1419   11 52 44  69.3 220.6  0.9      35.2   -11     1415   15 53 11
16 00 00  ---          11 59 45  68.3 224.3  1.0      38.3   409     1441   15 53 01

16 00 30  J1049+1429   12 00 15  67.3 228.2  1.2      41.5    19     1441   16 00 30
16 02 00  ---          12 01 45  67.0 228.9  1.2      42.0    90     1447   16 00 31

16 03 00  3C279        12 02 45  51.2 158.0 -0.9     -18.9     2     1447   16 03 00
16 08 00  ---          12 07 46  51.6 159.9 -0.8     -17.3   300     1466   16 03 01

16 10 00  J1049+1429   12 09 46  65.7 232.4  1.3      44.8    61     1466   16 10 00
16 13 00  ---          12 12 47  65.2 233.7  1.4      45.7   180     1478   16 10 01

16 13 00  J1056+1419   12 12 47  66.2 230.5  1.2      43.2   -10     1478   16 13 10
16 20 00  ---          12 19 48  65.0 233.5  1.4      45.5   410     1504   16 13 01

16 20 30  J1049+1429   12 20 18  63.8 236.6  1.5      47.8    20     1504   16 20 30
16 22 00  ---          12 21 48  63.6 237.1  1.5      48.2    90     1510   16 20 31

16 22 00  J1056+1419   12 21 48  64.7 234.2  1.4      46.1   -10     1510   16 22 10
16 29 00  ---          12 28 49  63.4 236.9  1.5      48.0   410     1536   16 22 01

16 29 30  J1049+1429   12 29 20  62.2 239.7  1.6      50.1    20     1536   16 29 30
16 31 00  ---          12 30 50  61.9 240.2  1.7      50.4    90     1542   16 29 31

16 31 00  J1056+1419   12 30 50  63.1 237.6  1.5      48.5   -10     1542   16 31 10
16 38 00  ---          12 37 51  61.8 240.0  1.7      50.2   410     1568   16 31 01

16 38 30  J1049+1429   12 38 21  60.5 242.6  1.8      52.1    20     1568   16 38 30
16 40 00  ---          12 39 51  60.2 243.0  1.8      52.4    90     1574   16 38 31

16 40 00  J1056+1419   12 39 51  61.4 240.7  1.7      50.7   -10     1574   16 40 10
16 47 00  ---          12 46 52  60.1 242.8  1.8      52.1   410     1601   16 40 01

16 47 30  J1049+1429   12 47 22  58.7 245.2  1.9      53.7    20     1601   16 47 30
16 49 00  ---          12 48 53  58.4 245.6  2.0      54.0    90     1606   16 47 31

16 49 00  J1056+1419   12 48 53  59.7 243.4  1.9      52.5   -10     1606   16 49 10
16 56 00  ---          12 55 54  58.3 245.4  2.0      53.8   410     1633   16 49 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

16 56 30  J1049+1429   12 56 24  57.0 247.6  2.1      55.2    19     1633   16 56 30
16 58 00  ---          12 57 54  56.7 248.0  2.1      55.4    90     1639   16 56 31

16 58 00  J1056+1419   12 57 54  57.9 245.9  2.0      54.1   -10     1639   16 58 10
17 05 00  ---          13 04 55  56.5 247.8  2.1      55.2   410     1665   16 58 01

17 05 30  J1049+1429   13 05 25  55.1 249.8  2.2      56.5    19     1665   17 05 30
17 07 00  ---          13 06 56  54.8 250.1  2.3      56.7    90     1671   17 05 31

17 07 00  J1056+1419   13 06 56  56.1 248.2  2.2      55.5   -11     1671   17 07 11
17 14 00  ---          13 13 57  54.7 249.9  2.3      56.5   409     1697   17 07 01

17 14 30  J1049+1429   13 14 27  53.3 251.8  2.4      57.6    19     1697   17 14 30
17 16 00  ---          13 15 57  53.0 252.1  2.4      57.7    90     1703   17 14 31

17 16 00  J1056+1419   13 15 57  54.3 250.4  2.3      56.7   -11     1703   17 16 11
17 23 00  ---          13 22 58  52.9 251.9  2.4      57.5   409     1729   17 16 01

17 23 30  J1049+1429   13 23 28  51.5 253.7  2.5      58.5    19     1729   17 23 30
17 25 00  ---          13 24 59  51.1 254.0  2.6      58.6    90     1735   17 23 31

17 25 00  J1056+1419   13 24 59  52.5 252.4  2.5      57.8   -11     1735   17 25 11
17 32 00  ---          13 32 00  51.0 253.8  2.6      58.5   409     1761   17 25 01

17 32 30  J1049+1429   13 32 30  49.6 255.5  2.7      59.3    19     1761   17 32 30
17 34 00  ---          13 34 00  49.3 255.8  2.7      59.4    90     1767   17 32 31

17 34 00  J1056+1419   13 34 00  50.6 254.2  2.6      58.7   -11     1767   17 34 11
17 41 00  ---          13 41 01  49.2 255.6  2.7      59.3   409     1794   17 34 01

17 41 30  J1049+1429   13 41 31  47.7 257.2  2.8      60.0    19     1794   17 41 30
17 43 00  ---          13 43 02  47.4 257.4  2.9      60.1    90     1799   17 41 31

17 43 00  J1056+1419   13 43 02  48.7 256.0  2.8      59.4   -11     1799   17 43 11
17 50 00  ---          13 50 03  47.3 257.2  2.9      60.0   409     1826   17 43 01

17 50 30  J1049+1429   13 50 33  45.8 258.7  3.0      60.6    19     1826   17 50 30
17 52 00  ---          13 52 03  45.5 259.0  3.0      60.7    90     1831   17 50 31

17 52 00  J1056+1419   13 52 03  46.8 257.6  2.9      60.1   -11     1831   17 52 11
17 59 00  ---          13 59 04  45.4 258.8  3.0      60.5   409     1858   17 52 01

17 59 30  J1049+1429   13 59 34  43.9 260.2  3.1      61.1    19     1858   17 59 30
18 01 00  ---          14 01 05  43.6 260.5  3.2      61.2    90     1864   17 59 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

18 01 00  J1056+1419   14 01 05  44.9 259.2  3.1      60.7   -11     1864   18 01 11
18 08 00  ---          14 08 06  43.5 260.3  3.2      61.0   409     1890   18 01 01

18 08 30  J1049+1429   14 08 36  42.0 261.7  3.3      61.5    19     1890   18 08 30
18 10 00  ---          14 10 06  41.7 261.9  3.3      61.6    90     1896   18 08 31

18 11 00  3C279        14 11 06  49.4 208.9  1.2      24.7    14     1896   18 11 00
18 16 00  ---          14 16 07  48.9 210.6  1.3      26.2   300     1915   18 11 01

18 18 00  J1049+1429   14 18 07  39.9 263.1  3.5      61.9    75     1915   18 18 00
18 21 00  ---          14 21 08  39.3 263.6  3.5      62.0   180     1927   18 18 01

18 21 00  J1056+1419   14 21 08  40.7 262.4  3.4      61.6   -11     1927   18 21 11
18 28 00  ---          14 28 09  39.2 263.4  3.5      61.8   409     1953   18 21 01

18 28 30  J1049+1429   14 28 39  37.7 264.7  3.6      62.2    19     1953   18 28 30
18 30 00  ---          14 30 09  37.4 264.9  3.7      62.2    90     1959   18 28 31

18 30 00  J1056+1419   14 30 09  38.8 263.7  3.5      61.9   -11     1959   18 30 11
18 37 00  ---          14 37 10  37.3 264.7  3.7      62.1   409     1985   18 30 01

18 37 30  J1049+1429   14 37 41  35.8 265.9  3.8      62.4    19     1985   18 37 30
18 39 00  ---          14 39 11  35.4 266.1  3.8      62.4    90     1991   18 37 31

18 39 00  J1056+1419   14 39 11  36.8 265.0  3.7      62.2   -11     1991   18 39 11
18 46 00  ---          14 46 12  35.3 266.0  3.8      62.3   409     2017   18 39 01

18 46 30  J1049+1429   14 46 42  33.8 267.2  3.9      62.5    19     2017   18 46 30
18 48 00  ---          14 48 12  33.5 267.4  4.0      62.5    90     2023   18 46 31

18 48 00  J1056+1419   14 48 12  34.9 266.3  3.8      62.3   -11     2023   18 48 11
18 55 00  ---          14 55 13  33.4 267.2  4.0      62.4   409     2049   18 48 01

18 55 30  J1049+1429   14 55 43  31.9 268.4  4.1      62.6    19     2049   18 55 30
18 57 00  ---          14 57 14  31.6 268.6  4.1      62.6    90     2055   18 55 31

18 57 00  J1056+1419   14 57 14  33.0 267.5  4.0      62.5   -11     2055   18 57 11
19 04 00  ---          15 04 15  31.4 268.4  4.1      62.5   409     2082   18 57 01

19 04 30  J1049+1429   15 04 45  29.9 269.5  4.2      62.6    19     2082   19 04 30
19 06 00  ---          15 06 15  29.6 269.7  4.3      62.7    90     2087   19 04 31

19 06 00  J1056+1419   15 06 15  31.0 268.7  4.1      62.5   -11     2087   19 06 11
19 13 00  ---          15 13 16  29.5 269.6  4.3      62.6   409     2114   19 06 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

19 13 30  J1049+1429   15 13 46  28.0 270.7  4.4      62.6    19     2114   19 13 30
19 15 00  ---          15 15 17  27.7 270.9  4.4      62.6    90     2120   19 13 31

19 15 00  J1056+1419   15 15 17  29.1 269.8  4.3      62.6   -11     2120   19 15 11
19 22 00  ---          15 22 18  27.6 270.7  4.4      62.6   409     2146   19 15 01

19 22 30  J1049+1429   15 22 48  26.1 271.8  4.5      62.6    19     2146   19 22 30
19 24 00  ---          15 24 18  25.7 272.0  4.6      62.6    90     2152   19 22 31

19 24 00  J1056+1419   15 24 18  27.1 271.0  4.4      62.6   -11     2152   19 24 11
19 31 00  ---          15 31 19  25.6 271.8  4.6      62.5   409     2178   19 24 01

19 31 30  J1049+1429   15 31 49  24.1 272.9  4.7      62.5    19     2178   19 31 30
19 33 00  ---          15 33 20  23.8 273.1  4.7      62.5    90     2184   19 31 31

19 33 00  J1056+1419   15 33 20  25.2 272.1  4.6      62.5   -11     2184   19 33 11
19 40 00  ---          15 40 21  23.7 273.0  4.7      62.4   409     2210   19 33 01

19 40 30  J1049+1429   15 40 51  22.2 274.0  4.8      62.4    19     2210   19 40 30
19 42 00  ---          15 42 21  21.9 274.2  4.9      62.4    90     2216   19 40 31

19 42 00  J1056+1419   15 42 21  23.3 273.2  4.7      62.4   -11     2216   19 42 11
19 49 00  ---          15 49 22  21.7 274.1  4.9      62.3   409     2242   19 42 01

19 49 30  J1049+1429   15 49 52  20.2 275.1  5.0      62.2    19     2242   19 49 30
19 51 00  ---          15 51 23  19.9 275.3  5.0      62.2    90     2248   19 49 31

19 51 00  J1056+1419   15 51 23  21.3 274.3  4.9      62.3   -11     2248   19 51 11
19 58 00  ---          15 58 24  19.8 275.2  5.0      62.1   409     2274   19 51 01

19 58 30  J1049+1429   15 58 54  18.3 276.2  5.1      62.0    19     2274   19 58 30
20 00 00  ---          16 00 24  18.0 276.4  5.2      62.0    90     2280   19 58 31

20 00 00  J1056+1419   16 00 24  19.4 275.4  5.0      62.1   -11     2280   20 00 11
20 07 00  ---          16 07 25  17.9 276.2  5.2      61.9   409     2307   20 00 01

20 07 30  J1049+1429   16 07 55  16.4 277.3  5.3      61.8    19     2307   20 07 30
20 09 00  ---          16 09 26  16.1 277.5  5.3      61.7    90     2312   20 07 31

20 09 00  J1056+1419   16 09 26  17.5 276.5  5.2      61.9   -11     2312   20 09 11
20 16 00  ---          16 16 27  16.0 277.3  5.3      61.7   409     2339   20 09 01

20 16 30  J1049+1429   16 16 57  14.5 278.4  5.4      61.5    19     2339   20 16 30
20 18 00  ---          16 18 27  14.1 278.5  5.5      61.5    90     2345   20 16 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2022   Day 308 ---

20 19 00  3C279        16 19 27  29.4 241.9  3.4      49.7    22     2345   20 19 00
20 24 00  ---          16 24 28  28.5 242.8  3.5      50.3   300     2364   20 19 01

20 26 00  J1049+1429   16 26 28  12.4 279.5  5.6      61.2    81     2364   20 26 00
20 29 00  ---          16 29 29  11.8 279.8  5.6      61.1   180     2375   20 26 01

20 29 00  J1056+1419   16 29 29  13.2 278.9  5.5      61.3   -11     2375   20 29 11
20 36 00  ---          16 36 30  11.7 279.7  5.6      61.0   409     2402   20 29 01

20 36 30  J1049+1429   16 37 00  10.2 280.8  5.8      60.8    19     2402   20 36 30
20 38 00  ---          16 38 30   9.9 280.9  5.8      60.7    90     2408   20 36 31

20 38 00  J1056+1419   16 38 30  11.3 280.0  5.7      61.0   -11     2408   20 38 11
20 45 00  ---          16 45 31   9.8 280.8  5.8      60.7   409     2434   20 38 01

20 45 30  J1049+1429   16 46 02   8.3 281.8  5.9      60.4    19     2434   20 45 30
20 47 00  ---          16 47 32   8.0 282.0  5.9      60.3    90     2440   20 45 31

20 47 00  J1056+1419   16 47 32   9.4 281.0  5.8      60.6   -11     2440   20 47 11
20 52 00  ---          16 52 33   8.3 281.6  5.9      60.4   289     2458   20 47 01

20 55 00  3C279        16 55 33  22.4 248.1  4.0      53.4   143     2458   20 55 00
21 00 00  ---          17 00 34  21.4 248.9  4.1      53.8   300     2478   20 55 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess322.H512globline
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  12  Setup file default.  Used with PCAL = off
   LO sum=   1285.75  1285.75  1301.75  1301.75  1317.75  1317.75  1333.75  1333.75
   BBC fr=    814.25   814.25   798.25   798.25   782.25   782.25   766.25   766.25
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     798.25    798.25    782.25    782.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  12  13  14  15  16  17  18  19  20  22

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * J1056+1419        10 54 00.287615   * 10 56 38.839000     10 57 49.803099       0.00
                     14 35 32.88937    * 14 19 30.50000      14 12 18.23102        0.00
                     From catalog imbedded in main SCHED input file.

 * J1049+1429        10 47 07.218284   * 10 49 46.327579     10 50 57.576304       0.00
                     14 45 32.15417    * 14 29 38.57375      14 22 30.24351        0.00
                     From catalog imbedded in main SCHED input file.

 * 4C39.25           09 23 55.319216   * 09 27 03.013937     09 28 27.600151       0.31
   J0927+3902        39 15 23.56644    * 39 02 20.85185      38 56 21.08656        0.16
   0923+392          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0927+39          GSFC 2016a X/S astro solution, 250526 observations.

 * 3C279             12 53 35.831310   * 12 56 11.166577     12 57 20.186117       0.34
   J1256-0547       -05 31 07.99627    *-05 47 21.52513     -05 54 34.96600        0.56
   1253-055          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J1256-05          GSFC 2016a X/S astro solution,  13160 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J1056+1419 sess322.H512globline  1 2 3 4 5 6 7 12 21              12.550  1028.290
  J1049+1429 sess322.H512globline  1 2 3 4 5 6 7 12 21               4.150   337.415
  4C39.25    sess322.H512globline  1 2 3 4 5 6 7 12 21               0.650    73.759
  3C279      sess322.H512globline  12 21                             0.333    14.069


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J1056+1419          62.0
   J1049+1429          63.6
   4C39.25             90.3
   3C279               26.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

