  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Global-VLBI-K-NGC315
 Exp. Code:  GP060   


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Jongho Park

Address:  Korea Astronomy and Space Science Institute
          776, Daedeok-daero, Yuseong-gu
          Daejeon
          Republic of Korea

Phone:    +82-42-865-3265
EMAIL:    jpark@kasi.re.kr
Fax:
Phone during observation: +82-42-865-3265

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
 
 
 


COVER LETTER:



Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

 Next scan frequencies:  22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
 Next BBC frequencies:     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

03 00 00  NGC0315      23 17 19  68.1  83.9 -1.7     -83.0     0        0   03 00 00
03 06 40  ---          23 24 00  69.6  84.3 -1.6     -83.5   400      103   03 00 01

03 07 10  J0029+3456   23 24 30  75.5  67.9 -1.1    -103.1    10      103   03 07 10
03 08 40  =0026+346    23 26 01  75.8  67.6 -1.1    -103.6    90      126   03 07 11

03 08 50  J0029+3456   23 26 11  75.8  67.5 -1.1    -103.7     4      126   03 08 50
03 09 50  =0026+346    23 27 11  76.0  67.3 -1.1    -104.0    60      142   03 08 51

03 10 14  NGC0315      23 27 35  70.3  84.6 -1.5     -83.7     4      142   03 10 14
03 16 14  ---          23 33 36  71.6  85.0 -1.4     -84.0   360      234   03 10 15

03 16 24  NGC0315      23 33 46  71.7  85.0 -1.4     -84.0     4      234   03 16 24
03 22 24  ---          23 39 47  73.0  85.4 -1.3     -84.4   360      327   03 16 25

03 22 50  J0029+3456   23 40 13  78.6  63.9 -0.8    -109.3     3      327   03 22 50
03 24 20  =0026+346    23 41 43  78.9  63.3 -0.8    -110.0    90      350   03 22 51

03 24 30  J0029+3456   23 41 53  78.9  63.3 -0.8    -110.1     4      350   03 24 30
03 25 30  =0026+346    23 42 54  79.1  62.9 -0.8    -110.6    60      366   03 24 31

03 25 56  NGC0315      23 43 20  73.7  85.7 -1.3     -84.6     2      366   03 25 56
03 31 56  ---          23 49 21  75.0  86.1 -1.2     -84.9   360      459   03 25 57

03 32 06  NGC0315      23 49 31  75.0  86.2 -1.2     -85.0     4      459   03 32 06
03 38 06  ---          23 55 32  76.3  86.6 -1.1     -85.3   360      551   03 32 07

03 39 10  3C84         23 56 36  47.9  60.3 -3.4     -88.0     0      551   03 39 10
03 42 00  ---          23 59 26  48.4  60.3 -3.4     -88.5   170      595   03 39 11

03 42 11  3C84         23 59 37  48.4  60.3 -3.4     -88.5     5      595   03 42 11
03 43 41  ---          00 01 08  48.7  60.3 -3.3     -88.8    90      618   03 42 12

03 43 51  3C84         00 01 18  48.7  60.3 -3.3     -88.8     4      618   03 43 51
03 45 51  ---          00 03 18  49.1  60.3 -3.3     -89.1   120      649   03 43 52

03 46 37  0235+164     00 04 04  51.9 102.4 -2.6     -61.4     8      649   03 46 37
03 49 27  ---          00 06 54  52.5 102.9 -2.6     -61.1   170      693   03 46 38

03 49 38  0235+164     00 07 05  52.6 102.9 -2.5     -61.1     5      693   03 49 38
03 51 08  ---          00 08 35  52.9 103.2 -2.5     -61.0    90      716   03 49 39
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

03 51 18  0235+164     00 08 45  52.9 103.2 -2.5     -61.0     4      716   03 51 18
03 53 18  ---          00 10 46  53.3 103.6 -2.5     -60.8   120      747   03 51 19

03 54 35  J0029+3456   00 12 04  84.1  39.8 -0.3    -137.7     9      747   03 54 35
03 57 35  =0026+346    00 15 04  84.5  35.0 -0.3    -142.9   180      794   03 54 36

03 57 45  J0029+3456   00 15 14  84.5  34.8 -0.3    -143.2     4      794   03 57 45
03 59 15  =0026+346    00 16 44  84.7  32.1 -0.2    -146.1    90      817   03 57 46

03 59 25  J0029+3456   00 16 54  84.7  31.8 -0.2    -146.4     4      817   03 59 25
04 00 25  =0026+346    00 17 55  84.8  29.9 -0.2    -148.4    60      832   03 59 26

04 01 03  NGC0315      00 18 32  81.3  88.5 -0.7     -86.4   -12      832   04 01 15
04 07 03  ---          00 24 33  82.6  89.0 -0.6     -86.6   348      922   04 01 04

04 07 13  NGC0315      00 24 43  82.6  89.0 -0.6     -86.6     4      922   04 07 13
04 13 13  ---          00 30 44  83.9  89.7 -0.5     -86.7   360     1015   04 07 14

04 13 48  J0029+3456   00 31 19  85.6  -2.3  0.0     177.6   -39     1015   04 14 27
04 15 37  =0026+346    00 32 49  85.5  -6.2  0.0     173.4    70     1033   04 13 49

04 15 47  J0029+3456   00 33 19  85.5  -7.5  0.0     172.1     2     1033   04 15 47
04 16 47  =0026+346    00 34 19  85.5 -10.1  0.1     169.4    60     1048   04 15 48

04 17 23  NGC0315      00 34 55  84.8  90.2 -0.4     -86.7   -44     1048   04 18 06
04 23 23  ---          00 40 56  86.1  91.2 -0.3     -86.5   316     1129   04 17 24

04 23 33  NGC0315      00 41 06  86.1  91.2 -0.3     -86.5     4     1129   04 23 33
04 29 33  ---          00 47 07  87.4  92.7 -0.2     -85.7   360     1222   04 23 34

04 30 40  3C84         00 48 14  57.5  59.6 -2.6     -97.2     0     1222   04 30 40
04 33 40  ---          00 51 14  58.1  59.4 -2.5     -97.8   180     1269   04 30 41

04 33 50  3C84         00 51 24  58.1  59.4 -2.5     -97.9     4     1269   04 33 50
04 35 20  ---          00 52 54  58.4  59.4 -2.5     -98.2    90     1292   04 33 51

04 35 30  3C84         00 53 05  58.4  59.3 -2.5     -98.2     4     1292   04 35 30
04 37 30  ---          00 55 05  58.8  59.2 -2.4     -98.6   120     1323   04 35 31

04 38 27  0235+164     00 56 03  62.6 114.5 -1.7     -54.8    10     1323   04 38 27
04 41 27  ---          00 59 03  63.1 115.4 -1.7     -54.2   180     1369   04 38 28

04 41 37  0235+164     00 59 13  63.2 115.5 -1.7     -54.2     4     1369   04 41 37
04 43 07  ---          01 00 43  63.5 116.0 -1.7     -53.9    90     1392   04 41 38
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

04 43 17  0235+164     01 00 53  63.5 116.0 -1.7     -53.8     4     1392   04 43 17
04 45 17  ---          01 02 54  63.9 116.6 -1.6     -53.4   120     1423   04 43 18

04 47 09  J0029+3456   01 04 46  81.5 -56.1  0.6     119.2   -19     1423   04 47 28
04 51 49  =0026+346    01 09 27  80.7 -59.0  0.6     115.7   261     1490   04 47 10

04 52 13  J0029+3456   01 09 50  80.6 -59.2  0.7     115.5    18     1490   04 52 13
04 53 43  =0026+346    01 11 21  80.3 -60.0  0.7     114.5    90     1514   04 52 14

04 53 53  J0029+3456   01 11 31  80.3 -60.1  0.7     114.4     4     1514   04 53 53
04 54 53  =0026+346    01 12 31  80.1 -60.5  0.7     113.7    60     1529   04 53 54

04 56 52  NGC0315      01 14 30  86.7 268.3  0.3      86.3  -123     1529   04 58 55
05 02 55  ---          01 20 31  85.4 269.4  0.4      86.7   240     1591   04 56 53

05 03 05  NGC0315      01 20 44  85.3 269.4  0.4      86.7     4     1591   05 03 05
05 09 05  ---          01 26 45  84.0 270.3  0.5      86.7   360     1684   05 03 06

05 10 01  J0029+3456   01 27 42  77.2 294.1  1.0     106.3    31     1684   05 10 01
05 12 10  =0026+346    01 29 12  76.9 293.7  1.0     105.7   129     1717   05 10 02

05 12 20  J0029+3456   01 30 01  76.7 293.5  1.0     105.4     3     1717   05 12 20
05 13 20  =0026+346    01 31 01  76.5 293.2  1.0     105.0    60     1732   05 12 21

05 14 08  NGC0315      01 31 50  82.9 270.8  0.5      86.6    24     1732   05 14 08
05 20 08  ---          01 37 51  81.7 271.4  0.6      86.5   360     1825   05 14 09

05 20 18  NGC0315      01 38 01  81.6 271.4  0.6      86.4     4     1825   05 20 18
05 26 18  ---          01 44 02  80.3 271.9  0.7      86.2   360     1918   05 20 19

05 28 32  3C84         01 46 15  68.0 413.6 -1.6    -112.2    24     1918   05 28 32
05 33 22  ---          01 51 06  68.8 412.6 -1.5    -113.9   290     1993   05 28 33

05 33 35  3C84         01 51 20  68.9 412.6 -1.5    -114.0     7     1993   05 33 35
05 35 05  ---          01 52 50  69.1 412.2 -1.5    -114.6    90     2016   05 33 36

05 35 15  3C84         01 53 00  69.2 412.2 -1.5    -114.6     4     2016   05 35 15
05 37 15  ---          01 55 00  69.5 411.8 -1.4    -115.4   120     2047   05 35 16

05 38 32  0235+164     01 56 17  72.9 142.0 -0.7     -33.6  -122     2047   05 40 34
05 41 42  ---          01 59 28  73.3 144.2 -0.7     -31.7    68     2064   05 38 33

05 41 58  0235+164     01 59 44  73.3 144.4 -0.7     -31.6    10     2064   05 41 58
05 43 28  ---          02 01 14  73.5 145.4 -0.6     -30.6    90     2087   05 41 59
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

05 43 38  0235+164     02 01 24  73.5 145.6 -0.6     -30.5     4     2087   05 43 38
05 45 38  ---          02 03 25  73.8 147.0 -0.6     -29.3   120     2118   05 43 39

05 47 25  J0029+3456   02 05 12  69.7 288.9  1.6      95.9    -2     2118   05 47 27
05 51 25  =0026+346    02 09 12  68.8 288.7  1.6      95.1   238     2180   05 47 26

05 51 48  J0029+3456   02 09 36  68.8 288.6  1.7      95.0    17     2180   05 51 48
05 53 18  =0026+346    02 11 06  68.5 288.6  1.7      94.8    90     2203   05 51 49

05 53 28  J0029+3456   02 11 16  68.4 288.6  1.7      94.7     4     2203   05 53 28
05 54 28  =0026+346    02 12 16  68.2 288.5  1.7      94.5    60     2218   05 53 29

05 54 54  NGC0315      02 12 42  74.2 274.1  1.2      84.7     6     2218   05 54 54
06 00 54  ---          02 18 43  72.9 274.6  1.3      84.4   360     2311   05 54 55

06 01 04  NGC0315      02 18 53  72.8 274.6  1.3      84.4     4     2311   06 01 04
06 07 04  ---          02 24 54  71.5 275.0  1.4      84.0   360     2404   06 01 05

06 07 30  J0029+3456   02 25 20  65.6 288.1  1.9      92.3     6     2404   06 07 30
06 09 00  =0026+346    02 26 50  65.2 288.1  1.9      92.0    90     2427   06 07 31

06 09 10  J0029+3456   02 27 00  65.2 288.1  1.9      92.0     4     2427   06 09 10
06 10 10  =0026+346    02 28 00  65.0 288.1  2.0      91.9    60     2442   06 09 11

06 10 35  NGC0315      02 28 26  70.8 275.3  1.5      83.8     6     2442   06 10 35
06 16 35  ---          02 34 27  69.5 275.7  1.6      83.4   360     2535   06 10 36

06 16 45  NGC0315      02 34 37  69.5 275.7  1.6      83.4     4     2535   06 16 45
06 22 45  ---          02 40 38  68.2 276.1  1.7      83.1   360     2628   06 16 46

06 24 41  3C84         02 42 34  76.6 392.8 -0.6    -141.5    25     2628   06 24 41
06 28 51  ---          02 46 45  77.0 390.0 -0.6    -144.8   250     2692   06 24 42

06 29 09  3C84         02 47 03  77.1 389.8 -0.6    -145.1    11     2692   06 29 09
06 30 39  ---          02 48 33  77.2 388.8 -0.5    -146.4    90     2716   06 29 10

06 30 49  3C84         02 48 43  77.2 388.7 -0.5    -146.5     4     2716   06 30 49
06 32 49  ---          02 50 43  77.4 387.2 -0.5    -148.2   120     2746   06 30 50

06 35 43  0235+164     02 53 38  75.7 193.4  0.2      12.0    28     2746   06 35 43
06 40 53  ---          02 58 48  75.4 198.3  0.3      16.3   310     2826   06 35 44

06 41 13  0235+164     02 59 09  75.4 198.6  0.3      16.6    14     2826   06 41 13
06 42 43  ---          03 00 39  75.3 199.9  0.3      17.8    90     2849   06 41 14
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

06 42 53  0235+164     03 00 49  75.3 200.1  0.3      18.0     4     2849   06 42 53
06 44 53  ---          03 02 49  75.1 201.9  0.4      19.5   120     2880   06 42 54

06 46 01  NGC0315      03 03 58  63.2 277.8  2.1      81.6     7     2880   06 46 01
06 52 31  ---          03 10 29  61.8 278.2  2.2      81.2   390     2981   06 46 02

06 52 41  NGC0315      03 10 39  61.8 278.2  2.2      81.2     4     2981   06 52 41
06 59 11  ---          03 17 10  60.4 278.7  2.3      80.7   390     3081   06 52 42

06 59 45  J0029+3456   03 17 44  54.8 288.6  2.8      85.2    15     3081   06 59 45
07 01 15  =0026+346    03 19 14  54.5 288.6  2.8      85.0    90     3105   06 59 46

07 01 25  J0029+3456   03 19 24  54.5 288.6  2.8      85.0     4     3105   07 01 25
07 02 25  =0026+346    03 20 24  54.3 288.7  2.8      84.8    60     3120   07 01 26

07 02 47  NGC0315      03 20 46  59.6 278.9  2.4      80.5     3     3120   07 02 47
07 08 47  ---          03 26 47  58.3 279.4  2.5      80.1   360     3213   07 02 48

07 08 57  NGC0315      03 26 57  58.3 279.4  2.5      80.1     4     3213   07 08 57
07 14 57  ---          03 32 58  57.0 279.8  2.6      79.7   360     3305   07 08 58

07 15 20  J0029+3456   03 33 21  51.7 289.1  3.0      83.3     4     3305   07 15 20
07 16 50  =0026+346    03 34 51  51.4 289.2  3.1      83.2    90     3329   07 15 21

07 17 00  J0029+3456   03 35 01  51.3 289.2  3.1      83.2     4     3329   07 17 00
07 18 00  =0026+346    03 36 01  51.1 289.2  3.1      83.0    60     3344   07 17 01

07 18 22  NGC0315      03 36 24  56.3 280.0  2.6      79.4     4     3344   07 18 22
07 24 22  ---          03 42 25  55.0 280.5  2.7      79.0   360     3437   07 18 23

07 24 32  NGC0315      03 42 35  55.0 280.5  2.7      79.0     4     3437   07 24 32
07 30 32  ---          03 48 36  53.7 280.9  2.8      78.6   360     3530   07 24 33

07 31 48  3C84         03 49 52  77.6 334.3  0.5     150.1    21     3530   07 31 48
07 34 58  ---          03 53 03  77.3 332.0  0.5     147.3   190     3579   07 31 49

07 35 08  3C84         03 53 13  77.3 331.8  0.5     147.1     4     3579   07 35 08
07 36 38  ---          03 54 43  77.1 330.8  0.6     145.8    90     3602   07 35 09

07 36 48  3C84         03 54 53  77.1 330.7  0.6     145.7     4     3602   07 36 48
07 38 48  ---          03 56 53  76.9 329.3  0.6     144.0   120     3633   07 36 49

07 40 18  0235+164     03 58 23  67.3 236.6  1.3      48.6    16     3633   07 40 18
07 44 28  ---          04 02 34  66.6 238.2  1.4      49.8   250     3697   07 40 19
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

07 44 38  0235+164     04 02 44  66.6 238.3  1.4      49.9     4     3697   07 44 38
07 46 08  ---          04 04 14  66.3 238.9  1.4      50.3    90     3720   07 44 39

07 46 18  0235+164     04 04 24  66.2 239.0  1.4      50.3     4     3720   07 46 18
07 48 18  ---          04 06 25  65.9 239.7  1.4      50.9   120     3751   07 46 19

07 49 15  J0029+3456   04 07 22  44.8 290.7  3.6      79.6     8     3751   07 49 15
07 52 35  =0026+346    04 10 43  44.1 290.9  3.7      79.2   200     3803   07 49 16

07 52 45  J0029+3456   04 10 53  44.1 290.9  3.7      79.2     4     3803   07 52 45
07 54 15  =0026+346    04 12 23  43.8 290.9  3.7      79.1    90     3826   07 52 46

07 54 25  J0029+3456   04 12 33  43.7 290.9  3.7      79.1     4     3826   07 54 25
07 55 25  =0026+346    04 13 33  43.5 291.0  3.7      78.9    60     3841   07 54 26

07 55 46  NGC0315      04 13 54  48.4 282.8  3.2      76.8     3     3841   07 55 46
08 01 46  ---          04 19 55  47.1 283.2  3.3      76.4   360     3934   07 55 47

08 01 56  NGC0315      04 20 05  47.1 283.2  3.4      76.4     4     3934   08 01 56
08 07 56  ---          04 26 06  45.8 283.7  3.5      76.0   360     4027   08 01 57

08 08 16  J0029+3456   04 26 25  41.0 291.7  3.9      77.6     2     4027   08 08 16
08 09 46  =0026+346    04 27 56  40.7 291.8  4.0      77.4    90     4050   08 08 17

08 09 56  J0029+3456   04 28 06  40.6 291.8  4.0      77.4     4     4050   08 09 56
08 10 56  =0026+346    04 29 06  40.4 291.9  4.0      77.3    60     4066   08 09 57

08 11 15  NGC0315      04 29 26  45.1 283.9  3.5      75.7     2     4066   08 11 15
08 17 15  ---          04 35 27  43.9 284.4  3.6      75.3   360     4158   08 11 16

08 17 25  NGC0315      04 35 37  43.9 284.4  3.6      75.3     4     4158   08 17 25
08 23 25  ---          04 41 38  42.6 284.8  3.7      74.8   360     4251   08 17 26

08 24 33  3C84         04 42 45  70.3 309.4  1.4     117.3     5     4251   08 24 33
08 27 33  ---          04 45 46  69.8 308.7  1.4     116.1   180     4297   08 24 34

08 27 43  3C84         04 45 56  69.8 308.6  1.4     116.0     4     4297   08 27 43
08 29 13  ---          04 47 26  69.5 308.3  1.4     115.5    90     4321   08 27 44

08 29 23  3C84         04 47 36  69.5 308.3  1.4     115.4     4     4321   08 29 23
08 31 23  ---          04 49 36  69.2 307.8  1.5     114.6   120     4352   08 29 24

08 32 24  0235+164     04 50 38  57.2 252.5  2.2      58.9    14     4352   08 32 24
08 35 34  ---          04 53 48  56.5 253.2  2.2      59.3   190     4400   08 32 25
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

08 35 44  0235+164     04 53 58  56.5 253.2  2.2      59.3     4     4400   08 35 44
08 37 14  ---          04 55 29  56.2 253.6  2.3      59.5    90     4424   08 35 45

08 37 24  0235+164     04 55 39  56.1 253.6  2.3      59.5     4     4424   08 37 24
08 39 24  ---          04 57 39  55.7 254.0  2.3      59.7   120     4455   08 37 25

08 40 13  J0029+3456   04 58 29  34.6 293.7  4.5      74.2     0     4455   08 40 14
08 43 13  =0026+346    05 01 29  34.0 294.0  4.5      73.9   180     4501   08 40 14

08 43 23  J0029+3456   05 01 39  34.0 294.0  4.5      73.9     4     4501   08 43 23
08 44 53  =0026+346    05 03 09  33.7 294.1  4.5      73.7    90     4524   08 43 24

08 45 03  J0029+3456   05 03 19  33.7 294.1  4.5      73.7     4     4524   08 45 03
08 46 03  =0026+346    05 04 19  33.5 294.1  4.6      73.6    60     4540   08 45 04

08 46 22  NGC0315      05 04 38  37.8 286.6  4.1      73.1     2     4540   08 46 22
08 52 22  ---          05 10 39  36.6 287.1  4.2      72.6   360     4632   08 46 23

08 52 32  NGC0315      05 10 49  36.6 287.1  4.2      72.6     4     4632   08 52 32
08 58 32  ---          05 16 50  35.3 287.6  4.3      72.1   360     4725   08 52 33

08 58 50  J0029+3456   05 17 09  30.9 295.1  4.8      72.2     2     4725   08 58 50
09 00 50  =0026+346    05 19 09  30.6 295.2  4.8      72.0   120     4756   08 58 51

09 01 00  J0029+3456   05 19 19  30.5 295.2  4.8      72.0     4     4756   09 01 00
09 02 00  =0026+346    05 20 19  30.3 295.3  4.8      71.9    60     4771   09 01 01

09 02 19  NGC0315      05 20 37  34.6 287.9  4.4      71.8     2     4771   09 02 19
09 08 19  ---          05 26 38  33.3 288.4  4.5      71.3   360     4864   09 02 20

09 08 29  NGC0315      05 26 48  33.3 288.4  4.5      71.3     4     4864   09 08 29
09 14 29  ---          05 32 49  32.1 288.9  4.6      70.8   360     4957   09 08 30

09 15 40  3C84         05 34 01  61.3 301.6  2.2     101.6     6     4957   09 15 40
09 18 40  ---          05 37 01  60.7 301.4  2.3     100.9   180     5003   09 15 41

09 18 50  3C84         05 37 11  60.7 301.4  2.3     100.9     4     5003   09 18 50
09 20 20  ---          05 38 42  60.4 301.3  2.3     100.6    90     5027   09 18 51

09 20 30  3C84         05 38 52  60.4 301.3  2.3     100.5     4     5027   09 20 30
09 22 30  ---          05 40 52  60.0 301.2  2.3     100.1   120     5057   09 20 31

09 23 26  0235+164     05 41 48  46.4 262.1  3.0      62.9    20     5057   09 23 26
09 26 26  ---          05 44 49  45.8 262.6  3.1      63.0   180     5104   09 23 27
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

09 26 36  0235+164     05 44 59  45.7 262.6  3.1      63.0     4     5104   09 26 36
09 28 06  ---          05 46 29  45.4 262.8  3.1      63.0    90     5127   09 26 37

09 28 16  0235+164     05 46 39  45.4 262.9  3.1      63.1     4     5127   09 28 16
09 30 16  ---          05 48 39  45.0 263.2  3.1      63.1   120     5158   09 28 17

09 31 18  J0029+3456   05 49 42  24.7 297.6  5.3      68.7    15     5158   09 31 18
09 34 18  =0026+346    05 52 42  24.1 297.8  5.4      68.4   180     5204   09 31 19

09 34 28  J0029+3456   05 52 52  24.1 297.8  5.4      68.4     4     5204   09 34 28
09 35 58  =0026+346    05 54 23  23.8 298.0  5.4      68.2    90     5227   09 34 29

09 36 08  J0029+3456   05 54 33  23.7 298.0  5.4      68.2     4     5227   09 36 08
09 37 08  =0026+346    05 55 33  23.6 298.1  5.4      68.1    60     5243   09 36 09

09 37 26  NGC0315      05 55 51  27.4 290.9  4.9      68.8     3     5243   09 37 26
09 43 26  ---          06 01 52  26.2 291.4  5.0      68.3   360     5336   09 37 27

09 43 36  NGC0315      06 02 02  26.2 291.5  5.0      68.3     4     5336   09 43 36
09 49 36  ---          06 08 03  25.0 292.0  5.1      67.8   360     5428   09 43 37

09 50 00  J0029+3456   06 08 26  21.1 299.2  5.6      66.7     8     5428   09 50 00
09 52 00  =0026+346    06 10 27  20.7 299.3  5.7      66.4   120     5459   09 50 01

09 52 10  J0029+3456   06 10 37  20.7 299.3  5.7      66.4     4     5459   09 52 10
09 53 10  =0026+346    06 11 37  20.5 299.4  5.7      66.3    60     5475   09 52 11

09 53 33  NGC0315      06 12 00  24.2 292.3  5.2      67.4     8     5475   09 53 33
09 59 33  ---          06 18 01  23.0 292.9  5.3      66.9   360     5568   09 53 34

09 59 43  NGC0315      06 18 11  23.0 292.9  5.3      66.9     4     5568   09 59 43
10 05 43  ---          06 24 12  21.8 293.5  5.4      66.3   360     5660   09 59 44

10 06 53  3C84         06 25 23  51.7 299.7  3.1      91.4     4     5660   10 06 53
10 09 53  ---          06 28 23  51.2 299.7  3.1      90.9   180     5707   10 06 54

10 10 03  3C84         06 28 33  51.1 299.7  3.1      90.9     4     5707   10 10 03
10 11 33  ---          06 30 03  50.9 299.6  3.1      90.6    90     5730   10 10 04

10 11 43  3C84         06 30 13  50.8 299.6  3.1      90.6     4     5730   10 11 43
10 13 43  ---          06 32 14  50.5 299.6  3.2      90.3   120     5761   10 11 44

10 14 41  0235+164     06 33 12  35.4 269.4  3.9      63.9    20     5761   10 14 41
10 17 11  ---          06 35 42  34.9 269.7  3.9      63.9   150     5799   10 14 42
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Global-VLBI-K-NGC315
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   9 Nov 2022   Day 313 ---

10 17 21  0235+164     06 35 52  34.8 269.7  3.9      63.9     4     5799   10 17 21
10 18 51  ---          06 37 22  34.5 269.9  4.0      63.9    90     5823   10 17 22

10 19 01  0235+164     06 37 32  34.5 269.9  4.0      63.9     4     5823   10 19 01
10 21 01  ---          06 39 33  34.0 270.2  4.0      63.9   120     5854   10 19 02

10 22 14  J0029+3456   06 40 46  15.1 302.1  6.2      62.9    28     5854   10 22 14
10 25 04  =0026+346    06 43 36  14.6 302.4  6.2      62.6   170     5897   10 22 15

10 25 21  J0029+3456   06 43 53  14.6 302.4  6.2      62.6    11     5897   10 25 21
10 26 51  =0026+346    06 45 23  14.3 302.6  6.2      62.4    90     5921   10 25 22

10 27 01  J0029+3456   06 45 33  14.3 302.6  6.3      62.4     4     5921   10 27 01
10 28 01  =0026+346    06 46 33  14.1 302.7  6.3      62.2    60     5936   10 27 02

10 28 23  NGC0315      06 46 56  17.3 295.6  5.8      64.2     8     5936   10 28 23
10 34 23  ---          06 52 57  16.2 296.2  5.9      63.6   360     6029   10 28 24

10 34 33  NGC0315      06 53 07  16.1 296.3  5.9      63.6     4     6029   10 34 33
10 40 33  ---          06 59 08  15.0 296.9  6.0      63.0   360     6121   10 34 34

10 40 55  J0029+3456   06 59 30  11.8 304.0  6.5      60.7     8     6121   10 40 55
10 42 55  =0026+346    07 01 30  11.4 304.2  6.5      60.4   120     6152   10 40 56

10 43 05  J0029+3456   07 01 40  11.4 304.2  6.5      60.4     4     6152   10 43 05
10 44 05  =0026+346    07 02 40  11.2 304.3  6.5      60.3    60     6168   10 43 06

10 44 26  NGC0315      07 03 02  14.2 297.3  6.1      62.6     8     6168   10 44 26
10 50 26  ---          07 09 03  13.1 297.9  6.2      61.9   360     6261   10 44 27

10 50 36  NGC0315      07 09 13  13.0 297.9  6.2      61.9     4     6261   10 50 36
10 56 36  ---          07 15 14  11.9 298.5  6.3      61.3   360     6353   10 50 37

10 57 47  3C84         07 16 24  42.2 300.3  3.9      83.4     2     6353   10 57 47
11 00 47  ---          07 19 25  41.7 300.4  4.0      83.0   180     6400   10 57 48

11 00 57  3C84         07 19 35  41.6 300.4  4.0      83.0     4     6400   11 00 57
11 02 27  ---          07 21 05  41.3 300.4  4.0      82.7    90     6423   11 00 58

11 02 37  3C84         07 21 15  41.3 300.4  4.0      82.7     4     6423   11 02 37
11 04 37  ---          07 23 15  40.9 300.5  4.0      82.4   120     6454   11 02 38


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess322.K2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   7  Setup file default.  Used with PCAL = off
   LO sum=   22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
   BBC fr=     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   7   8   9  10  11  12  13  14  15  16

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   0026+346          00 26 34.833664   * 00 29 14.242482     00 30 27.345953       0.22
 * J0029+3456        34 39 57.70738    * 34 56 32.24713      35 04 14.32185        0.16
   J0029+34          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,    272 observations.

 * NGC0315           00 55 05.631043   * 00 57 48.883348     00 59 03.827293       0.05
   J0057+3021        30 04 57.07677    * 30 21 08.81189      30 28 39.25274        0.05
   0055+300          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0057+30          GSFC 2016a X/S astro solution,    881 observations.

 * 0119+115          01 19 03.080126   * 01 21 41.595043     01 22 54.393692       0.00
   J0121+1149        11 34 09.31522    * 11 49 50.41321      11 57 04.11267        0.01
   J0121+11          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  62476 observations.

 * 0221+067          02 21 49.960395   * 02 24 28.428193     02 25 41.358971       0.02
   J0224+0659        06 45 50.43663    * 06 59 23.34146      07 05 38.43234        0.02
   J0224+06          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,   2444 observations.

 * 0235+164          02 35 52.630214   * 02 38 38.930106     02 39 55.448566       0.12
   J0238+1636        16 24 04.01612    * 16 36 59.27454      16 42 57.62523        0.16
   J0238+16          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  64441 observations.

 * 3C84              03 16 29.567265   * 03 19 48.160096     03 21 19.689331       1.50
   J0319+4130        41 19 51.91692    * 41 30 42.10404      41 35 41.50000        2.86
   0316+413          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0319+41          GSFC 2016a X/S astro solution,  10291 observations.

 * 3C138             05 18 16.514083   * 05 21 09.885965     05 22 29.428204       0.06
   J0521+1638        16 35 26.83414    * 16 38 22.05160      16 39 46.11323        0.06
   0518+165          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0521+16          GSFC 2016a X/S astro solution,    352 observations.

 * 1921-293          19 21 42.234126   * 19 24 51.055953     19 26 15.613470       0.00
   J1924-2914       -29 20 26.35397    *-29 14 30.12107     -29 11 54.87713        0.01
   J1924-29          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  63480 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J0029+3456 sess322.K2048glob     1 2 3 4 5 7 17 20 21 22 23  +     2.781   168.082
  NGC0315    sess322.K2048glob     1 2 3 4 5 7 17 20 21 22 23  +     8.435   720.363
  0119+115   sess322.K2048glob     1                                 0.067     0.000
  0221+067   sess322.K2048glob     1                                 0.033     0.000
  0235+164   sess322.K2048glob     1 2 3 4 5 7 17 20 21 22 23  +     2.284    96.593
  3C84       sess322.K2048glob     1 2 4 5 7 17 20 21 22 23 25 +     2.050   101.642
  3C138      sess322.K2048glob     5                                 0.050     0.000
  1921-293   sess322.K2048glob     1 2 3 4                           2.700    16.200

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 3C454.3           22 51 29.519739   * 22 53 57.747939     22 55 05.178039       0.65
   J2253+1608        15 52 54.34808    * 16 08 53.56091      16 16 16.55060        0.73
   2251+158          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J2253+16          GSFC 2016a X/S astro solution,  41272 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0029+3456         142.5
   NGC0315            149.7
   0119+115           156.4
   0221+067           167.3
   0235+164           175.6
   3C84               154.8
   3C138              145.5
   1921-293            62.1
   3C454.3            122.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

