  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GG087B
 Exp. Code:  GG087B  


Schedule Version:       4.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Stefano Giarratana

Address:  University of Bologna
          via Gobetti
          Bologna
          Italy

Phone:    +393487994415
EMAIL:    stefano.giarratana@inaf.it
Fax:
Phone during observation:

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
          v4: Irbene 32->16; adds Sr
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

 Next scan frequencies:  4612.00  4612.00  4740.00  4740.00  4868.00  4868.00  4996.00  4996.00
 Next BBC frequencies:    512.00   512.00   640.00   640.00   768.00   768.00   896.00   896.00
 Next scan bandwidths:    128.00   128.00   128.00   128.00   128.00   128.00   128.00   128.00

17 34 45 J191142+1952  13 33 48  14.3  75.1 -5.6     -62.2     0        0   17 34 45
17 35 50  ---          13 34 53  14.6  75.2 -5.6     -62.2    65       33   17 34 46

17 35 50 J191249+1940  13 34 53  14.2  75.3 -5.6     -62.1    -8       33   17 35 58
17 37 20  ---          13 36 23  14.6  75.5 -5.6     -62.2    82       76   17 35 51

17 37 40 J191142+1952  13 36 43  15.0  75.4 -5.6     -62.3    12       76   17 37 40
17 38 50  ---          13 37 54  15.2  75.6 -5.6     -62.4    70      112   17 37 41

17 38 50  GRB221009A   13 37 54  14.9  75.5 -5.6     -62.3    -8      112   17 38 58
17 43 25  ---          13 42 29  15.8  76.0 -5.5     -62.6   267      249   17 38 51

17 44 00 J191142+1952  13 43 04  16.3  76.2 -5.5     -62.7    27      249   17 44 00
17 45 30  ---          13 44 35  16.6  76.3 -5.5     -62.8    90      296   17 44 01

17 45 30  GRB221009A   13 44 35  16.3  76.3 -5.5     -62.7    -8      296   17 45 38
17 50 05  ---          13 49 10  17.2  76.8 -5.4     -62.9   267      433   17 45 31

17 50 20 J191142+1952  13 49 25  17.6  76.9 -5.4     -63.0     7      433   17 50 20
17 51 45  ---          13 50 51  17.9  77.0 -5.4     -63.1    85      477   17 50 21

17 51 45  GRB221009A   13 50 51  17.6  77.0 -5.4     -63.0    -8      477   17 51 53
17 56 20  ---          13 55 26  18.5  77.5 -5.3     -63.2   267      615   17 51 46

17 56 40 J191142+1952  13 55 47  18.9  77.6 -5.3     -63.3    12      615   17 56 40
17 57 45  ---          13 56 52  19.2  77.7 -5.3     -63.4    65      648   17 56 41

17 57 45  J1905+1943   13 56 52  20.4  78.5 -5.2     -63.6   -10      648   17 57 55
17 59 30  ---          13 58 37  20.8  78.7 -5.1     -63.7    95      697   17 57 46

17 59 30 J191142+1952  13 58 37  19.5  77.9 -5.2     -63.5   -10      697   17 59 40
18 00 55  ---          14 00 02  19.8  78.0 -5.2     -63.5    75      736   17 59 31

18 01 10  J1925+211    14 00 17  17.5  75.3 -5.4     -63.2     2      736   18 01 10
18 02 10  ---          14 01 17  17.7  75.4 -5.4     -63.2    60      767   18 01 11

18 02 10  GRB221009A   14 01 17  19.8  78.1 -5.2     -63.5   -12      767   18 02 22
18 06 45  ---          14 05 53  20.7  78.6 -5.1     -63.7   263      902   18 02 11

18 07 05 J191142+1952  14 06 13  21.1  78.7 -5.1     -63.8    12      902   18 07 05
18 08 30  ---          14 07 38  21.4  78.9 -5.1     -63.9    85      946   18 07 06
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

18 08 30  GRB221009A   14 07 38  21.1  78.8 -5.1     -63.8    -8      946   18 08 38
18 13 05  ---          14 12 14  22.1  79.3 -5.0     -64.0   267     1084   18 08 31

18 13 20 J191142+1952  14 12 29  22.5  79.4 -5.0     -64.1     7     1084   18 13 20
18 14 45  ---          14 13 55  22.8  79.6 -5.0     -64.2    85     1127   18 13 21

18 14 45  J1923+2010   14 13 55  20.5  78.0 -5.2     -63.8   -12     1127   18 14 57
18 16 20  ---          14 15 30  20.8  78.2 -5.1     -63.8    83     1170   18 14 46

18 16 40 J191142+1952  14 15 50  23.2  79.8 -4.9     -64.2     7     1170   18 16 40
18 18 10  ---          14 17 20  23.5  80.0 -4.9     -64.3    90     1217   18 16 41

18 18 10  GRB221009A   14 17 20  23.2  79.9 -4.9     -64.2    -8     1217   18 18 18
18 22 45  ---          14 21 56  24.1  80.4 -4.9     -64.4   267     1354   18 18 11

18 23 00  J1925+211    14 22 11  22.0  77.7 -5.1     -64.4     3     1354   18 23 00
18 24 00  ---          14 23 11  22.2  77.8 -5.1     -64.4    60     1385   18 23 01

18 24 00 J191142+1952  14 23 11  24.7  80.6 -4.8     -64.5   -13     1385   18 24 13
18 25 25  ---          14 24 36  25.0  80.8 -4.8     -64.6    72     1422   18 24 01

18 25 25  GRB221009A   14 24 36  24.7  80.7 -4.8     -64.5    -8     1422   18 25 33
18 30 00  ---          14 29 12  25.7  81.2 -4.7     -64.7   267     1560   18 25 26

18 30 20 J191142+1952  14 29 32  26.1  81.3 -4.7     -64.8    12     1560   18 30 20
18 31 25  ---          14 30 37  26.3  81.4 -4.7     -64.8    65     1593   18 30 21

18 31 45 J191249+1940  14 30 57  26.1  81.6 -4.7     -64.7    12     1593   18 31 45
18 33 15  ---          14 32 28  26.4  81.7 -4.7     -64.8    90     1640   18 31 46

18 33 35 J191142+1952  14 32 48  26.8  81.7 -4.7     -64.9    12     1640   18 33 35
18 34 45  ---          14 33 58  27.0  81.8 -4.6     -64.9    70     1676   18 33 36

18 34 45  GRB221009A   14 33 58  26.7  81.8 -4.7     -64.8    -8     1676   18 34 53
18 39 20  ---          14 38 34  27.7  82.3 -4.6     -65.0   267     1813   18 34 46

18 39 35 J191142+1952  14 38 49  28.1  82.4 -4.6     -65.1     7     1813   18 39 35
18 41 00  ---          14 40 14  28.4  82.5 -4.5     -65.1    85     1857   18 39 36

18 41 00  GRB221009A   14 40 14  28.0  82.5 -4.6     -65.1    -8     1857   18 41 08
18 45 35  ---          14 44 50  29.0  83.0 -4.5     -65.2   267     1995   18 41 01

18 45 55 J191142+1952  14 45 10  29.4  83.1 -4.5     -65.3    12     1995   18 45 55
18 47 00  ---          14 46 15  29.6  83.2 -4.4     -65.3    65     2028   18 45 56
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

18 47 00  J1905+1943   14 46 15  30.9  84.1 -4.3     -65.4   -11     2028   18 47 11
18 48 45  ---          14 48 00  31.3  84.3 -4.3     -65.5    94     2077   18 47 01

18 48 45 J191142+1952  14 48 00  30.0  83.4 -4.4     -65.4   -10     2077   18 48 55
18 50 10  ---          14 49 25  30.3  83.6 -4.4     -65.4    75     2115   18 48 46

18 50 25  J1925+211    14 49 40  27.8  80.7 -4.6     -65.6     2     2115   18 50 25
18 51 25  ---          14 50 41  28.1  80.8 -4.6     -65.6    60     2146   18 50 26

18 51 25  GRB221009A   14 50 41  30.3  83.6 -4.4     -65.4   -12     2146   18 51 37
18 56 00  ---          14 55 16  31.2  84.2 -4.3     -65.5   263     2282   18 51 26

18 56 20 J191142+1952  14 55 36  31.6  84.3 -4.3     -65.6    12     2282   18 56 20
18 57 45  ---          14 57 02  31.9  84.4 -4.3     -65.6    85     2325   18 56 21

18 57 45  GRB221009A   14 57 02  31.6  84.4 -4.3     -65.5    -8     2325   18 57 53
19 02 20  ---          15 01 37  32.6  84.9 -4.2     -65.6   267     2463   18 57 46

19 02 35 J191142+1952  15 01 52  33.0  85.0 -4.2     -65.7     7     2463   19 02 35
19 04 00  ---          15 03 18  33.3  85.1 -4.2     -65.8    85     2507   19 02 36

19 04 00  J1923+2010   15 03 18  31.0  83.5 -4.3     -65.7   -13     2507   19 04 13
19 05 35  ---          15 04 53  31.3  83.7 -4.3     -65.7    82     2549   19 04 01

19 05 55 J191142+1952  15 05 13  33.7  85.4 -4.1     -65.8     7     2549   19 05 55
19 07 25  ---          15 06 43  34.0  85.5 -4.1     -65.8    90     2595   19 05 56

19 07 25  GRB221009A   15 06 43  33.7  85.5 -4.1     -65.7    -8     2595   19 07 33
19 12 00  ---          15 11 19  34.7  86.0 -4.0     -65.8   267     2733   19 07 26

19 12 15  J1925+211    15 11 34  32.5  83.1 -4.3     -66.3     3     2733   19 12 15
19 13 15  ---          15 12 34  32.7  83.2 -4.2     -66.4    60     2764   19 12 16

19 13 15 J191142+1952  15 12 34  35.3  86.2 -4.0     -65.9   -13     2764   19 13 28
19 14 40  ---          15 13 59  35.6  86.4 -4.0     -66.0    72     2801   19 13 16

19 14 40  GRB221009A   15 13 59  35.3  86.3 -4.0     -65.9    -8     2801   19 14 48
19 19 15  ---          15 18 35  36.2  86.9 -3.9     -66.0   267     2939   19 14 41

19 19 35 J191142+1952  15 18 55  36.6  87.0 -3.9     -66.0    12     2939   19 19 35
19 20 40  ---          15 20 00  36.9  87.1 -3.9     -66.1    65     2972   19 19 36

19 21 00 J191249+1940  15 20 20  36.6  87.2 -3.9     -65.9    12     2972   19 21 00
19 22 30  ---          15 21 51  36.9  87.4 -3.9     -65.9    90     3018   19 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

19 22 50 J191142+1952  15 22 11  37.3  87.4 -3.8     -66.1    12     3018   19 22 50
19 24 00  ---          15 23 21  37.6  87.5 -3.8     -66.1    70     3055   19 22 51

19 24 00  GRB221009A   15 23 21  37.3  87.5 -3.8     -66.0    -8     3055   19 24 08
19 28 35  ---          15 27 57  38.3  88.0 -3.8     -66.1   267     3192   19 24 01

19 28 50 J191142+1952  15 28 12  38.6  88.1 -3.7     -66.2     7     3192   19 28 50
19 30 15  ---          15 29 37  38.9  88.3 -3.7     -66.2    85     3236   19 28 51

19 30 15  GRB221009A   15 29 37  38.6  88.2 -3.7     -66.1    -8     3236   19 30 23
19 34 50  ---          15 34 13  39.6  88.8 -3.7     -66.1   267     3374   19 30 16

19 35 10 J191142+1952  15 34 33  40.0  88.9 -3.6     -66.2    12     3374   19 35 10
19 36 15  ---          15 35 38  40.2  89.0 -3.6     -66.2    65     3407   19 35 11

19 36 15  J1905+1943   15 35 38  41.5  90.0 -3.5     -66.1   -11     3407   19 36 26
19 38 00  ---          15 37 23  41.9  90.2 -3.5     -66.1    94     3455   19 36 16

19 38 00 J191142+1952  15 37 23  40.6  89.2 -3.6     -66.2   -10     3455   19 38 10
19 39 25  ---          15 38 48  40.9  89.4 -3.6     -66.2    75     3494   19 38 01

19 39 40  J1925+211    15 39 03  38.4  86.2 -3.8     -67.0     2     3494   19 39 40
19 40 40  ---          15 40 04  38.6  86.3 -3.8     -67.0    60     3525   19 39 41

19 40 40  GRB221009A   15 40 04  40.9  89.5 -3.6     -66.1   -12     3525   19 40 52
19 45 15  ---          15 44 39  41.8  90.1 -3.5     -66.1   263     3661   19 40 41

19 45 35 J191142+1952  15 44 59  42.2  90.2 -3.5     -66.2    12     3661   19 45 35
19 47 00  ---          15 46 25  42.6  90.4 -3.4     -66.2    85     3704   19 45 36

19 47 00  GRB221009A   15 46 25  42.2  90.3 -3.5     -66.1    -8     3704   19 47 08
19 51 35  ---          15 51 00  43.2  90.9 -3.4     -66.1   267     3842   19 47 01

19 51 50 J191142+1952  15 51 15  43.6  91.0 -3.4     -66.2     7     3842   19 51 50
19 53 15  ---          15 52 41  43.9  91.2 -3.3     -66.2    85     3886   19 51 51

19 53 15  J1923+2010   15 52 41  41.6  89.3 -3.5     -66.5   -13     3886   19 53 28
19 54 50  ---          15 54 16  41.9  89.5 -3.5     -66.5    82     3928   19 53 16

19 55 10 J191142+1952  15 54 36  44.3  91.4 -3.3     -66.2     7     3928   19 55 10
19 56 40  ---          15 56 06  44.6  91.6 -3.3     -66.2    90     3974   19 55 11

19 56 40  GRB221009A   15 56 06  44.3  91.6 -3.3     -66.1    -8     3974   19 56 48
20 01 15  ---          16 00 42  45.3  92.2 -3.2     -66.1   267     4112   19 56 41
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

20 01 30  J1925+211    16 00 57  43.1  88.8 -3.4     -67.3     3     4112   20 01 30
20 02 30  ---          16 01 57  43.3  89.0 -3.4     -67.3    60     4143   20 01 31

20 02 30 J191142+1952  16 01 57  45.9  92.4 -3.2     -66.1   -13     4143   20 02 43
20 03 55  ---          16 03 22  46.2  92.6 -3.2     -66.1    72     4180   20 02 31

20 03 55  GRB221009A   16 03 22  45.9  92.6 -3.2     -66.0    -8     4180   20 04 03
20 08 30  ---          16 07 58  46.9  93.2 -3.1     -65.9   267     4318   20 03 56

20 08 50 J191142+1952  16 08 18  47.3  93.3 -3.1     -66.0    12     4318   20 08 50
20 09 55  ---          16 09 23  47.5  93.5 -3.1     -66.0    65     4351   20 08 51

20 10 15 J191249+1940  16 09 43  47.2  93.6 -3.1     -65.8    12     4351   20 10 15
20 11 45  ---          16 11 14  47.6  93.8 -3.0     -65.8    90     4397   20 10 16

20 12 05 J191142+1952  16 11 34  48.0  93.8 -3.0     -65.9    12     4397   20 12 05
20 13 15  ---          16 12 44  48.2  93.9 -3.0     -65.9    70     4433   20 12 06

20 13 45  J1925+2106   16 13 14  45.7  90.4 -3.2     -67.3    17     4433   20 13 45
20 19 20  =1923+210    16 18 50  46.9  91.1 -3.1     -67.3   335     4606   20 13 46

20 19 20  GRB221009A   16 18 50  49.2  94.8 -2.9     -65.7   -12     4606   20 19 32
20 23 55  ---          16 23 26  50.2  95.5 -2.8     -65.6   263     4742   20 19 21

20 24 10  J1925+211    16 23 41  48.0  91.8 -3.1     -67.2     3     4742   20 24 10
20 25 10  ---          16 24 41  48.2  91.9 -3.0     -67.2    60     4772   20 24 11

20 25 10 J191142+1952  16 24 41  50.8  95.7 -2.8     -65.6   -13     4772   20 25 23
20 26 35  ---          16 26 06  51.1  95.9 -2.8     -65.5    72     4810   20 25 11

20 26 35  GRB221009A   16 26 06  50.7  95.9 -2.8     -65.5    -8     4810   20 26 43
20 31 10  ---          16 30 42  51.7  96.6 -2.7     -65.3   267     4947   20 26 36

20 31 30 J191142+1952  16 31 02  52.1  96.7 -2.7     -65.3    12     4947   20 31 30
20 33 00  ---          16 32 32  52.4  97.0 -2.7     -65.3    90     4994   20 31 31

20 33 00  GRB221009A   16 32 32  52.1  96.9 -2.7     -65.2    -8     4994   20 33 08
20 37 35  ---          16 37 08  53.1  97.6 -2.6     -65.0   267     5131   20 33 01

20 37 50 J191142+1952  16 37 23  53.5  97.7 -2.6     -65.1     7     5131   20 37 50
20 39 15  ---          16 38 48  53.8  98.0 -2.6     -65.0    85     5175   20 37 51

20 39 15  GRB221009A   16 38 48  53.5  97.9 -2.6     -64.9    -8     5175   20 39 23
20 43 50  ---          16 43 24  54.4  98.7 -2.5     -64.7   267     5313   20 39 16
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

20 44 10 J191142+1952  16 43 44  54.8  98.8 -2.5     -64.7    12     5313   20 44 10
20 45 15  ---          16 44 49  55.1  99.0 -2.5     -64.7    65     5346   20 44 11

20 45 15  J1905+1943   16 44 49  56.3 100.4 -2.4     -64.1   -10     5346   20 45 25
20 47 00  ---          16 46 35  56.7 100.7 -2.3     -63.9    95     5395   20 45 16

20 47 00 J191142+1952  16 46 35  55.4  99.3 -2.4     -64.6   -10     5395   20 47 10
20 48 25  ---          16 48 00  55.7  99.6 -2.4     -64.5    75     5434   20 47 01

20 48 40  J1925+211    16 48 15  53.3  95.3 -2.6     -66.7     2     5434   20 48 40
20 49 40  ---          16 49 15  53.5  95.4 -2.6     -66.7    60     5465   20 48 41

20 49 40  GRB221009A   16 49 15  55.7  99.7 -2.4     -64.4   -12     5465   20 49 52
20 54 15  ---          16 53 51  56.7 100.6 -2.3     -64.0   263     5600   20 49 41

20 54 35 J191142+1952  16 54 11  57.0 100.7 -2.3     -64.0    12     5600   20 54 35
20 56 00  ---          16 55 36  57.3 101.0 -2.3     -63.9    85     5644   20 54 36

20 56 00  GRB221009A   16 55 36  57.0 100.9 -2.3     -63.9    -8     5644   20 56 08
21 00 35  ---          17 00 12  58.0 101.8 -2.2     -63.6   267     5781   20 56 01

21 00 50 J191142+1952  17 00 27  58.4 101.9 -2.2     -63.5     7     5781   21 00 50
21 02 15  ---          17 01 52  58.7 102.2 -2.2     -63.4    85     5825   21 00 51

21 02 15  J1923+2010   17 01 52  56.4  99.5 -2.4     -64.7   -12     5825   21 02 27
21 03 50  ---          17 03 27  56.7  99.8 -2.3     -64.6    83     5868   21 02 16

21 04 10 J191142+1952  17 03 47  59.1 102.6 -2.1     -63.3     7     5868   21 04 10
21 05 40  ---          17 05 18  59.4 102.9 -2.1     -63.1    90     5914   21 04 11

21 05 40  GRB221009A   17 05 18  59.1 102.8 -2.1     -63.1    -8     5914   21 05 48
21 10 15  ---          17 09 53  60.0 103.8 -2.1     -62.7   267     6052   21 05 41

21 10 30  J1925+211    17 10 08  57.9  98.9 -2.3     -65.7     3     6052   21 10 30
21 11 30  ---          17 11 09  58.1  99.1 -2.3     -65.6    60     6083   21 10 31

21 11 30 J191142+1952  17 11 09  60.6 104.2 -2.0     -62.5   -13     6083   21 11 43
21 12 55  ---          17 12 34  60.9 104.5 -2.0     -62.4    72     6120   21 11 31

21 12 55  GRB221009A   17 12 34  60.6 104.4 -2.0     -62.4    -8     6120   21 13 03
21 17 30  ---          17 17 10  61.5 105.4 -1.9     -61.8   267     6258   21 12 56

21 17 50 J191142+1952  17 17 30  61.9 105.6 -1.9     -61.8    12     6258   21 17 50
21 18 55  ---          17 18 35  62.2 105.9 -1.9     -61.7    65     6291   21 17 51
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

21 19 15 J191249+1940  17 18 55  61.9 106.1 -1.9     -61.4    12     6291   21 19 15
21 20 45  ---          17 20 25  62.2 106.4 -1.9     -61.2    90     6337   21 19 16

21 21 05 J191142+1952  17 20 45  62.6 106.4 -1.9     -61.4    12     6337   21 21 05
21 22 15  ---          17 21 55  62.8 106.7 -1.8     -61.2    70     6373   21 21 06

21 22 15  GRB221009A   17 21 55  62.5 106.6 -1.9     -61.2    -8     6373   21 22 23
21 26 50  ---          17 26 31  63.5 107.7 -1.8     -60.6   267     6511   21 22 16

21 27 05  J1925+211    17 26 46  61.5 102.2 -2.0     -64.4     3     6511   21 27 05
21 28 05  ---          17 27 46  61.7 102.4 -2.0     -64.3    60     6542   21 27 06

21 28 05 J191142+1952  17 27 46  64.0 108.2 -1.7     -60.4   -13     6542   21 28 18
21 29 30  ---          17 29 11  64.3 108.6 -1.7     -60.2    72     6579   21 28 06

21 29 30  GRB221009A   17 29 11  64.0 108.4 -1.7     -60.2    -8     6579   21 29 38
21 34 05  ---          17 33 47  65.0 109.7 -1.7     -59.5   267     6717   21 29 31

21 34 25 J191142+1952  17 34 07  65.3 110.0 -1.6     -59.3    12     6717   21 34 25
21 35 30  ---          17 35 12  65.6 110.3 -1.6     -59.1    65     6750   21 34 26

21 35 30  J1905+1943   17 35 12  66.7 112.5 -1.5     -57.7   -10     6750   21 35 40
21 37 15  ---          17 36 58  67.0 113.0 -1.5     -57.3    95     6799   21 35 31

21 37 15 J191142+1952  17 36 58  65.9 110.8 -1.6     -58.8   -10     6799   21 37 25
21 38 40  ---          17 38 23  66.2 111.2 -1.6     -58.5    75     6838   21 37 16

21 38 55  GRB221009A   17 38 38  65.9 111.1 -1.6     -58.6     7     6838   21 38 55
21 43 30  ---          17 43 14  66.8 112.5 -1.5     -57.7   275     6979   21 38 56

21 43 50 J191142+1952  17 43 34  67.2 112.9 -1.5     -57.5    12     6979   21 43 50
21 45 15  ---          17 44 59  67.5 113.3 -1.5     -57.2    85     7023   21 43 51

21 45 45  J1925+2106   17 45 29  65.4 106.6 -1.7     -62.2    17     7023   21 45 45
21 51 40  =1923+210    17 51 25  66.6 108.2 -1.6     -61.2   355     7206   21 45 46

21 52 00 J191142+1952  17 51 45  68.8 115.7 -1.3     -55.6     7     7206   21 52 00
21 53 30  ---          17 53 15  69.1 116.3 -1.3     -55.2    90     7253   21 52 01

21 53 30  GRB221009A   17 53 15  68.8 116.0 -1.3     -55.3    -8     7253   21 53 38
21 58 05  ---          17 57 51  69.7 117.7 -1.3     -54.1   267     7390   21 53 31

21 58 20  J1925+211    17 58 06  67.9 110.1 -1.5     -60.0     2     7390   21 58 20
21 59 20  ---          17 59 06  68.1 110.5 -1.5     -59.8    60     7421   21 58 21
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

21 59 20 J191142+1952  17 59 06  70.2 118.6 -1.2     -53.5   -14     7421   21 59 34
22 00 45  ---          18 00 32  70.5 119.2 -1.2     -53.0    71     7458   21 59 21

22 00 45  GRB221009A   18 00 32  70.2 118.8 -1.2     -53.3    -8     7458   22 00 53
22 05 20  ---          18 05 07  71.1 120.8 -1.1     -51.8   267     7595   22 00 46

22 05 40 J191142+1952  18 05 27  71.4 121.3 -1.1     -51.4    12     7595   22 05 40
22 06 45  ---          18 06 33  71.6 121.8 -1.1     -51.0    65     7629   22 05 41

22 06 45  J1905+1943   18 06 33  72.6 125.2 -1.0     -48.3   -10     7629   22 06 55
22 08 30  ---          18 08 18  72.9 126.2 -1.0     -47.6    95     7678   22 06 46

22 08 30 J191142+1952  18 08 18  71.9 122.7 -1.1     -50.4   -10     7678   22 08 40
22 09 55  ---          18 09 43  72.2 123.4 -1.1     -49.8    75     7716   22 08 31

22 10 10  GRB221009A   18 09 58  71.9 123.1 -1.1     -50.0     7     7716   22 10 10
22 14 45  ---          18 14 34  72.8 125.4 -1.0     -48.2   275     7858   22 10 11

22 15 05 J191142+1952  18 14 54  73.1 126.1 -1.0     -47.7    12     7858   22 15 05
22 16 30  ---          18 16 19  73.4 126.8 -0.9     -47.1    85     7902   22 15 06

22 16 30  GRB221009A   18 16 19  73.1 126.3 -1.0     -47.5    -8     7902   22 16 38
22 21 05  ---          18 20 55  73.9 129.0 -0.9     -45.3   267     8039   22 16 31

22 21 20  J1925+211    18 21 10  72.5 118.8 -1.1     -54.0     0     8039   22 21 20
22 22 20  ---          18 22 10  72.6 119.2 -1.1     -53.6    60     8070   22 21 21

22 22 20 J191142+1952  18 22 10  74.3 130.3 -0.8     -44.3   -16     8070   22 22 36
22 23 45  ---          18 23 35  74.6 131.2 -0.8     -43.5    69     8106   22 22 21

22 23 45  J1923+2010   18 23 35  72.8 123.8 -1.0     -49.7   -13     8106   22 23 58
22 25 20  ---          18 25 11  73.1 124.6 -1.0     -49.0    82     8148   22 23 46

22 25 40 J191142+1952  18 25 31  74.9 132.5 -0.8     -42.5     7     8148   22 25 40
22 27 10  ---          18 27 01  75.1 133.5 -0.8     -41.6    90     8194   22 25 41

22 27 10  GRB221009A   18 27 01  74.8 132.8 -0.8     -42.2    -8     8194   22 27 18
22 31 45  ---          18 31 37  75.6 136.0 -0.7     -39.4   267     8332   22 27 11

22 32 00 J191142+1952  18 31 52  75.9 136.9 -0.7     -38.7     7     8332   22 32 00
22 33 25  ---          18 33 17  76.1 138.0 -0.7     -37.7    85     8376   22 32 01

22 33 25  GRB221009A   18 33 17  75.8 137.2 -0.7     -38.4    -8     8376   22 33 33
22 38 00  ---          18 37 53  76.4 140.8 -0.6     -35.3   267     8513   22 33 26
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

22 38 20 J191142+1952  18 38 13  76.7 142.0 -0.6     -34.3    12     8513   22 38 20
22 39 25  ---          18 39 18  76.9 143.0 -0.6     -33.5    65     8547   22 38 21

22 39 40  J1925+211    18 39 33  75.7 128.9 -0.8     -45.9    -3     8547   22 39 43
22 40 40  ---          18 40 33  75.9 129.5 -0.8     -45.4    57     8576   22 39 41

22 40 40 J191249+1940  18 40 33  76.7 143.5 -0.6     -32.9   -18     8576   22 40 58
22 42 10  ---          18 42 03  76.9 144.9 -0.5     -31.7    72     8613   22 40 41

22 42 10 J191142+1952  18 42 03  77.2 145.4 -0.5     -31.3    -8     8613   22 42 18
22 43 40  ---          18 43 34  77.4 146.8 -0.5     -30.1    82     8656   22 42 11

22 43 40  GRB221009A   18 43 34  77.2 145.8 -0.5     -31.0    -8     8656   22 43 48
22 48 15  ---          18 48 09  77.7 150.1 -0.4     -27.1   267     8793   22 43 41

22 48 30 J191142+1952  18 48 24  78.0 151.5 -0.4     -25.9     6     8793   22 48 30
22 49 55  ---          18 49 50  78.1 153.0 -0.4     -24.6    85     8837   22 48 31

22 49 55  GRB221009A   18 49 50  77.9 151.8 -0.4     -25.6    -8     8837   22 50 03
22 54 30  ---          18 54 25  78.3 156.6 -0.3     -21.3   267     8975   22 49 56

22 54 45  J1925+211    18 54 40  78.1 140.7 -0.5     -35.8    -4     8975   22 54 49
22 55 45  ---          18 55 41  78.2 141.6 -0.5     -35.0    56     9003   22 54 46

22 55 45 J191142+1952  18 55 41  78.6 159.3 -0.3     -18.9   -21     9003   22 56 06
22 57 10  ---          18 57 06  78.7 160.9 -0.3     -17.4    64     9036   22 55 46

22 57 10  GRB221009A   18 57 06  78.5 159.5 -0.3     -18.7    -9     9036   22 57 19
23 01 45  ---          19 01 42  78.8 164.8 -0.2     -13.9   266     9173   22 57 11

23 02 05 J191142+1952  19 02 02  79.0 166.7 -0.2     -12.2    11     9173   23 02 05
23 03 10  ---          19 03 07  79.1 168.0 -0.2     -11.0    65     9207   23 02 06

23 03 10  J1905+1943   19 03 07  79.1 175.6 -0.1      -4.0   -13     9207   23 03 23
23 04 55  ---          19 04 52  79.1 177.8 -0.0      -2.0    92     9254   23 03 11

23 04 55 J191142+1952  19 04 52  79.1 170.2 -0.1      -9.0   -13     9254   23 05 08
23 06 20  ---          19 06 17  79.2 171.9 -0.1      -7.4    72     9291   23 04 56

23 06 35  GRB221009A   19 06 32  79.0 170.6 -0.1      -8.6     6     9291   23 06 35
23 11 10  ---          19 11 08  79.2 176.3 -0.0      -3.4   275     9433   23 06 36

23 11 30 J191142+1952  19 11 28  79.3 178.4 -0.0      -1.5    11     9433   23 11 30
23 12 55  ---          19 12 53  79.3 180.2  0.0       0.2    85     9477   23 11 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

23 12 55  GRB221009A   19 12 53  79.2 178.5 -0.0      -1.4    -9     9477   23 13 04
23 17 30  ---          19 17 29  79.2 184.3  0.1       3.9   266     9614   23 12 56

23 17 45  J1925+211    19 17 44  80.3 167.1 -0.2     -11.9    -5     9614   23 17 50
23 18 45  ---          19 18 44  80.3 168.4 -0.1     -10.7    55     9642   23 17 46

23 18 45 J191142+1952  19 18 44  79.2 187.6  0.1       6.9   -22     9642   23 19 07
23 20 10  ---          19 20 10  79.1 189.3  0.1       8.5    63     9675   23 18 46

23 20 10  J1923+2010   19 20 10  79.6 174.7 -0.1      -4.8   -18     9675   23 20 28
23 21 45  ---          19 21 45  79.6 176.8 -0.0      -3.0    77     9715   23 20 11

23 22 05 J191142+1952  19 22 05  79.1 191.7  0.2      10.7     2     9715   23 22 05
23 23 35  ---          19 23 35  79.0 193.5  0.2      12.3    90     9761   23 22 06

23 23 35  GRB221009A   19 23 35  79.0 191.8  0.2      10.7    -9     9761   23 23 44
23 28 10  ---          19 28 11  78.7 197.2  0.2      15.7   266     9898   23 23 36

23 28 25 J191142+1952  19 28 26  78.7 199.2  0.3      17.5     6     9898   23 28 25
23 29 50  ---          19 29 51  78.6 200.8  0.3      19.0    85     9942   23 28 26

23 29 50  GRB221009A   19 29 51  78.6 199.1  0.3      17.4    -9     9942   23 29 59
23 34 25  ---          19 34 27  78.2 204.2  0.3      22.0   266    10079   23 29 51

23 34 45 J191142+1952  19 34 47  78.2 206.2  0.4      23.8    11    10079   23 34 45
23 35 50  ---          19 35 52  78.1 207.3  0.4      24.8    65    10112   23 34 46

23 36 05  J1925+211    19 36 07  80.3 192.7  0.2      11.7    -3    10112   23 36 08
23 37 05  ---          19 37 07  80.3 194.1  0.2      13.0    57    10142   23 36 06

23 37 05 J191249+1940  19 37 07  77.9 207.0  0.4      24.5   -17    10142   23 37 22
23 38 35  ---          19 38 38  77.7 208.6  0.4      25.9    73    10179   23 37 06

23 38 35 J191142+1952  19 38 38  77.8 210.1  0.4      27.3    -9    10179   23 38 44
23 40 05  ---          19 40 08  77.6 211.5  0.5      28.6    81    10221   23 38 36

23 40 05  GRB221009A   19 40 08  77.7 210.0  0.4      27.2    -9    10221   23 40 14
23 44 40  ---          19 44 44  77.2 214.4  0.5      31.1   266    10358   23 40 06

23 44 55 J191142+1952  19 44 59  77.0 216.0  0.5      32.6     6    10358   23 44 55
23 46 20  ---          19 46 24  76.9 217.3  0.6      33.6    85    10402   23 44 56

23 46 20  GRB221009A   19 46 24  77.0 215.9  0.5      32.4    -9    10402   23 46 29
23 50 55  ---          19 51 00  76.3 219.7  0.6      35.8   266    10539   23 46 21
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   4 Nov 2023   Day 308 ---

23 51 10  J1925+211    19 51 15  79.1 211.3  0.4      28.6     1    10539   23 51 10
23 52 10  ---          19 52 15  79.0 212.4  0.4      29.6    60    10570   23 51 11

23 52 10 J191142+1952  19 52 15  76.1 222.0  0.7      37.8   -15    10570   23 52 25
23 53 35  ---          19 53 40  75.8 223.1  0.7      38.7    70    10606   23 52 11

23 53 35  GRB221009A   19 53 40  76.0 221.8  0.7      37.6    -9    10606   23 53 44
23 58 10  ---          19 58 16  75.3 225.2  0.7      40.5   266    10743   23 53 36

23 58 30 J191142+1952  19 58 36  75.1 226.6  0.8      41.7    11    10743   23 58 30
23 59 35  ---          19 59 41  74.9 227.4  0.8      42.3    65    10777   23 58 31

 --- Start: Sat   4 Nov 2023   Day 308 -- Stop: Sun   5 Nov 2023   Day 309 ---

23 59 35  J1905+1943   19 59 41  73.8 230.8  0.9      45.1   -10    10777   23 59 45
00 01 20  ---          20 01 26  73.5 231.9  0.9      46.0    95    10825   23 59 36

00 01 20 J191142+1952  20 01 26  74.6 228.5  0.8      43.3   -10    10825   00 01 30
00 02 45  ---          20 02 52  74.4 229.4  0.8      44.0    75    10864   00 01 21

00 03 00  GRB221009A   20 03 07  74.5 228.5  0.8      43.2     7    10864   00 03 00
00 07 35  ---          20 07 42  73.8 231.3  0.9      45.6   275    11006   00 03 01

00 07 55 J191142+1952  20 08 03  73.6 232.5  0.9      46.6    12    11006   00 07 55
00 09 20  ---          20 09 28  73.3 233.3  0.9      47.2    85    11050   00 07 56

00 09 20  GRB221009A   20 09 28  73.5 232.3  0.9      46.4    -8    11050   00 09 28
00 13 55  ---          20 14 04  72.7 234.9  1.0      48.4   267    11187   00 09 21

00 14 10  J1925+211    20 14 19  75.8 231.0  0.8      45.8     1    11187   00 14 10
00 15 10  ---          20 15 19  75.6 231.7  0.8      46.4    60    11218   00 14 11

00 15 10 J191142+1952  20 15 19  72.3 236.4  1.0      49.7   -15    11218   00 15 25
00 16 35  ---          20 16 44  72.0 237.1  1.1      50.2    70    11254   00 15 11

00 16 35  J1923+2010   20 16 44  74.3 231.7  0.9      46.0   -12    11254   00 16 47
00 18 10  ---          20 18 19  74.0 232.6  0.9      46.8    83    11297   00 16 36

00 18 30 J191142+1952  20 18 39  71.7 238.0  1.1      50.9     8    11297   00 18 30
00 20 00  ---          20 20 10  71.4 238.7  1.1      51.5    90    11343   00 18 31

00 20 00  GRB221009A   20 20 10  71.6 237.9  1.1      50.8    -8    11343   00 20 08
00 24 35  ---          20 24 45  70.7 240.0  1.2      52.4   267    11481   00 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

00 24 50 J191142+1952  20 25 00  70.5 240.9  1.2      53.1     7    11481   00 24 50
00 26 15  ---          20 26 26  70.2 241.5  1.2      53.5    85    11525   00 24 51

00 26 15  GRB221009A   20 26 26  70.4 240.7  1.2      52.9    -8    11525   00 26 23
00 30 50  ---          20 31 01  69.6 242.6  1.3      54.3   267    11662   00 26 16

00 31 10 J191142+1952  20 31 21  69.3 243.4  1.3      54.9    12    11662   00 31 10
00 32 15  ---          20 32 27  69.1 243.8  1.3      55.2    65    11696   00 31 11

00 32 30  J1925+211    20 32 42  72.5 241.1  1.1      53.9     0    11696   00 32 30
00 33 30  ---          20 33 42  72.3 241.6  1.1      54.2    60    11727   00 32 31

00 33 30 J191249+1940  20 33 42  68.9 243.4  1.3      54.8   -15    11727   00 33 45
00 35 00  ---          20 35 12  68.6 244.0  1.4      55.2    75    11765   00 33 31

00 35 00 J191142+1952  20 35 12  68.5 244.9  1.4      55.9    -8    11765   00 35 08
00 36 30  ---          20 36 42  68.3 245.4  1.4      56.3    82    11808   00 35 01

00 36 30  GRB221009A   20 36 42  68.5 244.7  1.4      55.8    -8    11808   00 36 38
00 41 05  ---          20 41 18  67.6 246.3  1.5      56.9   267    11945   00 36 31

00 41 20 J191142+1952  20 41 33  67.3 247.0  1.5      57.4     7    11945   00 41 20
00 42 45  ---          20 42 58  67.0 247.5  1.5      57.7    85    11989   00 41 21

00 42 45  GRB221009A   20 42 58  67.2 246.9  1.5      57.2    -8    11989   00 42 53
00 47 20  ---          20 47 34  66.3 248.3  1.6      58.2   267    12127   00 42 46

00 47 35  J1925+211    20 47 49  69.6 247.2  1.3      58.3     1    12127   00 47 35
00 48 35  ---          20 48 49  69.4 247.5  1.4      58.5    60    12157   00 47 36

00 48 35 J191142+1952  20 48 49  65.8 249.3  1.6      58.9   -15    12157   00 48 50
00 50 00  ---          20 50 14  65.6 249.7  1.6      59.1    70    12194   00 48 36

00 50 00  GRB221009A   20 50 14  65.8 249.1  1.6      58.7    -8    12194   00 50 08
00 54 35  ---          20 54 50  64.9 250.5  1.7      59.5   267    12331   00 50 01

00 54 55 J191142+1952  20 55 10  64.6 251.1  1.7      60.0    12    12331   00 54 55
00 56 00  ---          20 56 15  64.3 251.4  1.7      60.2    65    12365   00 54 56

00 56 00  J1905+1943   20 56 15  63.0 252.7  1.8      60.8   -11    12365   00 56 11
00 57 45  ---          20 58 01  62.7 253.1  1.9      61.0    94    12413   00 56 01

00 57 45 J191142+1952  20 58 01  64.0 251.9  1.8      60.4   -11    12413   00 57 56
00 59 10  ---          20 59 26  63.7 252.2  1.8      60.6    74    12451   00 57 46
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

00 59 25  GRB221009A   20 59 41  63.9 251.8  1.8      60.3     7    12451   00 59 25
01 04 00  ---          21 04 17  62.9 253.0  1.8      61.0   275    12593   00 59 26

01 04 20 J191142+1952  21 04 37  62.6 253.6  1.9      61.4    12    12593   01 04 20
01 05 45  ---          21 06 02  62.3 253.9  1.9      61.6    85    12637   01 04 21

01 05 45  GRB221009A   21 06 02  62.6 253.4  1.9      61.2    -8    12637   01 05 53
01 10 20  ---          21 10 38  61.6 254.5  1.9      61.8   267    12774   01 05 46

01 10 35  J1925+211    21 10 53  64.9 254.1  1.7      62.5     1    12774   01 10 35
01 11 35  ---          21 11 53  64.7 254.3  1.7      62.7    60    12805   01 10 36

01 11 35 J191142+1952  21 11 53  61.1 255.3  2.0      62.3   -15    12805   01 11 50
01 13 00  ---          21 13 18  60.8 255.6  2.0      62.4    70    12841   01 11 36

01 13 00  J1923+2010   21 13 18  63.4 253.5  1.8      61.5   -13    12841   01 13 13
01 14 35  ---          21 14 53  63.0 253.9  1.8      61.7    82    12883   01 13 01

01 14 55 J191142+1952  21 15 14  60.4 256.0  2.0      62.6     7    12883   01 14 55
01 16 25  ---          21 16 44  60.1 256.3  2.1      62.8    90    12930   01 14 56

01 16 25  GRB221009A   21 16 44  60.3 255.9  2.0      62.5    -8    12930   01 16 33
01 21 00  ---          21 21 20  59.4 256.9  2.1      63.0   267    13067   01 16 26

01 21 15 J191142+1952  21 21 35  59.1 257.4  2.1      63.2     7    13067   01 21 15
01 22 40  ---          21 23 00  58.8 257.7  2.2      63.4    85    13111   01 21 16

01 22 40  GRB221009A   21 23 00  59.0 257.2  2.1      63.1    -8    13111   01 22 48
01 27 15  ---          21 27 36  58.1 258.1  2.2      63.5   267    13249   01 22 41

01 27 35 J191142+1952  21 27 56  57.8 258.6  2.3      63.8    12    13249   01 27 35
01 28 40  ---          21 29 01  57.5 258.8  2.3      63.9    65    13282   01 27 36

01 28 55  J1925+211    21 29 16  61.0 258.2  2.0      64.6     0    13282   01 28 55
01 29 55  ---          21 30 16  60.8 258.5  2.1      64.7    60    13313   01 28 56

01 29 55 J191249+1940  21 30 16  57.4 258.5  2.3      63.6   -15    13313   01 30 10
01 31 25  ---          21 31 46  57.1 258.8  2.3      63.7    75    13352   01 29 56

01 31 25 J191142+1952  21 31 46  56.9 259.4  2.3      64.1    -8    13352   01 31 33
01 32 55  ---          21 33 16  56.6 259.7  2.3      64.2    82    13394   01 31 26

01 32 55  GRB221009A   21 33 16  56.9 259.2  2.3      64.0    -8    13394   01 33 03
01 37 30  ---          21 37 52  55.9 260.1  2.4      64.3   267    13532   01 32 56
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

01 37 45 J191142+1952  21 38 07  55.6 260.5  2.4      64.5     7    13532   01 37 45
01 39 10  ---          21 39 33  55.3 260.8  2.4      64.6    85    13575   01 37 46

01 39 10  GRB221009A   21 39 33  55.5 260.4  2.4      64.4    -8    13575   01 39 18
01 43 45  ---          21 44 08  54.6 261.2  2.5      64.7   267    13713   01 39 11

01 44 00  J1925+211    21 44 23  57.8 261.2  2.3      65.7     1    13713   01 44 00
01 45 00  ---          21 45 23  57.6 261.3  2.3      65.8    60    13744   01 44 01

01 45 00 J191142+1952  21 45 23  54.1 261.8  2.5      64.9   -15    13744   01 45 15
01 46 25  ---          21 46 49  53.8 262.0  2.6      65.0    70    13780   01 45 01

01 46 25  GRB221009A   21 46 49  54.0 261.7  2.5      64.8    -8    13780   01 46 33
01 51 00  ---          21 51 24  53.0 262.4  2.6      65.0   267    13918   01 46 26

01 51 20 J191142+1952  21 51 45  52.7 262.9  2.7      65.2    12    13918   01 51 20
01 52 25  ---          21 52 50  52.5 263.0  2.7      65.3    65    13951   01 51 21

01 52 25  J1905+1943   21 52 50  51.1 263.8  2.8      65.3   -11    13951   01 52 36
01 54 10  ---          21 54 35  50.7 264.1  2.8      65.4    94    14000   01 52 26

01 54 10 J191142+1952  21 54 35  52.1 263.3  2.7      65.4   -11    14000   01 54 21
01 55 35  ---          21 56 00  51.8 263.5  2.7      65.4    74    14038   01 54 11

01 55 50  GRB221009A   21 56 15  52.0 263.2  2.7      65.3     7    14038   01 55 50
02 00 25  ---          22 00 51  51.0 264.0  2.8      65.4   275    14179   01 55 51

02 00 45 J191142+1952  22 01 11  50.7 264.3  2.8      65.6    12    14179   02 00 45
02 02 10  ---          22 02 36  50.4 264.6  2.8      65.6    85    14223   02 00 46

02 02 10  GRB221009A   22 02 36  50.6 264.2  2.8      65.5    -8    14223   02 02 18
02 06 45  ---          22 07 12  49.6 264.9  2.9      65.6   267    14361   02 02 11

02 07 00  J1925+211    22 07 27  52.9 265.0  2.7      66.8     1    14361   02 07 00
02 08 00  ---          22 08 27  52.7 265.1  2.7      66.8    60    14392   02 07 01

02 08 00 J191142+1952  22 08 27  49.1 265.4  2.9      65.8   -15    14392   02 08 15
02 09 25  ---          22 09 52  48.8 265.6  3.0      65.9    70    14428   02 08 01

02 09 25  J1923+2010   22 09 52  51.4 264.4  2.8      65.9   -13    14428   02 09 38
02 11 00  ---          22 11 28  51.1 264.6  2.8      65.9    82    14470   02 09 26

02 11 20 J191142+1952  22 11 48  48.4 265.9  3.0      65.9     7    14470   02 11 20
02 12 50  ---          22 13 18  48.1 266.1  3.0      65.9    90    14516   02 11 21
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

02 12 50  GRB221009A   22 13 18  48.3 265.8  3.0      65.8    -8    14516   02 12 58
02 17 25  ---          22 17 54  47.4 266.5  3.1      65.9   267    14654   02 12 51

02 17 40 J191142+1952  22 18 09  47.0 266.8  3.1      66.0     7    14654   02 17 40
02 19 05  ---          22 19 34  46.7 267.0  3.1      66.0    85    14698   02 17 41

02 19 05  GRB221009A   22 19 34  47.0 266.7  3.1      65.9    -8    14698   02 19 13
02 23 40  ---          22 24 10  46.0 267.4  3.2      66.0   267    14835   02 19 06

02 24 00 J191142+1952  22 24 30  45.7 267.7  3.2      66.1    12    14835   02 24 00
02 25 05  ---          22 25 35  45.4 267.9  3.2      66.1    65    14869   02 24 01

02 25 20  J1925+211    22 25 50  49.0 267.6  3.0      67.2     0    14869   02 25 20
02 26 20  ---          22 26 50  48.7 267.8  3.0      67.2    60    14900   02 25 21

02 26 20 J191249+1940  22 26 50  45.3 267.6  3.2      65.9   -15    14900   02 26 35
02 27 50  ---          22 28 21  45.0 267.8  3.2      66.0    75    14938   02 26 21

02 27 50 J191142+1952  22 28 21  44.9 268.2  3.3      66.2    -8    14938   02 27 58
02 29 20  ---          22 29 51  44.5 268.4  3.3      66.2    82    14981   02 27 51

02 29 20  GRB221009A   22 29 51  44.8 268.1  3.3      66.1    -8    14981   02 29 28
02 33 55  ---          22 34 27  43.8 268.7  3.3      66.1   267    15118   02 29 21

02 34 10 J191142+1952  22 34 42  43.5 269.1  3.4      66.2     7    15118   02 34 10
02 35 35  ---          22 36 07  43.2 269.3  3.4      66.2    85    15162   02 34 11

02 35 35  GRB221009A   22 36 07  43.4 269.0  3.4      66.1    -8    15162   02 35 43
02 40 10  ---          22 40 43  42.4 269.6  3.4      66.1   267    15300   02 35 36

02 40 25  J1925+211    22 40 58  45.7 269.6  3.2      67.3     1    15300   02 40 25
02 41 25  ---          22 41 58  45.5 269.8  3.2      67.3    60    15331   02 40 26

02 41 25  GRB221009A   22 41 58  42.2 269.7  3.5      66.1   -15    15331   02 41 40
02 46 00  ---          22 46 33  41.2 270.3  3.5      66.1   260    15465   02 41 26

02 46 20 J191142+1952  22 46 54  40.9 270.6  3.6      66.2    12    15465   02 46 20
02 47 25  ---          22 47 59  40.6 270.8  3.6      66.2    65    15498   02 46 21

02 47 25  J1905+1943   22 47 59  39.3 271.3  3.7      66.1   -11    15498   02 47 36
02 49 10  ---          22 49 44  38.9 271.6  3.7      66.1    94    15546   02 47 26

02 49 10 J191142+1952  22 49 44  40.3 271.0  3.6      66.2   -11    15546   02 49 21
02 50 35  ---          22 51 09  39.9 271.2  3.6      66.2    74    15585   02 49 11
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

02 50 50  J1925+211    22 51 24  43.5 271.0  3.4      67.3     0    15585   02 50 50
02 51 50  ---          22 52 24  43.2 271.1  3.4      67.3    60    15615   02 50 51

02 51 50  GRB221009A   22 52 24  39.9 271.0  3.6      66.1   -15    15615   02 52 05
02 56 25  ---          22 57 00  38.9 271.6  3.7      66.1   260    15749   02 51 51

02 56 45 J191142+1952  22 57 20  38.6 271.9  3.7      66.2    12    15749   02 56 45
02 58 10  ---          22 58 45  38.3 272.1  3.8      66.1    85    15793   02 56 46

02 58 10  GRB221009A   22 58 45  38.6 271.8  3.7      66.1    -8    15793   02 58 18
03 02 45  ---          23 03 21  37.6 272.4  3.8      66.0   267    15931   02 58 11

03 03 00 J191142+1952  23 03 36  37.3 272.7  3.8      66.1     7    15931   03 03 00
03 04 25  ---          23 05 02  37.0 272.8  3.9      66.1    85    15975   03 03 01

03 04 25  J1923+2010   23 05 02  39.6 271.8  3.7      66.4   -13    15975   03 04 38
03 06 00  ---          23 06 37  39.2 272.0  3.7      66.4    82    16017   03 04 26

03 06 20 J191142+1952  23 06 57  36.6 273.1  3.9      66.0     7    16017   03 06 20
03 07 50  ---          23 08 27  36.2 273.3  3.9      66.0    90    16063   03 06 21

03 07 50  GRB221009A   23 08 27  36.5 273.0  3.9      66.0    -8    16063   03 07 58
03 12 25  ---          23 13 03  35.5 273.5  4.0      65.9   267    16201   03 07 51

03 12 40  J1925+211    23 13 18  38.8 273.6  3.8      67.0     1    16201   03 12 40
03 13 40  ---          23 14 18  38.5 273.7  3.8      67.0    60    16232   03 12 41

03 13 40 J191142+1952  23 14 18  35.0 273.9  4.0      65.9   -15    16232   03 13 55
03 15 05  ---          23 15 43  34.7 274.1  4.0      65.9    70    16268   03 13 41

03 15 05  GRB221009A   23 15 43  34.9 273.8  4.0      65.9    -8    16268   03 15 13
03 19 40  ---          23 20 19  33.9 274.4  4.1      65.8   267    16405   03 15 06

03 20 00 J191142+1952  23 20 39  33.6 274.7  4.1      65.8    12    16405   03 20 00
03 21 05  ---          23 21 44  33.4 274.8  4.2      65.8    65    16439   03 20 01

03 21 20 J191249+1940  23 21 59  33.5 274.5  4.1      65.7     7    16439   03 21 20
03 22 50  ---          23 23 30  33.2 274.7  4.2      65.6    90    16485   03 21 21

03 22 50 J191142+1952  23 23 30  33.0 275.0  4.2      65.7    -8    16485   03 22 58
03 24 20  ---          23 25 00  32.7 275.2  4.2      65.7    82    16528   03 22 51

03 24 40 J191142+1952  23 25 20  32.6 275.2  4.2      65.7    14    16528   03 24 40
03 26 10  ---          23 26 50  32.3 275.4  4.2      65.7    90    16574   03 24 41
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

03 26 10  GRB221009A   23 26 50  32.5 275.1  4.2      65.6    -8    16574   03 26 18
03 30 45  ---          23 31 26  31.6 275.7  4.3      65.5   267    16711   03 26 11

03 31 00  J1925+211    23 31 41  34.8 275.7  4.1      66.6     1    16711   03 31 00
03 32 00  ---          23 32 41  34.6 275.8  4.1      66.6    60    16742   03 31 01

03 32 00 J191142+1952  23 32 41  31.0 276.1  4.3      65.5   -15    16742   03 32 15
03 33 25  ---          23 34 06  30.7 276.2  4.4      65.5    70    16778   03 32 01

03 33 25  GRB221009A   23 34 06  31.0 276.0  4.3      65.5    -8    16778   03 33 33
03 38 00  ---          23 38 42  30.0 276.5  4.4      65.3   267    16916   03 33 26

03 38 20 J191142+1952  23 39 02  29.7 276.8  4.4      65.3    12    16916   03 38 20
03 39 25  ---          23 40 07  29.4 276.9  4.5      65.3    65    16950   03 38 21

03 39 25  J1905+1943   23 40 07  28.1 277.4  4.6      65.0   -11    16950   03 39 36
03 41 10  ---          23 41 53  27.7 277.6  4.6      65.0    94    16998   03 39 26

03 41 10 J191142+1952  23 41 53  29.1 277.1  4.5      65.2   -11    16998   03 41 21
03 42 35  ---          23 43 18  28.8 277.3  4.5      65.2    74    17036   03 41 11

03 42 50  GRB221009A   23 43 33  29.0 277.0  4.5      65.2     7    17036   03 42 50
03 47 25  ---          23 48 09  28.0 277.6  4.6      65.0   275    17178   03 42 51

03 47 45 J191142+1952  23 48 29  27.7 277.8  4.6      65.0    12    17178   03 47 45
03 49 10  ---          23 49 54  27.4 278.0  4.6      65.0    85    17222   03 47 46

03 49 10  GRB221009A   23 49 54  27.6 277.8  4.6      65.0    -8    17222   03 49 18
03 53 45  ---          23 54 30  26.6 278.3  4.7      64.8   267    17359   03 49 11

03 54 00  J1925+211    23 54 45  29.9 278.2  4.5      65.9     1    17359   03 54 00
03 55 00  ---          23 55 45  29.7 278.4  4.5      65.9    60    17390   03 54 01

03 55 00 J191142+1952  23 55 45  26.1 278.7  4.7      64.8   -15    17390   03 55 15
03 56 25  ---          23 57 10  25.8 278.8  4.7      64.7    70    17426   03 55 01

03 56 25  J1923+2010   23 57 10  28.4 277.9  4.5      65.3   -13    17426   03 56 38
03 58 00  ---          23 58 45  28.1 278.0  4.6      65.2    82    17468   03 56 26

03 58 20 J191142+1952  23 59 05  25.4 279.0  4.8      64.7     7    17468   03 58 20
03 59 50  ---          00 00 36  25.1 279.2  4.8      64.6    90    17515   03 58 21

03 59 50  GRB221009A   00 00 36  25.3 278.9  4.8      64.6    -8    17515   03 59 58
04 04 25  ---          00 05 11  24.4 279.5  4.9      64.4   267    17652   03 59 51
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

04 04 40 J191142+1952  00 05 26  24.1 279.7  4.9      64.4     7    17652   04 04 40
04 06 05  ---          00 06 52  23.8 279.9  4.9      64.4    85    17696   04 04 41

04 06 05  GRB221009A   00 06 52  24.0 279.6  4.9      64.4    -8    17696   04 06 13
04 10 40  ---          00 11 27  23.0 280.2  5.0      64.2   267    17834   04 06 06

04 11 00 J191142+1952  00 11 47  22.7 280.4  5.0      64.2    12    17834   04 11 00
04 12 05  ---          00 12 53  22.5 280.6  5.0      64.1    65    17867   04 11 01

04 12 20  J1925+211    00 13 08  26.0 280.3  4.8      65.2     0    17867   04 12 20
04 13 20  ---          00 14 08  25.8 280.4  4.8      65.2    60    17898   04 12 21

04 13 20 J191249+1940  00 14 08  22.4 280.4  5.0      64.0   -15    17898   04 13 35
04 14 50  ---          00 15 38  22.0 280.5  5.0      64.0    75    17937   04 13 21

04 14 50 J191142+1952  00 15 38  21.9 280.9  5.0      64.0    -8    17937   04 14 58
04 16 20  ---          00 17 08  21.6 281.0  5.1      63.9    82    17979   04 14 51

04 16 20  GRB221009A   00 17 08  21.8 280.8  5.1      64.0    -8    17979   04 16 28
04 20 55  ---          00 21 44  20.9 281.3  5.1      63.7   267    18117   04 16 21

04 21 10  J1925+211    00 21 59  24.1 281.2  4.9      64.8     1    18117   04 21 10
04 22 10  ---          00 22 59  23.9 281.3  4.9      64.8    60    18148   04 21 11

04 22 10 J191142+1952  00 22 59  20.3 281.7  5.2      63.7   -15    18148   04 22 25
04 23 35  ---          00 24 25  20.0 281.8  5.2      63.6    70    18184   04 22 11

04 23 35  GRB221009A   00 24 25  20.3 281.6  5.2      63.6    -8    18184   04 23 43
04 28 10  ---          00 29 00  19.3 282.1  5.2      63.4   267    18321   04 23 36

04 28 30 J191142+1952  00 29 20  19.0 282.4  5.3      63.4    12    18321   04 28 30
04 29 35  ---          00 30 26  18.8 282.5  5.3      63.3    65    18355   04 28 31

04 29 35  J1905+1943   00 30 26  17.4 283.0  5.4      63.0   -11    18355   04 29 46
04 31 20  ---          00 32 11  17.1 283.2  5.4      62.9    94    18403   04 29 36

04 31 20 J191142+1952  00 32 11  18.4 282.7  5.3      63.2   -11    18403   04 31 31
04 32 45  ---          00 33 36  18.1 282.9  5.3      63.1    74    18441   04 31 21

04 33 00  GRB221009A   00 33 51  18.3 282.7  5.3      63.2     7    18441   04 33 00
04 37 35  ---          00 38 27  17.3 283.2  5.4      62.9   275    18583   04 33 01

04 37 55 J191142+1952  00 38 47  17.0 283.4  5.4      62.9    12    18583   04 37 55
04 39 20  ---          00 40 12  16.7 283.6  5.5      62.8    85    18627   04 37 56
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

04 39 20  GRB221009A   00 40 12  17.0 283.4  5.4      62.9    -8    18627   04 39 28
04 43 55  ---          00 44 48  16.0 283.9  5.5      62.6   267    18764   04 39 21

04 44 10  J1925+211    00 45 03  19.3 283.7  5.3      63.7     1    18764   04 44 10
04 45 10  ---          00 46 03  19.1 283.8  5.3      63.6    60    18795   04 44 11

04 45 10 J191142+1952  00 46 03  15.5 284.3  5.6      62.5   -15    18795   04 45 25
04 46 35  ---          00 47 28  15.2 284.4  5.6      62.4    70    18831   04 45 11

04 46 35  J1923+2010   00 47 28  17.8 283.4  5.4      63.1   -13    18831   04 46 48
04 48 10  ---          00 49 04  17.4 283.6  5.4      63.0    82    18874   04 46 36

04 48 30 J191142+1952  00 49 24  14.8 284.6  5.6      62.3     7    18874   04 48 30
04 50 00  ---          00 50 54  14.5 284.8  5.6      62.2    90    18920   04 48 31

04 50 00  GRB221009A   00 50 54  14.7 284.6  5.6      62.3    -8    18920   04 50 08
04 54 35  ---          00 55 30  13.8 285.1  5.7      62.0   267    19058   04 50 01

04 54 50 J191142+1952  00 55 45  13.5 285.4  5.7      61.9     7    19058   04 54 50
04 56 15  ---          00 57 10  13.2 285.5  5.7      61.9    85    19101   04 54 51

04 56 15  GRB221009A   00 57 10  13.4 285.3  5.7      61.9    -8    19101   04 56 23
05 00 50  ---          01 01 46  12.5 285.8  5.8      61.6   267    19239   04 56 16

05 01 10 J191142+1952  01 02 06  12.2 286.1  5.8      61.6    12    19239   05 01 10
05 02 15  ---          01 03 11  12.0 286.2  5.8      61.5    65    19272   05 01 11

05 02 30  J1925+211    01 03 26  15.4 285.8  5.6      62.6     0    19272   05 02 30
05 03 30  ---          01 04 26  15.2 285.9  5.6      62.6    60    19303   05 02 31

05 03 30 J191249+1940  01 04 26  11.8 286.0  5.8      61.4   -15    19303   05 03 45
05 05 00  ---          01 05 56  11.5 286.2  5.9      61.4    75    19342   05 03 31

05 05 00 J191142+1952  01 05 56  11.4 286.5  5.9      61.3    -7    19342   05 05 07
05 06 30  ---          01 07 27  11.1 286.7  5.9      61.2    83    19385   05 05 01

05 06 30  GRB221009A   01 07 27  11.3 286.5  5.9      61.3    -8    19385   05 06 38
05 11 05  ---          01 12 02  10.4 287.0  6.0      61.0   267    19522   05 06 31

05 11 25 J191142+1952  01 12 22  10.1 287.3  6.0      60.9    12    19522   05 11 25
05 12 30  ---          01 13 28   9.8 287.4  6.0      60.8    65    19556   05 11 26

05 12 30  GRB221009A   01 13 28  10.1 287.2  6.0      60.9    -8    19556   05 12 38
05 17 05  ---          01 18 03   9.1 287.7  6.1      60.6   267    19693   05 12 31
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GG087B
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   5 Nov 2023   Day 309 ---

05 26 45  J1925+2106   01 27 45  10.4 288.5  6.0      61.0   566    19693   05 26 45
05 30 00  =1923+210    01 31 00   9.8 288.9  6.1      60.8   195    19794   05 26 46


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess323.C4096glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    7         Station: VLBA_FD           Total bit rate:  4096
   Format: VDIF              Bits per sample: 2         Sample rate:256.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  23  Setup file default.  Used with PCAL = off
   LO sum=   4612.00  4612.00  4740.00  4740.00  4868.00  4868.00  4996.00  4996.00
   BBC fr=    512.00   512.00   640.00   640.00   768.00   768.00   896.00   896.00
   Bandwd=    128.00   128.00   128.00   128.00   128.00   128.00   128.00   128.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     696.00    696.00    824.00    824.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  23  24  25  26  27  28  30  31  32  33

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * GRB221009A        19 10 52.500472   * 19 13 03.500400     19 14 04.828699       0.00
                     19 41 14.67648    * 19 46 24.22800      19 48 57.77799        0.00
                     From catalog imbedded in main SCHED input file.

 * J1905+1943        19 03 25.637172   * 19 05 36.472100     19 06 37.689322       0.00
                     19 38 29.62717    * 19 43 08.04500      19 45 26.68135        0.00
                     From catalog imbedded in main SCHED input file.

 * J1923+2010        19 21 02.282278   * 19 23 13.140228     19 24 14.445339       0.00
                     20 04 48.26646    * 20 10 39.75566      20 13 33.47311        0.00
                     From catalog imbedded in main SCHED input file.

 * J191142+1952      19 09 31.671206   * 19 11 42.510000     19 12 43.755250       0.00
                     19 46 56.06136    * 19 52 00.00000      19 54 30.88422        0.00
                     From catalog imbedded in main SCHED input file.

 * J191249+1940      19 10 38.054579   * 19 12 49.180000     19 13 50.567375       0.00
                     19 34 51.84540    * 19 40 00.40000      19 42 33.44890        0.00
                     From catalog imbedded in main SCHED input file.

 * J1925+211         19 23 49.792407   * 19 25 59.605370     19 27 00.422056       0.00
                     21 00 23.30510    * 21 06 26.16218      21 09 25.53566        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C286             13 28 49.657692   * 13 31 08.287984     13 32 12.744473       0.00
                     30 45 58.64021    * 30 30 32.95885      30 23 14.12633        0.00
                     From catalog imbedded in main SCHED input file.

   1923+210          19 23 49.792392   * 19 25 59.605356     19 27 00.422042       0.01
 * J1925+2106        21 00 23.30493    * 21 06 26.16201      21 09 25.53549        0.00
   J1925+21          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  38704 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  GRB221009A sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +    13.554  1442.278
  J1905+1943 sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +     0.875    83.268
  J1923+2010 sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +     0.713    57.507
  J191142+195sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +     5.656   618.213
  J191249+194sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +     0.675    67.624
  J1925+211  sess323.C4096glob     8 9 10 11 12 13 14 19 20 21 +     0.567    65.370
  3C286      sess323.C4096glob     13 14 29                          0.225     1.051
  J1925+2106 sess323.C4096glob     1 2 3 6 7 8 9 10 11 12 13 1 +     0.362    67.655


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   GRB221009A          76.4
   J1905+1943          74.7
   J1923+2010          78.7
   J191142+1952        76.1
   J191249+1940        76.3
   J1925+211           79.7
   3C286               48.5
   J1925+2106          79.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

