  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Mkn 273 GLOBAL 6cm
 Exp. Code:  GB055A  


Schedule Version:       2.00                                              
Processed by SCHED version:   6.02  July 2005                             

PI:       M. Bondi                                                        

Address:  Istituto di Radioastronomia                                     
          Via Gobetti 101, I-40129 Bologna                                
          Italy                                                           
                                                                          

Phone:    39-051-639 9386                                                 
EMAIL:    bondi@ira.inaf.it                                               
Fax:      39-051-639 9431                                                 
Phone during observation: 39-051-639 9386                                 

Observing mode: 256Mbps                                                   

Notes:    Phase referencing                                               
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

 Next scan frequencies:  4974.49  4974.49  4982.49  4982.49  4990.49  4990.49
                         4998.49  4998.49
 Next BBC frequencies:    874.49   874.49   882.49   882.49   890.49   890.49
                          898.49   898.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

13 11 00  J1337+550    08 15 33  29.9  40.7 -5.4     -78.2     0   1  1      0  13 11 00
13 13 00  ---          08 17 33  30.1  40.8 -5.3     -78.6   120   F  1      0  13 11 10

13 13 00  MKN273       08 17 33  29.4  39.6 -5.5     -77.8    -8   1  1      0  13 13 00
13 16 00  ---          08 20 34  29.8  39.7 -5.4     -78.3   172   F  1      0  13 13 10

13 16 00  J1337+550    08 20 34  30.6  40.9 -5.3     -79.1    -8   1  1      0  13 16 00
13 18 00  ---          08 22 34  30.8  41.0 -5.3     -79.5   112   F  1      0  13 16 10

13 18 00  MKN273       08 22 34  30.1  39.8 -5.4     -78.7    -8   1  1      0  13 18 00
13 21 00  ---          08 25 34  30.5  39.9 -5.3     -79.3   172   F  1      0  13 18 10

13 21 00  J1337+550    08 25 34  31.3  41.1 -5.2     -80.1    -8   1  1      0  13 21 00
13 23 00  ---          08 27 35  31.6  41.1 -5.2     -80.5   112   F  1      0  13 21 10

13 23 00  MKN273       08 27 35  30.7  39.9 -5.3     -79.7    -8   1  1      0  13 23 00
13 26 00  ---          08 30 35  31.2  40.0 -5.2     -80.2   172   F  1      0  13 23 10

13 26 00  J1337+550    08 30 35  32.0  41.2 -5.1     -81.0    -8   1  1      0  13 26 00
13 28 00  ---          08 32 36  32.3  41.3 -5.1     -81.4   112   F  1      0  13 26 10

13 28 00  MKN273       08 32 36  31.4  40.1 -5.2     -80.6    -8   1  1      0  13 28 00
13 31 00  ---          08 35 36  31.9  40.1 -5.2     -81.2   172   F  1      0  13 28 10

13 31 00  J1337+550    08 35 36  32.7  41.3 -5.0     -82.0    -8   1  1      0  13 31 00
13 33 00  ---          08 37 36  33.0  41.4 -5.0     -82.4   112   F  1      0  13 31 10

13 34 00  J1337+550    08 38 37  33.1  41.4 -5.0     -82.6    54   1  1      0  13 34 00
13 36 00  ---          08 40 37  33.4  41.4 -5.0     -83.0   120   F  1      0  13 34 10

13 36 00  MKN273       08 40 37  32.5  40.3 -5.1     -82.2    -8   1  1      0  13 36 00
13 39 00  ---          08 43 37  33.0  40.3 -5.0     -82.8   172   F  1      0  13 36 10

13 39 00  J1337+550    08 43 37  33.8  41.5 -4.9     -83.5    -8   1  1      0  13 39 00
13 41 00  ---          08 45 38  34.1  41.5 -4.9     -83.9   112   F  1      0  13 39 10
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

13 41 00  MKN273       08 45 38  33.2  40.4 -5.0     -83.2    -8   1  1      0  13 41 00
13 44 00  ---          08 48 38  33.7  40.4 -4.9     -83.8   172   F  1      0  13 41 10

13 44 00  J1337+550    08 48 38  34.5  41.6 -4.8     -84.5    -8   1  1      0  13 44 00
13 46 00  ---          08 50 39  34.8  41.6 -4.8     -84.9   112   F  1      0  13 44 10

13 46 00  MKN273       08 50 39  33.9  40.5 -4.9     -84.2    -8   1  1      0  13 46 00
13 49 00  ---          08 53 39  34.4  40.5 -4.9     -84.8   172   F  1      0  13 46 10

13 49 00  J1337+550    08 53 39  35.3  41.7 -4.7     -85.5    -8   1  1      0  13 49 00
13 51 00  ---          08 55 39  35.5  41.7 -4.7     -85.9   112   F  1      0  13 49 10

13 51 00  MKN273       08 55 39  34.6  40.5 -4.8     -85.1    -8   1  1      0  13 51 00
13 54 00  ---          08 58 40  35.1  40.6 -4.8     -85.7   172   F  1      0  13 51 10

13 54 00  J1337+550    08 58 40  36.0  41.7 -4.7     -86.5    -8   1  1      0  13 54 00
13 56 00  ---          09 00 40  36.3  41.7 -4.6     -86.9   112   F  1      0  13 54 10

13 57 00  J1337+550    09 01 40  36.4  41.8 -4.6     -87.1    54   1  1      0  13 57 00
13 59 00  ---          09 03 41  36.7  41.8 -4.6     -87.5   120   F  1      0  13 57 10

13 59 00  MKN273       09 03 41  35.8  40.6 -4.7     -86.8    -8   1  1      0  13 59 00
14 02 00  ---          09 06 41  36.2  40.7 -4.6     -87.4   172   F  1      0  13 59 10

14 02 00  J1337+550    09 06 41  37.1  41.8 -4.5     -88.1    -8   1  1      0  14 02 00
14 04 00  ---          09 08 42  37.4  41.8 -4.5     -88.5   112   F  1      0  14 02 10

14 04 00  MKN273       09 08 42  36.5  40.7 -4.6     -87.8    -8   1  1      0  14 04 00
14 07 00  ---          09 11 42  36.9  40.7 -4.6     -88.4   172   F  1      0  14 04 10

14 07 00  J1337+550    09 11 42  37.8  41.8 -4.4     -89.1    -8   1  1      0  14 07 00
14 09 00  ---          09 13 42  38.1  41.8 -4.4     -89.5   112   F  1      0  14 07 10

14 09 00  MKN273       09 13 42  37.2  40.7 -4.5     -88.8    -8   1  1      0  14 09 00
14 12 00  ---          09 16 43  37.6  40.7 -4.5     -89.4   172   F  1      0  14 09 10

14 12 00  J1337+550    09 16 43  38.6  41.8 -4.4     -90.1    -8   1  1      0  14 12 00
14 14 00  ---          09 18 43  38.9  41.8 -4.3     -90.5   112   F  1      0  14 12 10

14 14 00  MKN273       09 18 43  37.9  40.7 -4.4     -89.8    -8   1  1      0  14 14 00
14 17 00  ---          09 21 44  38.3  40.7 -4.4     -90.4   172   F  1      0  14 14 10

14 17 00  J1337+550    09 21 44  39.3  41.8 -4.3     -91.2    -8   1  1      0  14 17 00
14 19 00  ---          09 23 44  39.6  41.8 -4.2     -91.6   112   F  1      0  14 17 10
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

14 20 00  J1337+550    09 24 44  39.7  41.8 -4.2     -91.8    54   1  1      0  14 20 00
14 22 00  ---          09 26 44  40.0  41.8 -4.2     -92.2   120   F  1      0  14 20 10

14 22 00  MKN273       09 26 44  39.0  40.7 -4.3     -91.5    -8   1  1      0  14 22 00
14 25 00  ---          09 29 45  39.4  40.7 -4.3     -92.1   172   F  1      0  14 22 10

14 25 00  J1337+550    09 29 45  40.4  41.8 -4.1     -92.8    -8   1  1      0  14 25 00
14 27 00  ---          09 31 45  40.7  41.7 -4.1     -93.3   112   F  1      0  14 25 10

14 27 00  MKN273       09 31 45  39.7  40.7 -4.2     -92.5    -8   1  1      0  14 27 00
14 30 00  ---          09 34 46  40.1  40.6 -4.2     -93.2   172   F  1      0  14 27 10

14 30 00  J1337+550    09 34 46  41.2  41.7 -4.1     -93.9    -8   1  1      0  14 30 00
14 32 00  ---          09 36 46  41.4  41.7 -4.0     -94.3   112   F  1      0  14 30 10

14 32 00  MKN273       09 36 46  40.4  40.6 -4.1     -93.6    -8   1  1      0  14 32 00
14 35 00  ---          09 39 47  40.8  40.6 -4.1     -94.3   172   F  1      0  14 32 10

14 35 00  J1337+550    09 39 47  41.9  41.6 -4.0     -95.0    -8   1  1      0  14 35 00
14 37 00  ---          09 41 47  42.2  41.6 -3.9     -95.4   112   F  1      0  14 35 10

14 37 00  MKN273       09 41 47  41.1  40.5 -4.1     -94.7    -8   1  1      0  14 37 00
14 40 00  ---          09 44 47  41.5  40.5 -4.0     -95.4   172   F  1      0  14 37 10

14 40 00  J1337+550    09 44 47  42.6  41.5 -3.9     -96.1    -8   1  1      0  14 40 00
14 42 00  ---          09 46 48  42.9  41.5 -3.9     -96.5   112   F  1      0  14 40 10

14 43 00  J1337+550    09 47 48  43.0  41.5 -3.8     -96.7    54   1  1      0  14 43 00
14 45 00  ---          09 49 48  43.3  41.4 -3.8     -97.2   120   F  1      0  14 43 10

14 45 00  MKN273       09 49 48  42.2  40.4 -3.9     -96.5    -8   1  1      0  14 45 00
14 48 00  ---          09 52 49  42.6  40.3 -3.9     -97.1   172   F  1      0  14 45 10

14 48 00  J1337+550    09 52 49  43.7  41.3 -3.8     -97.8    -8   1  1      0  14 48 00
14 50 00  ---          09 54 49  44.0  41.3 -3.7     -98.3   112   F  1      0  14 48 10

14 50 00  MKN273       09 54 49  42.9  40.3 -3.8     -97.6    -8   1  1      0  14 50 00
14 53 00  ---          09 57 50  43.3  40.2 -3.8     -98.2   172   F  1      0  14 50 10

14 53 00  J1337+550    09 57 50  44.4  41.2 -3.7     -99.0    -8   1  1      0  14 53 00
14 55 00  ---          09 59 50  44.7  41.1 -3.6     -99.4   112   F  1      0  14 53 10

14 55 00  MKN273       09 59 50  43.6  40.1 -3.8     -98.7    -8   1  1      0  14 55 00
14 58 00  ---          10 02 50  44.0  40.1 -3.7     -99.4   172   F  1      0  14 55 10
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

14 58 00  J1337+550    10 02 50  45.1  41.0 -3.6    -100.1    -8   1  1      0  14 58 00
15 00 00  ---          10 04 51  45.4  41.0 -3.6    -100.6   112   F  1      0  14 58 10

15 00 00  MKN273       10 04 51  44.3  40.0 -3.7     -99.8    -8   1  1      0  15 00 00
15 03 00  ---          10 07 51  44.7  39.9 -3.6    -100.5   172   F  1      0  15 00 10

15 03 00  J1337+550    10 07 51  45.9  40.8 -3.5    -101.3    -8   1  1      0  15 03 00
15 05 00  ---          10 09 52  46.1  40.8 -3.5    -101.8   112   F  1      0  15 03 10

15 06 00  J1337+550    10 10 52  46.3  40.7 -3.5    -102.0    54   1  1      0  15 06 00
15 08 00  ---          10 12 52  46.6  40.6 -3.4    -102.5   120   F  1      0  15 06 10

15 08 00  MKN273       10 12 52  45.4  39.7 -3.5    -101.7    -8   1  1      0  15 08 00
15 11 00  ---          10 15 53  45.8  39.6 -3.5    -102.4   172   F  1      0  15 08 10

15 11 00  J1337+550    10 15 53  47.0  40.5 -3.4    -103.2    -8   1  1      0  15 11 00
15 13 00  ---          10 17 53  47.3  40.4 -3.3    -103.7   112   F  1      0  15 11 10

15 13 00  MKN273       10 17 53  46.1  39.5 -3.5    -102.9    -8   1  1      0  15 13 00
15 16 00  ---          10 20 53  46.5  39.3 -3.4    -103.6   172   F  1      0  15 13 10

15 16 00  J1337+550    10 20 53  47.7  40.2 -3.3    -104.4    -8   1  1      0  15 16 00
15 18 00  ---          10 22 54  48.0  40.1 -3.3    -104.9   112   F  1      0  15 16 10

15 18 00  MKN273       10 22 54  46.8  39.2 -3.4    -104.1    -8   1  1      0  15 18 00
15 21 00  ---          10 25 54  47.2  39.1 -3.3    -104.9   172   F  1      0  15 18 10

15 21 00  J1337+550    10 25 54  48.4  40.0 -3.2    -105.6    -8   1  1      0  15 21 00
15 23 00  ---          10 27 55  48.7  39.8 -3.2    -106.1   112   F  1      0  15 21 10

15 23 00  MKN273       10 27 55  47.5  39.0 -3.3    -105.3    -8   1  1      0  15 23 00
15 26 00  ---          10 30 55  47.9  38.8 -3.2    -106.1   172   F  1      0  15 23 10

15 26 00  J1337+550    10 30 55  49.1  39.6 -3.1    -106.9    -8   1  1      0  15 26 00
15 28 00  ---          10 32 55  49.3  39.5 -3.1    -107.4   112   F  1      0  15 26 10

15 29 00  J1337+550    10 33 56  49.5  39.5 -3.1    -107.6    55   1  1      0  15 29 00
15 31 00  ---          10 35 56  49.7  39.3 -3.0    -108.2   120   F  1      0  15 29 10

15 31 00  MKN273       10 35 56  48.6  38.5 -3.1    -107.4    -8   1  1      0  15 31 00
15 34 00  ---          10 38 56  49.0  38.3 -3.1    -108.1   172   F  1      0  15 31 10

15 34 00  J1337+550    10 38 56  50.2  39.1 -3.0    -108.9    -8   1  1      0  15 34 00
15 36 00  ---          10 40 57  50.4  39.0 -3.0    -109.5   112   F  1      0  15 34 10
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

15 36 00  MKN273       10 40 57  49.2  38.2 -3.1    -108.6    -8   1  1      0  15 36 00
15 39 00  ---          10 43 57  49.6  38.0 -3.0    -109.4   172   F  1      0  15 36 10

15 44 00  3C345        10 48 58  20.1  54.8 -5.9     -66.3   235   1  1      0  15 44 00
15 56 00  ---          11 01 00  22.2  55.8 -5.7     -67.9   720   F  1      0  15 44 10

16 01 00  J1337+550    11 06 01  53.7  36.7 -2.5    -116.4   231   1  1      0  16 01 00
16 03 00  ---          11 08 01  54.0  36.5 -2.5    -117.0   120   F  1      0  16 01 10

16 03 00  MKN273       11 08 01  52.7  35.9 -2.6    -116.0    -9   1  1      0  16 03 00
16 06 00  ---          11 11 02  53.1  35.6 -2.6    -116.9   171   F  1      0  16 03 10

16 06 00  J1337+550    11 11 02  54.4  36.1 -2.4    -117.9    -9   1  1      0  16 06 00
16 08 00  ---          11 13 02  54.6  35.9 -2.4    -118.5   111   F  1      0  16 06 10

16 08 00  MKN273       11 13 02  53.4  35.4 -2.5    -117.5    -9   1  1      0  16 08 00
16 11 00  ---          11 16 02  53.7  35.0 -2.5    -118.4   171   F  1      0  16 08 10

16 11 00  J1337+550    11 16 02  55.0  35.5 -2.4    -119.4    -9   1  1      0  16 11 00
16 13 00  ---          11 18 03  55.3  35.3 -2.3    -120.0   111   F  1      0  16 11 10

16 13 00  MKN273       11 18 03  54.0  34.8 -2.4    -119.0    -9   1  1      0  16 13 00
16 16 00  ---          11 21 03  54.4  34.4 -2.4    -119.9   171   F  1      0  16 13 10

16 16 00  J1337+550    11 21 03  55.6  34.9 -2.3    -120.9    -9   1  1      0  16 16 00
16 18 00  ---          11 23 04  55.9  34.6 -2.2    -121.6   111   F  1      0  16 16 10

16 18 00  MKN273       11 23 04  54.6  34.2 -2.4    -120.5    -9   1  1      0  16 18 00
16 21 00  ---          11 26 04  55.0  33.8 -2.3    -121.4   171   F  1      0  16 18 10

16 21 00  J1337+550    11 26 04  56.2  34.2 -2.2    -122.5    -9   1  1      0  16 21 00
16 23 00  ---          11 28 04  56.5  33.9 -2.2    -123.2   111   F  1      0  16 21 10

16 24 00  J1337+550    11 29 05  56.6  33.8 -2.1    -123.5    55   1  1      0  16 24 00
16 26 00  ---          11 31 05  56.8  33.5 -2.1    -124.2   120   F  1      0  16 24 10

16 26 00  MKN273       11 31 05  55.6  33.2 -2.2    -123.0    -9   1  1      0  16 26 00
16 29 00  ---          11 34 05  55.9  32.7 -2.2    -124.0   171   F  1      0  16 26 10

16 29 00  J1337+550    11 34 05  57.2  33.0 -2.1    -125.1    -9   1  1      0  16 29 00
16 31 00  ---          11 36 06  57.4  32.7 -2.0    -125.8   111   F  1      0  16 29 10

16 31 00  MKN273       11 36 06  56.1  32.5 -2.1    -124.6    -9   1  1      0  16 31 00
16 34 00  ---          11 39 06  56.5  32.0 -2.1    -125.6   171   F  1      0  16 31 10
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

16 34 00  J1337+550    11 39 06  57.8  32.3 -2.0    -126.8    -9   1  1      0  16 34 00
16 36 00  ---          11 41 07  58.0  31.9 -1.9    -127.5   111   F  1      0  16 34 10

16 36 00  MKN273       11 41 07  56.7  31.7 -2.1    -126.3    -9   1  1      0  16 36 00
16 39 00  ---          11 44 07  57.0  31.3 -2.0    -127.3   171   F  1      0  16 36 10

16 39 00  J1337+550    11 44 07  58.4  31.4 -1.9    -128.6    -9   1  1      0  16 39 00
16 41 00  ---          11 46 07  58.6  31.1 -1.9    -129.3   111   F  1      0  16 39 10

16 41 00  MKN273       11 46 07  57.3  30.9 -2.0    -128.0    -9   1  1      0  16 41 00
16 44 00  ---          11 49 08  57.6  30.5 -1.9    -129.0   171   F  1      0  16 41 10

16 44 00  J1337+550    11 49 08  58.9  30.5 -1.8    -130.3    -9   1  1      0  16 44 00
16 46 00  ---          11 51 08  59.1  30.2 -1.8    -131.1   111   F  1      0  16 44 10

16 47 00  J1337+550    11 52 08  59.2  30.0 -1.8    -131.4    55   1  1      0  16 47 00
16 49 00  ---          11 54 09  59.4  29.6 -1.7    -132.2   120   F  1      0  16 47 10

16 49 00  MKN273       11 54 09  58.1  29.6 -1.8    -130.8    -9   1  1      0  16 49 00
16 52 00  ---          11 57 09  58.5  29.1 -1.8    -131.8   171   F  1      0  16 49 10

16 52 00  J1337+550    11 57 09  59.8  29.0 -1.7    -133.3    -9   1  1      0  16 52 00
16 54 00  ---          11 59 09  60.0  28.6 -1.6    -134.0   111   F  1      0  16 52 10

16 54 00  MKN273       11 59 09  58.7  28.7 -1.8    -132.6    -9   1  1      0  16 54 00
16 57 00  ---          12 02 10  59.0  28.2 -1.7    -133.7   171   F  1      0  16 54 10

16 57 00  J1337+550    12 02 10  60.3  28.0 -1.6    -135.2    -9   1  1      0  16 57 00
16 59 00  ---          12 04 10  60.5  27.6 -1.6    -135.9   111   F  1      0  16 57 10

16 59 00  MKN273       12 04 10  59.2  27.8 -1.7    -134.4    -9   1  1      0  16 59 00
17 02 00  ---          12 07 11  59.5  27.2 -1.6    -135.5   171   F  1      0  16 59 10

17 02 00  J1337+550    12 07 11  60.8  27.0 -1.5    -137.1    -9   1  1      0  17 02 00
17 04 00  ---          12 09 11  61.0  26.5 -1.5    -137.9   111   F  1      0  17 02 10

17 04 00  MKN273       12 09 11  59.7  26.8 -1.6    -136.3    -9   1  1      0  17 04 00
17 07 00  ---          12 12 12  60.0  26.2 -1.5    -137.4   171   F  1      0  17 04 10

17 07 00  J1337+550    12 12 12  61.3  25.9 -1.4    -139.1    -9   1  1      0  17 07 00
17 09 00  ---          12 14 12  61.4  25.4 -1.4    -139.9   111   F  1      0  17 07 10

17 10 00  J1337+550    12 15 12  61.5  25.2 -1.4    -140.3    55   1  1      0  17 10 00
17 12 00  ---          12 17 12  61.7  24.7 -1.3    -141.2   120   F  1      0  17 10 10
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

17 12 00  MKN273       12 17 12  60.4  25.1 -1.5    -139.4    -9   1  1      0  17 12 00
17 15 00  ---          12 20 13  60.7  24.5 -1.4    -140.6   171   F  1      0  17 12 10

17 15 00  J1337+550    12 20 13  62.0  24.0 -1.3    -142.4    -9   1  1      0  17 15 00
17 17 00  ---          12 22 13  62.2  23.5 -1.3    -143.2   111   F  1      0  17 15 10

17 17 00  MKN273       12 22 13  60.9  24.0 -1.4    -141.4    -9   1  1      0  17 17 00
17 20 00  ---          12 25 14  61.1  23.3 -1.3    -142.6   171   F  1      0  17 17 10

17 20 00  J1337+550    12 25 14  62.4  22.8 -1.2    -144.5    -9   1  1      0  17 20 00
17 22 00  ---          12 27 14  62.6  22.3 -1.2    -145.4   111   F  1      0  17 20 10

17 22 00  MKN273       12 27 14  61.3  22.9 -1.3    -143.4    -9   1  1      0  17 22 00
17 25 00  ---          12 30 15  61.6  22.1 -1.2    -144.7   171   F  1      0  17 22 10

17 25 00  J1337+550    12 30 15  62.8  21.5 -1.1    -146.7    -9   1  1      0  17 25 00
17 27 00  ---          12 32 15  63.0  20.9 -1.1    -147.6   111   F  1      0  17 25 10

17 27 00  MKN273       12 32 15  61.7  21.7 -1.2    -145.5    -9   1  1      0  17 27 00
17 30 00  ---          12 35 15  62.0  20.9 -1.2    -146.8   171   F  1      0  17 27 10

17 30 00  J1337+550    12 35 15  63.2  20.1 -1.0    -148.9    -9   1  1      0  17 30 00
17 32 00  ---          12 37 16  63.4  19.6 -1.0    -149.8   111   F  1      0  17 30 10

17 34 00  J1337+550    12 39 16  63.5  19.0 -1.0    -150.7   114   1  1      0  17 34 00
17 36 00  ---          12 41 16  63.6  18.5 -0.9    -151.7   120   F  1      0  17 34 10

17 36 00  MKN273       12 41 16  62.4  19.4 -1.1    -149.4    -8   1  1      0  17 36 00
17 39 00  ---          12 44 17  62.6  18.6 -1.0    -150.7   172   F  1      0  17 36 10

17 39 00  J1337+550    12 44 17  63.8  17.6 -0.9    -153.0    -8   1  1      0  17 39 00
17 41 00  ---          12 46 17  64.0  17.0 -0.9    -154.0   112   F  1      0  17 39 10

17 41 00  MKN273       12 46 17  62.7  18.1 -1.0    -151.6    -8   1  1      0  17 41 00
17 44 00  ---          12 49 18  62.9  17.2 -0.9    -153.0   172   F  1      0  17 41 10

17 44 00  J1337+550    12 49 18  64.1  16.1 -0.8    -155.4    -8   1  1      0  17 44 00
17 46 00  ---          12 51 18  64.3  15.5 -0.8    -156.4   112   F  1      0  17 44 10

17 46 00  MKN273       12 51 18  63.1  16.7 -0.9    -153.9    -8   1  1      0  17 46 00
17 49 00  ---          12 54 19  63.2  15.8 -0.8    -155.3   172   F  1      0  17 46 10

17 49 00  J1337+550    12 54 19  64.4  14.6 -0.7    -157.8    -8   1  1      0  17 49 00
17 51 00  ---          12 56 19  64.5  14.0 -0.7    -158.8   112   F  1      0  17 49 10
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

17 51 00  MKN273       12 56 19  63.4  15.3 -0.8    -156.2    -8   1  1      0  17 51 00
17 54 00  ---          12 59 19  63.5  14.4 -0.8    -157.6   172   F  1      0  17 51 10

17 54 00  J1337+550    12 59 19  64.7  13.0 -0.6    -160.2    -8   1  1      0  17 54 00
17 56 00  ---          13 01 20  64.8  12.4 -0.6    -161.2   112   F  1      0  17 54 10

17 58 00  J1337+550    13 03 20  64.9  11.8 -0.6    -162.2   114   1  1      0  17 58 00
18 00 00  ---          13 05 20  65.0  11.1 -0.5    -163.2   120   F  1      0  17 58 10

18 00 00  MKN273       13 05 20  63.8  12.6 -0.7    -160.4    -8   1  1      0  18 00 00
18 03 00  ---          13 08 21  64.0  11.7 -0.6    -161.9   172   F  1      0  18 00 10

18 03 00  J1337+550    13 08 21  65.1  10.1 -0.5    -164.7    -8   1  1      0  18 03 00
18 05 00  ---          13 10 21  65.2   9.5 -0.5    -165.7   112   F  1      0  18 03 10

18 05 00  MKN273       13 10 21  64.1  11.1 -0.6    -162.8    -8   1  1      0  18 05 00
18 08 00  ---          13 13 22  64.2  10.2 -0.5    -164.3   172   F  1      0  18 05 10

18 08 00  J1337+550    13 13 22  65.3   8.5 -0.4    -167.2    -8   1  1      0  18 08 00
18 10 00  ---          13 15 22  65.3   7.8 -0.4    -168.3   112   F  1      0  18 08 10

18 10 00  MKN273       13 15 22  64.2   9.6 -0.5    -165.3    -8   1  1      0  18 10 00
18 13 00  ---          13 18 22  64.3   8.6 -0.4    -166.7   172   F  1      0  18 10 10

18 13 00  J1337+550    13 18 22  65.4   6.8 -0.3    -169.8    -8   1  1      0  18 13 00
18 15 00  ---          13 20 23  65.4   6.1 -0.3    -170.8   112   F  1      0  18 13 10

18 15 00  MKN273       13 20 23  64.4   8.0 -0.4    -167.7    -8   1  1      0  18 15 00
18 18 00  ---          13 23 23  64.5   7.0 -0.4    -169.2   172   F  1      0  18 15 10

18 18 00  J1337+550    13 23 23  65.5   5.1 -0.2    -172.4    -8   1  1      0  18 18 00
18 20 00  ---          13 25 24  65.5   4.4 -0.2    -173.4   112   F  1      0  18 18 10

18 22 00  J1337+550    13 27 24  65.6   3.7 -0.2    -174.5   114   1  1      0  18 22 00
18 24 00  ---          13 29 24  65.6   3.0 -0.1    -175.5   120   F  1      0  18 22 10

18 24 00  MKN273       13 29 24  64.6   5.1 -0.3    -172.2    -8   1  1      0  18 24 00
18 27 00  ---          13 32 25  64.7   4.1 -0.2    -173.7   172   F  1      0  18 24 10

18 27 00  J1337+550    13 32 25  65.6   1.9 -0.1    -177.1    -8   1  1      0  18 27 00
18 29 00  ---          13 34 25  65.6   1.3 -0.1    -178.1   112   F  1      0  18 27 10

18 29 00  MKN273       13 34 25  64.7   3.4 -0.2    -174.7    -8   1  1      0  18 29 00
18 32 00  ---          13 37 26  64.7   2.5 -0.1    -176.2   172   F  1      0  18 29 10
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

18 32 00  J1337+550    13 37 26  65.6   0.2  0.0    -179.7    -8   1  1      0  18 32 00
18 34 00  ---          13 39 26  65.6  -0.5  0.0     179.3   112   F  1      0  18 32 10

18 34 00  MKN273       13 39 26  64.8   1.8 -0.1    -177.2    -8   1  1      0  18 34 00
18 37 00  ---          13 42 26  64.8   0.8  0.0    -178.8   172   F  1      0  18 34 10

18 37 00  J1337+550    13 42 26  65.6  -1.5  0.1     177.7    -8   1  1      0  18 37 00
18 39 00  ---          13 44 27  65.6  -2.2  0.1     176.7   112   F  1      0  18 37 10

18 39 00  MKN273       13 44 27  64.8   0.1  0.0    -179.8    -8   1  1      0  18 39 00
18 42 00  ---          13 47 27  64.8  -0.8  0.0     178.7   172   F  1      0  18 39 10

18 42 00  J1337+550    13 47 27  65.6  -3.3  0.2     175.1    -8   1  1      0  18 42 00
18 44 00  ---          13 49 28  65.6  -4.0  0.2     174.0   112   F  1      0  18 42 10

18 46 00  J1337+550    13 51 28  65.5  -4.7  0.2     173.0   114   1  1      0  18 46 00
18 48 00  ---          13 53 28  65.5  -5.3  0.3     172.0   120   F  1      0  18 46 10

18 48 00  MKN273       13 53 28  64.7  -2.8  0.1     175.7    -8   1  1      0  18 48 00
18 51 00  ---          13 56 29  64.7  -3.8  0.2     174.2   172   F  1      0  18 48 10

18 51 00  J1337+550    13 56 29  65.4  -6.4  0.3     170.4    -8   1  1      0  18 51 00
18 53 00  ---          13 58 29  65.4  -7.1  0.3     169.4   112   F  1      0  18 51 10

18 53 00  MKN273       13 58 29  64.7  -4.5  0.2     173.2    -8   1  1      0  18 53 00
18 56 00  ---          14 01 30  64.6  -5.4  0.3     171.6   172   F  1      0  18 53 10

18 56 00  J1337+550    14 01 30  65.3  -8.1  0.4     167.9    -8   1  1      0  18 56 00
18 58 00  ---          14 03 30  65.2  -8.7  0.4     166.8   112   F  1      0  18 56 10

18 58 00  MKN273       14 03 30  64.6  -6.1  0.3     170.6    -8   1  1      0  18 58 00
19 01 00  ---          14 06 30  64.5  -7.1  0.4     169.2   172   F  1      0  18 58 10

19 01 00  J1337+550    14 06 30  65.1  -9.7  0.5     165.3    -8   1  1      0  19 01 00
19 03 00  ---          14 08 31  65.0 -10.4  0.5     164.3   112   F  1      0  19 01 10

19 03 00  MKN273       14 08 31  64.4  -7.7  0.4     168.2    -8   1  1      0  19 03 00
19 06 00  ---          14 11 31  64.3  -8.6  0.4     166.7   172   F  1      0  19 03 10

19 06 00  J1337+550    14 11 31  64.9 -11.4  0.6     162.8    -8   1  1      0  19 06 00
19 08 00  ---          14 13 31  64.8 -12.0  0.6     161.8   112   F  1      0  19 06 10

19 10 00  J1337+550    14 15 32  64.7 -12.7  0.6     160.8   114   1  1      0  19 10 00
19 12 00  ---          14 17 32  64.6 -13.3  0.7     159.8   120   F  1      0  19 10 10
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

19 12 00  MKN273       14 17 32  64.1 -10.5  0.5     163.7    -8   1  1      0  19 12 00
19 15 00  ---          14 20 33  64.0 -11.4  0.6     162.3   172   F  1      0  19 12 10

19 15 00  J1337+550    14 20 33  64.5 -14.2  0.7     158.4    -8   1  1      0  19 15 00
19 17 00  ---          14 22 33  64.4 -14.8  0.7     157.4   112   F  1      0  19 15 10

19 17 00  MKN273       14 22 33  63.9 -12.1  0.6     161.3    -8   1  1      0  19 17 00
19 20 00  ---          14 25 33  63.8 -13.0  0.7     159.9   172   F  1      0  19 17 10

19 20 00  J1337+550    14 25 33  64.2 -15.8  0.8     156.0    -8   1  1      0  19 20 00
19 22 00  ---          14 27 34  64.1 -16.4  0.8     155.0   112   F  1      0  19 20 10

19 22 00  MKN273       14 27 34  63.7 -13.6  0.7     158.9    -8   1  1      0  19 22 00
19 25 00  ---          14 30 34  63.5 -14.4  0.8     157.5   172   F  1      0  19 22 10

19 25 00  J1337+550    14 30 34  63.9 -17.2  0.9     153.6    -8   1  1      0  19 25 00
19 27 00  ---          14 32 35  63.8 -17.8  0.9     152.7   112   F  1      0  19 25 10

19 27 00  MKN273       14 32 35  63.4 -15.0  0.8     156.6    -8   1  1      0  19 27 00
19 30 00  ---          14 35 35  63.2 -15.9  0.8     155.2   172   F  1      0  19 27 10

19 30 00  J1337+550    14 35 35  63.6 -18.7  1.0     151.3    -8   1  1      0  19 30 00
19 32 00  ---          14 37 35  63.4 -19.3  1.0     150.4   112   F  1      0  19 30 10

19 34 00  J1337+550    14 39 36  63.3 -19.8  1.0     149.5   114   1  1      0  19 34 00
19 36 00  ---          14 41 36  63.1 -20.4  1.1     148.6   120   F  1      0  19 34 10

19 36 00  MKN273       14 41 36  62.9 -17.5  0.9     152.5    -8   1  1      0  19 36 00
19 39 00  ---          14 44 37  62.7 -18.4  1.0     151.1   172   F  1      0  19 36 10

19 39 00  J1337+550    14 44 37  62.9 -21.2  1.1     147.2    -8   1  1      0  19 39 00
19 41 00  ---          14 46 37  62.8 -21.7  1.1     146.3   112   F  1      0  19 39 10

19 41 00  MKN273       14 46 37  62.5 -18.9  1.0     150.2    -8   1  1      0  19 41 00
19 44 00  ---          14 49 37  62.3 -19.7  1.1     148.9   172   F  1      0  19 41 10

19 44 00  J1337+550    14 49 37  62.5 -22.5  1.2     145.0    -8   1  1      0  19 44 00
19 46 00  ---          14 51 38  62.3 -23.0  1.2     144.2   112   F  1      0  19 44 10

19 46 00  MKN273       14 51 38  62.2 -20.2  1.1     148.1    -8   1  1      0  19 46 00
19 49 00  ---          14 54 38  61.9 -20.9  1.2     146.8   172   F  1      0  19 46 10

19 49 00  J1337+550    14 54 38  62.1 -23.7  1.3     142.9    -8   1  1      0  19 49 00
19 51 00  ---          14 56 39  61.9 -24.2  1.3     142.1   112   F  1      0  19 49 10
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

19 51 00  MKN273       14 56 39  61.8 -21.4  1.2     145.9    -8   1  1      0  19 51 00
19 54 00  ---          14 59 39  61.5 -22.2  1.2     144.6   172   F  1      0  19 51 10

19 54 00  J1337+550    14 59 39  61.6 -24.9  1.4     140.8    -8   1  1      0  19 54 00
19 56 00  ---          15 01 39  61.5 -25.4  1.4     140.0   112   F  1      0  19 54 10

19 58 00  J1337+550    15 03 40  61.3 -25.8  1.4     139.2   114   1  1      0  19 58 00
20 00 00  ---          15 05 40  61.1 -26.3  1.5     138.4   120   F  1      0  19 58 10

20 00 00  MKN273       15 05 40  61.0 -23.6  1.3     142.2    -8   1  1      0  20 00 00
20 03 00  ---          15 08 41  60.8 -24.3  1.4     140.9   172   F  1      0  20 00 10

20 03 00  J1337+550    15 08 41  60.8 -26.9  1.5     137.2    -8   1  1      0  20 03 00
20 05 00  ---          15 10 41  60.6 -27.4  1.5     136.4   112   F  1      0  20 03 10

20 05 00  MKN273       15 10 41  60.6 -24.7  1.4     140.1    -8   1  1      0  20 05 00
20 08 00  ---          15 13 41  60.3 -25.4  1.5     139.0   172   F  1      0  20 05 10

20 08 00  J1337+550    15 13 41  60.3 -28.0  1.6     135.2    -8   1  1      0  20 08 00
20 10 00  ---          15 15 42  60.1 -28.4  1.6     134.5   112   F  1      0  20 08 10

20 10 00  MKN273       15 15 42  60.1 -25.8  1.5     138.2    -8   1  1      0  20 10 00
20 13 00  ---          15 18 42  59.9 -26.4  1.6     137.0   172   F  1      0  20 10 10

20 13 00  J1337+550    15 18 42  59.8 -29.0  1.7     133.3    -8   1  1      0  20 13 00
20 15 00  ---          15 20 42  59.6 -29.4  1.7     132.6   112   F  1      0  20 13 10

20 15 00  MKN273       15 20 42  59.7 -26.8  1.6     136.2    -8   1  1      0  20 15 00
20 18 00  ---          15 23 43  59.4 -27.4  1.6     135.1   172   F  1      0  20 15 10

20 18 00  J1337+550    15 23 43  59.3 -30.0  1.8     131.5    -8   1  1      0  20 18 00
20 20 00  ---          15 25 43  59.0 -30.3  1.8     130.8   112   F  1      0  20 18 10

20 22 00  J1337+550    15 27 44  58.8 -30.7  1.8     130.0   114   1  1      0  20 22 00
20 24 00  ---          15 29 44  58.6 -31.0  1.9     129.3   120   F  1      0  20 22 10

20 24 00  MKN273       15 29 44  58.8 -28.6  1.7     132.9    -8   1  1      0  20 24 00
20 27 00  ---          15 32 44  58.4 -29.1  1.8     131.8   172   F  1      0  20 24 10

20 27 00  J1337+550    15 32 44  58.3 -31.6  1.9     128.3    -8   1  1      0  20 27 00
20 29 00  ---          15 34 45  58.0 -31.9  1.9     127.6   112   F  1      0  20 27 10

20 29 00  MKN273       15 34 45  58.2 -29.5  1.8     131.1    -8   1  1      0  20 29 00
20 32 00  ---          15 37 45  57.9 -30.0  1.9     130.0   172   F  1      0  20 29 10
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

20 32 00  J1337+550    15 37 45  57.7 -32.4  2.0     126.6    -8   1  1      0  20 32 00
20 34 00  ---          15 39 46  57.5 -32.7  2.0     125.9   112   F  1      0  20 32 10

20 34 00  MKN273       15 39 46  57.7 -30.3  1.9     129.3    -8   1  1      0  20 34 00
20 37 00  ---          15 42 46  57.4 -30.8  2.0     128.3   172   F  1      0  20 34 10

20 37 00  J1337+550    15 42 46  57.1 -33.2  2.1     124.9    -8   1  1      0  20 37 00
20 39 00  ---          15 44 46  56.9 -33.5  2.1     124.2   112   F  1      0  20 37 10

20 39 00  MKN273       15 44 46  57.1 -31.1  2.0     127.6    -8   1  1      0  20 39 00
20 42 00  ---          15 47 47  56.8 -31.6  2.0     126.6   172   F  1      0  20 39 10

20 42 00  J1337+550    15 47 47  56.5 -33.9  2.2     123.2    -8   1  1      0  20 42 00
20 44 00  ---          15 49 47  56.3 -34.2  2.2     122.6   112   F  1      0  20 42 10

20 46 00  J1337+550    15 51 48  56.0 -34.5  2.2     121.9   114   1  1      0  20 46 00
20 48 00  ---          15 53 48  55.8 -34.7  2.3     121.3   120   F  1      0  20 46 10

20 48 00  MKN273       15 53 48  56.1 -32.5  2.1     124.6    -7   1  1      0  20 48 00
20 51 00  ---          15 56 48  55.8 -32.9  2.2     123.6   173   F  1      0  20 48 10

20 51 00  J1337+550    15 56 48  55.4 -35.1  2.3     120.4    -7   1  1      0  20 51 00
20 53 00  ---          15 58 49  55.2 -35.4  2.3     119.8   113   F  1      0  20 51 10

20 53 00  MKN273       15 58 49  55.5 -33.2  2.2     123.0    -7   1  1      0  20 53 00
20 56 00  ---          16 01 49  55.2 -33.6  2.3     122.0   173   F  1      0  20 53 10

20 56 00  J1337+550    16 01 49  54.8 -35.7  2.4     118.8    -7   1  1      0  20 56 00
20 58 00  ---          16 03 50  54.5 -36.0  2.4     118.2   113   F  1      0  20 56 10

20 58 00  MKN273       16 03 50  54.9 -33.8  2.3     121.4    -7   1  1      0  20 58 00
21 01 00  ---          16 06 50  54.6 -34.2  2.4     120.5   173   F  1      0  20 58 10

21 01 00  J1337+550    16 06 50  54.2 -36.3  2.5     117.3    -7   1  1      0  21 01 00
21 03 00  ---          16 08 50  53.9 -36.5  2.5     116.7   113   F  1      0  21 01 10

21 03 00  MKN273       16 08 50  54.3 -34.5  2.4     119.9    -7   1  1      0  21 03 00
21 06 00  ---          16 11 51  54.0 -34.8  2.4     118.9   173   F  1      0  21 03 10

21 06 00  J1337+550    16 11 51  53.5 -36.9  2.6     115.9    -7   1  1      0  21 06 00
21 08 00  ---          16 13 51  53.2 -37.1  2.6     115.3   113   F  1      0  21 06 10

21 09 00  J1337+550    16 14 51  53.1 -37.2  2.6     115.0    55   1  1      0  21 09 00
21 11 00  ---          16 16 52  52.9 -37.4  2.6     114.4   120   F  1      0  21 09 10
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

21 11 00  MKN273       16 16 52  53.4 -35.4  2.5     117.5    -7   1  1      0  21 11 00
21 14 00  ---          16 19 52  53.0 -35.7  2.6     116.6   173   F  1      0  21 11 10

21 14 00  J1337+550    16 19 52  52.5 -37.7  2.7     113.6    -7   1  1      0  21 14 00
21 16 00  ---          16 21 53  52.2 -37.9  2.7     113.0   113   F  1      0  21 14 10

21 16 00  MKN273       16 21 53  52.7 -35.9  2.6     116.0    -7   1  1      0  21 16 00
21 19 00  ---          16 24 53  52.3 -36.2  2.7     115.1   173   F  1      0  21 16 10

21 19 00  J1337+550    16 24 53  51.8 -38.1  2.8     112.2    -7   1  1      0  21 19 00
21 21 00  ---          16 26 53  51.5 -38.3  2.8     111.7   113   F  1      0  21 19 10

21 21 00  MKN273       16 26 53  52.1 -36.4  2.7     114.6    -7   1  1      0  21 21 00
21 24 00  ---          16 29 54  51.7 -36.7  2.8     113.7   173   F  1      0  21 21 10

21 24 00  J1337+550    16 29 54  51.1 -38.5  2.9     110.8    -7   1  1      0  21 24 00
21 26 00  ---          16 31 54  50.9 -38.7  2.9     110.3   113   F  1      0  21 24 10

21 26 00  MKN273       16 31 54  51.4 -36.8  2.8     113.2    -7   1  1      0  21 26 00
21 29 00  ---          16 34 55  51.1 -37.1  2.8     112.3   173   F  1      0  21 26 10

21 29 00  J1337+550    16 34 55  50.5 -38.9  2.9     109.5    -7   1  1      0  21 29 00
21 31 00  ---          16 36 55  50.2 -39.1  3.0     109.0   113   F  1      0  21 29 10

21 32 00  J1337+550    16 37 55  50.0 -39.2  3.0     108.7    55   1  1      0  21 32 00
21 34 00  ---          16 39 55  49.8 -39.3  3.0     108.2   120   F  1      0  21 32 10

21 34 00  MKN273       16 39 55  50.4 -37.5  2.9     111.0    -7   1  1      0  21 34 00
21 37 00  ---          16 42 56  50.0 -37.7  3.0     110.2   173   F  1      0  21 34 10

21 37 00  J1337+550    16 42 56  49.4 -39.5  3.1     107.4    -7   1  1      0  21 37 00
21 39 00  ---          16 44 56  49.1 -39.6  3.1     106.9   113   F  1      0  21 37 10

21 39 00  MKN273       16 44 56  49.7 -37.9  3.0     109.7    -7   1  1      0  21 39 00
21 42 00  ---          16 47 57  49.3 -38.1  3.1     108.9   173   F  1      0  21 39 10

21 42 00  J1337+550    16 47 57  48.7 -39.8  3.2     106.2    -7   1  1      0  21 42 00
21 44 00  ---          16 49 57  48.4 -39.9  3.2     105.7   113   F  1      0  21 42 10

21 44 00  MKN273       16 49 57  49.1 -38.2  3.1     108.4    -7   1  1      0  21 44 00
21 47 00  ---          16 52 58  48.7 -38.4  3.1     107.6   173   F  1      0  21 44 10

21 47 00  J1337+550    16 52 58  48.0 -40.1  3.2     104.9    -7   1  1      0  21 47 00
21 49 00  ---          16 54 58  47.7 -40.2  3.3     104.4   113   F  1      0  21 47 10
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

21 49 00  MKN273       16 54 58  48.4 -38.6  3.2     107.1    -7   1  1      0  21 49 00
21 52 00  ---          16 57 58  48.0 -38.8  3.2     106.3   173   F  1      0  21 49 10

21 52 00  J1337+550    16 57 58  47.3 -40.4  3.3     103.7    -7   1  1      0  21 52 00
21 54 00  ---          16 59 59  47.0 -40.5  3.4     103.2   113   F  1      0  21 52 10

21 55 00  J1337+550    17 00 59  46.9 -40.5  3.4     103.0    55   1  1      0  21 55 00
21 57 00  ---          17 02 59  46.6 -40.6  3.4     102.5   120   F  1      0  21 55 10

21 57 00  MKN273       17 02 59  47.3 -39.0  3.3     105.1    -7   1  1      0  21 57 00
22 00 00  ---          17 06 00  46.9 -39.2  3.4     104.3   173   F  1      0  21 57 10

22 00 00  J1337+550    17 06 00  46.2 -40.7  3.5     101.8    -7   1  1      0  22 00 00
22 02 00  ---          17 08 00  45.9 -40.8  3.5     101.3   113   F  1      0  22 00 10

22 02 00  MKN273       17 08 00  46.6 -39.3  3.4     103.8    -7   1  1      0  22 02 00
22 05 00  ---          17 11 01  46.2 -39.4  3.4     103.1   173   F  1      0  22 02 10

22 05 00  J1337+550    17 11 01  45.5 -40.9  3.5     100.6    -8   1  1      0  22 05 00
22 07 00  ---          17 13 01  45.2 -41.0  3.6     100.2   112   F  1      0  22 05 10

22 07 00  MKN273       17 13 01  46.0 -39.5  3.5     102.6    -8   1  1      0  22 07 00
22 10 00  ---          17 16 01  45.5 -39.7  3.5     101.9   172   F  1      0  22 07 10

22 10 00  J1337+550    17 16 01  44.8 -41.1  3.6      99.5    -8   1  1      0  22 10 00
22 12 00  ---          17 18 02  44.5 -41.2  3.7      99.0   112   F  1      0  22 10 10

22 12 00  MKN273       17 18 02  45.3 -39.7  3.6     101.5    -8   1  1      0  22 12 00
22 15 00  ---          17 21 02  44.9 -39.9  3.6     100.7   172   F  1      0  22 12 10

22 15 00  J1337+550    17 21 02  44.0 -41.3  3.7      98.3    -8   1  1      0  22 15 00
22 17 00  ---          17 23 03  43.8 -41.3  3.8      97.9   112   F  1      0  22 15 10

22 21 00  J1337+550    17 27 03  43.2 -41.4  3.8      97.0   233   1  1      0  22 21 00
22 23 00  ---          17 29 04  42.9 -41.5  3.9      96.6   120   F  1      0  22 21 10

22 23 00  MKN273       17 29 04  43.7 -40.1  3.7      98.9    -8   1  1      0  22 23 00
22 26 00  ---          17 32 04  43.3 -40.2  3.8      98.2   172   F  1      0  22 23 10

22 26 00  J1337+550    17 32 04  42.5 -41.6  3.9      95.9    -8   1  1      0  22 26 00
22 28 00  ---          17 34 04  42.2 -41.6  3.9      95.5   112   F  1      0  22 26 10

22 28 00  MKN273       17 34 04  43.1 -40.3  3.8      97.8    -8   1  1      0  22 28 00
22 31 00  ---          17 37 05  42.6 -40.3  3.9      97.1   172   F  1      0  22 28 10
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

22 31 00  J1337+550    17 37 05  41.8 -41.6  4.0      94.8    -8   1  1      0  22 31 00
22 33 00  ---          17 39 05  41.5 -41.7  4.0      94.4   112   F  1      0  22 31 10

22 38 00  J1310+322    17 44 06  32.7 -69.0  4.6      71.9   276   1  1      0  22 38 00
22 48 00  ---          17 54 08  30.7 -68.2  4.7      71.0   600   F  1      0  22 38 10

22 53 00  J1337+550    17 59 08  38.6 -41.8  4.4      90.2   276   1  1      0  22 53 00
22 55 00  ---          18 01 09  38.3 -41.8  4.4      89.8   120   F  1      0  22 53 10

22 55 00  MKN273       18 01 09  39.3 -40.7  4.3      91.9    -8   1  1      0  22 55 00
22 58 00  ---          18 04 09  38.8 -40.7  4.3      91.3   172   F  1      0  22 55 10

22 58 00  J1337+550    18 04 09  37.9 -41.8  4.4      89.1    -8   1  1      0  22 58 00
23 00 00  ---          18 06 10  37.6 -41.8  4.5      88.7   112   F  1      0  22 58 10

23 00 00  MKN273       18 06 10  38.6 -40.7  4.4      90.8    -8   1  1      0  23 00 00
23 03 00  ---          18 09 10  38.1 -40.7  4.4      90.2   172   F  1      0  23 00 10

23 03 00  J1337+550    18 09 10  37.2 -41.8  4.5      88.1    -8   1  1      0  23 03 00
23 05 00  ---          18 11 10  36.9 -41.8  4.6      87.7   112   F  1      0  23 03 10

23 05 00  MKN273       18 11 10  37.9 -40.7  4.4      89.8    -8   1  1      0  23 05 00
23 08 00  ---          18 14 11  37.4 -40.7  4.5      89.2   172   F  1      0  23 05 10

23 08 00  J1337+550    18 14 11  36.4 -41.8  4.6      87.1    -8   1  1      0  23 08 00
23 10 00  ---          18 16 11  36.2 -41.7  4.6      86.7   112   F  1      0  23 08 10

23 10 00  MKN273       18 16 11  37.2 -40.7  4.5      88.8    -8   1  1      0  23 10 00
23 13 00  ---          18 19 12  36.7 -40.7  4.6      88.1   172   F  1      0  23 10 10

23 13 00  J1337+550    18 19 12  35.7 -41.7  4.7      86.1    -8   1  1      0  23 13 00
23 15 00  ---          18 21 12  35.4 -41.7  4.7      85.7   112   F  1      0  23 13 10

23 16 00  J1337+550    18 22 12  35.3 -41.7  4.7      85.5    54   1  1      0  23 16 00
23 18 00  ---          18 24 13  35.0 -41.6  4.8      85.1   120   F  1      0  23 16 10

23 18 00  MKN273       18 24 13  36.0 -40.7  4.7      87.1    -8   1  1      0  23 18 00
23 21 00  ---          18 27 13  35.6 -40.6  4.7      86.5   172   F  1      0  23 18 10

23 21 00  J1337+550    18 27 13  34.6 -41.6  4.8      84.6    -8   1  1      0  23 21 00
23 23 00  ---          18 29 13  34.3 -41.6  4.9      84.2   112   F  1      0  23 21 10

23 23 00  MKN273       18 29 13  35.3 -40.6  4.7      86.1    -8   1  1      0  23 23 00
23 26 00  ---          18 32 14  34.9 -40.6  4.8      85.5   172   F  1      0  23 23 10
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  21 Oct 2005   Day 294 ---

23 26 00  J1337+550    18 32 14  33.9 -41.5  4.9      83.6    -8   1  1      0  23 26 00
23 28 00  ---          18 34 14  33.6 -41.5  4.9      83.2   112   F  1      0  23 26 10

23 28 00  MKN273       18 34 14  34.6 -40.5  4.8      85.1    -8   1  1      0  23 28 00
23 31 00  ---          18 37 15  34.2 -40.5  4.9      84.5   172   F  1      0  23 28 10

23 31 00  J1337+550    18 37 15  33.1 -41.4  5.0      82.6    -8   1  1      0  23 31 00
23 33 00  ---          18 39 15  32.9 -41.4  5.0      82.2   112   F  1      0  23 31 10

23 33 00  MKN273       18 39 15  33.9 -40.5  4.9      84.1    -8   1  1      0  23 33 00
23 36 00  ---          18 42 16  33.5 -40.4  5.0      83.5   172   F  1      0  23 33 10

23 36 00  J1337+550    18 42 16  32.4 -41.3  5.1      81.6    -8   1  1      0  23 36 00
23 38 00  ---          18 44 16  32.1 -41.2  5.1      81.3   112   F  1      0  23 36 10

23 39 00  J1337+550    18 45 16  32.0 -41.2  5.1      81.1    54   1  1      0  23 39 00
23 41 00  ---          18 47 16  31.7 -41.2  5.2      80.7   120   F  1      0  23 39 10

23 41 00  MKN273       18 47 16  32.8 -40.3  5.0      82.6    -8   1  1      0  23 41 00
23 44 00  ---          18 50 17  32.4 -40.2  5.1      82.0   172   F  1      0  23 41 10

23 44 00  J1337+550    18 50 17  31.3 -41.1  5.2      80.1    -8   1  1      0  23 44 00
23 46 00  ---          18 52 17  31.0 -41.0  5.2      79.7   112   F  1      0  23 44 10

23 46 00  MKN273       18 52 17  32.1 -40.2  5.1      81.6    -8   1  1      0  23 46 00
23 49 00  ---          18 55 18  31.7 -40.1  5.2      81.0   172   F  1      0  23 46 10

23 49 00  J1337+550    18 55 18  30.6 -40.9  5.3      79.2    -8   1  1      0  23 49 00
23 51 00  ---          18 57 18  30.3 -40.9  5.3      78.8   112   F  1      0  23 49 10

23 51 00  MKN273       18 57 18  31.4 -40.1  5.2      80.6    -8   1  1      0  23 51 00
23 54 00  ---          19 00 18  31.0 -40.0  5.3      80.0   172   F  1      0  23 51 10

23 54 00  J1337+550    19 00 18  29.9 -40.8  5.4      78.2    -8   1  1      0  23 54 00
23 56 00  ---          19 02 19  29.6 -40.7  5.4      77.8   112   F  1      0  23 54 10

23 56 00  MKN273       19 02 19  30.7 -39.9  5.3      79.6    -8   1  1      0  23 56 00
23 59 00  ---          19 05 19  30.3 -39.8  5.3      79.1   172   F  1      0  23 56 10

 --- Start: Fri  21 Oct 2005   Day 294 -- Stop: Sat  22 Oct 2005   Day 295 ---

23 59 00  J1337+550    19 05 19  29.2 -40.6  5.5      77.3    -8   1  1      0  23 59 00
00 01 00  ---          19 07 20  28.9 -40.5  5.5      76.9   112   F  1      0  23 59 10
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Mkn 273 GLOBAL 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

00 02 00  J1337+550    19 08 20  28.8 -40.5  5.5      76.7    55   1  1      0  00 02 00
00 04 00  ---          19 10 20  28.5 -40.4  5.5      76.3   120   F  1      0  00 02 10

00 04 00  MKN273       19 10 20  29.6 -39.7  5.4      78.1    -8   1  1      0  00 04 00
00 07 00  ---          19 13 21  29.2 -39.6  5.5      77.5   172   F  1      0  00 04 10

00 07 00  J1337+550    19 13 21  28.1 -40.3  5.6      75.8    -8   1  1      0  00 07 00
00 09 00  ---          19 15 21  27.8 -40.2  5.6      75.4   112   F  1      0  00 07 10

00 09 00  MKN273       19 15 21  28.9 -39.5  5.5      77.2    -8   1  1      0  00 09 00
00 12 00  ---          19 18 21  28.5 -39.4  5.6      76.6   172   F  1      0  00 09 10

00 12 00  J1337+550    19 18 21  27.4 -40.1  5.7      74.9    -8   1  1      0  00 12 00
00 14 00  ---          19 20 22  27.1 -40.0  5.7      74.5   112   F  1      0  00 12 10

00 14 00  MKN273       19 20 22  28.3 -39.3  5.6      76.2    -8   1  1      0  00 14 00
00 17 00  ---          19 23 22  27.8 -39.2  5.6      75.6   172   F  1      0  00 14 10

00 17 00  J1337+550    19 23 22  26.7 -39.8  5.8      73.9    -8   1  1      0  00 17 00
00 19 00  ---          19 25 23  26.4 -39.8  5.8      73.6   112   F  1      0  00 17 10

00 19 00  MKN273       19 25 23  27.6 -39.1  5.7      75.3    -8   1  1      0  00 19 00
00 22 00  ---          19 28 23  27.2 -39.0  5.7      74.7   172   F  1      0  00 19 10

00 22 00  J1337+550    19 28 23  26.0 -39.6  5.8      73.0    -8   1  1      0  00 22 00
00 24 00  ---          19 30 23  25.7 -39.5  5.9      72.6   112   F  1      0  00 22 10


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gb055a.6cm
   Matches group v6cm_2 in /irasoft/sched/catalogs/freq.dat

   Setup group:   11         Station: VLBA_FD           Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:  11  Setup file default.  Used pcal sets:   1
   LO sum=    4974.49   4974.49   4982.49   4982.49   4990.49   4990.49   4998.49   4998.49
   BBC fr=     874.49    874.49    882.49    882.49    890.49    890.49    898.49    898.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_off 
 SOURCE LIST -- Mkn 273 GLOBAL 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * MKN273            13 42 51.721505   * 13 44 42.142000     13 44 53.234698       0.00
                     56 08 13.98754    * 55 53 13.15000      55 51 29.25777        0.00
                     From catalog imbedded in main SCHED input file.
                        8.700 scan hours,    488.387 baseline hours above horizon.

 * J1337+550         13 35 55.218449   * 13 37 49.642224     13 38 01.230408       0.00
                     55 16 15.76062    * 55 01 02.11786      54 59 16.63763        0.00
                     From catalog imbedded in main SCHED input file.
                        7.233 scan hours,    402.390 baseline hours above horizon.

 * J1310+322         13 08 07.560126   * 13 10 28.663845     13 10 43.624011       0.00
                     32 36 40.23888    * 32 20 43.78295      32 18 55.77726        0.00
                     From catalog imbedded in main SCHED input file.
                        0.333 scan hours,      8.500 baseline hours above horizon.

   J1642+3948        16 41 17.606231   * 16 42 58.809968     16 43 09.232479       0.26
   1641+399          39 54 10.81493    * 39 48 36.99399      39 48 04.15753        0.40
 * 3C345             /irasoft/sched/catalogs/sources.vlba
   J1642+39          VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        0.200 scan hours,     14.699 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   MKN273              66.7
   J1337+550           65.9
   J1310+322           44.0
   3C345               65.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

