  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GW023A
 Exp. Code:  GW023A  


Schedule Version:       4.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Di Wen

Address:  Kapteyn Astronomical Institute
          Landleven 12
          9747 AD Groningen
          the Netherlands

Phone:    +31 503 638 324
EMAIL:    wen@astro.rug.nl
Fax:
Phone during observation: +31 685 842 225

Observing mode:

Notes:    v4 - DSS63 dropped
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

 Next scan frequencies:  8240.00  8240.00  8304.00  8304.00  8368.00  8368.00  8432.00  8432.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

16 00 02  J0132+4325   19 20 24  18.3  49.6 -6.2     -64.8     0        0   16 00 02
16 03 00  =0129+431    19 23 22  18.8  49.9 -6.2     -65.2   178       46   16 00 03

16 03 00  B0128+437    19 23 22  19.2  49.5 -6.2     -65.6    -9       46   16 03 09
16 06 30  ---          19 26 53  19.8  49.7 -6.1     -66.1   201       98   16 03 01

16 06 30  J0132+4325   19 26 53  19.3  50.2 -6.1     -65.7    -9       98   16 06 39
16 08 00  =0129+431    19 28 23  19.6  50.3 -6.1     -65.9    81      119   16 06 31

16 08 32  B0128+437    19 28 55  20.2  49.9 -6.1     -66.4    23      119   16 08 32
16 12 00  ---          19 32 24  20.7  50.2 -6.0     -66.9   208      172   16 08 33

 ---------- Scan set 10 ----------

16 12 36  J0132+4325   19 33 00  20.4  50.6 -6.0     -66.6    27      172   16 12 36
16 14 06  =0129+431    19 34 30  20.6  50.7 -6.0     -66.8    90      195   16 12 37

16 14 06  B0128+437    19 34 30  21.1  50.3 -6.0     -67.2    -9      195   16 14 15
16 17 36  ---          19 38 00  21.7  50.6 -5.9     -67.7   201      247   16 14 07

16 18 08  J0132+4325   19 38 33  21.3  51.0 -5.9     -67.4    23      247   16 18 08
16 19 36  =0129+431    19 40 01  21.5  51.2 -5.9     -67.6    88      270   16 18 09

16 19 36  B0128+437    19 40 01  22.0  50.7 -5.9     -68.0    -9      270   16 19 45
16 23 06  ---          19 43 31  22.6  51.0 -5.8     -68.6   201      322   16 19 37

16 23 06  J0132+4325   19 43 31  22.1  51.4 -5.8     -68.1    -9      322   16 23 15
16 24 36  =0129+431    19 45 02  22.4  51.5 -5.8     -68.3    81      342   16 23 07

16 24 36  B0128+437    19 45 02  22.8  51.1 -5.8     -68.8    -9      342   16 24 45
16 28 06  ---          19 48 32  23.4  51.3 -5.7     -69.3   201      394   16 24 37

16 28 38  J0132+4325   19 49 04  23.1  51.8 -5.8     -68.9    23      394   16 28 38
16 30 06  =0129+431    19 50 33  23.3  51.9 -5.7     -69.1    88      417   16 28 39

16 30 06  B0128+437    19 50 33  23.8  51.5 -5.7     -69.6    -9      417   16 30 15
16 33 36  ---          19 54 03  24.3  51.7 -5.6     -70.1   201      469   16 30 07

16 33 36  J0132+4325   19 54 03  23.9  52.2 -5.7     -69.7    -9      469   16 33 45
16 35 06  =0129+431    19 55 33  24.2  52.3 -5.6     -69.9    81      490   16 33 37
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

16 35 06  B0128+437    19 55 33  24.6  51.8 -5.6     -70.3    -9      490   16 35 15
16 36 06  ---          19 56 33  24.8  51.9 -5.6     -70.5    51      503   16 35 07

 ---------- Scan set 11 ----------

16 36 06  B0128+437    19 56 33  24.8  51.9 -5.6     -70.5    -6      503   16 36 12
16 39 36  ---          20 00 04  25.4  52.1 -5.5     -71.0   204      555   16 36 07

16 40 06  J0132+4325   20 00 34  25.0  52.6 -5.6     -70.6    21      555   16 40 06
16 41 36  =0129+431    20 02 04  25.3  52.7 -5.5     -70.8    90      578   16 40 07

16 41 36  B0128+437    20 02 04  25.7  52.2 -5.5     -71.3    -9      578   16 41 45
16 45 06  ---          20 05 35  26.3  52.5 -5.5     -71.8   201      630   16 41 37

16 45 06  J0132+4325   20 05 35  25.9  52.9 -5.5     -71.3    -9      630   16 45 15
16 46 36  =0129+431    20 07 05  26.1  53.0 -5.5     -71.5    81      651   16 45 07

 ---------- Scan set 11 ----------

16 46 36  B0128+437    20 07 05  26.6  52.5 -5.4     -72.0    -9      651   16 46 45
16 50 06  ---          20 10 36  27.2  52.8 -5.4     -72.5   201      703   16 46 37

16 50 36  J0132+4325   20 11 06  26.8  53.3 -5.4     -72.1    21      703   16 50 36
16 52 06  =0129+431    20 12 36  27.1  53.4 -5.4     -72.3    90      726   16 50 37

16 52 06  B0128+437    20 12 36  27.5  52.9 -5.3     -72.8    -9      726   16 52 15
16 55 36  ---          20 16 07  28.1  53.1 -5.3     -73.3   201      778   16 52 07

16 55 36  J0132+4325   20 16 07  27.7  53.6 -5.3     -72.8    -9      778   16 55 45
16 57 06  =0129+431    20 17 37  27.9  53.7 -5.3     -73.1    81      799   16 55 37

16 57 06  B0128+437    20 17 37  28.4  53.2 -5.3     -73.5    -9      799   16 57 15
16 58 06  ---          20 18 37  28.5  53.2 -5.2     -73.7    51      812   16 57 07

 ---------- Scan set 12 ----------

16 58 06  B0128+437    20 18 37  28.5  53.2 -5.2     -73.7    -6      812   16 58 12
17 01 36  ---          20 22 08  29.1  53.4 -5.2     -74.2   204      864   16 58 07

17 02 06  J0132+4325   20 22 38  28.8  54.0 -5.2     -73.8    21      864   17 02 06
17 03 36  =0129+431    20 24 08  29.1  54.1 -5.2     -74.0    90      888   17 02 07

17 03 36  B0128+437    20 24 08  29.5  53.5 -5.1     -74.5    -9      888   17 03 45
17 07 06  ---          20 27 39  30.1  53.7 -5.1     -75.0   201      939   17 03 37
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

17 07 06  J0132+4325   20 27 39  29.7  54.3 -5.1     -74.5    -9      939   17 07 15
17 08 36  =0129+431    20 29 09  30.0  54.3 -5.1     -74.7    81      960   17 07 07

 ---------- Scan set 12 ----------

17 08 36  B0128+437    20 29 09  30.4  53.8 -5.1     -75.2    -9      960   17 08 45
17 12 06  ---          20 32 39  31.0  54.0 -5.0     -75.8   201     1012   17 08 37

17 12 36  J0132+4325   20 33 09  30.7  54.6 -5.0     -75.3    21     1012   17 12 36
17 14 06  =0129+431    20 34 40  30.9  54.6 -5.0     -75.5    90     1035   17 12 37

17 14 06  B0128+437    20 34 40  31.3  54.1 -5.0     -76.1    -9     1035   17 14 15
17 17 36  ---          20 38 10  31.9  54.3 -4.9     -76.6   201     1087   17 14 07

17 17 36  J0132+4325   20 38 10  31.5  54.8 -4.9     -76.0    -8     1087   17 17 44
17 19 06  =0129+431    20 39 41  31.8  54.9 -4.9     -76.2    82     1108   17 17 37

17 19 06  B0128+437    20 39 41  32.2  54.4 -4.9     -76.8    -9     1108   17 19 15
17 20 06  ---          20 40 41  32.4  54.4 -4.9     -76.9    51     1121   17 19 07

 ---------- Scan set 13 ----------

17 20 06  B0128+437    20 40 41  32.4  54.4 -4.9     -76.9    -6     1121   17 20 12
17 23 36  ---          20 44 11  33.0  54.6 -4.8     -77.5   204     1174   17 20 07

17 24 06  J0132+4325   20 44 41  32.7  55.1 -4.8     -77.0    22     1174   17 24 06
17 25 36  =0129+431    20 46 12  33.0  55.2 -4.8     -77.2    90     1197   17 24 07

17 25 36  B0128+437    20 46 12  33.3  54.7 -4.8     -77.8    -9     1197   17 25 45
17 29 06  ---          20 49 42  34.0  54.8 -4.7     -78.3   201     1249   17 25 37

17 29 06  J0132+4325   20 49 42  33.6  55.4 -4.7     -77.7    -8     1249   17 29 14
17 30 36  =0129+431    20 51 12  33.8  55.5 -4.7     -77.9    82     1270   17 29 07

 ---------- Scan set 13 ----------

17 30 36  B0128+437    20 51 12  34.2  54.9 -4.7     -78.5    -8     1270   17 30 44
17 34 06  ---          20 54 43  34.8  55.0 -4.6     -79.0   202     1322   17 30 37

17 34 36  J0132+4325   20 55 13  34.6  55.6 -4.6     -78.5    22     1322   17 34 36
17 36 06  =0129+431    20 56 43  34.8  55.7 -4.6     -78.7    90     1345   17 34 37

17 36 06  B0128+437    20 56 43  35.2  55.1 -4.6     -79.3    -8     1345   17 36 14
17 39 36  ---          21 00 14  35.8  55.3 -4.5     -79.9   202     1397   17 36 07
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

17 39 36  J0132+4325   21 00 14  35.4  55.8 -4.6     -79.3    -8     1397   17 39 44
17 41 06  =0129+431    21 01 44  35.7  55.9 -4.5     -79.5    82     1418   17 39 37

17 41 06  B0128+437    21 01 44  36.1  55.3 -4.5     -80.1    -8     1418   17 41 14
17 42 06  ---          21 02 44  36.3  55.3 -4.5     -80.2    52     1432   17 41 07

 ---------- Scan set 14 ----------

17 42 06  B0128+437    21 02 44  36.3  55.3 -4.5     -80.2    -6     1432   17 42 12
17 45 36  ---          21 06 15  36.9  55.5 -4.4     -80.8   204     1484   17 42 07

17 46 06  J0132+4325   21 06 45  36.6  56.1 -4.5     -80.2    22     1484   17 46 06
17 47 36  =0129+431    21 08 15  36.9  56.2 -4.4     -80.5    90     1507   17 46 07

17 47 36  B0128+437    21 08 15  37.2  55.5 -4.4     -81.1    -8     1507   17 47 44
17 51 06  ---          21 11 46  37.9  55.7 -4.3     -81.6   202     1559   17 47 37

17 51 06  J0132+4325   21 11 46  37.5  56.3 -4.4     -81.0    -8     1559   17 51 14
17 52 36  =0129+431    21 13 16  37.8  56.3 -4.3     -81.2    82     1581   17 51 07

 ---------- Scan set 14 ----------

17 52 36  B0128+437    21 13 16  38.1  55.7 -4.3     -81.9    -8     1581   17 52 44
17 56 06  ---          21 16 47  38.7  55.8 -4.3     -82.4   202     1633   17 52 37

17 56 36  J0132+4325   21 17 17  38.5  56.5 -4.3     -81.8    22     1633   17 56 36
17 58 06  =0129+431    21 18 47  38.8  56.5 -4.3     -82.0    90     1656   17 56 37

17 58 06  B0128+437    21 18 47  39.1  55.9 -4.2     -82.7    -8     1656   17 58 14
18 01 36  ---          21 22 18  39.7  56.0 -4.2     -83.3   202     1708   17 58 07

18 01 36  J0132+4325   21 22 18  39.4  56.6 -4.2     -82.6    -8     1708   18 01 44
18 03 06  =0129+431    21 23 48  39.7  56.7 -4.2     -82.8    82     1729   18 01 37

18 03 06  B0128+437    21 23 48  40.0  56.0 -4.1     -83.5    -8     1729   18 03 14
18 04 06  ---          21 24 48  40.2  56.1 -4.1     -83.7    52     1742   18 03 07

 ---------- Scan set 15 ----------

18 04 06  B0128+437    21 24 48  40.2  56.1 -4.1     -83.7    -6     1742   18 04 12
18 07 36  ---          21 28 19  40.8  56.1 -4.1     -84.2   204     1795   18 04 07

18 08 06  J0132+4325   21 28 49  40.6  56.8 -4.1     -83.6    22     1795   18 08 06
18 09 36  =0129+431    21 30 19  40.8  56.9 -4.1     -83.8    90     1818   18 08 07
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

18 09 36  B0128+437    21 30 19  41.2  56.2 -4.0     -84.5    -8     1818   18 09 44
18 13 06  ---          21 33 49  41.8  56.3 -4.0     -85.1   202     1870   18 09 37

18 13 06  J0132+4325   21 33 49  41.5  57.0 -4.0     -84.4    -8     1870   18 13 14
18 14 36  =0129+431    21 35 20  41.7  57.0 -4.0     -84.6    82     1891   18 13 07

 ---------- Scan set 15 ----------

18 14 36  B0128+437    21 35 20  42.1  56.3 -4.0     -85.3    -8     1891   18 14 44
18 18 06  ---          21 38 50  42.7  56.4 -3.9     -85.9   202     1943   18 14 37

18 18 36  J0132+4325   21 39 20  42.5  57.1 -3.9     -85.2    22     1943   18 18 36
18 20 06  =0129+431    21 40 51  42.7  57.1 -3.9     -85.5    90     1967   18 18 37

18 20 06  B0128+437    21 40 51  43.0  56.4 -3.9     -86.2    -8     1967   18 20 14
18 23 36  ---          21 44 21  43.7  56.4 -3.8     -86.8   202     2019   18 20 07

18 23 36  J0132+4325   21 44 21  43.4  57.2 -3.8     -86.0    -8     2019   18 23 44
18 25 06  =0129+431    21 45 51  43.6  57.2 -3.8     -86.3    82     2040   18 23 37

18 25 06  B0128+437    21 45 51  43.9  56.5 -3.8     -87.0    -8     2040   18 25 14
18 26 06  ---          21 46 52  44.1  56.5 -3.8     -87.2    52     2053   18 25 07

 ---------- Scan set 16 ----------

18 26 06  B0128+437    21 46 52  44.1  56.5 -3.8     -87.2    -6     2053   18 26 12
18 29 36  ---          21 50 22  44.7  56.5 -3.7     -87.8   204     2106   18 26 07

18 30 06  J0132+4325   21 50 52  44.5  57.3 -3.7     -87.1    22     2106   18 30 06
18 31 36  =0129+431    21 52 22  44.8  57.3 -3.7     -87.3    90     2129   18 30 07

18 31 36  B0128+437    21 52 22  45.1  56.5 -3.7     -88.1    -8     2129   18 31 44
18 35 06  ---          21 55 53  45.7  56.6 -3.6     -88.7   202     2181   18 31 37

18 35 06  J0132+4325   21 55 53  45.5  57.3 -3.6     -87.9    -8     2181   18 35 14
18 36 36  =0129+431    21 57 23  45.7  57.3 -3.6     -88.2    82     2202   18 35 07

 ---------- Scan set 16 ----------

18 36 36  B0128+437    21 57 23  46.0  56.6 -3.6     -89.0    -8     2202   18 36 44
18 40 06  ---          22 00 54  46.6  56.6 -3.5     -89.6   202     2254   18 36 37

18 40 36  J0132+4325   22 01 24  46.4  57.4 -3.5     -88.8    22     2254   18 40 36
18 42 06  =0129+431    22 02 54  46.7  57.4 -3.5     -89.1    90     2277   18 40 37
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

18 42 06  B0128+437    22 02 54  47.0  56.6 -3.5     -89.9    -8     2277   18 42 14
18 45 36  ---          22 06 25  47.6  56.6 -3.4     -90.5   202     2329   18 42 07

18 45 36  J0132+4325   22 06 25  47.4  57.4 -3.5     -89.7    -8     2329   18 45 44
18 47 06  =0129+431    22 07 55  47.6  57.4 -3.4     -89.9    82     2350   18 45 37

18 47 06  B0128+437    22 07 55  47.9  56.6 -3.4     -90.8    -8     2350   18 47 14
18 48 06  ---          22 08 55  48.1  56.6 -3.4     -91.0    52     2364   18 47 07

 ---------- Scan set 17 ----------

18 48 06  B0128+437    22 08 55  48.1  56.6 -3.4     -91.0    -6     2364   18 48 12
18 51 36  ---          22 12 26  48.7  56.5 -3.3     -91.6   204     2416   18 48 07

18 52 06  J0132+4325   22 12 56  48.5  57.4 -3.4     -90.8    22     2416   18 52 06
18 53 36  =0129+431    22 14 26  48.8  57.4 -3.3     -91.1    90     2440   18 52 07

18 53 36  B0128+437    22 14 26  49.1  56.5 -3.3     -92.0    -8     2440   18 53 44
18 57 06  ---          22 17 57  49.7  56.5 -3.2     -92.6   202     2492   18 53 37

18 57 06  J0132+4325   22 17 57  49.4  57.3 -3.3     -91.7    -8     2492   18 57 14
18 58 36  =0129+431    22 19 27  49.7  57.3 -3.2     -92.0    82     2513   18 57 07

 ---------- Scan set 17 ----------

18 58 36  B0128+437    22 19 27  50.0  56.5 -3.2     -92.9    -8     2513   18 58 44
19 02 06  ---          22 22 57  50.6  56.4 -3.2     -93.5   202     2565   18 58 37

19 02 36  J0132+4325   22 23 28  50.4  57.3 -3.2     -92.7    22     2565   19 02 36
19 04 06  =0129+431    22 24 58  50.7  57.3 -3.2     -93.0    90     2588   19 02 37

19 04 06  B0128+437    22 24 58  51.0  56.4 -3.1     -93.9    -8     2588   19 04 14
19 07 36  ---          22 28 28  51.6  56.3 -3.1     -94.6   202     2640   19 04 07

19 07 36  J0132+4325   22 28 28  51.4  57.2 -3.1     -93.6    -8     2640   19 07 44
19 09 06  =0129+431    22 29 59  51.6  57.2 -3.1     -93.9    82     2661   19 07 37

19 09 06  B0128+437    22 29 59  51.9  56.3 -3.0     -94.9    -8     2661   19 09 14
19 10 06  ---          22 30 59  52.0  56.2 -3.0     -95.1    52     2675   19 09 07

 ---------- Scan set 18 ----------

19 10 06  B0128+437    22 30 59  52.0  56.2 -3.0     -95.1    -6     2675   19 10 12
19 13 06  ---          22 33 59  52.6  56.2 -3.0     -95.7   174     2719   19 10 07
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

19 13 36  J0132+4325   22 34 29  52.4  57.1 -3.0     -94.8    22     2719   19 13 36
19 15 06  =0129+431    22 36 00  52.7  57.0 -3.0     -95.0    90     2743   19 13 37

 ---------- Scan set 19 FF ----------

19 17 06  3C84         22 38 00  33.3  57.7 -4.7     -76.6    73     2743   19 17 06
19 20 06  ---          22 41 00  33.9  57.9 -4.7     -77.0   180     2789   19 17 07

19 22 06  J0132+4325   22 43 01  54.0  56.8 -2.9     -96.4    73     2789   19 22 06
19 23 36  =0129+431    22 44 31  54.2  56.8 -2.8     -96.7    90     2812   19 22 07

19 23 36  B0128+437    22 44 31  54.4  55.8 -2.8     -97.8    -8     2812   19 23 44
19 27 06  ---          22 48 02  55.1  55.6 -2.7     -98.5   202     2864   19 23 37

19 27 06  J0132+4325   22 48 02  54.9  56.6 -2.8     -97.4    -8     2864   19 27 14
19 28 36  =0129+431    22 49 32  55.1  56.6 -2.7     -97.8    82     2885   19 27 07

19 29 06  B0128+437    22 50 02  55.4  55.5 -2.7     -99.0    22     2885   19 29 06
19 31 06  ---          22 52 02  55.8  55.4 -2.7     -99.4   120     2916   19 29 07

19 31 06  B0128+437    22 52 02  55.8  55.4 -2.7     -99.4    -6     2916   19 31 12
19 32 06  ---          22 53 02  56.0  55.4 -2.7     -99.6    54     2930   19 31 07

 ---------- Scan set 21 ----------

19 34 06  J0132+4325   22 55 03  56.1  56.3 -2.7     -98.9   112     2930   19 34 06
19 36 36  =0129+431    22 57 33  56.6  56.2 -2.6     -99.5   150     2969   19 34 07

19 36 36  B0128+437    22 57 33  56.8  55.1 -2.6    -100.6    -8     2969   19 36 44
19 40 06  ---          23 01 04  57.4  54.9 -2.5    -101.4   202     3021   19 36 37

19 40 36  J0132+4325   23 01 34  57.3  56.0 -2.5    -100.3    22     3021   19 40 36
19 42 06  =0129+431    23 03 04  57.6  55.9 -2.5    -100.7    90     3044   19 40 37

19 42 06  B0128+437    23 03 04  57.7  54.8 -2.5    -101.9    -8     3044   19 42 14
19 45 36  ---          23 06 35  58.3  54.5 -2.4    -102.7   202     3096   19 42 07

19 45 36  J0132+4325   23 06 35  58.2  55.6 -2.5    -101.5    -8     3096   19 45 44
19 47 06  =0129+431    23 08 05  58.5  55.5 -2.4    -101.8    82     3117   19 45 37

19 47 06  B0128+437    23 08 05  58.6  54.4 -2.4    -103.0    -8     3117   19 47 14
19 48 06  ---          23 09 05  58.8  54.3 -2.4    -103.3    52     3131   19 47 07
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

 ---------- Scan set 22 ----------

19 48 06  B0128+437    23 09 05  58.8  54.3 -2.4    -103.3    -6     3131   19 48 12
19 51 36  ---          23 12 36  59.4  54.0 -2.3    -104.1   204     3183   19 48 07

19 52 06  J0132+4325   23 13 06  59.3  55.2 -2.4    -103.0    22     3183   19 52 06
19 53 36  =0129+431    23 14 36  59.6  55.0 -2.3    -103.4    90     3206   19 52 07

19 53 36  B0128+437    23 14 36  59.7  53.9 -2.3    -104.7    -9     3206   19 53 45
19 57 06  ---          23 18 07  60.4  53.5 -2.2    -105.5   201     3258   19 53 37

19 57 06  J0132+4325   23 18 07  60.2  54.7 -2.3    -104.2    -9     3258   19 57 15
20 00 00  =0129+431    23 21 01  60.7  54.5 -2.2    -105.0   165     3301   19 57 07

20 00 00  B0128+437    23 21 01  60.9  53.2 -2.2    -106.3    -9     3301   20 00 09
20 01 00  ---          23 22 01  61.0  53.1 -2.2    -106.6    51     3314   20 00 01

20 01 00  B0128+437    23 22 01  61.0  53.1 -2.2    -106.6    -6     3314   20 01 06
20 04 30  ---          23 25 32  61.6  52.7 -2.1    -107.5   204     3366   20 01 01

20 04 45  J0132+4325   23 25 47  61.6  54.0 -2.1    -106.2     6     3366   20 04 45
20 06 15  =0129+431    23 27 17  61.8  53.8 -2.1    -106.6    90     3389   20 04 46

20 06 15  B0128+437    23 27 17  61.9  52.5 -2.1    -108.0    -9     3389   20 06 24
20 09 45  ---          23 30 48  62.5  52.1 -2.0    -109.0   201     3441   20 06 16

20 09 45  J0132+4325   23 30 48  62.4  53.4 -2.1    -107.6    -9     3441   20 09 54
20 11 15  =0129+431    23 32 18  62.7  53.2 -2.0    -108.0    81     3462   20 09 46

20 11 15  B0128+437    23 32 18  62.8  51.9 -2.0    -109.4    -9     3462   20 11 24
20 14 45  ---          23 35 48  63.4  51.4 -1.9    -110.5   201     3514   20 11 16

20 15 00  J0132+4325   23 36 03  63.3  52.8 -2.0    -109.1     6     3514   20 15 00
20 16 30  =0129+431    23 37 34  63.6  52.6 -1.9    -109.5    90     3537   20 15 01

20 16 30  B0128+437    23 37 34  63.7  51.2 -1.9    -111.0    -9     3537   20 16 39
20 20 00  ---          23 41 04  64.3  50.7 -1.9    -112.1   201     3589   20 16 31

20 20 00  J0132+4325   23 41 04  64.2  52.1 -1.9    -110.6    -9     3589   20 20 09
20 21 30  =0129+431    23 42 35  64.5  51.8 -1.9    -111.0    81     3610   20 20 01

20 21 30  B0128+437    23 42 35  64.5  50.4 -1.8    -112.6    -9     3610   20 21 39
20 22 30  ---          23 43 35  64.7  50.3 -1.8    -112.9    51     3623   20 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

20 22 30  B0128+437    23 43 35  64.7  50.3 -1.8    -112.9    -6     3623   20 22 36
20 26 00  ---          23 47 05  65.3  49.7 -1.8    -114.0   204     3675   20 22 31

20 26 15  J0132+4325   23 47 20  65.3  51.1 -1.8    -112.5     6     3675   20 26 15
20 27 45  =0129+431    23 48 51  65.5  50.8 -1.8    -113.0    90     3699   20 26 16

20 27 45  B0128+437    23 48 51  65.5  49.4 -1.7    -114.6    -9     3699   20 27 54
20 31 15  ---          23 52 21  66.1  48.7 -1.7    -115.8   201     3750   20 27 46

20 31 15  J0132+4325   23 52 21  66.1  50.2 -1.7    -114.2    -9     3750   20 31 24
20 32 45  =0129+431    23 53 51  66.3  49.9 -1.7    -114.7    81     3771   20 31 16

20 32 45  B0128+437    23 53 51  66.4  48.4 -1.6    -116.3    -9     3771   20 32 54
20 36 15  ---          23 57 22  66.9  47.7 -1.6    -117.6   201     3823   20 32 46

20 36 30  J0132+4325   23 57 37  67.0  49.2 -1.6    -116.0     6     3823   20 36 30
20 38 00  =0129+431    23 59 07  67.2  48.9 -1.6    -116.6    90     3846   20 36 31

20 38 00  B0128+437    23 59 07  67.2  47.3 -1.6    -118.3    -9     3846   20 38 09
20 41 30  ---          00 02 38  67.7  46.5 -1.5    -119.6   201     3898   20 38 01

20 41 30  J0132+4325   00 02 38  67.8  48.1 -1.5    -117.9    -9     3898   20 41 39
20 43 00  =0129+431    00 04 08  68.0  47.8 -1.5    -118.4    81     3919   20 41 31

20 43 00  B0128+437    00 04 08  68.0  46.2 -1.5    -120.2    -9     3919   20 43 09
20 44 00  ---          00 05 08  68.1  45.9 -1.5    -120.6    51     3932   20 43 01

20 44 00  B0128+437    00 05 08  68.1  45.9 -1.5    -120.6    -6     3932   20 44 06
20 47 30  ---          00 08 39  68.7  45.0 -1.4    -122.1   204     3985   20 44 01

20 47 45  J0132+4325   00 08 54  68.8  46.6 -1.4    -120.3     6     3985   20 47 45
20 49 15  =0129+431    00 10 24  69.0  46.3 -1.4    -121.0    90     4008   20 47 46

20 49 15  B0128+437    00 10 24  68.9  44.6 -1.4    -122.8    -9     4008   20 49 24
20 52 45  ---          00 13 55  69.5  43.6 -1.3    -124.3   201     4060   20 49 16

20 52 45  J0132+4325   00 13 55  69.5  45.3 -1.3    -122.4    -9     4060   20 52 54
20 54 15  =0129+431    00 15 25  69.8  44.9 -1.3    -123.1    81     4080   20 52 46

20 54 15  B0128+437    00 15 25  69.7  43.1 -1.3    -125.0    -9     4080   20 54 24
20 57 45  ---          00 18 55  70.2  42.1 -1.2    -126.6   201     4132   20 54 16

20 58 00  J0132+4325   00 19 11  70.3  43.8 -1.2    -124.8     6     4132   20 58 00
20 59 30  =0129+431    00 20 41  70.6  43.3 -1.2    -125.5    90     4155   20 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

20 59 30  B0128+437    00 20 41  70.4  41.5 -1.2    -127.4    -9     4155   20 59 39
21 03 00  ---          00 24 11  70.9  40.3 -1.1    -129.2   201     4207   20 59 31

21 03 00  J0132+4325   00 24 11  71.1  42.2 -1.2    -127.2    -9     4207   21 03 09
21 04 30  =0129+431    00 25 42  71.3  41.6 -1.1    -127.9    81     4228   21 03 01

21 04 30  B0128+437    00 25 42  71.1  39.8 -1.1    -129.9    -9     4228   21 04 39
21 05 30  ---          00 26 42  71.3  39.4 -1.1    -130.5    51     4241   21 04 31

21 05 30  B0128+437    00 26 42  71.3  39.4 -1.1    -130.5    -6     4241   21 05 36
21 09 00  ---          00 30 12  71.8  38.1 -1.0    -132.3   204     4294   21 05 31

21 09 15  J0132+4325   00 30 27  71.9  39.9 -1.1    -130.4     6     4294   21 09 15
21 10 45  =0129+431    00 31 58  72.2  39.3 -1.0    -131.2    90     4317   21 09 16

21 10 45  B0128+437    00 31 58  72.0  37.4 -1.0    -133.3    -9     4317   21 10 54
21 14 15  ---          00 35 28  72.4  36.0 -1.0    -135.3   201     4369   21 10 46

21 14 15  J0132+4325   00 35 28  72.6  37.9 -1.0    -133.1    -9     4369   21 14 24
21 15 45  =0129+431    00 36 58  72.8  37.3 -1.0    -134.0    81     4390   21 14 16

21 15 45  B0128+437    00 36 58  72.6  35.3 -0.9    -136.1    -9     4390   21 15 54
21 19 15  ---          00 40 29  73.1  33.8 -0.9    -138.2   201     4441   21 15 46

21 19 30  J0132+4325   00 40 44  73.3  35.6 -0.9    -136.2     6     4441   21 19 30
21 21 00  =0129+431    00 42 14  73.5  34.9 -0.9    -137.2    90     4465   21 19 31

21 21 00  B0128+437    00 42 14  73.3  33.0 -0.8    -139.3    -9     4465   21 21 09
21 24 30  ---          00 45 45  73.7  31.3 -0.8    -141.6   201     4516   21 21 01

21 24 30  J0132+4325   00 45 45  73.9  33.2 -0.8    -139.4    -9     4516   21 24 39
21 26 00  =0129+431    00 47 15  74.1  32.5 -0.8    -140.4    81     4537   21 24 31

21 26 00  B0128+437    00 47 15  73.8  30.5 -0.8    -142.6    -9     4537   21 26 09
21 27 00  ---          00 48 15  73.9  30.0 -0.7    -143.2    51     4550   21 26 01

21 27 00  B0128+437    00 48 15  73.9  30.0 -0.7    -143.2    -6     4550   21 27 06
21 30 30  ---          00 51 46  74.3  28.1 -0.7    -145.6   204     4603   21 27 01

21 30 45  J0132+4325   00 52 01  74.6  30.0 -0.7    -143.6     6     4603   21 30 45
21 32 15  =0129+431    00 53 31  74.8  29.1 -0.7    -144.7    90     4626   21 30 46

21 32 15  B0128+437    00 53 31  74.5  27.1 -0.7    -146.9    -9     4626   21 32 24
21 35 45  ---          00 57 02  74.8  25.1 -0.6    -149.5   201     4678   21 32 16
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

21 35 45  J0132+4325   00 57 02  75.1  27.1 -0.6    -147.3    -9     4678   21 35 54
21 37 15  =0129+431    00 58 32  75.3  26.2 -0.6    -148.4    81     4699   21 35 46

21 37 15  B0128+437    00 58 32  75.0  24.2 -0.6    -150.6    -9     4699   21 37 24
21 40 45  ---          01 02 03  75.2  22.0 -0.5    -153.3   201     4751   21 37 16

21 41 00  J0132+4325   01 02 18  75.6  23.9 -0.5    -151.3     6     4751   21 41 00
21 42 30  =0129+431    01 03 48  75.8  22.9 -0.5    -152.5    90     4774   21 41 01

21 42 30  B0128+437    01 03 48  75.4  20.9 -0.5    -154.7    -9     4774   21 42 39
21 46 00  ---          01 07 18  75.6  18.6 -0.4    -157.5   201     4826   21 42 31

21 46 00  J0132+4325   01 07 18  76.0  20.5 -0.4    -155.4    -9     4826   21 46 09
21 47 30  =0129+431    01 08 49  76.1  19.5 -0.4    -156.7    81     4846   21 46 01

21 47 30  B0128+437    01 08 49  75.7  17.6 -0.4    -158.7    -9     4846   21 47 39
21 48 30  ---          01 09 49  75.8  16.9 -0.4    -159.6    51     4860   21 47 31

21 48 30  B0128+437    01 09 49  75.8  16.9 -0.4    -159.6    -6     4860   21 48 36
21 52 00  ---          01 13 19  76.0  14.5 -0.3    -162.6   204     4912   21 48 31

21 52 15  J0132+4325   01 13 34  76.5  16.1 -0.3    -160.8     6     4912   21 52 15
21 53 45  =0129+431    01 15 05  76.5  15.0 -0.3    -162.1    90     4935   21 52 16

21 53 45  B0128+437    01 15 05  76.1  13.2 -0.3    -164.1    -9     4935   21 53 54
21 57 15  ---          01 18 35  76.3  10.7 -0.2    -167.2   201     4987   21 53 46

21 57 15  J0132+4325   01 18 35  76.7  12.4 -0.3    -165.3    -9     4987   21 57 24
21 58 45  =0129+431    01 20 06  76.8  11.2 -0.2    -166.7    81     5008   21 57 16

21 58 45  B0128+437    01 20 06  76.3   9.6 -0.2    -168.5    -9     5008   21 58 54
22 02 15  ---          01 23 36  76.4   6.9 -0.2    -171.7   201     5060   21 58 46

22 02 30  J0132+4325   01 23 51  76.9   8.3 -0.2    -170.2     6     5060   22 02 30
22 04 00  =0129+431    01 25 21  77.0   7.1 -0.1    -171.6    90     5083   22 02 31

22 04 00  B0128+437    01 25 21  76.5   5.6 -0.1    -173.3    -9     5083   22 04 09
22 07 30  ---          01 28 52  76.5   2.9 -0.1    -176.5   201     5135   22 04 01

22 07 30  J0132+4325   01 28 52  77.0   4.3 -0.1    -174.9    -9     5135   22 07 39
22 09 00  =0129+431    01 30 22  77.1   3.1 -0.1    -176.4    81     5156   22 07 31

22 09 00  B0128+437    01 30 22  76.5   1.7 -0.0    -177.9    -9     5156   22 09 09
22 10 00  ---          01 31 22  76.5   1.0 -0.0    -178.8    51     5169   22 09 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

22 10 00  B0128+437    01 31 22  76.5   1.0 -0.0    -178.8    -6     5169   22 10 06
22 13 30  ---          01 34 53  76.5  -1.7  0.0     177.9   204     5221   22 10 01

22 13 45  J0132+4325   01 35 08  77.1  -0.8  0.0     179.0     6     5221   22 13 45
22 15 15  =0129+431    01 36 38  77.1  -2.0  0.0     177.6    90     5244   22 13 46

22 15 15  B0128+437    01 36 38  76.5  -3.1  0.1     176.3    -9     5244   22 15 24
22 18 45  ---          01 40 09  76.5  -5.8  0.1     173.1   201     5296   22 15 16

22 18 45  J0132+4325   01 40 09  77.0  -4.9  0.1     174.2    -9     5296   22 18 54
22 20 15  =0129+431    01 41 39  77.0  -6.1  0.1     172.8    81     5317   22 18 46

22 20 15  B0128+437    01 41 39  76.4  -6.9  0.2     171.7    -9     5317   22 20 24
22 23 45  ---          01 45 10  76.3  -9.5  0.2     168.5   201     5369   22 20 16

22 24 00  J0132+4325   01 45 25  76.9  -9.0  0.2     169.3     6     5369   22 24 00
22 25 30  =0129+431    01 46 55  76.8 -10.2  0.2     167.9    90     5392   22 24 01

22 25 30  B0128+437    01 46 55  76.2 -10.8  0.2     167.0    -9     5392   22 25 39
22 29 00  ---          01 50 25  76.1 -13.4  0.3     163.9   201     5444   22 25 31

22 29 00  J0132+4325   01 50 25  76.7 -12.9  0.3     164.6    -9     5444   22 29 09
22 30 30  =0129+431    01 51 56  76.6 -14.0  0.3     163.3    81     5465   22 29 01

22 30 30  B0128+437    01 51 56  76.0 -14.5  0.3     162.6    -9     5465   22 30 39
22 31 30  ---          01 52 56  76.0 -15.2  0.3     161.7    51     5478   22 30 31

22 31 30  B0128+437    01 52 56  76.0 -15.2  0.3     161.7    -6     5478   22 31 36
22 35 00  ---          01 56 26  75.7 -17.6  0.4     158.8   204     5530   22 31 31

22 35 15  J0132+4325   01 56 41  76.3 -17.5  0.4     159.0     6     5530   22 35 15
22 36 45  =0129+431    01 58 12  76.2 -18.6  0.4     157.7    90     5554   22 35 16

22 36 45  B0128+437    01 58 12  75.6 -18.8  0.4     157.3    -9     5554   22 36 54
22 40 15  ---          02 01 42  75.4 -21.1  0.5     154.5   201     5605   22 36 46

22 40 15  J0132+4325   02 01 42  76.0 -21.0  0.5     154.8    -9     5605   22 40 24
22 41 45  =0129+431    02 03 13  75.9 -22.0  0.5     153.6    81     5626   22 40 16

22 41 45  B0128+437    02 03 13  75.2 -22.0  0.5     153.3    -9     5626   22 41 54
22 45 15  ---          02 06 43  75.0 -24.2  0.6     150.6   201     5678   22 41 46

22 45 30  J0132+4325   02 06 58  75.5 -24.5  0.5     150.5     6     5678   22 45 30
22 47 00  =0129+431    02 08 28  75.4 -25.4  0.6     149.4    90     5701   22 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

22 47 00  B0128+437    02 08 28  74.8 -25.2  0.6     149.3    -9     5701   22 47 09
22 50 30  ---          02 11 59  74.5 -27.3  0.7     146.7   201     5753   22 47 01

22 50 30  J0132+4325   02 11 59  75.1 -27.5  0.6     146.7    -9     5753   22 50 39
22 52 00  =0129+431    02 13 29  74.9 -28.4  0.7     145.6    81     5774   22 50 31

22 52 00  B0128+437    02 13 29  74.3 -28.1  0.7     145.7    -9     5774   22 52 09
22 53 00  ---          02 14 29  74.2 -28.6  0.7     145.0    51     5787   22 52 01

22 53 00  B0128+437    02 14 29  74.2 -28.6  0.7     145.0    -6     5787   22 53 06
22 56 30  ---          02 18 00  73.8 -30.5  0.8     142.6   204     5840   22 53 01

22 56 45  J0132+4325   02 18 15  74.4 -31.0  0.7     142.3     6     5840   22 56 45
22 58 15  =0129+431    02 19 45  74.2 -31.8  0.8     141.2    90     5863   22 56 46

22 58 15  B0128+437    02 19 45  73.6 -31.4  0.8     141.4    -9     5863   22 58 24
23 01 45  ---          02 23 16  73.2 -33.1  0.8     139.2   201     5915   22 58 16

23 01 45  J0132+4325   02 23 16  73.8 -33.6  0.8     138.9    -9     5915   23 01 54
23 03 15  =0129+431    02 24 46  73.6 -34.3  0.8     138.0    81     5935   23 01 46

23 03 15  B0128+437    02 24 46  73.1 -33.8  0.9     138.2    -9     5935   23 03 24
23 06 45  ---          02 28 17  72.6 -35.3  0.9     136.1   201     5987   23 03 16

23 07 00  J0132+4325   02 28 32  73.2 -36.1  0.9     135.6     6     5987   23 07 00
23 08 30  =0129+431    02 30 02  73.0 -36.7  0.9     134.8    90     6010   23 07 01

23 08 30  B0128+437    02 30 02  72.4 -36.1  1.0     135.1    -9     6010   23 08 39
23 12 00  ---          02 33 33  72.0 -37.5  1.0     133.1   201     6062   23 08 31

23 12 00  J0132+4325   02 33 33  72.5 -38.2  1.0     132.7    -9     6062   23 12 09
23 13 30  =0129+431    02 35 03  72.3 -38.8  1.0     131.9    81     6083   23 12 01

23 13 30  B0128+437    02 35 03  71.8 -38.1  1.0     132.3    -9     6083   23 13 39
23 14 30  ---          02 36 03  71.6 -38.5  1.1     131.8    51     6096   23 13 31

23 14 30  B0128+437    02 36 03  71.6 -38.5  1.1     131.8    -6     6096   23 14 36
23 18 00  ---          02 39 34  71.2 -39.8  1.1     129.9   204     6149   23 14 31

23 18 15  J0132+4325   02 39 49  71.7 -40.6  1.1     129.3     6     6149   23 18 15
23 19 45  =0129+431    02 41 19  71.5 -41.2  1.1     128.6    90     6172   23 18 16

23 19 45  B0128+437    02 41 19  70.9 -40.4  1.1     129.1    -9     6172   23 19 54
23 23 15  ---          02 44 49  70.4 -41.6  1.2     127.3   201     6224   23 19 46
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

23 23 15  J0132+4325   02 44 49  71.0 -42.4  1.2     126.8    -9     6224   23 23 24
23 24 45  =0129+431    02 46 20  70.7 -42.9  1.2     126.1    81     6245   23 23 16

23 24 45  B0128+437    02 46 20  70.2 -42.1  1.2     126.6    -9     6245   23 24 54
23 28 15  ---          02 49 50  69.7 -43.1  1.3     125.0   201     6296   23 24 46

23 28 30  J0132+4325   02 50 05  70.2 -44.1  1.3     124.3     6     6296   23 28 30
23 30 00  =0129+431    02 51 35  70.0 -44.5  1.3     123.7    90     6320   23 28 31

23 30 00  B0128+437    02 51 35  69.4 -43.6  1.3     124.2    -9     6320   23 30 09
23 33 30  ---          02 55 06  68.9 -44.6  1.4     122.7   201     6371   23 30 01

23 33 30  J0132+4325   02 55 06  69.4 -45.5  1.3     122.1    -9     6371   23 33 39
23 35 00  =0129+431    02 56 36  69.2 -45.9  1.4     121.5    81     6392   23 33 31

23 35 00  B0128+437    02 56 36  68.7 -45.0  1.4     122.1    -9     6392   23 35 09
23 36 00  ---          02 57 36  68.5 -45.3  1.4     121.6    51     6405   23 35 01

23 36 00  B0128+437    02 57 36  68.5 -45.3  1.4     121.6    -6     6405   23 36 06
23 39 30  ---          03 01 07  68.0 -46.2  1.5     120.2   204     6458   23 36 01

23 39 45  J0132+4325   03 01 22  68.4 -47.1  1.5     119.5     6     6458   23 39 45
23 41 15  =0129+431    03 02 52  68.2 -47.5  1.5     118.9    90     6481   23 39 46

23 41 15  B0128+437    03 02 52  67.7 -46.6  1.5     119.5    -9     6481   23 41 24
23 44 45  ---          03 06 23  67.2 -47.4  1.6     118.2   201     6533   23 41 16

23 44 45  J0132+4325   03 06 23  67.6 -48.3  1.5     117.6    -9     6533   23 44 54
23 46 15  =0129+431    03 07 53  67.4 -48.6  1.6     117.0    81     6554   23 44 46

 ---------- Scan set 34 FF ----------

23 47 45  3C84         03 09 23  78.8  11.6 -0.2    -166.6    39     6554   23 47 45
23 50 45  ---          03 12 24  78.9   8.8 -0.1    -169.9   180     6600   23 47 46

23 52 15  J0132+4325   03 13 54  66.4 -49.8  1.7     114.9    41     6600   23 52 15
23 53 45  =0129+431    03 15 24  66.2 -50.1  1.7     114.4    90     6623   23 52 16

23 53 45  B0128+437    03 15 24  65.7 -49.2  1.7     115.0    -9     6623   23 53 54
23 56 45  ---          03 18 25  65.2 -49.7  1.8     113.9   171     6667   23 53 46

23 56 45  J0132+4325   03 18 25  65.7 -50.7  1.7     113.3    -9     6667   23 56 54
23 58 15  =0129+431    03 19 55  65.4 -50.9  1.8     112.9    81     6688   23 56 46
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  24 Feb 2024   Day  55 ---

23 58 15  B0128+437    03 19 55  65.0 -50.0  1.8     113.4    -9     6688   23 58 24
23 59 15  ---          03 20 55  64.8 -50.1  1.8     113.1    51     6701   23 58 16

 --- Start: Sat  24 Feb 2024   Day  55 -- Stop: Sun  25 Feb 2024   Day  56 ---

23 59 15  B0128+437    03 20 55  64.8 -50.1  1.8     113.1    -6     6701   23 59 21
00 02 45  ---          03 24 26  64.2 -50.7  1.9     112.0   204     6754   23 59 16

00 03 00  J0132+4325   03 24 41  64.6 -51.7  1.8     111.3     6     6754   00 03 00
00 04 30  =0129+431    03 26 11  64.4 -51.9  1.9     110.9    90     6777   00 03 01

00 04 30  B0128+437    03 26 11  63.9 -51.0  1.9     111.5    -9     6777   00 04 39
00 08 00  ---          03 29 42  63.3 -51.5  2.0     110.4   201     6829   00 04 31

00 08 00  J0132+4325   03 29 42  63.8 -52.4  1.9     109.8    -9     6829   00 08 09
00 09 30  =0129+431    03 31 12  63.5 -52.6  2.0     109.4    81     6850   00 08 01

00 09 30  B0128+437    03 31 12  63.1 -51.7  2.0     109.9    -9     6850   00 09 39
00 13 00  ---          03 34 43  62.5 -52.1  2.0     108.9   201     6902   00 09 31

00 13 15  J0132+4325   03 34 58  62.9 -53.1  2.0     108.3     6     6902   00 13 15
00 14 45  =0129+431    03 36 28  62.6 -53.3  2.0     107.9    90     6925   00 13 16

00 14 45  B0128+437    03 36 28  62.2 -52.4  2.1     108.4    -9     6925   00 14 54
00 18 15  ---          03 39 58  61.6 -52.8  2.1     107.5   201     6977   00 14 46

00 18 15  J0132+4325   03 39 58  62.0 -53.7  2.1     106.9    -9     6977   00 18 24
00 19 45  =0129+431    03 41 29  61.8 -53.9  2.1     106.5    81     6997   00 18 16

00 19 45  B0128+437    03 41 29  61.3 -52.9  2.1     107.0    -9     6997   00 19 54
00 20 45  ---          03 42 29  61.2 -53.0  2.2     106.8    51     7011   00 19 46

00 20 45  B0128+437    03 42 29  61.2 -53.0  2.2     106.8    -6     7011   00 20 51
00 24 15  ---          03 45 59  60.6 -53.4  2.2     105.8   204     7063   00 20 46

00 24 30  J0132+4325   03 46 14  60.9 -54.4  2.2     105.2     6     7063   00 24 30
00 26 00  =0129+431    03 47 45  60.7 -54.5  2.2     104.9    90     7086   00 24 31

00 26 00  B0128+437    03 47 45  60.3 -53.6  2.3     105.4    -9     7086   00 26 09
00 29 30  ---          03 51 15  59.6 -53.9  2.3     104.5   201     7138   00 26 01

00 29 30  J0132+4325   03 51 15  60.0 -54.8  2.3     104.0    -9     7138   00 29 39
00 31 00  =0129+431    03 52 46  59.8 -55.0  2.3     103.6    81     7159   00 29 31
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

00 31 00  B0128+437    03 52 46  59.4 -54.0  2.3     104.1    -9     7159   00 31 09
00 34 30  ---          03 56 16  58.8 -54.3  2.4     103.3   201     7211   00 31 01

00 34 45  J0132+4325   03 56 31  59.1 -55.3  2.4     102.7     7     7211   00 34 45
00 36 15  =0129+431    03 58 01  58.8 -55.4  2.4     102.3    90     7234   00 34 46

00 36 15  B0128+437    03 58 01  58.5 -54.5  2.4     102.8    -9     7234   00 36 24
00 39 45  ---          04 01 32  57.8 -54.7  2.5     102.0   201     7286   00 36 16

00 39 45  J0132+4325   04 01 32  58.2 -55.6  2.5     101.5    -8     7286   00 39 53
00 41 15  =0129+431    04 03 02  58.0 -55.7  2.5     101.2    82     7307   00 39 46

00 41 15  B0128+437    04 03 02  57.6 -54.8  2.5     101.7    -8     7307   00 41 23
00 42 15  ---          04 04 02  57.4 -54.9  2.5     101.4    52     7320   00 41 16

00 42 15  B0128+437    04 04 02  57.4 -54.9  2.5     101.4    -6     7320   00 42 21
00 45 45  ---          04 07 33  56.8 -55.1  2.6     100.6   204     7373   00 42 16

00 46 00  J0132+4325   04 07 48  57.1 -56.0  2.6     100.1     7     7373   00 46 00
00 47 30  =0129+431    04 09 18  56.8 -56.1  2.6      99.8    90     7396   00 46 01

00 47 30  B0128+437    04 09 18  56.5 -55.2  2.6     100.2    -8     7396   00 47 38
00 51 00  ---          04 12 49  55.9 -55.4  2.7      99.5   202     7448   00 47 31

00 51 00  J0132+4325   04 12 49  56.2 -56.3  2.6      99.0    -8     7448   00 51 08
00 52 30  =0129+431    04 14 19  55.9 -56.4  2.7      98.7    82     7469   00 51 01

00 52 30  B0128+437    04 14 19  55.6 -55.5  2.7      99.2    -8     7469   00 52 38
00 56 00  ---          04 17 50  55.0 -55.7  2.8      98.4   202     7521   00 52 31

00 56 15  J0132+4325   04 18 05  55.3 -56.5  2.7      97.9     7     7521   00 56 15
00 57 45  =0129+431    04 19 35  55.0 -56.6  2.8      97.6    90     7544   00 56 16

00 57 45  B0128+437    04 19 35  54.7 -55.7  2.8      98.0    -8     7544   00 57 53
01 01 15  ---          04 23 05  54.0 -55.9  2.8      97.3   202     7596   00 57 46

01 01 15  J0132+4325   04 23 05  54.4 -56.8  2.8      96.9    -8     7596   01 01 23
01 02 45  =0129+431    04 24 36  54.1 -56.8  2.8      96.6    82     7618   01 01 16

01 02 45  B0128+437    04 24 36  53.8 -55.9  2.9      97.0    -8     7618   01 02 53
01 03 45  ---          04 25 36  53.6 -56.0  2.9      96.8    52     7631   01 02 46

01 03 45  B0128+437    04 25 36  53.6 -56.0  2.9      96.8    -6     7631   01 03 51
01 07 15  ---          04 29 06  53.0 -56.1  2.9      96.1   204     7684   01 03 46
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

01 07 30  J0132+4325   04 29 22  53.2 -57.0  2.9      95.6     7     7684   01 07 30
01 09 00  =0129+431    04 30 52  53.0 -57.0  2.9      95.3    90     7707   01 07 31

01 09 00  B0128+437    04 30 52  52.6 -56.1  3.0      95.7    -8     7707   01 09 08
01 12 30  ---          04 34 22  52.0 -56.2  3.0      95.1   202     7759   01 09 01

01 12 30  J0132+4325   04 34 22  52.3 -57.1  3.0      94.6    -8     7759   01 12 38
01 14 00  =0129+431    04 35 53  52.1 -57.1  3.0      94.4    82     7780   01 12 31

01 14 00  B0128+437    04 35 53  51.7 -56.3  3.1      94.8    -8     7780   01 14 08
01 17 30  ---          04 39 23  51.1 -56.4  3.1      94.1   202     7832   01 14 01

01 17 45  J0132+4325   04 39 38  51.4 -57.2  3.1      93.6     7     7832   01 17 45
01 19 15  =0129+431    04 41 08  51.1 -57.2  3.1      93.4    90     7855   01 17 46

01 19 15  B0128+437    04 41 08  50.8 -56.4  3.1      93.8    -8     7855   01 19 23
01 22 45  ---          04 44 39  50.2 -56.5  3.2      93.1   202     7907   01 19 16

01 22 45  J0132+4325   04 44 39  50.5 -57.3  3.2      92.7    -8     7907   01 22 53
01 24 15  =0129+431    04 46 09  50.2 -57.3  3.2      92.4    82     7928   01 22 46

01 24 15  B0128+437    04 46 09  49.9 -56.5  3.2      92.8    -8     7928   01 24 23
01 25 15  ---          04 47 09  49.7 -56.5  3.2      92.6    52     7942   01 24 16

01 25 15  B0128+437    04 47 09  49.7 -56.5  3.2      92.6    -6     7942   01 25 21
01 28 45  ---          04 50 40  49.1 -56.5  3.3      92.0   204     7994   01 25 16

01 29 00  J0132+4325   04 50 55  49.3 -57.4  3.3      91.6     7     7994   01 29 00
01 30 30  =0129+431    04 52 25  49.1 -57.4  3.3      91.3    90     8017   01 29 01

01 30 30  B0128+437    04 52 25  48.8 -56.5  3.3      91.7    -8     8017   01 30 38
01 34 00  ---          04 55 56  48.2 -56.6  3.4      91.1   202     8069   01 30 31

01 34 00  J0132+4325   04 55 56  48.4 -57.4  3.4      90.7    -8     8069   01 34 08
01 35 30  =0129+431    04 57 26  48.2 -57.4  3.4      90.4    82     8091   01 34 01

01 35 30  B0128+437    04 57 26  47.9 -56.6  3.4      90.8    -8     8091   01 35 38
01 39 00  ---          05 00 57  47.3 -56.6  3.5      90.2   202     8143   01 35 31

01 39 15  J0132+4325   05 01 12  47.5 -57.4  3.5      89.8     7     8143   01 39 15
01 40 45  =0129+431    05 02 42  47.2 -57.4  3.5      89.5    90     8166   01 39 16

01 40 45  B0128+437    05 02 42  46.9 -56.6  3.5      89.9    -8     8166   01 40 53
01 44 15  ---          05 06 13  46.3 -56.6  3.6      89.3   202     8218   01 40 46
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

01 44 15  J0132+4325   05 06 13  46.6 -57.4  3.5      88.9    -8     8218   01 44 23
01 45 45  =0129+431    05 07 43  46.3 -57.4  3.6      88.7    82     8239   01 44 16

01 45 45  B0128+437    05 07 43  46.0 -56.6  3.6      89.0    -8     8239   01 45 53
01 46 45  ---          05 08 43  45.9 -56.6  3.6      88.8    52     8252   01 45 46

01 46 45  B0128+437    05 08 43  45.9 -56.6  3.6      88.8    -6     8252   01 46 51
01 50 15  ---          05 12 14  45.2 -56.5  3.7      88.2   204     8305   01 46 46

01 50 30  J0132+4325   05 12 29  45.4 -57.3  3.6      87.9     7     8305   01 50 30
01 52 00  =0129+431    05 13 59  45.2 -57.3  3.7      87.6    90     8328   01 50 31

01 52 00  B0128+437    05 13 59  44.9 -56.5  3.7      87.9    -8     8328   01 52 08
01 55 30  ---          05 17 29  44.3 -56.5  3.7      87.4   202     8380   01 52 01

01 55 30  J0132+4325   05 17 29  44.5 -57.3  3.7      87.1    -8     8380   01 55 38
01 57 00  =0129+431    05 19 00  44.3 -57.2  3.7      86.8    82     8401   01 55 31

01 57 00  B0128+437    05 19 00  44.0 -56.5  3.8      87.1    -8     8401   01 57 08
02 00 30  ---          05 22 30  43.4 -56.4  3.8      86.5   202     8453   01 57 01

02 00 45  J0132+4325   05 22 45  43.6 -57.2  3.8      86.2     7     8453   02 00 45
02 02 15  =0129+431    05 24 16  43.3 -57.2  3.8      86.0    90     8477   02 00 46

02 02 15  B0128+437    05 24 16  43.1 -56.4  3.9      86.2    -8     8477   02 02 23
02 05 45  ---          05 27 46  42.4 -56.3  3.9      85.7   202     8529   02 02 16

02 05 45  J0132+4325   05 27 46  42.7 -57.1  3.9      85.4    -8     8529   02 05 53
02 07 15  =0129+431    05 29 16  42.4 -57.1  3.9      85.2    82     8550   02 05 46

02 07 15  B0128+437    05 29 16  42.2 -56.3  3.9      85.4    -8     8550   02 07 23
02 08 15  ---          05 30 16  42.0 -56.3  4.0      85.3    52     8563   02 07 16

02 08 15  B0128+437    05 30 16  42.0 -56.3  4.0      85.3    -6     8563   02 08 21
02 11 45  ---          05 33 47  41.4 -56.2  4.0      84.7   204     8616   02 08 16

02 12 00  J0132+4325   05 34 02  41.5 -57.0  4.0      84.4     7     8616   02 12 00
02 13 30  =0129+431    05 35 32  41.3 -56.9  4.0      84.2    90     8639   02 12 01

02 13 30  B0128+437    05 35 32  41.1 -56.2  4.0      84.4    -8     8639   02 13 38
02 17 00  ---          05 39 03  40.4 -56.1  4.1      83.9   202     8691   02 13 31

02 17 00  J0132+4325   05 39 03  40.6 -56.8  4.1      83.6    -8     8691   02 17 08
02 18 30  =0129+431    05 40 33  40.4 -56.8  4.1      83.4    82     8712   02 17 01
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

02 18 30  B0128+437    05 40 33  40.2 -56.1  4.1      83.6    -8     8712   02 18 38
02 22 00  ---          05 44 04  39.5 -56.0  4.2      83.1   202     8764   02 18 31

02 22 15  J0132+4325   05 44 19  39.7 -56.7  4.2      82.8     7     8764   02 22 15
02 23 45  =0129+431    05 45 49  39.4 -56.6  4.2      82.6    90     8787   02 22 16

02 23 45  B0128+437    05 45 49  39.2 -55.9  4.2      82.8    -8     8787   02 23 53
02 27 15  ---          05 49 20  38.6 -55.8  4.3      82.3   202     8839   02 23 46

02 27 15  J0132+4325   05 49 20  38.8 -56.5  4.3      82.1    -8     8839   02 27 23
02 28 45  =0129+431    05 50 50  38.5 -56.5  4.3      81.8    82     8860   02 27 16

02 28 45  B0128+437    05 50 50  38.3 -55.8  4.3      82.0    -8     8860   02 28 53
02 29 45  ---          05 51 50  38.1 -55.7  4.3      81.9    52     8874   02 28 46

02 29 45  B0128+437    05 51 50  38.1 -55.7  4.3      81.9    -6     8874   02 29 51
02 33 15  ---          05 55 21  37.5 -55.6  4.4      81.3   204     8926   02 29 46

02 33 30  J0132+4325   05 55 36  37.7 -56.3  4.4      81.1     7     8926   02 33 30
02 35 00  =0129+431    05 57 06  37.4 -56.3  4.4      80.9    90     8950   02 33 31

02 35 00  B0128+437    05 57 06  37.2 -55.5  4.4      81.1    -8     8950   02 35 08
02 38 30  ---          06 00 36  36.6 -55.4  4.5      80.5   202     9002   02 35 01

02 38 30  J0132+4325   06 00 36  36.8 -56.1  4.4      80.4    -8     9002   02 38 38
02 40 00  =0129+431    06 02 07  36.5 -56.1  4.5      80.1    82     9023   02 38 31

02 40 00  B0128+437    06 02 07  36.3 -55.4  4.5      80.3    -8     9023   02 40 08
02 43 30  ---          06 05 37  35.7 -55.2  4.5      79.8   202     9075   02 40 01

02 43 45  J0132+4325   06 05 52  35.8 -55.9  4.5      79.6     7     9075   02 43 45
02 45 15  =0129+431    06 07 23  35.6 -55.9  4.6      79.4    90     9098   02 43 46

02 45 15  B0128+437    06 07 23  35.4 -55.2  4.6      79.5    -8     9098   02 45 23
02 48 45  ---          06 10 53  34.8 -55.0  4.6      79.0   202     9150   02 45 16

02 48 45  J0132+4325   06 10 53  34.9 -55.7  4.6      78.8    -8     9150   02 48 53
02 50 15  =0129+431    06 12 23  34.7 -55.7  4.6      78.6    82     9171   02 48 46

02 50 15  B0128+437    06 12 23  34.5 -55.0  4.7      78.8    -8     9171   02 50 23
02 51 15  ---          06 13 24  34.3 -54.9  4.7      78.6    52     9185   02 50 16

02 51 15  B0128+437    06 13 24  34.3 -54.9  4.7      78.6    -6     9185   02 51 21
02 54 45  ---          06 16 54  33.7 -54.8  4.7      78.1   204     9237   02 51 16
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

02 55 00  J0132+4325   06 17 09  33.8 -55.5  4.7      77.9     7     9237   02 55 00
02 56 30  =0129+431    06 18 39  33.6 -55.4  4.7      77.7    90     9260   02 55 01

02 56 30  B0128+437    06 18 39  33.4 -54.7  4.8      77.8    -8     9260   02 56 38
03 00 00  ---          06 22 10  32.8 -54.5  4.8      77.3   202     9312   02 56 31

03 00 00  J0132+4325   06 22 10  32.9 -55.2  4.8      77.2    -8     9312   03 00 08
03 01 30  =0129+431    06 23 40  32.7 -55.1  4.8      77.0    82     9333   03 00 01

03 01 30  B0128+437    06 23 40  32.5 -54.4  4.9      77.1    -8     9333   03 01 38
03 05 00  ---          06 27 11  31.9 -54.3  4.9      76.6   202     9386   03 01 31

03 05 15  J0132+4325   06 27 26  32.0 -55.0  4.9      76.4     7     9386   03 05 15
03 06 45  =0129+431    06 28 56  31.7 -54.9  4.9      76.2    90     9409   03 05 16

03 06 45  B0128+437    06 28 56  31.6 -54.2  4.9      76.3    -8     9409   03 06 53
03 10 15  ---          06 32 27  31.0 -54.0  5.0      75.8   202     9461   03 06 46

03 10 15  J0132+4325   06 32 27  31.1 -54.7  5.0      75.7    -8     9461   03 10 23
03 11 45  =0129+431    06 33 57  30.9 -54.6  5.0      75.5    82     9482   03 10 16

03 11 45  B0128+437    06 33 57  30.7 -53.9  5.0      75.6    -8     9482   03 11 53
03 12 45  ---          06 34 57  30.6 -53.9  5.0      75.4    52     9495   03 11 46

03 12 45  B0128+437    06 34 57  30.6 -53.9  5.0      75.4    -6     9495   03 12 51
03 16 15  ---          06 38 28  30.0 -53.7  5.1      74.9   204     9548   03 12 46

03 16 30  J0132+4325   06 38 43  30.0 -54.4  5.1      74.8     7     9548   03 16 30
03 18 00  =0129+431    06 40 13  29.8 -54.3  5.1      74.6    90     9571   03 16 31

03 18 00  B0128+437    06 40 13  29.6 -53.6  5.1      74.6    -8     9571   03 18 08
03 21 30  ---          06 43 44  29.0 -53.4  5.2      74.1   202     9623   03 18 01

03 21 30  J0132+4325   06 43 44  29.2 -54.1  5.2      74.1    -8     9623   03 21 38
03 23 00  =0129+431    06 45 14  28.9 -54.0  5.2      73.8    82     9644   03 21 31

03 23 00  B0128+437    06 45 14  28.8 -53.3  5.2      73.9    -8     9644   03 23 08
03 26 30  ---          06 48 44  28.2 -53.1  5.3      73.4   202     9696   03 23 01

03 26 45  J0132+4325   06 48 59  28.2 -53.8  5.2      73.3     7     9696   03 26 45
03 28 15  =0129+431    06 50 30  28.0 -53.7  5.3      73.1    90     9719   03 26 46

03 28 15  B0128+437    06 50 30  27.9 -53.0  5.3      73.1    -8     9719   03 28 23
03 31 45  ---          06 54 00  27.3 -52.8  5.4      72.6   202     9771   03 28 16
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GW023A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  25 Feb 2024   Day  56 ---

03 31 45  J0132+4325   06 54 00  27.4 -53.5  5.3      72.6    -8     9771   03 31 53
03 33 15  =0129+431    06 55 30  27.1 -53.4  5.4      72.4    82     9793   03 31 46

03 33 15  B0128+437    06 55 30  27.0 -52.7  5.4      72.4    -8     9793   03 33 23
03 34 15  ---          06 56 31  26.8 -52.7  5.4      72.3    52     9806   03 33 16

03 34 15  B0128+437    06 56 31  26.8 -52.7  5.4      72.3    -6     9806   03 34 21
03 37 45  ---          07 00 01  26.2 -52.4  5.5      71.7   204     9859   03 34 16

03 38 00  J0132+4325   07 00 16  26.3 -53.1  5.4      71.7     7     9859   03 38 00
03 39 30  =0129+431    07 01 46  26.0 -53.0  5.5      71.4    90     9882   03 38 01

03 39 30  B0128+437    07 01 46  25.9 -52.3  5.5      71.5    -8     9882   03 39 38
03 43 00  ---          07 05 17  25.4 -52.1  5.5      71.0   202     9934   03 39 31

03 43 00  J0132+4325   07 05 17  25.4 -52.8  5.5      70.9    -8     9934   03 43 08
03 44 30  =0129+431    07 06 47  25.2 -52.7  5.5      70.7    82     9955   03 43 01

03 44 30  B0128+437    07 06 47  25.1 -52.0  5.6      70.7    -8     9955   03 44 38
03 48 00  ---          07 10 18  24.5 -51.8  5.6      70.2   202    10007   03 44 31

03 48 15  J0132+4325   07 10 33  24.5 -52.4  5.6      70.2     7    10007   03 48 15
03 49 45  =0129+431    07 12 03  24.3 -52.3  5.6      70.0    90    10030   03 48 16

03 49 45  B0128+437    07 12 03  24.2 -51.6  5.7      70.0    -8    10030   03 49 53
03 53 15  ---          07 15 34  23.6 -51.4  5.7      69.5   202    10082   03 49 46

03 53 15  J0132+4325   07 15 34  23.7 -52.1  5.7      69.5    -8    10082   03 53 23
03 54 45  =0129+431    07 17 04  23.4 -52.0  5.7      69.2    82    10103   03 53 16

 ---------- Scan set 47 ----------

03 54 45  B0128+437    07 17 04  23.4 -51.3  5.7      69.2    -8    10103   03 54 53
03 58 15  ---          07 20 35  22.8 -51.1  5.8      68.7   202    10155   03 54 46

03 58 15  J0132+4325   07 20 35  22.8 -51.7  5.8      68.7    -8    10155   03 58 23
04 00 00  =0129+431    07 22 20  22.5 -51.6  5.8      68.5    97    10180   03 58 16


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess124.X2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    5         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  15  Setup file default.  Used with PCAL = off
   LO sum=   8240.00  8240.00  8304.00  8304.00  8368.00  8368.00  8432.00  8432.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  15  16  17  18  19  20  21  22  23  24

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * B0128+437         01 28 15.245932   * 01 31 13.491000     01 32 37.969199       0.00
                     43 42 46.77735    * 43 58 12.85100      44 05 45.58485        0.00
                     From catalog imbedded in main SCHED input file.

   0129+431          01 29 45.959987   * 01 32 44.126798     01 34 08.592046       0.20
 * J0132+4325        43 10 09.12650    * 43 25 32.66097      43 33 04.10289        0.19
                     /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,     94 observations.

 * 3C84              03 16 29.567265   * 03 19 48.160096     03 21 23.354163       1.50
   J0319+4130        41 19 51.91692    * 41 30 42.10404      41 36 05.20373        2.86
   0316+413          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0319+41          GSFC 2016a X/S astro solution,  10291 observations.

 * 3C147             05 38 43.517517   * 05 42 36.137894     05 44 28.938542       0.04
   J0542+4951        49 49 42.83709    * 49 51 07.23372      49 51 59.69153        0.03
   0538+498          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0542+49          GSFC 2016a X/S astro solution,   1444 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  B0128+437  sess124.X2048glob     1 2 3 4 5 6 7 8 10 11 12 13 +    13.083  1034.286
  J0132+4325 sess124.X2048glob     1 2 3 4 5 6 7 8 10 11 12 13 +     5.628   447.103
  3C84       sess124.X2048glob     1 2 3 4 5 6 7 8 10 11 12 13 +     0.200    18.767
  3C147      sess124.X2048glob     13                                0.054     0.000

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   0133+476          01 33 55.103060   * 01 36 58.594805     01 38 25.544592       0.00
 * J0136+4751        47 36 12.85364    * 47 51 29.10003      47 58 58.45144        0.00
   J0136+47          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution, 193511 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   B0128+437           67.7
   J0132+4325          67.5
   J0136+4751          70.9
   3C84                83.8
   3C147              109.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

