  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Exploring the jets of a new microquasar
 Exp. Code:  gr021a  


Schedule Version:       2.00                                              
Processed by SCHED version: Release of 28 April 2000                      

PI:       Marc Ribo                                                       

Address:  Departament Astronomia i Meteorologia                           
          Facultat de Fisica (UB)                                         
          Av. Diagonal, 647                                               
          E-08028 Barcelona, SPAIN                                        

Phone:    +34-93-402-11-22                                                
EMAIL:    Internet: mribo@am.ub.es                                        
Fax:      +34-93-402-11-33                                                
Phone during observation: +34-93-302-17-43                                

Observing mode: v6cm-256-8-2-L VLBA/MKIV (modified for Hh)                

Notes:    Target source LS5039/J1826-14.   Phase-reference J1825-17       
          Phase-references or checks             J1837-15, J1911-20       
          Fringe-finder                              3C345/J1642+39       
          MERLIN compact calibrator               2134+004/J2136+00       

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

 Next scan frequencies:  4960.49  4968.49  4976.49  4984.49  4992.49  5000.49
                         5008.49  5016.49
 Next BBC frequencies:    860.49   868.49   876.49   884.49   892.49   900.49
                          908.49   916.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

03 18 44  LS5039       13 10 32   1.7 108.4 -5.3  D  -57.6     0   1  1      0  03 18 44
03 21 44  ---          13 13 33   2.3 108.8 -5.2  H  -57.4     0   F  1   2400

03 23 14  LS5039       13 15 03   2.6 109.0 -5.2  H  -57.3    87   1  1   2400  03 23 14
03 26 04  ---          13 17 53   3.2 109.3 -5.1     -57.1     0   F  1   4667

03 26 04  J1825-17     13 17 53   1.9 111.5 -5.1  D  -57.0    -4   1  1   4667  03 26 04
03 27 34  ---          13 19 23   2.3 111.7 -5.1  H  -56.9     0   F  1   5867

03 27 34  LS5039       13 19 23   3.5 109.5 -5.1     -57.0    -4   1  1   5867  03 27 34
03 30 24  ---          13 22 14   4.0 109.9 -5.1     -56.8   166   F  1   8133

03 30 24  J1825-17     13 22 14   2.8 112.1 -5.1     -56.7    -4   1  1   8133  03 30 24
03 31 54  ---          13 23 44   3.1 112.2 -5.0     -56.5    86   F  1   9333

03 31 54  LS5039       13 23 44   4.3 110.1 -5.0     -56.7    -4   1  1   9333  03 31 54
03 34 44  ---          13 26 35   4.9 110.5 -5.0     -56.5   166   F  1  11600

03 34 44  J1825-17     13 26 35   3.7 112.6 -5.0     -56.3    -4   1  1  11600  03 34 44
03 36 14  ---          13 28 05   4.0 112.8 -5.0     -56.2    86   F  1  12800

03 36 14  J1837-15     13 28 05   2.5 109.8 -5.2  H  -57.2    -5   1  1  12800  03 36 14
03 37 44  ---          13 29 35   2.8 110.0 -5.1  H  -57.1     0   F  1  14000

03 40 11  J1825-17     13 32 02   4.8 113.4 -4.9     -55.8   141   1  1  14000  03 40 11
03 41 41  ---          13 33 32   5.1 113.6 -4.9     -55.7    90   F  1  15200

03 41 41  LS5039       13 33 32   6.3 111.4 -4.9     -56.0    -5   1  1  15200  03 41 41
03 44 41  ---          13 36 33   6.9 111.8 -4.8     -55.7   175   F  1  17600

03 44 41  J1825-17     13 36 33   5.7 114.0 -4.8     -55.4    -5   1  2  17600  03 44 41
03 46 11  ---          13 38 03   5.9 114.2 -4.8     -55.3    85   R  1  16400

03 46 11  LS5039       13 38 03   7.2 112.0 -4.8     -55.6    -5   1  2  16400  03 46 11
03 49 11  ---          13 41 04   7.8 112.5 -4.8     -55.4   175   R  1  14000
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

03 49 11  J1825-17     13 41 04   6.5 114.6 -4.7     -55.0    -5   1  2  14000  03 49 11
03 50 41  ---          13 42 34   6.8 114.8 -4.7     -54.9    85   R  1  12800

03 50 41  J1837-15     13 42 34   5.5 111.7 -4.9     -56.1    -5   1  2  12800  03 50 41
03 52 11  ---          13 44 04   5.8 111.9 -4.9     -56.0    85   R  1  11600

04 02 30  J1825-17     13 54 25   9.1 116.5 -4.5     -53.8   610   1  2  11600  04 02 30
04 05 00  ---          13 56 55   9.6 116.8 -4.5     -53.5   150   R  1   9600

04 05 00  LS5039       13 56 55  10.9 114.7 -4.5     -54.0    -5   1  2   9600  04 05 00
04 08 30  ---          14 00 26  11.6 115.2 -4.4     -53.6   205   R  1   6800

04 08 30  J1825-17     14 00 26  10.3 117.3 -4.4     -53.2    -5   1  2   6800  04 08 30
04 10 00  ---          14 01 56  10.6 117.5 -4.4     -53.0    85   R  1   5600

04 10 00  LS5039       14 01 56  11.9 115.4 -4.4     -53.5    -5   1  2   5600  04 10 00
04 13 30  ---          14 05 27  12.6 115.9 -4.3     -53.2   205   R  1   2800

04 13 30  J1825-17     14 05 27  11.2 118.1 -4.3     -52.7    -5   1  2   2800  04 13 30
04 15 00  ---          14 06 57  11.5 118.3 -4.3     -52.5    85   R  1   1600

04 15 00  J1837-15     14 06 57  10.3 115.1 -4.5     -54.0    -5   1  2   1600  04 15 00
04 16 30  ---          14 08 27  10.6 115.3 -4.5     -53.8    85   R  1    400

04 18 00  J1825-17     14 09 57  12.1 118.7 -4.3     -52.2    85   1  3    400  04 18 00
04 20 00  ---          14 11 58  12.5 119.0 -4.2     -52.0   120   F  1   2000

04 20 00  LS5039       14 11 58  13.9 116.9 -4.2     -52.5    -5   1  3   2000  04 20 00
04 22 30  ---          14 14 28  14.3 117.3 -4.2     -52.3   145   F  1   4000

04 22 30  J1825-17     14 14 28  12.9 119.4 -4.2     -51.7    -5   1  3   4000  04 22 30
04 24 00  ---          14 15 58  13.2 119.6 -4.2     -51.6    85   F  1   5200

04 24 00  LS5039       14 15 58  14.6 117.5 -4.2     -52.1    -5   1  3   5200  04 24 00
04 26 50  ---          14 18 49  15.2 118.0 -4.1     -51.8   165   F  1   7467

04 26 50  J1825-17     14 18 49  13.8 120.1 -4.1     -51.3    -5   1  3   7467  04 26 50
04 28 20  ---          14 20 19  14.0 120.3 -4.1     -51.1    85   F  1   8667

04 28 20  LS5039       14 20 19  15.5 118.2 -4.1     -51.7    -5   1  3   8667  04 28 20
04 31 10  ---          14 23 10  16.0 118.7 -4.1     -51.4   165   F  1  10933
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

04 31 10  J1825-17     14 23 10  14.6 120.7 -4.0     -50.8    -5   1  3  10933  04 31 10
04 32 40  ---          14 24 40  14.8 121.0 -4.0     -50.6    85   F  1  12133

04 32 40  LS5039       14 24 40  16.3 118.9 -4.0     -51.2    -5   1  3  12133  04 32 40
04 35 30  ---          14 27 30  16.8 119.3 -4.0     -50.9   165   F  1  14400

04 35 30  J1825-17     14 27 30  15.4 121.4 -4.0     -50.3    -5   1  3  14400  04 35 30
04 37 00  ---          14 29 01  15.6 121.7 -3.9     -50.1    85   F  1  15600

04 37 00  J1837-15     14 29 01  14.5 118.4 -4.1     -51.8    -4   1  3  15600  04 37 00
04 38 30  ---          14 30 31  14.8 118.6 -4.1     -51.6    86   F  1  16800

04 38 30  J1911-20     14 30 31   5.7 117.4 -4.7     -54.4   -20   1  4  16800  04 38 30
04 40 00  ---          14 32 01   6.0 117.6 -4.7     -54.3    70   R  1  17200

04 40 56  J1825-17     14 32 58  16.4 122.3 -3.9     -49.6    34   1  4  17200  04 40 56
04 42 26  ---          14 34 28  16.6 122.5 -3.9     -49.4    90   R  1  16000

04 42 26  LS5039       14 34 28  18.1 120.5 -3.9     -50.1    -5   1  4  16000  04 42 26
04 45 26  ---          14 37 28  18.7 121.0 -3.8     -49.8   175   R  1  13600

04 45 26  J1825-17     14 37 28  17.2 123.0 -3.8     -49.1    -5   1  4  13600  04 45 26
04 46 56  ---          14 38 59  17.4 123.3 -3.8     -48.9    85   R  1  12400

04 46 56  LS5039       14 38 59  18.9 121.2 -3.8     -49.6    -5   1  4  12400  04 46 56
04 49 46  ---          14 41 49  19.5 121.7 -3.7     -49.2   165   R  1  10133

04 49 46  J1825-17     14 41 49  18.0 123.7 -3.7     -48.5    -5   1  4  10133  04 49 46
04 51 16  ---          14 43 19  18.2 124.0 -3.7     -48.4    85   R  1   8933

04 51 16  LS5039       14 43 19  19.7 121.9 -3.7     -49.1    -5   1  4   8933  04 51 16
04 54 06  ---          14 46 10  20.3 122.4 -3.7     -48.7   165   R  1   6667

04 54 06  J1825-17     14 46 10  18.7 124.5 -3.7     -48.0    -5   1  4   6667  04 54 06
04 55 36  ---          14 47 40  19.0 124.7 -3.6     -47.8    85   R  1   5467

04 55 36  LS5039       14 47 40  20.5 122.7 -3.6     -48.5    -5   1  4   5467  04 55 36
04 58 26  ---          14 50 31  21.0 123.2 -3.6     -48.2   165   R  1   3200

04 58 26  J1825-17     14 50 31  19.5 125.2 -3.6     -47.4    -5   1  4   3200  04 58 26
04 59 56  ---          14 52 01  19.8 125.5 -3.6     -47.2    85   R  1   2000
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

04 59 56  J1837-15     14 52 01  18.8 122.0 -3.8     -49.2    -4   1  4   2000  04 59 56
05 01 26  ---          14 53 31  19.1 122.3 -3.7     -49.0    86   R  1    800

05 01 26  J1911-20     14 53 31  10.0 120.7 -4.3     -52.0   -20   1  5    800  05 01 26
05 02 56  ---          14 55 01  10.3 120.9 -4.3     -51.8    70   F  1    400

05 07 06  3C345        14 59 12  67.0  59.4 -1.7    -105.4   134   1  5    400  05 07 06
05 14 06  ---          15 06 13  68.3  58.4 -1.6    -107.5   420   F  1   6000

05 18 05  J1825-17     15 10 12  22.9 128.7 -3.3     -44.7   146   1  5   6000  05 18 05
05 21 05  ---          15 13 12  23.4 129.3 -3.2     -44.3   180   F  1   8400

05 21 05  LS5039       15 13 12  25.0 127.2 -3.2     -45.1    -5   1  5   8400  05 21 05
05 24 05  ---          15 16 13  25.5 127.8 -3.2     -44.7   175   F  1  10800

05 24 05  J1825-17     15 16 13  23.9 129.8 -3.2     -43.8    -5   1  5  10800  05 24 05
05 25 35  ---          15 17 43  24.1 130.1 -3.1     -43.6    85   F  1  12000

05 25 35  LS5039       15 17 43  25.8 128.1 -3.1     -44.5    -5   1  5  12000  05 25 35
05 28 35  ---          15 20 44  26.3 128.7 -3.1     -44.0   175   F  1  14400

05 28 35  J1825-17     15 20 44  24.6 130.7 -3.1     -43.1    -5   1  5  14400  05 28 35
05 30 05  ---          15 22 14  24.9 131.0 -3.1     -42.9    85   F  1  15600

05 30 05  J1837-15     15 22 14  24.1 127.3 -3.3     -45.2    -4   1  5  15600  05 30 05
05 31 35  ---          15 23 44  24.4 127.6 -3.2     -45.0    86   F  1  16800

05 31 35  J1911-20     15 23 44  15.5 125.3 -3.8     -48.4   -20   1  6  16800  05 31 35
05 33 05  ---          15 25 14  15.7 125.6 -3.8     -48.2    70   R  1  17200

05 33 49  J1825-17     15 25 59  25.5 131.7 -3.0     -42.3    22   1  6  17200  05 33 49
05 35 49  ---          15 27 59  25.8 132.1 -3.0     -42.0   120   R  1  15600

05 35 49  LS5039       15 27 59  27.5 130.1 -3.0     -42.9    -5   1  6  15600  05 35 49
05 39 19  ---          15 31 29  28.1 130.8 -2.9     -42.4   205   R  1  12800

05 39 19  J1825-17     15 31 29  26.4 132.8 -2.9     -41.4    -5   1  6  12800  05 39 19
05 41 19  ---          15 33 30  26.7 133.2 -2.9     -41.1   115   R  1  11200

05 41 19  LS5039       15 33 30  28.4 131.2 -2.9     -42.0    -5   1  6  11200  05 41 19
05 44 49  ---          15 37 00  29.0 131.9 -2.8     -41.5   205   R  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

05 44 49  J1825-17     15 37 00  27.2 133.9 -2.8     -40.5    -6   1  6   8400  05 44 49
05 46 49  ---          15 39 01  27.5 134.3 -2.8     -40.2   114   R  1   6800

05 46 49  LS5039       15 39 01  29.3 132.4 -2.8     -41.1    -6   1  6   6800  05 46 49
05 50 19  ---          15 42 31  29.8 133.1 -2.7     -40.5   204   R  1   4000

05 50 19  J1825-17     15 42 31  28.1 135.0 -2.7     -39.6    -6   1  6   4000  05 50 19
05 52 19  ---          15 44 32  28.4 135.5 -2.7     -39.2   114   R  1   2400

05 52 19  J1837-15     15 44 32  27.8 131.7 -2.9     -41.8    -5   1  6   2400  05 52 19
05 54 19  ---          15 46 32  28.2 132.1 -2.9     -41.5   115   R  1    800

05 54 19  J1911-20     15 46 32  19.4 129.2 -3.4     -45.3   -20   1  7    800  05 54 19
05 55 49  ---          15 48 02  19.6 129.4 -3.4     -45.0    70   F  1    400

05 57 49  J1825-17     15 50 02  29.2 136.6 -2.6     -38.2    99   1  7    400  05 57 49
05 59 49  ---          15 52 03  29.5 137.1 -2.6     -37.9   120   F  1   2000

05 59 49  LS5039       15 52 03  31.3 135.1 -2.6     -38.9    -6   1  7   2000  05 59 49
06 03 19  ---          15 55 33  31.8 135.9 -2.5     -38.3   204   F  1   4800

06 03 19  J1825-17     15 55 33  30.0 137.8 -2.5     -37.2    -6   1  7   4800  06 03 19
06 05 19  ---          15 57 34  30.3 138.3 -2.5     -36.9   114   F  1   6400

06 05 19  LS5039       15 57 34  32.1 136.4 -2.5     -37.9    -6   1  7   6400  06 05 19
06 08 49  ---          16 01 04  32.7 137.2 -2.4     -37.2   204   F  1   9200

06 08 49  J1825-17     16 01 04  30.8 139.1 -2.4     -36.2    -6   1  7   9200  06 08 49
06 10 49  ---          16 03 05  31.1 139.5 -2.4     -35.8   114   F  1  10800

06 10 49  LS5039       16 03 05  33.0 137.6 -2.4     -36.9    -6   1  7  10800  06 10 49
06 14 19  ---          16 06 35  33.5 138.4 -2.3     -36.2   204   F  1  13600

06 14 19  J1825-17     16 06 35  31.5 140.3 -2.3     -35.1    -6   1  7  13600  06 14 19
06 16 19  ---          16 08 36  31.8 140.8 -2.3     -34.8   114   F  1  15200

06 16 19  J1837-15     16 08 36  31.5 136.8 -2.5     -37.7    -5   1  7  15200  06 16 19
06 18 19  ---          16 10 36  31.8 137.3 -2.5     -37.3   115   F  1  16800

06 18 19  J1911-20     16 10 36  23.2 133.6 -3.0     -41.6   -19   1  8  16800  06 18 19
06 19 49  ---          16 12 06  23.5 133.9 -3.0     -41.4    71   R  1  17200
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

06 20 30  J1825-17     16 12 48  32.4 141.7 -2.2     -33.9    22   1  8  17200  06 20 30
06 22 30  ---          16 14 48  32.7 142.2 -2.2     -33.5   120   R  1  15600

06 22 30  LS5039       16 14 48  34.6 140.4 -2.2     -34.6    -6   1  8  15600  06 22 30
06 26 00  ---          16 18 19  35.1 141.3 -2.1     -33.9   204   R  1  12800

06 26 00  J1825-17     16 18 19  33.1 143.0 -2.1     -32.8    -6   1  8  12800  06 26 00
06 28 00  ---          16 20 19  33.4 143.5 -2.1     -32.4   114   R  1  11200

06 28 00  LS5039       16 20 19  35.4 141.8 -2.1     -33.4    -6   1  8  11200  06 28 00
06 31 30  ---          16 23 50  35.8 142.6 -2.0     -32.7   204   R  1   8400

06 31 30  J1825-17     16 23 50  33.8 144.4 -2.0     -31.7    -6   1  8   8400  06 31 30
06 33 30  ---          16 25 50  34.1 144.9 -2.0     -31.2   114   R  1   6800

06 33 30  LS5039       16 25 50  36.1 143.1 -2.0     -32.3    -6   1  8   6800  06 33 30
06 37 00  ---          16 29 21  36.5 144.0 -1.9     -31.5   204   R  1   4000

06 37 00  J1825-17     16 29 21  34.5 145.7 -1.9     -30.5    -6   1  8   4000  06 37 00
06 39 00  ---          16 31 21  34.7 146.2 -1.9     -30.0   114   R  1   2400

06 39 00  J1837-15     16 31 21  34.7 142.1 -2.1     -33.2    -5   1  8   2400  06 39 00
06 41 00  ---          16 33 21  35.0 142.6 -2.1     -32.8   115   R  1    800

06 41 00  J1911-20     16 33 21  26.7 138.1 -2.6     -37.7   -19   1  9    800  06 41 00
06 42 30  ---          16 34 52  26.9 138.4 -2.6     -37.5    71   F  1    400

06 43 11  J1825-17     16 35 32  35.2 147.3 -1.8     -29.1    21   1  9    400  06 43 11
06 45 11  ---          16 37 32  35.5 147.8 -1.8     -28.7   120   F  1   2000

06 45 11  LS5039       16 37 32  37.5 146.2 -1.8     -29.7    -6   1  9   2000  06 45 11
06 48 41  ---          16 41 03  38.0 147.1 -1.8     -28.9   204   F  1   4800

06 48 41  J1825-17     16 41 03  35.9 148.7 -1.7     -27.9    -6   1  9   4800  06 48 41
06 50 41  ---          16 43 03  36.1 149.3 -1.7     -27.4   114   F  1   6400

06 50 41  LS5039       16 43 03  38.2 147.6 -1.7     -28.5    -6   1  9   6400  06 50 41
06 54 11  ---          16 46 34  38.6 148.6 -1.7     -27.6   204   F  1   9200

06 54 11  J1825-17     16 46 34  36.5 150.2 -1.7     -26.6    -6   1  9   9200  06 54 11
06 56 11  ---          16 48 34  36.7 150.7 -1.6     -26.2   114   F  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

06 56 11  LS5039       16 48 34  38.8 149.1 -1.6     -27.2    -6   1  9  10800  06 56 11
06 59 41  ---          16 52 05  39.2 150.1 -1.6     -26.3   204   F  1  13600

06 59 41  J1825-17     16 52 05  37.0 151.7 -1.6     -25.3    -6   1  9  13600  06 59 41
07 01 41  ---          16 54 05  37.2 152.2 -1.5     -24.9   114   F  1  15200

07 01 41  J1837-15     16 54 05  37.5 148.0 -1.7     -28.3    -5   1  9  15200  07 01 41
07 03 41  ---          16 56 05  37.8 148.5 -1.7     -27.8   115   F  1  16800

07 03 41  J1911-20     16 56 05  29.8 143.0 -2.3     -33.4   -18   1 10  16800  07 03 41
07 05 11  ---          16 57 35  30.0 143.4 -2.2     -33.1    72   R  1  17200

07 05 49  J1825-17     16 58 14  37.6 153.3 -1.5     -23.9    21   1 10  17200  07 05 49
07 07 49  ---          17 00 14  37.8 153.9 -1.4     -23.4   120   R  1  15600

07 07 49  LS5039       17 00 14  40.0 152.4 -1.4     -24.3    -6   1 10  15600  07 07 49
07 11 19  ---          17 03 45  40.4 153.4 -1.4     -23.5   204   R  1  12800

07 11 19  J1825-17     17 03 45  38.2 154.9 -1.4     -22.5    -6   1 10  12800  07 11 19
07 13 19  ---          17 05 45  38.3 155.4 -1.3     -22.0   114   R  1  11200

07 13 19  LS5039       17 05 45  40.6 154.0 -1.3     -22.9    -6   1 10  11200  07 13 19
07 16 49  ---          17 09 16  40.9 155.1 -1.3     -22.0   204   R  1   8400

07 16 49  J1825-17     17 09 16  38.7 156.4 -1.3     -21.1    -6   1 10   8400  07 16 49
07 18 49  ---          17 11 16  38.8 157.0 -1.2     -20.6   114   R  1   6800

07 18 49  LS5039       17 11 16  41.1 155.7 -1.3     -21.5    -6   1 10   6800  07 18 49
07 22 19  ---          17 14 47  41.4 156.7 -1.2     -20.6   204   R  1   4000

07 22 19  J1825-17     17 14 47  39.1 158.0 -1.2     -19.7    -7   1 10   4000  07 22 19
07 24 19  ---          17 16 47  39.3 158.6 -1.1     -19.2   113   R  1   2400

07 24 19  J1837-15     17 16 47  39.9 154.3 -1.3     -22.8    -5   1 10   2400  07 24 19
07 26 19  ---          17 18 47  40.1 154.9 -1.3     -22.3   115   R  1    800

07 26 19  J1911-20     17 18 47  32.5 148.4 -1.9     -28.7   -17   1 11    800  07 26 19
07 27 49  ---          17 20 18  32.7 148.7 -1.8     -28.4    73   F  1    400

07 28 25  J1825-17     17 20 54  39.6 159.8 -1.1     -18.1    21   1 11    400  07 28 25
07 30 25  ---          17 22 54  39.7 160.4 -1.0     -17.6   120   F  1   2000
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

07 30 25  LS5039       17 22 54  42.0 159.2 -1.1     -18.4    -7   1 11   2000  07 30 25
07 33 55  ---          17 26 25  42.3 160.3 -1.0     -17.5   203   F  1   4800

07 33 55  J1825-17     17 26 25  40.0 161.4 -1.0     -16.7    -7   1 11   4800  07 33 55
07 35 55  ---          17 28 25  40.1 162.0 -1.0     -16.1   113   F  1   6400

07 35 55  LS5039       17 28 25  42.4 160.9 -1.0     -16.9    -7   1 11   6400  07 35 55
07 39 25  ---          17 31 56  42.7 162.0 -0.9     -16.0   203   F  1   9200

07 39 25  J1825-17     17 31 56  40.3 163.1 -0.9     -15.2    -7   1 11   9200  07 39 25
07 41 25  ---          17 33 56  40.5 163.7 -0.9     -14.7   113   F  1  10800

07 41 25  LS5039       17 33 56  42.8 162.6 -0.9     -15.4    -7   1 11  10800  07 41 25
07 44 55  ---          17 37 27  43.0 163.8 -0.8     -14.4   203   F  1  13600

07 44 55  J1825-17     17 37 27  40.7 164.8 -0.8     -13.7    -7   1 11  13600  07 44 55
07 46 55  ---          17 39 27  40.8 165.4 -0.8     -13.1   113   F  1  15200

07 46 55  J1837-15     17 39 27  41.7 161.1 -1.0     -16.8    -5   1 11  15200  07 46 55
07 48 55  ---          17 41 27  41.9 161.7 -0.9     -16.3   115   F  1  16800

07 48 55  J1911-20     17 41 27  34.9 154.1 -1.5     -23.6   -16   1 12  16800  07 48 55
07 50 25  ---          17 42 58  35.0 154.5 -1.5     -23.2    74   R  1  17200

07 50 59  J1825-17     17 43 32  41.0 166.6 -0.7     -12.0    20   1 12  17200  07 50 59
07 52 59  ---          17 45 32  41.1 167.3 -0.7     -11.5   120   R  1  15600

07 52 59  LS5039       17 45 32  43.5 166.4 -0.7     -12.1    -7   1 12  15600  07 52 59
07 56 29  ---          17 49 03  43.6 167.5 -0.6     -11.1   203   R  1  12800

07 56 29  J1825-17     17 49 03  41.3 168.4 -0.6     -10.5    -7   1 12  12800  07 56 29
07 58 29  ---          17 51 03  41.3 169.0 -0.6      -9.9   113   R  1  11200

07 58 29  LS5039       17 51 03  43.7 168.2 -0.6     -10.5    -7   1 12  11200  07 58 29
08 01 59  ---          17 54 34  43.9 169.3 -0.5      -9.5   203   R  1   8400

08 01 59  J1825-17     17 54 34  41.5 170.1 -0.5      -8.9    -7   1 12   8400  08 01 59
08 03 59  ---          17 56 34  41.5 170.7 -0.5      -8.4   113   R  1   6800

08 03 59  LS5039       17 56 34  44.0 170.0 -0.5      -8.9    -7   1 12   6800  08 03 59
08 07 29  ---          18 00 05  44.1 171.2 -0.4      -7.9   203   R  1   4000
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

08 07 29  J1825-17     18 00 05  41.7 171.8 -0.4      -7.4    -7   1 12   4000  08 07 29
08 09 29  ---          18 02 05  41.7 172.5 -0.4      -6.8   113   R  1   2400

08 09 29  J1837-15     18 02 05  43.0 168.2 -0.6     -10.5    -5   1 12   2400  08 09 29
08 11 29  ---          18 04 05  43.1 168.9 -0.6      -9.9   115   R  1    800

08 11 29  J1911-20     18 04 05  36.8 160.2 -1.1     -18.1   -15   1 13    800  08 11 29
08 12 59  ---          18 05 35  36.9 160.7 -1.1     -17.7    75   F  1    400

08 14 59  J1825-17     18 07 36  41.9 174.2 -0.3      -5.2   108   1 13    400  08 14 59
08 16 59  ---          18 09 36  41.9 174.9 -0.3      -4.6   120   F  1   2000

08 16 59  LS5039       18 09 36  44.3 174.4 -0.3      -5.0    -7   1 13   2000  08 16 59
08 20 29  ---          18 13 07  44.4 175.5 -0.2      -4.0   203   F  1   4800

08 20 29  J1825-17     18 13 07  42.0 176.0 -0.2      -3.6    -7   1 13   4800  08 20 29
08 22 29  ---          18 15 07  42.0 176.6 -0.2      -3.0   113   F  1   6400

08 22 29  LS5039       18 15 07  44.4 176.2 -0.2      -3.4    -7   1 13   6400  08 22 29
08 25 59  ---          18 18 38  44.5 177.4 -0.1      -2.3   203   F  1   9200

08 25 59  J1825-17     18 18 38  42.0 177.7 -0.1      -2.0    -7   1 13   9200  08 25 59
08 27 59  ---          18 20 38  42.0 178.4 -0.1      -1.4   113   F  1  10800

08 27 59  LS5039       18 20 38  44.5 178.1 -0.1      -1.7    -7   1 13  10800  08 27 59
08 31 29  ---          18 24 08  44.5 179.3  0.0      -0.6   203   F  1  13600

08 31 29  J1825-17     18 24 08  42.1 179.5  0.0      -0.4    -7   1 13  13600  08 31 29
08 33 29  ---          18 26 09  42.1 180.2  0.0       0.1   113   F  1  15200

08 33 29  J1837-15     18 26 09  43.7 176.2 -0.2      -3.4    -5   1 13  15200  08 33 29
08 35 29  ---          18 28 09  43.8 176.8 -0.2      -2.8   115   F  1  16800

08 35 29  J1911-20     18 28 09  38.2 167.1 -0.7     -11.8   -13   1 14  16800  08 35 29
08 36 59  ---          18 29 39  38.3 167.6 -0.7     -11.4    77   R  1  17200

08 37 34  J1825-17     18 30 14  42.0 181.5  0.1       1.3    23   1 14  17200  08 37 34
08 39 34  ---          18 32 14  42.0 182.1  0.1       1.9   120   R  1  15600

08 39 34  LS5039       18 32 14  44.5 182.0  0.1       1.8    -7   1 14  15600  08 39 34
08 43 04  ---          18 35 45  44.5 183.2  0.2       2.9   203   R  1  12800
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

08 43 04  J1825-17     18 35 45  42.0 183.2  0.2       2.9    -7   1 14  12800  08 43 04
08 45 04  ---          18 37 45  42.0 183.9  0.2       3.5   113   R  1  11200

08 45 04  LS5039       18 37 45  44.4 183.9  0.2       3.5    -7   1 14  11200  08 45 04
08 48 34  ---          18 41 16  44.4 185.1  0.2       4.5   203   R  1   8400

08 48 34  J1825-17     18 41 16  41.9 185.0  0.3       4.5    -7   1 14   8400  08 48 34
08 50 34  ---          18 43 16  41.9 185.7  0.3       5.1   113   R  1   6800

08 50 34  LS5039       18 43 16  44.3 185.7  0.3       5.1    -7   1 14   6800  08 50 34
08 54 04  ---          18 46 47  44.3 186.9  0.3       6.2   203   R  1   4000

08 54 04  J1825-17     18 46 47  41.8 186.8  0.4       6.1    -7   1 14   4000  08 54 04
08 56 04  ---          18 48 47  41.7 187.4  0.4       6.7   113   R  1   2400

08 56 04  J1837-15     18 48 47  43.7 183.7  0.2       3.3    -6   1 14   2400  08 56 04
08 58 04  ---          18 50 47  43.7 184.4  0.2       3.9   114   R  1    800

-----------  Tape Change ------------

08 58 04  J1911-20     18 50 47  39.0 173.8 -0.3      -5.6   -11   2  1    800  08 58 04
08 59 34  ---          18 52 17  39.0 174.3 -0.3      -5.2    79   F  1    400

09 00 09  J1825-17     18 52 53  41.6 188.7  0.5       7.8    24   2  1    400  09 00 09
09 02 09  ---          18 54 53  41.5 189.3  0.5       8.4   120   F  1   2000

09 02 09  LS5039       18 54 53  44.0 189.6  0.5       8.6    -7   2  1   2000  09 02 09
09 05 39  ---          18 58 24  43.9 190.8  0.5       9.6   203   F  1   4800

09 05 39  J1825-17     18 58 24  41.4 190.4  0.5       9.4    -7   2  1   4800  09 05 39
09 07 39  ---          19 00 24  41.3 191.1  0.6      10.0   113   F  1   6400

09 07 39  LS5039       19 00 24  43.8 191.5  0.6      10.2    -7   2  1   6400  09 07 39
09 11 09  ---          19 03 55  43.6 192.6  0.6      11.2   203   F  1   9200

09 11 09  J1825-17     19 03 55  41.2 192.2  0.6      11.0    -7   2  1   9200  09 11 09
09 13 09  ---          19 05 55  41.1 192.8  0.7      11.5   113   F  1  10800

09 13 09  LS5039       19 05 55  43.5 193.3  0.7      11.8    -7   2  1  10800  09 13 09
09 16 39  ---          19 09 26  43.3 194.4  0.7      12.8   203   F  1  13600

09 16 39  J1825-17     19 09 26  40.9 193.9  0.7      12.5    -7   2  1  13600  09 16 39
09 18 39  ---          19 11 26  40.8 194.5  0.8      13.0   113   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

09 18 39  J1837-15     19 11 26  43.1 191.2  0.6      10.0    -7   2  1  15200  09 18 39
09 20 39  ---          19 13 26  43.0 191.8  0.6      10.5   113   F  1  16800

09 20 39  J1911-20     19 13 26  39.2 180.7  0.0       0.6   -10   2  2  16800  09 20 39
09 22 09  ---          19 14 56  39.2 181.1  0.1       1.0    80   R  1  17200

09 25 17  3C345        19 18 05  57.3 297.1  2.6      94.0   108   2  2  17200  09 25 17
09 30 47  ---          19 23 36  56.3 296.9  2.7      93.1   330   R  1  12800

09 33 29  J1825-17     19 26 18  39.9 199.0  1.0      17.1    95   2  2  12800  09 33 29
09 36 29  ---          19 29 19  39.7 199.9  1.1      17.9   180   R  1  10400

09 36 29  LS5039       19 29 19  42.1 200.7  1.1      18.3    -7   2  2  10400  09 36 29
09 39 29  ---          19 32 19  41.8 201.6  1.1      19.2   173   R  1   8000

09 39 29  J1825-17     19 32 19  39.4 200.8  1.1      18.6    -7   2  2   8000  09 39 29
09 41 29  ---          19 34 19  39.3 201.4  1.1      19.2   113   R  1   6400

09 41 29  LS5039       19 34 19  41.7 202.2  1.1      19.7    -7   2  2   6400  09 41 29
09 44 29  ---          19 37 20  41.4 203.2  1.2      20.5   173   R  1   4000

09 44 29  J1825-17     19 37 20  39.0 202.2  1.2      19.9    -7   2  2   4000  09 44 29
09 46 29  ---          19 39 20  38.9 202.8  1.2      20.4   113   R  1   2400

09 46 29  J1837-15     19 39 20  41.5 200.0  1.0      17.8    -7   2  2   2400  09 46 29
09 48 29  ---          19 41 21  41.3 200.6  1.1      18.3   113   R  1    800

09 48 29  J1911-20     19 41 21  38.7 189.1  0.5       8.3   -10   2  3    800  09 48 29
09 49 59  ---          19 42 51  38.7 189.5  0.5       8.7    80   F  1    400

09 50 35  J1825-17     19 43 27  38.5 204.0  1.3      21.5    24   2  3    400  09 50 35
09 52 35  ---          19 45 27  38.4 204.5  1.3      22.0   120   F  1   2000

09 52 35  LS5039       19 45 27  40.7 205.6  1.3      22.6    -7   2  3   2000  09 52 35
09 56 05  ---          19 48 58  40.4 206.6  1.4      23.5   203   F  1   4800

09 56 05  J1825-17     19 48 58  38.0 205.5  1.4      22.9    -7   2  3   4800  09 56 05
09 58 05  ---          19 50 58  37.8 206.1  1.4      23.4   113   F  1   6400

09 58 05  LS5039       19 50 58  40.2 207.2  1.4      24.0    -7   2  3   6400  09 58 05
10 01 35  ---          19 54 29  39.8 208.2  1.5      24.9   203   F  1   9200
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

10 01 35  J1825-17     19 54 29  37.5 207.1  1.5      24.2    -7   2  3   9200  10 01 35
10 03 35  ---          19 56 29  37.3 207.6  1.5      24.7   113   F  1  10800

10 03 35  LS5039       19 56 29  39.6 208.8  1.5      25.4    -7   2  3  10800  10 03 35
10 07 05  ---          20 00 00  39.2 209.8  1.6      26.2   203   F  1  13600

10 07 05  J1825-17     20 00 00  37.0 208.6  1.6      25.5    -7   2  3  13600  10 07 05
10 09 05  ---          20 02 00  36.7 209.1  1.6      26.0   113   F  1  15200

10 09 05  J1837-15     20 02 00  39.6 206.7  1.4      23.7    -8   2  3  15200  10 09 05
10 11 05  ---          20 04 00  39.4 207.3  1.4      24.2   112   F  1  16800

10 11 05  J1911-20     20 04 00  37.7 195.7  0.9      14.4   -10   2  4  16800  10 11 05
10 12 35  ---          20 05 30  37.6 196.2  0.9      14.8    80   R  1  17200

10 13 10  J1825-17     20 06 06  36.3 210.2  1.7      27.0    24   2  4  17200  10 13 10
10 15 10  ---          20 08 06  36.1 210.7  1.7      27.4   120   R  1  15600

10 15 10  LS5039       20 08 06  38.3 212.0  1.7      28.1    -7   2  4  15600  10 15 10
10 18 40  ---          20 11 37  37.9 212.9  1.8      28.9   203   R  1  12800

10 18 40  J1825-17     20 11 37  35.7 211.6  1.8      28.2    -6   2  4  12800  10 18 40
10 20 40  ---          20 13 37  35.5 212.1  1.8      28.7   114   R  1  11200

10 20 40  LS5039       20 13 37  37.7 213.5  1.8      29.4    -6   2  4  11200  10 20 40
10 24 10  ---          20 17 08  37.3 214.4  1.8      30.2   204   R  1   8400

10 24 10  J1825-17     20 17 08  35.1 213.0  1.9      29.4    -6   2  4   8400  10 24 10
10 26 10  ---          20 19 08  34.8 213.6  1.9      29.9   114   R  1   6800

10 26 10  LS5039       20 19 08  37.0 214.9  1.9      30.6    -6   2  4   6800  10 26 10
10 29 40  ---          20 22 39  36.6 215.8  1.9      31.4   204   R  1   4000

10 29 40  J1825-17     20 22 39  34.4 214.4  2.0      30.6    -6   2  4   4000  10 29 40
10 31 40  ---          20 24 39  34.2 214.9  2.0      31.1   114   R  1   2400

10 31 40  J1837-15     20 24 39  37.1 213.0  1.8      29.1    -8   2  4   2400  10 31 40
10 33 40  ---          20 26 40  36.9 213.5  1.8      29.5   112   R  1    800

10 33 40  J1911-20     20 26 40  36.1 202.1  1.3      20.1   -10   2  5    800  10 33 40
10 35 10  ---          20 28 10  36.0 202.5  1.3      20.5    80   F  1    400
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

10 35 45  J1825-17     20 28 45  33.6 215.9  2.1      31.9    24   2  5    400  10 35 45
10 37 45  ---          20 30 45  33.4 216.4  2.1      32.4   120   F  1   2000

10 37 45  LS5039       20 30 45  35.6 217.9  2.1      33.1    -6   2  5   2000  10 37 45
10 41 15  ---          20 34 16  35.1 218.7  2.1      33.9   204   F  1   4800

10 41 15  J1825-17     20 34 16  32.9 217.3  2.1      33.1    -6   2  5   4800  10 41 15
10 43 15  ---          20 36 16  32.7 217.7  2.2      33.5   114   F  1   6400

10 43 15  LS5039       20 36 16  34.8 219.2  2.2      34.3    -6   2  5   6400  10 43 15
10 46 45  ---          20 39 47  34.3 220.1  2.2      35.0   204   F  1   9200

10 46 45  J1825-17     20 39 47  32.2 218.6  2.2      34.2    -6   2  5   9200  10 46 45
10 48 45  ---          20 41 47  31.9 219.0  2.3      34.6   114   F  1  10800

10 48 45  LS5039       20 41 47  34.1 220.6  2.3      35.4    -6   2  5  10800  10 48 45
10 52 15  ---          20 45 18  33.6 221.4  2.3      36.1   204   F  1  13600

10 52 15  J1825-17     20 45 18  31.5 219.8  2.3      35.3    -6   2  5  13600  10 52 15
10 54 15  ---          20 47 18  31.2 220.3  2.4      35.7   114   F  1  15200

10 54 15  J1837-15     20 47 18  34.3 218.7  2.2      33.9    -8   2  5  15200  10 54 15
10 56 15  ---          20 49 18  34.0 219.2  2.2      34.3   112   F  1  16800

10 56 15  J1911-20     20 49 18  34.0 208.1  1.6      25.5    -9   2  6  16800  10 56 15
10 57 45  ---          20 50 49  33.9 208.4  1.7      25.9    81   R  1  17200

10 59 45  J1825-17     20 52 49  30.4 221.5  2.5      36.7   109   2  6  17200  10 59 45
11 01 45  ---          20 54 49  30.1 222.0  2.5      37.1   120   R  1  15600

11 01 45  LS5039       20 54 49  32.2 223.6  2.5      37.9    -6   2  6  15600  11 01 45
11 05 15  ---          20 58 20  31.6 224.4  2.5      38.5   204   R  1  12800

11 05 15  J1825-17     20 58 20  29.6 222.7  2.5      37.7    -6   2  6  12800  11 05 15
11 07 15  ---          21 00 20  29.3 223.2  2.6      38.1   114   R  1  11200

11 07 15  LS5039       21 00 20  31.3 224.8  2.6      38.9    -6   2  6  11200  11 07 15
11 10 45  ---          21 03 51  30.8 225.6  2.6      39.5   204   R  1   8400

11 10 45  J1825-17     21 03 51  28.8 223.9  2.6      38.7    -6   2  6   8400  11 10 45
11 12 45  ---          21 05 51  28.5 224.4  2.7      39.1   114   R  1   6800
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

11 12 45  LS5039       21 05 51  30.5 226.0  2.7      39.8    -6   2  6   6800  11 12 45
11 16 15  ---          21 09 22  30.0 226.8  2.7      40.4   204   R  1   4000

11 16 15  J1825-17     21 09 22  28.0 225.1  2.7      39.7    -6   2  6   4000  11 16 15
11 18 15  ---          21 11 22  27.7 225.5  2.8      40.0   114   R  1   2400

11 18 15  J1837-15     21 11 22  30.9 224.2  2.6      38.5    -8   2  6   2400  11 18 15
11 20 15  ---          21 13 22  30.6 224.7  2.6      38.9   112   R  1    800

11 20 15  J1911-20     21 13 22  31.4 214.0  2.0      30.8    -9   2  7    800  11 20 15
11 21 45  ---          21 14 52  31.2 214.3  2.1      31.1    81   F  1    400

11 22 19  J1825-17     21 15 26  27.0 226.3  2.8      40.7    23   2  7    400  11 22 19
11 24 19  ---          21 17 26  26.7 226.7  2.9      41.0   120   F  1   2000

11 24 19  LS5039       21 17 26  28.7 228.5  2.9      41.8    -6   2  7   2000  11 24 19
11 27 49  ---          21 20 57  28.1 229.2  2.9      42.3   204   F  1   4800

11 27 49  J1825-17     21 20 57  26.2 227.4  2.9      41.6    -6   2  7   4800  11 27 49
11 29 49  ---          21 22 57  25.8 227.8  3.0      41.9   114   F  1   6400

11 29 49  LS5039       21 22 57  27.8 229.6  2.9      42.7    -6   2  7   6400  11 29 49
11 33 19  ---          21 26 28  27.2 230.3  3.0      43.2   204   F  1   9200

11 33 19  J1825-17     21 26 28  25.3 228.5  3.0      42.5    -6   2  7   9200  11 33 19
11 35 19  ---          21 28 28  25.0 228.9  3.0      42.8   114   F  1  10800

11 35 19  LS5039       21 28 28  26.9 230.7  3.0      43.5    -6   2  7  10800  11 35 19
11 38 49  ---          21 31 59  26.3 231.4  3.1      44.0   204   F  1  13600

11 38 49  J1825-17     21 31 59  24.4 229.6  3.1      43.3    -6   2  7  13600  11 38 49
11 40 49  ---          21 33 59  24.1 230.0  3.1      43.6   114   F  1  15200

11 40 49  J1837-15     21 33 59  27.3 229.0  2.9      42.4    -9   2  7  15200  11 40 49
11 42 49  ---          21 35 59  27.0 229.4  3.0      42.7   111   F  1  16800

11 42 49  J1911-20     21 35 59  28.5 219.1  2.4      35.3    -9   2  8  16800  11 42 49
11 44 19  ---          21 37 30  28.3 219.4  2.4      35.6    81   R  1  17200

11 44 51  J1825-17     21 38 02  23.4 230.7  3.2      44.2    21   2  8  17200  11 44 51
11 46 51  ---          21 40 03  23.1 231.1  3.2      44.5   120   R  1  15600
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

11 46 51  LS5039       21 40 03  24.9 232.9  3.2      45.2    -6   2  8  15600  11 46 51
11 50 21  ---          21 43 33  24.3 233.5  3.3      45.7   204   R  1  12800

11 50 21  J1825-17     21 43 33  22.5 231.7  3.3      45.1    -6   2  8  12800  11 50 21
11 52 21  ---          21 45 33  22.1 232.1  3.3      45.3   114   R  1  11200

11 52 21  LS5039       21 45 33  24.0 233.9  3.3      46.0    -6   2  8  11200  11 52 21
11 55 51  ---          21 49 04  23.3 234.6  3.4      46.5   204   R  1   8400

11 55 51  J1825-17     21 49 04  21.5 232.7  3.4      45.8    -6   2  8   8400  11 55 51
11 57 51  ---          21 51 04  21.2 233.1  3.4      46.1   114   R  1   6800

11 57 51  LS5039       21 51 04  23.0 234.9  3.4      46.8    -6   2  8   6800  11 57 51
12 01 21  ---          21 54 35  22.4 235.5  3.5      47.2   204   R  1   4000

12 01 21  J1825-17     21 54 35  20.6 233.7  3.5      46.6    -6   2  8   4000  12 01 21
12 03 21  ---          21 56 35  20.2 234.1  3.5      46.9   114   R  1   2400

12 03 21  J1837-15     21 56 35  23.5 233.3  3.3      45.7    -9   2  8   2400  12 03 21
12 05 21  ---          21 58 36  23.2 233.7  3.3      46.0   111   R  1    800

12 05 21  J1911-20     21 58 36  25.3 223.8  2.8      39.4    -9   2  9    800  12 05 21
12 06 51  ---          22 00 06  25.0 224.1  2.8      39.7    81   F  1    400

12 07 23  J1825-17     22 00 38  19.5 234.8  3.6      47.4    19   2  9    400  12 07 23
12 09 23  ---          22 02 38  19.2 235.1  3.6      47.7   120   F  1   2000

12 09 23  LS5039       22 02 38  20.9 237.0  3.6      48.3    -6   2  9   2000  12 09 23
12 12 53  ---          22 06 08  20.3 237.6  3.7      48.7   204   F  1   4800

12 12 53  J1825-17     22 06 08  18.5 235.7  3.7      48.1    -6   2  9   4800  12 12 53
12 14 53  ---          22 08 09  18.2 236.0  3.7      48.4   114   F  1   6400

12 14 53  LS5039       22 08 09  19.9 237.9  3.7      48.9    -5   2  9   6400  12 14 53
12 18 23  ---          22 11 39  19.3 238.5  3.8      49.4   205   F  1   9200

12 18 23  J1825-17     22 11 39  17.6 236.6  3.8      48.8    -5   2  9   9200  12 18 23
12 20 23  ---          22 13 40  17.2 237.0  3.8      49.1   115   F  1  10800

12 20 23  LS5039       22 13 40  18.9 238.8  3.8      49.6    -5   2  9  10800  12 20 23
12 23 53  ---          22 17 10  18.3 239.4  3.8      50.0   205   F  1  13600
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   3 Jun 2000   Day 155 ---

12 23 53  J1825-17     22 17 10  16.6 237.5  3.9      49.5    -5   2  9  13600  12 23 53
12 25 53  ---          22 19 11  16.2 237.8  3.9      49.7   115   F  1  15200

12 25 53  J1837-15     22 19 11  19.5 237.3  3.7      48.7    -9   2  9  15200  12 25 53
12 27 53  ---          22 21 11  19.2 237.6  3.7      49.0   111   F  1  16800

12 27 53  J1911-20     22 21 11  21.8 228.2  3.2      43.1    -8   2 10  16800  12 27 53
12 30 00  ---          22 23 18  21.4 228.6  3.2      43.4   119   R  1  16707


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gr021.set
   Matches group v6cm_2 in /usr/local/sched/catalogs/freq.dat

   Setup group:    8         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00
   Net SB=        U        U        U        U        U        U        U        U
   Pol.  =     LCP      LCP      LCP      LCP      LCP      LCP      LCP      LCP 
   BBC   =        1        2        3        4        5        6        7        8
   BBC SB=        U        U        U        U        U        U        U        U
   IF    =       C        C        C        C        C        C        C        C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=   4960.49  4968.49  4976.49  4984.49  4992.49  5000.49  5008.49  5016.49
   BBC fr=    860.49   868.49   876.49   884.49   892.49   900.49   908.49   916.49
   Bandwd=     8.000    8.000    8.000    8.000    8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- Exploring the jets of a new microquasar
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * LS5039            18 23 23.640326   * 18 26 15.056000     18 26 16.649228 
                    -14 52 42.58697    *-14 50 54.24000     -14 50 49.74834 
                     From catalog imbedded in main SCHED input file.
                     This is our VLBI target source

 * J1825-17          18 22 42.021602   * 18 25 36.540000     18 25 38.155259 
                    -17 20 35.14168    *-17 18 49.70000     -17 18 44.87400 
                     From catalog imbedded in main SCHED input file.
                     This is the phase-reference

 * J1837-15          18 34 45.502261   * 18 37 37.672000     18 37 39.237639 
                    -15 35 21.60577    *-15 32 43.98000     -15 32 39.08243 
                     From catalog imbedded in main SCHED input file.
                     This is a possible phase-reference

   J1911-2006        19 08 12.464444   * 19 11 09.652892     19 11 11.135632 
   1908-201         -20 11 55.17861    *-20 06 55.10920     -20 06 48.49955 
 * J1911-20          From catalog imbedded in main SCHED input file.
                     USNO - Ref Frame 1998-6, Eubanks June 1998

   J1642+3948        16 41 17.606463   * 16 42 58.810200     16 43 00.657353 
   1641+399          39 54 10.81592    * 39 48 36.99500      39 48 39.50438 
 * 3C345             From catalog imbedded in main SCHED input file.
   J1642+39          JVAS-Patnaik et al. 1992, mnras, 254, 655; S8.4GHz=5182 mJy

   J2136+0041        21 34 05.207384   * 21 36 38.586319     21 36 39.327412 
   2134+00           00 28 25.08063    * 00 41 54.21345      00 41 55.82342 
 * 2134+004          From catalog imbedded in main SCHED input file.
   J2136+00          USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   LS5039             155.1
   J1825-17           156.1
   J1837-15           152.8
   J1911-20           146.2
   3C345              117.8
   2134+004           105.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

