!*  Schedule for VLBA_FD   *!
!*  Experiment GG038C   *!
!* Schedule Version:       2.00 *!
!* Processed by SCHED version: Short term release of 12 Feb. 2001 *!
!* PI:       GABRIELE GIOVANNINI *!
!* Address:  ISTITUTO DI RADIOASTRONOMIA *!
!*           VIA GOBETTI 101 *!
!*           I-40129 BOLOGNA, ITALY *!
!*  *!
!* Phone:    +39-051-6399415 *!
!* EMAIL:    GGIOVANN@IRA.BO.CNR.IT *!
!* Fax:      +39-051-6399431 *!
!* Phone during observation: +39-051-6399415 *!
!* Observing mode: VLBA 128-8-1 - continuum at 3.6cm and 2cm *!
!* Notes:    Send Logs and Calibration Info to the PI *!
!*           One Thin Tape *!
!*           Greg Taylor is the local contact person *!
!*           at 4cm I am using a personal setup by H.Langevelde:gg038c.set *!
!*  Start at 00h21m09s     Sat, 2001 Jun 02  Day of year  153   *!
program=GG038C  
autoallocate=on
autoreverse=on

!* The first scan is preceeded by a setup scan *!
!* that ends at the start time of the first scan  *!

!* --- Scan from 00h21m09s to 00h25m09s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
maxcaltime= 120
fe=(2,4cm),(4,4cm)
fexfer=(2,norm)
noise=(1,low-s),(2,low-s),(3,low-s),(4,low-s)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
logging=STANDARD
nchan= 8
format=VLBA1:4
barrel=roll_auto
ifdistr=(1,0),(2,0),(3,0),(4,0)
baseband=(1,1),(2,2),(3,1),(4,2),(5,3),(6,4),(7,3),(8,4)
ifchan=(1,B),(2,D),(3,B),(4,D),(5,B),(6,D),(7,B),(8,D)
sideband=(1,L),(2,L),(3,U),(4,U),(5,L),(6,L),(7,U),(8,U)
bits=(1,1),(2,1),(3,1),(4,1),(5,1),(6,1),(7,1),(8,1)
period=(1,1),(2,1),(3,1),(4,1),(5,1),(6,1),(7,1),(8,1)
level=(1,-1),(2,-1),(3,-1),(4,-1),(5,-1),(6,-1),(7,-1),(8,-1)
azcolim=   0.00  elcolim=   0.00
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
bbfilter=(1,8M),(2,8M),(3,8M),(4,8M),(5,8M),(6,8M),(7,8M),(8,8M)
pcal=1MHZ
pcalxbit1=(1,S1),(2,S3),(3,S5),(4,S7),(5,S1),(6,S3),(7,S5),(8,S7)
pcalxbit2=(1,S2),(2,S4),(3,S6),(4,S8),(5,S2),(6,S4),(7,S6),(8,S8)
pcalxfreq1=(1,490),(2,510),(3,490),(4,510),(5,6490),(6,6510),(7,6490),(8,6510)
pcalxfreq2=(1,490),(2,510),(3,490),(4,510),(5,6490),(6,6510),(7,6490),(8,6510)
samplerate=16M
tape=(1,STOP)   write=(1,off)
  date = 2001Jun02
stop=00h21m09s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=00h25m09s   !NEXT!

!* --- Scan from 00h27m38s to 00h42m38s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=00h27m38s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=00h42m38s   !NEXT!

!* --- Scan from 00h43m18s to 00h58m18s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=00h43m18s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=00h58m18s   !NEXT!

!* --- Scan from 00h58m58s to 01h08m58s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=00h58m58s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=01h08m58s   !NEXT!

!* --- Scan from 01h11m12s to 01h15m12s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=01h11m12s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=01h15m12s   !NEXT!

!* --- Scan from 01h17m24s to 01h37m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=01h17m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=01h37m24s   !NEXT!

!* --- Scan from 01h39m24s to 01h59m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=01h39m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=01h59m24s   !NEXT!

!* --- Scan from 02h00m04s to 02h11m04s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=02h00m04s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h11m04s   !NEXT!

!* --- Scan from 02h11m44s to 02h22m44s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=02h11m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h22m44s   !NEXT!

!* --- Scan from 02h23m24s to 02h34m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=02h23m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h34m24s   !NEXT!

!* --- Scan from 02h35m04s to 02h46m04s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=02h35m04s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h46m04s   !NEXT!

!* --- Scan from 02h46m44s to 02h59m44s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=02h46m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h59m44s   !NEXT!

!* --- Scan from 03h00m24s to 03h13m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=03h00m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=03h13m24s   !NEXT!

!* --- Scan from 03h14m04s to 03h27m04s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=03h14m04s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=03h27m04s   !NEXT!

!* --- Scan from 03h30m12s to 03h35m12s   Sat, 2001 Jun 02 --- *!
sname='3C279'  ra=12h56m11.166558s  dec=-05d47'21.52460"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=03h30m12s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=03h35m12s   !NEXT!

!* --- Scan from 03h43m12s to 03h47m12s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=03h43m12s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=03h47m12s   !NEXT!

!* --- Scan from 03h49m21s to 04h02m21s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=03h49m21s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h02m21s   !NEXT!

!* --- Scan from 04h03m01s to 04h15m01s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=04h03m01s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h15m01s   !NEXT!

!* --- Scan from 04h15m41s to 04h25m41s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=04h15m41s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h25m41s   !NEXT!

!* --- Scan from 04h29m20s to 04h34m20s   Sat, 2001 Jun 02 --- *!
sname='3C279'  ra=12h56m11.166558s  dec=-05d47'21.52460"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=04h29m20s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h34m20s   !NEXT!

!* --- Scan from 04h38m01s to 04h49m01s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=04h38m01s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h49m01s   !NEXT!

!* --- Scan from 04h49m41s to 05h00m41s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=04h49m41s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h00m41s   !NEXT!

!* --- Scan from 05h01m21s to 05h12m21s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=05h01m21s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h12m21s   !NEXT!

!* --- Scan from 05h13m01s to 05h20m01s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=05h13m01s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h20m01s   !NEXT!

!* --- Scan from 05h24m44s to 05h28m44s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=05h24m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h28m44s   !NEXT!

!* --- Scan from 05h32m22s to 05h37m22s   Sat, 2001 Jun 02 --- *!
sname='1749+096'  ra=17h51m32.818573s  dec= 09d39'00.72837"  qual=999  calib='N'
fe=(2,4cm),(4,4cm)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
tape=(1,STOP)   write=(1,off)
stop=05h32m22s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h37m22s   !NEXT!

!* --- Scan from 05h40m44s to 05h57m44s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=05h40m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h57m44s   !NEXT!

!* --- Scan from 05h58m24s to 06h15m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=05h58m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h15m24s   !NEXT!

!* --- Scan from 06h16m04s to 06h21m04s   Sat, 2001 Jun 02 --- *!
sname='3C345'  ra=16h42m58.810200s  dec= 39d48'36.99500"  qual=999  calib='M'
tape=(1,STOP)   write=(1,off)
stop=06h16m04s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h21m04s   !NEXT!

!* --- Scan from 06h21m44s to 06h39m44s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=06h21m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h39m44s   !NEXT!

!* --- Scan from 06h40m24s to 06h57m24s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=06h40m24s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h57m24s   !NEXT!

!* --- Scan from 07h10m17s to 07h14m17s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=07h10m17s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h14m17s   !NEXT!

!* --- Scan from 07h18m02s to 07h23m02s   Sat, 2001 Jun 02 --- *!
sname='3C279'  ra=12h56m11.166558s  dec=-05d47'21.52460"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=07h18m02s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h23m02s   !NEXT!

!* --- Scan from 07h26m20s to 07h44m20s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=07h26m20s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h44m20s   !NEXT!

!* --- Scan from 07h46m04s to 07h50m04s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=07h46m04s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h50m04s   !NEXT!

!* --- Scan from 07h50m44s to 07h54m44s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
fe=(2,4cm),(4,4cm)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
tape=(1,STOP)   write=(1,off)
stop=07h50m44s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h54m44s   !NEXT!

!* --- Scan from 07h58m10s to 08h16m10s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=07h58m10s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=08h16m10s   !NEXT!

!* --- Scan from 08h16m50s to 08h38m50s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=08h16m50s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=08h38m50s   !NEXT!

!* --- Scan from 08h40m50s to 09h02m50s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,4cm),(4,4cm)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
tape=(1,STOP)   write=(1,off)
stop=08h40m50s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h02m50s   !NEXT!

!* --- Scan from 09h03m30s to 09h21m30s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=09h03m30s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h21m30s   !NEXT!

!* --- Scan from 09h23m19s to 09h27m19s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=09h23m19s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h27m19s   !NEXT!

!* --- Scan from 09h27m59s to 09h31m59s   Sat, 2001 Jun 02 --- *!
sname='OQ208'  ra=14h07m00.394411s  dec= 28d27'14.68994"  qual=999  calib='N'
fe=(2,4cm),(4,4cm)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
tape=(1,STOP)   write=(1,off)
stop=09h27m59s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h31m59s   !NEXT!

!* --- Scan from 09h34m33s to 09h52m33s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=09h34m33s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h52m33s   !NEXT!

!* --- Scan from 09h53m13s to 10h04m13s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=09h53m13s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h04m13s   !NEXT!

!* --- Scan from 10h05m59s to 10h11m29s   Sat, 2001 Jun 02 --- *!
sname='1749+096'  ra=17h51m32.818573s  dec= 09d39'00.72837"  qual=999  calib='N'
tape=(1,STOP)   write=(1,off)
stop=10h05m59s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h11m29s   !NEXT!

!* --- Scan from 10h12m09s to 10h17m39s   Sat, 2001 Jun 02 --- *!
sname='1749+096'  ra=17h51m32.818573s  dec= 09d39'00.72837"  qual=999  calib='N'
fe=(2,4cm),(4,4cm)
synth=( 1, 7.6),( 2,15.4),( 3,15.4)
bbsynth=( 1,813.49),( 2,813.49),( 3,813.49),( 4,813.49),( 5,829.49),( 6,829.49)
bbsynth=( 7,829.49),( 8,829.49)
tape=(1,STOP)   write=(1,off)
stop=10h12m09s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h17m39s   !NEXT!

!* --- Scan from 10h23m26s to 10h34m26s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=10h23m26s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h34m26s   !NEXT!

!* --- Scan from 10h35m06s to 10h46m06s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
tape=(1,STOP)   write=(1,off)
stop=10h35m06s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h46m06s   !NEXT!

!* --- Scan from 10h46m46s to 10h59m46s   Sat, 2001 Jun 02 --- *!
sname='3C338'  ra=16h28m38.243708s  dec= 39d33'04.18682"  qual=999  calib=' '
fe=(2,2cm),(4,2cm)
synth=( 1,14.6),( 2,10.9),( 3,10.9)
bbsynth=( 1,757.49),( 2,757.49),( 3,757.49),( 4,757.49),( 5,773.49),( 6,773.49)
bbsynth=( 7,773.49),( 8,773.49)
tape=(1,STOP)   write=(1,off)
stop=10h46m46s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h59m46s   !NEXT!

tape=(1,STOP)    write=(1,off)   dur=0s 
stop=10h59m51s  !NEXT! 
     !QUIT! 
