  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GP042 18cm global observation of M82
 Exp. Code:  GP042   


Schedule Version:       1.10                                              
Processed by SCHED version: NRAO internal release of 4 October 2004       

PI:       Alan Pedlar                                                     

Address:  Jodrell Bank Observatory                                        
          Macclesfield                                                    
          Cheshire, England                                               
                                                                          

Phone:    (+44) 1477 571321                                               
EMAIL:    ap@jb.man.ac.uk                                                 
Fax:                                                                      
Phone during observation: (+44) 1477 571321                               

Observing mode: 128-4-2-UL                                                

Notes:    WSRT - use single antenna ONLY                                  
          JB1 individually scheduled                                      
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

 ---------- Forward pass 1 ----------

 Next scan frequencies:  1659.49  1659.49  1667.49  1667.49
 Next BBC frequencies:    740.51   740.51   732.51   732.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00

13 00 00  J0958+65     16 49 50  22.7 -26.0  6.8      65.5     0   1  1      0  13 00 00
13 02 10  ---          16 52 01  22.5 -25.9  6.9      65.1   130   F  1    867

13 02 10  M82          16 52 01  23.9 -21.7  6.9      66.0    -9   1  1    867  13 02 10
13 06 20  ---          16 56 11  23.6 -21.5  7.0      65.1   241   F  1   2533

 ---------- Forward pass 1 ----------

13 06 20  J0958+65     16 56 11  22.1 -25.7  6.9      64.2    -9   1  1   2533  13 06 20
13 08 30  ---          16 58 22  21.9 -25.6  7.0      63.7   121   F  1   3400

13 08 30  M82          16 58 22  23.4 -21.4  7.0      64.6    -9   1  1   3400  13 08 30
13 12 40  ---          17 02 32  23.1 -21.2  7.1      63.7   241   F  1   5067

 ---------- Forward pass 1 ----------

13 12 40  J0958+65     17 02 32  21.5 -25.4  7.1      62.8    -9   1  1   5067  13 12 40
13 14 50  ---          17 04 43  21.3 -25.2  7.1      62.4   121   F  1   5933

13 14 50  M82          17 04 43  22.9 -21.2  7.1      63.3    -9   1  1   5933  13 14 50
13 19 00  ---          17 08 53  22.6 -21.0  7.2      62.4   241   F  1   7600

 ---------- Forward pass 1 ----------

13 19 00  J0958+65     17 08 53  20.9 -25.0  7.2      61.5    -9   1  1   7600  13 19 00
13 21 10  ---          17 11 04  20.7 -24.9  7.2      61.1   121   F  1   8467

13 21 10  M82          17 11 04  22.5 -20.9  7.2      61.9    -9   1  1   8467  13 21 10
13 25 20  ---          17 15 14  22.1 -20.7  7.3      61.0   241   F  1  10133

 ---------- Forward pass 1 ----------

13 25 20  J0958+65     17 15 14  20.4 -24.7  7.3      60.2   -10   1  1  10133  13 25 20
13 27 30  ---          17 17 25  20.2 -24.6  7.3      59.7   120   F  1  11000

13 27 30  M82          17 17 25  22.0 -20.6  7.4      60.5   -10   1  1  11000  13 27 30
13 31 40  ---          17 21 35  21.7 -20.4  7.4      59.6   240   F  1  12667
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

 ---------- Forward pass 1 ----------

13 31 40  J0958+65     17 21 35  19.8 -24.3  7.4      58.9   -10   1  1  12667  13 31 40
13 33 50  ---          17 23 46  19.6 -24.2  7.4      58.4   120   F  1  13533

13 33 50  M82          17 23 46  21.5 -20.3  7.5      59.1   -10   1  1  13533  13 33 50
13 38 00  ---          17 27 56  21.2 -20.1  7.5      58.2   240   F  1  15200

13 38 00  J0958+65     17 27 56  19.2 -24.0  7.5      57.6   -10   1  1  15200  13 38 00
13 40 00  ---          17 29 57  19.1 -23.8  7.5      57.1   110   F  1  16000

13 40 00  M82          17 29 57  21.0 -20.0  7.6      57.8   -10   1  1  16000  13 40 00
13 44 00  ---          17 33 57  20.7 -19.8  7.6      56.9   230   F  1  17600

 ---------- Reverse pass 1 ----------

13 44 40  J0958+65     17 34 38  18.7 -23.6  7.6      56.2    30   1  2  17600  13 44 40
13 46 50  ---          17 36 48  18.5 -23.4  7.6      55.7   130   R  1  16733

13 46 50  M82          17 36 48  20.5 -19.6  7.7      56.3   -10   1  2  16733  13 46 50
13 51 00  ---          17 40 59  20.2 -19.4  7.7      55.4   240   R  1  15067

13 51 00  J0958+65     17 40 59  18.1 -23.2  7.7      54.8   -10   1  2  15067  13 51 00
13 53 10  ---          17 43 09  17.9 -23.0  7.7      54.4   120   R  1  14200

13 53 10  M82          17 43 09  20.1 -19.3  7.8      54.9   -10   1  2  14200  13 53 10
13 57 20  ---          17 47 20  19.8 -19.1  7.8      54.0   240   R  1  12533

13 57 20  J0958+65     17 47 20  17.6 -22.8  7.8      53.5   -10   1  2  12533  13 57 20
13 59 30  ---          17 49 30  17.4 -22.6  7.8      53.1   120   R  1  11667

13 59 30  M82          17 49 30  19.6 -19.0  7.9      53.6   -10   1  2  11667  13 59 30
14 03 40  ---          17 53 41  19.3 -18.7  8.0      52.7   240   R  1  10000

14 03 40  J0958+65     17 53 41  17.1 -22.3  7.9      52.2   -11   1  2  10000  14 03 40
14 05 50  ---          17 55 51  16.9 -22.2  7.9      51.7   119   R  1   9133

14 05 50  M82          17 55 51  19.2 -18.6  8.0      52.2   -11   1  2   9133  14 05 50
14 10 00  ---          18 00 02  18.9 -18.4  8.1      51.3   239   R  1   7467

14 10 00  J0958+65     18 00 02  16.5 -21.9  8.0      50.9   -11   1  2   7467  14 10 00
14 12 10  ---          18 02 12  16.4 -21.8  8.0      50.4   119   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

14 12 10  M82          18 02 12  18.8 -18.3  8.1      50.8   -11   1  2   6600  14 12 10
14 16 20  ---          18 06 23  18.5 -18.0  8.2      49.9   239   R  1   4933

14 16 20  J0958+65     18 06 23  16.0 -21.5  8.1      49.6   -11   1  2   4933  14 16 20
14 18 30  ---          18 08 33  15.9 -21.3  8.2      49.1   119   R  1   4067

14 18 30  M82          18 08 33  18.3 -17.9  8.2      49.4   -11   1  2   4067  14 18 30
14 22 40  ---          18 12 44  18.1 -17.6  8.3      48.5   239   R  1   2400

14 22 40  J0958+65     18 12 44  15.5 -21.0  8.2      48.2   -11   1  2   2400  14 22 40
14 24 40  ---          18 14 44  15.4 -20.9  8.3      47.8   109   R  1   1600

14 24 40  M82          18 14 44  17.9 -17.5  8.3      48.1   -11   1  2   1600  14 24 40
14 28 40  ---          18 18 45  17.7 -17.3  8.4      47.2   229   R  1      0

 ---------- Forward pass 2 ----------

14 30 40  J0958+65     18 20 45  14.9 -20.4  8.4      46.6   109   1  3      0  14 30 40
14 32 50  ---          18 22 55  14.8 -20.3  8.4      46.1   130   F  1    867

14 32 50  M82          18 22 55  17.4 -17.0  8.4      46.3   -11   1  3    867  14 32 50
14 37 00  ---          18 27 06  17.2 -16.7  8.5      45.4   239   F  1   2533

14 37 00  J0958+65     18 27 06  14.5 -20.0  8.5      45.2   -11   1  3   2533  14 37 00
14 39 10  ---          18 29 16  14.3 -19.8  8.5      44.8   119   F  1   3400

14 39 10  M82          18 29 16  17.0 -16.6  8.5      45.0   -11   1  3   3400  14 39 10
14 43 20  ---          18 33 27  16.8 -16.3  8.6      44.1   239   F  1   5067

14 43 20  J0958+65     18 33 27  14.0 -19.5  8.6      43.9   -12   1  3   5067  14 43 20
14 45 30  ---          18 35 38  13.8 -19.3  8.6      43.5   118   F  1   5933

14 45 30  M82          18 35 38  16.6 -16.2  8.7      43.6   -12   1  3   5933  14 45 30
14 49 40  ---          18 39 48  16.4 -15.9  8.7      42.7   238   F  1   7600

14 49 40  J0958+65     18 39 48  13.5 -19.0  8.7      42.6   -12   1  3   7600  14 49 40
14 51 50  ---          18 41 59  13.4 -18.8  8.7      42.1   118   F  1   8467

14 51 50  M82          18 41 59  16.3 -15.8  8.8      42.2   -12   1  3   8467  14 51 50
14 56 00  ---          18 46 09  16.0 -15.5  8.8      41.3   238   F  1  10133

14 56 00  J0958+65     18 46 09  13.1 -18.5  8.8      41.2   -12   1  3  10133  14 56 00
14 58 10  ---          18 48 20  13.0 -18.3  8.8      40.8   118   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

14 58 10  M82          18 48 20  15.9 -15.3  8.9      40.9   -12   1  3  11000  14 58 10
15 02 20  ---          18 52 30  15.7 -15.0  8.9      40.0   238   F  1  12667

15 02 20  J0958+65     18 52 30  12.7 -18.0  8.9      39.9   -12   1  3  12667  15 02 20
15 04 30  ---          18 54 41  12.5 -17.8  8.9      39.5   118   F  1  13533

15 04 30  M82          18 54 41  15.5 -14.9  9.0      39.5   -12   1  3  13533  15 04 30
15 08 40  ---          18 58 51  15.3 -14.6  9.0      38.6   238   F  1  15200

15 08 40  J0958+65     18 58 51  12.3 -17.5  9.0      38.6   -12   1  3  15200  15 08 40
15 10 40  ---          19 00 52  12.1 -17.3  9.0      38.2   108   F  1  16000

15 10 40  M82          19 00 52  15.2 -14.5  9.1      38.2   -12   1  3  16000  15 10 40
15 14 40  ---          19 04 52  15.0 -14.2  9.1      37.3   228   F  1  17600

 ---------- Reverse pass 2 ----------

15 15 20  J0958+65     19 05 32  11.8 -16.9  9.1      37.2    28   1  4  17600  15 15 20
15 17 30  ---          19 07 43  11.7 -16.7  9.1      36.7   130   R  1  16733

15 17 30  M82          19 07 43  14.8 -14.0  9.2      36.7   -12   1  4  16733  15 17 30
15 21 40  ---          19 11 53  14.6 -13.7  9.3      35.8   238   R  1  15067

15 21 40  J0958+65     19 11 53  11.4 -16.4  9.2      35.8   -12   1  4  15067  15 21 40
15 23 50  ---          19 14 04  11.3 -16.2  9.2      35.4   118   R  1  14200

15 23 50  M82          19 14 04  14.5 -13.5  9.3      35.3   -12   1  4  14200  15 23 50
15 28 00  ---          19 18 14  14.3 -13.2  9.4      34.4   238   R  1  12533

15 28 00  J0958+65     19 18 14  11.1 -15.8  9.3      34.5   -12   1  4  12533  15 28 00
15 30 10  ---          19 20 25  10.9 -15.6  9.4      34.0   118   R  1  11667

15 30 10  M82          19 20 25  14.2 -13.0  9.4      33.9   -13   1  4  11667  15 30 10
15 34 20  ---          19 24 36  14.0 -12.7  9.5      33.0   237   R  1  10000

15 34 20  J0958+65     19 24 36  10.7 -15.3  9.4      33.2   -13   1  4  10000  15 34 20
15 36 30  ---          19 26 46  10.6 -15.1  9.5      32.7   117   R  1   9133

15 36 30  M82          19 26 46  13.9 -12.6  9.5      32.6   -13   1  4   9133  15 36 30
15 40 40  ---          19 30 57  13.7 -12.2  9.6      31.7   237   R  1   7467

15 40 40  J0958+65     19 30 57  10.3 -14.7  9.5      31.8   -13   1  4   7467  15 40 40
15 42 50  ---          19 33 07  10.2 -14.5  9.6      31.4   117   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

15 42 50  M82          19 33 07  13.6 -12.1  9.6      31.2   -13   1  4   6600  15 42 50
15 47 00  ---          19 37 18  13.4 -11.8  9.7      30.3   237   R  1   4933

15 47 00  J0958+65     19 37 18  10.0 -14.1  9.6      30.5   -13   1  4   4933  15 47 00
15 49 10  ---          19 39 28   9.9 -13.9  9.7      30.0   117   R  1   4067

15 49 10  M82          19 39 28  13.3 -11.6  9.7      29.8   -13   1  4   4067  15 49 10
15 53 20  ---          19 43 39  13.1 -11.3  9.8      28.9   237   R  1   2400

15 53 20  J0958+65     19 43 39   9.7 -13.5  9.7      29.1   -13   1  4   2400  15 53 20
15 55 20  ---          19 45 39   9.6 -13.4  9.8      28.7   107   R  1   1600

15 55 20  M82          19 45 39  13.1 -11.1  9.8      28.5   -13   1  4   1600  15 55 20
15 59 20  ---          19 49 40  12.9 -10.8  9.9      27.6   227   R  1      0

 ---------- Forward pass 3 ----------

16 01 20  J0958+65     19 51 40   9.3 -12.8  9.9      27.4   107   1  5      0  16 01 20
16 03 30  ---          19 53 50   9.2 -12.6  9.9      27.0   130   F  1    867

16 03 30  M82          19 53 50  12.7 -10.5 10.0      26.7   -13   1  5    867  16 03 30
16 07 40  ---          19 58 01  12.6 -10.1 10.0      25.8   237   F  1   2533

16 07 40  J0958+65     19 58 01   9.0 -12.2 10.0      26.1   -13   1  5   2533  16 07 40
16 09 50  ---          20 00 11   8.9 -12.0 10.0      25.6   117   F  1   3400

16 09 50  M82          20 00 11  12.5 -10.0 10.1      25.3   -13   1  5   3400  16 09 50
16 14 00  ---          20 04 22  12.3  -9.6 10.1      24.4   237   F  1   5067

16 14 00  J0958+65     20 04 22   8.7 -11.6 10.1      24.7   -13   1  5   5067  16 14 00
16 16 10  ---          20 06 32   8.6 -11.4 10.1      24.3   117   F  1   5933

16 16 10  M82          20 06 32  12.3  -9.4 10.2      23.9   -13   1  5   5933  16 16 10
16 20 20  ---          20 10 43  12.1  -9.1 10.2      23.0   237   F  1   7600

16 20 20  J0958+65     20 10 43   8.4 -11.0 10.2      23.4   -13   1  5   7600  16 20 20
16 22 30  ---          20 12 53   8.4 -10.8 10.2      22.9   117   F  1   8467

16 22 30  M82          20 12 53  12.0  -8.9 10.3      22.6   -13   1  5   8467  16 22 30
16 26 40  ---          20 17 04  11.9  -8.6 10.3      21.7   237   F  1  10133

16 26 40  J0958+65     20 17 04   8.2 -10.4 10.3      22.0   -13   1  5  10133  16 26 40
16 28 50  ---          20 19 14   8.1 -10.2 10.3      21.5   117   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

16 28 50  M82          20 19 14  11.8  -8.4 10.4      21.2   -13   1  5  11000  16 28 50
16 33 00  ---          20 23 25  11.7  -8.1 10.5      20.3   237   F  1  12667

16 33 00  J0958+65     20 23 25   7.9  -9.8 10.4      20.7   -14   1  5  12667  16 33 00
16 35 10  ---          20 25 36   7.9  -9.6 10.4      20.2   116   F  1  13533

16 35 10  M82          20 25 36  11.6  -7.9 10.5      19.8   -14   1  5  13533  16 35 10
16 39 20  ---          20 29 46  11.5  -7.5 10.6      18.9   236   F  1  15200

16 39 20  J0958+65     20 29 46   7.7  -9.1 10.5      19.3   -14   1  5  15200  16 39 20
16 41 20  ---          20 31 47   7.7  -9.0 10.5      18.9   106   F  1  16000

16 41 20  M82          20 31 47  11.5  -7.4 10.6      18.5   -14   1  5  16000  16 41 20
16 45 20  ---          20 35 47  11.4  -7.0 10.7      17.6   226   F  1  17600

 ---------- Reverse pass 3 ----------

16 46 00  J0958+65     20 36 27   7.5  -8.5 10.6      17.9    26   1  6  17600  16 46 00
16 48 10  ---          20 38 38   7.4  -8.3 10.7      17.4   130   R  1  16733

16 48 10  M82          20 38 38  11.3  -6.8 10.7      17.0   -14   1  6  16733  16 48 10
16 52 20  ---          20 42 48  11.2  -6.4 10.8      16.1   236   R  1  15067

16 52 20  J0958+65     20 42 48   7.3  -7.9 10.7      16.5   -14   1  6  15067  16 52 20
16 54 30  ---          20 44 59   7.2  -7.6 10.8      16.0   116   R  1  14200

16 54 30  M82          20 44 59  11.1  -6.2 10.8      15.6   -14   1  6  14200  16 54 30
16 58 40  ---          20 49 09  11.0  -5.9 10.9      14.7   236   R  1  12533

16 58 40  J0958+65     20 49 09   7.1  -7.2 10.8      15.1   -14   1  6  12533  16 58 40
17 00 50  ---          20 51 20   7.1  -7.0 10.9      14.7   116   R  1  11667

17 00 50  M82          20 51 20  11.0  -5.7 10.9      14.2   -14   1  6  11667  17 00 50
17 05 00  ---          20 55 30  10.9  -5.3 11.0      13.3   236   R  1  10000

17 05 00  J0958+65     20 55 30   7.0  -6.6 10.9      13.8   -14   1  6  10000  17 05 00
17 07 10  ---          20 57 41   6.9  -6.4 11.0      13.3   116   R  1   9133

17 07 10  M82          20 57 41  10.9  -5.1 11.0      12.8   -14   1  6   9133  17 07 10
17 11 20  ---          21 01 51  10.8  -4.8 11.1      11.9   236   R  1   7467

17 11 20  J0958+65     21 01 51   6.8  -5.9 11.0      12.4   -14   1  6   7467  17 11 20
17 13 30  ---          21 04 02   6.8  -5.7 11.1      11.9   116   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

17 13 30  M82          21 04 02  10.7  -4.6 11.1      11.4   -14   1  6   6600  17 13 30
17 17 40  ---          21 08 13  10.7  -4.2 11.2      10.5   236   R  1   4933

17 17 40  J0958+65     21 08 13   6.7  -5.3 11.1      11.0   -14   1  6   4933  17 17 40
17 19 50  ---          21 10 23   6.6  -5.1 11.2      10.6   116   R  1   4067

17 19 50  M82          21 10 23  10.6  -4.0 11.2      10.0   -14   1  6   4067  17 19 50
17 24 00  ---          21 14 34  10.6  -3.7 11.3       9.1   236   R  1   2400

17 24 00  J0958+65     21 14 34   6.6  -4.6 11.3       9.7   -14   1  6   2400  17 24 00
17 26 00  ---          21 16 34   6.5  -4.4 11.3       9.2   106   R  1   1600

17 26 00  M82          21 16 34  10.6  -3.5 11.3       8.7   -14   1  6   1600  17 26 00
17 30 00  ---          21 20 35  10.5  -3.2 11.4       7.8   226   R  1      0

 ----------  Sources Set at MK (No SC or MK) ----------

17 32 00  J0958+65     21 22 35   6.4  -3.8 11.4       7.9   106   1  7      0  17 32 00
17 34 10  ---          21 24 45   6.4  -3.6 11.4       7.5   130   F  1    867

17 34 10  M82          21 24 45  10.5  -2.8 11.5       6.9   -14   1  7    867  17 34 10
17 38 20  ---          21 28 56  10.4  -2.4 11.5       6.0   236   F  1   2533

17 38 20  J0958+65     21 28 56   6.4  -3.1 11.5       6.6   -14   1  7   2533  17 38 20
17 40 30  ---          21 31 06   6.3  -2.9 11.5       6.1   116   F  1   3400

17 40 30  M82          21 31 06  10.4  -2.2 11.6       5.5   -14   1  7   3400  17 40 30
17 44 40  ---          21 35 17  10.4  -1.9 11.6       4.6   236   F  1   5067

17 44 40  J0958+65     21 35 17   6.3  -2.5 11.6       5.2   -14   1  7   5067  17 44 40
17 46 50  ---          21 37 27   6.3  -2.3 11.6       4.7   116   F  1   5933

17 46 50  M82          21 37 27  10.4  -1.7 11.7       4.1   -14   1  7   5933  17 46 50
17 51 00  ---          21 41 38  10.3  -1.3 11.8       3.2   236   F  1   7600

17 51 00  J0958+65     21 41 38   6.2  -1.8 11.7       3.8   -14   1  7   7600  17 51 00
17 53 10  ---          21 43 48   6.2  -1.6 11.7       3.3   116   F  1   8467

17 53 10  M82          21 43 48  10.3  -1.1 11.8       2.7   -14   1  7   8467  17 53 10
17 57 20  ---          21 47 59  10.3  -0.7 11.9       1.8   236   F  1  10133

17 57 20  J0958+65     21 47 59   6.2  -1.2 11.8       2.4   -14   1  7  10133  17 57 20
17 59 30  ---          21 50 09   6.2  -0.9 11.8       2.0   116   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

17 59 30  M82          21 50 09  10.3  -0.5 11.9       1.4   -14   1  7  11000  17 59 30
18 03 40  ---          21 54 20  10.3  -0.2 12.0       0.4   236   F  1  12667

18 03 40  J0958+65     21 54 20   6.2  -0.5 11.9       1.1   -14   1  7  12667  18 03 40
18 05 50  ---          21 56 30   6.2  -0.3 12.0       0.6   116   F  1  13533

18 05 50  M82          21 56 30  10.3   0.0-12.0       0.0   -14   1  7  13533  18 05 50
18 10 00  ---          22 00 41  10.3   0.4-11.9      -0.9   236   F  1  15200

18 10 00  J0958+65     22 00 41   6.2   0.2-12.0      -0.3   -14   1  7  15200  18 10 00
18 12 00  ---          22 02 41   6.2   0.4-11.9      -0.7   106   F  1  16000

18 12 00  M82          22 02 41  10.3   0.6-11.9      -1.4   -14   1  7  16000  18 12 00
18 16 00  ---          22 06 42  10.3   0.9-11.8      -2.3   226   F  1  17600

 ---------- Reverse pass 4 ----------

18 16 40  J0958+65     22 07 22   6.2   0.8-11.9      -1.8    26   1  8  17600  18 16 40
18 18 50  ---          22 09 33   6.2   1.1-11.8      -2.2   130   R  1  16733

18 18 50  M82          22 09 33  10.3   1.2-11.8      -2.9   -14   1  8  16733  18 18 50
18 23 00  ---          22 13 43  10.3   1.5-11.7      -3.8   236   R  1  15067

18 23 00  J0958+65     22 13 43   6.2   1.5-11.8      -3.1   -14   1  8  15067  18 23 00
18 25 10  ---          22 15 54   6.2   1.7-11.7      -3.6   116   R  1  14200

18 25 10  M82          22 15 54  10.4   1.7-11.7      -4.3   -14   1  8  14200  18 25 10
18 29 20  ---          22 20 04  10.4   2.1-11.6      -5.2   236   R  1  12533

18 29 20  J0958+65     22 20 04   6.3   2.2-11.7      -4.5   -14   1  8  12533  18 29 20
18 31 30  ---          22 22 15   6.3   2.4-11.6      -5.0   116   R  1  11667

18 31 30  M82          22 22 15  10.4   2.3-11.6      -5.7   -14   1  8  11667  18 31 30
18 35 40  ---          22 26 25  10.4   2.7-11.5      -6.6   236   R  1  10000

18 35 40  J0958+65     22 26 25   6.3   2.8-11.5      -5.9   -14   1  8  10000  18 35 40
18 37 50  ---          22 28 36   6.3   3.1-11.5      -6.3   116   R  1   9133

18 37 50  M82          22 28 36  10.5   2.8-11.5      -7.0   -14   1  8   9133  18 37 50
18 42 00  ---          22 32 46  10.5   3.2-11.4      -8.0   236   R  1   7467

18 42 00  J0958+65     22 32 46   6.4   3.5-11.4      -7.3   -14   1  8   7467  18 42 00
18 44 10  ---          22 34 57   6.4   3.7-11.4      -7.7   116   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

18 44 10  M82          22 34 57  10.5   3.4-11.4      -8.4   -14   1  8   6600  18 44 10
18 48 20  ---          22 39 07  10.6   3.8-11.3      -9.3   236   R  1   4933

18 48 20  J0958+65     22 39 07   6.5   4.1-11.3      -8.6   -14   1  8   4933  18 48 20
18 50 30  ---          22 41 18   6.5   4.4-11.3      -9.1   116   R  1   4067

18 50 30  M82          22 41 18  10.6   4.0-11.3      -9.8   -14   1  8   4067  18 50 30
18 54 40  ---          22 45 28  10.7   4.3-11.2     -10.7   236   R  1   2400

18 54 40  J0958+65     22 45 28   6.6   4.8-11.2     -10.0   -14   1  8   2400  18 54 40
18 56 40  ---          22 47 29   6.6   5.0-11.2     -10.4   106   R  1   1600

18 56 40  M82          22 47 29  10.7   4.5-11.1     -11.2   -14   1  8   1600  18 56 40
19 00 40  ---          22 51 29  10.8   4.8-11.1     -12.0   226   R  1      0

 ----------  Sources rise at SC ----------

19 02 40  J0958+65     22 53 30   6.8   5.6-11.1     -11.7   106   1  9      0  19 02 40
19 04 50  ---          22 55 40   6.8   5.8-11.1     -12.2   130   F  1    867

19 04 50  M82          22 55 40  10.9   5.2-11.0     -13.0   -14   1  9    867  19 04 50
19 09 00  ---          22 59 51  11.0   5.6-10.9     -13.9   236   F  1   2533

19 09 00  J0958+65     22 59 51   6.9   6.3-11.0     -13.1   -14   1  9   2533  19 09 00
19 11 10  ---          23 02 01   6.9   6.5-11.0     -13.6   116   F  1   3400

19 11 10  M82          23 02 01  11.0   5.7-10.9     -14.3   -14   1  9   3400  19 11 10
19 15 20  ---          23 06 12  11.1   6.1-10.8     -15.3   236   F  1   5067

19 15 20  J0958+65     23 06 12   7.0   6.9-10.9     -14.5   -14   1  9   5067  19 15 20
19 17 30  ---          23 08 22   7.1   7.1-10.8     -14.9   116   F  1   5933

19 17 30  M82          23 08 22  11.1   6.3-10.8     -15.7   -14   1  9   5933  19 17 30
19 21 40  ---          23 12 33  11.2   6.6-10.7     -16.6   236   F  1   7600

19 21 40  J0958+65     23 12 33   7.2   7.5-10.8     -15.8   -14   1  9   7600  19 21 40
19 23 50  ---          23 14 43   7.3   7.8-10.7     -16.3   116   F  1   8467

19 23 50  M82          23 14 43  11.3   6.8-10.7     -17.1   -14   1  9   8467  19 23 50
19 28 00  ---          23 18 54  11.4   7.2-10.6     -18.0   236   F  1  10133

19 28 00  J0958+65     23 18 54   7.4   8.2-10.7     -17.2   -14   1  9  10133  19 28 00
19 30 10  ---          23 21 04   7.5   8.4-10.6     -17.7   116   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

19 30 10  M82          23 21 04  11.5   7.4-10.6     -18.5   -14   1  9  11000  19 30 10
19 34 20  ---          23 25 15  11.6   7.7-10.5     -19.4   236   F  1  12667

19 34 20  J0958+65     23 25 15   7.6   8.8-10.6     -18.6   -14   1  9  12667  19 34 20
19 36 30  ---          23 27 25   7.7   9.0-10.5     -19.0   116   F  1  13533

19 36 30  M82          23 27 25  11.7   7.9-10.5     -19.9   -14   1  9  13533  19 36 30
19 40 40  ---          23 31 36  11.8   8.2-10.4     -20.8   236   F  1  15200

19 40 40  J0958+65     23 31 36   7.8   9.4-10.5     -19.9   -14   1  9  15200  19 40 40
19 42 40  ---          23 33 36   7.9   9.6-10.4     -20.3   106   F  1  16000

19 42 40  M82          23 33 36  11.8   8.4-10.4     -21.2   -14   1  9  16000  19 42 40
19 46 40  ---          23 37 37  12.0   8.7-10.3     -22.1   226   F  1  17600

 ---------- Reverse pass 5 ----------

19 47 20  J0958+65     23 38 17   8.1  10.1-10.3     -21.3    26   1 10  17600  19 47 20
19 49 30  ---          23 40 27   8.2  10.3-10.3     -21.8   130   R  1  16733

19 49 30  M82          23 40 27  12.1   9.0-10.3     -22.7   -14   1 10  16733  19 49 30
19 53 40  ---          23 44 38  12.2   9.3-10.2     -23.6   236   R  1  15067

19 53 40  J0958+65     23 44 38   8.3  10.7-10.2     -22.7   -14   1 10  15067  19 53 40
19 55 50  ---          23 46 48   8.4  10.9-10.2     -23.2   116   R  1  14200

19 55 50  M82          23 46 48  12.3   9.5-10.2     -24.1   -14   1 10  14200  19 55 50
20 00 00  ---          23 50 59  12.4   9.8-10.1     -25.0   236   R  1  12533

20 00 00  J0958+65     23 50 59   8.6  11.3-10.1     -24.1   -14   1 10  12533  20 00 00
20 02 10  ---          23 53 10   8.7  11.5-10.1     -24.5   116   R  1  11667

20 02 10  M82          23 53 10  12.5  10.0-10.1     -25.5   -14   1 10  11667  20 02 10
20 06 20  ---          23 57 20  12.7  10.3-10.0     -26.4   236   R  1  10000

20 06 20  J0958+65     23 57 20   8.9  11.9-10.0     -25.4   -14   1 10  10000  20 06 20
20 08 30  ---          23 59 31   8.9  12.1-10.0     -25.9   116   R  1   9133

20 08 30  M82          23 59 31  12.8  10.5 -9.9     -26.8   -14   1 10   9133  20 08 30
20 12 40  ---          00 03 41  12.9  10.8 -9.9     -27.8   236   R  1   7467

20 12 40  J0958+65     00 03 41   9.1  12.5 -9.9     -26.8   -14   1 10   7467  20 12 40
20 14 50  ---          00 05 52   9.2  12.7 -9.9     -27.2   116   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

20 14 50  M82          00 05 52  13.0  11.0 -9.8     -28.2   -14   1 10   6600  20 14 50
20 19 00  ---          00 10 02  13.2  11.3 -9.8     -29.1   236   R  1   4933

20 19 00  J0958+65     00 10 02   9.4  13.1 -9.8     -28.1   -13   1 10   4933  20 19 00
20 21 10  ---          00 12 13   9.5  13.3 -9.8     -28.6   117   R  1   4067

20 21 10  M82          00 12 13  13.3  11.5 -9.7     -29.6   -13   1 10   4067  20 21 10
20 25 20  ---          00 16 23  13.5  11.8 -9.7     -30.5   237   R  1   2400

20 25 20  J0958+65     00 16 23   9.8  13.7 -9.7     -29.5   -13   1 10   2400  20 25 20
20 27 20  ---          00 18 24   9.9  13.9 -9.7     -29.9   107   R  1   1600

20 27 20  M82          00 18 24  13.6  12.0 -9.6     -30.9   -13   1 10   1600  20 27 20
20 31 20  ---          00 22 24  13.7  12.3 -9.6     -31.8   227   R  1      0

 ---------- Forward pass 6 ----------

20 33 20  J0958+65     00 24 25  10.2  14.4 -9.6     -31.2   107   1 11      0  20 33 20
20 35 20  ---          00 26 25  10.3  14.6 -9.5     -31.6   120   F  1    800

20 35 20  M82          00 26 25  13.9  12.6 -9.5     -32.7   -13   1 11    800  20 35 20
20 39 20  ---          00 30 26  14.1  12.9 -9.4     -33.5   227   F  1   2400

20 39 20  J0958+65     00 30 26  10.5  15.0 -9.5     -32.4   -13   1 11   2400  20 39 20
20 41 20  ---          00 32 26  10.6  15.1 -9.4     -32.9   107   F  1   3200

20 41 20  M82          00 32 26  14.2  13.0 -9.4     -34.0   -13   1 11   3200  20 41 20
20 45 20  ---          00 36 27  14.4  13.3 -9.3     -34.8   227   F  1   4800

20 45 20  J0958+65     00 36 27  10.8  15.5 -9.4     -33.7   -13   1 11   4800  20 45 20
20 47 20  ---          00 38 27  11.0  15.7 -9.3     -34.1   107   F  1   5600

20 47 20  M82          00 38 27  14.5  13.5 -9.3     -35.3   -13   1 11   5600  20 47 20
20 51 20  ---          00 42 28  14.7  13.8 -9.2     -36.1   227   F  1   7200

20 51 20  J0958+65     00 42 28  11.2  16.0 -9.3     -35.0   -13   1 11   7200  20 51 20
20 53 20  ---          00 44 28  11.3  16.2 -9.2     -35.4   107   F  1   8000

20 53 20  M82          00 44 28  14.8  13.9 -9.2     -36.6   -13   1 11   8000  20 53 20
20 57 20  ---          00 48 29  15.0  14.2 -9.1     -37.4   227   F  1   9600

20 57 20  J0958+65     00 48 29  11.6  16.5 -9.2     -36.2   -13   1 11   9600  20 57 20
20 59 20  ---          00 50 29  11.7  16.7 -9.1     -36.7   107   F  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

20 59 20  M82          00 50 29  15.1  14.4 -9.1     -37.9   -13   1 11  10400  20 59 20
21 03 20  ---          00 54 30  15.3  14.6 -9.0     -38.7   227   F  1  12000

21 03 20  J0958+65     00 54 30  11.9  17.0 -9.1     -37.5   -13   1 11  12000  21 03 20
21 05 20  ---          00 56 30  12.1  17.2 -9.0     -37.9   107   F  1  12800

21 05 20  M82          00 56 30  15.5  14.8 -9.0     -39.2   -13   1 11  12800  21 05 20
21 09 20  ---          01 00 31  15.7  15.1 -8.9     -40.0   227   F  1  14400

21 09 20  J0958+65     01 00 31  12.3  17.5 -9.0     -38.8   -13   1 11  14400  21 09 20
21 11 20  ---          01 02 31  12.4  17.7 -8.9     -39.2   107   F  1  15200

 ----------  Bring In Mk for FF ----------

21 22 20  3C84         01 13 33  62.4  58.0 -2.1    -103.0   554   1 11  15200  21 22 20
21 28 20  ---          01 19 34  63.5  57.4 -2.0    -104.5   360   F  1  17600

 ---------- Reverse pass 6 ----------

21 39 20  J0958+65     01 30 35  14.4  19.9 -8.5     -45.1   556   1 12  17600  21 39 20
21 41 30  ---          01 32 46  14.6  20.1 -8.4     -45.5   130   R  1  16733

21 41 30  M82          01 32 46  17.6  17.2 -8.4     -47.0   -12   1 12  16733  21 41 30
21 45 40  ---          01 36 57  17.9  17.4 -8.3     -47.9   238   R  1  15067

21 45 40  J0958+65     01 36 57  14.9  20.4 -8.4     -46.4   -12   1 12  15067  21 45 40
21 47 50  ---          01 39 07  15.0  20.6 -8.3     -46.8   118   R  1  14200

21 47 50  M82          01 39 07  18.0  17.6 -8.3     -48.4   -12   1 12  14200  21 47 50
21 52 00  ---          01 43 18  18.3  17.8 -8.2     -49.3   238   R  1  12533

21 52 00  J0958+65     01 43 18  15.3  20.9 -8.3     -47.7   -12   1 12  12533  21 52 00
21 54 10  ---          01 45 28  15.5  21.0 -8.2     -48.2   118   R  1  11667

21 54 10  M82          01 45 28  18.4  18.0 -8.2     -49.7   -12   1 12  11667  21 54 10
21 58 20  ---          01 49 39  18.7  18.2 -8.1     -50.6   238   R  1  10000

21 58 20  J0958+65     01 49 39  15.8  21.3 -8.2     -49.0   -12   1 12  10000  21 58 20
22 00 30  ---          01 51 49  16.0  21.5 -8.1     -49.5   118   R  1   9133

22 00 30  M82          01 51 49  18.9  18.3 -8.1     -51.1   -12   1 12   9133  22 00 30
22 04 40  ---          01 56 00  19.1  18.6 -8.0     -52.0   238   R  1   7467
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

22 04 40  J0958+65     01 56 00  16.3  21.8 -8.1     -50.4   -12   1 12   7467  22 04 40
22 06 50  ---          01 58 10  16.5  21.9 -8.0     -50.8   118   R  1   6600

22 06 50  M82          01 58 10  19.3  18.7 -8.0     -52.5   -12   1 12   6600  22 06 50
22 11 00  ---          02 02 21  19.6  18.9 -7.9     -53.4   238   R  1   4933

22 11 00  J0958+65     02 02 21  16.9  22.2 -7.9     -51.7   -11   1 12   4933  22 11 00
22 13 10  ---          02 04 31  17.0  22.3 -7.9     -52.1   119   R  1   4067

22 13 10  M82          02 04 31  19.7  19.0 -7.9     -53.8   -11   1 12   4067  22 13 10
22 17 20  ---          02 08 42  20.0  19.3 -7.8     -54.7   239   R  1   2400

22 17 20  J0958+65     02 08 42  17.4  22.6 -7.8     -53.0   -11   1 12   2400  22 17 20
22 19 20  ---          02 10 42  17.5  22.7 -7.8     -53.4   109   R  1   1600

22 19 20  M82          02 10 42  20.2  19.4 -7.8     -55.2   -11   1 12   1600  22 19 20
22 23 20  ---          02 14 43  20.5  19.6 -7.7     -56.0   229   R  1      0

 ---------- Forward pass 7 ----------

22 25 20  J0958+65     02 16 43  18.0  23.1 -7.7     -54.7   109   1 13      0  22 25 20
22 27 30  ---          02 18 53  18.2  23.3 -7.7     -55.1   130   F  1    867

22 27 30  M82          02 18 53  20.8  19.8 -7.6     -57.0   -11   1 13    867  22 27 30
22 31 40  ---          02 23 04  21.1  20.0 -7.6     -57.9   239   F  1   2533

22 31 40  J0958+65     02 23 04  18.6  23.5 -7.6     -56.0   -11   1 13   2533  22 31 40
22 33 50  ---          02 25 14  18.8  23.6 -7.6     -56.4   119   F  1   3400

22 33 50  M82          02 25 14  21.2  20.1 -7.5     -58.3   -11   1 13   3400  22 33 50
22 38 00  ---          02 29 25  21.5  20.3 -7.4     -59.2   239   F  1   5067

22 38 00  J0958+65     02 29 25  19.1  23.9 -7.5     -57.3   -11   1 13   5067  22 38 00
22 40 10  ---          02 31 35  19.3  24.0 -7.5     -57.8   119   F  1   5933

22 40 10  M82          02 31 35  21.7  20.4 -7.4     -59.7   -11   1 13   5933  22 40 10
22 44 20  ---          02 35 46  22.0  20.6 -7.3     -60.6   239   F  1   7600

22 44 20  J0958+65     02 35 46  19.7  24.3 -7.4     -58.6   -11   1 13   7600  22 44 20
22 46 30  ---          02 37 57  19.9  24.4 -7.4     -59.1   119   F  1   8467

22 46 30  M82          02 37 57  22.2  20.7 -7.3     -61.1   -11   1 13   8467  22 46 30
22 50 40  ---          02 42 07  22.5  20.9 -7.2     -62.0   239   F  1  10133
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

22 50 40  J0958+65     02 42 07  20.3  24.6 -7.3     -60.0   -10   1 13  10133  22 50 40
22 52 50  ---          02 44 18  20.5  24.7 -7.2     -60.4   120   F  1  11000

22 52 50  M82          02 44 18  22.7  21.0 -7.2     -62.5   -10   1 13  11000  22 52 50
22 57 00  ---          02 48 28  23.0  21.2 -7.1     -63.4   240   F  1  12667

22 57 00  J0958+65     02 48 28  20.8  25.0 -7.2     -61.3   -10   1 13  12667  22 57 00
22 59 10  ---          02 50 39  21.0  25.1 -7.1     -61.7   120   F  1  13533

22 59 10  M82          02 50 39  23.2  21.3 -7.1     -63.8   -10   1 13  13533  22 59 10
23 00 00  ---          02 51 29  23.2  21.3 -7.1     -64.0    40   F  1  13867

23 00 00  M82          02 51 29  23.2  21.3 -7.1     -64.0    -4   1 13  13867  23 00 00
23 03 20  ---          02 54 49  23.5  21.4 -7.0     -64.8   196   F  1  15200

23 03 20  J0958+65     02 54 49  21.4  25.3 -7.1     -62.6   -10   1 13  15200  23 03 20
23 05 20  ---          02 56 50  21.6  25.4 -7.0     -63.0   110   F  1  16000

23 05 20  M82          02 56 50  23.6  21.5 -7.0     -65.2   -10   1 13  16000  23 05 20
23 09 20  ---          03 00 50  24.0  21.7 -6.9     -66.1   230   F  1  17600

 ---------- Reverse pass 7 ----------

23 10 00  J0958+65     03 01 30  22.0  25.6 -7.0     -64.0    30   1 14  17600  23 10 00
23 12 00  ---          03 03 31  22.2  25.7 -6.9     -64.4   120   R  1  16800

23 12 00  M82          03 03 31  24.2  21.8 -6.9     -66.7   -10   1 14  16800  23 12 00
23 16 00  ---          03 07 31  24.5  21.9 -6.8     -67.5   230   R  1  15200

23 16 00  J0958+65     03 07 31  22.6  25.9 -6.9     -65.3   -10   1 14  15200  23 16 00
23 18 00  ---          03 09 32  22.8  26.0 -6.8     -65.7   110   R  1  14400

23 18 00  M82          03 09 32  24.7  22.0 -6.8     -68.0   -10   1 14  14400  23 18 00
23 22 00  ---          03 13 32  25.0  22.1 -6.7     -68.9   230   R  1  12800

23 22 00  J0958+65     03 13 32  23.2  26.2 -6.8     -66.5   -10   1 14  12800  23 22 00
23 24 00  ---          03 15 33  23.3  26.3 -6.7     -67.0   110   R  1  12000

23 24 00  M82          03 15 33  25.1  22.2 -6.7     -69.3   -10   1 14  12000  23 24 00
23 28 00  ---          03 19 33  25.5  22.3 -6.6     -70.2   230   R  1  10400

23 28 00  J0958+65     03 19 33  23.7  26.5 -6.7     -67.8    -9   1 14  10400  23 28 00
23 30 00  ---          03 21 34  23.9  26.5 -6.6     -68.2   111   R  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   3 Mar 2005   Day  62 ---

23 30 00  M82          03 21 34  25.6  22.4 -6.6     -70.6    -9   1 14   9600  23 30 00
23 34 00  ---          03 25 34  26.0  22.5 -6.5     -71.5   231   R  1   8000

23 34 00  J0958+65     03 25 34  24.3  26.7 -6.6     -69.1    -9   1 14   8000  23 34 00
23 36 00  ---          03 27 35  24.5  26.8 -6.5     -69.5   111   R  1   7200

23 36 00  M82          03 27 35  26.1  22.6 -6.5     -72.0    -9   1 14   7200  23 36 00
23 40 00  ---          03 31 35  26.5  22.7 -6.4     -72.8   231   R  1   5600

23 40 00  J0958+65     03 31 35  24.9  26.9 -6.5     -70.3    -9   1 14   5600  23 40 00
23 42 00  ---          03 33 36  25.1  27.0 -6.4     -70.8   111   R  1   4800

23 42 00  M82          03 33 36  26.6  22.8 -6.4     -73.3    -9   1 14   4800  23 42 00
23 46 00  ---          03 37 36  27.0  22.9 -6.3     -74.2   231   R  1   3200

23 46 00  J0958+65     03 37 36  25.5  27.2 -6.4     -71.6    -9   1 14   3200  23 46 00
23 48 00  ---          03 39 37  25.7  27.2 -6.3     -72.0   111   R  1   2400

23 48 00  M82          03 39 37  27.1  22.9 -6.3     -74.6    -9   1 14   2400  23 48 00
23 52 00  ---          03 43 37  27.5  23.0 -6.2     -75.5   231   R  1    800

23 52 00  J0958+65     03 43 37  26.1  27.4 -6.3     -72.9    -9   1 14    800  23 52 00
23 54 00  ---          03 45 38  26.3  27.4 -6.2     -73.3   111   R  1      0

 --- Fri   4 Mar 2005   Day  63 ---

 ---------- Forward pass 1 ----------

-----------  Tape Change ------------

00 09 00  J0958+65     04 00 40  27.8  27.9 -6.0     -76.5   891   2  1      0  00 09 00
00 11 10  ---          04 02 50  28.0  28.0 -5.9     -77.0   130   F  1    867

00 11 10  M82          04 02 50  29.1  23.4 -5.9     -79.8    -9   2  1    867  00 11 10
00 15 20  ---          04 07 01  29.5  23.5 -5.8     -80.8   241   F  1   2533

00 15 20  J0958+65     04 07 01  28.4  28.1 -5.9     -77.9    -9   2  1   2533  00 15 20
00 17 30  ---          04 09 11  28.6  28.1 -5.8     -78.4   121   F  1   3400

00 17 30  M82          04 09 11  29.6  23.5 -5.8     -81.3    -9   2  1   3400  00 17 30
00 21 40  ---          04 13 22  30.0  23.6 -5.7     -82.2   241   F  1   5067

00 21 40  J0958+65     04 13 22  29.1  28.2 -5.8     -79.3    -9   2  1   5067  00 21 40
00 23 50  ---          04 15 33  29.3  28.3 -5.7     -79.7   121   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

00 23 50  M82          04 15 33  30.2  23.6 -5.7     -82.7    -9   2  1   5933  00 23 50
00 28 00  ---          04 19 43  30.5  23.7 -5.6     -83.7   241   F  1   7600

00 28 00  J0958+65     04 19 43  29.7  28.3 -5.7     -80.7    -9   2  1   7600  00 28 00
00 30 00  ---          04 21 44  29.9  28.4 -5.6     -81.1   111   F  1   8400

00 30 00  M82          04 21 44  30.7  23.7 -5.6     -84.1    -9   2  1   8400  00 30 00
00 34 20  ---          04 26 04  31.1  23.7 -5.5     -85.1   251   F  1  10133

00 34 20  J0958+65     04 26 04  30.4  28.5 -5.6     -82.0    -9   2  1  10133  00 34 20
00 36 30  ---          04 28 15  30.6  28.5 -5.5     -82.5   121   F  1  11000

00 36 30  M82          04 28 15  31.3  23.8 -5.5     -85.6    -9   2  1  11000  00 36 30
00 40 40  ---          04 32 25  31.6  23.8 -5.4     -86.6   241   F  1  12667

00 40 40  J0958+65     04 32 25  31.0  28.6 -5.4     -83.4    -9   2  1  12667  00 40 40
00 42 50  ---          04 34 36  31.2  28.6 -5.4     -83.9   121   F  1  13533

00 42 50  M82          04 34 36  31.8  23.8 -5.4     -87.1    -9   2  1  13533  00 42 50
00 47 00  ---          04 38 46  32.2  23.8 -5.3     -88.1   241   F  1  15200

00 47 00  J0958+65     04 38 46  31.7  28.6 -5.3     -84.8    -9   2  1  15200  00 47 00
00 49 00  ---          04 40 47  31.9  28.7 -5.3     -85.3   111   F  1  16000

00 49 00  M82          04 40 47  32.4  23.8 -5.3     -88.5    -9   2  1  16000  00 49 00
00 53 00  ---          04 44 47  32.7  23.8 -5.2     -89.5   231   F  1  17600

 ---------- Sources Up at MK  (All telescopes in) ----------

00 53 40  J0958+65     04 45 27  32.4  28.7 -5.2     -86.3    31   2  2  17600  00 53 40
00 55 50  ---          04 47 38  32.6  28.7 -5.2     -86.8   130   R  1  16733

00 55 50  M82          04 47 38  33.0  23.8 -5.1     -90.1    -9   2  2  16733  00 55 50
01 00 00  ---          04 51 48  33.3  23.8 -5.1     -91.1   241   R  1  15067

01 00 00  J0958+65     04 51 48  33.0  28.7 -5.1     -87.8    -9   2  2  15067  01 00 00
01 02 10  ---          04 53 59  33.2  28.7 -5.1     -88.2   121   R  1  14200

01 02 10  M82          04 53 59  33.5  23.8 -5.0     -91.6    -9   2  2  14200  01 02 10
01 06 20  ---          04 58 10  33.9  23.8 -5.0     -92.6   241   R  1  12533

01 06 20  J0958+65     04 58 10  33.7  28.8 -5.0     -89.2    -9   2  2  12533  01 06 20
01 08 30  ---          05 00 20  33.9  28.8 -5.0     -89.7   121   R  1  11667
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

01 08 30  M82          05 00 20  34.1  23.8 -4.9     -93.1    -9   2  2  11667  01 08 30
01 12 40  ---          05 04 31  34.4  23.8 -4.9     -94.1   241   R  1  10000

01 12 40  J0958+65     05 04 31  34.3  28.8 -4.9     -90.6    -9   2  2  10000  01 12 40
01 14 50  ---          05 06 41  34.6  28.8 -4.9     -91.1   121   R  1   9133

01 14 50  M82          05 06 41  34.6  23.7 -4.8     -94.6    -9   2  2   9133  01 14 50
01 19 00  ---          05 10 52  35.0  23.7 -4.8     -95.6   241   R  1   7467

01 19 00  J0958+65     05 10 52  35.0  28.7 -4.8     -92.1    -9   2  2   7467  01 19 00
01 21 10  ---          05 13 02  35.2  28.7 -4.8     -92.6   121   R  1   6600

01 21 10  M82          05 13 02  35.2  23.7 -4.7     -96.2    -9   2  2   6600  01 21 10
01 25 20  ---          05 17 13  35.5  23.6 -4.7     -97.2   241   R  1   4933

01 25 20  J0958+65     05 17 13  35.6  28.7 -4.7     -93.6    -9   2  2   4933  01 25 20
01 27 30  ---          05 19 23  35.9  28.7 -4.7     -94.1   121   R  1   4067

01 27 30  M82          05 19 23  35.7  23.6 -4.6     -97.7    -9   2  2   4067  01 27 30
01 31 40  ---          05 23 34  36.1  23.5 -4.5     -98.7   241   R  1   2400

01 31 40  J0958+65     05 23 34  36.3  28.6 -4.6     -95.0    -9   2  2   2400  01 31 40
01 33 40  ---          05 25 34  36.5  28.6 -4.6     -95.5   111   R  1   1600

01 33 40  M82          05 25 34  36.3  23.5 -4.5     -99.2    -9   2  2   1600  01 33 40
01 37 40  ---          05 29 35  36.6  23.4 -4.4    -100.2   231   R  1      0

 ---------- Forward pass 2 ----------

01 39 40  J0958+65     05 31 35  37.1  28.5 -4.5     -96.9   111   2  3      0  01 39 40
01 41 50  ---          05 33 45  37.3  28.5 -4.4     -97.4   130   F  1    867

01 41 50  M82          05 33 45  37.0  23.3 -4.4    -101.2    -9   2  3    867  01 41 50
01 46 00  ---          05 37 56  37.3  23.3 -4.3    -102.3   241   F  1   2533

01 46 00  J0958+65     05 37 56  37.8  28.4 -4.4     -98.4    -9   2  3   2533  01 46 00
01 48 10  ---          05 40 06  38.0  28.4 -4.3     -99.0   121   F  1   3400

01 48 10  M82          05 40 06  37.5  23.2 -4.3    -102.8    -9   2  3   3400  01 48 10
01 52 20  ---          05 44 17  37.8  23.1 -4.2    -103.8   241   F  1   5067

01 52 20  J0958+65     05 44 17  38.4  28.3 -4.2    -100.0    -9   2  3   5067  01 52 20
01 54 30  ---          05 46 27  38.6  28.2 -4.2    -100.5   121   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

01 54 30  M82          05 46 27  38.0  23.0 -4.2    -104.4    -9   2  3   5933  01 54 30
01 58 40  ---          05 50 38  38.4  22.9 -4.1    -105.4   241   F  1   7600

01 58 40  J0958+65     05 50 38  39.1  28.1 -4.1    -101.5    -9   2  3   7600  01 58 40
02 00 50  ---          05 52 48  39.3  28.1 -4.1    -102.0   121   F  1   8467

02 00 50  M82          05 52 48  38.6  22.9 -4.1    -106.0    -9   2  3   8467  02 00 50
02 05 00  ---          05 56 59  38.9  22.7 -4.0    -107.1   241   F  1  10133

02 05 00  J0958+65     05 56 59  39.7  28.0 -4.0    -103.1    -9   2  3  10133  02 05 00
02 07 10  ---          05 59 09  39.9  27.9 -4.0    -103.6   121   F  1  11000

02 07 10  M82          05 59 09  39.1  22.7 -4.0    -107.6    -9   2  3  11000  02 07 10
02 11 20  ---          06 03 20  39.4  22.5 -3.9    -108.7   241   F  1  12667

02 11 20  J0958+65     06 03 20  40.3  27.7 -3.9    -104.6    -9   2  3  12667  02 11 20
02 13 30  ---          06 05 31  40.6  27.7 -3.9    -105.2   121   F  1  13533

02 13 30  M82          06 05 31  39.6  22.4 -3.8    -109.2    -9   2  3  13533  02 13 30
02 17 40  ---          06 09 41  40.0  22.3 -3.8    -110.3   241   F  1  15200

02 17 40  J0958+65     06 09 41  41.0  27.5 -3.8    -106.2    -9   2  3  15200  02 17 40
02 19 40  ---          06 11 42  41.2  27.4 -3.8    -106.7   111   F  1  16000

02 19 40  M82          06 11 42  40.1  22.2 -3.7    -110.8   -10   2  3  16000  02 19 40
02 23 40  ---          06 15 42  40.4  22.0 -3.7    -111.9   230   F  1  17600

 ---------- Reverse pass 2 ----------

02 24 20  J0958+65     06 16 22  41.6  27.2 -3.7    -107.9    31   2  4  17600  02 24 20
02 26 20  ---          06 18 23  41.8  27.2 -3.7    -108.5   120   R  1  16800

02 26 20  M82          06 18 23  40.7  21.9 -3.6    -112.6   -10   2  4  16800  02 26 20
02 30 20  ---          06 22 23  41.0  21.7 -3.6    -113.7   230   R  1  15200

02 30 20  J0958+65     06 22 23  42.2  27.0 -3.6    -109.5   -10   2  4  15200  02 30 20
02 32 20  ---          06 24 24  42.4  26.9 -3.6    -110.0   110   R  1  14400

02 32 20  M82          06 24 24  41.1  21.6 -3.5    -114.2   -10   2  4  14400  02 32 20
02 36 20  ---          06 28 24  41.5  21.4 -3.5    -115.3   230   R  1  12800

02 36 20  J0958+65     06 28 24  42.8  26.7 -3.5    -111.1    -9   2  4  12800  02 36 20
02 38 20  ---          06 30 25  43.0  26.6 -3.5    -111.6   111   R  1  12000
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

02 38 20  M82          06 30 25  41.6  21.3 -3.4    -115.8    -9   2  4  12000  02 38 20
02 42 20  ---          06 34 25  41.9  21.1 -3.4    -116.9   231   R  1  10400

02 42 20  J0958+65     06 34 25  43.4  26.4 -3.4    -112.6    -9   2  4  10400  02 42 20
02 44 20  ---          06 36 26  43.6  26.3 -3.4    -113.2   111   R  1   9600

02 44 20  M82          06 36 26  42.1  21.0 -3.3    -117.4    -9   2  4   9600  02 44 20
02 48 20  ---          06 40 26  42.4  20.8 -3.3    -118.5   231   R  1   8000

02 48 20  J0958+65     06 40 26  44.0  26.0 -3.3    -114.2    -9   2  4   8000  02 48 20
02 50 20  ---          06 42 27  44.2  25.9 -3.3    -114.8   111   R  1   7200

02 50 20  M82          06 42 27  42.5  20.7 -3.2    -119.0    -9   2  4   7200  02 50 20
02 54 20  ---          06 46 27  42.8  20.5 -3.2    -120.1   231   R  1   5600

02 54 20  J0958+65     06 46 27  44.5  25.7 -3.2    -115.9    -9   2  4   5600  02 54 20
02 56 20  ---          06 48 28  44.7  25.5 -3.2    -116.4   111   R  1   4800

02 56 20  M82          06 48 28  43.0  20.3 -3.1    -120.7    -9   2  4   4800  02 56 20
03 00 20  ---          06 52 28  43.3  20.1 -3.1    -121.8   231   R  1   3200

03 00 20  J0958+65     06 52 28  45.1  25.3 -3.1    -117.5   -10   2  4   3200  03 00 20
03 02 20  ---          06 54 29  45.3  25.1 -3.1    -118.1   110   R  1   2400

03 06 20  J0927+39     06 58 29  58.6  64.3 -2.5     -93.9   207   2  4   2400  03 06 20
03 12 20  ---          07 04 30  59.7  64.1 -2.4     -95.0   360   R  1      0

 ---------- Forward pass 3 ----------

03 16 20  J0958+65     07 08 31  46.5  24.1 -2.8    -122.0   207   2  5      0  03 16 20
03 18 30  ---          07 10 41  46.7  23.9 -2.8    -122.6   130   F  1    867

03 18 30  M82          07 10 41  44.6  18.8 -2.8    -126.9   -10   2  5    867  03 18 30
03 22 40  ---          07 14 52  44.9  18.5 -2.7    -128.1   240   F  1   2533

03 22 40  J0958+65     07 14 52  47.1  23.6 -2.7    -123.8   -10   2  5   2533  03 22 40
03 24 50  ---          07 17 02  47.3  23.4 -2.7    -124.5   120   F  1   3400

03 24 50  M82          07 17 02  45.0  18.4 -2.7    -128.8   -10   2  5   3400  03 24 50
03 29 00  ---          07 21 13  45.3  18.0 -2.6    -130.0   240   F  1   5067

03 29 00  J0958+65     07 21 13  47.6  23.0 -2.6    -125.7   -11   2  5   5067  03 29 00
03 31 10  ---          07 23 23  47.8  22.8 -2.6    -126.3   119   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

03 31 10  M82          07 23 23  45.5  17.9 -2.5    -130.6   -11   2  5   5933  03 31 10
03 35 20  ---          07 27 34  45.7  17.5 -2.5    -131.8   239   F  1   7600

03 35 20  J0958+65     07 27 34  48.1  22.4 -2.5    -127.6   -11   2  5   7600  03 35 20
03 37 30  ---          07 29 44  48.3  22.2 -2.5    -128.2   119   F  1   8467

03 37 30  M82          07 29 44  45.9  17.3 -2.4    -132.5   -11   2  5   8467  03 37 30
03 41 40  ---          07 33 55  46.1  17.0 -2.4    -133.7   239   F  1  10133

03 41 40  J0958+65     07 33 55  48.7  21.8 -2.4    -129.5   -11   2  5  10133  03 41 40
03 43 50  ---          07 36 05  48.8  21.6 -2.4    -130.1   119   F  1  11000

03 43 50  M82          07 36 05  46.3  16.8 -2.3    -134.3   -11   2  5  11000  03 43 50
03 48 00  ---          07 40 16  46.5  16.4 -2.3    -135.6   239   F  1  12667

03 48 00  J0958+65     07 40 16  49.2  21.2 -2.3    -131.4   -11   2  5  12667  03 48 00
03 50 10  ---          07 42 26  49.3  20.9 -2.3    -132.1   119   F  1  13533

03 50 10  M82          07 42 26  46.7  16.2 -2.2    -136.3   -11   2  5  13533  03 50 10
03 54 20  ---          07 46 37  46.9  15.8 -2.2    -137.5   239   F  1  15200

03 54 20  J0958+65     07 46 37  49.6  20.5 -2.2    -133.4   -11   2  5  15200  03 54 20
03 56 20  ---          07 48 37  49.8  20.2 -2.2    -134.0   109   F  1  16000

03 56 20  M82          07 48 37  47.0  15.6 -2.1    -138.1   -12   2  5  16000  03 56 20
04 00 20  ---          07 52 38  47.3  15.3 -2.1    -139.3   228   F  1  17600

 ---------- Reverse pass 3 ----------

04 01 00  J0958+65     07 53 18  50.1  19.7 -2.1    -135.5    28   2  6  17600  04 01 00
04 03 10  ---          07 55 29  50.3  19.5 -2.1    -136.2   130   R  1  16733

04 03 10  M82          07 55 29  47.4  15.0 -2.0    -140.2   -12   2  6  16733  04 03 10
04 07 20  ---          07 59 39  47.6  14.6 -1.9    -141.5   238   R  1  15067

04 07 20  J0958+65     07 59 39  50.6  19.0 -2.0    -137.5   -12   2  6  15067  04 07 20
04 09 30  ---          08 01 50  50.7  18.7 -2.0    -138.2   118   R  1  14200

04 09 30  M82          08 01 50  47.8  14.3 -1.9    -142.2   -12   2  6  14200  04 09 30
04 13 40  ---          08 06 00  48.0  13.9 -1.8    -143.5   238   R  1  12533

04 13 40  J0958+65     08 06 00  51.0  18.2 -1.9    -139.5   -12   2  6  12533  04 13 40
04 15 50  ---          08 08 11  51.2  17.9 -1.9    -140.3   118   R  1  11667
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

04 15 50  M82          08 08 11  48.1  13.7 -1.8    -144.2   -12   2  6  11667  04 15 50
04 20 00  ---          08 12 21  48.3  13.2 -1.7    -145.5   238   R  1  10000

04 20 00  J0958+65     08 12 21  51.4  17.4 -1.8    -141.6   -12   2  6  10000  04 20 00
04 22 10  ---          08 14 32  51.6  17.1 -1.7    -142.3   118   R  1   9133

04 22 10  M82          08 14 32  48.4  13.0 -1.7    -146.1   -12   2  6   9133  04 22 10
04 26 20  ---          08 18 42  48.6  12.5 -1.6    -147.5   238   R  1   7467

04 26 20  J0958+65     08 18 42  51.8  16.5 -1.7    -143.7   -12   2  6   7467  04 26 20
04 28 30  ---          08 20 53  52.0  16.2 -1.6    -144.5   118   R  1   6600

04 28 30  M82          08 20 53  48.7  12.3 -1.6    -148.2   -13   2  6   6600  04 28 30
04 32 40  ---          08 25 03  48.9  11.8 -1.5    -149.5   237   R  1   4933

04 32 40  J0958+65     08 25 03  52.2  15.7 -1.6    -145.9   -13   2  6   4933  04 32 40
04 34 50  ---          08 27 14  52.3  15.4 -1.5    -146.6   117   R  1   4067

04 34 50  M82          08 27 14  49.0  11.6 -1.5    -150.2   -13   2  6   4067  04 34 50
04 39 00  ---          08 31 24  49.2  11.1 -1.4    -151.5   237   R  1   2400

04 39 00  J0958+65     08 31 24  52.6  14.8 -1.5    -148.0   -13   2  6   2400  04 39 00
04 41 00  ---          08 33 25  52.7  14.5 -1.4    -148.7   107   R  1   1600

04 41 00  M82          08 33 25  49.2  10.9 -1.4    -152.2   -13   2  6   1600  04 41 00
04 45 00  ---          08 37 25  49.4  10.4 -1.3    -153.5   227   R  1      0

 ---------- Sources setting at WB for the rest of experiment ----------

04 47 00  J0958+65     08 39 26  53.0  13.6 -1.3    -150.8   107   2  7      0  04 47 00
04 49 10  ---          08 41 36  53.1  13.3 -1.3    -151.6   130   F  1    867

04 49 10  M82          08 41 36  49.6   9.9 -1.2    -154.8   -13   2  7    867  04 49 10
04 53 20  ---          08 45 47  49.7   9.4 -1.2    -156.2   237   F  1   2533

04 53 20  J0958+65     08 45 47  53.3  12.6 -1.2    -153.0   -13   2  7   2533  04 53 20
04 55 30  ---          08 47 57  53.4  12.3 -1.2    -153.8   117   F  1   3400

04 55 30  M82          08 47 57  49.8   9.1 -1.1    -156.9   -13   2  7   3400  04 55 30
04 59 40  ---          08 52 08  49.9   8.6 -1.1    -158.3   237   F  1   5067

04 59 40  J0958+65     08 52 08  53.6  11.6 -1.1    -155.3   -13   2  7   5067  04 59 40
05 01 50  ---          08 54 18  53.7  11.3 -1.1    -156.0   117   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

05 01 50  M82          08 54 18  50.0   8.3 -1.0    -159.0   -13   2  7   5933  05 01 50
05 06 00  ---          08 58 29  50.1   7.8 -1.0    -160.4   237   F  1   7600

05 06 00  J0958+65     08 58 29  53.9  10.6 -1.0    -157.5   -13   2  7   7600  05 06 00
05 08 10  ---          09 00 39  54.0  10.2 -1.0    -158.3   117   F  1   8467

05 08 10  M82          09 00 39  50.2   7.5 -0.9    -161.1   -14   2  7   8467  05 08 10
05 12 20  ---          09 04 50  50.3   7.0 -0.9    -162.5   236   F  1  10133

05 12 20  J0958+65     09 04 50  54.1   9.6 -0.9    -159.8   -14   2  7  10133  05 12 20
05 14 30  ---          09 07 00  54.2   9.2 -0.9    -160.6   116   F  1  11000

05 14 30  M82          09 07 00  50.4   6.7 -0.8    -163.3   -14   2  7  11000  05 14 30
05 18 40  ---          09 11 11  50.5   6.1 -0.8    -164.7   236   F  1  12667

05 18 40  J0958+65     09 11 11  54.3   8.5 -0.8    -162.1   -14   2  7  12667  05 18 40
05 20 50  ---          09 13 21  54.4   8.1 -0.8    -162.9   116   F  1  13533

05 20 50  M82          09 13 21  50.5   5.8 -0.7    -165.4   -14   2  7  13533  05 20 50
05 25 00  ---          09 17 32  50.6   5.3 -0.6    -166.8   236   F  1  15200

05 25 00  J0958+65     09 17 32  54.5   7.4 -0.7    -164.4   -14   2  7  15200  05 25 00
05 27 00  ---          09 19 32  54.6   7.1 -0.7    -165.2   106   F  1  16000

05 27 00  M82          09 19 32  50.6   5.0 -0.6    -167.5   -14   2  7  16000  05 27 00
05 31 00  ---          09 23 33  50.7   4.5 -0.5    -168.8   226   F  1  17600

 ---------- Reverse pass 4 ----------

05 31 40  J0958+65     09 24 13  54.7   6.3 -0.6    -166.9    26   2  8  17600  05 31 40
05 33 50  ---          09 26 23  54.7   5.9 -0.5    -167.7   130   R  1  16733

05 33 50  M82          09 26 23  50.7   4.1 -0.5    -169.8   -14   2  8  16733  05 33 50
05 38 00  ---          09 30 34  50.8   3.5 -0.4    -171.2   236   R  1  15067

05 38 00  J0958+65     09 30 34  54.8   5.1 -0.5    -169.3   -14   2  8  15067  05 38 00
05 40 10  ---          09 32 44  54.9   4.8 -0.4    -170.1   116   R  1  14200

05 40 10  M82          09 32 44  50.8   3.2 -0.4    -171.9   -14   2  8  14200  05 40 10
05 44 20  ---          09 36 55  50.9   2.7 -0.3    -173.4   236   R  1  12533

05 44 20  J0958+65     09 36 55  54.9   4.0 -0.4    -171.6   -14   2  8  12533  05 44 20
05 46 30  ---          09 39 06  55.0   3.6 -0.3    -172.4   116   R  1  11667
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

05 46 30  M82          09 39 06  50.9   2.4 -0.3    -174.1   -14   2  8  11667  05 46 30
05 50 40  ---          09 43 16  50.9   1.8 -0.2    -175.5   236   R  1  10000

05 50 40  J0958+65     09 43 16  55.0   2.9 -0.3    -174.0   -14   2  8  10000  05 50 40
05 52 50  ---          09 45 27  55.0   2.5 -0.2    -174.8   116   R  1   9133

05 52 50  M82          09 45 27  50.9   1.5 -0.2    -176.3   -14   2  8   9133  05 52 50
05 57 00  ---          09 49 37  51.0   0.9 -0.1    -177.7   236   R  1   7467

05 57 00  J0958+65     09 49 37  55.1   1.7 -0.2    -176.4   -14   2  8   7467  05 57 00
05 59 10  ---          09 51 48  55.1   1.3 -0.1    -177.2   116   R  1   6600

05 59 10  M82          09 51 48  51.0   0.6 -0.1    -178.4   -14   2  8   6600  05 59 10
06 03 20  ---          09 55 58  51.0   0.1  0.0    -179.9   236   R  1   4933

06 03 20  J0958+65     09 55 58  55.1   0.6 -0.1    -178.8   -14   2  8   4933  06 03 20
06 05 30  ---          09 58 09  55.1   0.2  0.0    -179.6   116   R  1   4067

06 05 30  M82          09 58 09  51.0  -0.2  0.0     179.4   -14   2  8   4067  06 05 30
06 09 40  ---          10 02 19  51.0  -0.8  0.1     178.0   236   R  1   2400

06 09 40  J0958+65     10 02 19  55.1  -0.6  0.1     178.8   -14   2  8   2400  06 09 40
06 11 40  ---          10 04 20  55.1  -0.9  0.1     178.1   106   R  1   1600

06 11 40  M82          10 04 20  51.0  -1.1  0.1     177.3   -14   2  8   1600  06 11 40
06 15 40  ---          10 08 20  50.9  -1.7  0.2     175.9   226   R  1      0

 ---------- Forward pass 5 ----------

06 17 40  J0958+65     10 10 21  55.1  -2.0  0.2     175.8   106   2  9      0  06 17 40
06 19 50  ---          10 12 31  55.0  -2.4  0.2     175.0   130   F  1    867

06 19 50  M82          10 12 31  50.9  -2.2  0.3     174.5   -14   2  9    867  06 19 50
06 24 00  ---          10 16 42  50.9  -2.8  0.3     173.1   236   F  1   2533

06 24 00  J0958+65     10 16 42  55.0  -3.1  0.3     173.4   -14   2  9   2533  06 24 00
06 26 10  ---          10 18 52  55.0  -3.5  0.3     172.6   116   F  1   3400

06 26 10  M82          10 18 52  50.8  -3.1  0.4     172.3   -14   2  9   3400  06 26 10
06 30 20  ---          10 23 03  50.8  -3.7  0.4     170.9   236   F  1   5067

06 30 20  J0958+65     10 23 03  54.9  -4.3  0.4     171.1   -14   2  9   5067  06 30 20
06 32 30  ---          10 25 13  54.9  -4.7  0.4     170.3   116   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

06 32 30  M82          10 25 13  50.8  -4.0  0.5     170.2   -14   2  9   5933  06 32 30
06 36 40  ---          10 29 24  50.7  -4.5  0.6     168.7   236   F  1   7600

06 36 40  J0958+65     10 29 24  54.8  -5.4  0.5     168.7   -14   2  9   7600  06 36 40
06 38 50  ---          10 31 34  54.7  -5.8  0.5     167.9   116   F  1   8467

06 38 50  M82          10 31 34  50.7  -4.8  0.6     168.0   -14   2  9   8467  06 38 50
06 43 00  ---          10 35 45  50.6  -5.4  0.7     166.6   236   F  1  10133

06 43 00  J0958+65     10 35 45  54.6  -6.5  0.6     166.4   -14   2  9  10133  06 43 00
06 45 10  ---          10 37 55  54.6  -6.9  0.6     165.6   116   F  1  11000

06 45 10  M82          10 37 55  50.5  -5.7  0.7     165.9   -14   2  9  11000  06 45 10
06 49 20  ---          10 42 06  50.4  -6.2  0.8     164.5   236   F  1  12667

06 49 20  J0958+65     10 42 06  54.5  -7.6  0.7     164.0   -14   2  9  12667  06 49 20
06 51 30  ---          10 44 16  54.4  -8.0  0.8     163.2   116   F  1  13533

06 51 30  M82          10 44 16  50.4  -6.5  0.8     163.7   -14   2  9  13533  06 51 30
06 55 40  ---          10 48 27  50.3  -7.0  0.9     162.3   236   F  1  15200

06 55 40  J0958+65     10 48 27  54.3  -8.7  0.8     161.7   -14   2  9  15200  06 55 40
06 57 40  ---          10 50 27  54.2  -9.0  0.9     161.0   106   F  1  16000

06 57 40  M82          10 50 27  50.2  -7.3  0.9     161.7   -14   2  9  16000  06 57 40
07 01 40  ---          10 54 28  50.1  -7.8  1.0     160.3   226   F  1  17600

 ---------- Reverse pass 5 ----------

07 02 20  J0958+65     10 55 08  54.1  -9.8  0.9     159.3    26   2 10  17600  07 02 20
07 04 30  ---          10 57 18  54.0 -10.2  1.0     158.5   130   R  1  16733

07 04 30  M82          10 57 18  50.0  -8.2  1.0     159.4   -14   2 10  16733  07 04 30
07 08 40  ---          11 01 29  49.9  -8.7  1.1     158.0   236   R  1  15067

07 08 40  J0958+65     11 01 29  53.8 -10.8  1.0     157.0   -14   2 10  15067  07 08 40
07 10 50  ---          11 03 39  53.7 -11.2  1.1     156.2   116   R  1  14200

07 10 50  M82          11 03 39  49.8  -9.0  1.1     157.3   -14   2 10  14200  07 10 50
07 15 00  ---          11 07 50  49.7  -9.5  1.2     155.9   236   R  1  12533

07 15 00  J0958+65     11 07 50  53.5 -11.9  1.1     154.7   -14   2 10  12533  07 15 00
07 17 10  ---          11 10 00  53.4 -12.2  1.2     154.0   116   R  1  11667
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

07 17 10  M82          11 10 00  49.6  -9.8  1.2     155.2   -14   2 10  11667  07 17 10
07 21 20  ---          11 14 11  49.4 -10.3  1.3     153.8   236   R  1  10000

07 21 20  J0958+65     11 14 11  53.2 -12.8  1.2     152.5   -14   2 10  10000  07 21 20
07 23 30  ---          11 16 21  53.1 -13.2  1.3     151.7   116   R  1   9133

07 23 30  M82          11 16 21  49.4 -10.5  1.3     153.1   -14   2 10   9133  07 23 30
07 27 40  ---          11 20 32  49.2 -11.0  1.4     151.8   236   R  1   7467

07 27 40  J0958+65     11 20 32  52.9 -13.8  1.4     150.3   -13   2 10   7467  07 27 40
07 29 50  ---          11 22 43  52.8 -14.1  1.4     149.5   117   R  1   6600

07 29 50  M82          11 22 43  49.1 -11.3  1.4     151.1   -13   2 10   6600  07 29 50
07 34 00  ---          11 26 53  48.9 -11.8  1.5     149.7   237   R  1   4933

07 34 00  J0958+65     11 26 53  52.6 -14.7  1.5     148.1   -13   2 10   4933  07 34 00
07 36 10  ---          11 29 04  52.5 -15.0  1.5     147.3   117   R  1   4067

07 36 10  M82          11 29 04  48.8 -12.0  1.5     149.0   -13   2 10   4067  07 36 10
07 40 20  ---          11 33 14  48.6 -12.5  1.6     147.7   237   R  1   2400

07 40 20  J0958+65     11 33 14  52.2 -15.6  1.6     145.9   -13   2 10   2400  07 40 20
07 42 20  ---          11 35 15  52.1 -15.9  1.6     145.3   107   R  1   1600

07 42 20  M82          11 35 15  48.5 -12.7  1.6     147.1   -13   2 10   1600  07 42 20
07 46 20  ---          11 39 15  48.4 -13.1  1.7     145.8   227   R  1      0

 ---------- Forward pass 6 ----------

07 48 20  J0958+65     11 41 16  51.8 -16.7  1.7     143.2   107   2 11      0  07 48 20
07 50 30  ---          11 43 26  51.6 -17.0  1.7     142.5   130   F  1    867

07 50 30  M82          11 43 26  48.1 -13.6  1.8     144.5   -13   2 11    867  07 50 30
07 54 40  ---          11 47 37  47.9 -14.0  1.9     143.2   237   F  1   2533

07 54 40  J0958+65     11 47 37  51.4 -17.6  1.8     141.1   -13   2 11   2533  07 54 40
07 56 50  ---          11 49 47  51.2 -17.9  1.8     140.4   117   F  1   3400

07 56 50  M82          11 49 47  47.8 -14.2  1.9     142.5   -13   2 11   3400  07 56 50
08 01 00  ---          11 53 58  47.6 -14.7  2.0     141.2   237   F  1   5067

08 01 00  J0958+65     11 53 58  50.9 -18.4  1.9     139.1   -13   2 11   5067  08 01 00
08 03 10  ---          11 56 08  50.8 -18.6  1.9     138.4   117   F  1   5933
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               GP042 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   4 Mar 2005   Day  63 ---

08 03 10  M82          11 56 08  47.5 -14.9  2.0     140.5   -13   2 11   5933  08 03 10
08 07 20  ---          12 00 19  47.2 -15.3  2.1     139.3   237   F  1   7600

08 07 20  J0958+65     12 00 19  50.5 -19.1  2.0     137.0   -12   2 11   7600  08 07 20
08 09 30  ---          12 02 29  50.3 -19.4  2.1     136.3   118   F  1   8467

08 09 30  M82          12 02 29  47.1 -15.5  2.1     138.6   -12   2 11   8467  08 09 30
08 13 40  ---          12 06 40  46.9 -15.9  2.2     137.3   238   F  1  10133

08 13 40  J0958+65     12 06 40  50.0 -19.9  2.1     135.0   -12   2 11  10133  08 13 40
08 15 50  ---          12 08 50  49.9 -20.1  2.2     134.3   118   F  1  11000

08 15 50  M82          12 08 50  46.7 -16.1  2.2     136.7   -12   2 11  11000  08 15 50
08 20 00  ---          12 13 01  46.5 -16.5  2.3     135.4   238   F  1  12667

08 20 00  J0958+65     12 13 01  49.6 -20.6  2.2     133.0   -12   2 11  12667  08 20 00
08 22 10  ---          12 15 11  49.4 -20.8  2.3     132.4   118   F  1  13533

08 22 10  M82          12 15 11  46.4 -16.7  2.3     134.8   -12   2 11  13533  08 22 10
08 26 20  ---          12 19 22  46.1 -17.0  2.4     133.5   238   F  1  15200

08 26 20  J0958+65     12 19 22  49.1 -21.3  2.3     131.1   -12   2 11  15200  08 26 20
08 30 00  ---          12 23 02  48.8 -21.6  2.4     129.9   208   F  1  16667


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/vlbi_sched/setups/v18cm-128-4-2.set
   Matches group v20cm_2 in /usr/local/vlbi_sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    6         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         L         L
   IF    =        A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   6  Setup file default.  Used pcal sets:   1
   LO sum=    1659.49   1659.49   1667.49   1667.49
   BBC fr=     740.51    740.51    732.51    732.51
   Bandwd=      8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510  6510  6510     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_off 
 SOURCE LIST -- GP042 18cm global observation of M82
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * M82               09 51 41.957031   * 09 55 50.694000     09 56 20.476115 
                     69 54 57.38676    * 69 40 43.69000      69 39 22.43490 
                     From catalog imbedded in main SCHED input file.
                       11.836 scan hours,   1109.467 baseline hours above horizon.

   J0319+4130        03 16 29.567273   * 03 19 48.160103     03 20 07.295285 
   0316+413          41 19 51.91592    * 41 30 42.10305      41 31 59.69380 
 * 3C84              /usr/local/vlbi_sched/catalogs/sources.vlba
   J0319+41          ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.100 scan hours,     12.000 baseline hours above horizon.

   J0927+3902        09 23 55.319195   * 09 27 03.013916     09 27 23.808078 
   0923+392          39 15 23.56655    * 39 02 20.85195      39 01 04.62874 
   4C39.25           /usr/local/vlbi_sched/catalogs/sources.vlba
 * J0927+39          ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.100 scan hours,     12.000 baseline hours above horizon.

   J0958+6533        09 54 57.847921   * 09 58 47.245102     09 59 14.327938 
   0954+658          65 48 15.53887    * 65 33 54.81806      65 32 31.97035 
 * J0958+65          /usr/local/vlbi_sched/catalogs/sources.vlba
                     ICRF - Ext.1 Source - 1998 IERS Annual Report
                        6.258 scan hours,    547.958 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82                116.0
   3C84                76.3
   J0927+39           141.5
   J0958+65           120.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

