  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron polarization imaging
 Exp. Code:  GG085F  


Schedule Version:       2.00
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es
Fax:
Phone during observation:

Observing mode: K-band dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

01 00 00  0851+202     05 37 35  44.3  91.3 -3.3     -66.3     0        0   01 00 00
01 09 30  ---          05 47 06  46.4  92.5 -3.1     -66.2   570       73   01 00 01

01 10 30  0851+202     05 48 06  46.6  92.7 -3.1     -66.2    54       73   01 10 30
01 18 30  ---          05 56 08  48.3  93.8 -3.0     -66.0   480      135   01 10 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

01 19 30  0851+202     05 57 08  48.5  93.9 -3.0     -66.0    54      135   01 19 30
01 28 30  ---          06 06 09  50.5  95.3 -2.8     -65.8   540      205   01 19 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 29 30  0851+202     06 07 10  50.7  95.4 -2.8     -65.7    54      205   01 29 30
01 34 00  ---          06 11 40  51.6  96.1 -2.7     -65.6   270      240   01 29 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

01 35 00  0851+202     06 12 40  51.9  96.3 -2.7     -65.6    54      240   01 35 00
01 44 30  ---          06 22 12  53.9  97.8 -2.6     -65.1   570      313   01 35 01

01 45 00  0923+392     06 22 42  51.4  64.6 -3.1     -87.9    -2      313   01 45 02
01 47 30  ---          06 25 13  51.9  64.6 -3.1     -88.2   148      332   01 45 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

01 48 30  0923+392     06 26 13  52.1  64.6 -3.0     -88.4    54      332   01 48 30
01 57 00  ---          06 34 44  53.8  64.7 -2.9     -89.7   510      398   01 48 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 58 00  0923+392     06 35 44  54.0  64.7 -2.9     -89.9    54      398   01 58 00
02 02 30  ---          06 40 15  54.8  64.7 -2.8     -90.6   270      433   01 58 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

02 03 30  0923+392     06 41 15  55.0  64.6 -2.8     -90.7    54      433   02 03 30
02 10 30  ---          06 48 16  56.4  64.6 -2.7     -91.9   420      487   02 03 31

02 11 00  0851+202     06 48 46  59.5 102.8 -2.1     -63.3    -5      487   02 11 05
02 14 00  ---          06 51 47  60.1 103.4 -2.1     -63.0   175      509   02 11 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

02 14 30  0851+202     06 52 17  60.2 103.5 -2.1     -62.9    24      509   02 14 30
02 23 30  ---          07 01 18  62.1 105.6 -1.9     -61.9   540      579   02 14 31

02 24 00  0851+202     07 01 49  62.2 105.7 -1.9     -61.9    24      579   02 24 00
02 33 20  ---          07 11 10  64.2 108.0 -1.7     -60.6   560      651   02 24 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

02 34 00  0851+202     07 11 50  64.3 108.2 -1.7     -60.5    34      651   02 34 00
02 43 30  ---          07 21 22  66.2 110.9 -1.6     -58.8   570      724   02 34 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

02 44 30  0851+202     07 22 22  66.4 111.2 -1.6     -58.6    54      724   02 44 30
02 49 00  ---          07 26 53  67.3 112.6 -1.5     -57.7   270      759   02 44 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

02 50 00  0851+202     07 27 53  67.5 113.0 -1.5     -57.5    54      759   02 50 00
02 59 30  ---          07 37 24  69.4 116.3 -1.3     -55.2   570      833   02 50 01

03 00 00  0851+202     07 37 54  69.5 116.5 -1.3     -55.0    24      833   03 00 00
03 09 30  ---          07 47 26  71.3 120.5 -1.1     -52.1   570      906   03 00 01

03 10 00  0851+202     07 47 56  71.4 120.7 -1.1     -51.9    24      906   03 10 00
03 19 30  ---          07 57 28  73.1 125.4 -1.0     -48.3   570      979   03 10 01

03 20 00  0851+202     07 57 58  73.2 125.7 -1.0     -48.1    24      979   03 20 00
03 29 30  ---          08 07 29  74.8 131.3 -0.8     -43.4   570     1053   03 20 01

03 30 00  0923+392     08 07 59  71.6  57.7 -1.3    -110.8   -30     1053   03 30 30
03 32 40  ---          08 10 40  72.1  57.1 -1.3    -111.8   130     1070   03 30 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

03 34 10  0923+392     08 12 10  72.4  56.7 -1.3    -112.3    84     1070   03 34 10
03 42 30  ---          08 20 31  73.8  54.4 -1.1    -115.8   500     1134   03 34 11

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

03 43 30  0923+392     08 21 32  74.0  54.1 -1.1    -116.3    54     1134   03 43 30
03 48 00  ---          08 26 02  74.8  52.6 -1.0    -118.4   270     1169   03 43 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

03 49 00  0923+392     08 27 02  75.0  52.3 -1.0    -118.9    54     1169   03 49 00
03 56 30  ---          08 34 34  76.2  49.2 -0.9    -123.0   450     1227   03 49 01

03 57 00  0851+202     08 35 04  78.4 154.9 -0.3     -22.9   -54     1227   03 57 54
04 06 00  ---          08 44 05  79.1 165.2 -0.2     -13.5   486     1289   03 57 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

04 06 30  0851+202     08 44 35  79.1 165.8 -0.2     -13.0    24     1289   04 06 30
04 16 30  ---          08 54 37  79.4 178.3 -0.0      -1.5   600     1367   04 06 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

04 17 00  0851+202     08 55 07  79.4 179.0 -0.0      -0.9    24     1367   04 17 00
04 24 00  ---          09 02 08  79.3 187.9  0.1       7.2   420     1421   04 17 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

04 24 30  0851+202     09 02 38  79.3 188.5  0.1       7.8    24     1421   04 24 30
04 29 30  ---          09 07 39  79.1 194.7  0.2      13.4   300     1459   04 24 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

04 30 00  0851+202     09 08 09  79.0 195.3  0.2      14.0    24     1459   04 30 00
04 40 00  ---          09 18 11  78.3 206.6  0.4      24.2   600     1537   04 30 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

04 40 30  0851+202     09 18 41  78.2 207.2  0.4      24.7    24     1537   04 40 30
04 47 00  ---          09 25 12  77.5 213.6  0.5      30.5   390     1587   04 40 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

04 47 30  0851+202     09 25 42  77.5 214.1  0.5      30.9    24     1587   04 47 30
04 52 00  ---          09 30 13  76.9 218.1  0.6      34.4   270     1622   04 47 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

04 53 30  0355+508     09 31 43  27.7 315.2  5.5      74.6   -15     1622   04 53 45
04 56 30  ---          09 34 44  27.2 315.3  5.6      74.0   165     1643   04 53 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

04 57 30  0355+508     09 35 44  27.1 315.4  5.6      73.9    54     1643   04 57 30
05 07 30  ---          09 45 45  25.6 315.9  5.7      72.2   600     1720   04 57 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

05 08 30  0355+508     09 46 46  25.4 316.0  5.8      72.0    54     1720   05 08 30
05 13 30  ---          09 51 46  24.7 316.2  5.8      71.1   300     1759   05 08 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

05 14 30  0355+508     09 52 47  24.5 316.3  5.9      71.0    54     1759   05 14 30
05 18 30  ---          09 56 47  23.9 316.5  5.9      70.3   240     1790   05 14 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

05 20 00  0851+202     09 58 17  72.4 236.6  1.0      49.9   -13     1790   05 20 13
05 29 30  ---          10 07 49  70.6 241.0  1.2      53.2   557     1862   05 20 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

05 30 00  0851+202     10 08 19  70.5 241.2  1.2      53.4    24     1862   05 30 00
05 39 00  ---          10 17 21  68.8 244.8  1.4      55.9   540     1931   05 30 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

05 39 30  0851+202     10 17 51  68.7 244.9  1.4      56.1    24     1931   05 39 30
05 45 30  ---          10 23 52  67.5 247.0  1.5      57.5   360     1978   05 39 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

05 46 00  0851+202     10 24 22  67.4 247.2  1.5      57.6    24     1978   05 46 00
05 50 00  ---          10 28 22  66.6 248.5  1.5      58.4   240     2008   05 46 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

05 50 30  0851+202     10 28 52  66.5 248.6  1.5      58.5    24     2008   05 50 30
06 00 30  ---          10 38 54  64.5 251.5  1.7      60.3   600     2086   05 50 31

06 01 00  0851+202     10 39 24  64.4 251.7  1.7      60.4    24     2086   06 01 00
06 08 30  ---          10 46 55  62.9 253.6  1.9      61.5   450     2144   06 01 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 09 00  0851+202     10 47 25  62.8 253.7  1.9      61.5    24     2144   06 09 00
06 14 30  ---          10 52 56  61.6 255.0  2.0      62.2   330     2186   06 09 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

06 17 00  0355+508     10 55 27  15.6 320.6  6.9      60.2    52     2186   06 17 00
06 19 00  ---          10 57 27  15.3 320.8  6.9      59.9   120     2202   06 17 01

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

06 20 00  0355+508     10 58 27  15.2 320.9  7.0      59.7    54     2202   06 20 00
06 29 30  ---          11 07 59  13.9 321.7  7.1      58.1   570     2275   06 20 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

06 30 30  0355+508     11 08 59  13.7 321.7  7.1      57.9    54     2275   06 30 30
06 36 30  ---          11 15 00  13.0 322.3  7.2      56.8   360     2321   06 30 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 37 30  0355+508     11 16 00  12.8 322.4  7.3      56.7    54     2321   06 37 30
06 42 00  ---          11 20 31  12.2 322.8  7.3      55.9   270     2356   06 37 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

06 43 30  0851+202     11 22 01  55.5 260.9  2.4      64.7    -3     2356   06 43 33
06 53 00  ---          11 31 33  53.5 262.5  2.6      65.2   567     2429   06 43 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

06 53 30  0851+202     11 32 03  53.4 262.6  2.6      65.3    24     2429   06 53 30
07 03 30  ---          11 42 04  51.2 264.2  2.8      65.7   600     2507   06 53 31

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

07 04 00  0851+202     11 42 35  51.1 264.3  2.8      65.7    24     2507   07 04 00
07 13 00  ---          11 51 36  49.2 265.6  2.9      65.9   540     2576   07 04 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Mar 2019   Day  75 ---

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 13 30  0851+202     11 52 06  49.1 265.7  2.9      66.0    24     2576   07 13 30
07 18 30  ---          11 57 07  48.0 266.4  3.0      66.1   300     2615   07 13 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

07 19 00  0851+202     11 57 37  47.9 266.5  3.0      66.1    24     2615   07 19 00
07 28 00  ---          12 06 38  46.0 267.7  3.2      66.2   540     2684   07 19 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

07 28 30  0851+202     12 07 09  45.8 267.8  3.2      66.2    24     2684   07 28 30
07 35 30  ---          12 14 10  44.3 268.7  3.3      66.3   420     2738   07 28 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 36 00  0851+202     12 14 40  44.2 268.8  3.3      66.3    24     2738   07 36 00
07 40 00  ---          12 18 40  43.4 269.3  3.4      66.3   240     2769   07 36 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

07 40 30  0923+392     12 19 11  54.3 295.3  2.8      90.1     0     2769   07 40 30
07 43 30  ---          12 22 11  53.7 295.3  2.9      89.6   180     2793   07 40 31

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25

07 44 00  0923+392     12 22 41  53.6 295.3  2.9      89.6    24     2793   07 44 00
07 51 00  ---          12 29 42  52.2 295.4  3.0      88.5   420     2847   07 44 01

 Next scan frequencies:  22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
 Next BBC frequencies:     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00

07 51 30  0923+392     12 30 12  52.1 295.4  3.0      88.4    24     2847   07 51 30
07 56 00  ---          12 34 43  51.3 295.4  3.1      87.7   270     2881   07 51 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 56 30  0923+392     12 35 13  51.2 295.4  3.1      87.7    24     2881   07 56 30
07 59 30  ---          12 38 14  50.6 295.5  3.2      87.2   180     2905   07 56 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    8         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  26  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22156.00  22156.00  22188.00  22188.00  22220.00  22220.00  22252.00  22252.00
   BBC fr=     656.00    656.00    688.00    688.00    720.00    720.00    752.00    752.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     695.99    695.99    727.99    727.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  26  27  28  29  30  31  32  33  34  58

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:   48         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  36  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
   BBC fr=     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     767.25    767.25    799.25    799.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  36  37  38  39  40  41  42  43  44  45

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   35         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  48  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
   BBC fr=     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     776.99    776.99    808.99    808.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  48  49  50  51  52  53  54  55  56  57

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   1328+307          13 28 49.657783   * 13 31 08.288075     13 32 01.760916       0.18
   J1331+3030        30 45 58.64055    * 30 30 32.95919      30 24 33.64697        0.17
 * 3C286             From catalog imbedded in main SCHED input file.
                     rfc_2018a Petrov and Kovalev, in preparation  603 observations

 * 0355+508          03 55 45.261377   * 03 59 29.747278     04 00 54.175951       0.16
   J0359+5057        50 49 20.28597    * 50 57 50.16192      51 01 04.82333        0.10
   NRAO150           /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  27427 observations

 * 0851+202          08 51 57.250617   * 08 54 48.874929     08 55 54.600792       0.11
   J0854+2006        20 17 58.41738    * 20 06 30.64083      20 02 02.58372        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  311901 observations

 * 0923+392          09 23 55.319219   * 09 27 03.013940     09 28 14.962793       0.13
   J0927+3902        39 15 23.56640    * 39 02 20.85180      38 57 20.77176        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  259044 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  3C286      ra1cm2.set            22                                0.350     0.000
             ra2cm2.set            23                                0.350     0.000
             ra7mm2.set            21                                0.350     0.000
  0355+508   ra1cm2.set            1 2 3 4 5 6 7 8 9 11 20 22  +    11.018   390.924
             ra2cm2.set            23 47 48                          0.142     7.792
             ra7mm2.set            15 16 17 21 35 36                 3.500    44.616
  0851+202   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 11 20  +    12.086   686.955
             ra2cm2.set            23 46 47 48                       0.617    39.933
             ra7mm2.set            15 16 17 21 35 36                 3.608   108.242
  0923+392   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 11 20  +     3.664   219.868
             ra2cm2.set            23 46 47 48                       0.200    15.000
             ra7mm2.set            15 16 17 21 35 36                 1.086    44.600


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   3C286              141.5
   0355+508            75.8
   0851+202           135.4
   0923+392           131.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

