  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 6cm global VLBI observations of IC860
 Exp. Code:  GV025   


Schedule Version:       3.00
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Eskil Varenius

Address:  Jodrell Bank Observatory, The University of Manchester
          Lower Withington, Macclesfield
          Cheshire, SK11 9DL
          UK

Phone:    +46706755341
EMAIL:    eskil.varenius@manchester.ac.uk
Fax:
Phone during observation: +46706755341

Observing mode: 6cm 1Gbps global VLBI (EVN+VLBA+eMERLIN)

Notes:    NB: Key file includes 1h eMERLIN+Jb after (08-09UT) allocation (20-08UT), if antennas are idle.
          Phase calibrator: J1303+2433
          Fringe finder / pol. cal / bandpass cal: J1327+2210
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

 ---------- End of block 7, VLBA_FD, VLBA_LA join ----------

 Next scan frequencies:  4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
 Next BBC frequencies:    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

03 06 44  J1327+2210   07 01 17   5.7  67.7 -6.4  H  -59.2     0        0   03 06 44
03 11 44  =1324+224    07 06 18   6.7  68.3 -6.4     -59.6     0       77   03 06 45

03 12 38  J1314+2348   07 07 12  10.1  68.4 -6.1     -60.9    40       77   03 12 38
03 14 38  =1312+240    07 09 13  10.5  68.6 -6.1     -61.0   120      108   03 12 39

03 15 07  IC860        07 09 42  11.0  67.9 -6.1     -61.2    21      108   03 15 07
03 19 07  ---          07 13 42  11.8  68.3 -6.0     -61.5   240      170   03 15 08

03 19 36  J1314+2348   07 14 12  11.5  69.1 -6.0     -61.4    21      170   03 19 36
03 21 36  =1312+240    07 16 12  11.9  69.4 -6.0     -61.6   120      201   03 19 37

 ---------- Ur leaves, VLBA_BR, VLBA_PT, VLBA_KP join ----------

03 22 05  IC860        07 16 41  12.3  68.7 -6.0     -61.7    21      201   03 22 05
03 26 05  ---          07 20 42  13.2  69.1 -5.9     -62.1   240      263   03 22 06

03 26 34  J1314+2348   07 21 11  12.9  69.9 -5.9     -62.0    21      263   03 26 34
03 28 34  =1312+240    07 23 11  13.3  70.1 -5.9     -62.1   120      294   03 26 35

03 29 03  IC860        07 23 40  13.8  69.4 -5.9     -62.3    20      294   03 29 03
03 33 03  ---          07 27 41  14.6  69.9 -5.8     -62.6   240      356   03 29 04

03 33 32  J1314+2348   07 28 10  14.3  70.7 -5.8     -62.5    21      356   03 33 32
03 35 32  =1312+240    07 30 10  14.8  70.9 -5.8     -62.6   120      386   03 33 33

03 36 01  IC860        07 30 39  15.2  70.2 -5.8     -62.8    20      386   03 36 01
03 40 01  ---          07 34 40  16.0  70.6 -5.7     -63.1   240      448   03 36 02

03 40 30  J1314+2348   07 35 09  15.8  71.4 -5.7     -63.0    21      448   03 40 30
03 42 30  =1312+240    07 37 09  16.2  71.7 -5.6     -63.1   120      479   03 40 31

03 42 58  IC860        07 37 38  16.6  70.9 -5.6     -63.3    20      479   03 42 58
03 46 58  ---          07 41 38  17.4  71.3 -5.6     -63.6   240      541   03 42 59

03 47 27  J1314+2348   07 42 07  17.2  72.2 -5.6     -63.5    21      541   03 47 27
03 49 27  =1312+240    07 44 08  17.6  72.4 -5.5     -63.6   120      572   03 47 28

03 49 56  IC860        07 44 36  18.0  71.7 -5.5     -63.9    21      572   03 49 56
03 53 56  ---          07 48 37  18.8  72.1 -5.5     -64.1   240      634   03 49 57
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

03 54 25  J1314+2348   07 49 06  18.6  72.9 -5.4     -63.9    21      634   03 54 25
03 56 25  =1312+240    07 51 06  19.0  73.1 -5.4     -64.1   120      665   03 54 26

03 56 54  IC860        07 51 35  19.4  72.4 -5.4     -64.3    21      665   03 56 54
04 00 54  ---          07 55 36  20.2  72.8 -5.3     -64.6   240      727   03 56 55

04 01 22  J1314+2348   07 56 05  20.1  73.7 -5.3     -64.4    21      727   04 01 22
04 03 22  =1312+240    07 58 05  20.5  73.9 -5.3     -64.5   120      757   04 01 23

04 03 51  IC860        07 58 34  20.9  73.1 -5.3     -64.8    21      757   04 03 51
04 07 51  ---          08 02 35  21.7  73.5 -5.2     -65.1   240      819   04 03 52

 ---------- End of block 8, VLBA_OV joins ----------

04 08 44  J1327+2210   08 03 27  18.3  74.7 -5.4     -63.6    37      819   04 08 44
04 13 44  =1324+224    08 08 28  19.4  75.2 -5.3     -63.9   300      897   04 08 45

04 14 35  J1314+2348   08 09 19  22.8  75.1 -5.1     -65.2    37      897   04 14 35
04 16 35  =1312+240    08 11 20  23.2  75.3 -5.1     -65.3   120      927   04 14 36

04 17 04  IC860        08 11 49  23.6  74.5 -5.1     -65.7    21      927   04 17 04
04 21 04  ---          08 15 49  24.4  74.9 -5.0     -65.9   240      989   04 17 05

04 21 32  J1314+2348   08 16 18  24.3  75.8 -5.0     -65.6    21      989   04 21 32
04 23 32  =1312+240    08 18 18  24.7  76.0 -5.0     -65.8   120     1020   04 21 33

04 24 01  IC860        08 18 47  25.0  75.2 -5.0     -66.1    21     1020   04 24 01
04 28 01  ---          08 22 48  25.9  75.6 -4.9     -66.3   240     1082   04 24 02

04 28 30  J1314+2348   08 23 17  25.7  76.5 -4.9     -66.0    20     1082   04 28 30
04 30 30  =1312+240    08 25 17  26.1  76.7 -4.8     -66.1   120     1113   04 28 31

04 30 59  IC860        08 25 46  26.5  75.9 -4.8     -66.5    21     1113   04 30 59
04 34 59  ---          08 29 47  27.3  76.3 -4.8     -66.8   240     1175   04 31 00

04 35 27  J1314+2348   08 30 15  27.2  77.2 -4.8     -66.4    20     1175   04 35 27
04 37 27  =1312+240    08 32 16  27.6  77.4 -4.7     -66.5   120     1206   04 35 28

04 37 56  IC860        08 32 45  28.0  76.6 -4.7     -66.9    21     1206   04 37 56
04 41 56  ---          08 36 45  28.8  77.0 -4.7     -67.1   240     1268   04 37 57

04 42 25  J1314+2348   08 37 14  28.6  77.9 -4.6     -66.8    20     1268   04 42 25
04 44 25  =1312+240    08 39 14  29.1  78.1 -4.6     -66.9   120     1298   04 42 26
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

04 44 54  IC860        08 39 43  29.4  77.3 -4.6     -67.3    21     1298   04 44 54
04 48 54  ---          08 43 44  30.3  77.7 -4.5     -67.5   240     1360   04 44 55

04 49 22  J1314+2348   08 44 12  30.1  78.7 -4.5     -67.1    20     1360   04 49 22
04 51 22  =1312+240    08 46 13  30.5  78.9 -4.5     -67.2   120     1391   04 49 23

 ---------- Hh leaves ----------

04 51 51  IC860        08 46 42  30.9  78.0 -4.5     -67.7    21     1391   04 51 51
04 55 51  ---          08 50 42  31.7  78.4 -4.4     -67.9   240     1453   04 51 52

04 56 19  J1314+2348   08 51 11  31.6  79.4 -4.4     -67.5    20     1453   04 56 19
04 58 19  =1312+240    08 53 11  32.0  79.6 -4.4     -67.6   120     1484   04 56 20

04 58 48  IC860        08 53 40  32.4  78.7 -4.4     -68.0    21     1484   04 58 48
05 02 48  ---          08 57 41  33.2  79.1 -4.3     -68.2   240     1546   04 58 49

05 03 17  J1314+2348   08 58 09  33.1  80.1 -4.3     -67.8    20     1546   05 03 17
05 05 17  =1312+240    09 00 10  33.5  80.3 -4.3     -67.9   120     1577   05 03 18

05 05 45  IC860        09 00 38  33.8  79.4 -4.3     -68.4    21     1577   05 05 45
05 09 45  ---          09 04 39  34.7  79.8 -4.2     -68.6   240     1639   05 05 46

 ---------- End of block 9 ----------

05 10 35  J1327+2210   09 05 29  31.4  81.3 -4.4     -66.6    35     1639   05 10 35
05 15 35  =1324+224    09 10 30  32.4  81.9 -4.3     -66.8   300     1716   05 10 36

05 16 23  J1314+2348   09 11 18  35.9  81.5 -4.1     -68.3    33     1716   05 16 23
05 18 23  =1312+240    09 13 18  36.3  81.7 -4.0     -68.4   120     1747   05 16 24

05 18 51  IC860        09 13 47  36.6  80.7 -4.0     -69.0    20     1747   05 18 51
05 22 51  ---          09 17 47  37.5  81.2 -4.0     -69.1   240     1809   05 18 52

05 23 20  J1314+2348   09 18 16  37.3  82.2 -4.0     -68.6    20     1809   05 23 20
05 25 20  =1312+240    09 20 16  37.8  82.4 -3.9     -68.7   120     1840   05 23 21

05 25 48  IC860        09 20 45  38.1  81.5 -3.9     -69.3    20     1840   05 25 48
05 29 48  ---          09 24 45  38.9  81.9 -3.9     -69.4   240     1901   05 25 49

05 30 17  J1314+2348   09 25 14  38.8  82.9 -3.8     -68.8    20     1901   05 30 17
05 32 17  =1312+240    09 27 14  39.3  83.1 -3.8     -68.9   120     1932   05 30 18

05 32 45  IC860        09 27 43  39.6  82.2 -3.8     -69.5    20     1932   05 32 45
05 36 45  ---          09 31 43  40.4  82.6 -3.7     -69.7   240     1994   05 32 46
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

05 37 13  J1314+2348   09 32 12  40.3  83.7 -3.7     -69.1    20     1994   05 37 13
05 39 13  =1312+240    09 34 12  40.7  83.9 -3.7     -69.1   120     2025   05 37 14

05 39 42  IC860        09 34 40  41.1  82.9 -3.7     -69.8    20     2025   05 39 42
05 43 42  ---          09 38 41  41.9  83.3 -3.6     -69.9   240     2087   05 39 43

05 44 10  J1314+2348   09 39 09  41.8  84.4 -3.6     -69.3    20     2087   05 44 10
05 46 10  =1312+240    09 41 10  42.2  84.6 -3.6     -69.3   120     2118   05 44 11

05 46 38  IC860        09 41 38  42.5  83.6 -3.6     -70.0    20     2118   05 46 38
05 50 38  ---          09 45 39  43.4  84.0 -3.5     -70.2   240     2180   05 46 39

05 51 07  J1314+2348   09 46 07  43.3  85.2 -3.5     -69.5    20     2180   05 51 07
05 53 07  =1312+240    09 48 07  43.7  85.4 -3.5     -69.5   120     2211   05 51 08

05 53 35  IC860        09 48 36  44.0  84.4 -3.5     -70.2    20     2211   05 53 35
05 57 35  ---          09 52 37  44.9  84.8 -3.4     -70.4   240     2272   05 53 36

05 58 03  J1314+2348   09 53 05  44.8  86.0 -3.4     -69.6    20     2272   05 58 03
06 00 03  =1312+240    09 55 05  45.2  86.2 -3.3     -69.7   120     2303   05 58 04

06 00 31  IC860        09 55 33  45.5  85.1 -3.3     -70.4    20     2303   06 00 31
06 04 31  ---          09 59 34  46.4  85.6 -3.3     -70.5   240     2365   06 00 32

06 05 00  J1314+2348   10 00 02  46.3  86.7 -3.3     -69.8    20     2365   06 05 00
06 07 00  =1312+240    10 02 03  46.7  87.0 -3.2     -69.8   120     2396   06 05 01

06 07 28  IC860        10 02 31  47.0  85.9 -3.2     -70.6    20     2396   06 07 28
06 11 28  ---          10 06 32  47.9  86.3 -3.2     -70.7   240     2458   06 07 29

 ---------- End of block 10, Zc leaves ----------

06 12 15  J1327+2210   10 07 19  44.6  88.3 -3.3     -68.1    33     2458   06 12 15
06 17 15  =1324+224    10 12 20  45.7  88.9 -3.3     -68.2   300     2535   06 12 16

06 18 01  J1314+2348   10 13 05  49.1  88.3 -3.0     -69.9    31     2535   06 18 01
06 20 01  =1312+240    10 15 06  49.5  88.5 -3.0     -70.0   120     2566   06 18 02

06 20 29  IC860        10 15 34  49.8  87.4 -3.0     -70.9    20     2566   06 20 29
06 24 29  ---          10 19 35  50.7  87.8 -2.9     -70.9   240     2628   06 20 30

06 24 57  J1314+2348   10 20 03  50.6  89.1 -2.9     -70.0    20     2628   06 24 57
06 26 57  =1312+240    10 22 03  51.0  89.4 -2.9     -70.0   120     2659   06 24 58
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

06 27 25  IC860        10 22 31  51.3  88.2 -2.9     -70.9    19     2659   06 27 25
06 31 25  ---          10 26 32  52.2  88.6 -2.8     -71.0   240     2721   06 27 26

06 31 53  J1314+2348   10 27 00  52.1  90.0 -2.8     -70.0    20     2721   06 31 53
06 33 53  =1312+240    10 29 00  52.5  90.2 -2.8     -70.0   120     2752   06 31 54

06 34 21  IC860        10 29 28  52.8  89.0 -2.8     -71.0    19     2752   06 34 21
06 38 21  ---          10 33 29  53.7  89.5 -2.7     -71.0   240     2813   06 34 22

06 38 49  J1314+2348   10 33 57  53.6  90.9 -2.7     -70.0    19     2813   06 38 49
06 40 49  =1312+240    10 35 58  54.0  91.2 -2.7     -70.0   120     2844   06 38 50

06 41 17  IC860        10 36 26  54.3  89.9 -2.7     -71.0    19     2844   06 41 17
06 45 17  ---          10 40 26  55.2  90.4 -2.6     -71.0   240     2906   06 41 18

06 45 45  J1314+2348   10 40 54  55.1  91.8 -2.6     -69.9    19     2906   06 45 45
06 47 45  =1312+240    10 42 55  55.5  92.1 -2.5     -69.9   120     2937   06 45 46

06 48 13  IC860        10 43 23  55.8  90.8 -2.5     -71.0    19     2937   06 48 13
06 52 13  ---          10 47 23  56.7  91.3 -2.5     -71.0   240     2999   06 48 14

06 52 41  J1314+2348   10 47 52  56.6  92.8 -2.5     -69.8    19     2999   06 52 41
06 54 41  =1312+240    10 49 52  57.0  93.1 -2.4     -69.8   120     3030   06 52 42

06 55 09  IC860        10 50 20  57.3  91.7 -2.4     -71.0    19     3030   06 55 09
06 59 09  ---          10 54 20  58.2  92.3 -2.4     -70.9   240     3092   06 55 10

06 59 37  J1314+2348   10 54 49  58.1  93.8 -2.3     -69.7    19     3092   06 59 37
07 01 37  =1312+240    10 56 49  58.5  94.1 -2.3     -69.6   120     3123   06 59 38

07 02 04  IC860        10 57 17  58.8  92.7 -2.3     -70.8    19     3123   07 02 04
07 06 04  ---          11 01 17  59.6  93.3 -2.2     -70.8   240     3184   07 02 05

07 06 33  J1314+2348   11 01 45  59.5  94.9 -2.2     -69.4    19     3184   07 06 33
07 08 33  =1312+240    11 03 46  60.0  95.2 -2.2     -69.4   120     3215   07 06 34

07 09 00  IC860        11 04 13  60.3  93.7 -2.2     -70.7    19     3215   07 09 00
07 13 00  ---          11 08 14  61.1  94.3 -2.1     -70.6   240     3277   07 09 01

 ---------- End of block 11, VLBA_MK joins ----------

07 13 46  J1327+2210   11 09 00  57.9  97.0 -2.3     -67.2    31     3277   07 13 46
07 18 46  =1324+224    11 14 01  58.9  97.8 -2.2     -66.9   300     3354   07 13 47
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

07 19 30  J1314+2348   11 14 45  62.3  97.1 -2.0     -68.8    30     3354   07 19 30
07 21 30  =1312+240    11 16 45  62.8  97.4 -2.0     -68.7   120     3385   07 19 31

07 21 58  IC860        11 17 13  63.1  95.8 -2.0     -70.2    19     3385   07 21 58
07 25 58  ---          11 21 14  63.9  96.5 -1.9     -70.0   240     3447   07 21 59

07 26 26  J1314+2348   11 21 42  63.8  98.4 -1.9     -68.4    19     3447   07 26 26
07 28 26  =1312+240    11 23 42  64.2  98.7 -1.9     -68.2   120     3478   07 26 27

07 28 54  IC860        11 24 10  64.6  97.0 -1.9     -69.8    19     3478   07 28 54
07 32 54  ---          11 28 11  65.4  97.8 -1.8     -69.6   240     3540   07 28 55

07 33 22  J1314+2348   11 28 39  65.3  99.7 -1.8     -67.8    19     3540   07 33 22
07 35 22  =1312+240    11 30 39  65.7 100.2 -1.7     -67.7   120     3571   07 33 23

07 35 50  IC860        11 31 07  66.0  98.3 -1.7     -69.3    18     3571   07 35 50
07 39 50  ---          11 35 08  66.9  99.1 -1.7     -69.0   240     3633   07 35 51

07 40 18  J1314+2348   11 35 36  66.8 101.2 -1.7     -67.2    19     3633   07 40 18
07 42 18  =1312+240    11 37 37  67.2 101.7 -1.6     -67.0   120     3664   07 40 19

07 42 46  IC860        11 38 04  67.5  99.8 -1.6     -68.7    18     3664   07 42 46
07 46 46  ---          11 42 05  68.4 100.7 -1.6     -68.3   240     3725   07 42 47

07 47 14  J1314+2348   11 42 33  68.2 102.9 -1.6     -66.4    19     3725   07 47 14
07 49 14  =1312+240    11 44 34  68.6 103.4 -1.5     -66.1   120     3756   07 47 15

07 49 42  IC860        11 45 01  69.0 101.3 -1.5     -68.0    18     3756   07 49 42
07 53 42  ---          11 49 02  69.8 102.3 -1.4     -67.5   240     3818   07 49 43

 ---------- End of block 12, EVN leaves ----------

07 54 27  J1327+2210   11 49 47  66.5 105.4 -1.6     -63.5    30     3818   07 54 27
07 59 27  =1324+224    11 54 48  67.5 106.8 -1.6     -62.8   300     3895   07 54 28

07 59 59  J1314+2348   11 55 20  70.9 106.4 -1.3     -64.4    18     3895   07 59 59
08 01 59  =1312+240    11 57 21  71.3 107.0 -1.3     -64.0   120     3926   08 00 00

08 02 15  IC860        11 57 37  71.6 104.7 -1.3     -66.2     7     3926   08 02 15
08 06 15  ---          12 01 38  72.5 105.9 -1.2     -65.5   240     3988   08 02 16

08 06 32  J1314+2348   12 01 55  72.2 108.5 -1.2     -63.0     7     3988   08 06 32
08 08 32  =1312+240    12 03 55  72.6 109.2 -1.2     -62.6   120     4019   08 06 33
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

08 08 49  IC860        12 04 12  73.0 106.7 -1.2     -64.9     7     4019   08 08 49
08 12 49  ---          12 08 12  73.8 108.1 -1.1     -64.0   240     4081   08 08 50

08 13 06  J1314+2348   12 08 30  73.6 110.9 -1.1     -61.4     7     4081   08 13 06
08 15 06  =1312+240    12 10 30  74.0 111.6 -1.1     -60.9   120     4112   08 13 07

08 15 22  IC860        12 10 46  74.3 109.0 -1.1     -63.4     7     4112   08 15 22
08 19 22  ---          12 14 47  75.1 110.6 -1.0     -62.3   240     4174   08 15 23

08 19 39  J1314+2348   12 15 04  74.9 113.6 -1.0     -59.5     7     4174   08 19 39
08 21 39  =1312+240    12 17 05  75.3 114.5 -1.0     -58.8   120     4205   08 19 40

08 21 56  IC860        12 17 21  75.7 111.7 -1.0     -61.5     7     4205   08 21 56
08 25 56  ---          12 21 22  76.5 113.5 -0.9     -60.1   240     4266   08 21 57

08 26 13  J1314+2348   12 21 39  76.1 116.8 -0.9     -57.0     7     4266   08 26 13
08 28 13  =1312+240    12 23 39  76.5 117.8 -0.9     -56.2   120     4297   08 26 14

08 28 30  IC860        12 23 56  77.0 114.8 -0.9     -59.1     7     4297   08 28 30
08 32 30  ---          12 27 57  77.7 117.0 -0.8     -57.4   240     4359   08 28 31

08 32 47  J1314+2348   12 28 14  77.4 120.5 -0.8     -54.1     7     4359   08 32 47
08 34 47  =1312+240    12 30 14  77.8 121.7 -0.8     -53.1   120     4390   08 32 48

08 35 03  IC860        12 30 31  78.2 118.5 -0.8     -56.2     6     4390   08 35 03
08 39 03  ---          12 34 31  79.0 121.2 -0.7     -54.0   240     4452   08 35 04

08 39 20  J1314+2348   12 34 48  78.6 124.9 -0.7     -50.4     7     4452   08 39 20
08 41 20  =1312+240    12 36 49  78.9 126.4 -0.6     -49.1   120     4483   08 39 21

08 41 37  IC860        12 37 05  79.4 123.0 -0.6     -52.4     6     4483   08 41 37
08 45 37  ---          12 41 06  80.1 126.3 -0.6     -49.7   240     4545   08 41 38

08 45 54  J1314+2348   12 41 23  79.7 130.2 -0.6     -45.8     7     4545   08 45 54
08 47 54  =1312+240    12 43 23  80.0 132.1 -0.5     -44.2   120     4576   08 45 55

08 48 11  IC860        12 43 40  80.6 128.6 -0.5     -47.7     6     4576   08 48 11
08 52 11  ---          12 47 41  81.2 132.6 -0.5     -44.1   240     4637   08 48 12

08 52 28  J1314+2348   12 47 58  80.7 136.7 -0.5     -40.1     6     4637   08 52 28
08 54 28  =1312+240    12 49 58  81.0 139.0 -0.4     -38.1   120     4668   08 52 29

08 54 44  IC860        12 50 15  81.6 135.5 -0.4     -41.5     6     4668   08 54 44
08 58 44  ---          12 54 16  82.2 140.5 -0.4     -37.0   240     4730   08 54 45
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

 ---------- End of block 13, eMERLIN leaves. Only VLBA now. ----------

08 59 17  J1327+2210   12 54 48  78.7 137.1 -0.6     -39.2    17     4730   08 59 17
09 04 17  =1324+224    12 59 49  79.4 142.0 -0.5     -34.9   300     4808   08 59 18

09 04 32  J1314+2348   13 00 04  82.3 152.5 -0.3     -25.7     0     4808   09 04 32
09 06 32  =1312+240    13 02 05  82.4 155.7 -0.2     -22.8   120     4838   09 04 33

09 06 42  IC860        13 02 15  83.2 152.7 -0.2     -25.7     0     4838   09 06 42
09 10 42  ---          13 06 15  83.5 160.0 -0.2     -18.8   240     4900   09 06 43

09 10 52  J1314+2348   13 06 26  82.8 163.0 -0.2     -16.0     0     4900   09 10 52
09 12 52  =1312+240    13 08 26  82.9 166.5 -0.1     -12.6   120     4931   09 10 53

09 13 02  IC860        13 08 36  83.7 164.6 -0.1     -14.5     1     4931   09 13 02
09 17 02  ---          13 12 37  83.8 172.8 -0.1      -6.8   240     4993   09 13 03

09 17 13  J1314+2348   13 12 47  83.0 174.6 -0.0      -5.1     1     4993   09 17 13
09 19 13  =1312+240    13 14 47  83.1 178.4 -0.0      -1.5   120     5024   09 17 14

09 19 23  IC860        13 14 57  83.9 177.8 -0.0      -2.1     1     5024   09 19 23
09 23 23  ---          13 18 58  83.8 186.4  0.0       6.0   240     5086   09 19 24

09 23 33  J1314+2348   13 19 08  83.0 186.6  0.1       6.2     1     5086   09 23 33
09 25 33  =1312+240    13 21 09  83.0 190.3  0.1       9.7   120     5117   09 23 34

09 25 43  IC860        13 21 19  83.8 191.2  0.1      10.6     0     5117   09 25 43
09 29 43  ---          13 25 19  83.5 199.2  0.2      18.2   240     5179   09 25 44

09 29 53  J1314+2348   13 25 29  82.7 198.1  0.2      17.0     0     5179   09 29 53
09 31 53  =1312+240    13 27 30  82.6 201.5  0.2      20.1   120     5209   09 29 54

09 32 03  IC860        13 27 40  83.4 203.6  0.2      22.3     0     5209   09 32 03
09 36 03  ---          13 31 40  83.0 210.5  0.3      28.7   240     5271   09 31 54

09 36 13  J1314+2348   13 31 50  82.2 208.4  0.3      26.5     0     5271   09 36 12
09 38 13  =1312+240    13 33 50  82.0 211.3  0.3      29.3   120     5302   09 36 04

09 38 22  IC860        13 34 00  82.7 214.2  0.3      32.1     0     5302   09 38 22
09 42 22  ---          13 38 01  82.2 219.9  0.4      37.3   240     5364   09 38 14

09 42 32  J1314+2348   13 38 11  81.5 217.2  0.4      34.6     0     5364   09 42 32
09 44 32  =1312+240    13 40 11  81.2 219.7  0.4      36.9   120     5395   09 42 23
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

09 44 42  IC860        13 40 21  81.8 222.9  0.4      40.1     0     5395   09 44 42
09 48 42  ---          13 44 22  81.2 227.5  0.5      44.2   240     5457   09 44 43

09 48 52  J1314+2348   13 44 32  80.6 224.5  0.5      41.2     0     5457   09 48 52
09 50 52  =1312+240    13 46 32  80.2 226.6  0.5      43.0   120     5488   09 48 53

09 51 03  IC860        13 46 42  80.9 229.9  0.5      46.3     0     5488   09 51 03
09 55 03  ---          13 50 43  80.2 233.6  0.6      49.6   240     5550   09 51 04

 ---------- End of block 14 ----------

09 55 25  J1327+2210   13 51 06  80.0 212.6  0.4      30.0     0     5550   09 55 25
10 00 25  =1324+224    13 56 07  79.4 218.1  0.5      34.9   300     5627   09 55 26

10 00 47  J1314+2348   13 56 29  78.6 235.1  0.7      50.4     2     5627   10 00 47
10 02 47  =1312+240    13 58 29  78.2 236.5  0.7      51.6   120     5658   10 00 48

10 02 57  IC860        13 58 39  78.7 239.7  0.7      54.7     0     5658   10 02 57
10 06 57  ---          14 02 40  78.0 242.2  0.8      56.8   240     5720   10 02 58

10 07 07  J1314+2348   14 02 50  77.4 239.4  0.8      54.0     0     5720   10 07 07
10 09 07  =1312+240    14 04 50  77.1 240.6  0.8      54.9   120     5750   10 07 08

10 09 17  IC860        14 05 00  77.5 243.6  0.8      57.9     0     5750   10 09 17
10 13 17  ---          14 09 01  76.8 245.7  0.9      59.5   240     5812   10 09 18

10 13 27  J1314+2348   14 09 11  76.2 243.0  0.9      56.9     0     5812   10 13 27
10 15 27  =1312+240    14 11 11  75.9 244.0  0.9      57.6   120     5843   10 13 18

10 15 37  IC860        14 11 21  76.3 246.8  0.9      60.4     0     5843   10 15 37
10 19 37  ---          14 15 22  75.5 248.7  1.0      61.7   240     5905   10 15 28

10 19 47  J1314+2348   14 15 31  75.0 246.1  1.0      59.2     0     5905   10 19 47
10 21 47  =1312+240    14 17 32  74.6 247.0  1.0      59.9   120     5936   10 19 38

10 21 56  IC860        14 17 41  75.0 249.6  1.0      62.4     0     5936   10 21 56
10 25 56  ---          14 21 42  74.2 251.2  1.1      63.5   240     5998   10 21 48

10 26 06  J1314+2348   14 21 52  73.7 248.8  1.1      61.2     0     5998   10 26 06
10 28 06  =1312+240    14 23 52  73.3 249.5  1.1      61.7   120     6029   10 25 57

10 28 16  IC860        14 24 02  73.7 252.0  1.1      64.1     0     6029   10 28 16
10 32 16  ---          14 28 03  72.9 253.4  1.2      65.0   240     6091   10 28 07
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

10 32 26  J1314+2348   14 28 12  72.5 251.1  1.2      62.8     0     6091   10 32 25
10 34 26  =1312+240    14 30 13  72.1 251.8  1.2      63.2   120     6121   10 32 17

10 34 35  IC860        14 30 22  72.4 254.2  1.2      65.5     0     6121   10 34 35
10 38 35  ---          14 34 23  71.6 255.4  1.3      66.2   240     6183   10 34 27

10 38 45  J1314+2348   14 34 33  71.2 253.2  1.3      64.1     0     6183   10 38 45
10 40 45  =1312+240    14 36 33  70.8 253.8  1.3      64.5   120     6214   10 38 36

10 40 55  IC860        14 36 43  71.1 256.0  1.3      66.6     0     6214   10 40 54
10 44 55  ---          14 40 43  70.3 257.1  1.4      67.2   240     6276   10 40 46

10 45 04  J1314+2348   14 40 53  69.9 255.1  1.4      65.2     0     6276   10 45 04
10 47 04  =1312+240    14 42 53  69.4 255.6  1.5      65.5   120     6307   10 44 56

10 47 14  IC860        14 43 03  69.8 257.7  1.5      67.5     0     6307   10 47 14
10 51 14  ---          14 47 04  69.0 258.7  1.5      68.0   240     6369   10 47 05

 ---------- End of block 15 ----------

10 51 32  J1327+2210   14 47 22  70.3 249.0  1.3      60.1     3     6369   10 51 32
10 56 32  =1324+224    14 52 23  69.3 250.7  1.4      61.2   300     6446   10 51 33

10 56 48  J1314+2348   14 52 39  67.4 258.1  1.6      66.8     3     6446   10 56 48
10 58 48  =1312+240    14 54 39  67.0 258.5  1.7      67.1   120     6477   10 56 49

10 58 58  IC860        14 54 49  67.3 260.4  1.6      68.8     0     6477   10 58 58
11 02 58  ---          14 58 50  66.5 261.3  1.7      69.2   240     6539   10 58 49

11 03 08  J1314+2348   14 58 59  66.1 259.5  1.7      67.5     0     6539   11 03 07
11 05 08  =1312+240    15 01 00  65.6 259.9  1.8      67.7   120     6570   11 02 59

11 05 17  IC860        15 01 09  66.0 261.7  1.8      69.4     0     6570   11 05 17
11 09 17  ---          15 05 10  65.1 262.5  1.8      69.7   240     6632   11 05 09

11 09 27  J1314+2348   15 05 19  64.7 260.8  1.8      68.1     1     6632   11 09 26
11 11 27  =1312+240    15 07 20  64.3 261.2  1.9      68.2   120     6663   11 09 18

11 11 36  IC860        15 07 29  64.6 262.9  1.9      69.8     1     6663   11 11 36
11 15 36  ---          15 11 30  63.8 263.6  1.9      70.0   240     6725   11 11 28

11 15 46  J1314+2348   15 11 40  63.4 262.0  1.9      68.5     1     6725   11 15 45
11 17 46  =1312+240    15 13 40  62.9 262.4  2.0      68.7   120     6756   11 15 37
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

11 17 55  IC860        15 13 50  63.3 264.1  2.0      70.2     1     6756   11 17 55
11 21 55  ---          15 17 50  62.4 264.7  2.0      70.3   240     6818   11 17 47

11 22 05  J1314+2348   15 18 00  62.0 263.2  2.0      68.9     1     6818   11 22 04
11 24 05  =1312+240    15 20 00  61.6 263.5  2.1      69.0   120     6849   11 21 56

11 24 15  IC860        15 20 10  61.9 265.1  2.1      70.4     1     6849   11 24 14
11 28 15  ---          15 24 10  61.0 265.7  2.1      70.6   240     6911   11 24 06

11 28 24  J1314+2348   15 24 20  60.7 264.3  2.1      69.2     1     6911   11 28 23
11 30 24  =1312+240    15 26 20  60.2 264.6  2.2      69.3   120     6943   11 28 16

11 30 34  IC860        15 26 30  60.5 266.1  2.2      70.6     1     6943   11 30 33
11 34 34  ---          15 30 31  59.7 266.7  2.2      70.8   240     7005   11 30 25

11 34 44  J1314+2348   15 30 40  59.3 265.3  2.3      69.5     1     7005   11 34 43
11 36 44  =1312+240    15 32 41  58.9 265.6  2.3      69.5   120     7036   11 34 35

11 36 53  IC860        15 32 51  59.2 267.1  2.3      70.8     1     7036   11 36 52
11 40 53  ---          15 36 51  58.3 267.6  2.3      70.9   240     7098   11 36 45

11 41 03  J1314+2348   15 37 01  57.9 266.3  2.4      69.7     1     7098   11 41 03
11 43 03  =1312+240    15 39 02  57.5 266.6  2.4      69.7   120     7129   11 41 04

11 43 13  IC860        15 39 12  57.8 268.0  2.4      70.9     1     7129   11 43 13
11 47 13  ---          15 43 12  57.0 268.5  2.5      71.0   240     7191   11 43 14

 ---------- End of block 16 ----------

11 47 29  J1327+2210   15 43 28  58.6 262.4  2.3      67.0     3     7191   11 47 29
11 52 29  =1324+224    15 48 28  57.5 263.3  2.3      67.2   300     7268   11 47 30

11 52 43  J1314+2348   15 48 42  55.4 267.9  2.6      69.9     2     7268   11 52 43
11 54 43  =1312+240    15 50 43  55.0 268.2  2.6      69.9   120     7299   11 52 44

11 54 53  IC860        15 50 53  55.3 269.5  2.6      71.0     2     7299   11 54 53
11 58 53  ---          15 54 54  54.4 270.0  2.6      71.0   240     7361   11 54 54

11 59 03  J1314+2348   15 55 04  54.1 268.8  2.7      70.0     2     7361   11 59 03
12 01 03  =1312+240    15 57 05  53.6 269.1  2.7      70.0   120     7392   11 59 04

12 01 14  IC860        15 57 15  53.9 270.3  2.7      71.0     2     7392   12 01 14
12 05 14  ---          16 01 16  53.1 270.8  2.8      71.0   240     7453   12 01 15
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

12 05 25  J1314+2348   16 01 26  52.7 269.6  2.8      70.0     2     7453   12 05 25
12 07 25  =1312+240    16 03 27  52.3 269.9  2.8      70.0   120     7484   12 05 26

12 07 35  IC860        16 03 38  52.6 271.1  2.8      71.0     2     7484   12 07 35
12 11 35  ---          16 07 38  51.7 271.6  2.9      71.0   240     7546   12 07 36

12 11 46  J1314+2348   16 07 49  51.3 270.5  2.9      70.0     2     7546   12 11 46
12 13 46  =1312+240    16 09 50  50.9 270.7  2.9      70.0   120     7577   12 11 47

12 13 57  IC860        16 10 01  51.2 271.9  2.9      70.9     3     7577   12 13 57
12 17 57  ---          16 14 01  50.3 272.4  3.0      70.9   240     7639   12 13 58

12 18 09  J1314+2348   16 14 13  49.9 271.2  3.0      70.0     3     7639   12 18 09
12 20 09  =1312+240    16 16 13  49.5 271.5  3.0      70.0   120     7670   12 18 10

12 20 20  IC860        16 16 24  49.8 272.6  3.0      70.9     3     7670   12 20 20
12 24 20  ---          16 20 25  49.0 273.1  3.1      70.8   240     7732   12 20 21

12 24 31  J1314+2348   16 20 36  48.6 272.0  3.1      69.9     3     7732   12 24 31
12 26 31  =1312+240    16 22 37  48.1 272.2  3.1      69.9   120     7763   12 24 32

12 26 43  IC860        16 22 48  48.4 273.4  3.1      70.7     3     7763   12 26 43
12 30 43  ---          16 26 49  47.6 273.8  3.2      70.7   240     7824   12 26 44

12 30 54  J1314+2348   16 27 00  47.2 272.8  3.2      69.8     3     7824   12 30 54
12 32 54  =1312+240    16 29 00  46.8 273.0  3.2      69.8   120     7855   12 30 55

12 33 05  IC860        16 29 12  47.1 274.1  3.2      70.6     3     7855   12 33 05
12 37 05  ---          16 33 12  46.2 274.5  3.3      70.5   240     7917   12 33 06

12 37 15  J1314+2348   16 33 22  45.8 273.5  3.3      69.7     2     7917   12 37 15
12 39 15  =1312+240    16 35 23  45.4 273.7  3.3      69.7   120     7948   12 37 16

12 39 25  IC860        16 35 33  45.7 274.8  3.3      70.5     1     7948   12 39 24
12 43 25  ---          16 39 33  44.8 275.2  3.4      70.3   240     8010   12 39 16

12 43 35  J1314+2348   16 39 43  44.5 274.2  3.4      69.6     1     8010   12 43 33
12 45 35  =1312+240    16 41 43  44.0 274.4  3.4      69.5   120     8041   12 43 26

12 45 44  IC860        16 41 53  44.4 275.5  3.4      70.3     1     8041   12 45 43
12 49 44  ---          16 45 53  43.5 275.9  3.5      70.2   240     8103   12 45 36
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

 ---------- End of block 17, VLBA_SC leaves ----------

12 50 25  J1327+2210   16 46 34  45.0 271.4  3.3      68.2    30     8103   12 50 25
12 55 25  =1324+224    16 51 35  44.0 272.0  3.4      68.1   300     8181   12 50 26

12 56 04  J1314+2348   16 52 14  41.8 275.6  3.6      69.3    27     8181   12 56 04
12 58 04  =1312+240    16 54 15  41.4 275.8  3.6      69.2   120     8212   12 56 05

12 58 16  IC860        16 54 27  41.7 276.8  3.6      69.9     3     8212   12 58 16
13 02 16  ---          16 58 27  40.8 277.2  3.7      69.7   240     8274   12 58 17

13 02 28  J1314+2348   16 58 39  40.4 276.3  3.7      69.1     4     8274   13 02 28
13 04 28  =1312+240    17 00 40  40.0 276.5  3.8      69.0   120     8304   13 02 29

13 04 40  IC860        17 00 52  40.3 277.5  3.7      69.7     4     8304   13 04 40
13 08 40  ---          17 04 52  39.4 277.9  3.8      69.5   240     8366   13 04 41

13 08 52  J1314+2348   17 05 04  39.0 277.0  3.8      68.9     4     8366   13 08 52
13 10 52  =1312+240    17 07 05  38.6 277.2  3.9      68.8   120     8397   13 08 53

13 11 04  IC860        17 07 16  38.9 278.1  3.9      69.4     3     8397   13 11 04
13 15 04  ---          17 11 17  38.1 278.6  3.9      69.3   240     8459   13 11 05

13 15 15  J1314+2348   17 11 29  37.7 277.6  3.9      68.6     3     8459   13 15 15
13 17 15  =1312+240    17 13 29  37.2 277.9  4.0      68.6   120     8490   13 15 16

13 17 27  IC860        17 13 41  37.6 278.8  4.0      69.2     3     8490   13 17 27
13 21 27  ---          17 17 41  36.7 279.2  4.0      69.0   240     8552   13 17 28

13 21 38  J1314+2348   17 17 52  36.3 278.3  4.0      68.4     3     8552   13 21 38
13 23 38  =1312+240    17 19 53  35.9 278.5  4.1      68.3   120     8583   13 21 39

13 23 49  IC860        17 20 04  36.2 279.4  4.1      68.9     3     8583   13 23 49
13 27 49  ---          17 24 04  35.4 279.9  4.1      68.7   240     8645   13 23 50

13 28 00  J1314+2348   17 24 15  35.0 279.0  4.1      68.2     2     8645   13 28 00
13 30 00  =1312+240    17 26 16  34.5 279.2  4.2      68.1   120     8675   13 28 01

13 30 11  IC860        17 26 26  34.9 280.1  4.2      68.6     2     8675   13 30 11
13 34 11  ---          17 30 27  34.0 280.5  4.2      68.4   240     8737   13 30 12

13 34 21  J1314+2348   17 30 38  33.6 279.6  4.2      67.9     2     8737   13 34 21
13 36 21  =1312+240    17 32 38  33.2 279.8  4.3      67.8   120     8768   13 34 22
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               6cm global VLBI observations of IC860
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   5 Mar 2019   Day  64 ---

13 36 32  IC860        17 32 48  33.5 280.7  4.3      68.3     2     8768   13 36 32
13 40 32  ---          17 36 49  32.7 281.1  4.3      68.1   240     8830   13 36 33

13 40 42  J1314+2348   17 36 59  32.3 280.3  4.4      67.6     2     8830   13 40 42
13 42 42  =1312+240    17 39 00  31.8 280.5  4.4      67.5   120     8861   13 40 43

13 42 52  IC860        17 39 10  32.2 281.4  4.4      68.0     2     8861   13 42 52
13 46 52  ---          17 43 11  31.3 281.8  4.5      67.8   240     8923   13 42 53

13 47 02  J1314+2348   17 43 21  30.9 281.0  4.5      67.3     2     8923   13 47 02
13 49 02  =1312+240    17 45 21  30.5 281.2  4.5      67.2   120     8954   13 47 03

13 49 12  IC860        17 45 31  30.8 282.0  4.5      67.7     2     8954   13 49 12
13 53 12  ---          17 49 32  30.0 282.4  4.6      67.5   240     9016   13 49 13

 ---------- End of block 18 ----------

13 53 27  J1327+2210   17 49 46  31.5 278.6  4.4      66.7     3     9016   13 53 27
13 59 27  =1324+224    17 55 47  30.2 279.2  4.5      66.4   360     9108   13 53 28


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess119.C2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  22  Setup file default.  Used with PCAL = off
   LO sum=   4740.00  4740.00  4804.00  4804.00  4868.00  4868.00  4932.00  4932.00
   BBC fr=    640.00   640.00   704.00   704.00   768.00   768.00   832.00   832.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  22  23  24  25  26  27  28  29  30  31

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * IC860             13 12 39.491919   * 13 15 03.505200     13 15 58.838854       0.00
                     24 52 58.11061    * 24 37 07.73800      24 30 58.85718        0.00
                     From catalog imbedded in main SCHED input file.
                     Position from EVN project EP055.

   1312+240          13 12 19.391286   * 13 14 43.806206     13 15 39.291242       0.35
 * J1314+2348        24 04 17.61682    * 23 48 26.78172      23 42 17.83530        0.41
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,     56 observations.

   1324+224          13 24 37.118627   * 13 27 00.861311     13 27 56.051955       0.00
 * J1327+2210        22 26 22.70245    * 22 10 50.16289      22 04 48.33664        0.00
   J1327+22          /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  46958 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  IC860      sess119.C2048glob     1 2 8 9 10 11 12 13 14 15 1 +     9.400  1674.500
  J1314+2348 sess119.C2048glob     1 2 8 9 10 11 12 13 14 15 1 +     4.900   880.698
  J1327+2210 sess119.C2048glob     1 2 8 9 10 11 12 13 14 15 1 +     1.617   292.649


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   IC860              143.1
   J1314+2348         143.5
   J1327+2210         141.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

