  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gb079   


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Baczko

Address:  Max Planck Institute for Radio Astronomy
          Auf dem Hugel 69
          D-53121 Bonn
 

Phone:    +79165452842
EMAIL:    abaczko@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 ---------- VLBA+Ef+Hart FF scan in Q/K bands ----------

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

00 59 00  0234+285     21 05 57  19.6  67.3 -5.5     -65.1     0        0   00 59 00
01 10 00  ---          21 16 59  21.8  68.4 -5.4     -66.0   660       85   00 58 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 11 00  0234+285     21 17 59  22.0  68.5 -5.3     -66.1    54       85   01 10 49
01 19 00  ---          21 26 00  23.6  69.3 -5.2     -66.8   480      148   01 10 50

 ---------- K/Q-band VLBI scans. Ground segment 4: 0238-084 with VLBA+Hart+Ef ----------

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 20 00  0238-084     21 27 00   5.4 102.8 -5.2     -57.9    16      148   01 19 49
01 26 00  ---          21 33 01   6.6 103.6 -5.1     -57.7   360      196   01 19 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 27 00  0238-084     21 34 02   6.9 103.8 -5.1     -57.6    54      196   01 26 49
01 30 00  ---          21 37 02   7.5 104.2 -5.1     -57.4   180      221   01 26 50

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 31 00  0238-084     21 38 02   7.7 104.3 -5.1     -57.4    54      221   01 30 49
01 37 00  ---          21 44 03   8.9 105.1 -5.0     -57.1   360      268   01 30 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 38 00  0238-084     21 45 03   9.2 105.3 -4.9     -57.0    54      268   01 37 49
01 41 00  ---          21 48 04   9.8 105.7 -4.9     -56.8   180      293   01 37 50

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 42 00  0238-084     21 49 04  10.0 105.8 -4.9     -56.8    54      293   01 41 49
01 48 00  ---          21 55 05  11.2 106.6 -4.8     -56.4   360      341   01 41 50
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 49 00  0238-084     21 56 05  11.4 106.8 -4.8     -56.3    54      341   01 48 49
01 52 00  ---          21 59 06  12.1 107.2 -4.7     -56.1   180      365   01 48 50

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 53 00  0238-084     22 00 06  12.3 107.3 -4.7     -56.1    54      365   01 52 49
01 59 00  ---          22 06 07  13.5 108.2 -4.6     -55.7   360      413   01 52 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

02 00 00  0238-084     22 07 07  13.7 108.3 -4.6     -55.6    54      413   01 59 49
02 03 00  ---          22 10 07  14.3 108.8 -4.5     -55.4   180      438   01 59 50

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

02 04 00  0238-084     22 11 08  14.5 108.9 -4.5     -55.3    54      438   02 03 49
02 10 00  ---          22 17 09  15.7 109.8 -4.4     -54.9   360      486   02 03 50

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

02 11 00  0238-084     22 18 09  15.9 110.0 -4.4     -54.8    54      486   02 10 49
02 14 00  ---          22 21 09  16.5 110.4 -4.3     -54.6   180      510   02 10 50

 ---------- K-band VLBI scans. Space segment 05: 0238-084 with VLA+VLBA + Hart (till 03:00) ----------

02 15 00  0238-084     22 22 09  16.7 110.5 -4.3     -54.5    54      510   02 14 49
02 23 50  ---          22 31 01  18.5 111.9 -4.2     -53.8   530      580   02 14 50

02 24 00  0238-084     22 31 11  18.6 111.9 -4.2     -53.7     4      580   02 23 56
02 25 00  ---          22 32 11  18.8 112.1 -4.2     -53.7    60      588   02 23 51

02 25 30  0238-084     22 32 41  18.9 112.2 -4.2     -53.6    24      588   02 25 19
02 33 50  ---          22 41 03  20.5 113.5 -4.0     -52.9   500      654   02 25 20

02 34 00  0238-084     22 41 13  20.5 113.5 -4.0     -52.9     4      654   02 33 56
02 35 00  ---          22 42 13  20.7 113.7 -4.0     -52.8    60      662   02 33 51

02 35 30  0238-084     22 42 43  20.8 113.7 -4.0     -52.7    24      662   02 35 19
02 43 50  ---          22 51 04  22.5 115.1 -3.8     -51.9   500      728   02 35 20

02 44 00  0238-084     22 51 14  22.5 115.1 -3.8     -51.9     4      728   02 43 56
02 45 00  ---          22 52 14  22.7 115.3 -3.8     -51.8    60      736   02 43 51
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

02 45 30  0238-084     22 52 44  22.8 115.4 -3.8     -51.8    24      736   02 45 19
02 53 50  ---          23 01 06  24.4 116.8 -3.7     -50.9   500      802   02 45 20

02 54 00  0238-084     23 01 16  24.5 116.8 -3.7     -50.9     4      802   02 53 56
02 55 00  ---          23 02 16  24.6 117.0 -3.7     -50.8    60      810   02 53 51

02 55 30  0238-084     23 02 46  24.7 117.1 -3.7     -50.7    24      810   02 55 19
03 03 50  ---          23 11 07  26.3 118.5 -3.5     -49.8   500      876   02 55 20

03 04 00  0238-084     23 11 17  26.4 118.6 -3.5     -49.8     4      876   03 03 56
03 05 00  ---          23 12 18  26.6 118.7 -3.5     -49.7    60      884   03 03 51

03 07 00  0234+285     23 14 18  45.9  78.8 -3.4     -74.5    74      884   03 06 49
03 10 00  ---          23 17 18  46.6  79.0 -3.4     -74.7   180      909   03 06 50

03 10 10  0234+285     23 17 28  46.6  79.0 -3.4     -74.7     4      909   03 10 06
03 11 10  ---          23 18 29  46.8  79.1 -3.3     -74.8    60      917   03 10 01

03 11 20  0234+285     23 18 39  46.9  79.1 -3.3     -74.8     4      917   03 11 16
03 16 20  ---          23 23 40  47.9  79.5 -3.3     -75.1   300      956   03 11 11

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

03 17 20  0234+285     23 24 40  48.1  79.6 -3.2     -75.1    54      956   03 17 09
03 18 20  ---          23 25 40  48.4  79.7 -3.2     -75.2    60      966   03 17 10

03 18 30  0234+285     23 25 50  48.4  79.7 -3.2     -75.2     4      966   03 18 26
03 28 30  ---          23 35 52  50.5  80.6 -3.1     -75.8   600     1043   03 18 21

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 30 00  0238-084     23 37 22  31.2 123.5 -3.1     -46.5    44     1043   03 29 49
03 33 00  ---          23 40 22  31.7 124.1 -3.0     -46.1   180     1068   03 29 50

03 33 30  0238-084     23 40 52  31.8 124.2 -3.0     -46.0    24     1068   03 33 19
03 34 30  ---          23 41 52  32.0 124.4 -3.0     -45.8    60     1077   03 33 20

03 34 40  0238-084     23 42 03  32.0 124.4 -3.0     -45.8     4     1077   03 34 36
03 37 40  ---          23 45 03  32.5 125.0 -2.9     -45.4   180     1101   03 34 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

03 38 10  0238-084     23 45 33  32.6 125.1 -2.9     -45.3    24     1101   03 37 59
03 39 10  ---          23 46 33  32.8 125.3 -2.9     -45.2    60     1110   03 38 00

03 39 20  0238-084     23 46 43  32.8 125.4 -2.9     -45.1     4     1110   03 39 16
03 45 20  ---          23 52 44  33.9 126.6 -2.8     -44.2   360     1157   03 39 11

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 45 50  0238-084     23 53 14  34.0 126.8 -2.8     -44.1    24     1157   03 45 39
03 46 50  ---          23 54 15  34.1 127.0 -2.8     -44.0    60     1166   03 45 40

03 47 00  0238-084     23 54 25  34.2 127.0 -2.8     -44.0     4     1166   03 46 56
03 50 00  ---          23 57 25  34.7 127.7 -2.7     -43.5   180     1190   03 46 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

03 50 30  0238-084     23 57 55  34.8 127.8 -2.7     -43.4    24     1190   03 50 19
03 51 30  ---          23 58 55  34.9 128.0 -2.7     -43.2    60     1199   03 50 20

03 51 40  0238-084     23 59 05  35.0 128.0 -2.7     -43.2     4     1199   03 51 36
03 57 40  ---          00 05 06  36.0 129.4 -2.6     -42.2   360     1246   03 51 31

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 58 10  0238-084     00 05 36  36.1 129.5 -2.6     -42.1    24     1246   03 57 59
03 59 10  ---          00 06 37  36.2 129.7 -2.6     -42.0    60     1255   03 58 00

03 59 20  0238-084     00 06 47  36.3 129.7 -2.6     -41.9     4     1255   03 59 16
04 02 20  ---          00 09 47  36.7 130.4 -2.5     -41.4   180     1279   03 59 11

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 02 50  0238-084     00 10 17  36.8 130.6 -2.5     -41.3    24     1279   04 02 39
04 03 50  ---          00 11 17  37.0 130.8 -2.5     -41.2    60     1288   04 02 40

04 04 00  0238-084     00 11 27  37.0 130.8 -2.5     -41.1     4     1288   04 03 56
04 10 00  ---          00 17 28  38.0 132.3 -2.4     -40.0   360     1335   04 03 51
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 10 30  0238-084     00 17 58  38.1 132.4 -2.4     -40.0    24     1335   04 10 19
04 11 30  ---          00 18 59  38.2 132.6 -2.4     -39.8    60     1344   04 10 20

04 11 40  0238-084     00 19 09  38.3 132.7 -2.4     -39.7     4     1344   04 11 36
04 14 40  ---          00 22 09  38.7 133.4 -2.3     -39.2   180     1368   04 11 31

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 15 10  0238-084     00 22 39  38.8 133.5 -2.3     -39.1    24     1368   04 14 59
04 16 10  ---          00 23 39  39.0 133.8 -2.3     -38.9    60     1377   04 15 00

04 16 20  0238-084     00 23 49  39.0 133.8 -2.3     -38.9     4     1377   04 16 16
04 22 20  ---          00 29 50  39.9 135.3 -2.2     -37.7   360     1424   04 16 11

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 22 50  0238-084     00 30 20  40.0 135.4 -2.2     -37.6    24     1424   04 22 39
04 23 50  ---          00 31 21  40.1 135.7 -2.2     -37.4    60     1433   04 22 40

04 24 00  0238-084     00 31 31  40.2 135.7 -2.2     -37.3     4     1433   04 23 56
04 27 00  ---          00 34 31  40.6 136.5 -2.1     -36.7   180     1456   04 23 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 27 30  0238-084     00 35 01  40.7 136.7 -2.1     -36.6    24     1456   04 27 19
04 28 30  ---          00 36 01  40.8 136.9 -2.1     -36.4    60     1466   04 27 20

04 28 40  0238-084     00 36 11  40.9 137.0 -2.1     -36.4     4     1466   04 28 36
04 34 40  ---          00 42 12  41.7 138.6 -2.0     -35.1   360     1512   04 28 31

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 35 10  0238-084     00 42 42  41.8 138.7 -2.0     -35.0    24     1512   04 34 59
04 36 10  ---          00 43 43  41.9 139.0 -2.0     -34.8    60     1522   04 35 00

04 36 20  0238-084     00 43 53  42.0 139.0 -2.0     -34.7     4     1522   04 36 16
04 39 20  ---          00 46 53  42.4 139.9 -1.9     -34.1   180     1545   04 36 11
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 39 50  0238-084     00 47 23  42.5 140.0 -1.9     -34.0    24     1545   04 39 39
04 40 50  ---          00 48 23  42.6 140.3 -1.9     -33.7    60     1554   04 39 40

04 41 00  0238-084     00 48 33  42.6 140.3 -1.9     -33.7     4     1554   04 40 56
04 47 00  ---          00 54 34  43.4 142.0 -1.8     -32.3   360     1601   04 40 51

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 47 30  0238-084     00 55 04  43.5 142.2 -1.8     -32.2    24     1601   04 47 19
04 48 30  ---          00 56 05  43.6 142.5 -1.8     -32.0    60     1610   04 47 20

04 48 40  0238-084     00 56 15  43.6 142.5 -1.8     -31.9     4     1610   04 48 36
04 51 40  ---          00 59 15  44.0 143.4 -1.7     -31.2   180     1634   04 48 31

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 52 10  0238-084     00 59 45  44.1 143.5 -1.7     -31.1    24     1634   04 51 59
04 53 10  ---          01 00 45  44.2 143.8 -1.7     -30.9    60     1643   04 52 00

04 53 20  0238-084     01 00 55  44.2 143.9 -1.7     -30.8     4     1643   04 53 16
04 59 20  ---          01 06 56  45.0 145.7 -1.6     -29.3   360     1690   04 53 11

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 59 50  0238-084     01 07 27  45.1 145.8 -1.6     -29.2    24     1690   04 59 39
05 00 50  ---          01 08 27  45.2 146.2 -1.6     -29.0    60     1699   04 59 40

05 01 00  0238-084     01 08 37  45.2 146.2 -1.6     -28.9     4     1699   05 00 56
05 03 50  ---          01 11 27  45.5 147.1 -1.5     -28.2   170     1722   05 00 51

05 04 00  0238-084     01 11 37  45.5 147.1 -1.5     -28.1     4     1722   05 03 56
05 07 00  ---          01 14 38  45.9 148.1 -1.5     -27.4   180     1745   05 03 51

05 07 30  0238-084     01 15 08  46.0 148.2 -1.4     -27.2    24     1745   05 07 19
05 08 30  ---          01 16 08  46.1 148.6 -1.4     -27.0    60     1755   05 07 20

05 08 40  0238-084     01 16 18  46.1 148.6 -1.4     -26.9     4     1755   05 08 36
05 11 40  ---          01 19 18  46.4 149.6 -1.4     -26.1   180     1778   05 08 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

05 12 10  0238-084     01 19 49  46.5 149.7 -1.4     -26.0    24     1778   05 11 59
05 13 10  ---          01 20 49  46.6 150.1 -1.4     -25.7    60     1787   05 12 00

05 13 20  0238-084     01 20 59  46.6 150.1 -1.3     -25.7     4     1787   05 13 16
05 19 20  ---          01 27 00  47.2 152.1 -1.2     -24.0   360     1834   05 13 11

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 19 50  0238-084     01 27 30  47.3 152.3 -1.2     -23.9    24     1834   05 19 39
05 20 50  ---          01 28 30  47.4 152.6 -1.2     -23.6    60     1844   05 19 40

05 21 00  0238-084     01 28 40  47.4 152.7 -1.2     -23.5     4     1844   05 20 56
05 24 00  ---          01 31 40  47.7 153.7 -1.2     -22.7   180     1867   05 20 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

05 24 30  0238-084     01 32 11  47.7 153.8 -1.2     -22.5    24     1867   05 24 19
05 25 30  ---          01 33 11  47.8 154.2 -1.1     -22.3    60     1876   05 24 20

05 25 40  0238-084     01 33 21  47.8 154.2 -1.1     -22.2     4     1876   05 25 36
05 31 40  ---          01 39 22  48.4 156.3 -1.0     -20.4   360     1923   05 25 31

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 32 30  0238-084     01 40 12  48.5 156.6 -1.0     -20.2    44     1923   05 32 19
05 33 30  ---          01 41 12  48.5 157.0 -1.0     -19.9    60     1932   05 32 20

05 33 40  0238-084     01 41 22  48.6 157.0 -1.0     -19.8     4     1932   05 33 36
05 36 40  ---          01 44 23  48.8 158.1 -1.0     -18.9   180     1956   05 33 31

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

05 37 10  0238-084     01 44 53  48.8 158.3 -1.0     -18.8    24     1956   05 36 59
05 38 10  ---          01 45 53  48.9 158.6 -0.9     -18.5    60     1965   05 37 00

05 38 20  0238-084     01 46 03  48.9 158.7 -0.9     -18.4     4     1965   05 38 16
05 44 20  ---          01 52 04  49.4 160.8 -0.8     -16.6   360     2012   05 38 11

05 44 50  0238-084     01 52 34  49.4 161.0 -0.8     -16.4    24     2012   05 44 39
05 45 50  ---          01 53 34  49.5 161.4 -0.8     -16.1    60     2021   05 44 40

05 46 00  0238-084     01 53 44  49.5 161.5 -0.8     -16.1     4     2021   05 45 56
05 53 00  ---          02 00 45  49.9 164.0 -0.7     -13.8   420     2076   05 45 51
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2016   Day 311 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 54 00  0238-084     02 01 45  50.0 164.4 -0.7     -13.5    54     2076   05 53 49
05 58 00  ---          02 05 46  50.2 165.9 -0.6     -12.2   240     2108   05 53 50

05 58 30  0238-084     02 06 16  50.2 166.1 -0.6     -12.0    24     2108   05 58 19
05 59 30  ---          02 07 16  50.3 166.5 -0.6     -11.7    60     2117   05 58 20

 ---------- K-band VLBI scans. Space segment 06: 0238-084 with VLA+VLBA ----------

06 00 00  0238-084     02 07 46  50.3 166.7 -0.6     -11.5    24     2117   05 59 49
06 08 50  ---          02 16 38  50.7 170.1 -0.4      -8.6   530     2187   05 59 50

06 09 00  0238-084     02 16 48  50.7 170.2 -0.4      -8.5     4     2187   06 08 56
06 10 00  ---          02 17 48  50.8 170.5 -0.4      -8.2    60     2195   06 08 51

06 10 30  0238-084     02 18 18  50.8 170.7 -0.4      -8.0    24     2195   06 10 19
06 18 50  ---          02 26 39  51.0 174.0 -0.3      -5.2   500     2261   06 10 20

06 19 00  0238-084     02 26 50  51.0 174.1 -0.3      -5.2     4     2261   06 18 56
06 20 00  ---          02 27 50  51.0 174.4 -0.2      -4.8    60     2269   06 18 51

06 20 30  0238-084     02 28 20  51.0 174.6 -0.2      -4.7    24     2269   06 20 19
06 28 50  ---          02 36 41  51.2 177.9 -0.1      -1.8   500     2335   06 20 20

06 29 00  0238-084     02 36 51  51.2 178.0 -0.1      -1.7     4     2335   06 28 56
06 30 00  ---          02 37 51  51.2 178.4 -0.1      -1.4    60     2343   06 28 51

06 30 30  0238-084     02 38 21  51.2 178.6 -0.1      -1.2    24     2343   06 30 19
06 38 50  ---          02 46 43  51.2 181.9  0.1       1.6   500     2409   06 30 20

06 39 00  0238-084     02 46 53  51.2 182.0  0.1       1.7     4     2409   06 38 56
06 40 00  ---          02 47 53  51.2 182.4  0.1       2.0    60     2418   06 38 51

06 40 30  0238-084     02 48 23  51.1 182.5  0.1       2.2    24     2418   06 40 19
06 48 50  ---          02 56 44  51.0 185.8  0.2       5.1   500     2483   06 40 20

06 49 00  0238-084     02 56 54  51.0 185.9  0.2       5.1     4     2483   06 48 56
06 50 00  ---          02 57 55  51.0 186.3  0.3       5.5    60     2492   06 48 51

06 50 30  0238-084     02 58 25  51.0 186.5  0.3       5.6    24     2492   06 50 19
06 58 50  ---          03 06 46  50.7 189.7  0.4       8.5   500     2557   06 50 20

06 59 00  0238-084     03 06 56  50.7 189.8  0.4       8.5     4     2557   06 58 56
07 00 00  ---          03 07 56  50.7 190.2  0.4       8.8    60     2566   06 58 51


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra7mm2.set
   Matching groups in ./gb079_freq.dat:
     v7mm_c8

   Setup group:   41         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  28  Setup file default.  Used with PCAL = off
   LO sum=   43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
   BBC fr=     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.00    754.00    786.00    786.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  28  29  30  31  32  33  34  45  46  48

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra1cm2.set
   Matching groups in ./gb079_freq.dat:
     v1cm_b3

   Setup group:    6         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  25  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
   BBC fr=     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     759.99    759.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  25  26  35  36  37  38  39  42  43  47

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 34.104620       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 11.67342        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 1934-638          04 20 04.230487   * 19 39 25.024972     04 20 47.695161       0.00
                    -63 49 48.04871    *-63 42 45.62440     -63 40 24.82043        0.00
                     From catalog imbedded in main SCHED input file.
                     ATCA flux calibrator

 * 0134+329          01 34 49.826373   * 01 37 41.299439     01 38 40.499141       0.00
   J0137+3309        32 54 20.25866    * 33 09 35.13284      33 14 44.81588        0.00
   3C48              ./gb079_sources.radioastron
                     rfc_2016c Petrov and Kovalev, in preparation  147 observations

 * 2251+158          22 51 29.519741   * 22 53 57.747940     22 54 48.031641       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 14 27.51855        0.00
   3C454.3           ./gb079_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO4-06, RA-AO3-0

 * 0234+285          02 34 55.589591   * 02 37 52.405678     02 38 53.303332       0.00
   J0237+2848        28 35 11.40774    * 28 48 08.98999      28 52 27.53754        0.00
                     ./gb079_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 57147 observations, RA-AO4-07, RA-AO3-0

 * 0238-084          02 38 37.351926   * 02 41 04.798502     02 41 55.301775       0.00
   J0241-0815       -08 28 08.92072    *-08 15 20.75192     -08 11 06.03352        0.00
   NGC1052           ./gb079_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, RA-AO4-09

 * 0528+134          05 28 06.759218   * 05 30 56.416749     05 31 54.185533       0.00
   J0530+1331        13 29 42.28878    * 13 31 55.14945      13 32 31.09082        0.00
                     ./gb079_sources.radioastron
                     AGN, MASIV, rfc_2013d Petrov, 2013, unpublished 139206 observations, RA-AO3-04,



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            9                                 5.275     0.000
  1934-638   ra1cm2.set            10                                0.111     0.000
  0134+329   ra1cm2.set            40                                0.100     0.000
             ra7mm2.set            44                                0.133     0.000
  2251+158   ra1cm2.set            1 2 3 4 5 6                       0.117     3.169
  0234+285   ra1cm2.set            5 6 11 12 15 16 17 18 19 21 +     0.950    60.179
             ra7mm2.set            27 28 44                          0.367    13.383
  0238-084   ra1cm2.set            1 2 3 4 5 6 10 11 12 13 15  +    14.964   911.905
             ra7mm2.set            27 28 44                          1.800    76.197
  0528+134   ra1cm2.set            1 2 3 4 10                        0.133     1.276


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             102.2
   1934-638            98.2
   0134+329           157.1
   2251+158           124.7
   0234+285           167.0
   0238-084           155.8
   0528+134           139.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

