  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg079b  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez, Andrei Lobanov

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: L-band, dual-pol

Notes:    L-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

 ---------- VLBA OBSERVING CALIBRATORS: 0235+164 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

17 00 00  0235+164     23 45 18  48.0  99.2 -2.9     -62.5     0        0   17 00 00
17 04 00  ---          23 49 18  48.9  99.9 -2.8     -62.2   240       15   17 00 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

17 04 10  0235+164     23 49 28  48.9  99.9 -2.8     -62.2     4       15   17 04 10
17 10 10  ---          23 55 29  50.2 100.9 -2.7     -61.9   360       39   17 04 11

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

17 10 20  0235+164     23 55 39  50.2 101.0 -2.7     -61.9     4       39   17 10 20
17 15 20  ---          00 00 40  51.3 101.9 -2.6     -61.5   300       58   17 10 21

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

17 15 30  0235+164     00 00 50  51.3 101.9 -2.6     -61.5     4       58   17 15 30
17 20 30  ---          00 05 51  52.4 102.8 -2.6     -61.1   300       77   17 15 31

 ---------- VLBA OBSERVING CALIBRATORS: 3C84 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

17 21 30  3C84         00 06 51  49.9  60.4 -3.2     -89.7    22       77   17 21 30
17 25 30  ---          00 10 52  50.6  60.4 -3.2     -90.4   240       93   17 21 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

17 25 40  3C84         00 11 02  50.7  60.4 -3.2     -90.4     4       93   17 25 40
17 31 40  ---          00 17 03  51.8  60.4 -3.1     -91.5   360      116   17 25 41

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

17 31 50  3C84         00 17 13  51.8  60.4 -3.1     -91.5     4      116   17 31 50
17 36 50  ---          00 22 14  52.8  60.3 -3.0     -92.4   300      135   17 31 51
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

17 37 00  3C84         00 22 24  52.8  60.3 -3.0     -92.4     4      135   17 37 00
17 42 00  ---          00 27 24  53.7  60.2 -2.9     -93.3   300      155   17 37 01

 ---------- VLBA OBSERVING CALIBRATORS: 0235+164 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

17 42 10  0235+164     00 27 34  56.9 107.3 -2.2     -59.0   -31      155   17 42 41
17 46 10  ---          00 31 35  57.7 108.2 -2.1     -58.6   209      168   17 42 11

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

17 46 20  0235+164     00 31 45  57.7 108.3 -2.1     -58.5     4      168   17 46 20
17 52 20  ---          00 37 46  59.0 109.7 -2.0     -57.7   360      191   17 46 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

17 52 30  0235+164     00 37 56  59.0 109.7 -2.0     -57.7     4      191   17 52 30
17 57 30  ---          00 42 57  60.0 111.0 -1.9     -57.0   300      211   17 52 31

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

17 57 40  0235+164     00 43 07  60.0 111.1 -1.9     -56.9     4      211   17 57 40
18 02 40  ---          00 48 08  61.0 112.4 -1.9     -56.1   300      230   17 57 41

 ---------- VLBA OBSERVING CALIBRATORS: 3C84 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

18 03 40  3C84         00 49 08  57.8  59.6 -2.5     -97.4    15      230   18 03 40
18 07 40  ---          00 53 09  58.5  59.4 -2.5     -98.3   240      245   18 03 41

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

18 07 50  3C84         00 53 19  58.5  59.4 -2.5     -98.3     4      245   18 07 50
18 13 50  ---          00 59 20  59.6  59.0 -2.4     -99.6   360      269   18 07 51
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

18 14 00  3C84         00 59 30  59.7  59.0 -2.4     -99.6     4      269   18 14 00
18 19 00  ---          01 04 30  60.6  58.7 -2.3    -100.8   300      288   18 14 01

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

18 19 10  3C84         01 04 41  60.6  58.7 -2.3    -100.8     4      288   18 19 10
18 24 10  ---          01 09 41  61.6  58.3 -2.2    -102.0   300      307   18 19 11

 ---------- VLBA OBSERVING CALIBRATORS: 0235+164 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

18 24 20  0235+164     01 09 51  65.3 119.2 -1.5     -51.6   -41      307   18 25 01
18 28 20  ---          01 13 52  66.0 120.7 -1.4     -50.6   199      320   18 24 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

18 28 30  0235+164     01 14 02  66.0 120.7 -1.4     -50.5     4      320   18 28 30
18 34 30  ---          01 20 03  67.1 123.1 -1.3     -48.8   360      343   18 28 31

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

18 34 40  0235+164     01 20 13  67.2 123.1 -1.3     -48.8     4      343   18 34 40
18 39 40  ---          01 25 14  68.1 125.3 -1.2     -47.2   300      362   18 34 41

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

18 39 50  0235+164     01 25 24  68.1 125.3 -1.2     -47.1     4      362   18 39 50
18 44 50  ---          01 30 25  69.0 127.6 -1.2     -45.4   300      382   18 39 51

 ---------- VLBA OBSERVING CALIBRATORS: 3C84 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

18 45 50  3C84         01 31 25  65.5  56.0 -1.8    -107.6     1      382   18 45 50
18 49 50  ---          01 35 26  66.2  55.4 -1.8    -108.8   240      397   18 45 51
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

18 50 00  3C84         01 35 36  66.2  55.4 -1.8    -108.9     4      397   18 50 00
18 56 00  ---          01 41 37  67.3  54.4 -1.7    -110.8   360      420   18 50 01

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

18 56 10  3C84         01 41 47  67.3  54.4 -1.7    -110.8     4      420   18 56 10
19 01 10  ---          01 46 47  68.2  53.4 -1.6    -112.5   300      440   18 56 11

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

19 01 20  3C84         01 46 57  68.2  53.4 -1.6    -112.6     4      440   19 01 20
19 06 20  ---          01 51 58  69.1  52.4 -1.5    -114.3   300      459   19 01 21

 ---------- VLBA OBSERVING CALIBRATORS: NRAO150 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

19 07 20  NRAO150      01 52 58  58.8  40.0 -2.1    -118.5    32      459   19 07 20
19 11 20  ---          01 56 59  59.4  39.4 -2.1    -119.8   240      475   19 07 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

19 11 30  NRAO150      01 57 09  59.4  39.4 -2.1    -119.8     4      475   19 11 30
19 17 30  ---          02 03 10  60.2  38.4 -2.0    -121.8   360      498   19 11 31

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

19 17 40  NRAO150      02 03 20  60.2  38.4 -2.0    -121.9     4      498   19 17 40
19 22 40  ---          02 08 21  60.9  37.5 -1.9    -123.6   300      517   19 17 41

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

19 22 50  NRAO150      02 08 31  60.9  37.5 -1.9    -123.7     4      517   19 22 50
19 27 50  ---          02 13 32  61.6  36.6 -1.8    -125.5   300      536   19 22 51
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

 ---------- VLBA OBSERVING CALIBRATORS: 0235+164 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

19 28 50  0235+164     02 14 32  74.9 156.4 -0.4     -21.1   -33      536   19 29 23
19 32 50  ---          02 18 33  75.2 159.9 -0.3     -18.0   207      550   19 28 51

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

19 33 00  0235+164     02 18 43  75.3 160.0 -0.3     -17.9     4      550   19 33 00
19 39 00  ---          02 24 44  75.6 165.6 -0.2     -12.9   360      573   19 33 01

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

19 39 10  0235+164     02 24 54  75.7 165.7 -0.2     -12.8     4      573   19 39 10
19 44 10  ---          02 29 54  75.9 170.5 -0.2      -8.5   300      592   19 39 11

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

19 44 20  0235+164     02 30 05  75.9 170.7 -0.2      -8.4     4      592   19 44 20
19 49 20  ---          02 35 05  76.0 175.6 -0.1      -4.0   300      612   19 44 21

 ---------- VLBA OBSERVING CALIBRATORS: 3C84 ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

19 50 20  3C84         02 36 05  75.8  36.4 -0.7    -137.0   -47      612   19 51 07
19 54 20  ---          02 40 06  76.3  34.1 -0.7    -139.9   193      624   19 50 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

19 54 40  0851+202     02 40 26   6.9  70.8 -6.3     -59.9  -124      624   19 56 44
20 04 10  ---          02 49 58   8.9  71.9 -6.1     -60.5   446      653   19 54 41

20 04 40  0851+202     02 50 28   9.0  72.0 -6.1     -60.6    24      653   20 04 40
20 14 10  ---          02 59 59  10.9  73.1 -5.9     -61.2   570      689   20 04 41

 ---------- L-band VLBI scans. Space segment 02 ----------

20 20 00  0851+202     03 05 50  12.1  73.7 -5.8     -61.6   344      689   20 20 00
20 36 20  ---          03 22 13  15.5  75.6 -5.6     -62.5   980      753   20 20 01

20 36 50  0851+202     03 22 43  15.6  75.6 -5.6     -62.5    24      753   20 36 50
20 53 10  ---          03 39 06  19.1  77.5 -5.3     -63.4   980      816   20 36 51
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

20 53 40  0851+202     03 39 36  19.2  77.5 -5.3     -63.4    24      816   20 53 40
21 10 00  ---          03 55 59  22.6  79.4 -5.0     -64.2   980      879   20 53 41

 ---------- VLBA-only scans on 0716+714 at X,L,U,C ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

21 11 30  0716+714     03 57 29  40.9  19.4 -3.4    -117.0    39      879   21 11 30
21 15 30  ---          04 01 29  41.1  19.2 -3.4    -118.1   240      894   21 11 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

21 15 40  0716+714     04 01 40  41.1  19.2 -3.4    -118.1     4      894   21 15 40
21 21 40  ---          04 07 41  41.6  18.9 -3.3    -119.8   360      917   21 15 41

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

21 21 50  0716+714     04 07 51  41.6  18.8 -3.3    -119.8     4      917   21 21 50
21 26 50  ---          04 12 51  41.9  18.6 -3.2    -121.2   300      937   21 21 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

21 27 00  0716+714     04 13 01  41.9  18.6 -3.2    -121.2     4      937   21 27 00
21 37 00  ---          04 23 03  42.6  18.0 -3.0    -124.0   600      975   21 27 01

 ---------- Back to the target source ----------

21 42 00  0851+202     04 28 04  29.4  82.9 -4.5     -65.4   246      975   21 42 00
21 51 30  ---          04 37 35  31.5  84.0 -4.3     -65.6   570     1012   21 42 01

21 52 00  0851+202     04 38 05  31.6  84.1 -4.3     -65.6    24     1012   21 52 00
22 01 30  ---          04 47 37  33.6  85.1 -4.1     -65.9   570     1049   21 52 01

22 02 00  0851+202     04 48 07  33.7  85.2 -4.1     -65.9    24     1049   22 02 00
22 11 30  ---          04 57 39  35.8  86.3 -4.0     -66.1   570     1086   22 02 01

22 12 00  0851+202     04 58 09  35.9  86.4 -4.0     -66.1    24     1086   22 12 00
22 21 30  ---          05 07 40  37.9  87.5 -3.8     -66.2   570     1122   22 12 01

22 22 00  0851+202     05 08 10  38.0  87.6 -3.8     -66.2    24     1122   22 22 00
22 31 30  ---          05 17 42  40.1  88.7 -3.6     -66.3   570     1159   22 22 01

22 32 00  0851+202     05 18 12  40.2  88.8 -3.6     -66.3    24     1159   22 32 00
22 41 30  ---          05 27 44  42.2  90.0 -3.5     -66.3   570     1196   22 32 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  16 Apr 2016   Day 107 ---

22 42 00  0851+202     05 28 14  42.3  90.0 -3.5     -66.3    24     1196   22 42 00
22 51 30  ---          05 37 45  44.4  91.3 -3.3     -66.3   570     1232   22 42 01

22 52 00  0851+202     05 38 15  44.5  91.3 -3.3     -66.3    24     1232   22 52 00
23 01 30  ---          05 47 47  46.6  92.6 -3.1     -66.2   570     1269   22 52 01

23 02 00  0851+202     05 48 17  46.7  92.7 -3.1     -66.2    24     1269   23 02 00
23 10 00  ---          05 56 18  48.4  93.8 -3.0     -66.0   480     1300   23 02 01

23 10 30  0851+202     05 56 48  48.5  93.9 -3.0     -66.0    24     1300   23 10 30
23 18 30  ---          06 04 50  50.2  95.1 -2.8     -65.8   480     1331   23 10 31

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

23 19 00  0851+202     06 05 20  50.3  95.2 -2.8     -65.8    24     1331   23 19 00
23 23 00  ---          06 09 20  51.2  95.8 -2.8     -65.7   240     1346   23 19 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

23 23 10  0851+202     06 09 30  51.2  95.8 -2.8     -65.7     4     1346   23 23 10
23 29 10  ---          06 15 31  52.5  96.7 -2.7     -65.4   360     1370   23 23 11

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

23 29 20  0851+202     06 15 41  52.5  96.8 -2.7     -65.4     4     1370   23 29 20
23 34 20  ---          06 20 42  53.6  97.6 -2.6     -65.2   300     1389   23 29 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

23 34 30  0851+202     06 20 52  53.6  97.6 -2.6     -65.2     4     1389   23 34 30
23 39 30  ---          06 25 53  54.7  98.5 -2.5     -64.9   300     1408   23 34 31

 ---------- L-band VLBI scans. Space segment 03 ----------

23 40 00  0851+202     06 26 23  54.8  98.6 -2.5     -64.9    24     1408   23 40 00
23 56 20  ---          06 42 46  58.3 101.6 -2.2     -63.8   980     1471   23 40 01

 --- Start: Sat  16 Apr 2016   Day 107 -- Stop: Sun  17 Apr 2016   Day 108 ---

23 56 50  0851+202     06 43 16  58.4 101.7 -2.2     -63.8    24     1471   23 56 50
00 13 10  ---          06 59 39  61.8 105.2 -1.9     -62.1   980     1534   23 56 51
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

00 13 40  0851+202     07 00 09  61.9 105.3 -1.9     -62.1    24     1534   00 13 40
00 30 00  ---          07 16 31  65.3 109.5 -1.7     -59.7   980     1598   00 13 41

 ---------- VLBA-only scans on 0716+714 at X,L,U,C ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

00 34 00  0716+714     07 20 32  49.3   0.4 -0.1    -179.0   155     1598   00 34 00
00 38 00  ---          07 24 33  49.3  -0.1  0.0     179.7   240     1613   00 34 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

00 38 10  0716+714     07 24 43  49.3  -0.1  0.0     179.7     4     1613   00 38 10
00 44 10  ---          07 30 44  49.3  -0.9  0.1     177.7   360     1636   00 38 11

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

00 44 20  0716+714     07 30 54  49.3  -0.9  0.1     177.6     4     1636   00 44 20
00 49 20  ---          07 35 55  49.3  -1.5  0.2     176.0   300     1656   00 44 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

00 49 30  0716+714     07 36 05  49.3  -1.5  0.2     175.9     4     1656   00 49 30
00 54 30  ---          07 41 05  49.3  -2.1  0.3     174.3   300     1675   00 49 31

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

00 54 40  0851+202     07 41 15  70.2 117.9 -1.2     -54.1   -84     1675   00 56 04
00 58 40  ---          07 45 16  70.9 119.6 -1.2     -52.8   156     1685   00 54 41

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

00 58 50  0851+202     07 45 26  70.9 119.6 -1.2     -52.8     4     1685   00 58 50
01 04 50  ---          07 51 27  72.1 122.4 -1.1     -50.7   360     1708   00 58 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

01 05 00  0851+202     07 51 37  72.1 122.5 -1.1     -50.6     4     1708   01 05 00
01 10 00  ---          07 56 38  73.0 125.0 -1.0     -48.6   300     1727   01 05 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

01 10 10  0851+202     07 56 48  73.0 125.1 -1.0     -48.5     4     1727   01 10 10
01 15 10  ---          08 01 49  73.9 127.9 -0.9     -46.3   300     1747   01 10 11

 ---------- GBT+VLBA only L-band scans: 0851+202 ----------

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

01 15 40  0851+202     08 02 19  74.0 128.2 -0.9     -46.0    24     1747   01 15 40
01 25 10  ---          08 11 51  75.5 134.4 -0.7     -40.9   570     1784   01 15 41

01 25 40  0851+202     08 12 21  75.6 134.7 -0.7     -40.6    24     1784   01 25 40
01 35 10  ---          08 21 52  76.9 142.2 -0.6     -34.1   570     1820   01 25 41

01 35 40  0851+202     08 22 22  77.0 142.7 -0.6     -33.7    24     1820   01 35 40
01 45 10  ---          08 31 54  78.1 151.7 -0.4     -25.7   570     1857   01 35 41

01 45 40  0851+202     08 32 24  78.2 152.2 -0.4     -25.3    24     1857   01 45 40
01 55 10  ---          08 41 55  79.0 162.8 -0.2     -15.7   570     1894   01 45 41

01 55 40  0851+202     08 42 26  79.0 163.4 -0.2     -15.2    24     1894   01 55 40
02 03 10  ---          08 49 57  79.3 172.6 -0.1      -6.8   450     1923   01 55 41

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

02 03 30  0851+202     08 50 17  79.3 173.0 -0.1      -6.4    14     1923   02 03 30
02 07 30  ---          08 54 17  79.4 178.1 -0.0      -1.7   240     1938   02 03 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

02 07 40  0851+202     08 54 27  79.4 178.4 -0.0      -1.5     4     1938   02 07 40
02 13 40  ---          09 00 28  79.4 186.0  0.1       5.5   360     1961   02 07 41

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

02 13 50  0851+202     09 00 38  79.4 186.2  0.1       5.7     4     1961   02 13 50
02 18 50  ---          09 05 39  79.2 192.5  0.2      11.4   300     1981   02 13 51
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

02 19 00  0851+202     09 05 49  79.2 192.7  0.2      11.6     4     1981   02 19 00
02 24 00  ---          09 10 50  78.9 198.7  0.3      17.1   300     2000   02 19 01

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

02 24 10  0851+202     09 11 00  78.9 198.9  0.3      17.2     4     2000   02 24 10
02 29 10  ---          09 16 01  78.5 204.5  0.3      22.3   300     2019   02 24 11

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

02 29 20  0851+202     09 16 11  78.5 204.7  0.3      22.5     4     2019   02 29 20
02 34 20  ---          09 21 12  78.0 209.9  0.4      27.2   300     2039   02 29 21

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

02 34 30  0851+202     09 21 22  77.9 210.1  0.4      27.3     4     2039   02 34 30
02 40 30  ---          09 27 23  77.2 215.8  0.5      32.4   360     2062   02 34 31

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

02 40 40  0851+202     09 27 33  77.2 215.9  0.5      32.5     4     2062   02 40 40
02 44 40  ---          09 31 34  76.7 219.4  0.6      35.6   240     2077   02 40 41

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

02 44 50  0851+202     09 31 44  76.7 219.5  0.6      35.7     4     2077   02 44 50
02 49 50  ---          09 36 44  75.9 223.5  0.7      39.1   300     2097   02 44 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

02 50 00  0851+202     09 36 54  75.9 223.6  0.7      39.2     4     2097   02 50 00
02 59 20  ---          09 46 16  74.5 230.0  0.8      44.6   560     2133   02 50 01

 ---------- L-band VLBI scans. Space segment 04 ----------

03 00 00  0851+202     09 46 56  74.3 230.4  0.9      44.9    34     2133   03 00 00
03 16 20  ---          10 03 19  71.5 239.1  1.1      51.8   980     2196   03 00 01

03 16 50  0851+202     10 03 49  71.4 239.4  1.1      52.0    24     2196   03 16 50
03 33 10  ---          10 20 12  68.2 245.9  1.4      56.7   980     2259   03 16 51

03 33 40  0851+202     10 20 42  68.1 246.0  1.4      56.8    24     2259   03 33 40
03 50 00  ---          10 37 04  64.9 251.1  1.7      60.0   980     2322   03 33 41
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

 ---------- Ground-only segment 04, VLBA+GBT L-band scans: 0851+202 ----------

03 51 00  0851+202     10 38 04  64.7 251.4  1.7      60.2    54     2322   03 51 00
03 53 00  ---          10 40 05  64.2 251.9  1.7      60.5   120     2330   03 51 01

03 53 30  0851+202     10 40 35  64.1 252.0  1.7      60.6    24     2330   03 53 30
04 03 00  ---          10 50 06  62.2 254.4  1.9      61.9   570     2366   03 53 31

04 03 30  0851+202     10 50 37  62.1 254.5  1.9      62.0    24     2366   04 03 30
04 13 00  ---          11 00 08  60.1 256.7  2.1      63.0   570     2403   04 03 31

04 13 30  0851+202     11 00 38  60.0 256.8  2.1      63.1    24     2403   04 13 30
04 22 30  ---          11 09 40  58.1 258.6  2.2      63.9   540     2438   04 13 31

 ---------- VLBA-only fringe finder 0716+714 at X,L,U,C ----------

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

04 24 30  0716+714     11 11 40  39.3 339.7  3.8     111.3    54     2438   04 24 30
04 29 30  ---          11 16 41  38.9 339.5  3.9     110.0   300     2457   04 24 31

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

04 29 40  0716+714     11 16 51  38.9 339.5  3.9     109.9     4     2457   04 29 40
04 34 40  ---          11 21 52  38.5 339.3  4.0     108.6   300     2477   04 29 41

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

04 34 50  0716+714     11 22 02  38.5 339.3  4.0     108.6     4     2477   04 34 50
04 40 50  ---          11 28 03  38.0 339.1  4.1     107.0   360     2500   04 34 51

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

04 41 00  0716+714     11 28 13  38.0 339.1  4.1     107.0     4     2500   04 41 00
04 45 00  ---          11 32 13  37.7 339.0  4.1     106.0   240     2515   04 41 01

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

04 45 10  0851+202     11 32 23  53.3 262.7  2.6      65.3   -52     2515   04 46 02
04 49 10  ---          11 36 24  52.4 263.3  2.7      65.5   188     2527   04 45 11
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

04 49 20  0851+202     11 36 34  52.4 263.4  2.7      65.5     4     2527   04 49 20
04 55 20  ---          11 42 35  51.1 264.3  2.8      65.7   360     2550   04 49 21

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

04 55 30  0851+202     11 42 45  51.0 264.3  2.8      65.7     4     2550   04 55 30
05 00 30  ---          11 47 46  50.0 265.1  2.9      65.9   300     2570   04 55 31

 Next scan frequencies:  8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
 Next BBC frequencies:    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00

05 00 40  0851+202     11 47 56  49.9 265.1  2.9      65.9     4     2570   05 00 40
05 05 40  ---          11 52 57  48.9 265.8  3.0      66.0   300     2589   05 00 41

 ---------- VLBA-only scans on OJ287 at X,L,U,C ----------

05 05 50  0851+202     11 53 07  48.8 265.9  3.0      66.0     4     2589   05 05 50
05 10 50  ---          11 58 08  47.8 266.6  3.0      66.1   300     2608   05 05 51

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

05 11 00  0851+202     11 58 18  47.7 266.6  3.0      66.1     4     2608   05 11 00
05 16 00  ---          12 03 18  46.6 267.3  3.1      66.2   300     2628   05 11 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00

05 16 10  0851+202     12 03 28  46.6 267.3  3.1      66.2     4     2628   05 16 10
05 22 10  ---          12 09 29  45.3 268.2  3.2      66.3   360     2651   05 16 11

 Next scan frequencies:  4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00

05 22 20  0851+202     12 09 39  45.3 268.2  3.2      66.3     4     2651   05 22 20
05 26 20  ---          12 13 40  44.4 268.7  3.3      66.3   240     2666   05 22 21

 ---------- VLBA-only scans on OJ287 at L ----------

 Next scan frequencies:  1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00

05 26 50  0851+202     12 14 10  44.3 268.8  3.3      66.3    24     2666   05 26 50
05 37 20  ---          12 24 42  42.0 270.1  3.5      66.3   630     2707   05 26 51
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  17 Apr 2016   Day 108 ---

 ---------- VLBA-only scans on OJ287 at L ----------

05 37 50  0851+202     12 25 12  41.9 270.2  3.5      66.3    24     2707   05 37 50
05 48 20  ---          12 35 44  39.7 271.5  3.7      66.3   630     2748   05 37 51

 ---------- VLBA-only scans on OJ287 at L ----------

05 48 50  0851+202     12 36 14  39.6 271.6  3.7      66.3    24     2748   05 48 50
05 59 20  ---          12 46 46  37.3 272.8  3.9      66.2   630     2788   05 48 51

05 59 50  0851+202     12 47 16  37.2 272.9  3.9      66.2    24     2788   05 59 50
06 09 50  ---          12 57 17  35.0 274.1  4.0      66.0   600     2827   05 59 51

 ---------- L-band VLBI scans. Space segment 05 ----------

06 10 00  0851+202     12 57 27  35.0 274.1  4.0      66.0     4     2827   06 10 00
06 26 20  ---          13 13 50  31.5 276.0  4.3      65.6   980     2890   06 10 01

06 26 50  0851+202     13 14 20  31.4 276.0  4.3      65.6    24     2890   06 26 50
06 43 10  ---          13 30 43  27.9 277.9  4.6      65.1   980     2953   06 26 51

06 43 40  0851+202     13 31 13  27.8 277.9  4.6      65.1    24     2953   06 43 40
07 00 00  ---          13 47 36  24.3 279.8  4.9      64.5   980     3016   06 43 41


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra6cm2.set
   Matching groups in ./gg079b_freq.dat:
     vc_d

   Setup group:   32         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = 1MHz
   LO sum=   4804.00  4804.00  4804.00  4868.00  4836.00  4836.00  4836.00  4836.00
   BBC fr=    704.00   704.00   704.00   768.00   736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     703.99    767.99    736.01    736.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20  48  51

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg079b_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   52         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  21  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15337.00  15401.00  15369.00  15369.00  15369.00  15369.00
   BBC fr=     737.00    737.00    737.00    801.00    769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     736.99    800.99    769.01    769.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  21  22  23  24  25  26  27  28  29  52

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra18cm2.set
   Matching groups in ./gg079b_freq.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:    7         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         L         L         U         U         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  11  Setup file default.  Used with PCAL = 1MHz
   LO sum=   1636.00  1636.00  1636.00  1636.00  1668.00  1668.00  1668.00  1668.00
   BBC fr=    764.00   764.00   764.00   764.00   732.00   732.00   732.00   732.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     764.01    764.01    731.99    731.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  11  30  31  32  33  34  35  36  37  38

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra4cm2.set
   Matching groups in ./gg079b_freq.dat:
     v4cm_3

   Setup group:   42         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  39  Setup file default.  Used with PCAL = 1MHz
   LO sum=   8393.00  8393.00  8393.00  8457.00  8425.00  8425.00  8425.00  8425.00
   BBC fr=    793.00   793.00   793.00   857.00   825.00   825.00   825.00   825.00
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     792.99    856.99    825.01    825.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  39  40  41  42  43  44  45  46  47  53

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 55.484092       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 43.33930        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0235+164          02 35 52.630215   * 02 38 38.930107     02 39 31.772115       0.00
   J0238+1636        16 24 04.01610    * 16 36 59.27452      16 40 57.53786        0.00
                     ./gg079b_sources.radioastron
                     AGN, IDV, rfc_2013d Petrov, 2013, unpublished 65224 observations, RA-AO3-04, RA-

   0316+413          03 16 29.567283   * 03 19 48.160114     03 20 51.499663       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 03.15833        0.00
 * 3C84              ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

   0355+508          03 55 45.261370   * 03 59 29.747271     04 00 41.417188       0.00
   J0359+5057        50 49 20.28584    * 50 57 50.16179      51 00 28.15118        0.00
 * NRAO150           ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 19270 observations, RA-AO3-04, RA-AO2-1

 * 0716+714          07 16 13.029739   * 07 21 53.448474     07 23 42.151649       0.00
   J0721+7120        71 26 15.17406    * 71 20 36.36340      71 18 48.85325        0.00
                     ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 42370 observations, RA-AO3-04, RA-AO2-1

 * 0851+202          08 51 57.250618   * 08 54 48.874930     08 55 44.665021       0.00
   J0854+2006        20 17 58.41733    * 20 06 30.64078      20 02 38.75769        0.00
   OJ287             ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 213710 observations, RA-AO3-04, RA-AO3-

 * 1633+382          16 33 30.625100   * 16 35 15.492975     16 35 50.554035       0.00
   J1635+3808        38 14 10.08266    * 38 08 04.50043      38 06 02.23933        0.00
   4C38.41           ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 16451 observations, RA-AO3-04, RA-AO3-0

   1641+399          16 41 17.606226   * 16 42 58.809963     16 43 32.680895       0.00
   J1642+3948        39 54 10.81479    * 39 48 36.99385      39 46 44.64413        0.00
 * 3C345             ./gg079b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 51938 observations, RA-AO3-04, RA-AO3-0



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra18cm2.set           12                                4.083     0.000
  0235+164   ra18cm2.set           11                                0.333     9.500
             ra6cm2.set            13                                0.267     6.290
             ra4cm2.set            39                                0.333     9.500
             ra2cm2.set            21                                0.400    10.600
  3C84       ra18cm2.set           11                                0.333     8.250
             ra6cm2.set            13                                0.267     7.273
             ra4cm2.set            39                                0.333     8.250
             ra2cm2.set            21                                0.400     9.900
  NRAO150    ra18cm2.set           11                                0.083     1.750
             ra6cm2.set            13                                0.133     1.800
             ra4cm2.set            39                                0.083     1.750
             ra2cm2.set            21                                0.100     2.100
  0716+714   ra18cm2.set           1 2 3 4 5 6 7 8 9 11 49 50  +     1.275    39.046
             ra6cm2.set            13                                0.200     9.000
             ra4cm2.set            39                                0.250    11.250
             ra2cm2.set            21                                0.300    13.500
  0851+202   ra18cm2.set           1 2 3 4 5 6 7 8 9 10 11 49  +    12.422   868.507
             ra6cm2.set            13                                0.400    15.974
             ra4cm2.set            39                                0.500    22.500
             ra2cm2.set            21                                0.683    30.750
  1633+382   ra18cm2.set           1 2 3 4 5 6 7 8 9 10 49 50        2.603    98.563
  3C345      ra18cm2.set           1 2 3 4 5 6 7 8 9 10 49 50        3.056   116.782


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              84.1
   0235+164            15.3
   3C84                37.9
   NRAO150             49.4
   0716+714            78.6
   0851+202           103.3
   1633+382           116.6
   3C345              114.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

