  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg079c  


Schedule Version:       1.10
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez, Andrei Lobanov

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 ---------- VLBA on calibrators at the beginning of experiment ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00

16 00 00  2351+456     23 20 37  73.3  21.2 -0.6    -153.3     0        0   16 00 00
16 05 00  ---          23 25 37  73.6  18.5 -0.5    -156.9   300       19   16 00 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

16 05 30  2351+456     23 26 08  73.7  18.2 -0.5    -157.3    24       19   16 05 30
16 10 30  ---          23 31 08  74.0  15.3 -0.4    -161.0   300       39   16 05 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

16 11 00  2351+456     23 31 38  74.0  15.0 -0.4    -161.3    24       39   16 11 00
16 17 00  ---          23 37 39  74.3  11.3 -0.3    -166.0   360       62   16 11 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

16 17 30  0059+581     23 38 10  58.6  21.4 -1.4    -143.0    -9       62   16 17 39
16 22 30  ---          23 43 10  58.9  20.4 -1.3    -145.0   291       81   16 17 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

16 23 00  0059+581     23 43 40  59.0  20.3 -1.3    -145.1    24       81   16 23 00
16 28 00  ---          23 48 41  59.3  19.3 -1.3    -147.1   300      100   16 23 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

16 28 30  0059+581     23 49 11  59.4  19.1 -1.2    -147.3    24      100   16 28 30
16 34 30  ---          23 55 12  59.8  17.8 -1.1    -149.8   360      123   16 28 31

 ---------- VLBA on calibrators at the beginning of experiment ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

16 35 00  2351+456     23 55 42  74.7  -0.4  0.0     179.6    -7      123   16 35 07
16 40 00  ---          00 00 43  74.6  -3.6  0.1     175.5   293      142   16 35 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

16 40 30  2351+456     00 01 13  74.6  -4.0  0.1     175.1    24      142   16 40 30
16 45 30  ---          00 06 14  74.5  -7.2  0.2     171.1   300      161   16 40 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

16 46 00  2351+456     00 06 44  74.5  -7.5  0.2     170.7    24      161   16 46 00
16 52 00  ---          00 12 45  74.3 -11.3  0.3     165.9   360      184   16 46 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

16 52 30  0059+581     00 13 15  60.8  13.6 -0.8    -157.3    -4      184   16 52 34
16 57 30  ---          00 18 16  61.1  12.3 -0.8    -159.5   296      204   16 52 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

16 58 00  0059+581     00 18 46  61.1  12.2 -0.7    -159.7    24      204   16 58 00
17 03 00  ---          00 23 47  61.3  10.9 -0.7    -161.9   300      223   16 58 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

17 03 30  0059+581     00 24 17  61.3  10.8 -0.7    -162.1    24      223   17 03 30
17 09 30  ---          00 30 18  61.6   9.2 -0.6    -164.8   360      246   17 03 31

 ---------- VLBA on calibrators at the beginning of experiment ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

17 10 00  2351+456     00 30 48  73.2 -21.8  0.6     152.6    -1      246   17 10 01
17 15 00  ---          00 35 49  72.7 -24.4  0.7     149.2   299      265   17 10 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

17 15 30  2351+456     00 36 19  72.7 -24.7  0.7     148.9    24      265   17 15 30
17 20 30  ---          00 41 20  72.2 -27.1  0.8     145.7   300      285   17 15 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

17 21 00  2351+456     00 41 50  72.2 -27.3  0.8     145.3    24      285   17 21 00
17 27 00  ---          00 47 51  71.6 -30.0  0.9     141.7   360      308   17 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

17 27 30  0059+581     00 48 21  62.0   4.3 -0.3    -172.9    -2      308   17 27 32
17 32 30  ---          00 53 22  62.1   2.9 -0.2    -175.2   298      327   17 27 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

17 33 00  0059+581     00 53 52  62.1   2.8 -0.2    -175.5    24      327   17 33 00
17 38 00  ---          00 58 53  62.1   1.4 -0.1    -177.8   300      346   17 33 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

17 38 30  0059+581     00 59 23  62.1   1.2 -0.1    -178.0    24      346   17 38 30
17 44 30  ---          01 05 24  62.1  -0.5  0.0     179.2   360      370   17 38 31

 ---------- VLBA on calibrators at the beginning of experiment ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

17 45 00  2351+456     01 05 54  69.4 -36.9  1.2     132.0    -4      370   17 45 04
17 50 00  ---          01 10 55  68.8 -38.5  1.3     129.6   296      389   17 45 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

17 50 30  2351+456     01 11 25  68.7 -38.6  1.3     129.4    24      389   17 50 30
17 55 30  ---          01 16 26  68.0 -40.1  1.4     127.1   300      408   17 50 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

17 56 00  2351+456     01 16 56  67.9 -40.2  1.4     126.9    24      408   17 56 00
18 02 00  ---          01 22 57  67.1 -41.8  1.5     124.3   360      431   17 56 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

18 02 30  0059+581     01 23 27  61.9  -5.5  0.3     171.0    -4      431   18 02 34
18 07 30  ---          01 28 28  61.8  -6.8  0.4     168.7   296      450   18 02 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

18 08 00  0059+581     01 28 58  61.8  -7.0  0.4     168.5    24      450   18 08 00
18 13 00  ---          01 33 59  61.7  -8.3  0.5     166.2   300      469   18 08 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

18 13 30  0059+581     01 34 29  61.7  -8.5  0.5     166.0    24      469   18 13 30
18 19 30  ---          01 40 30  61.4 -10.1  0.6     163.3   360      493   18 13 31

 ---------- VLBA on calibrators at the beginning of experiment ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

18 20 00  2351+456     01 41 00  64.4 -45.8  1.8     117.5    -3      493   18 20 03
18 25 00  ---          01 46 00  63.6 -46.6  1.8     115.8   297      512   18 20 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

18 25 30  2351+456     01 46 31  63.5 -46.7  1.9     115.6    24      512   18 25 30
18 30 30  ---          01 51 31  62.7 -47.5  1.9     114.0   300      531   18 25 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

18 31 00  2351+456     01 52 01  62.7 -47.6  1.9     113.9    24      531   18 31 00
18 37 00  ---          01 58 02  61.7 -48.5  2.0     112.0   360      554   18 31 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

18 37 30  0059+581     01 58 33  60.6 -14.6  0.9     155.5    -2      554   18 37 32
18 42 30  ---          02 03 33  60.3 -15.8  1.0     153.3   298      574   18 37 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

18 43 00  0059+581     02 04 03  60.3 -15.9  1.0     153.1    24      574   18 43 00
18 48 00  ---          02 09 04  60.0 -17.1  1.1     151.1   300      593   18 43 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

18 48 30  0059+581     02 09 34  60.0 -17.2  1.1     150.8    24      593   18 48 30
18 54 30  ---          02 15 35  59.6 -18.6  1.2     148.4   360      616   18 48 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

18 55 00  2351+456     02 16 05  58.7 -50.6  2.3     106.9    -1      616   18 55 01
19 00 00  ---          02 21 06  57.9 -51.1  2.4     105.6   299      635   18 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

19 00 30  2351+456     02 21 36  57.8 -51.1  2.4     105.5    24      635   19 00 30
19 05 30  ---          02 26 37  57.0 -51.5  2.5     104.3   300      655   19 00 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

19 06 00  2351+456     02 27 07  56.9 -51.6  2.5     104.1    24      655   19 06 00
19 12 00  ---          02 33 08  55.9 -52.0  2.6     102.7   360      678   19 06 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

19 12 30  0059+581     02 33 38  58.2 -22.3  1.5     141.4     1      678   19 12 30
19 17 30  ---          02 38 39  57.8 -23.2  1.6     139.5   300      697   19 12 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

19 18 00  0059+581     02 39 09  57.8 -23.3  1.6     139.3    24      697   19 18 00
19 23 00  ---          02 44 10  57.3 -24.3  1.7     137.5   300      716   19 18 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

19 23 30  0059+581     02 44 40  57.3 -24.3  1.7     137.3    24      716   19 23 30
19 29 30  ---          02 50 41  56.7 -25.4  1.8     135.1   360      740   19 23 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

19 30 00  2351+456     02 51 11  52.8 -53.0  2.9      98.6     2      740   19 30 00
19 35 00  ---          02 56 12  51.9 -53.2  3.0      97.6   300      759   19 30 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

19 35 30  2351+456     02 56 42  51.9 -53.2  3.0      97.5    24      759   19 35 30
19 40 30  ---          03 01 43  51.0 -53.4  3.1      96.4   300      778   19 35 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

19 41 00  2351+456     03 02 13  50.9 -53.4  3.1      96.3    24      778   19 41 00
19 47 00  ---          03 08 14  49.9 -53.6  3.2      95.1   360      801   19 41 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

19 47 30  0059+581     03 08 44  55.0 -28.2  2.1     128.9     4      801   19 47 30
19 52 30  ---          03 13 45  54.5 -28.9  2.2     127.3   300      821   19 47 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

19 53 00  0059+581     03 14 15  54.4 -29.0  2.2     127.1    24      821   19 53 00
19 58 00  ---          03 19 16  53.9 -29.6  2.3     125.5   300      840   19 53 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

19 58 30  0059+581     03 19 46  53.8 -29.7  2.3     125.4    24      840   19 58 30
20 04 30  ---          03 25 47  53.2 -30.4  2.4     123.5   360      863   19 58 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

20 05 00  0059+581     03 26 17  53.1 -30.5  2.4     123.3    24      863   20 05 00
20 09 00  ---          03 30 18  52.7 -31.0  2.4     122.1   240      879   20 05 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

20 09 30  0059+581     03 30 48  52.6 -31.0  2.5     122.0    24      879   20 09 30
20 13 30  ---          03 34 48  52.2 -31.5  2.5     120.7   240      894   20 09 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

20 14 00  0059+581     03 35 18  52.1 -31.5  2.5     120.6    24      894   20 14 00
20 19 00  ---          03 40 19  51.6 -32.1  2.6     119.1   300      914   20 14 01

 ---------- Ground-only segment 02: K-band scans on fringe-finder source ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

20 21 00  0716+714     03 42 20  39.8  20.0 -3.7    -113.0    75      914   20 21 00
20 24 00  ---          03 45 20  40.0  19.9 -3.6    -113.8   180      925   20 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 ---------- Ground-only VLBA U,Q-band scans on 0716+714 ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

20 24 10  0716+714     03 45 30  40.0  19.9 -3.6    -113.8     4      925   20 24 10
20 26 10  ---          03 47 30  40.1  19.8 -3.6    -114.4   120      933   20 24 11

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

20 26 40  0716+714     03 48 00  40.2  19.8 -3.6    -114.5    24      933   20 26 40
20 31 00  ---          03 52 21  40.5  19.6 -3.5    -115.6   260      950   20 26 41

 ----------  EVN+VLBA K-band scans on target source ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

20 31 30  0851+202     03 52 51  22.0  79.0 -5.0     -64.0   -20      950   20 31 50
20 41 00  ---          04 02 23  24.0  80.1 -4.9     -64.4   550      985   20 31 31

20 41 30  0851+202     04 02 53  24.1  80.1 -4.9     -64.5    24      985   20 41 30
20 51 00  ---          04 12 24  26.1  81.2 -4.7     -64.8   570     1022   20 41 31

20 51 30  0851+202     04 12 55  26.2  81.2 -4.7     -64.9    24     1022   20 51 30
21 01 00  ---          04 22 26  28.2  82.3 -4.6     -65.2   570     1058   20 51 31

 ---------- Ground-only VLBA U,Q-band scans on target source ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

21 01 00  0851+202     04 22 26  28.2  82.3 -4.6     -65.2    -6     1058   21 01 06
21 06 30  ---          04 27 57  29.4  82.9 -4.5     -65.4   324     1079   21 01 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

21 07 00  0851+202     04 28 27  29.5  83.0 -4.5     -65.4    24     1079   21 07 00
21 10 30  ---          04 31 58  30.3  83.4 -4.4     -65.5   210     1093   21 07 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 ----------  EVN+VLBA K-band scans on target source ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

21 11 30  0851+202     04 32 58  30.5  83.5 -4.4     -65.5    54     1093   21 11 30
21 20 30  ---          04 41 59  32.4  84.5 -4.2     -65.7   540     1128   21 11 31

 ----------  EVN+VLBA K-band scans on target source ----------

21 21 30  0851+202     04 42 59  32.6  84.6 -4.2     -65.8    54     1128   21 21 30
21 31 00  ---          04 52 31  34.7  85.7 -4.1     -66.0   570     1164   21 21 31

21 31 30  0851+202     04 53 01  34.8  85.8 -4.0     -66.0    24     1164   21 31 30
21 41 00  ---          05 02 33  36.8  86.9 -3.9     -66.1   570     1201   21 31 31

21 41 30  0851+202     05 03 03  36.9  87.0 -3.9     -66.2    24     1201   21 41 30
21 51 00  ---          05 12 34  39.0  88.1 -3.7     -66.3   570     1238   21 41 31

21 51 30  0851+202     05 13 04  39.1  88.2 -3.7     -66.3    24     1238   21 51 30
22 01 00  ---          05 22 36  41.1  89.3 -3.6     -66.3   570     1274   21 51 31

22 01 30  0851+202     05 23 06  41.2  89.4 -3.5     -66.3    24     1274   22 01 30
22 07 30  ---          05 29 07  42.5  90.2 -3.4     -66.3   360     1298   22 01 31

 ---------- Ground-only VLBA U,Q-band +Ef U-band scans on target source ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

22 08 00  0851+202     05 29 37  42.6  90.2 -3.4     -66.3    24     1298   22 08 00
22 13 30  ---          05 35 08  43.8  90.9 -3.3     -66.3   330     1319   22 08 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

22 14 00  0851+202     05 35 38  43.9  91.0 -3.3     -66.3    24     1319   22 14 00
22 17 30  ---          05 39 09  44.7  91.5 -3.3     -66.3   210     1332   22 14 01

 ---------- Ground-only U,Q,K-band scans on fringe-finder  0716+71 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

22 21 00  0716+714     05 42 39  47.1  11.6 -1.7    -147.4   145     1332   22 21 00
22 25 00  ---          05 46 40  47.2  11.2 -1.6    -148.6   240     1348   22 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

22 25 30  0716+714     05 47 10  47.2  11.1 -1.6    -148.8    24     1348   22 25 30
22 29 30  ---          05 51 11  47.4  10.7 -1.5    -150.0   240     1363   22 25 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

22 30 00  0716+714     05 51 41  47.4  10.7 -1.5    -150.2    24     1363   22 30 00
22 34 30  ---          05 56 11  47.6  10.2 -1.5    -151.6   270     1381   22 30 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

22 35 00  0716+714     05 56 42  47.6  10.1 -1.5    -151.8    24     1381   22 35 00
22 39 00  ---          06 00 42  47.8   9.7 -1.4    -153.0   240     1396   22 35 01

 ---------- K-band VLBI scans. Space segment 03: 0851+202 ----------

22 40 00  0851+202     06 01 42  49.5  94.6 -2.9     -65.9    -8     1396   22 40 08
22 50 00  ---          06 11 44  51.7  96.1 -2.7     -65.6   592     1434   22 40 01

22 50 30  0851+202     06 12 14  51.8  96.2 -2.7     -65.6    24     1434   22 50 30
23 00 00  ---          06 21 46  53.8  97.8 -2.6     -65.2   570     1471   22 50 31

23 00 30  0851+202     06 22 16  53.9  97.9 -2.6     -65.1    24     1471   23 00 30
23 10 00  ---          06 31 47  56.0  99.5 -2.4     -64.6   570     1508   23 00 31

23 10 30  0851+202     06 32 17  56.1  99.6 -2.4     -64.6    24     1508   23 10 30
23 20 00  ---          06 41 49  58.1 101.4 -2.2     -63.9   570     1544   23 10 31

23 20 30  0851+202     06 42 19  58.2 101.5 -2.2     -63.8    24     1544   23 20 30
23 30 00  ---          06 51 51  60.2 103.4 -2.1     -63.0   570     1581   23 20 31

23 30 30  0851+202     06 52 21  60.3 103.5 -2.1     -62.9    24     1581   23 30 30
23 40 00  ---          07 01 52  62.3 105.7 -1.9     -61.9   570     1618   23 30 31

 ---------- Ground-only U,Q-band scans on  0851+202 ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

23 41 00  0851+202     07 02 52  62.5 105.9 -1.9     -61.7    54     1618   23 41 00
23 46 30  ---          07 08 23  63.6 107.3 -1.8     -61.0   330     1639   23 41 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  25 Apr 2016   Day 116 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

23 47 00  0851+202     07 08 53  63.7 107.4 -1.8     -60.9    24     1639   23 47 00
23 50 30  ---          07 12 24  64.4 108.4 -1.7     -60.4   210     1653   23 47 01

 --- Start: Mon  25 Apr 2016   Day 116 -- Stop: Tue  26 Apr 2016   Day 117 ---

 ---------- Ground-only segment 03: K-band scans: 0851+202 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

23 51 00  0851+202     07 12 54  64.5 108.5 -1.7     -60.3    24     1653   23 51 00
00 00 30  ---          07 22 26  66.5 111.2 -1.6     -58.6   570     1689   23 51 01

00 01 00  0851+202     07 22 56  66.6 111.4 -1.5     -58.5    24     1689   00 01 00
00 10 30  ---          07 32 27  68.5 114.5 -1.4     -56.4   570     1726   00 01 01

00 11 00  0851+202     07 32 57  68.6 114.7 -1.4     -56.3    24     1726   00 11 00
00 20 30  ---          07 42 29  70.4 118.4 -1.2     -53.7   570     1763   00 11 01

00 21 00  0851+202     07 42 59  70.5 118.6 -1.2     -53.5    24     1763   00 21 00
00 30 30  ---          07 52 31  72.2 122.9 -1.1     -50.2   570     1800   00 21 01

00 31 00  0851+202     07 53 01  72.3 123.2 -1.0     -50.1    24     1800   00 31 00
00 40 30  ---          08 02 32  74.0 128.3 -0.9     -45.9   570     1836   00 31 01

00 41 00  0851+202     08 03 02  74.1 128.6 -0.9     -45.7    24     1836   00 41 00
00 50 30  ---          08 12 34  75.6 134.9 -0.7     -40.5   570     1873   00 41 01

 ---------- Ground-only U,Q-band scans on  0851+202 ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

00 51 00  0851+202     08 13 04  75.7 135.3 -0.7     -40.1    24     1873   00 51 00
00 56 30  ---          08 18 35  76.5 139.5 -0.6     -36.5   330     1894   00 51 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

00 57 00  0851+202     08 19 05  76.6 139.9 -0.6     -36.2    24     1894   00 57 00
01 00 40  ---          08 22 45  77.1 143.0 -0.5     -33.4   220     1908   00 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  26 Apr 2016   Day 117 ---

 ---------- Ground-only segment K-band scans: 0851+202 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

01 01 30  0851+202     08 23 36  77.2 143.7 -0.5     -32.8    44     1908   01 01 30
01 11 00  ---          08 33 07  78.2 153.0 -0.4     -24.6   570     1945   01 01 31

01 11 30  0851+202     08 33 37  78.3 153.5 -0.4     -24.1    24     1945   01 11 30
01 21 00  ---          08 43 09  79.0 164.3 -0.2     -14.4   570     1982   01 11 31

01 21 30  0851+202     08 43 39  79.1 164.9 -0.2     -13.8    24     1982   01 21 30
01 31 00  ---          08 53 10  79.4 176.7 -0.0      -3.0   570     2019   01 21 31

01 31 30  0851+202     08 53 41  79.4 177.4 -0.0      -2.4    24     2019   01 31 30
01 41 00  ---          09 03 12  79.3 189.5  0.1       8.7   570     2055   01 31 31

01 41 30  0851+202     09 03 42  79.3 190.1  0.1       9.2    24     2055   01 41 30
01 51 00  ---          09 13 14  78.7 201.4  0.3      19.6   570     2092   01 41 31

01 51 30  0851+202     09 13 44  78.7 202.0  0.3      20.1    24     2092   01 51 30
02 01 00  ---          09 23 15  77.7 212.0  0.5      29.0   570     2129   01 51 31

 ---------- Ground-only segment U,Q-band scans on fringe-finder 0716+714 ----------

02 01 30  0716+714     09 23 45  46.2 346.6  2.0     141.6   -74     2129   02 02 44
02 05 30  ---          09 27 46  46.0 346.3  2.1     140.4   166     2139   02 01 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

02 06 00  0716+714     09 28 16  45.9 346.2  2.1     140.2    24     2139   02 06 00
02 10 00  ---          09 32 17  45.7 345.9  2.1     139.0   240     2155   02 06 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

02 10 30  0716+714     09 32 47  45.7 345.8  2.2     138.9    24     2155   02 10 30
02 15 00  ---          09 37 18  45.5 345.4  2.2     137.5   270     2172   02 10 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

02 15 30  0851+202     09 37 48  75.8 224.3  0.7      39.8   -64     2172   02 16 34
02 20 30  ---          09 42 49  75.0 227.8  0.8      42.7   236     2187   02 15 31

02 21 30  0851+202     09 43 49  74.9 228.5  0.8      43.3    54     2187   02 21 30
02 29 30  ---          09 51 50  73.5 233.3  0.9      47.3   480     2218   02 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  26 Apr 2016   Day 117 ---

 ---------- K-band VLBI scans. Space segment 04: 0851+202 ----------

02 30 00  0851+202     09 52 20  73.4 233.6  0.9      47.5    24     2218   02 30 00
02 40 00  ---          10 02 22  71.6 238.7  1.1      51.5   600     2257   02 30 01

02 40 30  0851+202     10 02 52  71.5 238.9  1.1      51.7    24     2257   02 40 30
02 50 00  ---          10 12 23  69.7 243.0  1.3      54.7   570     2294   02 40 31

02 50 30  0851+202     10 12 54  69.7 243.2  1.3      54.8    24     2294   02 50 30
03 00 00  ---          10 22 25  67.8 246.6  1.4      57.2   570     2330   02 50 31

03 00 30  0851+202     10 22 55  67.7 246.8  1.5      57.3    24     2330   03 00 30
03 10 00  ---          10 32 27  65.8 249.8  1.6      59.2   570     2367   03 00 31

03 10 30  0851+202     10 32 57  65.7 249.9  1.6      59.3    24     2367   03 10 30
03 20 00  ---          10 42 28  63.8 252.5  1.8      60.9   570     2404   03 10 31

 ---------- Ground-only segment U,Q-band scans: 0851+202 ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

03 21 00  0851+202     10 43 29  63.5 252.8  1.8      61.0    54     2404   03 21 00
03 26 30  ---          10 48 59  62.4 254.1  1.9      61.8   330     2425   03 21 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

03 27 00  0851+202     10 49 30  62.3 254.3  1.9      61.8    24     2425   03 27 00
03 30 40  ---          10 53 10  61.5 255.1  2.0      62.3   220     2439   03 27 01

 ---------- Ground-only segment: K-band scans: 0851+202 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

03 31 10  0851+202     10 53 40  61.4 255.2  2.0      62.3    24     2439   03 31 10
03 40 40  ---          11 03 12  59.4 257.3  2.1      63.3   570     2476   03 31 11

03 41 10  0851+202     11 03 42  59.3 257.4  2.1      63.4    24     2476   03 41 10
03 50 40  ---          11 13 13  57.3 259.3  2.3      64.2   570     2513   03 41 11

03 51 10  0851+202     11 13 43  57.2 259.4  2.3      64.2    24     2513   03 51 10
04 00 40  ---          11 23 15  55.2 261.1  2.5      64.8   570     2549   03 51 11

04 01 10  0851+202     11 23 45  55.1 261.2  2.5      64.8    24     2549   04 01 10
04 10 40  ---          11 33 17  53.1 262.8  2.6      65.3   570     2586   04 01 11
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  26 Apr 2016   Day 117 ---

04 11 10  0851+202     11 33 47  53.0 262.9  2.6      65.4    24     2586   04 11 10
04 20 40  ---          11 43 18  50.9 264.4  2.8      65.7   570     2623   04 11 11

04 21 10  0851+202     11 43 48  50.8 264.5  2.8      65.7    24     2623   04 21 10
04 30 40  ---          11 53 20  48.8 265.9  3.0      66.0   570     2660   04 21 11

 ---------- Ground-only segment 03: K-band scans: 0851+202 while GBT performs pointing ----------

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

04 31 10  0851+202     11 53 50  48.7 266.0  3.0      66.0    24     2660   04 31 10
04 36 40  ---          11 59 21  47.5 266.8  3.1      66.1   330     2681   04 31 11

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

04 37 10  0851+202     11 59 51  47.4 266.8  3.1      66.1    24     2681   04 37 10
04 40 40  ---          12 03 22  46.6 267.3  3.1      66.2   210     2694   04 37 11

 ---------- Ground-only segment U,Q-band scans on fringe-finder 0716+714 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

04 41 30  0716+714     12 04 12  35.2 338.4  4.7      98.0    -8     2694   04 41 38
04 45 30  ---          12 08 12  34.9 338.3  4.7      97.0   232     2709   04 41 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

04 46 00  0716+714     12 08 42  34.8 338.3  4.8      96.9    24     2709   04 46 00
04 50 00  ---          12 12 43  34.5 338.3  4.8      95.9   240     2725   04 46 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

04 50 30  0716+714     12 13 13  34.5 338.3  4.8      95.8    24     2725   04 50 30
04 55 00  ---          12 17 44  34.1 338.2  4.9      94.7   270     2742   04 50 31

 ---------- Ground-only segment: K-band scans: 0851+202 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

04 55 30  0851+202     12 18 14  43.4 269.3  3.4      66.3   -27     2742   04 55 57
05 05 00  ---          12 27 46  41.4 270.5  3.5      66.3   543     2777   04 55 31

05 05 30  0851+202     12 28 16  41.3 270.6  3.5      66.3    24     2777   05 05 30
05 15 00  ---          12 37 47  39.2 271.8  3.7      66.3   570     2814   05 05 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  26 Apr 2016   Day 117 ---

05 15 30  0851+202     12 38 17  39.1 271.8  3.7      66.3    24     2814   05 15 30
05 25 00  ---          12 47 49  37.1 273.0  3.9      66.2   570     2851   05 15 31

05 25 30  0851+202     12 48 19  37.0 273.0  3.9      66.2    24     2851   05 25 30
05 35 00  ---          12 57 51  34.9 274.2  4.0      66.0   570     2887   05 25 31

05 35 30  0851+202     12 58 21  34.8 274.2  4.0      66.0    24     2887   05 35 30
05 45 00  ---          13 07 52  32.8 275.3  4.2      65.8   570     2924   05 35 31

05 45 30  0851+202     13 08 22  32.7 275.4  4.2      65.8    24     2924   05 45 30
05 55 00  ---          13 17 54  30.6 276.5  4.4      65.5   570     2961   05 45 31

 ---------- Ground-only segment: K-band scans: 0851+202 ----------

05 55 30  0851+202     13 18 24  30.5 276.5  4.4      65.5    24     2961   05 55 30
06 03 30  ---          13 26 25  28.8 277.4  4.5      65.3   480     2992   05 55 31

 ---------- K-band VLBI scans. Space segment 05: 0851+202 ----------

06 10 00  0851+202     13 32 56  27.4 278.1  4.6      65.1   383     2992   06 10 00
06 20 00  ---          13 42 58  25.3 279.3  4.8      64.7   600     3030   06 10 01

06 20 30  0851+202     13 43 28  25.2 279.3  4.8      64.7    24     3030   06 20 30
06 30 00  ---          13 53 00  23.2 280.4  5.0      64.3   570     3067   06 20 31

06 30 30  0851+202     13 53 30  23.0 280.4  5.0      64.3    24     3067   06 30 30
06 40 00  ---          14 03 01  21.0 281.5  5.1      63.8   570     3104   06 30 31

06 40 30  0851+202     14 03 31  20.9 281.5  5.1      63.8    24     3104   06 40 30
06 50 00  ---          14 13 03  18.9 282.6  5.3      63.4   570     3140   06 40 31

06 50 30  0851+202     14 13 33  18.8 282.6  5.3      63.3    24     3140   06 50 30
07 00 00  ---          14 23 05  16.8 283.7  5.5      62.8   570     3177   06 50 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg079c_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   38         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  19  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
   BBC fr=     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     736.99    736.99    769.01    769.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  19  20  21  22  23  24  25  26  27  28

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg079c_freq.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  29  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
   BBC fr=     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     735.99    735.99    768.01    768.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  29  30  31  32  33  34  35  36  37  38

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg079c_freq.dat:
     v7mm_c8

   Setup group:   49         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  39  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
   BBC fr=     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     730.25    730.25    762.25    762.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  39  40  41  42  43  44  45  46  47  48

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 54.228301       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 45.83009        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0059+581          00 59 43.470970   * 01 02 45.762378     01 03 43.932811       0.00
   J0102+5824        58 08 04.84745    * 58 24 11.13660      58 29 12.08599        0.00
                     ./gg079c_sources.radioastron
                     AGN, MASIV, rfc_2013d Petrov, 2013, unpublished 319479 observations, RA-AO3-04,

 * 0716+714          07 16 13.029739   * 07 21 53.448474     07 23 41.581091       0.00
   J0721+7120        71 26 15.17406    * 71 20 36.36340      71 18 48.34423        0.00
                     ./gg079c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 42370 observations, RA-AO3-04, RA-AO2-1

 * 0851+202          08 51 57.250618   * 08 54 48.874930     08 55 44.488404       0.00
   J0854+2006        20 17 58.41733    * 20 06 30.64078      20 02 39.31337        0.00
   OJ287             ./gg079c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 213710 observations, RA-AO3-04, RA-AO3-

 * 1633+382          16 33 30.625100   * 16 35 15.492975     16 35 50.735816       0.00
   J1635+3808        38 14 10.08266    * 38 08 04.50043      38 06 04.33594        0.00
   4C38.41           ./gg079c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 16451 observations, RA-AO3-04, RA-AO3-0

   1641+399          16 41 17.606226   * 16 42 58.809963     16 43 32.872709       0.00
   J1642+3948        39 54 10.81479    * 39 48 36.99385      39 46 46.74911        0.00
 * 3C345             ./gg079c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 51938 observations, RA-AO3-04, RA-AO3-0

 * 2351+456          23 51 49.972507   * 23 54 21.680217     23 55 10.238966       0.00
   J2354+4553        45 36 22.77745    * 45 53 04.23639      45 58 16.29707        0.00
                     ./gg079c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 2579 observations, RA-AO3-04, RA-AO2-12



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            49                                4.475     0.000
  0059+581   ra1cm2.set            29                                0.650    25.283
             ra2cm2.set            19                                0.650    24.067
             ra7mm2.set            39                                0.783    30.433
  0716+714   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 17 29  +     0.367    26.503
             ra2cm2.set            19                                0.233     9.600
             ra7mm2.set            39                                0.297    12.050
  0851+202   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 13 16  +    12.833  1352.410
             ra2cm2.set            19 51                             0.356    16.583
             ra7mm2.set            39                                0.550    23.040
  1633+382   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 16 17  +     3.458   226.227
  3C345      ra1cm2.set            1 2 3 4 5 6 7 8 9 10 16 17  +     3.458   224.479
  2351+456   ra1cm2.set            29                                0.583    23.417
             ra2cm2.set            19                                0.583    22.250
             ra7mm2.set            39                                0.700    28.100


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              80.7
   0059+581            46.9
   0716+714            73.0
   0851+202            94.5
   1633+382           118.7
   3C345              116.5
   2351+456            43.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

