  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The anomalous equatorial emission region of SS433
 Exp. Code:  GP025A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 1 July 1999                        

PI:       Zsolt Paragi                                                    

Address:  FOMI Satellite Geodetic Observatory                             
          P. O. Box 546                                                   
          H-1373 Budapest                                                 
          HUNGARY                                                         

Phone:    36 27 374 980                                                   
EMAIL:    paragi@sgo.fomi.hu                                              
Fax:      36 27 374 982                                                   
Phone during observation: 36 27 374 980                                   

Observing mode: Continuum 18 cm; Recording mode: 128-4-2 (VLBA/MKIV).     

Notes:    Global VLBI monitoring at 18cm. Observe RCP+LCP, but we         
          do not need crosspol. Fringe-finders: OQ208, 3C454.3            
          Send logs and calibration information to Zsolt Paragi.          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

 Next scan frequencies:  1654.99  1654.99  1662.99  1662.99
 Next BBC frequencies:    745.01   745.01   737.01   737.01
 Next scan bandwidths:      8.00     8.00     8.00     8.00

11 04 44  SS433        13 40 10   8.6  89.3 -5.5     -59.7     0   1  1      0  11 04 34
11 15 24  ---          13 50 52  10.9  90.7 -5.3     -59.7   640   F  1   4334

11 15 34  SS433        13 51 02  11.0  90.7 -5.3     -59.7     8   1  1   4334  11 15 24
11 26 14  ---          14 01 44  13.3  92.1 -5.2     -59.7   640   F  1   8669

11 29 14  SS433        14 04 45  13.9  92.5 -5.1     -59.6   177   1  1   8669  11 28 54
11 50 54  ---          14 26 28  18.6  95.3 -4.8     -59.3  1300   F  1  17469

11 53 54  SS433        14 29 29  19.2  95.7 -4.7     -59.2   177   1  2  17469  11 53 34
12 15 34  ---          14 51 12  23.9  98.7 -4.3     -58.6  1300   R  1   8669

12 18 34  J1907+0127   14 54 13  23.6 103.1 -4.2     -57.0   175   1  2   8669  12 18 14
12 19 14  ---          14 54 53  23.7 103.2 -4.2     -56.9    40   R  1   8269

12 19 59  SS433        14 55 38  24.8  99.4 -4.3     -58.5    41   1  2   8269  12 19 14
12 20 59  ---          14 56 38  25.0  99.5 -4.3     -58.4    60   R  1   7568

12 21 10  1910+052     14 56 50  25.0  99.1 -4.3     -58.6     9   1  2   7568  12 20 59
12 22 10  ---          14 57 50  25.2  99.2 -4.3     -58.5    60   R  1   7092

12 23 03  J1907+0127   14 58 42  24.5 103.8 -4.1     -56.7    47   1  2   7092  12 22 10
12 24 03  ---          14 59 42  24.7 103.9 -4.1     -56.7    60   R  1   6345

12 24 48  SS433        15 00 27  25.8 100.0 -4.2     -58.3    41   1  2   6345  12 24 03
12 25 48  ---          15 01 28  26.0 100.2 -4.2     -58.2    60   R  1   5644

12 25 59  1910+052     15 01 39  26.0  99.8 -4.2     -58.4     9   1  2   5644  12 25 48
12 26 59  ---          15 02 39  26.2  99.9 -4.2     -58.3    60   R  1   5169

12 27 51  J1907+0127   15 03 31  25.5 104.5 -4.1     -56.4    47   1  2   5169  12 26 59
12 28 51  ---          15 04 31  25.7 104.6 -4.0     -56.4    60   R  1   4422

12 29 36  SS433        15 05 17  26.8 100.8 -4.1     -58.1    40   1  2   4422  12 28 51
12 30 36  ---          15 06 17  27.1 100.9 -4.1     -58.0    60   R  1   3722

12 30 47  1910+052     15 06 28  27.0 100.5 -4.1     -58.2     9   1  2   3722  12 30 36
12 31 47  ---          15 07 28  27.2 100.6 -4.1     -58.1    60   R  1   3247
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

12 32 39  J1907+0127   15 08 20  26.5 105.2 -4.0     -56.1    47   1  2   3247  12 31 47
12 33 39  ---          15 09 21  26.7 105.4 -4.0     -56.1    60   R  1   2500

12 34 24  SS433        15 10 06  27.9 101.5 -4.0     -57.8    40   1  2   2500  12 33 39
12 35 24  ---          15 11 06  28.1 101.6 -4.0     -57.8    60   R  1   1800

12 35 36  1910+052     15 11 17  28.1 101.2 -4.0     -58.0     9   1  2   1800  12 35 24
12 36 36  ---          15 12 17  28.3 101.3 -4.0     -57.9    60   R  1   1325

12 37 28  J1907+0127   15 13 09  27.5 106.0 -3.9     -55.8    47   1  2   1325  12 36 36
12 38 28  ---          15 14 10  27.7 106.2 -3.9     -55.8    60   R  1    578

12 39 12  SS433        15 14 55  28.9 102.2 -3.9     -57.6    40   1  3    578  12 38 28
13 02 12  ---          15 37 58  33.7 105.9 -3.6     -56.2  1380   F  1   8921

13 04 12  SS433        15 39 59  34.1 106.2 -3.5     -56.0   117   1  3   8921  13 03 52
13 14 52  ---          15 50 40  36.3 108.0 -3.4     -55.2   640   F  1  13321

13 18 07  J2101+0341   15 53 55  13.1  93.5 -5.1     -59.4   146   1  4  13321  13 17 47
13 28 47  =2059+034    16 04 37  15.4  94.9 -4.9     -59.2   640   R  1  17479

13 32 01  J1907+0127   16 07 52  38.5 115.7 -3.0     -50.8   146   1  4  17479  13 31 41
13 32 41  ---          16 08 32  38.7 115.9 -3.0     -50.8    40   R  1  17079

13 33 25  SS433        16 09 16  40.1 111.5 -3.0     -53.5    39   1  4  17079  13 32 41
13 34 25  ---          16 10 16  40.3 111.7 -3.0     -53.4    60   R  1  16386

13 34 36  1910+052     16 10 27  40.3 111.2 -3.0     -53.7     9   1  4  16386  13 34 25
13 35 36  ---          16 11 27  40.5 111.4 -3.0     -53.6    60   R  1  15911

13 36 27  J1907+0127   16 12 19  39.4 116.6 -2.9     -50.3    46   1  4  15911  13 35 36
13 37 27  ---          16 13 19  39.6 116.8 -2.9     -50.2    60   R  1  15168

13 38 11  SS433        16 14 03  41.0 112.4 -3.0     -53.0    39   1  4  15168  13 37 27
13 39 11  ---          16 15 03  41.2 112.6 -2.9     -52.9    60   R  1  14476

13 39 23  1910+052     16 15 15  41.2 112.1 -3.0     -53.2     9   1  4  14476  13 39 11
13 40 23  ---          16 16 15  41.4 112.3 -2.9     -53.1    60   R  1  14001

13 41 14  J1907+0127   16 17 06  40.3 117.6 -2.8     -49.7    46   1  4  14001  13 40 23
13 42 14  ---          16 18 06  40.5 117.8 -2.8     -49.6    60   R  1  13258
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

13 42 58  SS433        16 18 50  42.0 113.4 -2.9     -52.4    39   1  4  13258  13 42 14
13 43 58  ---          16 19 51  42.2 113.6 -2.9     -52.3    60   R  1  12566

13 44 09  1910+052     16 20 02  42.2 113.1 -2.9     -52.7     9   1  4  12566  13 43 58
13 45 09  ---          16 21 02  42.4 113.3 -2.9     -52.5    60   R  1  12091

13 46 00  J1907+0127   16 21 53  41.2 118.7 -2.8     -49.0    46   1  4  12091  13 45 09
13 47 00  ---          16 22 54  41.4 118.9 -2.7     -48.9    60   R  1  11349

13 47 44  SS433        16 23 37  42.9 114.4 -2.8     -51.9    39   1  4  11349  13 47 00
13 48 44  ---          16 24 38  43.1 114.6 -2.8     -51.8    60   R  1  10658

13 48 55  1910+052     16 24 49  43.1 114.1 -2.8     -52.1     9   1  4  10658  13 48 44
13 49 55  ---          16 25 49  43.3 114.3 -2.8     -52.0    60   R  1  10182

13 50 47  J1907+0127   16 26 40  42.1 119.7 -2.7     -48.4    46   1  4  10182  13 49 55
13 51 47  ---          16 27 41  42.3 119.9 -2.7     -48.2    60   R  1   9441

13 53 47  SS433        16 29 41  44.1 115.7 -2.7     -51.1   114   1  4   9441  13 53 27
14 15 27  ---          16 51 25  48.2 120.7 -2.3     -47.9  1300   R  1    641

14 17 27  SS433        16 53 25  48.6 121.2 -2.3     -47.6   117   1  5    641  14 17 07
14 39 07  ---          17 15 08  52.4 127.2 -1.9     -43.5  1300   F  1   8159

14 42 07  SS433        17 18 09  53.0 128.1 -1.9     -42.8   177   1  5   8159  14 41 47
14 52 47  ---          17 28 51  54.7 131.5 -1.7     -40.3   640   F  1  12559

14 52 49  SS433        17 28 53  54.7 131.5 -1.7     -40.3     0   1  6  12559  14 52 47
15 23 49  ---          17 59 58  59.3 143.0 -1.2     -31.3  1860   R  1  10227

15 26 49  J1907+0127   18 02 58  57.1 149.4 -1.1     -26.0   174   1  6  10227  15 26 29
15 27 29  ---          18 03 38  57.2 149.7 -1.1     -25.7    40   R  1   9827

15 27 38  SS433        18 03 48  59.8 144.7 -1.1     -30.0     2   1  6   9827  15 27 29
15 28 38  ---          18 04 48  59.9 145.1 -1.1     -29.6    60   R  1   9364

15 28 41  1910+052     18 04 51  60.0 144.3 -1.1     -30.3     0   1  6   9364  15 28 38
15 29 41  ---          18 05 51  60.2 144.8 -1.1     -29.9    60   R  1   8946

15 29 51  J1907+0127   18 06 01  57.4 150.7 -1.0     -24.9     3   1  6   8946  15 29 41
15 30 51  ---          18 07 01  57.5 151.1 -1.0     -24.6    60   R  1   8478
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

15 31 00  SS433        18 07 11  60.2 146.1 -1.1     -28.8     2   1  6   8478  15 30 51
15 32 00  ---          18 08 11  60.3 146.6 -1.1     -28.4    60   R  1   8015

15 32 03  1910+052     18 08 14  60.5 145.8 -1.1     -29.1     0   1  6   8015  15 32 00
15 33 03  ---          18 09 14  60.6 146.2 -1.1     -28.7    60   R  1   7596

15 33 13  J1907+0127   18 09 24  57.8 152.1 -1.0     -23.7     3   1  6   7596  15 33 03
15 34 13  ---          18 10 24  57.9 152.6 -0.9     -23.4    60   R  1   7128

15 34 23  SS433        18 10 34  60.6 147.6 -1.0     -27.5     2   1  6   7128  15 34 13
15 35 23  ---          18 11 34  60.7 148.1 -1.0     -27.2    60   R  1   6666

15 35 26  1910+052     18 11 37  60.9 147.3 -1.0     -27.8     0   1  6   6666  15 35 23
15 36 26  ---          18 12 37  61.0 147.8 -1.0     -27.4    60   R  1   6247

15 36 36  J1907+0127   18 12 47  58.1 153.6 -0.9     -22.5     2   1  6   6247  15 36 26
15 37 36  ---          18 13 47  58.2 154.0 -0.9     -22.1    60   R  1   5779

15 37 45  SS433        18 13 57  61.0 149.2 -1.0     -26.3     2   1  6   5779  15 37 36
15 38 45  ---          18 14 57  61.1 149.6 -0.9     -25.9    60   R  1   5316

15 38 48  1910+052     18 15 00  61.2 148.9 -1.0     -26.5     0   1  6   5316  15 38 45
15 39 48  ---          18 16 00  61.3 149.3 -0.9     -26.2    60   R  1   4898

15 39 58  J1907+0127   18 16 10  58.4 155.1 -0.9     -21.3     2   1  6   4898  15 39 48
15 40 58  ---          18 17 10  58.5 155.5 -0.8     -20.9    60   R  1   4430

15 41 08  SS433        18 17 20  61.3 150.7 -0.9     -25.0     2   1  7   4430  15 40 58
16 02 48  ---          18 39 03  63.2 161.7 -0.5     -15.8  1300   F  1   4300

16 04 48  J2101+0341   18 41 04  47.3 122.1 -2.3     -46.9    86   1  7   4300  16 04 28
16 09 58  =2059+034    18 46 14  48.2 123.4 -2.3     -46.0   310   F  1   6500

16 10 17  J2025+0316   18 46 33  54.1 134.8 -1.6     -37.7     5   1  7   6500  16 09 58
16 15 07  =2022+031    18 51 24  54.8 136.4 -1.6     -36.4   290   F  1   8560

16 16 07  SS433        18 52 24  63.9 168.9 -0.3      -9.5    36   1  8   8560  16 15 07
16 48 47  ---          19 25 10  64.2 187.7  0.2       6.6  1960   R  1  13173

16 51 47  SS433        19 28 10  64.1 189.4  0.3       8.1   177   1  9  13173  16 51 27
17 35 27  ---          20 11 57  60.7 211.9  1.0      27.1  2620   F  1   4427
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

17 38 27  J1907+0127   20 14 58  56.7 212.0  1.1      27.2   170   1  9   4427  17 38 07
17 39 07  ---          20 15 38  56.6 212.3  1.1      27.4    40   F  1   4827

17 39 16  SS433        20 15 48  60.3 213.6  1.1      28.6     0   1  9   4827  17 39 07
17 40 16  ---          20 16 48  60.1 214.0  1.1      28.9    60   F  1   5289

17 40 19  1910+052     20 16 50  60.5 213.9  1.1      28.8     0   1  9   5289  17 40 16
17 41 19  ---          20 17 51  60.4 214.3  1.1      29.2    60   F  1   5708

17 41 29  J1907+0127   20 18 01  56.3 213.3  1.2      28.2     0   1  9   5708  17 41 19
17 42 29  ---          20 19 01  56.2 213.7  1.2      28.5    60   F  1   6176

17 42 39  SS433        20 19 11  59.8 215.1  1.1      29.8     0   1  9   6176  17 42 29
17 43 39  ---          20 20 11  59.7 215.5  1.1      30.1    60   F  1   6639

17 43 41  1910+052     20 20 14  60.1 215.4  1.1      30.0     0   1  9   6639  17 43 39
17 44 41  ---          20 21 14  60.0 215.8  1.1      30.4    60   F  1   7058

17 44 52  J1907+0127   20 21 24  55.9 214.6  1.2      29.3     0   1  9   7058  17 44 41
17 45 52  ---          20 22 24  55.8 215.0  1.3      29.6    60   F  1   7526

17 46 01  SS433        20 22 34  59.4 216.5  1.2      30.9     0   1  9   7526  17 45 52
17 47 01  ---          20 23 34  59.3 216.9  1.2      31.3    60   F  1   7989

17 47 04  1910+052     20 23 37  59.7 216.8  1.2      31.2     0   1  9   7989  17 47 01
17 48 04  ---          20 24 37  59.6 217.2  1.2      31.5    60   F  1   8407

17 48 14  J1907+0127   20 24 47  55.5 215.9  1.3      30.3     0   1  9   8407  17 48 04
17 49 14  ---          20 25 47  55.4 216.3  1.3      30.6    60   F  1   8876

17 49 23  SS433        20 25 57  59.0 217.9  1.2      32.1     0   1  9   8876  17 49 14
17 50 23  ---          20 26 57  58.8 218.3  1.3      32.4    60   F  1   9338

17 50 26  1910+052     20 27 00  59.2 218.2  1.2      32.3     0   1  9   9338  17 50 23
17 51 26  ---          20 28 00  59.1 218.6  1.3      32.7    60   F  1   9757

17 51 37  J1907+0127   20 28 10  55.1 217.2  1.3      31.3     0   1  9   9757  17 51 26
17 52 37  ---          20 29 10  54.9 217.6  1.4      31.6    60   F  1  10225

17 52 46  SS433        20 29 20  58.5 219.3  1.3      33.2     0   1 10  10225  17 52 37
18 14 26  ---          20 51 03  55.3 227.3  1.7      39.4  1300   R  1  16245
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

18 17 26  SS433        20 54 04  54.8 228.3  1.7      40.1   177   1 11  16245  18 17 06
19 01 06  ---          21 37 51  47.2 240.7  2.4      48.8  2620   F  1   1355

19 03 06  J2101+0341   21 39 51  61.6 200.4  0.6      17.5    89   1 11   1355  19 02 46
19 08 16  =2059+034    21 45 02  61.2 202.9  0.7      19.6   310   F  1   3555

19 08 36  J2025+0316   21 45 22  56.7 218.6  1.3      32.5     7   1 11   3555  19 08 16
19 13 26  =2022+031    21 50 12  56.1 220.4  1.4      34.0   290   F  1   5619

19 16 26  J1907+0127   21 53 13  41.1 241.5  2.8      49.2   148   1 11   5619  19 16 06
19 17 06  ---          21 53 53  40.9 241.6  2.8      49.2    40   F  1   6019

19 17 15  SS433        21 54 02  44.1 244.4  2.7      51.1     1   1 11   6019  19 17 06
19 18 15  ---          21 55 03  43.9 244.6  2.7      51.3    60   F  1   6481

19 18 18  1910+052     21 55 05  44.3 244.7  2.7      51.4     0   1 11   6481  19 18 15
19 19 18  ---          21 56 06  44.1 244.9  2.7      51.5    60   F  1   6900

19 19 28  J1907+0127   21 56 16  40.5 242.2  2.8      49.6     1   1 11   6900  19 19 18
19 20 28  ---          21 57 16  40.3 242.4  2.8      49.7    60   F  1   7368

19 20 37  SS433        21 57 25  43.4 245.1  2.8      51.6     1   1 11   7368  19 20 28
19 21 37  ---          21 58 26  43.2 245.3  2.8      51.7    60   F  1   7831

19 21 40  1910+052     21 58 28  43.6 245.4  2.8      51.8     0   1 11   7831  19 21 37
19 22 40  ---          21 59 29  43.4 245.6  2.8      51.9    60   F  1   8250

19 22 50  J1907+0127   21 59 39  39.8 242.9  2.9      50.0     1   1 11   8250  19 22 40
19 23 50  ---          22 00 39  39.7 243.1  2.9      50.1    60   F  1   8718

19 24 00  SS433        22 00 48  42.7 245.8  2.8      52.0     1   1 11   8718  19 23 50
19 25 00  ---          22 01 49  42.5 246.0  2.8      52.1    60   F  1   9181

19 25 03  1910+052     22 01 51  42.9 246.1  2.8      52.2     0   1 11   9181  19 25 00
19 26 03  ---          22 02 52  42.7 246.3  2.8      52.3    60   F  1   9600

19 26 13  J1907+0127   22 03 02  39.2 243.6  2.9      50.4     1   1 11   9600  19 26 03
19 27 13  ---          22 04 02  39.0 243.8  2.9      50.5    60   F  1  10068

19 27 22  SS433        22 04 11  42.1 246.5  2.9      52.4     1   1 11  10068  19 27 13
19 28 22  ---          22 05 12  41.9 246.7  2.9      52.5    60   F  1  10530
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  13 Feb 2000   Day  44 ---

19 28 25  1910+052     22 05 14  42.3 246.8  2.9      52.6     0   1 11  10530  19 28 22
19 29 25  ---          22 06 15  42.1 247.0  2.9      52.7    60   F  1  10949

19 29 35  J1907+0127   22 06 25  38.5 244.3  3.0      50.8     1   1 11  10949  19 29 25
19 30 35  ---          22 07 25  38.4 244.5  3.0      51.0    60   F  1  11417

19 30 45  SS433        22 07 34  41.4 247.2  2.9      52.8     1   1 11  11417  19 30 35
19 41 25  ---          22 18 16  39.3 249.3  3.1      53.9   640   F  1  15746

19 44 25  SS433        22 21 17  38.7 249.8  3.2      54.2   177   1 12  15746  19 44 05
20 28 05  ---          23 05 04  29.6 257.2  3.9      57.4  2620   R  1   1854

20 31 05  SS433        23 08 04  29.0 257.7  3.9      57.6   177   1 13   1854  20 30 45
21 14 45  ---          23 51 51  19.7 264.0  4.7      59.2  2620   F  1  15746

21 15 41  J2101+0341   23 52 48  41.5 244.9  2.9      51.3    11   1 14  15746  21 15 21
21 20 51  =2059+034    23 57 59  40.5 246.0  2.9      51.9   310   R  1  17254

21 21 53  3C454.3      23 59 00  69.2 229.4  1.1      42.9     2   1 14  17254  21 20 51
21 29 53  ---          00 07 02  67.9 233.2  1.2      45.8   480   R  1  13645


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v18cm-128-4-2.set
   Matches group v20cm_2 in /vlbi/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    9         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=  2400.00  2400.00  2400.00  2400.00
   Net SB=        U        U        U        U
   Pol.  =     RCP      LCP      RCP      LCP 
   BBC   =        1        2        3        4
   BBC SB=        L        L        L        L
   IF    =       A        C        A        C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=   1654.99  1654.99  1662.99  1662.99
   BBC fr=    745.01   745.01   737.01   737.01
   Bandwd=     8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=    10    10  6010  6010     0     0     0     0
    PCALFR2=    10    10  6010  6010     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- The anomalous equatorial emission region of SS433
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SS433             19 09 21.270093   * 19 11 49.555000     19 11 48.006828 
                     04 53 53.11612    * 04 58 56.94900      04 58 53.05770 
                     From catalog imbedded in main SCHED input file.

 * J1907+0127        19 04 39.789145   * 19 07 11.996900     19 07 10.449025 
                     01 22 24.61197    * 01 27 08.97400      01 27 05.79524 
                     From catalog imbedded in main SCHED input file.

 * 1910+052          19 10 26.308007   * 19 12 54.247000     19 12 52.696653 
                     05 12 51.18616    * 05 17 59.52000      05 17 55.55975 
                     From catalog imbedded in main SCHED input file.

   J1407+2827        14 04 45.615152   * 14 07 00.394411     14 07 00.325472 
 * 1404+286          28 41 29.23491    * 28 27 14.68994      28 27 05.11639 
   J1407+28          /vlbi/sched/catalogs/sources.vlba
   OQ208             USNO - Ref Frame 1998-6, Eubanks June 1998

 * J2025+0316        20 22 38.861003   * 20 25 09.626900     20 25 07.907210 
 + 2022+031          03 06 55.70001    * 03 16 44.42000      03 16 39.61050 
   J2025+03          /vlbi/sched/catalogs/sources.vlba
                     VLA Calibrator Source List

 * J2101+0341        20 59 08.011544   * 21 01 38.834164     21 01 37.081386 
 + 2059+034          03 29 41.48334    * 03 41 31.32060      03 41 25.82148 
   J2101+03          /vlbi/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998

   J2253+1608        22 51 29.519701   * 22 53 57.747900     22 53 56.126028 
   2251+158          15 52 54.35017    * 16 08 53.56300      16 08 47.77958 
 * 3C454.3           /vlbi/sched/catalogs/sources.vlba
   J2253+16          VLA Calibrator Source List



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SS433               42.4
   J1907+0127          42.1
   1910+052            42.4
   1404+286           117.9
   J2025+0316          26.1
   2022+031            26.1
   J2101+0341          20.4
   2059+034            20.4
   3C454.3             34.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

