  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The anomalous equatorial emission region of SS433
 Exp. Code:  GP025B  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 1 July 1999                        

PI:       Zsolt Paragi                                                    

Address:  FOMI Satellite Geodetic Observatory                             
          P. O. Box 546                                                   
          H-1373 Budapest                                                 
          HUNGARY                                                         

Phone:    36 27 374 980                                                   
EMAIL:    paragi@sgo.fomi.hu                                              
Fax:      36 27 374 982                                                   
Phone during observation: 36 27 374 980                                   

Observing mode: Continuum 18 cm; Recording mode: 128-4-2 (VLBA/MKIV).     

Notes:    Global VLBI monitoring at 18cm. Observe RCP+LCP, but we         
          do not need crosspol. Fringe-finders: OQ208, 3C454.3            
          Send logs and calibration information to Zsolt Paragi.          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

 Next scan frequencies:  1654.99  1654.99  1662.99  1662.99
 Next BBC frequencies:    745.01   745.01   737.01   737.01
 Next scan bandwidths:      8.00     8.00     8.00     8.00

10 34 35  SS433        13 37 33   8.1  89.0 -5.6     -59.7     0   1  1      0  10 34 25
10 45 15  ---          13 48 15  10.4  90.3 -5.4     -59.7   640   F  1   4334

10 45 25  SS433        13 48 25  10.4  90.4 -5.4     -59.7     8   1  1   4334  10 45 15
10 56 05  ---          13 59 07  12.7  91.7 -5.2     -59.7   640   F  1   8669

10 59 05  SS433        14 02 07  13.4  92.1 -5.2     -59.7   177   1  1   8669  10 58 45
11 20 45  ---          14 23 51  18.0  95.0 -4.8     -59.4  1300   F  1  17469

11 23 45  SS433        14 26 51  18.7  95.4 -4.7     -59.3   177   1  2  17469  11 23 25
11 45 25  ---          14 48 35  23.3  98.3 -4.4     -58.7  1300   R  1   8669

11 48 25  J1907+0127   14 51 35  23.0 102.7 -4.3     -57.1   175   1  2   8669  11 48 05
11 49 05  ---          14 52 15  23.2 102.8 -4.2     -57.1    40   R  1   8269

11 49 51  SS433        14 53 01  24.2  99.0 -4.3     -58.6    41   1  2   8269  11 49 05
11 50 51  ---          14 54 01  24.5  99.1 -4.3     -58.5    60   R  1   7567

11 51 02  1910+052     14 54 12  24.4  98.7 -4.3     -58.7     9   1  2   7567  11 50 51
11 52 02  ---          14 55 12  24.6  98.8 -4.3     -58.6    60   R  1   7092

11 52 54  J1907+0127   14 56 04  24.0 103.4 -4.2     -56.9    47   1  2   7092  11 52 02
11 53 54  ---          14 57 05  24.2 103.5 -4.2     -56.8    60   R  1   6345

11 54 39  SS433        14 57 50  25.3  99.7 -4.2     -58.4    41   1  2   6345  11 53 54
11 55 39  ---          14 58 50  25.5  99.8 -4.2     -58.3    60   R  1   5644

11 55 51  1910+052     14 59 01  25.5  99.4 -4.2     -58.5     9   1  2   5644  11 55 39
11 56 51  ---          15 00 02  25.7  99.5 -4.2     -58.5    60   R  1   5169

11 57 43  J1907+0127   15 00 54  25.0 104.1 -4.1     -56.6    47   1  2   5169  11 56 51
11 58 43  ---          15 01 54  25.2 104.2 -4.1     -56.5    60   R  1   4421

11 59 28  SS433        15 02 39  26.3 100.4 -4.2     -58.2    40   1  2   4421  11 58 43
12 00 28  ---          15 03 39  26.5 100.5 -4.1     -58.1    60   R  1   3721

12 00 39  1910+052     15 03 51  26.5 100.1 -4.2     -58.3     9   1  2   3721  12 00 28
12 01 39  ---          15 04 51  26.7 100.2 -4.1     -58.3    60   R  1   3246
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

12 02 31  J1907+0127   15 05 43  26.0 104.8 -4.0     -56.3    47   1  2   3246  12 01 39
12 03 31  ---          15 06 43  26.2 105.0 -4.0     -56.2    60   R  1   2498

12 04 16  SS433        15 07 28  27.3 101.1 -4.1     -58.0    40   1  2   2498  12 03 31
12 05 16  ---          15 08 28  27.5 101.2 -4.1     -57.9    60   R  1   1798

12 05 27  1910+052     15 08 40  27.5 100.8 -4.1     -58.1     9   1  2   1798  12 05 16
12 06 27  ---          15 09 40  27.7 100.9 -4.1     -58.0    60   R  1   1323

12 07 19  J1907+0127   15 10 32  27.0 105.6 -3.9     -56.0    47   1  2   1323  12 06 27
12 08 19  ---          15 11 32  27.2 105.7 -3.9     -55.9    60   R  1    576

12 09 04  SS433        15 12 17  28.3 101.8 -4.0     -57.7    40   1  3    576  12 08 19
12 32 04  ---          15 35 21  33.1 105.4 -3.6     -56.4  1380   F  1   8923

12 34 04  SS433        15 37 21  33.6 105.8 -3.6     -56.2   117   1  3   8923  12 33 44
12 44 44  ---          15 48 03  35.8 107.6 -3.4     -55.4   640   F  1  13323

12 48 00  J2101+0341   15 51 19  12.6  93.2 -5.2     -59.4   147   1  4  13323  12 47 40
12 58 40  =2059+034    16 02 01  14.9  94.6 -5.0     -59.3   640   R  1  17477

13 01 55  J1907+0127   16 05 16  38.0 115.2 -3.0     -51.1   147   1  4  17477  13 01 35
13 02 35  ---          16 05 57  38.2 115.3 -3.0     -51.1    40   R  1  17077

13 03 19  SS433        16 06 41  39.5 111.0 -3.1     -53.7    39   1  4  17077  13 02 35
13 04 19  ---          16 07 41  39.7 111.2 -3.1     -53.6    60   R  1  16384

13 04 30  1910+052     16 07 52  39.8 110.7 -3.1     -53.9     9   1  4  16384  13 04 19
13 05 30  ---          16 08 52  40.0 110.9 -3.1     -53.8    60   R  1  15909

13 06 21  J1907+0127   16 09 44  38.9 116.1 -3.0     -50.6    46   1  4  15909  13 05 30
13 07 21  ---          16 10 44  39.1 116.3 -2.9     -50.5    60   R  1  15166

13 08 05  SS433        16 11 28  40.5 111.9 -3.0     -53.3    39   1  4  15166  13 07 21
13 09 05  ---          16 12 28  40.7 112.1 -3.0     -53.1    60   R  1  14473

13 09 17  1910+052     16 12 40  40.7 111.6 -3.0     -53.5     9   1  4  14473  13 09 05
13 10 17  ---          16 13 40  40.9 111.8 -3.0     -53.4    60   R  1  13998

13 11 08  J1907+0127   16 14 31  39.8 117.1 -2.9     -50.0    46   1  4  13998  13 10 17
13 12 08  ---          16 15 31  40.0 117.3 -2.9     -49.9    60   R  1  13255
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

13 12 52  SS433        16 16 15  41.5 112.9 -2.9     -52.7    39   1  4  13255  13 12 08
13 13 52  ---          16 17 16  41.7 113.1 -2.9     -52.6    60   R  1  12563

13 14 03  1910+052     16 17 27  41.7 112.5 -2.9     -52.9     9   1  4  12563  13 13 52
13 15 03  ---          16 18 27  41.9 112.7 -2.9     -52.8    60   R  1  12088

13 15 54  J1907+0127   16 19 18  40.7 118.1 -2.8     -49.4    46   1  4  12088  13 15 03
13 16 54  ---          16 20 19  40.9 118.3 -2.8     -49.3    60   R  1  11346

13 17 38  SS433        16 21 02  42.4 113.8 -2.8     -52.2    39   1  4  11346  13 16 54
13 18 38  ---          16 22 03  42.6 114.0 -2.8     -52.1    60   R  1  10654

13 18 49  1910+052     16 22 14  42.6 113.5 -2.8     -52.4     9   1  4  10654  13 18 38
13 19 49  ---          16 23 14  42.8 113.7 -2.8     -52.3    60   R  1  10179

13 20 41  J1907+0127   16 24 06  41.6 119.1 -2.7     -48.7    46   1  4  10179  13 19 49
13 21 41  ---          16 25 06  41.8 119.4 -2.7     -48.6    60   R  1   9437

13 23 41  SS433        16 27 06  43.6 115.1 -2.7     -51.4   114   1  4   9437  13 23 21
13 45 21  ---          16 48 50  47.7 120.1 -2.4     -48.4  1300   R  1    637

13 47 21  SS433        16 50 50  48.1 120.6 -2.3     -48.0   117   1  5    637  13 47 01
14 09 01  ---          17 12 33  52.0 126.4 -2.0     -44.0  1300   F  1   8163

14 12 01  SS433        17 15 34  52.5 127.3 -1.9     -43.4   177   1  5   8163  14 11 41
14 22 41  ---          17 26 16  54.3 130.6 -1.8     -40.9   640   F  1  12563

14 22 43  SS433        17 26 18  54.3 130.7 -1.8     -40.9     0   1  6  12563  14 22 41
14 53 43  ---          17 57 23  58.9 142.0 -1.2     -32.1  1860   R  1  10223

14 56 43  J1907+0127   18 00 23  56.8 148.4 -1.1     -26.8   174   1  6  10223  14 56 23
14 57 23  ---          18 01 04  56.9 148.6 -1.1     -26.6    40   R  1   9823

14 57 32  SS433        18 01 13  59.4 143.6 -1.2     -30.9     2   1  6   9823  14 57 23
14 58 32  ---          18 02 13  59.6 144.0 -1.2     -30.5    60   R  1   9361

14 58 35  1910+052     18 02 16  59.7 143.2 -1.2     -31.2     0   1  6   9361  14 58 32
14 59 35  ---          18 03 16  59.8 143.7 -1.2     -30.8    60   R  1   8942

14 59 45  J1907+0127   18 03 26  57.1 149.6 -1.1     -25.8     3   1  6   8942  14 59 35
15 00 45  ---          18 04 26  57.2 150.0 -1.0     -25.5    60   R  1   8474
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

15 00 55  SS433        18 04 36  59.9 145.0 -1.1     -29.7     2   1  6   8474  15 00 45
15 01 55  ---          18 05 36  60.0 145.4 -1.1     -29.3    60   R  1   8011

15 01 57  1910+052     18 05 39  60.1 144.7 -1.1     -30.0     0   1  6   8011  15 01 55
15 02 57  ---          18 06 39  60.3 145.1 -1.1     -29.6    60   R  1   7593

15 03 08  J1907+0127   18 06 49  57.5 151.0 -1.0     -24.6     3   1  6   7593  15 02 57
15 04 08  ---          18 07 49  57.6 151.5 -1.0     -24.3    60   R  1   7125

15 04 17  SS433        18 07 59  60.3 146.5 -1.1     -28.5     2   1  6   7125  15 04 08
15 05 17  ---          18 08 59  60.4 146.9 -1.0     -28.1    60   R  1   6662

15 05 20  1910+052     18 09 02  60.5 146.2 -1.1     -28.8     0   1  6   6662  15 05 17
15 06 20  ---          18 10 02  60.7 146.6 -1.0     -28.4    60   R  1   6244

15 06 30  J1907+0127   18 10 12  57.8 152.5 -0.9     -23.4     3   1  6   6244  15 06 20
15 07 30  ---          18 11 12  57.9 152.9 -0.9     -23.1    60   R  1   5775

15 07 39  SS433        18 11 22  60.7 148.0 -1.0     -27.2     2   1  6   5775  15 07 30
15 08 39  ---          18 12 22  60.8 148.4 -1.0     -26.9    60   R  1   5313

15 08 42  1910+052     18 12 25  60.9 147.7 -1.0     -27.5     0   1  6   5313  15 08 39
15 09 42  ---          18 13 25  61.1 148.1 -1.0     -27.1    60   R  1   4894

15 09 52  J1907+0127   18 13 35  58.2 153.9 -0.9     -22.2     2   1  6   4894  15 09 42
15 10 52  ---          18 14 35  58.3 154.4 -0.9     -21.8    60   R  1   4426

15 11 02  SS433        18 14 45  61.0 149.5 -1.0     -26.0     2   1  7   4426  15 10 52
15 32 42  ---          18 36 28  63.0 160.3 -0.6     -16.9  1300   F  1   4303

15 34 42  J2101+0341   18 38 29  46.8 121.5 -2.4     -47.3    86   1  7   4303  15 34 22
15 39 52  =2059+034    18 43 39  47.8 122.8 -2.3     -46.5   310   F  1   6503

15 40 11  J2025+0316   18 43 59  53.7 133.9 -1.7     -38.4     5   1  7   6503  15 39 52
15 45 01  =2022+031    18 48 50  54.4 135.6 -1.6     -37.1   290   F  1   8565

15 46 01  SS433        18 49 50  63.8 167.5 -0.4     -10.8    37   1  8   8565  15 45 01
16 18 41  ---          19 22 35  64.2 186.2  0.2       5.3  1960   R  1  13168

16 21 41  SS433        19 25 36  64.1 187.9  0.2       6.8   177   1  9  13168  16 21 21
17 05 21  ---          20 09 23  61.0 210.7  1.0      26.2  2620   F  1   4432
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

17 08 21  J1907+0127   20 12 23  57.0 211.0  1.1      26.3   170   1  9   4432  17 08 01
17 09 01  ---          20 13 03  56.9 211.3  1.1      26.5    40   F  1   4832

17 09 10  SS433        20 13 13  60.6 212.4  1.0      27.6     0   1  9   4832  17 09 01
17 10 10  ---          20 14 13  60.4 212.9  1.0      28.0    60   F  1   5294

17 10 13  1910+052     20 14 16  60.8 212.7  1.0      27.9     0   1  9   5294  17 10 10
17 11 13  ---          20 15 16  60.7 213.2  1.0      28.2    60   F  1   5713

17 11 24  J1907+0127   20 15 26  56.6 212.2  1.1      27.3     0   1  9   5713  17 11 13
17 12 24  ---          20 16 26  56.5 212.6  1.2      27.7    60   F  1   6181

17 12 33  SS433        20 16 36  60.2 214.0  1.1      28.8     0   1  9   6181  17 12 24
17 13 33  ---          20 17 36  60.0 214.4  1.1      29.2    60   F  1   6644

17 13 36  1910+052     20 17 39  60.4 214.2  1.1      29.1     0   1  9   6644  17 13 33
17 14 36  ---          20 18 39  60.3 214.7  1.1      29.5    60   F  1   7063

17 14 46  J1907+0127   20 18 49  56.2 213.6  1.2      28.4     0   1  9   7063  17 14 36
17 15 46  ---          20 19 49  56.1 214.0  1.2      28.8    60   F  1   7531

17 15 55  SS433        20 19 59  59.7 215.4  1.1      30.0     0   1  9   7531  17 15 46
17 16 55  ---          20 20 59  59.6 215.8  1.2      30.4    60   F  1   7994

17 16 58  1910+052     20 21 02  60.0 215.7  1.1      30.3     0   1  9   7994  17 16 55
17 17 58  ---          20 22 02  59.9 216.2  1.2      30.6    60   F  1   8413

17 18 08  J1907+0127   20 22 12  55.8 214.9  1.3      29.5     0   1  9   8413  17 17 58
17 19 08  ---          20 23 12  55.7 215.3  1.3      29.8    60   F  1   8881

17 19 18  SS433        20 23 22  59.3 216.8  1.2      31.2     0   1  9   8881  17 19 08
17 20 18  ---          20 24 22  59.2 217.3  1.2      31.5    60   F  1   9344

17 20 21  1910+052     20 24 25  59.6 217.2  1.2      31.5     0   1  9   9344  17 20 18
17 21 21  ---          20 25 25  59.5 217.6  1.2      31.8    60   F  1   9762

17 21 31  J1907+0127   20 25 35  55.4 216.2  1.3      30.6     0   1  9   9762  17 21 21
17 22 31  ---          20 26 35  55.3 216.6  1.3      30.9    60   F  1  10230

17 22 40  SS433        20 26 45  58.9 218.2  1.2      32.3     0   1 10  10230  17 22 31
17 44 20  ---          20 48 28  55.7 226.4  1.6      38.7  1300   R  1  16240
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

17 47 20  SS433        20 51 29  55.2 227.4  1.7      39.5   177   1 11  16240  17 47 00
18 31 00  ---          21 35 16  47.6 240.0  2.4      48.4  2620   F  1   1360

18 33 00  J2101+0341   21 37 16  61.8 199.1  0.6      16.4    90   1 11   1360  18 32 40
18 38 10  =2059+034    21 42 27  61.4 201.7  0.7      18.6   310   F  1   3560

18 38 30  J2025+0316   21 42 47  57.1 217.6  1.3      31.7     7   1 11   3560  18 38 10
18 43 20  =2022+031    21 47 38  56.4 219.5  1.4      33.2   290   F  1   5624

18 46 20  J1907+0127   21 50 38  41.6 240.9  2.7      48.8   148   1 11   5624  18 46 00
18 47 00  ---          21 51 18  41.4 241.1  2.7      48.9    40   F  1   6024

18 47 09  SS433        21 51 28  44.6 243.8  2.7      50.8     1   1 11   6024  18 47 00
18 48 09  ---          21 52 28  44.4 244.0  2.7      50.9    60   F  1   6486

18 48 12  1910+052     21 52 31  44.8 244.1  2.7      51.0     0   1 11   6486  18 48 09
18 49 12  ---          21 53 31  44.6 244.4  2.7      51.2    60   F  1   6905

18 49 22  J1907+0127   21 53 41  41.0 241.6  2.8      49.2     1   1 11   6905  18 49 12
18 50 22  ---          21 54 41  40.8 241.8  2.8      49.3    60   F  1   7374

18 50 32  SS433        21 54 51  43.9 244.5  2.7      51.2     1   1 11   7374  18 50 22
18 51 32  ---          21 55 51  43.7 244.7  2.7      51.4    60   F  1   7836

18 51 35  1910+052     21 55 54  44.1 244.9  2.7      51.5     0   1 11   7836  18 51 32
18 52 35  ---          21 56 54  43.9 245.1  2.7      51.6    60   F  1   8255

18 52 45  J1907+0127   21 57 04  40.3 242.3  2.8      49.7     1   1 11   8255  18 52 35
18 53 45  ---          21 58 04  40.2 242.5  2.8      49.8    60   F  1   8723

18 53 54  SS433        21 58 14  43.2 245.3  2.8      51.7     1   1 11   8723  18 53 45
18 54 54  ---          21 59 14  43.1 245.5  2.8      51.8    60   F  1   9186

18 54 57  1910+052     21 59 17  43.5 245.6  2.8      51.9     0   1 11   9186  18 54 54
18 55 57  ---          22 00 17  43.3 245.8  2.8      52.0    60   F  1   9605

18 56 07  J1907+0127   22 00 27  39.7 243.0  2.9      50.1     1   1 11   9605  18 55 57
18 57 07  ---          22 01 27  39.5 243.3  2.9      50.2    60   F  1  10073

18 57 17  SS433        22 01 37  42.6 246.0  2.8      52.1     1   1 11  10073  18 57 07
18 58 17  ---          22 02 37  42.4 246.2  2.8      52.2    60   F  1  10535
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2000   Day  51 ---

18 58 19  1910+052     22 02 40  42.8 246.3  2.8      52.3     0   1 11  10535  18 58 17
18 59 19  ---          22 03 40  42.6 246.5  2.8      52.4    60   F  1  10955

18 59 30  J1907+0127   22 03 50  39.0 243.7  2.9      50.5     1   1 11  10955  18 59 19
19 00 30  ---          22 04 50  38.9 243.9  3.0      50.6    60   F  1  11423

19 00 39  SS433        22 05 00  41.9 246.7  2.9      52.5     1   1 11  11423  19 00 30
19 11 19  ---          22 15 41  39.8 248.8  3.1      53.6   640   F  1  15752

19 14 19  SS433        22 18 42  39.2 249.4  3.1      53.9   177   1 12  15752  19 13 59
19 57 59  ---          23 02 29  30.2 256.8  3.8      57.2  2620   R  1   1848

20 00 59  SS433        23 05 30  29.5 257.3  3.9      57.4   177   1 13   1848  20 00 39
20 44 39  ---          23 49 17  20.3 263.6  4.6      59.1  2620   F  1  15752

20 45 36  J2101+0341   23 50 14  42.0 244.3  2.8      51.0    12   1 14  15752  20 45 16
20 50 46  =2059+034    23 55 25  41.0 245.4  2.9      51.6   310   R  1  17248

20 51 47  3C454.3      23 56 26  69.7 228.1  1.0      41.8     2   1 14  17248  20 50 46
20 59 47  ---          00 04 28  68.3 232.0  1.2      44.9   480   R  1  13640


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v18cm-128-4-2.set
   Matches group v20cm_2 in /vlbi/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    9         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=  2400.00  2400.00  2400.00  2400.00
   Net SB=        U        U        U        U
   Pol.  =     RCP      LCP      RCP      LCP 
   BBC   =        1        2        3        4
   BBC SB=        L        L        L        L
   IF    =       A        C        A        C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=   1654.99  1654.99  1662.99  1662.99
   BBC fr=    745.01   745.01   737.01   737.01
   Bandwd=     8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=    10    10  6010  6010     0     0     0     0
    PCALFR2=    10    10  6010  6010     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- The anomalous equatorial emission region of SS433
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SS433             19 09 21.270093   * 19 11 49.555000     19 11 48.190154 
                     04 53 53.11612    * 04 58 56.94900      04 58 52.26983 
                     From catalog imbedded in main SCHED input file.

 * J1907+0127        19 04 39.789145   * 19 07 11.996900     19 07 10.636737 
                     01 22 24.61197    * 01 27 08.97400      01 27 05.10766 
                     From catalog imbedded in main SCHED input file.

 * 1910+052          19 10 26.308007   * 19 12 54.247000     19 12 52.879245 
                     05 12 51.18616    * 05 17 59.52000      05 17 54.76396 
                     From catalog imbedded in main SCHED input file.

   J1407+2827        14 04 45.615152   * 14 07 00.394411     14 07 00.565362 
 * 1404+286          28 41 29.23491    * 28 27 14.68994      28 27 04.62698 
   J1407+28          /vlbi/sched/catalogs/sources.vlba
   OQ208             USNO - Ref Frame 1998-6, Eubanks June 1998

 * J2025+0316        20 22 38.861003   * 20 25 09.626900     20 25 08.047438 
 + 2022+031          03 06 55.70001    * 03 16 44.42000      03 16 39.02953 
   J2025+03          /vlbi/sched/catalogs/sources.vlba
                     VLA Calibrator Source List

 * J2101+0341        20 59 08.011544   * 21 01 38.834164     21 01 37.196583 
 + 2059+034          03 29 41.48334    * 03 41 31.32060      03 41 25.30211 
   J2101+03          /vlbi/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998

   J2253+1608        22 51 29.519701   * 22 53 57.747900     22 53 56.155138 
   2251+158          15 52 54.35017    * 16 08 53.56300      16 08 47.01395 
 * 3C454.3           /vlbi/sched/catalogs/sources.vlba
   J2253+16          VLA Calibrator Source List



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SS433               47.8
   J1907+0127          47.8
   1910+052            47.7
   1404+286           122.8
   J2025+0316          30.4
   2022+031            30.4
   J2101+0341          23.1
   2059+034            23.1
   3C454.3             29.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

