!*  Schedule for VLBA_FD   *!
!*  Experiment GX006    *!
!* Schedule Version:       6.00 *!
!* Processed by SCHED version: Release of 1 July 1999 *!
!* PI:       Emily Xanthopoulos *!
!* Address:  NRAL Jodrell Bank *!
!*           Macclesfield, Cheshire *!
!*           SK11, 9DL *!
!*            United Kingdom *!
!* Phone:     +44 1477 572635 *!
!* EMAIL:    emily@jb.man.ac.uk *!
!* Fax:       +44 1477- 571618 *!
!* Phone during observation:  +44 1477 572635 *!
!* Observing mode: Continuum *!
!* Notes: *!
!*           using 3 fringe finders *!
!*  *!
!*  *!
!*  Start at 01h00m00s     Sat, 2000 Feb 12  Day of year   43   *!
program=GX006   
autoallocate=on
autoreverse=on

!* The first scan is preceeded by a setup scan *!
!* that ends at the start time of the first scan  *!

!* --- Scan from 01h00m00s to 01h05m00s   Sat, 2000 Feb 12 --- *!
sname='DA193'  ra=05h55m30.806000s  dec= 39d48'49.16600"  qual=999  calib='C'
maxcaltime= 120
fe=(1,20cm),(3,20cm)
fexfer=(2,norm)
noise=(1,low-s),(2,low-s),(3,low-s),(4,low-s)
synth=( 1,15.4),( 2, 2.4),( 3,15.4)
logging=STANDARD
nchan= 4
format=VLBA1:4
barrel=roll_auto
ifdistr=(1,0),(2,0),(3,0),(4,0)
baseband=(1,1),(2,2),(3,3),(4,4)
ifchan=(1,A),(2,C),(3,A),(4,C)
sideband=(1,L),(2,L),(3,L),(4,L)
bits=(1,2),(2,2),(3,2),(4,2)
period=(1,1),(2,1),(3,1),(4,1)
level=(1,-1),(2,-1),(3,-1),(4,-1)
azcolim=   0.00  elcolim=   0.00
bbsynth=( 1,749.51),( 2,749.51),( 3,741.51),( 4,741.51)
bbfilter=(1,8M),(2,8M),(3,8M),(4,8M)
pcal=1MHZ
pcalxbit1=(1,S1),(2,S3),(3,S1),(4,S3),(5,S1),(6,S2),(7,S3),(8,S4)
pcalxbit2=(1,S2),(2,S4),(3,S2),(4,S4),(5,M1),(6,M2),(7,M3),(8,M4)
pcalxfreq1=(1,510),(2,510),(3,6510),(4,6510),(5,0),(6,0),(7,0),(8,0)
pcalxfreq2=(1,510),(2,510),(3,6510),(4,6510),(5,0),(6,0),(7,0),(8,0)
samplerate=16M
tape=(1,STOP)   write=(1,off)
  date = 2000Feb12
stop=01h00m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=01h05m00s   !NEXT!

!* --- Scan from 01h50m00s to 02h34m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=01h50m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=02h34m00s   !NEXT!

!* --- Scan from 02h37m00s to 03h21m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=02h37m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=03h21m00s   !NEXT!

!* --- Scan from 03h24m00s to 04h02m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=03h24m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h02m00s   !NEXT!

!* --- Scan from 04h05m00s to 04h08m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=04h05m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h08m00s   !NEXT!

!* --- Scan from 04h11m00s to 04h14m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=04h11m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=04h14m00s   !NEXT!

!* --- Scan from 04h17m00s to 05h01m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=04h17m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h01m00s   !NEXT!

!* --- Scan from 05h04m00s to 05h48m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=05h04m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h48m00s   !NEXT!

!* --- Scan from 05h51m00s to 05h54m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=05h51m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=05h54m00s   !NEXT!

!* --- Scan from 05h57m00s to 06h00m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=05h57m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h00m00s   !NEXT!

!* --- Scan from 06h03m00s to 06h35m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=06h03m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h35m00s   !NEXT!

!* --- Scan from 06h38m00s to 06h41m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=06h38m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h41m00s   !NEXT!

!* --- Scan from 06h44m00s to 06h47m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=06h44m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=06h47m00s   !NEXT!

!* --- Scan from 06h50m00s to 07h28m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=06h50m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h28m00s   !NEXT!

!* --- Scan from 07h31m00s to 07h34m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=07h31m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h34m00s   !NEXT!

!* --- Scan from 07h37m00s to 07h40m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=07h37m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h40m00s   !NEXT!

!* --- Scan from 07h51m00s to 07h54m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=07h51m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=07h54m00s   !NEXT!

!* --- Scan from 08h05m00s to 08h08m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=08h05m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=08h08m00s   !NEXT!

!* --- Scan from 08h19m00s to 08h24m00s   Sat, 2000 Feb 12 --- *!
sname='4C39.25'  ra=09h27m03.014000s  dec= 39d02'20.85200"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=08h19m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=08h24m00s   !NEXT!

!* --- Scan from 08h35m00s to 09h02m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=08h35m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h02m00s   !NEXT!

!* --- Scan from 09h13m00s to 09h16m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=09h13m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h16m00s   !NEXT!

!* --- Scan from 09h27m00s to 09h30m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=09h27m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=09h30m00s   !NEXT!

!* --- Scan from 09h41m00s to 10h25m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=09h41m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=10h25m00s   !NEXT!

!* --- Scan from 10h36m00s to 11h20m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=10h36m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=11h20m00s   !NEXT!

!* --- Scan from 11h31m00s to 11h36m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=11h31m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=11h36m00s   !NEXT!

!* --- Scan from 11h47m00s to 11h52m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=11h47m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=11h52m00s   !NEXT!

!* --- Scan from 12h03m00s to 12h27m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=12h03m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=12h27m00s   !NEXT!

!* --- Scan from 12h38m00s to 12h43m00s   Sat, 2000 Feb 12 --- *!
sname='1038+064'  ra=10h41m17.162900s  dec= 06d10'16.92500"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=12h38m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=12h43m00s   !NEXT!

!* --- Scan from 12h54m00s to 12h59m00s   Sat, 2000 Feb 12 --- *!
sname='1130+009'  ra=11h33m20.055766s  dec= 00d40'52.83795"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=12h54m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=12h59m00s   !NEXT!

!* --- Scan from 13h10m00s to 13h54m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=13h10m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=13h54m00s   !NEXT!

!* --- Scan from 14h05m00s to 14h44m00s   Sat, 2000 Feb 12 --- *!
sname='1030+074'  ra=10h33m34.024600s  dec= 07d11'26.12200"  qual=999  calib='T'
tape=(1,STOP)   write=(1,off)
stop=14h05m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=14h44m00s   !NEXT!

!* --- Scan from 14h55m00s to 15h00m00s   Sat, 2000 Feb 12 --- *!
sname='3C345'  ra=16h42m58.809600s  dec= 39d48'36.99200"  qual=999  calib='C'
tape=(1,STOP)   write=(1,off)
stop=14h55m00s   !NEXT!        
qual=  0
tape=(1,+RUN)  write=(1,on)
stop=15h00m00s   !NEXT!

tape=(1,STOP)    write=(1,off)   dur=0s 
stop=15h00m05s  !NEXT! 
     !QUIT! 
