  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Probing the disc-jet coupling in the neutron star binary Sco X-1
 Exp. Code:  gm074b  


Schedule Version:       2.30
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Sara Motta

Address:  University of Oxford
          Department of Physics, Astrophysics
          Denys Wilkinson Building, Keble Road
          Oxford OX1 3RH, UK

Phone:    +44-1865-283133
EMAIL:    sara.motta@physics.ox.ac.uk
Fax:
Phone during observation: +61-4-8848-4825

Observing mode: LBA,EVN,VLBA 8.4 GHz continuum

Notes:    Target (phase ref):                 Sco X-1 (J1628-1415)
          In-beam cal:                                       NEIBC
          Fringe finders: J1229+0203,1921-293,J1642+3948,J1800+3848,J1549+0237,J1256-0547,J1743-0350,J2253+1608
          ATCA phasing source:          J1558-1409, Fringe Finders

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

 Next scan frequencies:  8331.00  8331.00  8363.00  8363.00  8395.00  8395.00  8427.00  8427.00
 Next BBC frequencies:    731.00   731.00   763.00   763.00   795.00   795.00   827.00   827.00
 Next scan bandwidths:     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00

08 00 00  J1642+3948   11 15 56  24.8  56.9 -5.5     -69.8     0        0   08 00 00
08 05 10  =1641+399    11 21 07  25.7  57.3 -5.4     -70.4   310       40   08 00 01

08 05 50  J1628-1415   11 21 47   3.5 108.9 -5.1     -57.1   -12       40   08 06 02
08 10 00  =1625-141    11 25 58   4.4 109.5 -5.1     -56.8   238       71   08 05 51

08 10 00  SCOX1OFF     11 25 58   5.4 111.8 -4.9     -56.1   -10       71   08 10 10
08 13 30  ---          11 29 28   6.1 112.3 -4.9     -55.8   200       96   08 10 01

08 13 30  J1628-1415   11 29 28   5.1 109.9 -5.0     -56.6   -10       96   08 13 40
08 14 50  =1625-141    11 30 48   5.4 110.1 -5.0     -56.5    70      105   08 13 31

08 14 50  SCOX1OFF     11 30 48   6.4 112.5 -4.8     -55.7   -10      105   08 15 00
08 18 20  ---          11 34 19   7.1 112.9 -4.8     -55.4   200      131   08 14 51

08 19 00  J1628-1415   11 34 59   6.2 110.7 -4.9     -56.2    30      131   08 19 00
08 20 10  =1625-141    11 36 09   6.4 110.8 -4.9     -56.1    70      140   08 19 01

08 20 10  SCOX1OFF     11 36 09   7.4 113.2 -4.7     -55.2   -10      140   08 20 20
08 23 40  ---          11 39 40   8.1 113.7 -4.7     -54.9   200      166   08 20 11

08 23 40  J1628-1415   11 39 40   7.1 111.3 -4.8     -55.8   -10      166   08 23 50
08 25 00  =1625-141    11 41 00   7.4 111.5 -4.8     -55.7    70      175   08 23 41

08 25 00  SCOX1OFF     11 41 00   8.4 113.9 -4.7     -54.8   -10      175   08 25 10
08 28 30  ---          11 44 31   9.1 114.4 -4.6     -54.5   200      201   08 25 01

08 28 30  J1628-1415   11 44 31   8.1 112.0 -4.8     -55.4   -10      201   08 28 40
08 29 50  =1625-141    11 45 51   8.4 112.2 -4.7     -55.3    70      210   08 28 31

08 29 50  SCOX1OFF     11 45 51   9.3 114.5 -4.6     -54.4   -10      210   08 30 00
08 33 20  ---          11 49 22  10.0 115.0 -4.5     -54.1   200      235   08 29 51

08 34 00  J1628-1415   11 50 02   9.2 112.8 -4.7     -55.0    30      235   08 34 00
08 35 10  =1625-141    11 51 12   9.4 112.9 -4.6     -54.9    70      244   08 34 01

08 35 10  SCOX1OFF     11 51 12  10.4 115.3 -4.5     -53.9   -10      244   08 35 20
08 38 40  ---          11 54 42  11.0 115.8 -4.4     -53.6   200      270   08 35 11

08 38 40  J1628-1415   11 54 42  10.1 113.4 -4.6     -54.6   -10      270   08 38 50
08 40 00  =1625-141    11 56 03  10.4 113.6 -4.6     -54.5    70      279   08 38 41
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

08 40 00  SCOX1OFF     11 56 03  11.3 116.0 -4.4     -53.4   -10      279   08 40 10
08 43 30  ---          11 59 33  12.0 116.5 -4.4     -53.1   200      305   08 40 01

08 43 30  J1628-1415   11 59 33  11.1 114.1 -4.5     -54.1   -10      305   08 43 40
08 44 50  =1625-141    12 00 53  11.3 114.3 -4.5     -54.0    70      314   08 43 31

08 44 50  SCOX1OFF     12 00 53  12.2 116.7 -4.3     -53.0   -10      314   08 45 00
08 48 20  ---          12 04 24  12.9 117.3 -4.3     -52.6   200      340   08 44 51

08 49 00  J1628-1415   12 05 04  12.2 114.9 -4.4     -53.6    30      340   08 49 00
08 50 10  =1625-141    12 06 14  12.4 115.1 -4.4     -53.5    70      349   08 49 01

08 50 10  SCOX1OFF     12 06 14  13.3 117.5 -4.2     -52.4   -10      349   08 50 20
08 53 40  ---          12 09 45  13.9 118.1 -4.2     -52.1   200      375   08 50 11

08 53 40  J1628-1415   12 09 45  13.1 115.6 -4.3     -53.2   -10      375   08 53 50
08 55 00  =1625-141    12 11 05  13.3 115.8 -4.3     -53.1    70      384   08 53 41

08 55 00  SCOX1OFF     12 11 05  14.2 118.3 -4.2     -51.9   -10      384   08 55 10
08 58 40  ---          12 14 46  14.9 118.8 -4.1     -51.5   210      411   08 55 01

08 58 40  J1628-1415   12 14 46  14.0 116.4 -4.3     -52.7   -10      411   08 58 50
09 00 00  =1625-141    12 16 06  14.3 116.6 -4.2     -52.6    70      420   08 58 41

 ---------- >>>> EFLSBERG pointing scan <<<< ----------

09 00 00  SCOX1OFF     12 16 06  15.1 119.0 -4.1     -51.4   -10      420   09 00 10
09 03 20  ---          12 19 26  15.8 119.6 -4.0     -51.0   190      444   09 00 01

09 04 00  J1628-1415   12 20 07  15.1 117.2 -4.2     -52.2    30      444   09 04 00
09 05 10  =1625-141    12 21 17  15.3 117.4 -4.1     -52.1    70      453   09 04 01

09 05 10  SCOX1OFF     12 21 17  16.1 119.9 -4.0     -50.8   -10      453   09 05 20
09 08 40  ---          12 24 47  16.8 120.4 -3.9     -50.4   200      479   09 05 11

09 08 40  J1628-1415   12 24 47  16.0 117.9 -4.1     -51.7   -10      479   09 08 50
09 10 00  =1625-141    12 26 08  16.2 118.1 -4.1     -51.6    70      488   09 08 41

09 10 00  SCOX1OFF     12 26 08  17.0 120.6 -3.9     -50.3   -10      488   09 10 10
09 13 30  ---          12 29 38  17.7 121.2 -3.9     -49.9   200      514   09 10 01

09 13 30  J1628-1415   12 29 38  16.9 118.7 -4.0     -51.2   -10      514   09 13 40
09 14 50  =1625-141    12 30 58  17.1 118.9 -4.0     -51.0    70      523   09 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

09 14 50  SCOX1OFF     12 30 58  17.9 121.4 -3.8     -49.7   -10      523   09 15 00
09 18 20  ---          12 34 29  18.5 122.0 -3.8     -49.3   200      549   09 14 51

09 19 00  J1628-1415   12 35 09  17.9 119.6 -3.9     -50.6    30      549   09 19 00
09 20 10  =1625-141    12 36 19  18.1 119.7 -3.9     -50.4    70      558   09 19 01

09 20 10  SCOX1OFF     12 36 19  18.9 122.3 -3.7     -49.1   -10      558   09 20 20
09 23 40  ---          12 39 50  19.5 122.9 -3.7     -48.6   200      583   09 20 11

09 23 40  J1628-1415   12 39 50  18.8 120.3 -3.8     -50.0   -10      583   09 23 50
09 25 00  =1625-141    12 41 10  19.0 120.5 -3.8     -49.9    70      592   09 23 41

09 25 00  SCOX1OFF     12 41 10  19.8 123.1 -3.7     -48.5   -10      592   09 25 10
09 28 30  ---          12 44 41  20.4 123.7 -3.6     -48.0   200      618   09 25 01

09 28 30  J1628-1415   12 44 41  19.7 121.1 -3.8     -49.5   -10      618   09 28 40
09 29 50  =1625-141    12 46 01  19.9 121.3 -3.7     -49.3    70      627   09 28 31

09 29 50  SCOX1OFF     12 46 01  20.6 123.9 -3.6     -47.8   -10      627   09 30 00
09 33 20  ---          12 49 31  21.2 124.6 -3.5     -47.4   200      653   09 29 51

09 34 00  J1628-1415   12 50 11  20.7 122.0 -3.7     -48.8    30      653   09 34 00
09 35 10  =1625-141    12 51 22  20.9 122.2 -3.6     -48.7    70      662   09 34 01

09 35 10  SCOX1OFF     12 51 22  21.6 124.9 -3.5     -47.2   -10      662   09 35 20
09 38 40  ---          12 54 52  22.2 125.5 -3.4     -46.7   200      688   09 35 11

09 38 40  J1628-1415   12 54 52  21.5 122.9 -3.6     -48.2   -10      688   09 38 50
09 40 00  =1625-141    12 56 12  21.8 123.1 -3.6     -48.1    70      697   09 38 41

09 40 00  SCOX1OFF     12 56 12  22.4 125.7 -3.4     -46.5   -10      697   09 40 10
09 43 30  ---          12 59 43  23.0 126.4 -3.4     -46.0   200      722   09 40 01

09 43 30  J1628-1415   12 59 43  22.4 123.7 -3.5     -47.6   -10      722   09 43 40
09 44 50  =1625-141    13 01 03  22.7 123.9 -3.5     -47.4    70      731   09 43 31

09 44 50  SCOX1OFF     13 01 03  23.3 126.6 -3.3     -45.8   -10      731   09 45 00
09 48 20  ---          13 04 34  23.9 127.3 -3.3     -45.3   200      757   09 44 51

09 49 00  J1628-1415   13 05 14  23.4 124.7 -3.4     -46.9    30      757   09 49 00
09 50 10  =1625-141    13 06 24  23.6 124.9 -3.4     -46.7    70      766   09 49 01

09 50 10  SCOX1OFF     13 06 24  24.2 127.6 -3.2     -45.1   -10      766   09 50 20
09 53 40  ---          13 09 55  24.8 128.3 -3.2     -44.6   200      792   09 50 11
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

09 53 40  J1628-1415   13 09 55  24.2 125.5 -3.3     -46.3   -10      792   09 53 50
09 55 00  =1625-141    13 11 15  24.5 125.8 -3.3     -46.1    70      801   09 53 41

09 55 00  SCOX1OFF     13 11 15  25.0 128.5 -3.2     -44.4   -10      801   09 55 10
09 58 40  ---          13 14 56  25.6 129.2 -3.1     -43.8   210      828   09 55 01

09 58 40  J1628-1415   13 14 56  25.1 126.5 -3.2     -45.6   -10      828   09 58 50
10 00 00  =1625-141    13 16 16  25.3 126.7 -3.2     -45.4    70      837   09 58 41

10 00 00  SCOX1OFF     13 16 16  25.8 129.5 -3.1     -43.6   -10      837   10 00 10
10 03 40  ---          13 19 56  26.4 130.2 -3.0     -43.1   210      864   10 00 01

10 03 40  J1628-1415   13 19 56  26.0 127.4 -3.2     -44.9   -10      864   10 03 50
10 05 00  =1625-141    13 21 17  26.2 127.7 -3.1     -44.7    70      873   10 03 41

10 05 00  SCOX1OFF     13 21 17  26.7 130.5 -3.0     -42.8   -10      873   10 05 10
10 08 40  ---          13 24 57  27.3 131.2 -2.9     -42.3   210      900   10 05 01

10 08 40  J1628-1415   13 24 57  26.8 128.4 -3.1     -44.1   -10      900   10 08 50
10 10 00  =1625-141    13 26 17  27.0 128.6 -3.1     -43.9    70      909   10 08 41

10 10 00  SCOX1OFF     13 26 17  27.5 131.5 -2.9     -42.1   -10      909   10 10 10
10 13 40  ---          13 29 58  28.1 132.2 -2.9     -41.5   210      936   10 10 01

10 13 40  J1628-1415   13 29 58  27.6 129.4 -3.0     -43.3   -10      936   10 13 50
10 15 00  =1625-141    13 31 18  27.9 129.6 -3.0     -43.1    70      945   10 13 41

10 15 00  SCOX1OFF     13 31 18  28.3 132.5 -2.8     -41.2   -10      945   10 15 10
10 18 40  ---          13 34 59  28.9 133.2 -2.8     -40.6   210      972   10 15 01

10 18 40  J1628-1415   13 34 59  28.5 130.4 -2.9     -42.6   -10      972   10 18 50
10 20 00  =1625-141    13 36 19  28.7 130.6 -2.9     -42.4    70      981   10 18 41

10 20 00  SCOX1OFF     13 36 19  29.1 133.5 -2.7     -40.4   -10      981   10 20 10
10 23 40  ---          13 40 00  29.6 134.3 -2.7     -39.8   210     1008   10 20 01

10 23 40  J1628-1415   13 40 00  29.3 131.4 -2.8     -41.8   -10     1008   10 23 50
10 25 00  =1625-141    13 41 20  29.5 131.7 -2.8     -41.5    70     1017   10 23 41

10 25 00  SCOX1OFF     13 41 20  29.8 134.6 -2.7     -39.5   -10     1017   10 25 10
10 28 40  ---          13 45 00  30.4 135.4 -2.6     -38.9   210     1044   10 25 01

10 28 40  J1628-1415   13 45 00  30.1 132.5 -2.7     -40.9   -10     1044   10 28 50
10 30 00  =1625-141    13 46 21  30.3 132.7 -2.7     -40.7    70     1053   10 28 41
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

10 30 00  SCOX1OFF     13 46 21  30.6 135.7 -2.6     -38.7   -10     1053   10 30 10
10 33 40  ---          13 50 01  31.2 136.5 -2.5     -38.0   210     1081   10 30 01

10 33 40  J1628-1415   13 50 01  30.9 133.5 -2.7     -40.1   -10     1081   10 33 50
10 35 00  =1625-141    13 51 22  31.1 133.8 -2.6     -39.8    70     1090   10 33 41

10 35 00  SCOX1OFF     13 51 22  31.4 136.8 -2.5     -37.7   -10     1090   10 35 10
10 38 40  ---          13 55 02  31.9 137.6 -2.4     -37.1   210     1117   10 35 01

10 38 40  J1628-1415   13 55 02  31.7 134.6 -2.6     -39.2   -10     1117   10 38 50
10 40 00  =1625-141    13 56 22  31.9 134.9 -2.6     -39.0    70     1126   10 38 41

10 40 00  SCOX1OFF     13 56 22  32.1 137.9 -2.4     -36.8   -10     1126   10 40 10
10 43 40  ---          14 00 03  32.6 138.7 -2.3     -36.1   210     1153   10 40 01

10 43 40  J1628-1415   14 00 03  32.4 135.7 -2.5     -38.3   -10     1153   10 43 50
10 45 00  =1625-141    14 01 23  32.6 136.0 -2.5     -38.1    70     1162   10 43 41

10 45 00  SCOX1OFF     14 01 23  32.8 139.0 -2.3     -35.9   -10     1162   10 45 10
10 48 40  ---          14 05 04  33.3 139.9 -2.3     -35.1   210     1189   10 45 01

10 48 40  J1628-1415   14 05 04  33.2 136.9 -2.4     -37.4   -10     1189   10 48 50
10 50 00  =1625-141    14 06 24  33.4 137.2 -2.4     -37.1    70     1198   10 48 41

10 50 00  SCOX1OFF     14 06 24  33.5 140.2 -2.2     -34.9   -10     1198   10 50 10
10 53 40  ---          14 10 05  34.0 141.1 -2.2     -34.1   210     1225   10 50 01

10 53 40  J1628-1415   14 10 05  33.9 138.0 -2.3     -36.4   -10     1225   10 53 50
10 55 00  =1625-141    14 11 25  34.1 138.4 -2.3     -36.2    70     1234   10 53 41

10 55 00  SCOX1OFF     14 11 25  34.2 141.4 -2.2     -33.9   -10     1234   10 55 10
10 58 40  ---          14 15 05  34.7 142.3 -2.1     -33.1   210     1261   10 55 01

10 58 40  J1628-1415   14 15 05  34.6 139.2 -2.2     -35.4   -10     1261   10 58 50
11 00 00  =1625-141    14 16 26  34.8 139.6 -2.2     -35.2    70     1270   10 58 41

11 00 00  SCOX1OFF     14 16 26  34.8 142.6 -2.1     -32.8   -10     1270   11 00 10
11 03 40  ---          14 20 06  35.3 143.6 -2.0     -32.1   210     1297   11 00 01

11 03 40  J1628-1415   14 20 06  35.3 140.4 -2.2     -34.4   -10     1297   11 03 50
11 05 00  =1625-141    14 21 26  35.5 140.8 -2.1     -34.2    70     1306   11 03 41

11 05 00  SCOX1OFF     14 21 26  35.5 143.9 -2.0     -31.8   -10     1306   11 05 10
11 08 40  ---          14 25 07  35.9 144.8 -1.9     -31.0   210     1333   11 05 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

11 08 40  J1628-1415   14 25 07  36.0 141.7 -2.1     -33.4   -10     1333   11 08 50
11 10 00  =1625-141    14 26 27  36.2 142.0 -2.1     -33.1    70     1342   11 08 41

11 10 00  SCOX1OFF     14 26 27  36.1 145.2 -1.9     -30.7   -10     1342   11 10 10
11 13 40  ---          14 30 08  36.6 146.1 -1.8     -29.9   210     1369   11 10 01

11 13 40  J1628-1415   14 30 08  36.6 143.0 -2.0     -32.3   -10     1369   11 13 50
11 15 00  =1625-141    14 31 28  36.8 143.3 -2.0     -32.1    70     1378   11 13 41

11 15 00  SCOX1OFF     14 31 28  36.7 146.5 -1.8     -29.6   -10     1378   11 15 10
11 18 40  ---          14 35 09  37.2 147.4 -1.8     -28.8   210     1405   11 15 01

11 18 40  J1628-1415   14 35 09  37.3 144.2 -1.9     -31.3   -10     1405   11 18 50
11 20 00  =1625-141    14 36 29  37.4 144.6 -1.9     -31.0    70     1414   11 18 41

11 20 00  SCOX1OFF     14 36 29  37.3 147.8 -1.7     -28.5   -10     1414   11 20 10
11 23 40  ---          14 40 10  37.7 148.8 -1.7     -27.6   210     1441   11 20 01

11 23 40  J1628-1415   14 40 10  37.9 145.6 -1.8     -30.1   -10     1441   11 23 50
11 25 00  =1625-141    14 41 30  38.1 145.9 -1.8     -29.8    70     1450   11 23 41

11 25 00  SCOX1OFF     14 41 30  37.9 149.1 -1.7     -27.3   -10     1450   11 25 10
11 28 40  ---          14 45 10  38.3 150.1 -1.6     -26.4   210     1477   11 25 01

11 28 40  J1628-1415   14 45 10  38.5 146.9 -1.7     -29.0   -10     1477   11 28 50
11 30 00  =1625-141    14 46 31  38.7 147.3 -1.7     -28.7    70     1486   11 28 41

11 30 00  SCOX1OFF     14 46 31  38.4 150.5 -1.6     -26.1   -10     1486   11 30 10
11 33 40  ---          14 50 11  38.8 151.5 -1.5     -25.2   210     1513   11 30 01

11 33 40  J1628-1415   14 50 11  39.1 148.3 -1.7     -27.8   -10     1513   11 33 50
11 35 00  =1625-141    14 51 31  39.2 148.6 -1.6     -27.5    70     1522   11 33 41

11 35 00  SCOX1OFF     14 51 31  38.9 151.9 -1.5     -24.9   -10     1522   11 35 10
11 38 40  ---          14 55 12  39.3 152.9 -1.4     -24.0   210     1549   11 35 01

11 38 40  J1628-1415   14 55 12  39.6 149.7 -1.6     -26.6   -10     1549   11 38 50
11 40 00  =1625-141    14 56 32  39.8 150.1 -1.6     -26.3    70     1558   11 38 41

11 40 00  SCOX1OFF     14 56 32  39.4 153.3 -1.4     -23.7   -10     1558   11 40 10
11 43 40  ---          15 00 13  39.8 154.4 -1.3     -22.7   210     1586   11 40 01

11 43 40  J1628-1415   15 00 13  40.2 151.1 -1.5     -25.4   -10     1586   11 43 50
11 45 00  =1625-141    15 01 33  40.3 151.5 -1.5     -25.1    70     1595   11 43 41
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

11 45 00  SCOX1OFF     15 01 33  39.9 154.8 -1.3     -22.4   -10     1595   11 45 10
11 48 40  ---          15 05 14  40.2 155.8 -1.3     -21.5   210     1622   11 45 01

11 48 40  J1628-1415   15 05 14  40.7 152.5 -1.4     -24.2   -10     1622   11 48 50
11 50 00  =1625-141    15 06 34  40.8 152.9 -1.4     -23.8    70     1631   11 48 41

11 50 00  SCOX1OFF     15 06 34  40.3 156.2 -1.2     -21.1   -10     1631   11 50 10
11 53 40  ---          15 10 14  40.7 157.3 -1.2     -20.2   210     1658   11 50 01

11 53 40  J1628-1415   15 10 14  41.2 154.0 -1.3     -22.9   -10     1658   11 53 50
11 55 00  =1625-141    15 11 35  41.3 154.4 -1.3     -22.5    70     1667   11 53 41

11 55 00  SCOX1OFF     15 11 35  40.8 157.7 -1.2     -19.8   -10     1667   11 55 10
11 58 40  ---          15 15 15  41.1 158.8 -1.1     -18.8   210     1694   11 55 01

11 58 40  J1628-1415   15 15 15  41.6 155.5 -1.2     -21.6   -10     1694   11 58 50
12 00 00  =1625-141    15 16 35  41.7 155.9 -1.2     -21.2    70     1703   11 58 41

12 00 30  J1229+0203   15 17 06  41.2 242.2  2.8      49.6   -39     1703   12 01 09
12 05 30  =1226+023    15 22 06  40.3 243.3  2.9      50.3   261     1736   12 00 31

12 06 00  J1628-1415   15 22 36  42.2 157.8 -1.1     -19.6   -39     1736   12 06 39
12 10 00  =1625-141    15 26 37  42.6 159.0 -1.1     -18.6   201     1762   12 06 01

12 10 00  SCOX1OFF     15 26 37  41.9 162.3 -0.9     -15.8   -10     1762   12 10 10
12 13 40  ---          15 30 18  42.1 163.5 -0.8     -14.7   210     1789   12 10 01

12 13 40  J1628-1415   15 30 18  42.8 160.2 -1.0     -17.5   -10     1789   12 13 50
12 15 00  =1625-141    15 31 38  42.9 160.6 -1.0     -17.2    70     1798   12 13 41

12 15 00  SCOX1OFF     15 31 38  42.2 163.9 -0.8     -14.4   -10     1798   12 15 10
12 18 40  ---          15 35 19  42.4 165.0 -0.8     -13.3   210     1825   12 15 01

12 18 40  J1628-1415   15 35 19  43.2 161.7 -0.9     -16.1   -10     1825   12 18 50
12 20 00  =1625-141    15 36 39  43.3 162.2 -0.9     -15.8    70     1834   12 18 41

12 20 00  SCOX1OFF     15 36 39  42.5 165.5 -0.7     -13.0   -10     1834   12 20 10
12 23 40  ---          15 40 19  42.7 166.6 -0.7     -11.9   210     1861   12 20 01

12 23 40  J1628-1415   15 40 19  43.5 163.4 -0.8     -14.7   -10     1861   12 23 50
12 25 00  =1625-141    15 41 40  43.6 163.8 -0.8     -14.4    70     1870   12 23 41

12 25 00  SCOX1OFF     15 41 40  42.7 167.1 -0.7     -11.5   -10     1870   12 25 10
12 28 40  ---          15 45 20  42.9 168.2 -0.6     -10.5   210     1898   12 25 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

12 28 40  J1628-1415   15 45 20  43.8 165.0 -0.7     -13.3   -10     1898   12 28 50
12 30 00  =1625-141    15 46 40  43.9 165.4 -0.7     -12.9    70     1907   12 28 41

12 30 00  SCOX1OFF     15 46 40  43.0 168.7 -0.6     -10.1   -10     1907   12 30 10
12 33 40  ---          15 50 21  43.1 169.9 -0.5      -9.0   210     1934   12 30 01

12 33 40  J1628-1415   15 50 21  44.1 166.6 -0.7     -11.8   -10     1934   12 33 50
12 35 00  =1625-141    15 51 41  44.1 167.1 -0.6     -11.5    70     1943   12 33 41

12 35 00  SCOX1OFF     15 51 41  43.2 170.3 -0.5      -8.7   -10     1943   12 35 10
12 38 40  ---          15 55 22  43.3 171.5 -0.4      -7.6   210     1970   12 35 01

12 38 40  J1628-1415   15 55 22  44.3 168.3 -0.6     -10.4   -10     1970   12 38 50
12 40 00  =1625-141    15 56 42  44.4 168.7 -0.6     -10.0    70     1979   12 38 41

12 40 00  SCOX1OFF     15 56 42  43.3 171.9 -0.4      -7.2   -10     1979   12 40 10
12 43 40  ---          16 00 23  43.4 173.2 -0.3      -6.1   210     2006   12 40 01

12 43 40  J1628-1415   16 00 23  44.5 170.0 -0.5      -8.9   -10     2006   12 43 50
12 45 00  =1625-141    16 01 43  44.6 170.4 -0.5      -8.5    70     2015   12 43 41

12 45 00  SCOX1OFF     16 01 43  43.5 173.6 -0.3      -5.7   -10     2015   12 45 10
12 48 40  ---          16 05 23  43.5 174.8 -0.3      -4.6   210     2042   12 45 01

12 48 40  J1628-1415   16 05 23  44.7 171.7 -0.4      -7.4   -10     2042   12 48 50
12 50 00  =1625-141    16 06 44  44.7 172.1 -0.4      -7.0    70     2051   12 48 41

12 50 00  SCOX1OFF     16 06 44  43.6 175.3 -0.2      -4.2   -10     2051   12 50 10
12 53 40  ---          16 10 24  43.6 176.5 -0.2      -3.2   210     2078   12 50 01

12 53 40  J1628-1415   16 10 24  44.8 173.4 -0.3      -5.9   -10     2078   12 53 50
12 55 00  =1625-141    16 11 45  44.9 173.8 -0.3      -5.5    70     2087   12 53 41

12 55 00  SCOX1OFF     16 11 45  43.6 176.9 -0.2      -2.8   -10     2087   12 55 10
12 58 40  ---          16 15 25  43.7 178.1 -0.1      -1.7   210     2114   12 55 01

12 58 40  J1628-1415   16 15 25  44.9 175.1 -0.2      -4.4   -11     2114   12 58 51
13 00 00  =1625-141    16 16 45  45.0 175.5 -0.2      -4.0    69     2123   12 58 41

13 00 00  SCOX1OFF     16 16 45  43.7 178.6 -0.1      -1.3   -11     2123   13 00 11
13 03 40  ---          16 20 26  43.7 179.8 -0.0      -0.2   209     2150   13 00 01

13 03 40  J1628-1415   16 20 26  45.0 176.8 -0.2      -2.9   -11     2150   13 03 51
13 05 00  =1625-141    16 21 46  45.0 177.2 -0.1      -2.5    69     2159   13 03 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

13 05 00  SCOX1OFF     16 21 46  43.7 180.3  0.0       0.2   -11     2159   13 05 11
13 08 40  ---          16 25 27  43.7 181.5  0.1       1.3   209     2186   13 05 01

13 08 40  J1628-1415   16 25 27  45.1 178.5 -0.1      -1.3   -11     2186   13 08 51
13 10 00  =1625-141    16 26 47  45.1 179.0 -0.1      -0.9    69     2194   13 08 41

13 10 00  SCOX1OFF     16 26 47  43.7 181.9  0.1       1.7   -11     2194   13 10 11
13 13 40  ---          16 30 28  43.6 183.1  0.2       2.8   209     2221   13 10 01

13 13 40  J1628-1415   16 30 28  45.1 180.2  0.0       0.2   -11     2221   13 13 51
13 15 00  =1625-141    16 31 48  45.1 180.7  0.0       0.6    69     2230   13 13 41

13 15 00  SCOX1OFF     16 31 48  43.6 183.6  0.2       3.2   -11     2230   13 15 11
13 18 40  ---          16 35 28  43.6 184.8  0.2       4.3   209     2257   13 15 01

13 18 40  J1628-1415   16 35 28  45.0 181.9  0.1       1.7   -11     2257   13 18 51
13 20 00  =1625-141    16 36 49  45.0 182.4  0.1       2.1    69     2266   13 18 41

13 20 00  SCOX1OFF     16 36 49  43.5 185.2  0.3       4.7   -11     2266   13 20 11
13 23 40  ---          16 40 29  43.5 186.5  0.3       5.8   209     2293   13 20 01

13 23 40  J1628-1415   16 40 29  45.0 183.6  0.2       3.2   -11     2293   13 23 51
13 25 00  =1625-141    16 41 49  45.0 184.1  0.2       3.6    69     2302   13 23 41

13 25 00  SCOX1OFF     16 41 49  43.4 186.9  0.3       6.2   -11     2302   13 25 11
13 28 40  ---          16 45 30  43.3 188.1  0.4       7.2   209     2329   13 25 01

13 28 40  J1628-1415   16 45 30  44.9 185.4  0.3       4.8   -11     2329   13 28 51
13 30 00  =1625-141    16 46 50  44.9 185.8  0.3       5.2    69     2338   13 28 41

13 30 00  SCOX1OFF     16 46 50  43.3 188.6  0.4       7.6   -11     2338   13 30 11
13 33 40  ---          16 50 31  43.1 189.8  0.5       8.7   209     2365   13 30 01

13 33 40  J1628-1415   16 50 31  44.8 187.1  0.3       6.3   -11     2365   13 33 51
13 35 00  =1625-141    16 51 51  44.8 187.5  0.4       6.7    69     2373   13 33 41

13 35 00  SCOX1OFF     16 51 51  43.1 190.2  0.5       9.1   -11     2373   13 35 11
13 38 40  ---          16 55 32  43.0 191.4  0.6      10.2   209     2400   13 35 01

13 38 40  J1628-1415   16 55 32  44.6 188.8  0.4       7.8   -11     2400   13 38 51
13 40 00  =1625-141    16 56 52  44.6 189.2  0.5       8.2    69     2409   13 38 41

13 40 00  SCOX1OFF     16 56 52  42.9 191.8  0.6      10.5   -11     2409   13 40 11
13 43 40  ---          17 00 33  42.7 193.0  0.7      11.6   209     2436   13 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

13 43 40  J1628-1415   17 00 33  44.5 190.4  0.5       9.3   -11     2436   13 43 51
13 45 00  =1625-141    17 01 53  44.4 190.9  0.5       9.7    69     2445   13 43 41

13 45 00  SCOX1OFF     17 01 53  42.7 193.4  0.7      12.0   -11     2445   13 45 11
13 48 40  ---          17 05 33  42.5 194.6  0.7      13.0   209     2472   13 45 01

13 48 40  J1628-1415   17 05 33  44.2 192.1  0.6      10.7   -12     2472   13 48 52
13 50 00  =1625-141    17 06 54  44.2 192.6  0.6      11.1    68     2481   13 48 41

13 50 00  SCOX1OFF     17 06 54  42.4 195.0  0.8      13.4   -12     2481   13 50 12
13 53 40  ---          17 10 34  42.2 196.2  0.8      14.4   208     2508   13 50 01

13 53 40  J1628-1415   17 10 34  44.0 193.8  0.7      12.2   -12     2508   13 53 52
13 55 00  =1625-141    17 11 54  43.9 194.2  0.7      12.6    68     2516   13 53 41

13 55 00  SCOX1OFF     17 11 54  42.1 196.6  0.8      14.8   -12     2516   13 55 12
13 58 40  ---          17 15 35  41.9 197.8  0.9      15.8   208     2543   13 55 01

13 58 40  J1628-1415   17 15 35  43.7 195.4  0.8      13.7   -12     2543   13 58 52
14 00 00  =1625-141    17 16 55  43.7 195.9  0.8      14.0    68     2552   13 58 41

14 00 00  SCOX1OFF     17 16 55  41.8 198.2  0.9      16.2   -12     2552   14 00 12
14 03 40  ---          17 20 36  41.5 199.3  1.0      17.2   208     2579   14 00 01

14 03 40  J1628-1415   17 20 36  43.4 197.0  0.8      15.1   -12     2579   14 03 52
14 05 00  =1625-141    17 21 56  43.3 197.5  0.9      15.5    68     2587   14 03 41

14 05 00  SCOX1OFF     17 21 56  41.4 199.7  1.0      17.5   -12     2587   14 05 12
14 08 40  ---          17 25 37  41.2 200.8  1.1      18.5   208     2614   14 05 01

14 08 40  J1628-1415   17 25 37  43.1 198.7  0.9      16.5   -12     2614   14 08 52
14 10 00  =1625-141    17 26 57  43.0 199.1  1.0      16.9    68     2623   14 08 41

14 10 00  SCOX1OFF     17 26 57  41.0 201.2  1.1      18.9   -12     2623   14 10 12
14 13 40  ---          17 30 37  40.8 202.3  1.2      19.9   208     2650   14 10 01

14 13 40  J1628-1415   17 30 37  42.7 200.2  1.0      17.9   -12     2650   14 13 52
14 15 00  =1625-141    17 31 58  42.6 200.7  1.0      18.3    68     2659   14 13 41

14 15 00  SCOX1OFF     17 31 58  40.6 202.7  1.2      20.2   -12     2659   14 15 12
14 18 40  ---          17 35 38  40.3 203.8  1.2      21.2   208     2685   14 15 01

14 18 40  J1628-1415   17 35 38  42.4 201.8  1.1      19.3   -12     2685   14 18 52
14 20 00  =1625-141    17 36 58  42.3 202.2  1.1      19.6    68     2694   14 18 41
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

14 20 00  SCOX1OFF     17 36 58  40.2 204.2  1.3      21.5   -12     2694   14 20 12
14 23 40  ---          17 40 39  39.9 205.3  1.3      22.4   208     2721   14 20 01

14 23 40  J1628-1415   17 40 39  41.9 203.3  1.2      20.6   -12     2721   14 23 52
14 25 00  =1625-141    17 41 59  41.8 203.7  1.2      20.9    68     2730   14 23 41

14 25 00  SCOX1OFF     17 41 59  39.8 205.7  1.3      22.8   -12     2730   14 25 12
14 28 40  ---          17 45 40  39.4 206.7  1.4      23.7   208     2756   14 25 01

14 28 40  J1628-1415   17 45 40  41.5 204.9  1.3      21.9   -12     2756   14 28 52
14 30 00  =1625-141    17 47 00  41.4 205.3  1.3      22.3    68     2765   14 28 41

14 30 00  SCOX1OFF     17 47 00  39.3 207.1  1.4      24.0   -12     2765   14 30 12
14 33 40  ---          17 50 41  38.9 208.2  1.5      24.9   208     2792   14 30 01

14 33 40  J1628-1415   17 50 41  41.0 206.3  1.3      23.2   -12     2792   14 33 52
14 35 00  =1625-141    17 52 01  40.9 206.7  1.4      23.5    68     2801   14 33 41

14 35 00  SCOX1OFF     17 52 01  38.8 208.5  1.5      25.3   -12     2801   14 35 12
14 38 40  ---          17 55 42  38.4 209.6  1.6      26.2   208     2828   14 35 01

14 38 40  J1628-1415   17 55 42  40.5 207.8  1.4      24.5   -12     2828   14 38 52
14 40 00  =1625-141    17 57 02  40.4 208.2  1.5      24.8    68     2836   14 38 41

14 40 00  SCOX1OFF     17 57 02  38.3 209.9  1.6      26.5   -12     2836   14 40 12
14 43 40  ---          18 00 42  37.8 210.9  1.7      27.3   208     2863   14 40 01

14 43 40  J1628-1415   18 00 42  40.0 209.3  1.5      25.7   -12     2863   14 43 52
14 45 00  =1625-141    18 02 03  39.9 209.6  1.5      26.0    68     2872   14 43 41

14 45 00  SCOX1OFF     18 02 03  37.7 211.3  1.7      27.6   -12     2872   14 45 12
14 48 40  ---          18 05 43  37.3 212.3  1.7      28.5   208     2899   14 45 01

14 48 40  J1628-1415   18 05 43  39.5 210.7  1.6      26.9   -12     2899   14 48 52
14 50 00  =1625-141    18 07 03  39.3 211.0  1.6      27.3    68     2907   14 48 41

14 50 00  SCOX1OFF     18 07 03  37.1 212.6  1.8      28.8   -12     2907   14 50 12
14 53 40  ---          18 10 44  36.7 213.6  1.8      29.6   208     2934   14 50 01

14 53 40  J1628-1415   18 10 44  38.9 212.1  1.7      28.1   -12     2934   14 53 52
14 55 00  =1625-141    18 12 04  38.8 212.4  1.7      28.4    68     2943   14 53 41

14 55 00  SCOX1OFF     18 12 04  36.5 213.9  1.9      29.9   -12     2943   14 55 12
14 58 40  ---          18 15 45  36.1 214.9  1.9      30.7   208     2970   14 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

14 58 40  J1628-1415   18 15 45  38.3 213.4  1.8      29.3   -12     2970   14 58 52
15 00 00  =1625-141    18 17 05  38.2 213.8  1.8      29.6    68     2979   14 58 41

15 00 00  J1229+0203   18 17 05   3.8 270.0  5.8  H   59.4   -76     2979   15 01 16
15 04 00  =1226+023    18 21 06   2.9 270.5  5.9  H   59.4     0     3000   15 00 01

15 06 00  J1558-1409   18 23 06  33.4 222.9  2.4      37.2    52     3000   15 06 00
15 08 30  =1555-140    18 25 36  33.0 223.5  2.4      37.7   150     3019   15 06 01

15 08 30  J1628-1415   18 25 36  37.1 216.0  1.9      31.5   -16     3019   15 08 46
15 10 00  =1625-141    18 27 07  36.9 216.4  2.0      31.8    74     3029   15 08 31

15 10 00  SCOX1OFF     18 27 07  34.6 217.7  2.1      33.2   -13     3029   15 10 13
15 13 40  ---          18 30 47  34.2 218.6  2.2      33.9   207     3055   15 10 01

15 13 40  J1628-1415   18 30 47  36.5 217.4  2.0      32.6   -13     3055   15 13 53
15 15 00  =1625-141    18 32 08  36.3 217.7  2.0      32.9    67     3064   15 13 41

15 15 00  SCOX1OFF     18 32 08  34.0 218.9  2.2      34.2   -13     3064   15 15 13
15 18 20  ---          18 35 28  33.5 219.7  2.2      34.8   187     3088   15 15 01

15 18 50  J1628-1415   18 35 58  35.8 218.7  2.1      33.7    17     3088   15 18 50
15 20 00  =1625-141    18 37 08  35.6 219.0  2.1      33.9    70     3097   15 18 51

15 20 00  SCOX1OFF     18 37 08  33.3 220.1  2.3      35.2   -13     3097   15 20 13
15 23 40  ---          18 40 49  32.8 221.0  2.3      35.9   207     3124   15 20 01

15 23 40  J1628-1415   18 40 49  35.1 219.9  2.2      34.7   -13     3124   15 23 53
15 25 00  =1625-141    18 42 09  34.9 220.2  2.2      35.0    67     3132   15 23 41

15 25 00  SCOX1OFF     18 42 09  32.6 221.3  2.4      36.1   -13     3132   15 25 13
15 28 40  ---          18 45 50  32.1 222.1  2.4      36.8   207     3159   15 25 01

15 28 40  J1628-1415   18 45 50  34.4 221.1  2.3      35.7   -13     3159   15 28 53
15 30 00  =1625-141    18 47 10  34.2 221.4  2.3      35.9    67     3168   15 28 41

15 30 00  SCOX1OFF     18 47 10  31.9 222.5  2.4      37.1   -13     3168   15 30 13
15 33 20  ---          18 50 31  31.4 223.2  2.5      37.7   187     3192   15 30 01

15 33 50  J1628-1415   18 51 01  33.7 222.3  2.4      36.7    17     3192   15 33 50
15 35 00  =1625-141    18 52 11  33.5 222.6  2.4      36.9    70     3201   15 33 51

15 35 00  SCOX1OFF     18 52 11  31.1 223.6  2.5      38.0   -13     3201   15 35 13
15 38 40  ---          18 55 51  30.6 224.4  2.6      38.7   207     3227   15 35 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

15 38 40  J1628-1415   18 55 51  33.0 223.4  2.4      37.6   -13     3227   15 38 53
15 40 00  =1625-141    18 57 12  32.8 223.7  2.5      37.8    67     3236   15 38 41

15 40 00  SCOX1OFF     18 57 12  30.4 224.7  2.6      38.9   -13     3236   15 40 13
15 43 40  ---          19 00 52  29.8 225.5  2.7      39.6   207     3263   15 40 01

15 43 40  J1628-1415   19 00 52  32.2 224.5  2.5      38.5   -13     3263   15 43 53
15 45 00  =1625-141    19 02 12  32.0 224.8  2.5      38.8    67     3271   15 43 41

15 45 50  J1558-1409   19 03 03  27.1 231.4  3.1      43.9    32     3271   15 45 50
15 47 20  =1555-140    19 04 33  26.8 231.7  3.1      44.2    90     3283   15 45 51

15 47 20  J1628-1415   19 04 33  31.7 225.4  2.6      39.2   -18     3283   15 47 38
15 48 50  =1625-141    19 06 03  31.4 225.7  2.6      39.4    72     3292   15 47 21

15 48 50  SCOX1OFF     19 06 03  29.0 226.6  2.8      40.5   -13     3292   15 49 03
15 52 40  ---          19 09 54  28.4 227.4  2.8      41.1   217     3320   15 48 51

15 52 40  J1628-1415   19 09 54  30.8 226.5  2.7      40.1   -13     3320   15 52 53
15 54 00  =1625-141    19 11 14  30.6 226.8  2.7      40.3    67     3329   15 52 41

15 54 00  SCOX1OFF     19 11 14  28.2 227.6  2.8      41.3   -13     3329   15 54 13
15 57 30  ---          19 14 44  27.6 228.3  2.9      41.9   197     3354   15 54 01

15 58 00  J1628-1415   19 15 15  30.0 227.7  2.8      41.0    17     3354   15 58 00
15 59 10  =1625-141    19 16 25  29.8 227.9  2.8      41.2    70     3363   15 58 01

15 59 10  SCOX1OFF     19 16 25  27.4 228.7  2.9      42.2   -13     3363   15 59 23
16 03 00  ---          19 20 15  26.7 229.5  3.0      42.8   217     3391   15 59 11

16 03 00  J1628-1415   19 20 15  29.2 228.7  2.8      41.9   -13     3391   16 03 13
16 04 20  =1625-141    19 21 36  29.0 229.0  2.9      42.1    67     3400   16 03 01

16 04 20  SCOX1OFF     19 21 36  26.5 229.7  3.0      43.0   -13     3400   16 04 33
16 08 10  ---          19 25 26  25.9 230.5  3.1      43.6   217     3428   16 04 21

16 08 10  J1628-1415   19 25 26  28.4 229.8  2.9      42.7   -13     3428   16 08 23
16 09 30  =1625-141    19 26 46  28.1 230.0  2.9      42.9    67     3436   16 08 11

16 09 30  SCOX1OFF     19 26 46  25.7 230.7  3.1      43.8   -13     3436   16 09 43
16 13 00  ---          19 30 17  25.1 231.4  3.2      44.3   197     3462   16 09 31

16 13 30  J1628-1415   19 30 47  27.5 230.8  3.0      43.5    17     3462   16 13 30
16 14 40  =1625-141    19 31 57  27.3 231.1  3.0      43.7    70     3471   16 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

16 14 40  SCOX1OFF     19 31 57  24.8 231.7  3.2      44.5   -13     3471   16 14 53
16 18 30  ---          19 35 48  24.1 232.4  3.2      45.1   217     3499   16 14 41

16 18 30  J1628-1415   19 35 48  26.6 231.8  3.1      44.3   -13     3499   16 18 43
16 19 50  =1625-141    19 37 08  26.4 232.1  3.1      44.5    67     3507   16 18 31

16 19 50  SCOX1OFF     19 37 08  23.9 232.7  3.3      45.3   -13     3507   16 20 03
16 23 40  ---          19 40 59  23.3 233.4  3.3      45.8   217     3535   16 19 51

16 23 40  J1628-1415   19 40 59  25.7 232.8  3.2      45.0   -13     3535   16 23 53
16 25 00  =1625-141    19 42 19  25.5 233.1  3.2      45.2    67     3544   16 23 41

16 25 50  J1558-1409   19 43 09  20.0 238.7  3.7      49.3    31     3544   16 25 50
16 27 20  =1555-140    19 44 39  19.7 239.0  3.8      49.5    90     3555   16 25 51

16 27 20  J1628-1415   19 44 39  25.1 233.5  3.2      45.6   -19     3555   16 27 39
16 28 50  =1625-141    19 46 10  24.8 233.8  3.3      45.8    71     3565   16 27 21

16 28 50  SCOX1OFF     19 46 10  22.4 234.3  3.4      46.6   -13     3565   16 29 03
16 32 40  ---          19 50 00  21.7 235.0  3.5      47.1   217     3593   16 28 51

16 32 40  J1628-1415   19 50 00  24.2 234.5  3.3      46.3   -13     3593   16 32 53
16 34 00  =1625-141    19 51 20  23.9 234.8  3.4      46.5    67     3601   16 32 41

16 34 00  SCOX1OFF     19 51 20  21.4 235.2  3.5      47.2   -13     3601   16 34 13
16 37 30  ---          19 54 51  20.8 235.9  3.6      47.7   197     3627   16 34 01

16 38 00  J1628-1415   19 55 21  23.2 235.5  3.4      47.0    17     3627   16 38 00
16 39 10  =1625-141    19 56 31  23.0 235.7  3.4      47.2    70     3636   16 38 01

16 39 10  SCOX1OFF     19 56 31  20.5 236.1  3.6      47.9   -13     3636   16 39 23
16 43 00  ---          20 00 22  19.8 236.8  3.7      48.4   217     3663   16 39 11

16 43 00  J1628-1415   20 00 22  22.3 236.4  3.5      47.7   -13     3663   16 43 13
16 44 20  =1625-141    20 01 42  22.1 236.6  3.5      47.8    67     3672   16 43 01

16 44 20  SCOX1OFF     20 01 42  19.6 237.0  3.7      48.6   -13     3672   16 44 33
16 48 10  ---          20 05 33  18.9 237.7  3.7      49.0   217     3700   16 44 21

16 48 10  J1628-1415   20 05 33  21.4 237.3  3.6      48.3   -13     3700   16 48 23
16 49 30  =1625-141    20 06 53  21.2 237.5  3.6      48.5    67     3709   16 48 11

16 49 30  SCOX1OFF     20 06 53  18.7 237.9  3.8      49.2   -13     3709   16 49 43
16 53 00  ---          20 10 24  18.0 238.5  3.8      49.6   197     3734   16 49 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

16 53 30  J1628-1415   20 10 54  20.4 238.2  3.7      49.0    17     3734   16 53 30
16 54 40  =1625-141    20 12 04  20.2 238.4  3.7      49.1    70     3743   16 53 31

16 54 40  SCOX1OFF     20 12 04  17.7 238.8  3.9      49.8   -13     3743   16 54 53
16 58 30  ---          20 15 55  17.0 239.4  3.9      50.3   217     3771   16 54 41

16 58 30  J1628-1415   20 15 55  19.5 239.0  3.8      49.6   -13     3771   16 58 43
16 59 50  =1625-141    20 17 15  19.3 239.3  3.8      49.7    67     3780   16 58 31

16 59 50  SCOX1OFF     20 17 15  16.8 239.6  3.9      50.4   -13     3780   17 00 03
17 03 40  ---          20 21 05  16.0 240.2  4.0      50.8   217     3808   16 59 51

17 03 40  J1628-1415   20 21 05  18.6 239.9  3.9      50.2   -13     3808   17 03 53
17 05 00  =1625-141    20 22 26  18.3 240.1  3.9      50.3    67     3816   17 03 41

17 05 50  J1558-1409   20 23 16  12.4 245.0  4.4      53.6    31     3816   17 05 50
17 07 20  =1555-140    20 24 46  12.1 245.2  4.4      53.7    90     3828   17 05 51

17 07 20  J1628-1415   20 24 46  17.9 240.5  3.9      50.6   -19     3828   17 07 39
17 08 50  =1625-141    20 26 16  17.6 240.7  3.9      50.8    71     3837   17 07 21

17 08 50  SCOX1OFF     20 26 16  15.1 241.0  4.1      51.4   -13     3837   17 09 03
17 12 40  ---          20 30 07  14.3 241.6  4.2      51.8   217     3865   17 08 51

17 12 40  J1628-1415   20 30 07  16.9 241.3  4.0      51.2   -13     3865   17 12 53
17 14 00  =1625-141    20 31 27  16.6 241.6  4.0      51.3    67     3874   17 12 41

17 14 00  SCOX1OFF     20 31 27  14.1 241.8  4.2      52.0   -13     3874   17 14 13
17 17 30  ---          20 34 58  13.4 242.3  4.2      52.3   197     3899   17 14 01

17 18 00  J1628-1415   20 35 28  15.9 242.2  4.1      51.8    17     3899   17 18 00
17 19 10  =1625-141    20 36 38  15.6 242.4  4.1      51.9    70     3908   17 18 01

17 19 10  SCOX1OFF     20 36 38  13.1 242.6  4.3      52.5   -13     3908   17 19 23
17 23 00  ---          20 40 29  12.4 243.2  4.3      52.9   217     3936   17 19 11

17 23 00  J1628-1415   20 40 29  14.9 243.0  4.2      52.3   -13     3936   17 23 13
17 24 20  =1625-141    20 41 49  14.6 243.2  4.2      52.4    67     3945   17 23 01

17 24 20  SCOX1OFF     20 41 49  12.1 243.4  4.3      53.0   -13     3945   17 24 33
17 28 10  ---          20 45 39  11.4 243.9  4.4      53.4   217     3973   17 24 21

17 28 10  J1628-1415   20 45 39  13.9 243.7  4.3      52.8   -13     3973   17 28 23
17 29 30  =1625-141    20 47 00  13.6 243.9  4.3      52.9    67     3981   17 28 11
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

17 29 30  SCOX1OFF     20 47 00  11.1 244.1  4.4      53.5   -13     3981   17 29 43
17 33 00  ---          20 50 30  10.4 244.6  4.5      53.9   197     4007   17 29 31

17 33 30  J1628-1415   20 51 00  12.9 244.5  4.4      53.3    17     4007   17 33 30
17 34 40  =1625-141    20 52 10  12.6 244.7  4.4      53.4    70     4016   17 33 31

17 34 40  SCOX1OFF     20 52 10  10.1 244.9  4.5      54.0   -13     4016   17 34 53
17 38 30  ---          20 56 01   9.4 245.4  4.6      54.4   217     4044   17 34 41

17 38 30  J1628-1415   20 56 01  11.9 245.3  4.4      53.8   -13     4044   17 38 43
17 39 50  =1625-141    20 57 21  11.6 245.5  4.5      53.9    67     4052   17 38 31

17 39 50  SCOX1OFF     20 57 21   9.1 245.6  4.6      54.5   -13     4052   17 40 03
17 43 40  ---          21 01 12   8.3 246.2  4.7      54.8   217     4080   17 39 51

17 43 40  J1628-1415   21 01 12  10.9 246.0  4.5      54.2   -13     4080   17 43 53
17 45 00  =1625-141    21 02 32  10.6 246.2  4.5      54.4    67     4089   17 43 41

17 45 50  J1558-1409   21 03 22   4.4 250.6  5.1      56.9    30     4089   17 45 50
17 47 20  =1555-140    21 04 53   4.1 250.8  5.1      57.0    90     4100   17 45 51

17 47 20  J1628-1415   21 04 53  10.1 246.6  4.6      54.6   -20     4100   17 47 40
17 48 50  =1625-141    21 06 23   9.9 246.8  4.6      54.7    70     4109   17 47 21

17 48 50  SCOX1OFF     21 06 23   7.3 246.9  4.8      55.3   -13     4109   17 49 03
17 52 40  ---          21 10 13   6.6 247.4  4.8      55.6   217     4137   17 48 51

17 52 40  J1628-1415   21 10 13   9.1 247.3  4.7      55.0   -13     4137   17 52 53
17 54 00  =1625-141    21 11 34   8.8 247.5  4.7      55.1    67     4146   17 52 41

17 54 00  SCOX1OFF     21 11 34   6.3 247.6  4.8      55.7   -13     4146   17 54 13
17 57 30  ---          21 15 04   5.6 248.1  4.9      56.0   197     4171   17 54 01

17 58 00  J1628-1415   21 15 34   8.0 248.1  4.8      55.5    17     4171   17 58 00
17 59 10  =1625-141    21 16 44   7.8 248.2  4.8      55.6    70     4180   17 58 01

17 59 10  SCOX1OFF     21 16 44   5.3 248.3  4.9      56.1   -13     4180   17 59 23
18 03 00  ---          21 20 35   4.5 248.8  5.0      56.4   217     4208   17 59 11

18 03 00  J1628-1415   21 20 35   7.0 248.8  4.8      55.9   -13     4208   18 03 13
18 04 20  =1625-141    21 21 55   6.8 248.9  4.9      56.0    67     4217   18 03 01

18 04 20  SCOX1OFF     21 21 55   4.2 249.0  5.0      56.5   -13     4217   18 04 33
18 08 10  ---          21 25 46   3.4 249.5  5.1      56.8   217     4245   18 04 21
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  23 Feb 2019   Day  54 ---

18 08 10  J1628-1415   21 25 46   6.0 249.5  4.9      56.3   -13     4245   18 08 23
18 09 30  =1625-141    21 27 06   5.7 249.6  5.0      56.4    67     4253   18 08 11

18 09 30  SCOX1OFF     21 27 06   3.2 249.7  5.1      56.9   -13     4253   18 09 43
18 13 00  ---          21 30 37   2.5 250.1  5.2  H   57.2     0     4279   18 09 31

18 13 30  J1628-1415   21 31 07   4.9 250.2  5.0      56.7    17     4279   18 13 30
18 14 40  =1625-141    21 32 17   4.7 250.3  5.0      56.7    70     4288   18 13 31

18 18 30  J1628-1415   21 36 08   3.9 250.9  5.1      57.0   224     4288   18 18 30
18 19 50  =1625-141    21 37 28   3.6 251.0  5.1      57.1    80     4298   18 18 31

18 23 40  J1628-1415   21 41 19   2.8 251.5  5.2  H   57.4   224     4298   18 23 40
18 25 00  =1625-141    21 42 39   2.6 251.7  5.2  H   57.5     0     4308   18 23 41

18 26 30  J1743-0350   21 44 09  23.4 250.0  4.0      54.1    41     4308   18 26 30
18 29 00  =1741-038    21 46 39  22.9 250.4  4.0      54.3   150     4328   18 26 31

18 29 30  J1800+3848   21 47 09  43.6 296.2  3.8      82.1   -19     4328   18 29 49
18 32 30  =1758+388    21 50 10  43.0 296.3  3.8      81.7   161     4349   18 29 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess119.X1024glob
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  22  Setup file default.  Used with PCAL = off
   LO sum=   8331.00  8331.00  8363.00  8363.00  8395.00  8395.00  8427.00  8427.00
   BBC fr=    731.00   731.00   763.00   763.00   795.00   795.00   827.00   827.00
   Bandwd=     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     771.00    771.00    803.00    803.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  22  23  24  25  26  27  28  29  30  31

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SCOX1OFF          16 17 05.647600   * 16 19 56.254500     16 21 00.549744       0.00
                    -15 30 45.21542    *-15 37 54.63500     -15 40 32.40541        0.00
                     From catalog imbedded in main SCHED input file.

   1226+023          12 26 33.245836   * 12 29 06.699732     12 30 05.584007       0.10
 * J1229+0203        02 19 43.30553    * 02 03 08.59803      01 56 46.63413        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  32342 observations

   1253-055          12 53 35.831306   * 12 56 11.166574     12 57 10.730876       0.10
 * J1256-0547       -05 31 07.99629    *-05 47 21.52515     -05 53 32.95880        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  14021 observations

   1546+027          15 46 58.292172   * 15 49 29.436846     15 50 26.513040       0.10
 * J1549+0237        02 46 06.07588    * 02 37 01.16323      02 33 32.74636        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  28615 observations

   1555-140          15 55 33.749896   * 15 58 21.947995     15 59 25.469790       0.18
 * J1558-1409       -14 01 26.50709    *-14 09 59.05322     -14 13 08.99929        0.29
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  221 observations

   1625-141          16 25 57.284276   * 16 28 46.619750     16 29 50.373438       0.21
 * J1628-1415       -14 09 07.75118    *-14 15 41.88634     -14 18 06.78686        0.42
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  105 observations

   1641+399          16 41 17.606226   * 16 42 58.809963     16 43 36.608067       0.13
 * J1642+3948        39 54 10.81487    * 39 48 36.99393      39 46 18.21672        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  52534 observations

   1741-038          17 41 20.616012   * 17 43 58.856136     17 44 57.956813       0.10
 * J1743-0350       -03 48 48.89994    *-03 50 04.61674     -03 50 32.99091        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  244125 observations

   1758+388          17 58 44.703949   * 18 00 24.765358     18 01 01.663213       0.13
 * J1800+3848        38 48 32.47351    * 38 48 30.69749      38 48 18.95193        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  5981 observations

 * 1934-638          19 34 47.602806   * 19 39 25.022408     19 41 06.574080       0.88
   J1939-6342       -63 49 37.72332    *-63 42 45.62520     -63 39 55.65187        0.37
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  82 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  SCOX1OFF   sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +    18.028   775.074
  J1229+0203 sess119.X1024glob     1 2 4 5 6 7 9 22                  0.217     6.159
  J1256-0547 sess119.X1024glob     1 4 5 7 9 11 12 13 15 16 17 +     0.050     7.400
  J1549+0237 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     0.106    12.510
  J1558-1409 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     0.597    26.848
  J1628-1415 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     7.161   282.487
  J1642+3948 sess119.X1024glob     11 12 13 15 16 17 18 20 21  +     0.164    12.921
  J1743-0350 sess119.X1024glob     1 2 4 5 6 7 9 22                  0.083     2.607
  J1800+3848 sess119.X1024glob     6 7 22                            0.100     1.747
  1934-638   sess119.X1024glob     1                                 0.250     0.000


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SCOX1OFF            88.2
   J1229+0203         147.8
   J1256-0547         138.8
   J1549+0237          98.9
   J1558-1409          93.6
   J1628-1415          86.3
   J1642+3948          92.7
   J1743-0350          69.6
   J1800+3848          78.2
   1934-638            61.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

