  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Probing the disc-jet coupling in the neutron star binary Sco X-1
 Exp. Code:  gm074c  


Schedule Version:       2.30
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Sara Motta

Address:  University of Oxford
          Department of Physics, Astrophysics
          Denys Wilkinson Building, Keble Road
          Oxford OX1 3RH, UK

Phone:    +44-1865-283133
EMAIL:    sara.motta@physics.ox.ac.uk
Fax:
Phone during observation: +61-4-8848-4825

Observing mode: LBA,EVN,VLBA 8.4 GHz continuum

Notes:    Target (phase ref):                 Sco X-1 (J1628-1415)
          In-beam cal:                                       NEIBC
          Fringe finders: J1229+0203,1921-293,J1642+3948,J1800+3848,J1549+0237,J1256-0547,J1743-0350,J2253+1608
          ATCA phasing source:          J1558-1409, Fringe Finders

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

 Next scan frequencies:  8331.00  8331.00  8363.00  8363.00  8395.00  8395.00  8427.00  8427.00
 Next BBC frequencies:    731.00   731.00   763.00   763.00   795.00   795.00   827.00   827.00
 Next scan bandwidths:     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00

08 00 00  J1642+3948   11 19 53  25.5  57.2 -5.4     -70.3     0        0   08 00 00
08 05 10  =1641+399    11 25 03  26.4  57.6 -5.3     -70.9   310       40   08 00 01

08 05 50  J1628-1415   11 25 44   4.3 109.4 -5.1     -56.9   -11       40   08 06 01
08 10 00  =1625-141    11 29 54   5.2 110.0 -5.0     -56.6   239       71   08 05 51

08 10 00  SCOX1OFF     11 29 54   6.2 112.3 -4.9     -55.8   -10       71   08 10 10
08 13 30  ---          11 33 25   6.9 112.8 -4.8     -55.5   200       96   08 10 01

08 13 30  J1628-1415   11 33 25   5.9 110.5 -4.9     -56.3   -10       96   08 13 40
08 14 50  =1625-141    11 34 45   6.1 110.6 -4.9     -56.2    70      106   08 13 31

08 14 50  SCOX1OFF     11 34 45   7.1 113.0 -4.8     -55.4   -10      106   08 15 00
08 18 20  ---          11 38 16   7.8 113.5 -4.7     -55.1   200      131   08 14 51

08 19 00  J1628-1415   11 38 56   7.0 111.2 -4.8     -55.9    30      131   08 19 00
08 20 10  =1625-141    11 40 06   7.2 111.4 -4.8     -55.8    70      140   08 19 01

08 20 10  SCOX1OFF     11 40 06   8.2 113.7 -4.7     -54.9   -10      140   08 20 20
08 23 40  ---          11 43 36   8.9 114.2 -4.6     -54.6   200      166   08 20 11

08 23 40  J1628-1415   11 43 36   7.9 111.9 -4.8     -55.5   -10      166   08 23 50
08 25 00  =1625-141    11 44 57   8.2 112.0 -4.7     -55.4    70      175   08 23 41

08 25 00  SCOX1OFF     11 44 57   9.1 114.4 -4.6     -54.5   -10      175   08 25 10
08 28 30  ---          11 48 27   9.8 114.9 -4.5     -54.1   200      201   08 25 01

08 28 30  J1628-1415   11 48 27   8.9 112.5 -4.7     -55.1   -10      201   08 28 40
08 29 50  =1625-141    11 49 48   9.2 112.7 -4.7     -55.0    70      210   08 28 31

08 29 50  SCOX1OFF     11 49 48  10.1 115.1 -4.5     -54.0   -10      210   08 30 00
08 33 20  ---          11 53 18  10.8 115.6 -4.5     -53.7   200      236   08 29 51

08 34 00  J1628-1415   11 53 58  10.0 113.3 -4.6     -54.6    30      236   08 34 00
08 35 10  =1625-141    11 55 08  10.2 113.5 -4.6     -54.5    70      245   08 34 01

08 35 10  SCOX1OFF     11 55 08  11.1 115.9 -4.4     -53.5   -10      245   08 35 20
08 38 40  ---          11 58 39  11.8 116.4 -4.4     -53.2   200      270   08 35 11

08 38 40  J1628-1415   11 58 39  10.9 114.0 -4.5     -54.2   -10      270   08 38 50
08 40 00  =1625-141    11 59 59  11.2 114.2 -4.5     -54.1    70      279   08 38 41
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

08 40 00  SCOX1OFF     11 59 59  12.1 116.6 -4.4     -53.0   -10      279   08 40 10
08 43 30  ---          12 03 30  12.7 117.1 -4.3     -52.7   200      305   08 40 01

08 43 30  J1628-1415   12 03 30  11.9 114.7 -4.4     -53.8   -10      305   08 43 40
08 44 50  =1625-141    12 04 50  12.1 114.9 -4.4     -53.7    70      314   08 43 31

08 44 50  SCOX1OFF     12 04 50  13.0 117.3 -4.3     -52.6   -10      314   08 45 00
08 48 20  ---          12 08 21  13.7 117.9 -4.2     -52.2   200      340   08 44 51

08 49 00  J1628-1415   12 09 01  12.9 115.5 -4.3     -53.3    30      340   08 49 00
08 50 10  =1625-141    12 10 11  13.2 115.7 -4.3     -53.2    70      349   08 49 01

08 50 10  SCOX1OFF     12 10 11  14.0 118.1 -4.2     -52.0   -10      349   08 50 20
08 53 40  ---          12 13 41  14.7 118.7 -4.1     -51.6   200      375   08 50 11

08 53 40  J1628-1415   12 13 41  13.8 116.2 -4.3     -52.8   -10      375   08 53 50
08 55 00  =1625-141    12 15 02  14.1 116.4 -4.2     -52.7    70      384   08 53 41

08 55 00  SCOX1OFF     12 15 02  14.9 118.9 -4.1     -51.5   -10      384   08 55 10
08 58 40  ---          12 18 42  15.6 119.5 -4.0     -51.1   210      411   08 55 01

08 58 40  J1628-1415   12 18 42  14.8 117.0 -4.2     -52.3   -10      411   08 58 50
09 00 00  =1625-141    12 20 02  15.1 117.2 -4.2     -52.2    70      420   08 58 41

 ---------- >>>> EFLSBERG pointing scan <<<< ----------

09 00 00  SCOX1OFF     12 20 02  15.9 119.7 -4.0     -50.9   -10      420   09 00 10
09 03 20  ---          12 23 23  16.5 120.2 -4.0     -50.6   190      444   09 00 01

09 04 00  J1628-1415   12 24 03  15.8 117.8 -4.1     -51.8    30      444   09 04 00
09 05 10  =1625-141    12 25 13  16.0 118.0 -4.1     -51.6    70      453   09 04 01

09 05 10  SCOX1OFF     12 25 13  16.8 120.5 -3.9     -50.4   -10      453   09 05 20
09 08 40  ---          12 28 44  17.5 121.1 -3.9     -50.0   200      479   09 05 11

09 08 40  J1628-1415   12 28 44  16.7 118.5 -4.0     -51.3   -10      479   09 08 50
09 10 00  =1625-141    12 30 04  17.0 118.7 -4.0     -51.1    70      488   09 08 41

09 10 00  SCOX1OFF     12 30 04  17.7 121.3 -3.8     -49.8   -10      488   09 10 10
09 13 30  ---          12 33 35  18.4 121.8 -3.8     -49.4   200      514   09 10 01

09 13 30  J1628-1415   12 33 35  17.6 119.3 -3.9     -50.7   -10      514   09 13 40
09 14 50  =1625-141    12 34 55  17.9 119.5 -3.9     -50.6    70      523   09 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

09 14 50  SCOX1OFF     12 34 55  18.6 122.1 -3.8     -49.2   -10      523   09 15 00
09 18 20  ---          12 38 25  19.3 122.7 -3.7     -48.8   200      549   09 14 51

09 19 00  J1628-1415   12 39 06  18.7 120.2 -3.8     -50.1    30      549   09 19 00
09 20 10  =1625-141    12 40 16  18.9 120.4 -3.8     -50.0    70      558   09 19 01

09 20 10  SCOX1OFF     12 40 16  19.6 123.0 -3.7     -48.6   -10      558   09 20 20
09 23 40  ---          12 43 46  20.2 123.6 -3.6     -48.1   200      583   09 20 11

09 23 40  J1628-1415   12 43 46  19.5 121.0 -3.8     -49.6   -10      583   09 23 50
09 25 00  =1625-141    12 45 07  19.8 121.2 -3.7     -49.4    70      592   09 23 41

09 25 00  SCOX1OFF     12 45 07  20.5 123.8 -3.6     -48.0   -10      592   09 25 10
09 28 30  ---          12 48 37  21.1 124.4 -3.5     -47.5   200      618   09 25 01

09 28 30  J1628-1415   12 48 37  20.4 121.8 -3.7     -49.0   -10      618   09 28 40
09 29 50  =1625-141    12 49 57  20.7 122.0 -3.7     -48.8    70      627   09 28 31

09 29 50  SCOX1OFF     12 49 57  21.3 124.6 -3.5     -47.3   -10      627   09 30 00
09 33 20  ---          12 53 28  21.9 125.2 -3.5     -46.9   200      653   09 29 51

09 34 00  J1628-1415   12 54 08  21.4 122.7 -3.6     -48.3    30      653   09 34 00
09 35 10  =1625-141    12 55 18  21.6 122.9 -3.6     -48.2    70      662   09 34 01

09 35 10  SCOX1OFF     12 55 18  22.3 125.6 -3.4     -46.6   -10      662   09 35 20
09 38 40  ---          12 58 49  22.9 126.2 -3.4     -46.1   200      688   09 35 11

09 38 40  J1628-1415   12 58 49  22.3 123.5 -3.5     -47.7   -10      688   09 38 50
09 40 00  =1625-141    13 00 09  22.5 123.8 -3.5     -47.6    70      697   09 38 41

09 40 00  SCOX1OFF     13 00 09  23.1 126.4 -3.3     -46.0   -10      697   09 40 10
09 43 30  ---          13 03 40  23.7 127.1 -3.3     -45.5   200      723   09 40 01

09 43 30  J1628-1415   13 03 40  23.1 124.4 -3.4     -47.1   -10      723   09 43 40
09 44 50  =1625-141    13 05 00  23.4 124.6 -3.4     -46.9    70      732   09 43 31

09 44 50  SCOX1OFF     13 05 00  23.9 127.3 -3.3     -45.3   -10      732   09 45 00
09 48 20  ---          13 08 30  24.5 128.0 -3.2     -44.8   200      757   09 44 51

09 49 00  J1628-1415   13 09 11  24.1 125.4 -3.3     -46.4    30      757   09 49 00
09 50 10  =1625-141    13 10 21  24.3 125.6 -3.3     -46.2    70      766   09 49 01

09 50 10  SCOX1OFF     13 10 21  24.8 128.3 -3.2     -44.5   -10      766   09 50 20
09 53 40  ---          13 13 51  25.4 129.0 -3.1     -44.0   200      792   09 50 11
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

09 53 40  J1628-1415   13 13 51  24.9 126.3 -3.3     -45.7   -10      792   09 53 50
09 55 00  =1625-141    13 15 12  25.1 126.5 -3.2     -45.5    70      801   09 53 41

09 55 00  SCOX1OFF     13 15 12  25.7 129.3 -3.1     -43.8   -10      801   09 55 10
09 58 40  ---          13 18 52  26.3 130.0 -3.0     -43.2   210      828   09 55 01

09 58 40  J1628-1415   13 18 52  25.8 127.2 -3.2     -45.0   -10      828   09 58 50
10 00 00  =1625-141    13 20 12  26.0 127.5 -3.2     -44.8    70      837   09 58 41

10 00 00  SCOX1OFF     13 20 12  26.5 130.2 -3.0     -43.0   -10      837   10 00 10
10 03 40  ---          13 23 53  27.1 131.0 -3.0     -42.4   210      864   10 00 01

10 03 40  J1628-1415   13 23 53  26.6 128.2 -3.1     -44.3   -10      864   10 03 50
10 05 00  =1625-141    13 25 13  26.9 128.4 -3.1     -44.1    70      873   10 03 41

10 05 00  SCOX1OFF     13 25 13  27.3 131.2 -2.9     -42.2   -10      873   10 05 10
10 08 40  ---          13 28 54  27.9 132.0 -2.9     -41.6   210      900   10 05 01

10 08 40  J1628-1415   13 28 54  27.5 129.2 -3.0     -43.5   -10      900   10 08 50
10 10 00  =1625-141    13 30 14  27.7 129.4 -3.0     -43.3    70      909   10 08 41

10 10 00  SCOX1OFF     13 30 14  28.1 132.3 -2.8     -41.4   -10      909   10 10 10
10 13 40  ---          13 33 55  28.7 133.0 -2.8     -40.8   210      936   10 10 01

10 13 40  J1628-1415   13 33 55  28.3 130.2 -2.9     -42.7   -10      936   10 13 50
10 15 00  =1625-141    13 35 15  28.5 130.4 -2.9     -42.5    70      945   10 13 41

10 15 00  SCOX1OFF     13 35 15  28.9 133.3 -2.8     -40.6   -10      945   10 15 10
10 18 40  ---          13 38 55  29.5 134.1 -2.7     -40.0   210      972   10 15 01

10 18 40  J1628-1415   13 38 55  29.1 131.2 -2.8     -41.9   -10      972   10 18 50
10 20 00  =1625-141    13 40 16  29.3 131.5 -2.8     -41.7    70      981   10 18 41

10 20 00  SCOX1OFF     13 40 16  29.7 134.3 -2.7     -39.7   -10      981   10 20 10
10 23 40  ---          13 43 56  30.2 135.1 -2.6     -39.1   210     1009   10 20 01

10 23 40  J1628-1415   13 43 56  29.9 132.2 -2.8     -41.1   -10     1009   10 23 50
10 25 00  =1625-141    13 45 16  30.1 132.5 -2.7     -40.9    70     1018   10 23 41

10 25 00  SCOX1OFF     13 45 16  30.4 135.4 -2.6     -38.8   -10     1018   10 25 10
10 28 40  ---          13 48 57  31.0 136.2 -2.5     -38.2   210     1045   10 25 01

10 28 40  J1628-1415   13 48 57  30.7 133.3 -2.7     -40.3   -10     1045   10 28 50
10 30 00  =1625-141    13 50 17  30.9 133.6 -2.7     -40.0    70     1054   10 28 41
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

10 30 00  SCOX1OFF     13 50 17  31.2 136.5 -2.5     -37.9   -10     1054   10 30 10
10 33 40  ---          13 53 58  31.7 137.3 -2.5     -37.3   210     1081   10 30 01

10 33 40  J1628-1415   13 53 58  31.5 134.4 -2.6     -39.4   -10     1081   10 33 50
10 35 00  =1625-141    13 55 18  31.7 134.7 -2.6     -39.2    70     1090   10 33 41

10 35 00  SCOX1OFF     13 55 18  31.9 137.7 -2.4     -37.0   -10     1090   10 35 10
10 38 40  ---          13 58 59  32.5 138.5 -2.4     -36.3   210     1117   10 35 01

10 38 40  J1628-1415   13 58 59  32.3 135.5 -2.5     -38.5   -10     1117   10 38 50
10 40 00  =1625-141    14 00 19  32.5 135.8 -2.5     -38.2    70     1126   10 38 41

10 40 00  SCOX1OFF     14 00 19  32.6 138.8 -2.3     -36.1   -10     1126   10 40 10
10 43 40  ---          14 03 59  33.2 139.7 -2.3     -35.3   210     1153   10 40 01

10 43 40  J1628-1415   14 03 59  33.0 136.6 -2.4     -37.6   -10     1153   10 43 50
10 45 00  =1625-141    14 05 20  33.2 136.9 -2.4     -37.3    70     1162   10 43 41

10 45 00  SCOX1OFF     14 05 20  33.4 140.0 -2.3     -35.1   -10     1162   10 45 10
10 48 40  ---          14 09 00  33.9 140.8 -2.2     -34.4   210     1189   10 45 01

10 48 40  J1628-1415   14 09 00  33.7 137.8 -2.3     -36.6   -10     1189   10 48 50
10 50 00  =1625-141    14 10 21  33.9 138.1 -2.3     -36.4    70     1198   10 48 41

10 50 00  SCOX1OFF     14 10 21  34.0 141.2 -2.2     -34.1   -10     1198   10 50 10
10 53 40  ---          14 14 01  34.5 142.1 -2.1     -33.3   210     1225   10 50 01

10 53 40  J1628-1415   14 14 01  34.5 139.0 -2.3     -35.6   -10     1225   10 53 50
10 55 00  =1625-141    14 15 21  34.6 139.3 -2.2     -35.4    70     1234   10 53 41

10 55 00  SCOX1OFF     14 15 21  34.7 142.4 -2.1     -33.1   -10     1234   10 55 10
10 58 40  ---          14 19 02  35.2 143.3 -2.0     -32.3   210     1261   10 55 01

10 58 40  J1628-1415   14 19 02  35.2 140.2 -2.2     -34.6   -10     1261   10 58 50
11 00 00  =1625-141    14 20 22  35.3 140.5 -2.2     -34.4    70     1270   10 58 41

11 00 00  SCOX1OFF     14 20 22  35.4 143.6 -2.0     -32.0   -10     1270   11 00 10
11 03 40  ---          14 24 03  35.8 144.6 -1.9     -31.2   210     1297   11 00 01

11 03 40  J1628-1415   14 24 03  35.8 141.4 -2.1     -33.6   -10     1297   11 03 50
11 05 00  =1625-141    14 25 23  36.0 141.8 -2.1     -33.3    70     1306   11 03 41

11 05 00  SCOX1OFF     14 25 23  36.0 144.9 -1.9     -30.9   -10     1306   11 05 10
11 08 40  ---          14 29 04  36.4 145.8 -1.9     -30.1   210     1333   11 05 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

11 08 40  J1628-1415   14 29 04  36.5 142.7 -2.0     -32.6   -10     1333   11 08 50
11 10 00  =1625-141    14 30 24  36.7 143.0 -2.0     -32.3    70     1342   11 08 41

11 10 00  SCOX1OFF     14 30 24  36.6 146.2 -1.8     -29.8   -10     1342   11 10 10
11 13 40  ---          14 34 04  37.0 147.1 -1.8     -29.0   210     1369   11 10 01

11 13 40  J1628-1415   14 34 04  37.1 144.0 -1.9     -31.5   -10     1369   11 13 50
11 15 00  =1625-141    14 35 25  37.3 144.3 -1.9     -31.2    70     1378   11 13 41

11 15 00  SCOX1OFF     14 35 25  37.2 147.5 -1.8     -28.7   -10     1378   11 15 10
11 18 40  ---          14 39 05  37.6 148.5 -1.7     -27.9   210     1405   11 15 01

11 18 40  J1628-1415   14 39 05  37.8 145.3 -1.8     -30.4   -10     1405   11 18 50
11 20 00  =1625-141    14 40 25  37.9 145.6 -1.8     -30.1    70     1414   11 18 41

11 20 00  SCOX1OFF     14 40 25  37.8 148.8 -1.7     -27.5   -10     1414   11 20 10
11 23 40  ---          14 44 06  38.2 149.8 -1.6     -26.7   210     1441   11 20 01

11 23 40  J1628-1415   14 44 06  38.4 146.6 -1.8     -29.2   -10     1441   11 23 50
11 25 00  =1625-141    14 45 26  38.5 147.0 -1.7     -28.9    70     1450   11 23 41

11 25 00  SCOX1OFF     14 45 26  38.3 150.2 -1.6     -26.4   -10     1450   11 25 10
11 28 40  ---          14 49 07  38.7 151.2 -1.5     -25.5   210     1477   11 25 01

11 28 40  J1628-1415   14 49 07  39.0 148.0 -1.7     -28.1   -10     1477   11 28 50
11 30 00  =1625-141    14 50 27  39.1 148.4 -1.7     -27.8    70     1486   11 28 41

11 30 00  SCOX1OFF     14 50 27  38.8 151.6 -1.5     -25.2   -10     1486   11 30 10
11 33 40  ---          14 54 08  39.2 152.6 -1.4     -24.3   210     1513   11 30 01

11 33 40  J1628-1415   14 54 08  39.5 149.4 -1.6     -26.9   -10     1513   11 33 50
11 35 00  =1625-141    14 55 28  39.7 149.8 -1.6     -26.6    70     1523   11 33 41

11 35 00  SCOX1OFF     14 55 28  39.3 153.0 -1.4     -23.9   -10     1523   11 35 10
11 38 40  ---          14 59 09  39.7 154.1 -1.4     -23.0   210     1550   11 35 01

11 38 40  J1628-1415   14 59 09  40.0 150.8 -1.5     -25.7   -10     1550   11 38 50
11 40 00  =1625-141    15 00 29  40.2 151.2 -1.5     -25.3    70     1559   11 38 41

11 40 00  SCOX1OFF     15 00 29  39.8 154.4 -1.3     -22.7   -10     1559   11 40 10
11 43 40  ---          15 04 09  40.1 155.5 -1.3     -21.7   210     1586   11 40 01

11 43 40  J1628-1415   15 04 09  40.6 152.2 -1.4     -24.4   -10     1586   11 43 50
11 45 00  =1625-141    15 05 30  40.7 152.6 -1.4     -24.1    70     1595   11 43 41
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

11 45 00  SCOX1OFF     15 05 30  40.3 155.9 -1.3     -21.4   -10     1595   11 45 10
11 48 40  ---          15 09 10  40.6 157.0 -1.2     -20.4   210     1622   11 45 01

11 48 40  J1628-1415   15 09 10  41.1 153.7 -1.3     -23.2   -10     1622   11 48 50
11 50 00  =1625-141    15 10 30  41.2 154.1 -1.3     -22.8    70     1631   11 48 41

11 50 00  SCOX1OFF     15 10 30  40.7 157.4 -1.2     -20.1   -10     1631   11 50 10
11 53 40  ---          15 14 11  41.0 158.5 -1.1     -19.1   210     1658   11 50 01

11 53 40  J1628-1415   15 14 11  41.5 155.2 -1.3     -21.9   -10     1658   11 53 50
11 55 00  =1625-141    15 15 31  41.6 155.6 -1.2     -21.5    70     1667   11 53 41

11 55 00  SCOX1OFF     15 15 31  41.1 158.9 -1.1     -18.8   -10     1667   11 55 10
11 58 40  ---          15 19 12  41.4 160.0 -1.0     -17.8   210     1694   11 55 01

11 58 40  J1628-1415   15 19 12  42.0 156.7 -1.2     -20.6   -10     1694   11 58 50
12 00 00  =1625-141    15 20 32  42.1 157.1 -1.2     -20.2    70     1703   11 58 41

12 00 30  J1229+0203   15 21 02  40.5 243.0  2.8      50.1   -39     1703   12 01 09
12 06 00  =1226+023    15 26 33  39.4 244.2  2.9      50.8   291     1740   12 00 31

12 06 00  J1628-1415   15 26 33  42.6 159.0 -1.1     -18.6   -68     1740   12 07 08
12 10 00  =1625-141    15 30 34  42.9 160.2 -1.0     -17.5   172     1763   12 06 01

12 10 00  SCOX1OFF     15 30 34  42.1 163.5 -0.8     -14.7   -10     1763   12 10 10
12 13 40  ---          15 34 14  42.3 164.7 -0.8     -13.6   210     1790   12 10 01

12 13 40  J1628-1415   15 34 14  43.1 161.4 -0.9     -16.4   -10     1790   12 13 50
12 15 00  =1625-141    15 35 35  43.2 161.8 -0.9     -16.1    70     1799   12 13 41

12 15 00  SCOX1OFF     15 35 35  42.4 165.1 -0.8     -13.3   -10     1799   12 15 10
12 18 40  ---          15 39 15  42.6 166.3 -0.7     -12.2   210     1826   12 15 01

12 18 40  J1628-1415   15 39 15  43.4 163.0 -0.8     -15.0   -10     1826   12 18 50
12 20 00  =1625-141    15 40 35  43.5 163.4 -0.8     -14.7    70     1835   12 18 41

12 20 00  SCOX1OFF     15 40 35  42.7 166.7 -0.7     -11.9   -10     1835   12 20 10
12 23 40  ---          15 44 16  42.9 167.9 -0.6     -10.8   210     1862   12 20 01

12 23 40  J1628-1415   15 44 16  43.7 164.6 -0.8     -13.6   -10     1862   12 23 50
12 25 00  =1625-141    15 45 36  43.8 165.1 -0.7     -13.2    70     1871   12 23 41

12 25 00  SCOX1OFF     15 45 36  42.9 168.3 -0.6     -10.4   -10     1871   12 25 10
12 28 40  ---          15 49 17  43.1 169.5 -0.5      -9.4   210     1898   12 25 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

12 28 40  J1628-1415   15 49 17  44.0 166.3 -0.7     -12.2   -10     1898   12 28 50
12 30 00  =1625-141    15 50 37  44.1 166.7 -0.7     -11.8    70     1907   12 28 41

12 30 00  SCOX1OFF     15 50 37  43.1 170.0 -0.5      -9.0   -10     1907   12 30 10
12 33 40  ---          15 54 18  43.2 171.2 -0.4      -7.9   210     1934   12 30 01

12 33 40  J1628-1415   15 54 18  44.3 167.9 -0.6     -10.7   -10     1934   12 33 50
12 35 00  =1625-141    15 55 38  44.3 168.4 -0.6     -10.3    70     1943   12 33 41

12 35 00  SCOX1OFF     15 55 38  43.3 171.6 -0.4      -7.5   -10     1943   12 35 10
12 38 40  ---          15 59 18  43.4 172.8 -0.4      -6.4   210     1970   12 35 01

12 38 40  J1628-1415   15 59 18  44.5 169.6 -0.5      -9.2   -10     1970   12 38 50
12 40 00  =1625-141    16 00 39  44.5 170.1 -0.5      -8.8    70     1979   12 38 41

12 40 00  SCOX1OFF     16 00 39  43.4 173.2 -0.3      -6.0   -10     1979   12 40 10
12 43 40  ---          16 04 19  43.5 174.5 -0.3      -5.0   210     2006   12 40 01

12 43 40  J1628-1415   16 04 19  44.6 171.3 -0.4      -7.7   -10     2006   12 43 50
12 45 00  =1625-141    16 05 39  44.7 171.7 -0.4      -7.3    70     2015   12 43 41

12 45 00  SCOX1OFF     16 05 39  43.5 174.9 -0.3      -4.6   -10     2015   12 45 10
12 48 40  ---          16 09 20  43.6 176.1 -0.2      -3.5   210     2042   12 45 01

12 48 40  J1628-1415   16 09 20  44.8 173.0 -0.3      -6.2   -10     2042   12 48 50
12 50 00  =1625-141    16 10 40  44.8 173.4 -0.3      -5.8    70     2051   12 48 41

12 50 00  SCOX1OFF     16 10 40  43.6 176.6 -0.2      -3.1   -10     2051   12 50 10
12 53 40  ---          16 14 21  43.7 177.8 -0.1      -2.0   210     2078   12 50 01

12 53 40  J1628-1415   16 14 21  44.9 174.7 -0.3      -4.7   -10     2078   12 53 50
12 55 00  =1625-141    16 15 41  44.9 175.2 -0.2      -4.3    70     2087   12 53 41

12 55 00  SCOX1OFF     16 15 41  43.7 178.2 -0.1      -1.6   -11     2087   12 55 11
12 58 40  ---          16 19 22  43.7 179.5 -0.0      -0.5   209     2114   12 55 01

12 58 40  J1628-1415   16 19 22  45.0 176.4 -0.2      -3.2   -11     2114   12 58 51
13 00 00  =1625-141    16 20 42  45.0 176.9 -0.2      -2.8    69     2123   12 58 41

13 00 00  SCOX1OFF     16 20 42  43.7 179.9 -0.0      -0.1   -11     2123   13 00 11
13 03 40  ---          16 24 22  43.7 181.1  0.1       1.0   209     2150   13 00 01

13 03 40  J1628-1415   16 24 22  45.0 178.1 -0.1      -1.7   -11     2150   13 03 51
13 05 00  =1625-141    16 25 43  45.1 178.6 -0.1      -1.3    69     2159   13 03 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

13 05 00  SCOX1OFF     16 25 43  43.7 181.6  0.1       1.4   -11     2159   13 05 11
13 08 40  ---          16 29 23  43.6 182.8  0.1       2.5   209     2186   13 05 01

13 08 40  J1628-1415   16 29 23  45.1 179.8 -0.0      -0.1   -11     2186   13 08 51
13 10 00  =1625-141    16 30 44  45.1 180.3  0.0       0.3    69     2195   13 08 41

13 10 00  SCOX1OFF     16 30 44  43.6 183.2  0.2       2.9   -11     2195   13 10 11
13 13 40  ---          16 34 24  43.6 184.5  0.2       4.0   209     2221   13 10 01

13 13 40  J1628-1415   16 34 24  45.0 181.6  0.1       1.4   -11     2221   13 13 51
13 15 00  =1625-141    16 35 44  45.0 182.0  0.1       1.8    69     2230   13 13 41

13 15 00  SCOX1OFF     16 35 44  43.6 184.9  0.2       4.4   -11     2230   13 15 11
13 18 40  ---          16 39 25  43.5 186.1  0.3       5.5   209     2257   13 15 01

13 18 40  J1628-1415   16 39 25  45.0 183.3  0.2       2.9   -11     2257   13 18 51
13 20 00  =1625-141    16 40 45  45.0 183.7  0.2       3.3    69     2266   13 18 41

13 20 00  SCOX1OFF     16 40 45  43.4 186.6  0.3       5.9   -11     2266   13 20 11
13 23 40  ---          16 44 26  43.3 187.8  0.4       6.9   209     2293   13 20 01

13 23 40  J1628-1415   16 44 26  44.9 185.0  0.2       4.4   -11     2293   13 23 51
13 25 00  =1625-141    16 45 46  44.9 185.5  0.3       4.8    69     2302   13 23 41

13 25 00  SCOX1OFF     16 45 46  43.3 188.2  0.4       7.3   -11     2302   13 25 11
13 28 40  ---          16 49 27  43.2 189.4  0.5       8.4   209     2329   13 25 01

13 28 40  J1628-1415   16 49 27  44.8 186.7  0.3       5.9   -11     2329   13 28 51
13 30 00  =1625-141    16 50 47  44.8 187.2  0.3       6.4    69     2338   13 28 41

13 30 00  SCOX1OFF     16 50 47  43.1 189.8  0.5       8.8   -11     2338   13 30 11
13 33 40  ---          16 54 27  43.0 191.0  0.6       9.9   209     2365   13 30 01

13 33 40  J1628-1415   16 54 27  44.7 188.4  0.4       7.5   -11     2365   13 33 51
13 35 00  =1625-141    16 55 48  44.6 188.9  0.4       7.9    69     2374   13 33 41

13 35 00  SCOX1OFF     16 55 48  42.9 191.5  0.6      10.2   -11     2374   13 35 11
13 38 40  ---          16 59 28  42.8 192.7  0.6      11.3   209     2401   13 35 01

13 38 40  J1628-1415   16 59 28  44.5 190.1  0.5       8.9   -11     2401   13 38 51
13 40 00  =1625-141    17 00 48  44.4 190.5  0.5       9.3    69     2409   13 38 41

13 40 00  SCOX1OFF     17 00 48  42.7 193.1  0.7      11.7   -11     2409   13 40 11
13 43 40  ---          17 04 29  42.5 194.3  0.7      12.7   209     2436   13 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

13 43 40  J1628-1415   17 04 29  44.3 191.8  0.6      10.4   -12     2436   13 43 52
13 45 00  =1625-141    17 05 49  44.2 192.2  0.6      10.8    68     2445   13 43 41

13 45 00  SCOX1OFF     17 05 49  42.5 194.7  0.7      13.1   -12     2445   13 45 12
13 48 40  ---          17 09 30  42.2 195.8  0.8      14.1   208     2472   13 45 01

13 48 40  J1628-1415   17 09 30  44.1 193.4  0.7      11.9   -12     2472   13 48 52
13 50 00  =1625-141    17 10 50  44.0 193.9  0.7      12.3    68     2481   13 48 41

13 50 00  SCOX1OFF     17 10 50  42.2 196.3  0.8      14.5   -12     2481   13 50 12
13 53 40  ---          17 14 31  41.9 197.4  0.9      15.5   208     2507   13 50 01

13 53 40  J1628-1415   17 14 31  43.8 195.1  0.7      13.3   -12     2507   13 53 52
13 55 00  =1625-141    17 15 51  43.7 195.5  0.8      13.7    68     2516   13 53 41

13 55 00  SCOX1OFF     17 15 51  41.8 197.8  0.9      15.9   -12     2516   13 55 12
13 58 40  ---          17 19 32  41.6 199.0  1.0      16.9   208     2543   13 55 01

13 58 40  J1628-1415   17 19 32  43.5 196.7  0.8      14.8   -12     2543   13 58 52
14 00 00  =1625-141    17 20 52  43.4 197.1  0.9      15.2    68     2552   13 58 41

14 00 00  SCOX1OFF     17 20 52  41.5 199.4  1.0      17.3   -12     2552   14 00 12
14 03 40  ---          17 24 32  41.2 200.5  1.1      18.2   208     2579   14 00 01

14 03 40  J1628-1415   17 24 32  43.2 198.3  0.9      16.2   -12     2579   14 03 52
14 05 00  =1625-141    17 25 53  43.1 198.7  0.9      16.6    68     2587   14 03 41

14 05 00  SCOX1OFF     17 25 53  41.1 200.9  1.1      18.6   -12     2587   14 05 12
14 08 40  ---          17 29 33  40.8 202.0  1.1      19.6   208     2614   14 05 01

14 08 40  J1628-1415   17 29 33  42.8 199.9  1.0      17.6   -12     2614   14 08 52
14 10 00  =1625-141    17 30 53  42.7 200.3  1.0      18.0    68     2623   14 08 41

14 10 00  SCOX1OFF     17 30 53  40.7 202.4  1.2      19.9   -12     2623   14 10 12
14 13 40  ---          17 34 34  40.4 203.5  1.2      20.9   208     2650   14 10 01

14 13 40  J1628-1415   17 34 34  42.4 201.5  1.1      19.0   -12     2650   14 13 52
14 15 00  =1625-141    17 35 54  42.3 201.9  1.1      19.3    68     2658   14 13 41

14 15 00  SCOX1OFF     17 35 54  40.3 203.9  1.2      21.2   -12     2658   14 15 12
14 18 40  ---          17 39 35  40.0 205.0  1.3      22.2   208     2685   14 15 01

14 18 40  J1628-1415   17 39 35  42.0 203.0  1.2      20.3   -12     2685   14 18 52
14 20 00  =1625-141    17 40 55  41.9 203.4  1.2      20.7    68     2694   14 18 41
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

14 20 00  SCOX1OFF     17 40 55  39.9 205.4  1.3      22.5   -12     2694   14 20 12
14 23 40  ---          17 44 36  39.5 206.4  1.4      23.4   208     2721   14 20 01

14 23 40  J1628-1415   17 44 36  41.6 204.5  1.2      21.6   -12     2721   14 23 52
14 25 00  =1625-141    17 45 56  41.5 204.9  1.3      22.0    68     2730   14 23 41

14 25 00  SCOX1OFF     17 45 56  39.4 206.8  1.4      23.8   -12     2730   14 25 12
14 28 40  ---          17 49 36  39.0 207.9  1.5      24.7   208     2756   14 25 01

14 28 40  J1628-1415   17 49 36  41.1 206.0  1.3      22.9   -12     2756   14 28 52
14 30 00  =1625-141    17 50 57  41.0 206.4  1.4      23.3    68     2765   14 28 41

14 30 00  SCOX1OFF     17 50 57  38.9 208.2  1.5      25.0   -12     2765   14 30 12
14 33 40  ---          17 54 37  38.5 209.3  1.6      25.9   208     2792   14 30 01

14 33 40  J1628-1415   17 54 37  40.7 207.5  1.4      24.2   -12     2792   14 33 52
14 35 00  =1625-141    17 55 58  40.5 207.9  1.4      24.5    68     2801   14 33 41

14 35 00  SCOX1OFF     17 55 58  38.4 209.6  1.6      26.2   -12     2801   14 35 12
14 38 40  ---          17 59 38  38.0 210.6  1.6      27.1   208     2827   14 35 01

14 38 40  J1628-1415   17 59 38  40.1 209.0  1.5      25.5   -12     2827   14 38 52
14 40 00  =1625-141    18 00 58  40.0 209.3  1.5      25.8    68     2836   14 38 41

14 40 00  SCOX1OFF     18 00 58  37.8 211.0  1.7      27.4   -12     2836   14 40 12
14 43 40  ---          18 04 39  37.4 212.0  1.7      28.2   208     2863   14 40 01

14 43 40  J1628-1415   18 04 39  39.6 210.4  1.6      26.7   -12     2863   14 43 52
14 45 00  =1625-141    18 05 59  39.5 210.7  1.6      27.0    68     2872   14 43 41

14 45 00  SCOX1OFF     18 05 59  37.3 212.3  1.7      28.6   -12     2872   14 45 12
14 48 40  ---          18 09 40  36.8 213.3  1.8      29.4   208     2899   14 45 01

14 48 40  J1628-1415   18 09 40  39.1 211.8  1.7      27.9   -12     2899   14 48 52
14 50 00  =1625-141    18 11 00  38.9 212.1  1.7      28.2    68     2907   14 48 41

14 50 00  SCOX1OFF     18 11 00  36.7 213.7  1.8      29.7   -12     2907   14 50 12
14 53 40  ---          18 14 41  36.2 214.6  1.9      30.5   208     2934   14 50 01

14 53 40  J1628-1415   18 14 41  38.5 213.1  1.7      29.0   -12     2934   14 53 52
14 55 00  =1625-141    18 16 01  38.3 213.5  1.8      29.3    68     2943   14 53 41

14 55 00  SCOX1OFF     18 16 01  36.1 215.0  1.9      30.8   -13     2943   14 55 13
14 58 40  ---          18 19 41  35.6 215.9  2.0      31.6   207     2970   14 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

14 58 40  J1628-1415   18 19 41  37.9 214.5  1.8      30.2   -12     2970   14 58 52
15 00 00  =1625-141    18 21 02  37.7 214.8  1.9      30.5    68     2978   14 58 41

15 00 00  SCOX1OFF     18 21 02  35.4 216.2  2.0      31.9   -13     2978   15 00 13
15 03 40  ---          18 24 42  35.0 217.1  2.1      32.7   207     3005   15 00 01

15 03 40  J1628-1415   18 24 42  37.3 215.8  1.9      31.3   -13     3005   15 03 53
15 05 00  =1625-141    18 26 02  37.1 216.1  1.9      31.6    67     3014   15 03 41

15 05 00  SCOX1OFF     18 26 02  34.8 217.5  2.1      32.9   -13     3014   15 05 13
15 08 40  ---          18 29 43  34.3 218.4  2.1      33.7   207     3040   15 05 01

15 08 40  J1628-1415   18 29 43  36.6 217.1  2.0      32.4   -13     3040   15 08 53
15 10 00  =1625-141    18 31 03  36.4 217.4  2.0      32.7    67     3049   15 08 41

15 10 00  SCOX1OFF     18 31 03  34.1 218.7  2.2      34.0   -13     3049   15 10 13
15 13 40  ---          18 34 44  33.6 219.6  2.2      34.7   207     3076   15 10 01

15 13 40  J1628-1415   18 34 44  36.0 218.4  2.1      33.4   -13     3076   15 13 53
15 15 00  =1625-141    18 36 04  35.8 218.7  2.1      33.7    67     3084   15 13 41

15 15 00  SCOX1OFF     18 36 04  33.4 219.9  2.3      35.0   -13     3084   15 15 13
15 18 40  ---          18 39 45  32.9 220.7  2.3      35.7   207     3111   15 15 01

15 18 40  J1628-1415   18 39 45  35.3 219.6  2.2      34.5   -13     3111   15 18 53
15 20 00  =1625-141    18 41 05  35.1 219.9  2.2      34.7    67     3119   15 18 41

15 20 00  SCOX1OFF     18 41 05  32.7 221.1  2.3      35.9   -13     3119   15 20 13
15 23 40  ---          18 44 45  32.2 221.9  2.4      36.6   207     3146   15 20 01

15 23 40  J1628-1415   18 44 45  34.6 220.8  2.2      35.5   -13     3146   15 23 53
15 25 00  =1625-141    18 46 06  34.4 221.1  2.3      35.7    67     3155   15 23 41

15 25 00  SCOX1OFF     18 46 06  32.0 222.2  2.4      36.9   -13     3155   15 25 13
15 28 40  ---          18 49 46  31.5 223.0  2.5      37.6   207     3181   15 25 01

15 28 40  J1628-1415   18 49 46  33.9 222.0  2.3      36.4   -13     3181   15 28 53
15 30 00  =1625-141    18 51 07  33.7 222.3  2.4      36.7    67     3190   15 28 41

15 30 00  SCOX1OFF     18 51 07  31.3 223.3  2.5      37.8   -13     3190   15 30 13
15 33 40  ---          18 54 47  30.7 224.1  2.6      38.5   207     3217   15 30 01

15 33 40  J1628-1415   18 54 47  33.1 223.2  2.4      37.4   -13     3217   15 33 53
15 35 00  =1625-141    18 56 07  32.9 223.5  2.4      37.7    67     3225   15 33 41
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

15 35 00  SCOX1OFF     18 56 07  30.5 224.4  2.6      38.7   -13     3225   15 35 13
15 38 40  ---          18 59 48  30.0 225.2  2.6      39.4   207     3252   15 35 01

15 38 40  J1628-1415   18 59 48  32.4 224.3  2.5      38.3   -13     3252   15 38 53
15 40 00  =1625-141    19 01 08  32.2 224.6  2.5      38.6    67     3261   15 38 41

15 40 00  SCOX1OFF     19 01 08  29.8 225.5  2.7      39.6   -13     3261   15 40 13
15 43 40  ---          19 04 49  29.2 226.3  2.7      40.2   207     3287   15 40 01

15 43 40  J1628-1415   19 04 49  31.6 225.4  2.6      39.2   -13     3287   15 43 53
15 45 00  =1625-141    19 06 09  31.4 225.7  2.6      39.5    67     3296   15 43 41

15 45 00  SCOX1OFF     19 06 09  29.0 226.6  2.8      40.5   -13     3296   15 45 13
15 48 40  ---          19 09 50  28.4 227.3  2.8      41.1   207     3323   15 45 01

15 48 40  J1628-1415   19 09 50  30.9 226.5  2.7      40.1   -13     3323   15 48 53
15 50 00  =1625-141    19 11 10  30.6 226.8  2.7      40.3    67     3331   15 48 41

15 50 00  SCOX1OFF     19 11 10  28.2 227.6  2.8      41.3   -13     3331   15 50 13
15 53 40  ---          19 14 50  27.6 228.4  2.9      41.9   207     3358   15 50 01

15 53 40  J1628-1415   19 14 50  30.1 227.6  2.8      41.0   -13     3358   15 53 53
15 55 00  =1625-141    19 16 11  29.9 227.9  2.8      41.2    67     3367   15 53 41

15 55 00  SCOX1OFF     19 16 11  27.4 228.6  2.9      42.1   -13     3367   15 55 13
15 58 40  ---          19 19 51  26.8 229.4  3.0      42.7   207     3393   15 55 01

15 58 40  J1628-1415   19 19 51  29.3 228.6  2.8      41.8   -13     3393   15 58 53
16 00 00  =1625-141    19 21 11  29.0 228.9  2.9      42.0    67     3402   15 58 41

16 00 30  J1800+3848   19 21 42  71.6 301.8  1.3     110.2   -61     3402   16 01 31
16 05 30  =1758+388    19 26 42  70.7 300.8  1.4     108.5   239     3433   16 00 31

16 06 00  J1628-1415   19 27 12  28.1 230.1  3.0      43.0   -62     3433   16 07 02
16 10 00  =1625-141    19 31 13  27.4 230.9  3.0      43.6   178     3456   16 06 01

16 10 00  SCOX1OFF     19 31 13  24.9 231.6  3.2      44.4   -13     3456   16 10 13
16 13 40  ---          19 34 54  24.3 232.3  3.2      45.0   207     3482   16 10 01

16 13 40  J1628-1415   19 34 54  26.8 231.7  3.1      44.1   -13     3482   16 13 53
16 15 00  =1625-141    19 36 14  26.6 231.9  3.1      44.3    67     3491   16 13 41

16 15 00  SCOX1OFF     19 36 14  24.1 232.5  3.3      45.2   -13     3491   16 15 13
16 18 40  ---          19 39 55  23.4 233.2  3.3      45.7   207     3518   16 15 01
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

16 18 40  J1628-1415   19 39 55  25.9 232.6  3.2      44.9   -13     3518   16 18 53
16 20 00  =1625-141    19 41 15  25.7 232.9  3.2      45.1    67     3526   16 18 41

16 20 00  SCOX1OFF     19 41 15  23.2 233.4  3.3      45.9   -13     3526   16 20 13
16 23 40  ---          19 44 55  22.6 234.1  3.4      46.4   207     3553   16 20 01

16 23 40  J1628-1415   19 44 55  25.1 233.6  3.3      45.6   -13     3553   16 23 53
16 25 00  =1625-141    19 46 16  24.8 233.8  3.3      45.8    67     3561   16 23 41

16 25 00  SCOX1OFF     19 46 16  22.3 234.3  3.4      46.6   -13     3561   16 25 13
16 28 40  ---          19 49 56  21.7 235.0  3.5      47.1   207     3588   16 25 01

16 28 40  J1628-1415   19 49 56  24.2 234.5  3.3      46.3   -13     3588   16 28 53
16 30 00  =1625-141    19 51 16  24.0 234.7  3.4      46.5    67     3597   16 28 41

16 30 00  SCOX1OFF     19 51 16  21.5 235.2  3.5      47.2   -13     3597   16 30 13
16 33 40  ---          19 54 57  20.8 235.9  3.6      47.7   207     3623   16 30 01

16 33 40  J1628-1415   19 54 57  23.3 235.4  3.4      47.0   -13     3623   16 33 53
16 35 00  =1625-141    19 56 17  23.1 235.6  3.4      47.1    67     3632   16 33 41

16 35 00  SCOX1OFF     19 56 17  20.6 236.1  3.6      47.9   -13     3632   16 35 13
16 38 40  ---          19 59 58  19.9 236.7  3.6      48.4   207     3659   16 35 01

16 38 40  J1628-1415   19 59 58  22.4 236.3  3.5      47.6   -13     3659   16 38 53
16 40 00  =1625-141    20 01 18  22.2 236.5  3.5      47.8    67     3667   16 38 41

16 40 00  SCOX1OFF     20 01 18  19.7 237.0  3.7      48.5   -13     3667   16 40 13
16 43 40  ---          20 04 59  19.0 237.6  3.7      49.0   207     3694   16 40 01

16 43 40  J1628-1415   20 04 59  21.5 237.2  3.6      48.3   -13     3694   16 43 53
16 45 00  =1625-141    20 06 19  21.3 237.4  3.6      48.4    67     3703   16 43 41

16 45 00  SCOX1OFF     20 06 19  18.8 237.8  3.8      49.1   -13     3703   16 45 13
16 48 40  ---          20 09 59  18.1 238.4  3.8      49.6   207     3729   16 45 01

16 48 40  J1628-1415   20 09 59  20.6 238.0  3.7      48.9   -13     3729   16 48 53
16 50 00  =1625-141    20 11 20  20.4 238.3  3.7      49.0    67     3738   16 48 41

16 50 00  SCOX1OFF     20 11 20  17.8 238.6  3.8      49.7   -13     3738   16 50 13
16 53 40  ---          20 15 00  17.2 239.2  3.9      50.2   207     3765   16 50 01

16 53 40  J1628-1415   20 15 00  19.7 238.9  3.8      49.5   -13     3765   16 53 53
16 55 00  =1625-141    20 16 20  19.4 239.1  3.8      49.6    67     3773   16 53 41
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

16 55 00  SCOX1OFF     20 16 20  16.9 239.4  3.9      50.3   -13     3773   16 55 13
16 58 40  ---          20 20 01  16.2 240.0  4.0      50.7   207     3800   16 55 01

16 58 40  J1628-1415   20 20 01  18.8 239.7  3.8      50.1   -13     3800   16 58 53
17 00 00  =1625-141    20 21 21  18.5 239.9  3.9      50.2    67     3809   16 58 41

17 00 00  SCOX1OFF     20 21 21  16.0 240.2  4.0      50.9   -13     3809   17 00 13
17 03 40  ---          20 25 02  15.3 240.8  4.1      51.3   207     3835   17 00 01

17 03 40  J1628-1415   20 25 02  17.8 240.5  3.9      50.6   -13     3835   17 03 53
17 05 00  =1625-141    20 26 22  17.6 240.7  3.9      50.8    67     3844   17 03 41

17 05 00  SCOX1OFF     20 26 22  15.0 241.0  4.1      51.4   -13     3844   17 05 13
17 08 40  ---          20 30 03  14.4 241.6  4.2      51.8   207     3870   17 05 01

17 08 40  J1628-1415   20 30 03  16.9 241.3  4.0      51.2   -13     3870   17 08 53
17 10 00  =1625-141    20 31 23  16.6 241.5  4.0      51.3    67     3879   17 08 41

17 10 00  SCOX1OFF     20 31 23  14.1 241.8  4.2      52.0   -13     3879   17 10 13
17 13 40  ---          20 35 04  13.4 242.4  4.2      52.3   207     3906   17 10 01

17 13 40  J1628-1415   20 35 04  15.9 242.1  4.1      51.7   -13     3906   17 13 53
17 15 00  =1625-141    20 36 24  15.7 242.3  4.1      51.9    67     3914   17 13 41

17 15 00  SCOX1OFF     20 36 24  13.1 242.6  4.3      52.5   -13     3914   17 15 13
17 18 40  ---          20 40 04  12.4 243.1  4.3      52.8   207     3941   17 15 01

17 18 40  J1628-1415   20 40 04  15.0 242.9  4.2      52.2   -13     3941   17 18 53
17 20 00  =1625-141    20 41 25  14.7 243.1  4.2      52.4    67     3950   17 18 41

17 20 00  SCOX1OFF     20 41 25  12.2 243.3  4.3      53.0   -13     3950   17 20 13
17 23 40  ---          20 45 05  11.5 243.9  4.4      53.3   207     3976   17 20 01

17 23 40  J1628-1415   20 45 05  14.0 243.7  4.3      52.7   -13     3976   17 23 53
17 25 00  =1625-141    20 46 25  13.8 243.9  4.3      52.9    67     3985   17 23 41

17 25 00  SCOX1OFF     20 46 25  11.2 244.0  4.4      53.5   -13     3985   17 25 13
17 28 40  ---          20 50 06  10.5 244.6  4.5      53.8   207     4012   17 25 01

17 28 40  J1628-1415   20 50 06  13.0 244.4  4.3      53.2   -13     4012   17 28 53
17 30 00  =1625-141    20 51 26  12.8 244.6  4.4      53.3    67     4020   17 28 41

17 30 00  SCOX1OFF     20 51 26  10.2 244.8  4.5      53.9   -13     4020   17 30 13
17 33 40  ---          20 55 07   9.5 245.3  4.6      54.3   207     4047   17 30 01
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

17 33 40  J1628-1415   20 55 07  12.1 245.2  4.4      53.7   -13     4047   17 33 53
17 35 00  =1625-141    20 56 27  11.8 245.4  4.4      53.8    67     4056   17 33 41

17 35 00  SCOX1OFF     20 56 27   9.3 245.5  4.6      54.4   -13     4056   17 35 13
17 38 40  ---          21 00 08   8.5 246.0  4.7      54.7   207     4082   17 35 01

17 38 40  J1628-1415   21 00 08  11.1 245.9  4.5      54.1   -13     4082   17 38 53
17 40 00  =1625-141    21 01 28  10.8 246.1  4.5      54.3    67     4091   17 38 41

17 40 00  SCOX1OFF     21 01 28   8.3 246.2  4.7      54.9   -13     4091   17 40 13
17 43 40  ---          21 05 08   7.6 246.7  4.7      55.2   207     4118   17 40 01

17 43 40  J1628-1415   21 05 08  10.1 246.6  4.6      54.6   -13     4118   17 43 53
17 45 00  =1625-141    21 06 29   9.8 246.8  4.6      54.7    67     4126   17 43 41

17 45 00  SCOX1OFF     21 06 29   7.3 246.9  4.8      55.3   -13     4126   17 45 13
17 48 40  ---          21 10 09   6.6 247.4  4.8      55.6   207     4153   17 45 01

17 48 40  J1628-1415   21 10 09   9.1 247.3  4.7      55.0   -13     4153   17 48 53
17 50 00  =1625-141    21 11 30   8.8 247.5  4.7      55.1    67     4162   17 48 41

17 50 00  SCOX1OFF     21 11 30   6.3 247.6  4.8      55.7   -13     4162   17 50 13
17 53 40  ---          21 15 10   5.6 248.1  4.9      56.0   207     4188   17 50 01

17 53 40  J1628-1415   21 15 10   8.1 248.0  4.8      55.4   -13     4188   17 53 53
17 55 00  =1625-141    21 16 30   7.8 248.2  4.8      55.5    67     4197   17 53 41

17 55 00  SCOX1OFF     21 16 30   5.3 248.3  4.9      56.1   -13     4197   17 55 13
17 58 40  ---          21 20 11   4.6 248.8  5.0      56.4   207     4223   17 55 01

17 58 40  J1628-1415   21 20 11   7.1 248.7  4.8      55.8   -13     4223   17 58 53
18 00 00  =1625-141    21 21 31   6.8 248.9  4.9      55.9    67     4232   17 58 41

18 00 00  SCOX1OFF     21 21 31   4.3 248.9  5.0      56.5   -13     4232   18 00 13
18 03 40  ---          21 25 12   3.6 249.4  5.1      56.8   207     4259   18 00 01

18 03 40  J1628-1415   21 25 12   6.1 249.4  4.9      56.2   -13     4259   18 03 53
18 05 00  =1625-141    21 26 32   5.8 249.6  4.9      56.3    67     4267   18 03 41

18 05 00  SCOX1OFF     21 26 32   3.3 249.6  5.1      56.9   -13     4267   18 05 13
18 08 40  ---          21 30 13   2.5 250.1  5.2  H   57.2     0     4294   18 05 01

18 08 40  J1628-1415   21 30 13   5.1 250.1  5.0      56.6   -13     4294   18 08 53
18 10 00  =1625-141    21 31 33   4.8 250.2  5.0      56.7    67     4303   18 08 41
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Probing the disc-jet coupling in the neutron star binary Sco X-1
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  24 Feb 2019   Day  55 ---

18 10 00  SCOX1OFF     21 31 33   2.3 250.3  5.2  H   57.3   -13     4303   18 10 13
18 13 40  ---          21 35 13   1.5 250.7  5.2  D   57.5     0     4329   18 10 01

18 13 40  J1628-1415   21 35 13   4.1 250.7  5.1      57.0   -12     4329   18 13 52
18 15 00  =1625-141    21 36 34   3.8 250.9  5.1      57.0    68     4338   18 13 41

18 18 40  J1628-1415   21 40 14   3.0 251.4  5.2  H   57.3   214     4338   18 18 40
18 20 00  =1625-141    21 41 34   2.8 251.6  5.2  H   57.4     0     4348   18 18 41

18 55 30  J2253+1608   22 17 10  73.2 147.0 -0.6     -29.2  1993     4348   18 55 30
19 00 00  =2251+158    22 21 41  73.7 150.3 -0.6     -26.3   270     4383   18 55 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess119.X1024glob
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  22  Setup file default.  Used with PCAL = off
   LO sum=   8331.00  8331.00  8363.00  8363.00  8395.00  8395.00  8427.00  8427.00
   BBC fr=    731.00   731.00   763.00   763.00   795.00   795.00   827.00   827.00
   Bandwd=     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     771.00    771.00    803.00    803.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  22  23  24  25  26  27  28  29  30  31

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SCOX1OFF          16 17 05.647600   * 16 19 56.254500     16 21 00.575763       0.00
                    -15 30 45.21542    *-15 37 54.63500     -15 40 32.46944        0.00
                     From catalog imbedded in main SCHED input file.

   1226+023          12 26 33.245836   * 12 29 06.699732     12 30 05.597773       0.10
 * J1229+0203        02 19 43.30553    * 02 03 08.59803      01 56 46.57291        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  32342 observations

   1253-055          12 53 35.831306   * 12 56 11.166574     12 57 10.747018       0.10
 * J1256-0547       -05 31 07.99629    *-05 47 21.52515     -05 53 33.05801        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  14021 observations

   1546+027          15 46 58.292172   * 15 49 29.436846     15 50 26.537742       0.10
 * J1549+0237        02 46 06.07588    * 02 37 01.16323      02 33 32.68213        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  28615 observations

   1555-140          15 55 33.749896   * 15 58 21.947995     15 59 25.495492       0.18
 * J1558-1409       -14 01 26.50709    *-14 09 59.05322     -14 13 09.07261        0.29
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  221 observations

   1625-141          16 25 57.284276   * 16 28 46.619750     16 29 50.399279       0.21
 * J1628-1415       -14 09 07.75118    *-14 15 41.88634     -14 18 06.84750        0.42
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  105 observations

   1641+399          16 41 17.606226   * 16 42 58.809963     16 43 36.639482       0.13
 * J1642+3948        39 54 10.81487    * 39 48 36.99393      39 46 18.14666        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  52534 observations

   1741-038          17 41 20.616012   * 17 43 58.856136     17 44 57.980375       0.10
 * J1743-0350       -03 48 48.89994    *-03 50 04.61674     -03 50 33.04461        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  244125 observations

   1758+388          17 58 44.703949   * 18 00 24.765358     18 01 01.691632       0.13
 * J1800+3848        38 48 32.47351    * 38 48 30.69749      38 48 18.81270        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  5981 observations

 * 1934-638          19 34 47.602806   * 19 39 25.022408     19 41 06.611044       0.88
   J1939-6342       -63 49 37.72332    *-63 42 45.62520     -63 39 55.43403        0.37
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  82 observations

   2251+158          22 51 29.519743   * 22 53 57.747942     22 54 52.400725       0.10
 * J2253+1608        15 52 54.34805    * 16 08 53.56088      16 14 50.99477        0.10
                     /home/guest/rmc/SCHED/sched11.5/catalogs/sources.rfc
                     rfc_2018a Petrov and Kovalev, in preparation  41804 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  SCOX1OFF   sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +    18.364   778.303
  J1229+0203 sess119.X1024glob     1 2 4 5 6 7 9 22                  0.158     5.834
  J1256-0547 sess119.X1024glob     1 4 5 7 9 11 12 13 15 16 17 +     0.050     7.410
  J1549+0237 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     0.106    12.513
  J1558-1409 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     0.431    23.267
  J1628-1415 sess119.X1024glob     1 2 4 5 6 7 9 11 12 13 15 1 +     7.244   283.445
  J1642+3948 sess119.X1024glob     11 12 13 15 16 17 18 20 21  +     0.164    12.926
  J1743-0350 sess119.X1024glob     1 2 4 5 6 7 9                     0.042     1.441
  J1800+3848 sess119.X1024glob     6 7 22                            0.133     2.773
  1934-638   sess119.X1024glob     1                                 0.250     0.000
  J2253+1608 sess119.X1024glob     22                                0.075     2.965


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SCOX1OFF            89.2
   J1229+0203         148.8
   J1256-0547         139.9
   J1549+0237          99.8
   J1558-1409          94.6
   J1628-1415          87.3
   J1642+3948          93.2
   J1743-0350          70.5
   J1800+3848          78.6
   1934-638            61.6
   J2253+1608          26.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

