  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Huygens Probe VLBI Tracking
 Exp. Code:  GG057C  


Schedule Version:       3.00                                              
Processed by SCHED version: Trial release of 30 July 2004                 

PI:       Leonid Gurvits                                                  

Address:  JIVE                                                            
          Postbus 2                                                       
          7990 AA Dwingeloo                                               
          the Netherlands                                                 

Phone:    +31 521 596 512 (or 540)                                        
EMAIL:    lgurvits@jive.nl                                                
Fax:      +31 521 596 539                                                 
Phone during observation: +1 304 456 2341 (GBT control rm)                

Observing mode: Cassini spacecraft at S band                              

Notes:    Nod from Huygens to phase reference J0744+2120                  
          Dual Pol, 8x16MHz Bands                                         
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

 Next scan frequencies:  2034.99  2034.99  2034.99  2034.99  2139.99  2139.99
                         2286.99  2286.99
 Next BBC frequencies:    865.01   865.01   865.01   865.01   760.01   760.01
                          613.01   613.01
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00

09 01 00  DA193        09 40 56  43.9 -62.4  3.8      83.2     0   1  1      0  09 01 00
09 10 00  ---          09 49 58  42.2 -62.1  3.9      82.0   540   F  1   7200

09 15 00  J0728+2153   09 54 59  56.2 263.9  2.4      67.2    77   1  1   7200  09 15 00
09 25 00  ---          10 05 00  54.1 265.5  2.6      67.6   600   F  1  15200

09 30 00  J0744+2120   10 10 01  56.3 262.7  2.4      66.4   290   1  1  15200  09 30 00
09 31 10  ---          10 11 11  56.0 262.9  2.4      66.4    70   F  1  16133

09 31 10  0930TITAN    10 11 11  55.6 263.4  2.5      66.6    -7   1  1  16133  09 31 10
09 33 00  ---          10 13 02  55.2 263.7  2.5      66.7   103   F  1  17600

09 33 00  J0744+2120   10 13 02  55.6 263.2  2.5      66.5    -7   1  1  17600  09 33 00
09 34 10  ---          10 14 12  55.4 263.4  2.5      66.6    63   F  1  18533

09 34 10  0930TITAN    10 14 12  55.0 263.9  2.5      66.7    -7   1  1  18533  09 34 10
09 36 00  ---          10 16 02  54.6 264.2  2.6      66.8   103   F  1  20000

09 36 00  J0744+2120   10 16 02  55.0 263.7  2.5      66.7    -7   1  1  20000  09 36 00
09 37 10  ---          10 17 12  54.8 263.9  2.5      66.7    63   F  1  20933

09 37 10  0930TITAN    10 17 12  54.3 264.3  2.6      66.8    -7   1  1  20933  09 37 10
09 39 00  ---          10 19 03  53.9 264.6  2.6      66.9   103   F  1  22400

09 39 00  J0744+2120   10 19 03  54.4 264.2  2.6      66.8    -7   1  1  22400  09 39 00
09 40 10  ---          10 20 13  54.1 264.4  2.6      66.8    63   F  1  23333

09 40 10  0930TITAN    10 20 13  53.7 264.8  2.6      66.9    -7   1  1  23333  09 40 10
09 42 00  ---          10 22 03  53.3 265.1  2.7      67.0   103   F  1  24800

09 42 00  J0744+2120   10 22 03  53.7 264.7  2.6      66.9    -7   1  1  24800  09 42 00
09 43 10  ---          10 23 13  53.5 264.9  2.6      66.9    63   F  1  25733

09 43 10  0930TITAN    10 23 13  53.0 265.3  2.7      67.0    -7   1  1  25733  09 43 10
09 45 00  ---          10 25 03  52.6 265.5  2.7      67.1   103   F  1  27200
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

09 45 00  J0744+2120   10 25 03  53.1 265.1  2.7      67.0    -7   1  1  27200  09 45 00
09 46 10  ---          10 26 14  52.8 265.3  2.7      67.0    63   F  1  28133

09 46 10  1000TITAN    10 26 14  52.4 265.7  2.7      67.1    -7   1  1  28133  09 46 10
09 48 00  ---          10 28 04  52.0 266.0  2.8      67.2   103   F  1  29600

09 48 00  J0744+2120   10 28 04  52.4 265.6  2.7      67.1    -7   1  1  29600  09 48 00
09 49 10  ---          10 29 14  52.2 265.8  2.7      67.1    63   F  1  30533

09 49 10  1000TITAN    10 29 14  51.7 266.2  2.8      67.2    -7   1  1  30533  09 49 10
09 51 00  ---          10 31 04  51.3 266.4  2.8      67.2   103   F  1  32000

09 51 00  J0744+2120   10 31 04  51.8 266.0  2.8      67.1    -7   1  1  32000  09 51 00
09 52 10  ---          10 32 15  51.5 266.2  2.8      67.2    63   F  1  32933

09 52 10  1000TITAN    10 32 15  51.1 266.6  2.8      67.3    -7   1  1  32933  09 52 10
09 54 00  ---          10 34 05  50.7 266.9  2.9      67.3   103   F  1  34400

09 54 00  J0744+2120   10 34 05  51.1 266.5  2.8      67.2    -7   1  1  34400  09 54 00
09 55 10  ---          10 35 15  50.9 266.6  2.8      67.2    63   F  1  35333

09 55 10  1000TITAN    10 35 15  50.4 267.0  2.9      67.3    -7   1  1  35333  09 55 10
09 57 00  ---          10 37 05  50.1 267.3  2.9      67.4   103   F  1  36800

09 57 00  J0744+2120   10 37 05  50.5 266.9  2.9      67.3    -7   1  1  36800  09 57 00
09 58 10  ---          10 38 16  50.2 267.1  2.9      67.3    63   F  1  37733

09 58 10  1000TITAN    10 38 16  49.8 267.4  2.9      67.4    -7   1  1  37733  09 58 10
10 00 00  ---          10 40 06  49.4 267.7  3.0      67.4   103   F  1  39200

10 00 00  J0744+2120   10 40 06  49.8 267.3  2.9      67.3    -7   1  1  39200  10 00 00
10 01 10  ---          10 41 16  49.6 267.5  2.9      67.3    63   F  1  40133

10 01 10  1000TITAN    10 41 16  49.2 267.9  3.0      67.4    -7   1  1  40133  10 01 10
10 03 00  ---          10 43 06  48.8 268.1  3.0      67.4   103   F  1  41600

10 03 00  J0744+2120   10 43 06  49.2 267.7  3.0      67.4    -7   1  1  41600  10 03 00
10 04 10  ---          10 44 17  48.9 267.9  3.0      67.4    63   F  1  42533

10 04 10  1000TITAN    10 44 17  48.5 268.3  3.0      67.4    -7   1  1  42533  10 04 10
10 06 00  ---          10 46 07  48.1 268.5  3.1      67.5   103   F  1  44000

10 06 00  J0744+2120   10 46 07  48.6 268.2  3.0      67.4    -7   1  1  44000  10 06 00
10 07 10  ---          10 47 17  48.3 268.3  3.0      67.4    63   F  1  44933
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

10 07 10  1000TITAN    10 47 17  47.9 268.7  3.1      67.5    -7   1  1  44933  10 07 10
10 09 00  ---          10 49 07  47.5 268.9  3.1      67.5   103   F  1  46400

10 09 00  J0744+2120   10 49 07  47.9 268.6  3.1      67.4    -7   1  1  46400  10 09 00
10 10 10  ---          10 50 18  47.7 268.7  3.1      67.4    63   F  1  47333

10 10 10  1000TITAN    10 50 18  47.2 269.1  3.1      67.5    -7   1  1  47333  10 10 10
10 12 00  ---          10 52 08  46.8 269.3  3.2      67.5   103   F  1  48800

10 12 00  J0744+2120   10 52 08  47.3 269.0  3.1      67.4    -7   1  1  48800  10 12 00
10 13 10  ---          10 53 18  47.0 269.1  3.1      67.4    63   F  1  49733

10 13 10  1000TITAN    10 53 18  46.6 269.5  3.2      67.5    -7   1  1  49733  10 13 10
10 15 00  ---          10 55 08  46.2 269.7  3.2      67.5   103   F  1  51200

10 15 00  J0744+2120   10 55 08  46.6 269.4  3.2      67.5    -7   1  1  51200  10 15 00
10 16 10  ---          10 56 19  46.4 269.5  3.2      67.5    63   F  1  52133

10 16 10  1030TITAN    10 56 19  45.9 269.8  3.2      67.5    -7   1  1  52133  10 16 10
10 18 00  ---          10 58 09  45.5 270.1  3.3      67.5   103   F  1  53600

10 18 00  J0744+2120   10 58 09  46.0 269.7  3.2      67.5    -7   1  1  53600  10 18 00
10 19 10  ---          10 59 19  45.7 269.9  3.2      67.5    63   F  1  54533

10 19 10  1030TITAN    10 59 19  45.3 270.2  3.3      67.5    -7   1  1  54533  10 19 10
10 21 00  ---          11 01 09  44.9 270.5  3.3      67.5   103   F  1  56000

10 21 00  J0744+2120   11 01 09  45.3 270.1  3.3      67.5    -7   1  1  56000  10 21 00
10 22 10  ---          11 02 20  45.1 270.3  3.3      67.5    63   F  1  56933

10 22 10  1030TITAN    11 02 20  44.6 270.6  3.3      67.5    -7   1  1  56933  10 22 10
10 24 00  ---          11 04 10  44.2 270.8  3.4      67.5   103   F  1  58400

10 24 00  J0744+2120   11 04 10  44.7 270.5  3.3      67.5    -7   1  1  58400  10 24 00
10 25 10  ---          11 05 20  44.4 270.7  3.3      67.5    63   F  1  59333

10 25 10  1030TITAN    11 05 20  44.0 271.0  3.4      67.5    -7   1  1  59333  10 25 10
10 27 00  ---          11 07 10  43.6 271.2  3.4      67.5   103   F  1  60800

10 27 00  J0744+2120   11 07 10  44.0 270.9  3.4      67.5    -7   1  1  60800  10 27 00
10 28 10  ---          11 08 21  43.8 271.0  3.4      67.4    63   F  1  61733

10 28 10  1030TITAN    11 08 21  43.3 271.3  3.4      67.5    -7   1  1  61733  10 28 10
10 30 00  ---          11 10 11  42.9 271.6  3.5      67.5   103   F  1  63200
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

10 30 00  J0744+2120   11 10 11  43.4 271.3  3.4      67.4    -7   1  1  63200  10 30 00
10 31 10  ---          11 11 21  43.1 271.4  3.4      67.4    63   F  1  64133

10 31 10  1030TITAN    11 11 21  42.7 271.7  3.5      67.4    -7   1  1  64133  10 31 10
10 33 00  ---          11 13 11  42.3 271.9  3.5      67.4   103   F  1  65600

10 33 00  J0744+2120   11 13 11  42.7 271.6  3.5      67.4    -7   1  1  65600  10 33 00
10 34 10  ---          11 14 22  42.5 271.8  3.5      67.4    63   F  1  66533

10 34 10  1030TITAN    11 14 22  42.0 272.1  3.5      67.4    -7   1  1  66533  10 34 10
10 36 00  ---          11 16 12  41.6 272.3  3.6      67.4   103   F  1  68000

10 36 00  J0744+2120   11 16 12  42.1 272.0  3.5      67.4    -7   1  1  68000  10 36 00
10 37 10  ---          11 17 22  41.8 272.1  3.5      67.4    63   F  1  68933

10 37 10  1030TITAN    11 17 22  41.4 272.4  3.6      67.4    -7   1  1  68933  10 37 10
10 39 00  ---          11 19 12  41.0 272.7  3.6      67.4   103   F  1  70400

10 39 00  J0744+2120   11 19 12  41.4 272.3  3.6      67.4    -7   1  1  70400  10 39 00
10 40 10  ---          11 20 23  41.2 272.5  3.6      67.3    63   F  1  71333

10 40 10  1030TITAN    11 20 23  40.7 272.8  3.6      67.3    -7   1  1  71333  10 40 10
10 42 00  ---          11 22 13  40.3 273.0  3.7      67.3   103   F  1  72800

10 42 00  J0744+2120   11 22 13  40.8 272.7  3.6      67.3    -7   1  1  72800  10 42 00
10 43 10  ---          11 23 23  40.5 272.8  3.6      67.3    63   F  1  73733

10 43 10  1030TITAN    11 23 23  40.1 273.2  3.7      67.3    -7   1  1  73733  10 43 10
10 45 00  ---          11 25 13  39.7 273.4  3.7      67.3   103   F  1  75200

10 45 00  J0744+2120   11 25 13  40.1 273.1  3.7      67.3    -7   1  1  75200  10 45 00
10 46 10  ---          11 26 24  39.9 273.2  3.7      67.3    63   F  1  76133

10 46 10  1100TITAN    11 26 24  39.4 273.5  3.7      67.3    -7   1  1  76133  10 46 10
10 48 00  ---          11 28 14  39.1 273.7  3.8      67.2   103   F  1  77600

10 48 00  J0744+2120   11 28 14  39.5 273.4  3.7      67.2    -7   1  1  77600  10 48 00
10 49 10  ---          11 29 24  39.2 273.5  3.7      67.2    63   F  1  78533

10 49 10  1100TITAN    11 29 24  38.8 273.9  3.8      67.2    -7   1  1  78533  10 49 10
10 51 00  ---          11 31 14  38.4 274.1  3.8      67.2   103   F  1  80000

10 51 00  J0744+2120   11 31 14  38.9 273.8  3.8      67.2    -7   1  1  80000  10 51 00
10 52 10  ---          11 32 25  38.6 273.9  3.8      67.1    63   F  1  80933
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

10 52 10  1100TITAN    11 32 25  38.2 274.2  3.8      67.1    -7   1  1  80933  10 52 10
10 54 00  ---          11 34 15  37.8 274.4  3.9      67.1   103   F  1  82400

10 54 00  J0744+2120   11 34 15  38.2 274.1  3.8      67.1    -7   1  1  82400  10 54 00
10 55 10  ---          11 35 25  38.0 274.2  3.8      67.1    63   F  1  83333

10 55 10  1100TITAN    11 35 25  37.5 274.5  3.9      67.1    -7   1  1  83333  10 55 10
10 57 00  ---          11 37 15  37.1 274.8  3.9      67.0   103   F  1  84800

10 57 00  J0744+2120   11 37 15  37.6 274.5  3.9      67.1    -7   1  1  84800  10 57 00
10 58 10  ---          11 38 26  37.3 274.6  3.9      67.0    63   F  1  85733

10 58 10  1100TITAN    11 38 26  36.9 274.9  3.9      67.0    -7   1  1  85733  10 58 10
11 00 00  ---          11 40 16  36.5 275.1  4.0      67.0   103   F  1  87200

11 00 00  J0744+2120   11 40 16  36.9 274.8  3.9      67.0    -7   1  1  87200  11 00 00
11 01 10  ---          11 41 26  36.7 274.9  3.9      67.0    63   F  1  88133

11 01 10  1100TITAN    11 41 26  36.2 275.2  4.0      66.9    -7   1  1  88133  11 01 10
11 03 00  ---          11 43 16  35.8 275.4  4.0      66.9   103   F  1  89600

11 03 00  J0744+2120   11 43 16  36.3 275.1  4.0      66.9    -7   1  1  89600  11 03 00
11 04 10  ---          11 44 26  36.0 275.3  4.0      66.9    63   F  1  90533

11 04 10  1100TITAN    11 44 26  35.6 275.6  4.0      66.9    -7   1  1  90533  11 04 10
11 06 00  ---          11 46 17  35.2 275.8  4.1      66.8   103   F  1  92000

11 06 00  J0744+2120   11 46 17  35.6 275.5  4.0      66.8    -7   1  1  92000  11 06 00
11 07 10  ---          11 47 27  35.4 275.6  4.0      66.8    63   F  1  92933

11 07 10  1100TITAN    11 47 27  34.9 275.9  4.1      66.8    -7   1  1  92933  11 07 10
11 09 00  ---          11 49 17  34.5 276.1  4.1      66.7   103   F  1  94400

11 09 00  J0744+2120   11 49 17  35.0 275.8  4.1      66.8    -7   1  1  94400  11 09 00
11 10 10  ---          11 50 27  34.7 275.9  4.1      66.7    63   F  1  95333

11 10 10  1100TITAN    11 50 27  34.3 276.2  4.1      66.7    -7   1  1  95333  11 10 10
11 12 00  ---          11 52 18  33.9 276.4  4.2      66.7   103   F  1  96800

11 12 00  J0744+2120   11 52 18  34.3 276.2  4.1      66.7    -7   1  1  96800  11 12 00
11 13 10  ---          11 53 28  34.1 276.3  4.1      66.7    63   F  1  97733

11 13 10  1100TITAN    11 53 28  33.6 276.6  4.2      66.6    -7   1  1  97733  11 13 10
11 15 00  ---          11 55 18  33.3 276.8  4.2      66.6   103   F  1  99200
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

11 15 00  J0744+2120   11 55 18  33.7 276.5  4.2      66.6    -7   1  1  99200  11 15 00
11 16 10  ---          11 56 28  33.4 276.6  4.2      66.6    63   F  1 100133

11 16 10  1130TITAN    11 56 28  33.0 276.9  4.2      66.5    -7   1  1 100133  11 16 10
11 18 00  ---          11 58 19  32.6 277.1  4.3      66.5   103   F  1 101600

11 18 00  J0744+2120   11 58 19  33.1 276.8  4.2      66.5    -7   1  1 101600  11 18 00
11 19 10  ---          11 59 29  32.8 277.0  4.2      66.5    63   F  1 102533

11 19 10  1130TITAN    11 59 29  32.4 277.2  4.3      66.4    -7   1  1 102533  11 19 10
11 21 00  ---          12 01 19  32.0 277.4  4.3      66.4   103   F  1 104000

11 21 00  J0744+2120   12 01 19  32.4 277.2  4.3      66.4    -7   1  1 104000  11 21 00
11 22 10  ---          12 02 29  32.2 277.3  4.3      66.4    63   F  1 104933

11 22 10  1130TITAN    12 02 29  31.7 277.6  4.3      66.3    -7   1  1 104933  11 22 10
11 24 00  ---          12 04 20  31.3 277.8  4.4      66.3   103   F  1 106400

11 24 00  J0744+2120   12 04 20  31.8 277.5  4.3      66.3    -7   1  1 106400  11 24 00
11 25 10  ---          12 05 30  31.5 277.6  4.3      66.3    63   F  1 107333

11 25 10  1130TITAN    12 05 30  31.1 277.9  4.4      66.2    -7   1  1 107333  11 25 10
11 27 00  ---          12 07 20  30.7 278.1  4.4      66.2   103   F  1 108800

11 27 00  J0744+2120   12 07 20  31.1 277.8  4.4      66.2    -7   1  1 108800  11 27 00
11 28 10  ---          12 08 30  30.9 277.9  4.4      66.2    63   F  1 109733

11 28 10  1130TITAN    12 08 30  30.4 278.2  4.4      66.1    -7   1  1 109733  11 28 10
11 30 00  ---          12 10 21  30.0 278.4  4.5      66.1   103   F  1 111200

11 30 00  J0744+2120   12 10 21  30.5 278.1  4.4      66.1    -7   1  1 111200  11 30 00
11 31 10  ---          12 11 31  30.2 278.3  4.4      66.1    63   F  1 112133

11 31 10  1130TITAN    12 11 31  29.8 278.6  4.5      66.0    -7   1  1 112133  11 31 10
11 33 00  ---          12 13 21  29.4 278.8  4.5      65.9   103   F  1 113600

11 33 00  J0744+2120   12 13 21  29.8 278.5  4.5      66.0    -7   1  1 113600  11 33 00
11 34 10  ---          12 14 31  29.6 278.6  4.5      66.0    63   F  1 114533

11 34 10  1130TITAN    12 14 31  29.2 278.9  4.5      65.9    -7   1  1 114533  11 34 10
11 36 00  ---          12 16 22  28.8 279.1  4.6      65.8   103   F  1 116000

11 36 00  J0744+2120   12 16 22  29.2 278.8  4.5      65.9    -7   1  1 116000  11 36 00
11 37 10  ---          12 17 32  29.0 278.9  4.5      65.8    63   F  1 116933
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

11 37 10  1130TITAN    12 17 32  28.5 279.2  4.6      65.8    -7   1  1 116933  11 37 10
11 39 00  ---          12 19 22  28.1 279.4  4.6      65.7   103   F  1 118400

11 39 00  J0744+2120   12 19 22  28.6 279.1  4.6      65.8    -7   1  1 118400  11 39 00
11 40 10  ---          12 20 32  28.3 279.3  4.6      65.7    63   F  1 119333

11 40 10  1130TITAN    12 20 32  27.9 279.5  4.6      65.7    -7   1  1 119333  11 40 10
11 42 00  ---          12 22 23  27.5 279.7  4.7      65.6   103   F  1 120800

11 42 00  J0744+2120   12 22 23  27.9 279.5  4.6      65.7    -7   1  1 120800  11 42 00
11 43 10  ---          12 23 33  27.7 279.6  4.6      65.6    63   F  1 121733

11 43 10  1130TITAN    12 23 33  27.2 279.9  4.7      65.5    -7   1  1 121733  11 43 10
11 45 00  ---          12 25 23  26.9 280.1  4.7      65.5   103   F  1 123200

11 45 00  J0744+2120   12 25 23  27.3 279.8  4.7      65.5    -7   1  1 123200  11 45 00
11 46 10  ---          12 26 33  27.0 279.9  4.7      65.5    63   F  1 124133

11 46 10  1200TITAN    12 26 33  26.6 280.2  4.7      65.4    -7   1  1 124133  11 46 10
11 48 00  ---          12 28 24  26.2 280.4  4.8      65.3   103   F  1 125600

11 48 00  J0744+2120   12 28 24  26.7 280.1  4.7      65.4    -7   1  1 125600  11 48 00
11 49 10  ---          12 29 34  26.4 280.2  4.7      65.4    63   F  1 126533

11 49 10  1200TITAN    12 29 34  26.0 280.5  4.8      65.3    -7   1  1 126533  11 49 10
11 51 00  ---          12 31 24  25.6 280.7  4.8      65.2   103   F  1 128000

11 51 00  J0744+2120   12 31 24  26.0 280.4  4.8      65.3    -7   1  1 128000  11 51 00
11 52 10  ---          12 32 34  25.8 280.6  4.8      65.2    63   F  1 128933

11 52 10  1200TITAN    12 32 34  25.3 280.8  4.8      65.2    -7   1  1 128933  11 52 10
11 54 00  ---          12 34 25  24.9 281.0  4.9      65.1   103   F  1 130400

11 54 00  J0744+2120   12 34 25  25.4 280.8  4.8      65.1    -7   1  1 130400  11 54 00
11 55 10  ---          12 35 35  25.1 280.9  4.8      65.1    63   F  1 131333

11 55 10  1200TITAN    12 35 35  24.7 281.2  4.9      65.0    -7   1  1 131333  11 55 10
11 57 00  ---          12 37 25  24.3 281.4  4.9      64.9   103   F  1 132800

11 57 00  J0744+2120   12 37 25  24.7 281.1  4.9      65.0    -7   1  1 132800  11 57 00
11 58 10  ---          12 38 35  24.5 281.2  4.9      65.0    63   F  1 133733

11 58 10  1200TITAN    12 38 35  24.1 281.5  4.9      64.9    -7   1  1 133733  11 58 10
12 00 00  ---          12 40 26  23.7 281.7  5.0      64.8   103   F  1 135200
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

12 00 00  J0744+2120   12 40 26  24.1 281.4  4.9      64.9    -7   1  1 135200  12 00 00
12 01 10  ---          12 41 36  23.9 281.5  4.9      64.8    63   F  1 136133

12 01 10  1200TITAN    12 41 36  23.4 281.8  5.0      64.7    -7   1  1 136133  12 01 10
12 03 00  ---          12 43 26  23.0 282.0  5.0      64.6   103   F  1 137600

12 03 00  J0744+2120   12 43 26  23.5 281.7  5.0      64.7    -7   1  1 137600  12 03 00
12 04 10  ---          12 44 36  23.2 281.9  5.0      64.7    63   F  1 138533

12 04 10  1200TITAN    12 44 36  22.8 282.2  5.0      64.6    -7   1  1 138533  12 04 10
12 06 00  ---          12 46 27  22.4 282.4  5.1      64.5   103   F  1 140000

12 06 00  J0744+2120   12 46 27  22.8 282.1  5.0      64.6    -7   1  1 140000  12 06 00
12 07 10  ---          12 47 37  22.6 282.2  5.0      64.5    63   F  1 140933

12 07 10  1200TITAN    12 47 37  22.2 282.5  5.1      64.4    -7   1  1 140933  12 07 10
12 09 00  ---          12 49 27  21.8 282.7  5.1      64.3   103   F  1 142400

12 09 00  J0744+2120   12 49 27  22.2 282.4  5.1      64.4    -7   1  1 142400  12 09 00
12 10 10  ---          12 50 37  22.0 282.5  5.1      64.4    63   F  1 143333

12 10 10  1200TITAN    12 50 37  21.5 282.8  5.1      64.3    -7   1  1 143333  12 10 10
12 12 00  ---          12 52 28  21.1 283.0  5.2      64.2   103   F  1 144800

12 12 00  J0744+2120   12 52 28  21.6 282.7  5.1      64.3    -7   1  1 144800  12 12 00
12 13 10  ---          12 53 38  21.3 282.8  5.1      64.2    63   F  1 145733

12 13 10  1200TITAN    12 53 38  20.9 283.1  5.2      64.1    -7   1  1 145733  12 13 10
12 15 00  ---          12 55 28  20.5 283.3  5.2      64.0   103   F  1 147200

12 15 00  J0744+2120   12 55 28  20.9 283.0  5.2      64.1    -7   1  1 147200  12 15 00
12 16 10  ---          12 56 38  20.7 283.2  5.2      64.1    63   F  1 148133

12 16 10  1230TITAN    12 56 38  20.3 283.5  5.2      64.0    -7   1  1 148133  12 16 10
12 18 00  ---          12 58 29  19.9 283.7  5.3      63.9   103   F  1 149600

12 18 00  J0744+2120   12 58 29  20.3 283.4  5.2      64.0    -7   1  1 149600  12 18 00
12 19 10  ---          12 59 39  20.1 283.5  5.2      63.9    63   F  1 150533

12 19 10  1230TITAN    12 59 39  19.6 283.8  5.3      63.8    -7   1  1 150533  12 19 10
12 21 00  ---          13 01 29  19.3 284.0  5.3      63.7   103   F  1 152000

12 21 00  J0744+2120   13 01 29  19.7 283.7  5.3      63.8    -7   1  1 152000  12 21 00
12 22 10  ---          13 02 39  19.4 283.8  5.3      63.7    63   F  1 152933
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

12 22 10  1230TITAN    13 02 39  19.0 284.1  5.3      63.6    -7   1  1 152933  12 22 10
12 24 00  ---          13 04 30  18.6 284.3  5.4      63.5   103   F  1 154400

12 24 00  J0744+2120   13 04 30  19.1 284.0  5.3      63.6    -7   1  1 154400  12 24 00
12 25 10  ---          13 05 40  18.8 284.2  5.3      63.6    63   F  1 155333

12 25 10  1230TITAN    13 05 40  18.4 284.4  5.4      63.5    -7   1  1 155333  12 25 10
12 27 00  ---          13 07 30  18.0 284.6  5.4      63.4   103   F  1 156800

12 27 00  J0744+2120   13 07 30  18.4 284.4  5.4      63.5    -7   1  1 156800  12 27 00
12 28 10  ---          13 08 40  18.2 284.5  5.4      63.4    63   F  1 157733

12 28 10  1230TITAN    13 08 40  17.8 284.8  5.4      63.3    -7   1  1 157733  12 28 10
12 30 00  ---          13 10 31  17.4 285.0  5.5      63.2   103   F  1 159200

12 30 00  J0744+2120   13 10 31  17.8 284.7  5.4      63.3    -7   1  1 159200  12 30 00
12 31 10  ---          13 11 41  17.6 284.8  5.4      63.2    63   F  1 160133

12 31 10  1230TITAN    13 11 41  17.1 285.1  5.5      63.1    -7   1  1 160133  12 31 10
12 33 00  ---          13 13 31  16.8 285.3  5.5      63.0   103   F  1 161600

12 33 00  J0744+2120   13 13 31  17.2 285.0  5.5      63.1    -7   1  1 161600  12 33 00
12 34 10  ---          13 14 41  16.9 285.2  5.5      63.1    63   F  1 162533

12 34 10  1230TITAN    13 14 41  16.5 285.4  5.5      63.0    -7   1  1 162533  12 34 10
12 36 00  ---          13 16 32  16.1 285.6  5.6      62.8   103   F  1 164000

12 36 00  J0744+2120   13 16 32  16.6 285.4  5.5      63.0    -7   1  1 164000  12 36 00
12 37 10  ---          13 17 42  16.3 285.5  5.5      62.9    63   F  1 164933

12 37 10  1230TITAN    13 17 42  15.9 285.8  5.6      62.8    -7   1  1 164933  12 37 10
12 39 00  ---          13 19 32  15.5 286.0  5.6      62.7   103   F  1 166400

12 39 00  J0744+2120   13 19 32  15.9 285.7  5.6      62.8    -7   1  1 166400  12 39 00
12 40 10  ---          13 20 42  15.7 285.8  5.6      62.7    63   F  1 167333

12 40 10  1230TITAN    13 20 42  15.3 286.1  5.6      62.6    -7   1  1 167333  12 40 10
12 42 00  ---          13 22 33  14.9 286.3  5.7      62.5   103   F  1 168800

12 42 00  J0744+2120   13 22 33  15.3 286.0  5.6      62.6    -7   1  1 168800  12 42 00
12 43 10  ---          13 23 43  15.1 286.2  5.6      62.5    63   F  1 169733

12 43 10  1230TITAN    13 23 43  14.6 286.4  5.7      62.4    -7   1  1 169733  12 43 10
12 45 00  ---          13 25 33  14.3 286.6  5.7      62.3   103   F  1 171200
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

12 45 00  J0744+2120   13 25 33  14.7 286.4  5.7      62.4    -7   1  1 171200  12 45 00
12 46 10  ---          13 26 43  14.4 286.5  5.7      62.3    63   F  1 172133

12 46 10  1300TITAN    13 26 43  14.0 286.8  5.7      62.2    -7   1  1 172133  12 46 10
12 48 00  ---          13 28 34  13.6 287.0  5.8      62.1   103   F  1 173600

12 48 00  J0744+2120   13 28 34  14.1 286.7  5.7      62.2    -7   1  1 173600  12 48 00
12 49 10  ---          13 29 44  13.8 286.8  5.7      62.1    63   F  1 174533

12 49 10  1300TITAN    13 29 44  13.4 287.1  5.8      62.0    -7   1  1 174533  12 49 10
12 51 00  ---          13 31 34  13.0 287.3  5.8      61.9   103   F  1 176000

12 51 00  J0744+2120   13 31 34  13.5 287.0  5.8      62.0    -7   1  1 176000  12 51 00
12 52 10  ---          13 32 44  13.2 287.2  5.8      61.9    63   F  1 176933

12 52 10  1300TITAN    13 32 44  12.8 287.5  5.8      61.8    -7   1  1 176933  12 52 10
12 54 00  ---          13 34 35  12.4 287.7  5.9      61.7   103   F  1 178400

12 54 00  J0744+2120   13 34 35  12.8 287.4  5.8      61.8    -7   1  1 178400  12 54 00
12 55 10  ---          13 35 45  12.6 287.5  5.8      61.8    63   F  1 179333

12 55 10  1300TITAN    13 35 45  12.2 287.8  5.9      61.6    -7   1  1 179333  12 55 10
12 57 00  ---          13 37 35  11.8 288.0  5.9      61.5   103   F  1 180800

12 57 00  J0744+2120   13 37 35  12.2 287.7  5.9      61.6    -7   1  1 180800  12 57 00
12 58 10  ---          13 38 45  12.0 287.8  5.9      61.6    63   F  1 181733

12 58 10  1300TITAN    13 38 45  11.6 288.1  5.9      61.4    -7   1  1 181733  12 58 10
13 00 00  ---          13 40 36  11.2 288.3  6.0      61.3   103   F  1 183200

13 00 00  J0744+2120   13 40 36  11.6 288.1  5.9      61.4    -7   1  1 183200  13 00 00
13 01 10  ---          13 41 46  11.4 288.2  5.9      61.3    63   F  1 184133

13 01 10  1300TITAN    13 41 46  10.9 288.5  6.0      61.2    -7   1  1 184133  13 01 10
13 03 00  ---          13 43 36  10.6 288.7  6.0      61.1   103   F  1 185600

13 03 00  J0744+2120   13 43 36  11.0 288.4  6.0      61.2    -7   1  1 185600  13 03 00
13 04 10  ---          13 44 46  10.7 288.5  6.0      61.1    63   F  1 186533

13 04 10  1300TITAN    13 44 46  10.3 288.8  6.0      61.0    -7   1  1 186533  13 04 10
13 06 00  ---          13 46 37  10.0 289.0  6.1      60.9   103   F  1 188000

13 06 00  J0744+2120   13 46 37  10.4 288.7  6.0      61.0    -7   1  1 188000  13 06 00
13 07 10  ---          13 47 47  10.1 288.9  6.0      60.9    63   F  1 188933
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

13 07 10  1300TITAN    13 47 47   9.7 289.2  6.1      60.8    -7   1  1 188933  13 07 10
13 09 00  ---          13 49 37   9.3 289.4  6.1      60.6   103   F  1 190400

13 09 00  J0744+2120   13 49 37   9.8 289.1  6.1      60.8    -7   1  1 190400  13 09 00
13 10 10  ---          13 50 47   9.5 289.2  6.1      60.7    63   F  1 191333

13 10 10  1300TITAN    13 50 47   9.1 289.5  6.1      60.6    -7   1  1 191333  13 10 10
13 12 00  ---          13 52 37   8.7 289.7  6.2      60.4   103   F  1 192800

13 12 00  J0744+2120   13 52 37   9.1 289.4  6.1      60.6    -7   1  1 192800  13 12 00
13 13 10  ---          13 53 48   8.9 289.6  6.1      60.5    63   F  1 193733

13 13 10  1300TITAN    13 53 48   8.5 289.9  6.2      60.3    -7   1  1 193733  13 13 10
13 15 00  ---          13 55 38   8.1 290.1  6.2      60.2   103   F  1 195200

13 15 00  J0744+2120   13 55 38   8.5 289.8  6.2      60.4    -7   1  1 195200  13 15 00
13 16 10  ---          13 56 48   8.3 289.9  6.2      60.3    63   F  1 196133

13 16 10  1330TITAN    13 56 48   7.9 290.2  6.2      60.1    -7   1  1 196133  13 16 10
13 18 00  ---          13 58 38   7.5 290.4  6.3      60.0   103   F  1 197600

13 18 00  J0744+2120   13 58 38   7.9 290.1  6.2      60.1    -7   1  1 197600  13 18 00
13 19 10  ---          13 59 49   7.7 290.3  6.2      60.0    63   F  1 198533

13 19 10  1330TITAN    13 59 49   7.3 290.6  6.3      59.9    -7   1  1 198533  13 19 10
13 21 00  ---          14 01 39   6.9 290.8  6.3      59.7   103   F  1 200000

13 21 00  J0744+2120   14 01 39   7.3 290.5  6.3      59.9    -7   1  1 200000  13 21 00
13 22 10  ---          14 02 49   7.1 290.6  6.3      59.8    63   F  1 200933

13 22 10  1330TITAN    14 02 49   6.7 290.9  6.3      59.7    -7   1  1 200933  13 22 10
13 24 00  ---          14 04 39   6.3 291.1  6.4      59.5   103   F  1 202400

13 24 00  J0744+2120   14 04 39   6.7 290.8  6.3      59.7    -7   1  1 202400  13 24 00
13 25 10  ---          14 05 50   6.5 291.0  6.3      59.6    63   F  1 203333

13 25 10  1330TITAN    14 05 50   6.1 291.3  6.4      59.4    -7   1  1 203333  13 25 10
13 27 00  ---          14 07 40   5.7 291.5  6.4      59.3   103   F  1 204800

13 27 00  J0744+2120   14 07 40   6.1 291.2  6.4      59.4    -7   1  1 204800  13 27 00
13 28 10  ---          14 08 50   5.9 291.3  6.4      59.4    63   F  1 205733

13 28 10  1330TITAN    14 08 50   5.5 291.6  6.4      59.2    -7   1  1 205733  13 28 10
13 30 00  ---          14 10 40   5.1 291.9  6.5      59.0   103   F  1 207200
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Huygens Probe VLBI Tracking
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  14 Jan 2005   Day  14 ---

13 30 00  J0744+2120   14 10 40   5.5 291.6  6.4      59.2    -7   1  1 207200  13 30 00
13 31 10  ---          14 11 51   5.3 291.7  6.4      59.1    63   F  1 208133

13 31 10  1330TITAN    14 11 51   4.9 292.0  6.5      58.9    -7   1  1 208133  13 31 10
13 33 00  ---          14 13 41   4.5 292.2  6.5      58.8   103   F  1 209600

13 33 00  J0744+2120   14 13 41   4.9 291.9  6.5      59.0    -7   1  1 209600  13 33 00
13 34 10  ---          14 14 51   4.7 292.1  6.5      58.9    63   F  1 210533

13 34 10  1330TITAN    14 14 51   4.3 292.4  6.5      58.7    -7   1  1 210533  13 34 10
13 36 00  ---          14 16 41   3.9 292.6  6.6      58.5   103   F  1 212000

13 36 00  J0744+2120   14 16 41   4.3 292.3  6.5      58.7    -7   1  1 212000  13 36 00
13 37 10  ---          14 17 52   4.1 292.4  6.5      58.6    63   F  1 212933

13 37 10  1330TITAN    14 17 52   3.7 292.7  6.6      58.5    -7   1  1 212933  13 37 10
13 39 00  ---          14 19 42   3.3 293.0  6.6      58.3   103   F  1 214400

13 39 00  J0744+2120   14 19 42   3.7 292.6  6.6      58.5    -7   1  1 214400  13 39 00
13 40 10  ---          14 20 52   3.5 292.8  6.6      58.4    63   F  1 215333

13 40 10  1330TITAN    14 20 52   3.1 293.1  6.6      58.2    -7   1  1 215333  13 40 10
13 42 00  ---          14 22 42   2.7 293.3  6.7      58.0   103   F  1 216800

13 42 00  J0744+2120   14 22 42   3.1 293.0  6.6      58.2    -7   1  1 216800  13 42 00
13 43 10  ---          14 23 53   2.9 293.2  6.6      58.1    63   F  1 217733

13 43 10  1330TITAN    14 23 53   2.5 293.5  6.7      57.9    -7   1  1 217733  13 43 10
13 45 00  ---          14 25 43   2.1 293.7  6.7  D   57.8     0   F  1 219200

14 53 00  J1215-1731   15 33 54  22.3 231.6  3.3      45.0  4033   1  1 219200  14 53 00
15 00 00  =1213-172    15 40 55  21.1 232.8  3.4      46.0   420   F  1 224800


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: huygS.set
   Matches group v13cm_1 in ./freq_gg057c.dat
    LA,NL only 2200-2400

   Setup group:    6         Station: VLBA              Total bit rate:  512
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for 399999 ft, High density tapes is: 08:20:00
   Two tape drives will be used.  Required by this setup.

   1st LO=   2900.00   2900.00   2900.00   2900.00   2900.00   2900.00   2900.00   2900.00
   Net SB=         L         L         U         U         L         U         L         U
   Pol.  =      RCP       LCP       RCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         2         1         2         3         3         4         4
   BBC SB=         U         U         L         L         U         L         U         L
   IF    =        A         C         A         C         C         C         C         C 

   VLBA FE=     13cm     omit     13cm     omit
   VLBA Synth=  15.4      2.9     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   6  Setup file default.  Used pcal sets:   1
   LO sum=    2034.99   2034.99   2034.99   2034.99   2139.99   2139.99   2286.99   2286.99
   BBC fr=     865.01    865.01    865.01    865.01    760.01    760.01    613.01    613.01
   Bandwd=     16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    S3    S4    S5    S6    S7    S8 
    PCALXB2=   M1    M2    M3    M4    M5    M6    M7    M8 
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19, 66, 82, 67, 83
    barrel=roll_off 
 SOURCE LIST -- Huygens Probe VLBI Tracking
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * J0728+2153        07 25 21.869713   * 07 28 20.608295     07 28 39.692965 
                     21 59 17.09448    * 21 53 06.39058      21 52 33.48805 
                     From catalog imbedded in main SCHED input file.
                     2.5 deg 0.565 Jy @ X-Band
                        0.333 scan hours,      4.833 baseline hours above horizon.

 * J0744+2120        07 41 49.975805   * 07 44 47.277000     07 45 06.220698 
                     21 27 16.93999    * 21 20 00.40500      21 19 20.28697 
                     From catalog imbedded in main SCHED input file.
                     A, 30 mJy
                        2.450 scan hours,    128.422 baseline hours above horizon.

 * 0930TITAN         07 39 42.508522   * 07 42 39.970000     07 42 58.929540 
                     21 29 57.66118    * 21 22 49.50000      21 22 10.30151 
                     From catalog imbedded in main SCHED input file.
                     Titan at 09:30 UT
                        0.403 scan hours,      3.959 baseline hours above horizon.

 * 1000TITAN         07 39 41.957674   * 07 42 39.420000     07 42 58.379625 
                     21 29 58.82492    * 21 22 50.70000      21 22 11.50549 
                     From catalog imbedded in main SCHED input file.
                     Titan at 10:00 UT
                        0.806 scan hours,     10.613 baseline hours above horizon.

 * 1030TITAN         07 39 41.406792   * 07 42 38.870000     07 42 57.829714 
                     21 30 00.08866    * 21 22 52.00000      21 22 12.80947 
                     From catalog imbedded in main SCHED input file.
                     Titan at 10:30 UT
                        0.806 scan hours,     19.250 baseline hours above horizon.

 * 1100TITAN         07 39 40.845903   * 07 42 38.310000     07 42 57.269803 
                     21 30 01.35173    * 21 22 53.30000      21 22 14.11353 
                     From catalog imbedded in main SCHED input file.
                     Titan at 1100 UT
                        0.806 scan hours,     21.666 baseline hours above horizon.

 * 1130TITAN         07 39 40.295055   * 07 42 37.760000     07 42 56.719889 
                     21 30 02.51547    * 21 22 54.50000      21 22 15.31751 
                     From catalog imbedded in main SCHED input file.
                     Titan at 11:30 UT
                        0.806 scan hours,     23.478 baseline hours above horizon.

 * 1200TITAN         07 39 39.744173   * 07 42 37.210000     07 42 56.169978 
                     21 30 03.77920    * 21 22 55.80000      21 22 16.62149 
                     From catalog imbedded in main SCHED input file.
                     Titan at 12:00 UT
                        0.806 scan hours,     24.677 baseline hours above horizon.

 * 1230TITAN         07 39 39.193325   * 07 42 36.660000     07 42 55.620063 
                     21 30 04.94293    * 21 22 57.00000      21 22 17.82547 
                     From catalog imbedded in main SCHED input file.
                     Titan at 12:30 UT
                        0.806 scan hours,     23.696 baseline hours above horizon.

 * 1300TITAN         07 39 38.632436   * 07 42 36.100000     07 42 55.060152 
                     21 30 06.20601    * 21 22 58.30000      21 22 19.12952 
                     From catalog imbedded in main SCHED input file.
                     Titan at 13:00 UT
                        0.806 scan hours,     25.890 baseline hours above horizon.

 * 1330TITAN         07 39 38.081588   * 07 42 35.550000     07 42 54.510238 
                     21 30 07.36974    * 21 22 59.50000      21 22 20.33350 
                     From catalog imbedded in main SCHED input file.
                     Titan at 13:30 UT
                        0.806 scan hours,     21.850 baseline hours above horizon.

 * 1400TITAN         07 39 37.530740   * 07 42 35.000000     07 42 53.960323 
                     21 30 08.53347    * 21 23 00.70000      21 22 21.53748 
                     From catalog imbedded in main SCHED input file.
                     Titan at 14:00 UT
                        0.806 scan hours,     17.104 baseline hours above horizon.

 * 1430TITAN         07 39 36.969884   * 07 42 34.440000     07 42 53.400409 
                     21 30 09.69654    * 21 23 01.90000      21 22 22.74154 
                     From catalog imbedded in main SCHED input file.
                     Titan at 14:30 UT
                        0.806 scan hours,     12.376 baseline hours above horizon.

 * 1500TITAN         07 39 36.419037   * 07 42 33.890000     07 42 52.850494 
                     21 30 10.86027    * 21 23 03.10000      21 22 23.94552 
                     From catalog imbedded in main SCHED input file.
                     Titan at 15:00 UT
                        0.192 scan hours,      3.526 baseline hours above horizon.

 * 1530TITAN         07 39 35.858147   * 07 42 33.330000     07 42 52.290584 
                     21 30 12.12334    * 21 23 04.40000      21 22 25.24957 
                     From catalog imbedded in main SCHED input file.
                     Titan at 15:30 UT
                        0.306 scan hours,      7.632 baseline hours above horizon.

 * 1600TITAN         07 39 35.307299   * 07 42 32.780000     07 42 51.740669 
                     21 30 13.28707    * 21 23 05.60000      21 22 26.45355 
                     From catalog imbedded in main SCHED input file.
                     Titan at 16:00 UT
                        0.153 scan hours,      3.422 baseline hours above horizon.

   J0555+3948        05 52 01.407166   * 05 55 30.805609     05 55 52.990051 
   0552+398          39 48 21.94585    * 39 48 49.16500      39 49 01.47036 
 * DA193             /export/jive/avruch/work/scheds/sched_files/catalogs/sources.vlba
   J0555+39          ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.300 scan hours,      4.298 baseline hours above horizon.

 * J0927+3902        09 23 55.319195   * 09 27 03.013916     09 27 23.257969 
   0923+392          39 15 23.56655    * 39 02 20.85195      39 00 59.39052 
   4C39.25           /export/jive/avruch/work/scheds/sched_files/catalogs/sources.vlba
   J0927+39          ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.167 scan hours,      3.292 baseline hours above horizon.

 * J1215-1731        12 13 11.668015   * 12 15 46.751770     12 16 02.271562 
   1213-172         -17 15 05.20052    *-17 31 45.40289     -17 33 21.41361 
   J1215-17          /export/jive/avruch/work/scheds/sched_files/catalogs/sources.vlba
                     ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.233 scan hours,      7.313 baseline hours above horizon.

 * J1256-0547        12 53 35.831293   * 12 56 11.166560     12 56 26.563083 
   1253-055         -05 31 07.99572    *-05 47 21.52458     -05 49 00.14552 
   3C279             /export/jive/avruch/work/scheds/sched_files/catalogs/sources.vlba
   J1256-05          ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.208 scan hours,      4.139 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0728+2153         176.0
   J0744+2120         179.9
   0930TITAN          179.4
   1000TITAN          179.4
   1030TITAN          179.4
   1100TITAN          179.4
   1130TITAN          179.4
   1200TITAN          179.4
   1230TITAN          179.4
   1300TITAN          179.4
   1330TITAN          179.4
   1400TITAN          179.4
   1430TITAN          179.4
   1500TITAN          179.4
   1530TITAN          179.4
   1600TITAN          179.4
   DA193              150.2
   J0927+3902         151.9
   J1215-1731         103.2
   J1256-0547          99.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

