  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RA KSP: Structure and physics of compact jets
 Exp. Code:  gl038c  


Schedule Version:       0.20
Processed by SCHED version:  11.10  Version 11.1 Beta of about April 26, 201

PI:       Andrei Lobanov

Address:  MPIfR Bonn
          Auf dem Huegel 69
          53121 Bonn, Germany
 

Phone:    +49 228 525 191
EMAIL:    alobanov@mpifr-bonn.mpg.de
Fax:      +49 228 525 229
Phone during observation: +7 903 661 4865

Observing mode: C/K-band, dual-pol

Notes:    C/K-band, Radioastron-compatible frequency setup
          P-CAL is ON, Tsys is ON
          auto-level (AGC) is ON
          Please, send Mk5 disk packs to MPIfR-Bonn

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 ---------- BLOCK 11: C/K-band ground VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00
 Next scan bandwidths:     16.00    16.00    16.00    16.00

00 05 30  0836+710     00 31 26  19.2  17.0 -8.2     -49.9     0        0   00 05 30
00 10 00  ---          00 35 57  19.4  17.2 -8.1     -50.9   270        9   00 05 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

00 10 30  0836+710     00 36 27  19.5  17.2 -8.1     -51.0    15        9   00 10 30
00 15 00  ---          00 40 58  19.8  17.5 -8.0     -52.0   270       17   00 10 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

00 15 30  0836+710     00 41 28  19.8  17.5 -8.0     -52.1    15       17   00 15 30
00 20 00  ---          00 45 59  20.1  17.8 -7.9     -53.1   270       26   00 15 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

00 20 30  0836+710     00 46 29  20.1  17.8 -7.9     -53.2    15       26   00 20 30
00 25 00  ---          00 50 59  20.4  18.0 -7.9     -54.2   270       35   00 20 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 25 30  0836+710     00 51 29  20.5  18.0 -7.9     -54.3    24       35   00 25 30
00 30 00  ---          00 56 00  20.8  18.3 -7.8     -55.3   270       43   00 25 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

00 30 30  0836+710     00 56 30  20.8  18.3 -7.8     -55.4    24       43   00 30 30
00 35 00  ---          01 01 01  21.1  18.5 -7.7     -56.4   270       52   00 30 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

00 35 30  0836+710     01 01 31  21.1  18.5 -7.7     -56.5    24       52   00 35 30
00 40 00  ---          01 06 02  21.4  18.8 -7.6     -57.5   270       61   00 35 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

00 40 30  0836+710     01 06 32  21.5  18.8 -7.6     -57.6    24       61   00 40 30
00 45 00  ---          01 11 03  21.8  19.0 -7.5     -58.6   270       69   00 40 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 45 30  0836+710     01 11 33  21.8  19.0 -7.5     -58.7    24       69   00 45 30
00 50 00  ---          01 16 03  22.1  19.2 -7.4     -59.7   270       78   00 45 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

00 50 30  0836+710     01 16 34  22.2  19.2 -7.4     -59.8    24       78   00 50 30
00 55 00  ---          01 21 04  22.5  19.4 -7.4     -60.8   270       87   00 50 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

00 55 30  0836+710     01 21 34  22.5  19.5 -7.4     -60.9    24       87   00 55 30
01 00 00  ---          01 26 05  22.9  19.7 -7.3     -61.9   270       95   00 55 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

01 00 30  0836+710     01 26 35  22.9  19.7 -7.3     -62.0    24       95   01 00 30
01 05 00  ---          01 31 06  23.2  19.9 -7.2     -63.0   270      104   01 00 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

01 05 30  0836+710     01 31 36  23.3  19.9 -7.2     -63.1    24      104   01 05 30
01 10 00  ---          01 36 07  23.6  20.1 -7.1     -64.1   270      112   01 05 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

01 10 30  0836+710     01 36 37  23.6  20.1 -7.1     -64.2    24      112   01 10 30
01 16 30  ---          01 42 38  24.1  20.3 -7.0     -65.5   360      124   01 10 31

 ---------- BLOCK 12: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

01 17 00  0836+710     01 43 08  24.1  20.3 -7.0     -65.6    24      124   01 17 00
01 26 30  ---          01 52 39  24.8  20.7 -6.8     -67.7   570      142   01 17 01

01 27 00  0836+710     01 53 10  24.9  20.7 -6.8     -67.8    24      142   01 27 00
01 36 30  ---          02 02 41  25.6  21.0 -6.7     -70.0   570      161   01 27 01

01 37 00  0836+710     02 03 11  25.6  21.0 -6.7     -70.1    24      161   01 37 00
01 47 00  ---          02 13 13  26.4  21.3 -6.5     -72.3   600      180   01 37 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 ---------- BLOCK 13: C/K-band ground VLBI scans ----------

01 47 30  0836+710     02 13 43  26.5  21.3 -6.5     -72.4    24      180   01 47 30
01 52 00  ---          02 18 14  26.8  21.4 -6.4     -73.4   270      188   01 47 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

01 52 30  0836+710     02 18 44  26.8  21.5 -6.4     -73.5    24      188   01 52 30
01 57 00  ---          02 23 14  27.2  21.6 -6.3     -74.6   270      197   01 52 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

01 57 30  0836+710     02 23 45  27.2  21.6 -6.3     -74.7    24      197   01 57 30
02 02 00  ---          02 28 15  27.6  21.7 -6.2     -75.7   270      206   01 57 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

02 02 30  0836+710     02 28 45  27.6  21.7 -6.2     -75.8    24      206   02 02 30
02 07 00  ---          02 33 16  28.0  21.8 -6.2     -76.8   270      214   02 02 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 07 30  0836+710     02 33 46  28.0  21.8 -6.2     -76.9    24      214   02 07 30
02 12 00  ---          02 38 17  28.4  21.9 -6.1     -78.0   270      223   02 07 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

02 12 30  0836+710     02 38 47  28.4  21.9 -6.1     -78.1    24      223   02 12 30
02 17 00  ---          02 43 18  28.8  22.0 -6.0     -79.1   270      232   02 12 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

02 17 30  0836+710     02 43 48  28.8  22.0 -6.0     -79.2    24      232   02 17 30
02 22 00  ---          02 48 19  29.2  22.1 -5.9     -80.2   270      240   02 17 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

02 22 30  0836+710     02 48 49  29.3  22.1 -5.9     -80.4    24      240   02 22 30
02 27 00  ---          02 53 19  29.6  22.2 -5.8     -81.4   270      249   02 22 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 27 30  0836+710     02 53 49  29.7  22.2 -5.8     -81.5    24      249   02 27 30
02 32 00  ---          02 58 20  30.0  22.2 -5.7     -82.5   270      258   02 27 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

02 32 30  0836+710     02 58 50  30.1  22.2 -5.7     -82.7    24      258   02 32 30
02 37 00  ---          03 03 21  30.4  22.3 -5.7     -83.7   270      266   02 32 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

02 37 30  0836+710     03 03 51  30.5  22.3 -5.7     -83.8    24      266   02 37 30
02 42 00  ---          03 08 22  30.8  22.3 -5.6     -84.9   270      275   02 37 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

02 42 30  0836+710     03 08 52  30.9  22.3 -5.6     -85.0    24      275   02 42 30
02 47 00  ---          03 13 23  31.3  22.4 -5.5     -86.0   270      284   02 42 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 47 30  0836+710     03 13 53  31.3  22.4 -5.5     -86.1    24      284   02 47 30
02 52 00  ---          03 18 23  31.7  22.4 -5.4     -87.2   270      292   02 47 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

02 52 30  0836+710     03 18 54  31.7  22.4 -5.4     -87.3    24      292   02 52 30
02 58 30  ---          03 24 55  32.2  22.4 -5.3     -88.7   360      304   02 52 31

 ---------- BLOCK 14: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 59 00  0836+710     03 25 25  32.2  22.4 -5.3     -88.8    24      304   02 59 00
03 08 30  ---          03 34 56  33.0  22.4 -5.1     -91.1   570      322   02 59 01

03 09 00  0836+710     03 35 26  33.1  22.4 -5.1     -91.2    24      322   03 09 00
03 18 30  ---          03 44 58  33.8  22.4 -5.0     -93.5   570      340   03 09 01

03 19 00  0836+710     03 45 28  33.9  22.4 -5.0     -93.6    24      340   03 19 00
03 29 00  ---          03 55 30  34.7  22.3 -4.8     -96.0   600      360   03 19 01

 ---------- BLOCK 15: C/K-band ground VLBI scans ----------

03 29 30  0836+710     03 56 00  34.7  22.3 -4.8     -96.1    24      360   03 29 30
03 34 00  ---          04 00 30  35.1  22.2 -4.7     -97.2   270      368   03 29 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

03 34 30  0836+710     04 01 00  35.2  22.2 -4.7     -97.3    24      368   03 34 30
03 39 00  ---          04 05 31  35.5  22.2 -4.6     -98.4   270      377   03 34 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

03 39 30  0836+710     04 06 01  35.6  22.2 -4.6     -98.6    24      377   03 39 30
03 44 00  ---          04 10 32  35.9  22.1 -4.5     -99.7   270      386   03 39 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

03 44 30  0836+710     04 11 02  36.0  22.1 -4.5     -99.8    24      386   03 44 30
03 49 00  ---          04 15 33  36.3  22.0 -4.5    -100.9   270      394   03 44 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

03 49 30  0836+710     04 16 03  36.4  22.0 -4.4    -101.0    24      394   03 49 30
03 54 00  ---          04 20 34  36.7  21.9 -4.4    -102.2   270      403   03 49 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

03 54 30  0836+710     04 21 04  36.8  21.9 -4.4    -102.3    24      403   03 54 30
03 59 00  ---          04 25 34  37.1  21.8 -4.3    -103.4   270      412   03 54 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

03 59 30  0836+710     04 26 05  37.2  21.8 -4.3    -103.5    24      412   03 59 30
04 04 00  ---          04 30 35  37.5  21.7 -4.2    -104.7   270      420   03 59 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

04 04 30  0836+710     04 31 05  37.6  21.6 -4.2    -104.8    24      420   04 04 30
04 09 00  ---          04 35 36  37.9  21.5 -4.1    -105.9   270      429   04 04 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

04 09 30  0836+710     04 36 06  38.0  21.5 -4.1    -106.1    24      429   04 09 30
04 14 00  ---          04 40 37  38.3  21.4 -4.0    -107.2   270      437   04 09 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

04 14 30  0836+710     04 41 07  38.4  21.4 -4.0    -107.3    24      437   04 14 30
04 19 00  ---          04 45 38  38.7  21.2 -4.0    -108.5   270      446   04 14 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

04 19 30  0836+710     04 46 08  38.8  21.2 -3.9    -108.6    24      446   04 19 30
04 24 00  ---          04 50 39  39.1  21.0 -3.9    -109.8   270      455   04 19 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

04 24 30  0836+710     04 51 09  39.1  21.0 -3.9    -109.9    24      455   04 24 30
04 29 00  ---          04 55 39  39.5  20.8 -3.8    -111.1   270      463   04 24 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

04 29 30  0836+710     04 56 09  39.5  20.8 -3.8    -111.2    24      463   04 29 30
04 34 00  ---          05 00 40  39.9  20.7 -3.7    -112.4   270      472   04 29 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

04 34 30  0836+710     05 01 10  39.9  20.6 -3.7    -112.5    24      472   04 34 30
04 39 00  ---          05 05 41  40.3  20.4 -3.6    -113.7   270      481   04 34 31

 ---------- BLOCK 16: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

04 41 00  0836+710     05 07 41  40.4  20.4 -3.6    -114.3   114      481   04 41 00
04 50 30  ---          05 17 13  41.1  19.9 -3.4    -116.8   570      499   04 41 01

04 51 00  0836+710     05 17 43  41.1  19.9 -3.4    -116.9    24      499   04 51 00
05 00 30  ---          05 27 15  41.8  19.4 -3.3    -119.5   570      517   04 51 01

05 01 00  0836+710     05 27 45  41.9  19.4 -3.3    -119.6    24      517   05 01 00
05 11 00  ---          05 37 46  42.6  18.8 -3.1    -122.4   600      537   05 01 01

 ---------- BLOCK 17: C/K-band ground VLBI scans ----------

05 11 30  0836+710     05 38 16  42.6  18.8 -3.1    -122.5    24      537   05 11 30
05 16 00  ---          05 42 47  42.9  18.5 -3.0    -123.8   270      545   05 11 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

05 16 30  0836+710     05 43 17  43.0  18.5 -3.0    -123.9    24      545   05 16 30
05 21 00  ---          05 47 48  43.3  18.2 -2.9    -125.2   270      554   05 16 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

05 21 30  0836+710     05 48 18  43.3  18.1 -2.9    -125.3    24      554   05 21 30
05 26 00  ---          05 52 49  43.6  17.8 -2.8    -126.6   270      562   05 21 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

05 26 30  0836+710     05 53 19  43.6  17.8 -2.8    -126.7    24      562   05 26 30
05 31 00  ---          05 57 50  43.9  17.5 -2.8    -128.0   270      571   05 26 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

05 31 30  0836+710     05 58 20  43.9  17.5 -2.7    -128.2    24      571   05 31 30
05 36 00  ---          06 02 50  44.2  17.1 -2.7    -129.5   270      580   05 31 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

05 36 30  0836+710     06 03 20  44.3  17.1 -2.7    -129.6    24      580   05 36 30
05 41 00  ---          06 07 51  44.6  16.8 -2.6    -130.9   270      588   05 36 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

05 41 30  0836+710     06 08 21  44.6  16.7 -2.6    -131.0    24      588   05 41 30
05 46 00  ---          06 12 52  44.9  16.4 -2.5    -132.4   270      597   05 41 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

05 46 30  0836+710     06 13 22  44.9  16.3 -2.5    -132.5    24      597   05 46 30
05 51 00  ---          06 17 53  45.2  16.0 -2.4    -133.8   270      606   05 46 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

05 51 30  0836+710     06 18 23  45.2  15.9 -2.4    -134.0    24      606   05 51 30
05 56 00  ---          06 22 54  45.5  15.6 -2.3    -135.3   270      614   05 51 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

05 56 30  0836+710     06 23 24  45.5  15.5 -2.3    -135.4    24      614   05 56 30
06 01 00  ---          06 27 55  45.7  15.1 -2.2    -136.8   270      623   05 56 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

06 01 30  0836+710     06 28 25  45.8  15.1 -2.2    -136.9    24      623   06 01 30
06 06 00  ---          06 32 55  46.0  14.7 -2.2    -138.3   270      632   06 01 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

06 06 30  0836+710     06 33 25  46.0  14.7 -2.2    -138.4    24      632   06 06 30
06 11 00  ---          06 37 56  46.3  14.3 -2.1    -139.8   270      640   06 06 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

06 11 30  0836+710     06 38 26  46.3  14.2 -2.1    -139.9    24      640   06 11 30
06 16 00  ---          06 42 57  46.5  13.8 -2.0    -141.3   270      649   06 11 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

06 16 30  0836+710     06 43 27  46.6  13.8 -2.0    -141.5    24      649   06 16 30
06 22 30  ---          06 49 28  46.9  13.2 -1.9    -143.3   360      661   06 16 31

 ---------- BLOCK 18: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

06 23 00  0836+710     06 49 58  46.9  13.1 -1.9    -143.4    24      661   06 23 00
06 32 30  ---          06 59 30  47.3  12.2 -1.7    -146.4   570      679   06 23 01

06 33 00  0836+710     07 00 00  47.4  12.1 -1.7    -146.5    24      679   06 33 00
06 42 30  ---          07 09 31  47.8  11.2 -1.6    -149.5   570      697   06 33 01

06 43 00  0836+710     07 10 01  47.8  11.1 -1.5    -149.7    24      697   06 43 00
06 53 00  ---          07 20 03  48.2  10.0 -1.4    -152.8   600      716   06 43 01

 ---------- BLOCK 19: C/K-band ground VLBI scans ----------

06 53 30  0836+710     07 20 33  48.2  10.0 -1.4    -153.0    24      716   06 53 30
06 58 00  ---          07 25 04  48.4   9.5 -1.3    -154.4   270      725   06 53 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

06 58 30  0836+710     07 25 34  48.4   9.4 -1.3    -154.6    24      725   06 58 30
07 03 00  ---          07 30 05  48.6   8.9 -1.2    -156.0   270      734   06 58 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

07 03 30  0836+710     07 30 35  48.6   8.9 -1.2    -156.2    24      734   07 03 30
07 08 00  ---          07 35 06  48.7   8.3 -1.1    -157.7   270      742   07 03 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

07 08 30  0836+710     07 35 36  48.7   8.3 -1.1    -157.8    24      742   07 08 30
07 13 00  ---          07 40 06  48.9   7.8 -1.0    -159.3   270      751   07 08 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

07 13 30  0836+710     07 40 36  48.9   7.7 -1.0    -159.4    24      751   07 13 30
07 18 00  ---          07 45 07  49.0   7.2 -1.0    -160.9   270      760   07 13 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

07 18 30  0836+710     07 45 37  49.0   7.1 -1.0    -161.1    24      760   07 18 30
07 23 00  ---          07 50 08  49.1   6.6 -0.9    -162.5   270      768   07 18 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

07 23 30  0836+710     07 50 38  49.2   6.5 -0.9    -162.7    24      768   07 23 30
07 28 00  ---          07 55 09  49.3   6.0 -0.8    -164.2   270      777   07 23 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

07 28 30  0836+710     07 55 39  49.3   5.9 -0.8    -164.3    24      777   07 28 30
07 33 00  ---          08 00 10  49.4   5.4 -0.7    -165.8   270      786   07 28 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

07 33 30  0836+710     08 00 40  49.4   5.3 -0.7    -166.0    24      786   07 33 30
07 38 00  ---          08 05 10  49.5   4.7 -0.6    -167.5   270      794   07 33 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

07 38 30  0836+710     08 05 41  49.5   4.7 -0.6    -167.6    24      794   07 38 30
07 43 00  ---          08 10 11  49.5   4.1 -0.5    -169.1   270      803   07 38 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

07 43 30  0836+710     08 10 41  49.5   4.1 -0.5    -169.3    24      803   07 43 30
07 48 00  ---          08 15 12  49.6   3.5 -0.5    -170.8   270      812   07 43 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

07 48 30  0836+710     08 15 42  49.6   3.4 -0.5    -171.0    24      812   07 48 30
07 53 00  ---          08 20 13  49.7   2.9 -0.4    -172.5   270      820   07 48 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

07 53 30  0836+710     08 20 43  49.7   2.8 -0.4    -172.6    24      820   07 53 30
07 58 00  ---          08 25 14  49.7   2.2 -0.3    -174.1   270      829   07 53 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

07 58 30  0836+710     08 25 44  49.7   2.2 -0.3    -174.3    24      829   07 58 30
08 04 30  ---          08 31 45  49.8   1.4 -0.2    -176.3   360      840   07 58 31

 ---------- BLOCK 20: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 05 00  0836+710     08 32 15  49.8   1.4 -0.2    -176.5    24      840   08 05 00
08 14 30  ---          08 41 46  49.8   0.1 -0.0    -179.6   570      859   08 05 01

08 15 00  0836+710     08 42 17  49.8   0.1 -0.0    -179.8    24      859   08 15 00
08 24 30  ---          08 51 48  49.8  -1.1  0.1     177.0   570      877   08 15 01

08 25 00  0836+710     08 52 18  49.8  -1.2  0.2     176.9    24      877   08 25 00
08 35 00  ---          09 02 20  49.7  -2.5  0.3     173.5   600      896   08 25 01

 ---------- BLOCK 21: C/K-band ground VLBI scans ----------

08 35 30  0836+710     09 02 50  49.7  -2.5  0.3     173.4    24      896   08 35 30
08 40 00  ---          09 07 21  49.7  -3.1  0.4     171.9   270      905   08 35 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

08 40 30  0836+710     09 07 51  49.6  -3.2  0.4     171.7    24      905   08 40 30
08 45 00  ---          09 12 21  49.6  -3.7  0.5     170.2   270      913   08 40 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

08 45 30  0836+710     09 12 52  49.6  -3.8  0.5     170.0    24      913   08 45 30
08 50 00  ---          09 17 22  49.5  -4.3  0.6     168.5   270      922   08 45 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

08 50 30  0836+710     09 17 52  49.5  -4.4  0.6     168.4    24      922   08 50 30
08 55 00  ---          09 22 23  49.4  -5.0  0.7     166.9   270      931   08 50 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 55 30  0836+710     09 22 53  49.4  -5.0  0.7     166.7    24      931   08 55 30
09 00 00  ---          09 27 24  49.3  -5.6  0.7     165.2   270      939   08 55 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

09 00 30  0836+710     09 27 54  49.3  -5.6  0.8     165.1    24      939   09 00 30
09 05 00  ---          09 32 25  49.2  -6.2  0.8     163.6   270      948   09 00 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

09 05 30  0836+710     09 32 55  49.2  -6.2  0.8     163.4    24      948   09 05 30
09 10 00  ---          09 37 26  49.1  -6.8  0.9     162.0   270      957   09 05 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

09 10 30  0836+710     09 37 56  49.1  -6.8  0.9     161.8    24      957   09 10 30
09 15 00  ---          09 42 26  49.0  -7.4  1.0     160.3   270      965   09 10 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

09 15 30  0836+710     09 42 56  48.9  -7.4  1.0     160.2    24      965   09 15 30
09 20 00  ---          09 47 27  48.8  -8.0  1.1     158.7   270      974   09 15 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

09 20 30  0836+710     09 47 57  48.8  -8.0  1.1     158.5    24      974   09 20 30
09 25 00  ---          09 52 28  48.7  -8.5  1.2     157.1   270      983   09 20 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

09 25 30  0836+710     09 52 58  48.6  -8.6  1.2     156.9    24      983   09 25 30
09 30 00  ---          09 57 29  48.5  -9.1  1.2     155.5   270      991   09 25 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

09 30 30  0836+710     09 57 59  48.5  -9.2  1.3     155.3    24      991   09 30 30
09 35 00  ---          10 02 30  48.3  -9.7  1.3     153.9   270     1000   09 30 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

09 35 30  0836+710     10 03 00  48.3  -9.7  1.3     153.7    24     1000   09 35 30
09 40 00  ---          10 07 30  48.1 -10.2  1.4     152.3   270     1009   09 35 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RA KSP: Structure and physics of compact jets
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  11 Jan 2014   Day  11 ---

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

09 40 30  0836+710     10 08 01  48.1 -10.3  1.4     152.1    24     1009   09 40 30
09 45 00  ---          10 12 31  47.9 -10.8  1.5     150.7   270     1017   09 40 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

09 45 30  0836+710     10 13 01  47.9 -10.8  1.5     150.5    24     1017   09 45 30
09 50 00  ---          10 17 32  47.7 -11.3  1.6     149.1   270     1026   09 45 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

09 50 30  0836+710     10 18 02  47.7 -11.3  1.6     148.9    24     1026   09 50 30
09 55 00  ---          10 22 33  47.5 -11.8  1.7     147.5   270     1035   09 50 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

09 55 30  0836+710     10 23 03  47.5 -11.9  1.7     147.4    24     1035   09 55 30
10 00 00  ---          10 27 34  47.3 -12.3  1.7     146.0   270     1043   09 55 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra6cm2.set
   Matching groups in ./gl038c_freq_sess313rdbe.dat:
     vc_d

   Setup group:    4         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.1      4.1     15.1

  The following frequency sets based on these setups were used.

   Frequency Set:  14  Setup file default.
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
    Matching frequency sets:  14  15  16  17  18  19  20  21  22  51

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gl038c_freq_sess313rdbe.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   39         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     11.4     11.4

  The following frequency sets based on these setups were used.

   Frequency Set:  23  Setup file default.
   LO sum=   15369.00  15369.00  15369.00  15369.00
   BBC fr=     769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  23  24  25  26  27  28  29  30  31  55

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gl038c_freq_sess313rdbe.dat:
     v7mm_c8

   Setup group:   50         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.

   Frequency Set:  33  Setup file default.
   LO sum=   43120.00  43120.00  43136.00  43136.00
   BBC fr=     720.00    720.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  33  34  35  36  37  38  39  40  41  56

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra1cm2.set
   Matching groups in ./gl038c_freq_sess313rdbe.dat:
     v1cm_b3

   Setup group:   24         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.1     12.4

  The following frequency sets based on these setups were used.

   Frequency Set:  42  Setup file default.
   LO sum=   22236.00  22236.00  22236.00  22236.00
   BBC fr=     736.00    736.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  42  43  44  45  46  47  48  49  50  57

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 42.234022       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 55.00899        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0836+710          08 36 21.556646   * 08 41 24.365284     08 42 52.671494       0.00
   J0841+7053        71 04 22.42740    * 70 53 42.17302      70 50 22.34628        0.00
                     ./gl038c_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 4321 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra6cm2.set            5                                 4.833     0.000
  0836+710   ra6cm2.set            1 2 3 4 5 11 13 14 53            16.475   573.800
             ra1cm2.set            6 7 8 9 12 42                    14.400   246.867
             ra2cm2.set            23 54                             1.900    97.575
             ra7mm2.set            32 33                             1.425    76.125


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             113.7
   0836+710           129.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

