  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN imaging
 Exp. Code:  gl041a  


Schedule Version:       1.00
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Andrei Lobanov

Address:  MPIfR
          Auf dem Huegel 69
          53121 Bonn, Germany
 

Phone:    +7-903-6614865
EMAIL:    kirx@kirx.net, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +7-903-6614865

Observing mode: K-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          Mark5C stations should record in Mk5B+ format
          P-CAL is ON, Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Jan 2015   Day   3 ---

 ---------- Space segment 01: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00

22 00 00  0716+714     21 57 02  15.5  11.9 -9.4     -33.6     0        0   22 00 00
22 09 30  ---          22 06 34  15.9  12.6 -9.3     -35.7   570       37   22 00 01

22 10 00  0716+714     22 07 04  15.9  12.6 -9.3     -35.8    24       37   22 10 00
22 19 30  ---          22 16 36  16.4  13.2 -9.1     -37.9   570       73   22 10 01

22 20 00  0716+714     22 17 06  16.4  13.3 -9.1     -38.0    24       73   22 20 00
22 29 30  ---          22 26 37  16.9  13.9 -9.0     -40.1   570      110   22 20 01

22 30 00  0716+714     22 27 07  16.9  13.9 -8.9     -40.2    24      110   22 30 00
22 39 30  ---          22 36 39  17.4  14.5 -8.8     -42.3   570      147   22 30 01

22 40 00  0716+714     22 37 09  17.4  14.5 -8.8     -42.4    24      147   22 40 00
22 49 30  ---          22 46 40  18.0  15.1 -8.6     -44.5   570      184   22 40 01

22 50 00  0716+714     22 47 11  18.0  15.2 -8.6     -44.6    24      184   22 50 00
22 59 30  ---          22 56 42  18.5  15.7 -8.4     -46.7   570      220   22 50 01

23 00 00  0716+714     22 57 12  18.6  15.7 -8.4     -46.8    24      220   23 00 00
23 09 30  ---          23 06 44  19.1  16.3 -8.3     -48.8   570      257   23 00 01

23 10 00  0716+714     23 07 14  19.2  16.3 -8.3     -49.0    24      257   23 10 00
23 19 30  ---          23 16 45  19.7  16.8 -8.1     -51.0   570      294   23 10 01

23 20 00  0716+714     23 17 15  19.8  16.9 -8.1     -51.1    24      294   23 20 00
23 29 30  ---          23 26 47  20.4  17.4 -7.9     -53.2   570      330   23 20 01

23 30 00  0716+714     23 27 17  20.4  17.4 -7.9     -53.3    24      330   23 30 00
23 39 30  ---          23 36 49  21.0  17.9 -7.8     -55.4   570      367   23 30 01

23 40 00  0716+714     23 37 19  21.1  17.9 -7.8     -55.5    24      367   23 40 00
23 49 30  ---          23 46 50  21.7  18.3 -7.6     -57.6   570      404   23 40 01

23 50 00  0716+714     23 47 20  21.7  18.4 -7.6     -57.7    24      404   23 50 00
23 59 30  ---          23 56 52  22.4  18.8 -7.4     -59.8   570      441   23 50 01

 --- Sun   4 Jan 2015   Day   4 ---

00 00 00  0716+714     23 57 22  22.4  18.8 -7.4     -59.9    24      441   00 00 00
00 09 30  ---          00 06 54  23.1  19.2 -7.3     -62.0   570      477   00 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

00 10 00  0716+714     00 07 24  23.1  19.2 -7.3     -62.2    24      477   00 10 00
00 19 30  ---          00 16 55  23.8  19.6 -7.1     -64.3   570      514   00 10 01

00 20 00  0716+714     00 17 25  23.8  19.6 -7.1     -64.4    24      514   00 20 00
00 29 30  ---          00 26 57  24.5  20.0 -6.9     -66.5   570      551   00 20 01

00 30 00  0716+714     00 27 27  24.6  20.0 -6.9     -66.6    24      551   00 30 00
00 40 00  ---          00 37 29  25.3  20.3 -6.8     -68.8   600      589   00 30 01

 ---------- Ground segment 01: Q/U-band VLBI scans ----------

00 42 00  0836+710     00 39 29  19.7  17.4 -8.1     -51.7   101      589   00 42 00
00 46 00  ---          00 43 30  19.9  17.6 -8.0     -52.5   240      605   00 42 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

00 46 30  0836+710     00 44 00  20.0  17.7 -8.0     -52.6    24      605   00 46 30
00 51 30  ---          00 49 01  20.3  17.9 -7.9     -53.7   300      624   00 46 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

00 52 00  0836+710     00 49 31  20.3  17.9 -7.9     -53.8    24      624   00 52 00
00 57 00  ---          00 54 31  20.6  18.2 -7.8     -54.9   300      643   00 52 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

00 59 00  0716+714     00 56 32  26.8  20.9 -6.5     -73.1   100      643   00 59 00
01 04 00  ---          01 01 33  27.1  21.0 -6.4     -74.2   300      663   00 59 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

01 04 30  0716+714     01 02 03  27.2  21.0 -6.4     -74.3    24      663   01 04 30
01 09 30  ---          01 07 03  27.6  21.1 -6.3     -75.5   300      682   01 04 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

01 10 30  0716+714     01 08 04  27.6  21.2 -6.3     -75.7    54      682   01 10 30
01 15 00  ---          01 12 34  28.0  21.3 -6.2     -76.7   270      699   01 10 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

01 15 30  0716+714     01 13 04  28.0  21.3 -6.2     -76.8    24      699   01 15 30
01 20 00  ---          01 17 35  28.4  21.4 -6.1     -77.9   270      717   01 15 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

01 20 30  0716+714     01 18 05  28.4  21.4 -6.1     -78.0    24      717   01 20 30
01 25 00  ---          01 22 36  28.8  21.4 -6.0     -79.0   270      734   01 20 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

01 26 30  0836+710     01 24 06  22.7  19.6 -7.3     -61.4    70      734   01 26 30
01 30 00  ---          01 27 37  23.0  19.7 -7.3     -62.2   210      748   01 26 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

01 30 30  0836+710     01 28 07  23.0  19.7 -7.2     -62.3    24      748   01 30 30
01 35 00  ---          01 32 38  23.3  19.9 -7.2     -63.3   270      765   01 30 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

01 35 30  0836+710     01 33 08  23.4  19.9 -7.2     -63.4    24      765   01 35 30
01 40 00  ---          01 37 38  23.7  20.1 -7.1     -64.4   270      783   01 35 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

01 41 30  0716+714     01 39 09  30.1  21.7 -5.7     -82.8    70      783   01 41 30
01 45 00  ---          01 42 39  30.4  21.7 -5.7     -83.6   210      796   01 41 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

01 45 30  0716+714     01 43 09  30.4  21.7 -5.7     -83.7    24      796   01 45 30
01 50 00  ---          01 47 40  30.8  21.8 -5.6     -84.8   270      813   01 45 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

01 50 30  0716+714     01 48 10  30.8  21.8 -5.6     -84.9    24      813   01 50 30
01 55 00  ---          01 52 41  31.2  21.8 -5.5     -86.0   270      831   01 50 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

01 56 30  0836+710     01 54 11  24.9  20.7 -6.8     -68.1    70      831   01 56 30
02 00 00  ---          01 57 42  25.2  20.8 -6.8     -68.8   210      844   01 56 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

02 00 30  0836+710     01 58 12  25.2  20.9 -6.7     -68.9    24      844   02 00 30
02 05 00  ---          02 02 43  25.6  21.0 -6.7     -69.9   270      862   02 00 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

02 05 30  0836+710     02 03 13  25.6  21.0 -6.7     -70.1    24      862   02 05 30
02 10 00  ---          02 07 43  26.0  21.2 -6.6     -71.1   270      879   02 05 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

02 12 30  0716+714     02 10 14  32.6  21.9 -5.2     -90.1   129      879   02 12 30
02 16 00  ---          02 13 44  32.9  21.9 -5.2     -90.9   210      893   02 12 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

02 16 30  0716+714     02 14 14  32.9  21.9 -5.2     -91.0    24      893   02 16 30
02 21 00  ---          02 18 45  33.3  21.8 -5.1     -92.1   270      910   02 16 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

02 21 30  0716+714     02 19 15  33.3  21.8 -5.1     -92.2    24      910   02 21 30
02 26 00  ---          02 23 46  33.7  21.8 -5.0     -93.3   270      927   02 21 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

02 27 30  0836+710     02 25 16  27.4  21.6 -6.3     -75.0    69      927   02 27 30
02 31 00  ---          02 28 47  27.6  21.7 -6.2     -75.8   210      941   02 27 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

02 31 30  0836+710     02 29 17  27.7  21.7 -6.2     -75.9    24      941   02 31 30
02 36 00  ---          02 33 48  28.0  21.8 -6.2     -76.9   270      958   02 31 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

02 36 30  0836+710     02 34 18  28.1  21.8 -6.1     -77.0    24      958   02 36 30
02 41 00  ---          02 38 48  28.4  21.9 -6.1     -78.1   270      976   02 36 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

02 42 30  0716+714     02 40 19  35.0  21.7 -4.7     -97.3    69      976   02 42 30
02 46 00  ---          02 43 49  35.3  21.6 -4.7     -98.2   210      989   02 42 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

02 46 30  0716+714     02 44 19  35.3  21.6 -4.7     -98.3    24      989   02 46 30
02 51 00  ---          02 48 50  35.6  21.6 -4.6     -99.4   270     1007   02 46 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

02 51 30  0716+714     02 49 20  35.7  21.5 -4.6     -99.5    24     1007   02 51 30
02 55 30  ---          02 53 21  36.0  21.5 -4.5    -100.5   240     1022   02 51 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

02 56 01  0716+714     02 53 52  36.0  21.5 -4.5    -100.6    25     1022   02 56 01
03 04 01  ---          03 01 53  36.7  21.3 -4.4    -102.6   480     1053   02 56 02

 ---------- Space segment 02: K-band VLBI scans ----------

03 05 00  0716+714     03 02 52  36.8  21.3 -4.3    -102.9    53     1053   03 05 00
03 14 30  ---          03 12 24  37.5  21.1 -4.2    -105.3   570     1090   03 05 01

03 15 00  0716+714     03 12 54  37.5  21.0 -4.2    -105.4    24     1090   03 15 00
03 24 30  ---          03 22 26  38.3  20.8 -4.0    -107.8   570     1127   03 15 01

03 25 00  0716+714     03 22 56  38.3  20.7 -4.0    -108.0    24     1127   03 25 00
03 34 30  ---          03 32 27  39.0  20.4 -3.9    -110.4   570     1163   03 25 01

03 35 00  0716+714     03 32 57  39.1  20.4 -3.8    -110.5    24     1163   03 35 00
03 45 00  ---          03 42 59  39.8  20.0 -3.7    -113.2   600     1202   03 35 01

 ---------- Ground segment 02: Q/K/U-band VLBI scans ----------

03 45 30  0716+714     03 43 29  39.8  20.0 -3.7    -113.3    24     1202   03 45 30
03 49 00  ---          03 47 00  40.1  19.9 -3.6    -114.2   210     1215   03 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

03 49 30  0716+714     03 47 30  40.1  19.8 -3.6    -114.4    24     1215   03 49 30
03 54 00  ---          03 52 00  40.5  19.6 -3.5    -115.6   270     1233   03 49 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

03 54 30  0716+714     03 52 31  40.5  19.6 -3.5    -115.7    24     1233   03 54 30
03 59 00  ---          03 57 01  40.8  19.4 -3.4    -116.9   270     1250   03 54 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

04 00 00  0836+710     03 58 01  34.9  22.3 -4.7     -96.6    40     1250   04 00 00
04 04 00  ---          04 02 02  35.2  22.2 -4.7     -97.6   240     1266   04 00 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

04 04 30  0836+710     04 02 32  35.3  22.2 -4.7     -97.7    24     1266   04 04 30
04 09 00  ---          04 07 03  35.6  22.2 -4.6     -98.8   270     1283   04 04 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

04 09 30  0836+710     04 07 33  35.7  22.1 -4.6     -98.9    24     1283   04 09 30
04 14 00  ---          04 12 04  36.0  22.1 -4.5    -100.0   270     1300   04 09 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

04 15 00  0716+714     04 13 04  41.9  18.6 -3.2    -121.2    40     1300   04 15 00
04 19 00  ---          04 17 05  42.2  18.3 -3.1    -122.3   240     1316   04 15 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

04 19 30  0716+714     04 17 35  42.3  18.3 -3.1    -122.5    24     1316   04 19 30
04 24 00  ---          04 22 05  42.6  18.0 -3.0    -123.7   270     1333   04 19 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

04 24 30  0716+714     04 22 35  42.6  18.0 -3.0    -123.9    24     1333   04 24 30
04 29 00  ---          04 27 06  42.9  17.7 -2.9    -125.1   270     1351   04 24 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 ---------- Space segment 03: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

04 30 00  0716+714     04 28 06  43.0  17.7 -2.9    -125.4    54     1351   04 30 00
04 39 30  ---          04 37 38  43.6  17.0 -2.8    -128.1   570     1387   04 30 01

04 40 00  0716+714     04 38 08  43.6  17.0 -2.8    -128.2    24     1387   04 40 00
04 49 30  ---          04 47 40  44.2  16.3 -2.6    -131.0   570     1424   04 40 01

04 50 00  0716+714     04 48 10  44.2  16.3 -2.6    -131.1    24     1424   04 50 00
05 00 00  ---          04 58 11  44.8  15.5 -2.4    -134.0   600     1463   04 50 01

 ---------- Ground segment 03: Q/K/U-band VLBI scans ----------

05 00 30  0716+714     04 58 41  44.8  15.5 -2.4    -134.2    24     1463   05 00 30
05 05 00  ---          05 03 12  45.1  15.1 -2.3    -135.5   270     1480   05 00 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

05 05 30  0716+714     05 03 42  45.1  15.1 -2.3    -135.6    24     1480   05 05 30
05 10 00  ---          05 08 13  45.4  14.7 -2.3    -137.0   270     1498   05 05 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

05 10 30  0716+714     05 08 43  45.4  14.7 -2.2    -137.1    24     1498   05 10 30
05 15 00  ---          05 13 14  45.6  14.3 -2.2    -138.5   270     1515   05 10 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

05 16 00  0836+710     05 14 14  40.9  20.1 -3.5    -116.0    42     1515   05 16 00
05 20 30  ---          05 18 45  41.2  19.8 -3.4    -117.2   270     1532   05 16 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

05 21 00  0836+710     05 19 15  41.3  19.8 -3.4    -117.3    24     1532   05 21 00
05 26 00  ---          05 24 16  41.6  19.6 -3.3    -118.7   300     1552   05 21 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

05 26 30  0836+710     05 24 46  41.7  19.5 -3.3    -118.8    24     1552   05 26 30
05 31 00  ---          05 29 16  42.0  19.3 -3.2    -120.0   270     1569   05 26 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

05 37 00  4C39.25      05 35 17  42.3  63.3 -3.9     -81.4   321     1569   05 37 00
05 41 00  ---          05 39 18  43.1  63.5 -3.8     -81.9   240     1584   05 37 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

05 41 30  4C39.25      05 39 48  43.2  63.5 -3.8     -82.0    24     1584   05 41 30
05 45 30  ---          05 43 49  44.0  63.6 -3.7     -82.5   240     1600   05 41 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

05 46 00  4C39.25      05 44 19  44.1  63.6 -3.7     -82.6    24     1600   05 46 00
05 50 00  ---          05 48 20  44.8  63.8 -3.7     -83.1   240     1615   05 46 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

05 53 30  0716+714     05 51 50  47.4  10.6 -1.5    -150.3   165     1615   05 53 30
05 58 30  ---          05 56 51  47.6  10.1 -1.4    -151.8   300     1635   05 53 31

05 59 00  0716+714     05 57 21  47.7  10.1 -1.4    -152.0    24     1635   05 59 00
06 04 00  ---          06 02 22  47.8   9.5 -1.4    -153.6   300     1654   05 59 01

 ---------- Space segment 04: K-band VLBI scans ----------

06 05 00  0716+714     06 03 22  47.9   9.4 -1.3    -153.9    54     1654   06 05 00
06 14 30  ---          06 12 54  48.2   8.4 -1.2    -156.9   570     1691   06 05 01

06 15 00  0716+714     06 13 24  48.2   8.3 -1.2    -157.1    24     1691   06 15 00
06 24 30  ---          06 22 55  48.5   7.3 -1.0    -160.1   570     1727   06 15 01

06 25 00  0716+714     06 23 25  48.5   7.2 -1.0    -160.3    24     1727   06 25 00
06 35 00  ---          06 33 27  48.7   6.1 -0.8    -163.5   600     1766   06 25 01

 ---------- Ground segment 04: Q/K/U-band VLBI scans ----------

06 35 30  0716+714     06 33 57  48.8   6.0 -0.8    -163.7    24     1766   06 35 30
06 40 00  ---          06 38 28  48.9   5.5 -0.8    -165.2   270     1784   06 35 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

06 40 30  0716+714     06 38 58  48.9   5.4 -0.7    -165.3    24     1784   06 40 30
06 45 00  ---          06 43 29  49.0   4.9 -0.7    -166.8   270     1801   06 40 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

06 45 30  0716+714     06 43 59  49.0   4.8 -0.7    -167.0    24     1801   06 45 30
06 50 00  ---          06 48 29  49.0   4.3 -0.6    -168.4   270     1818   06 45 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

06 51 00  0836+710     06 49 30  46.9  13.2 -1.9    -143.3    46     1818   06 51 00
06 55 30  ---          06 54 00  47.1  12.8 -1.8    -144.7   270     1836   06 51 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

06 56 00  0836+710     06 54 30  47.1  12.7 -1.8    -144.8    24     1836   06 56 00
07 01 00  ---          06 59 31  47.3  12.2 -1.7    -146.4   300     1855   06 56 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

07 01 30  0836+710     07 00 01  47.4  12.2 -1.7    -146.5    24     1855   07 01 30
07 06 00  ---          07 04 32  47.6  11.7 -1.6    -147.9   270     1872   07 01 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

07 11 30  4C39.25      07 10 03  60.7  64.0 -2.3     -95.8   285     1872   07 11 30
07 15 30  ---          07 14 04  61.4  63.8 -2.2     -96.6   240     1888   07 11 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

07 16 00  4C39.25      07 14 34  61.5  63.8 -2.2     -96.7    24     1888   07 16 00
07 20 30  ---          07 19 04  62.4  63.6 -2.1     -97.6   270     1905   07 16 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

07 21 00  4C39.25      07 19 34  62.5  63.6 -2.1     -97.7    24     1905   07 21 00
07 25 30  ---          07 24 05  63.4  63.3 -2.1     -98.7   270     1923   07 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

07 30 30  0716+714     07 29 06  49.3  -0.7  0.1     178.2   247     1923   07 30 30
07 35 00  ---          07 33 37  49.3  -1.2  0.2     176.7   270     1940   07 30 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

07 35 30  0716+714     07 34 07  49.3  -1.3  0.2     176.5    24     1940   07 35 30
07 39 30  ---          07 38 08  49.3  -1.8  0.2     175.2   240     1955   07 35 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

07 40 00  0716+714     07 38 38  49.3  -1.8  0.2     175.1    24     1955   07 40 00
07 44 00  ---          07 42 38  49.2  -2.3  0.3     173.7   240     1971   07 40 01

 ---------- Space segment 05: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

07 45 00  0716+714     07 43 38  49.2  -2.4  0.3     173.4    54     1971   07 45 00
07 54 30  ---          07 53 10  49.1  -3.6  0.5     170.3   570     2008   07 45 01

07 55 00  0716+714     07 53 40  49.1  -3.7  0.5     170.1    24     2008   07 55 00
08 04 30  ---          08 03 12  49.0  -4.8  0.7     167.0   570     2044   07 55 01

08 05 00  0716+714     08 03 42  49.0  -4.9  0.7     166.8    24     2044   08 05 00
08 15 00  ---          08 13 43  48.8  -6.0  0.8     163.6   600     2083   08 05 01

 ---------- Ground segment 05: Q/K/U-band VLBI scans ----------

08 15 30  0716+714     08 14 13  48.7  -6.1  0.8     163.4    24     2083   08 15 30
08 20 00  ---          08 18 44  48.6  -6.6  0.9     161.9   270     2100   08 15 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

08 20 30  0716+714     08 19 14  48.6  -6.7  0.9     161.8    24     2100   08 20 30
08 25 00  ---          08 23 45  48.5  -7.2  1.0     160.3   270     2118   08 20 31

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

08 25 30  0716+714     08 24 15  48.5  -7.3  1.0     160.2    24     2118   08 25 30
08 30 00  ---          08 28 46  48.4  -7.8  1.1     158.7   270     2135   08 25 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

08 31 00  0836+710     08 29 46  49.8   1.7 -0.2    -175.6    45     2135   08 31 00
08 35 30  ---          08 34 17  49.8   1.1 -0.1    -177.1   270     2153   08 31 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

08 36 00  0836+710     08 34 47  49.8   1.0 -0.1    -177.3    24     2153   08 36 00
08 41 00  ---          08 39 48  49.8   0.4 -0.1    -178.9   300     2172   08 36 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

08 41 30  0836+710     08 40 18  49.8   0.3 -0.0    -179.1    24     2172   08 41 30
08 46 00  ---          08 44 48  49.8  -0.2  0.0     179.4   270     2189   08 41 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

08 50 30  4C39.25      08 49 19  78.5  40.9 -0.6    -133.5   207     2189   08 50 30
08 54 30  ---          08 53 20  79.1  38.1 -0.6    -136.9   240     2205   08 50 31

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

08 55 00  4C39.25      08 53 50  79.1  37.7 -0.6    -137.4    24     2205   08 55 00
08 59 00  ---          08 57 51  79.6  34.5 -0.5    -141.2   240     2220   08 55 01

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

08 59 30  4C39.25      08 58 21  79.7  34.1 -0.5    -141.7    24     2220   08 59 30
09 03 30  ---          09 02 21  80.1  30.5 -0.4    -145.8   240     2236   08 59 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

09 07 00  0716+714     09 05 52  47.0 -11.7  1.7     147.0   137     2236   09 07 00
09 11 30  ---          09 10 23  46.8 -12.1  1.8     145.6   270     2253   09 07 01

 Next scan frequencies:  42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
 Next BBC frequencies:     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00

09 12 00  0716+714     09 10 53  46.8 -12.2  1.8     145.5    24     2253   09 12 00
09 16 00  ---          09 14 53  46.6 -12.6  1.9     144.3   240     2269   09 12 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Jan 2015   Day   4 ---

 Next scan frequencies:  15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
 Next BBC frequencies:     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00

09 16 30  0716+714     09 15 23  46.6 -12.6  1.9     144.1    24     2269   09 16 30
09 20 30  ---          09 19 24  46.4 -13.0  1.9     142.9   240     2284   09 16 31

 ---------- Space segment 06: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

09 30 00  0716+714     09 28 56  45.9 -13.9  2.1     140.0   564     2284   09 30 00
09 39 30  ---          09 38 27  45.4 -14.7  2.2     137.2   570     2321   09 30 01

09 40 00  0716+714     09 38 57  45.4 -14.7  2.3     137.0    24     2321   09 40 00
09 49 30  ---          09 48 29  44.8 -15.5  2.4     134.2   570     2357   09 40 01

09 50 00  0716+714     09 48 59  44.8 -15.5  2.4     134.1    24     2357   09 50 00
10 00 00  ---          09 59 01  44.2 -16.3  2.6     131.2   600     2396   09 50 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gl041a_freq.dat:
     v1cm_b3

   Setup group:    3         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  11  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
   BBC fr=     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     735.99    735.99    768.01    768.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  11  12  13  14  15  16  17  18  19  41

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm4.set
   Matching groups in ./gl041a_freq.dat:
     v2cm_d2         Fourth 2cm filter

   Setup group:   34         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14400.00  14400.00  14400.00  14400.00  14400.00  14400.00  14400.00  14400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.4     10.1     10.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  21  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15112.00  15112.00  15112.00  15112.00  15144.00  15144.00  15144.00  15144.00
   BBC fr=     712.00    712.00    712.00    712.00    744.00    744.00    744.00    744.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     711.99    711.99    744.01    744.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  21  22  23  24  25  26  27  28  29  39

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm4.set
   Matching groups in ./gl041a_freq.dat:
     v7mm_c8

   Setup group:   23         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  30  Setup file default.  Used with PCAL = 1MHz
   LO sum=   42928.00  42928.00  42928.00  42928.00  42960.00  42960.00  42960.00  42960.00
   BBC fr=     528.00    528.00    528.00    528.00    560.00    560.00    560.00    560.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     527.99    527.99    560.01    560.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  30  31  32  33  34  35  36  37  38  40

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 42.121174       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 36.86358        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0716+714          07 16 13.029739   * 07 21 53.448474     07 23 39.380491       0.00
   J0721+7120        71 26 15.17406    * 71 20 36.36340      71 18 36.84378        0.00
                     ./gl041a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 42370 observations, RA-AO2-10, RA-AO2-1

 * 0836+710          08 36 21.556646   * 08 41 24.365284     08 42 57.540347       0.00
   J0841+7053        71 04 22.42740    * 70 53 42.17302      70 50 08.09899        0.00
                     ./gl041a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 4321 observations, RA-AO2-12

   0923+392          09 23 55.319218   * 09 27 03.013939     09 28 00.522059       0.00
   J0927+3902        39 15 23.56637    * 39 02 20.85177      38 58 06.90453        0.00
 * 4C39.25           ./gl041a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 245863 observations, RA-AO2-12



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            20                                5.117     0.000
  0716+714   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 11           7.925  1135.156
             ra7mm4.set            30                                0.892    40.125
             ra2cm4.set            21 42                             0.883    40.417
  0836+710   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 11           1.608   126.006
             ra7mm4.set            30                                0.633    26.400
             ra2cm4.set            21                                0.608    25.275
  4C39.25    ra1cm2.set            1 2 3 4 5 6 7 8 9 10 11           0.844    45.953
             ra7mm4.set            30                                0.208     8.775
             ra2cm4.set            21                                0.208     8.775


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             113.9
   0716+714           131.3
   0836+710           129.6
   4C39.25            144.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

