  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN imaging
 Exp. Code:  gl042b  


Schedule Version:       1.10
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Manel Perucho Pla

Address:  Departamento de Astronomia y Astrofisica
          Universidad de Valencia
          E-46100 Burjassot (Valencia), Spain
 

Phone:    +7-903-6614865
EMAIL:    kirx@kirx.net, manel.perucho@uv.es
Fax:      +7-495-3332378
Phone during observation: +7-903-6614865

Observing mode: C/L-band, dual-pol

Notes:    C/L-band, Radioastron-compatible frequency setup
          Mark5C stations should record in Mk5B+ format
          P-CAL is ON, Tsys is ON, auto-level (AGC) is ON
          Please ship data to MPIfR-Bonn

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  20 Jan 2015   Day  20 ---

 ---------- Space Segment 01: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00
 Next scan bandwidths:     16.00    16.00    16.00    16.00

21 00 00  1642+690     22 03 54  31.8 -24.7  5.4      86.6     0        0   21 00 00
21 09 30  ---          22 13 25  30.9 -24.6  5.5      84.4   570       18   21 00 01

21 10 00  1642+690     22 13 56  30.9 -24.6  5.5      84.3    24       18   21 10 00
21 19 30  ---          22 23 27  30.0 -24.5  5.7      82.1   570       37   21 10 01

21 20 00  1642+690     22 23 57  30.0 -24.5  5.7      82.0    24       37   21 20 00
21 29 30  ---          22 33 29  29.1 -24.3  5.9      79.9   570       55   21 20 01

21 30 00  1642+690     22 33 59  29.1 -24.3  5.9      79.8    24       55   21 30 00
21 35 00  ---          22 39 00  28.7 -24.2  5.9      78.7   300       65   21 30 01

 ---------- Space Segment 01: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

21 40 00  1642+690     22 44 00  28.2 -24.1  6.0      77.5   294       65   21 40 00
21 49 30  ---          22 53 32  27.4 -23.9  6.2      75.4   570       83   21 40 01

21 50 00  1642+690     22 54 02  27.3 -23.9  6.2      75.3    24       83   21 50 00
21 59 30  ---          23 03 34  26.5 -23.6  6.4      73.2   570      101   21 50 01

22 00 00  1642+690     23 04 04  26.5 -23.6  6.4      73.1    24      101   22 00 00
22 10 00  ---          23 14 05  25.6 -23.3  6.5      70.9   600      121   22 00 01

 ---------- Ground Segment 01: L-band VLBI scans ----------

22 10 30  1642+690     23 14 35  25.6 -23.3  6.5      70.8    24      121   22 10 30
22 20 00  ---          23 24 07  24.8 -22.9  6.7      68.7   570      139   22 10 31

22 20 30  1642+690     23 24 37  24.7 -22.9  6.7      68.6    24      139   22 20 30
22 30 00  ---          23 34 09  23.9 -22.5  6.9      66.5   570      157   22 20 31

22 30 30  1642+690     23 34 39  23.9 -22.5  6.9      66.4    24      157   22 30 30
22 40 00  ---          23 44 10  23.1 -22.1  7.0      64.3   570      176   22 30 31

22 40 30  1642+690     23 44 40  23.1 -22.1  7.0      64.2    24      176   22 40 30
22 50 00  ---          23 54 12  22.3 -21.7  7.2      62.2   570      194   22 40 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  20 Jan 2015   Day  20 ---

22 50 30  1642+690     23 54 42  22.3 -21.7  7.2      62.1    24      194   22 50 30
23 00 00  ---          00 04 14  21.5 -21.2  7.4      60.0   570      213   22 50 31

 ---------- Ground Segment 01: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

23 05 00  1642+690     00 09 14  21.1 -21.0  7.5      58.9   294      213   23 05 00
23 15 00  ---          00 19 16  20.4 -20.5  7.6      56.8   600      232   23 05 01

23 15 30  1642+690     00 19 46  20.3 -20.4  7.6      56.7    24      232   23 15 30
23 25 00  ---          00 29 18  19.6 -19.9  7.8      54.6   570      250   23 15 31

23 25 30  1642+690     00 29 48  19.6 -19.9  7.8      54.5    24      250   23 25 30
23 35 00  ---          00 39 19  18.9 -19.4  8.0      52.5   570      269   23 25 31

23 35 30  1642+690     00 39 49  18.9 -19.3  8.0      52.4    24      269   23 35 30
23 45 00  ---          00 49 21  18.2 -18.8  8.1      50.3   570      287   23 35 31

23 45 30  1642+690     00 49 51  18.2 -18.7  8.1      50.2    24      287   23 45 30
23 54 30  ---          00 58 53  17.5 -18.2  8.3      48.3   540      304   23 45 31

 ---------- Space Segment 02: C-band VLBI scans ----------

23 55 00  1642+690     00 59 23  17.5 -18.1  8.3      48.2    24      304   23 55 00
23 59 30  ---          01 03 53  17.2 -17.9  8.4      47.2   270      313   23 55 01

 --- Wed  21 Jan 2015   Day  21 ---

00 00 00  1642+690     01 04 23  17.2 -17.8  8.4      47.1    24      313   00 00 00
00 04 30  ---          01 08 54  16.9 -17.5  8.4      46.1   270      322   00 00 01

00 05 00  1642+690     01 09 24  16.8 -17.5  8.5      46.0    24      322   00 05 00
00 14 30  ---          01 18 56  16.2 -16.9  8.6      44.0   570      340   00 05 01

00 15 00  1642+690     01 19 26  16.2 -16.8  8.6      43.9    24      340   00 15 00
00 20 00  ---          01 24 27  15.9 -16.5  8.7      42.8   300      350   00 15 01

 ---------- Space Segment 02: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

00 25 00  1642+690     01 29 28  15.6 -16.2  8.8      41.7   294      350   00 25 00
00 34 30  ---          01 38 59  15.0 -15.5  8.9      39.7   570      368   00 25 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

00 35 00  1642+690     01 39 29  15.0 -15.4  9.0      39.6    24      368   00 35 00
00 44 30  ---          01 49 01  14.5 -14.8  9.1      37.5   570      386   00 35 01

00 45 00  1642+690     01 49 31  14.4 -14.7  9.1      37.4    24      386   00 45 00
00 55 00  ---          01 59 33  13.9 -14.0  9.3      35.2   600      406   00 45 01

 ---------- Ground Segment 02: L-band VLBI scans ----------

00 55 30  1642+690     02 00 03  13.9 -13.9  9.3      35.1    24      406   00 55 30
01 05 00  ---          02 09 34  13.4 -13.2  9.5      33.1   570      424   00 55 31

01 05 30  1642+690     02 10 04  13.4 -13.2  9.5      33.0    24      424   01 05 30
01 15 00  ---          02 19 36  12.9 -12.4  9.6      30.9   570      442   01 05 31

01 15 30  1642+690     02 20 06  12.9 -12.4  9.6      30.8    24      442   01 15 30
01 25 00  ---          02 29 37  12.5 -11.6  9.8      28.8   570      461   01 15 31

01 25 30  1642+690     02 30 08  12.5 -11.6  9.8      28.7    24      461   01 25 30
01 35 00  ---          02 39 39  12.1 -10.8 10.0      26.6   570      479   01 25 31

01 35 30  1642+690     02 40 09  12.0 -10.8 10.0      26.5    24      479   01 35 30
01 45 00  ---          02 49 41  11.7 -10.0 10.1      24.4   570      498   01 35 31

01 45 30  1642+690     02 50 11  11.7  -9.9 10.1      24.3    24      498   01 45 30
01 55 00  ---          02 59 42  11.3  -9.1 10.3      22.3   570      516   01 45 31

01 55 30  1642+690     03 00 12  11.3  -9.1 10.3      22.2    24      516   01 55 30
02 05 00  ---          03 09 44  11.0  -8.3 10.5      20.1   570      534   01 55 31

02 05 30  1642+690     03 10 14  11.0  -8.2 10.5      20.0    24      534   02 05 30
02 10 00  ---          03 14 45  10.8  -7.8 10.5      19.0   270      543   02 05 31

 ---------- Ground Segment 02: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 15 00  1642+690     03 19 46  10.7  -7.4 10.6      17.9   294      543   02 15 00
02 25 00  ---          03 29 47  10.4  -6.5 10.8      15.7   600      562   02 15 01

02 25 30  1642+690     03 30 17  10.4  -6.5 10.8      15.6    24      562   02 25 30
02 35 00  ---          03 39 49  10.2  -5.6 11.0      13.6   570      581   02 25 31

02 35 30  1642+690     03 40 19  10.2  -5.6 11.0      13.4    24      581   02 35 30
02 45 00  ---          03 49 51  10.0  -4.7 11.1      11.4   570      599   02 35 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

02 45 30  1642+690     03 50 21  10.0  -4.7 11.1      11.3    24      599   02 45 30
02 55 00  ---          03 59 52   9.9  -3.8 11.3       9.2   570      617   02 45 31

02 55 30  1642+690     04 00 22   9.8  -3.8 11.3       9.1    24      617   02 55 30
03 05 00  ---          04 09 54   9.7  -2.9 11.5       7.0   570      636   02 55 31

03 05 30  1642+690     04 10 24   9.7  -2.9 11.5       6.9    24      636   03 05 30
03 15 00  ---          04 19 56   9.6  -2.0 11.6       4.8   570      654   03 05 31

03 15 30  1642+690     04 20 26   9.6  -2.0 11.6       4.7    24      654   03 15 30
03 25 00  ---          04 29 57   9.6  -1.1 11.8       2.6   570      672   03 15 31

03 25 30  1642+690     04 30 27   9.6  -1.1 11.8       2.5    24      672   03 25 30
03 29 30  ---          04 34 28   9.6  -0.7 11.9       1.7   240      680   03 25 31

 ---------- Space Segment 03: C-band VLBI scans ----------

03 30 00  1642+690     04 34 58   9.6  -0.6 11.9       1.5    24      680   03 30 00
03 39 30  ---          04 44 30   9.6   0.2-12.0      -0.5   570      699   03 30 01

03 40 00  1642+690     04 45 00   9.6   0.3-12.0      -0.6    24      699   03 40 00
03 45 00  ---          04 50 00   9.6   0.7-11.9      -1.7   300      708   03 40 01

 ---------- Space Segment 03: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

03 50 00  1642+690     04 55 01   9.6   1.2-11.8      -2.8   294      708   03 50 00
03 59 30  ---          05 04 33   9.6   2.1-11.6      -4.9   570      727   03 50 01

04 00 00  1642+690     05 05 03   9.6   2.1-11.6      -5.0    24      727   04 00 00
04 10 00  ---          05 15 05   9.7   3.0-11.4      -7.2   600      746   04 00 01

 ---------- Ground Segment 03: L-band VLBI scans ----------

04 10 30  1642+690     05 15 35   9.7   3.1-11.4      -7.3    24      746   04 10 30
04 20 00  ---          05 25 06   9.9   3.9-11.3      -9.4   570      764   04 10 31

04 20 30  1642+690     05 25 36   9.9   4.0-11.3      -9.5    24      764   04 20 30
04 30 00  ---          05 35 08  10.0   4.8-11.1     -11.6   570      783   04 20 31

04 30 30  1642+690     05 35 38  10.0   4.9-11.1     -11.7    24      783   04 30 30
04 35 00  ---          05 40 09  10.1   5.3-11.0     -12.7   270      791   04 30 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

 ---------- Ground Segment 03: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

04 40 00  1642+690     05 45 09  10.2   5.7-10.9     -13.8   294      791   04 40 00
04 50 00  ---          05 55 11  10.5   6.6-10.8     -15.9   600      811   04 40 01

04 50 30  1642+690     05 55 41  10.5   6.6-10.8     -16.0    24      811   04 50 30
05 00 00  ---          06 05 13  10.7   7.5-10.6     -18.1   570      829   04 50 31

05 00 30  1642+690     06 05 43  10.7   7.5-10.6     -18.2    24      829   05 00 30
05 04 30  ---          06 09 44  10.9   7.9-10.5     -19.1   240      837   05 00 31

 ---------- Space Segment 04: C-band VLBI scans ----------

05 05 00  1642+690     06 10 14  10.9   7.9-10.5     -19.2    24      837   05 05 00
05 14 30  ---          06 19 45  11.2   8.7-10.4     -21.3   570      855   05 05 01

05 15 00  1642+690     06 20 15  11.2   8.8-10.4     -21.4    24      855   05 15 00
05 20 00  ---          06 25 16  11.3   9.2-10.3     -22.5   300      865   05 15 01

 ---------- Space Segment 04: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

05 25 00  1642+690     06 30 17  11.5   9.6-10.2     -23.5   294      865   05 25 00
05 34 30  ---          06 39 48  11.9  10.4-10.0     -25.6   570      883   05 25 01

05 35 00  1642+690     06 40 19  11.9  10.5-10.0     -25.7    24      883   05 35 00
05 45 00  ---          06 50 20  12.3  11.3 -9.9     -27.9   600      902   05 35 01

 ---------- Ground Segment 04: L-band VLBI scans ----------

05 45 30  1642+690     06 50 50  12.3  11.3 -9.9     -28.0    24      902   05 45 30
05 55 00  ---          07 00 22  12.7  12.1 -9.7     -30.0   570      921   05 45 31

05 55 30  1642+690     07 00 52  12.8  12.1 -9.7     -30.2    24      921   05 55 30
06 05 00  ---          07 10 23  13.2  12.9 -9.5     -32.2   570      939   05 55 31

06 05 30  1642+690     07 10 54  13.2  12.9 -9.5     -32.3    24      939   06 05 30
06 15 00  ---          07 20 25  13.7  13.7 -9.4     -34.4   570      957   06 05 31

06 15 30  1642+690     07 20 55  13.7  13.7 -9.4     -34.5    24      957   06 15 30
06 20 00  ---          07 25 26  14.0  14.0 -9.3     -35.4   270      966   06 15 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

 ---------- Ground Segment 04: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

06 25 00  1642+690     07 30 27  14.2  14.4 -9.2     -36.5   294      966   06 25 00
06 35 00  ---          07 40 28  14.8  15.1 -9.0     -38.7   600      985   06 25 01

06 35 30  1642+690     07 40 58  14.8  15.2 -9.0     -38.8    24      985   06 35 30
06 45 00  ---          07 50 30  15.4  15.9 -8.9     -40.8   570     1004   06 35 31

06 45 30  1642+690     07 51 00  15.4  15.9 -8.9     -40.9    24     1004   06 45 30
06 54 30  ---          08 00 02  15.9  16.5 -8.7     -42.9   540     1021   06 45 31

 ---------- Space Segment 05: C-band VLBI scans ----------

06 55 00  1642+690     08 00 32  16.0  16.6 -8.7     -43.0    24     1021   06 55 00
07 04 30  ---          08 10 03  16.6  17.2 -8.5     -45.0   570     1040   06 55 01

07 05 00  1642+690     08 10 33  16.6  17.2 -8.5     -45.1    24     1040   07 05 00
07 10 00  ---          08 15 34  16.9  17.6 -8.4     -46.2   300     1049   07 05 01

 ---------- Space Segment 05: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

07 15 00  1642+690     08 20 35  17.2  17.9 -8.4     -47.3   294     1049   07 15 00
07 24 30  ---          08 30 07  17.9  18.5 -8.2     -49.3   570     1068   07 15 01

07 25 00  1642+690     08 30 37  17.9  18.5 -8.2     -49.4    24     1068   07 25 00
07 35 00  ---          08 40 38  18.6  19.1 -8.0     -51.6   600     1087   07 25 01

 ---------- Ground Segment 05: L-band VLBI scans ----------

07 35 30  1642+690     08 41 08  18.6  19.2 -8.0     -51.7    24     1087   07 35 30
07 45 00  ---          08 50 40  19.3  19.7 -7.9     -53.7   570     1105   07 35 31

07 45 30  1642+690     08 51 10  19.4  19.7 -7.8     -53.8    24     1105   07 45 30
07 55 00  ---          09 00 42  20.1  20.3 -7.7     -55.9   570     1124   07 45 31

07 55 30  1642+690     09 01 12  20.1  20.3 -7.7     -56.0    24     1124   07 55 30
08 05 00  ---          09 10 43  20.8  20.8 -7.5     -58.0   570     1142   07 55 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

 ---------- Ground Segment 05: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

08 10 00  1642+690     09 15 44  21.2  21.0 -7.4     -59.1   294     1142   08 10 00
08 20 00  ---          09 25 46  22.0  21.5 -7.3     -61.3   600     1161   08 10 01

08 20 30  1642+690     09 26 16  22.0  21.5 -7.3     -61.4    24     1161   08 20 30
08 30 00  ---          09 35 47  22.8  22.0 -7.1     -63.4   570     1180   08 20 31

08 30 30  1642+690     09 36 17  22.8  22.0 -7.1     -63.6    24     1180   08 30 30
08 39 30  ---          09 45 19  23.6  22.4 -6.9     -65.5   540     1197   08 30 31

 ---------- Space Segment 06: C-band VLBI scans ----------

08 40 00  1642+690     09 45 49  23.6  22.4 -6.9     -65.6    24     1197   08 40 00
08 49 30  ---          09 55 20  24.4  22.8 -6.8     -67.7   570     1215   08 40 01

 ---------- Space Segment 06: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

08 55 00  1642+690     10 00 51  24.8  23.0 -6.7     -68.9   324     1215   08 55 00
08 59 30  ---          10 05 22  25.2  23.1 -6.6     -69.9   270     1224   08 55 01

09 00 00  1642+690     10 05 52  25.3  23.1 -6.6     -70.0    24     1224   09 00 00
09 10 00  ---          10 15 54  26.1  23.5 -6.4     -72.2   600     1243   09 00 01

 ---------- Ground Segment 06: L-band VLBI scans ----------

09 10 30  1642+690     10 16 24  26.2  23.5 -6.4     -72.3    24     1243   09 10 30
09 20 00  ---          10 25 55  27.0  23.7 -6.3     -74.4   570     1262   09 10 31

09 20 30  1642+690     10 26 26  27.0  23.8 -6.3     -74.5    24     1262   09 20 30
09 30 00  ---          10 35 57  27.9  24.0 -6.1     -76.6   570     1280   09 20 31

09 30 30  1642+690     10 36 27  27.9  24.0 -6.1     -76.7    24     1280   09 30 30
09 40 00  ---          10 45 59  28.7  24.2 -5.9     -78.9   570     1298   09 30 31

09 40 30  1642+690     10 46 29  28.8  24.2 -5.9     -79.0    24     1298   09 40 30
09 50 00  ---          10 56 00  29.6  24.4 -5.8     -81.1   570     1317   09 40 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  21 Jan 2015   Day  21 ---

 ---------- Ground Segment 06: C-band VLBI scans ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

09 55 00  1642+690     11 01 01  30.1  24.5 -5.7     -82.2   294     1317   09 55 00
10 05 00  ---          11 11 03  31.0  24.6 -5.5     -84.5   600     1336   09 55 01

10 05 30  1642+690     11 11 33  31.0  24.6 -5.5     -84.6    24     1336   10 05 30
10 15 00  ---          11 21 05  31.9  24.7 -5.3     -86.8   570     1355   10 05 31

10 15 30  1642+690     11 21 35  31.9  24.7 -5.3     -86.9    24     1355   10 15 30
10 25 00  ---          11 31 06  32.8  24.7 -5.2     -89.1   570     1373   10 15 31

10 25 30  1642+690     11 31 36  32.8  24.7 -5.2     -89.2    24     1373   10 25 30
10 29 30  ---          11 35 37  33.2  24.7 -5.1     -90.2   240     1381   10 25 31

 ---------- Space Segment 07: C-band VLBI scans ----------

10 30 00  1642+690     11 36 07  33.2  24.7 -5.1     -90.3    24     1381   10 30 00
10 39 30  ---          11 45 39  34.1  24.7 -4.9     -92.5   570     1399   10 30 01

 ---------- Space Segment 07: L-band VLBI scans ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    932.00   932.00   932.00   932.00

10 45 00  1642+690     11 51 09  34.6  24.7 -4.8     -93.8   324     1399   10 45 00
10 49 30  ---          11 55 40  35.0  24.6 -4.8     -94.9   270     1408   10 45 01

10 50 00  1642+690     11 56 10  35.0  24.6 -4.8     -95.0    24     1408   10 50 00
11 00 00  ---          12 06 12  35.9  24.5 -4.6     -97.4   600     1427   10 50 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra6cm2.set
   Matching groups in ./gl042b_freq.dat:
     vc_d

   Setup group:   20         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.1      4.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  16  Setup file default.  Used with PCAL = 1MHz
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     736.01    736.01    735.99    735.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  16  17  18  19  20  21  22  23  24  25

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra18cm2.set
   Matching groups in ./gl042b_freq.dat:
     v20cm_2         Beware RFI at high end.

   Setup group:    2         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2600.00   2600.00   2600.00   2600.00
   Net SB=         L         L         U         U
   IF SB =         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         L         L
   IF    =        A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.6     15.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  27  Setup file default.  Used with PCAL = 1MHz
   LO sum=   1668.00  1668.00  1668.00  1668.00
   BBC fr=    932.00   932.00   932.00   932.00
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     931.99    931.99    932.01    932.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  27  28  29  30  31  32  33  34  35  36

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 46.490840       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 37.80091        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 1642+690          16 42 18.064877   * 16 42 07.848507     16 42 01.818607       0.00
   J1642+6856        69 02 13.21708    * 68 56 39.75636      68 54 51.61784        0.00
                     ./gl042b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 18956 observations, RA-AO2-11, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra6cm2.set            37                                4.958     0.000
  1642+690   ra18cm2.set           1 9 10 11 12 13 14 26 27         19.300   484.550
             ra6cm2.set            2 3 4 5 7 8 15 16                18.708   488.333

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 50.098626       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 42.65523        0.00
 * 3C286             ./gl042b_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             112.7
   3C286              108.3
   1642+690            96.5

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

