  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The anomalous equatorial emission region of SS433
 Exp. Code:  GP025C  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 28 April 2000                      

PI:       Zsolt Paragi                                                    

Address:  FOMI Satellite Geodetic Observatory                             
          P. O. Box 546                                                   
          H-1373 Budapest                                                 
          HUNGARY                                                         

Phone:    36 27 374 980                                                   
EMAIL:    paragi@sgo.fomi.hu                                              
Fax:      36 27 374 982                                                   
Phone during observation: 36 27 374 980                                   

Observing mode: Continuum 18 cm; Recording mode: 128-4-2 (VLBA/MKIV).     

Notes:    Global VLBI monitoring at 18cm. Observe RCP+LCP, but we         
          do not need crosspol. Fringe-finders: OQ208, 3C454.3            
          Send logs and calibration information to Zsolt Paragi.          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

 Next scan frequencies:  1654.99  1654.99  1662.99  1662.99
 Next BBC frequencies:    745.01   745.01   737.01   737.01
 Next scan bandwidths:      8.00     8.00     8.00     8.00

04 17 33  J1907+0127   13 45 51   9.0  93.7 -5.4     -59.2     0   1  1      0  04 17 13
04 18 13  ---          13 46 31   9.2  93.8 -5.3     -59.2    40   F  1    400

04 18 43  SS433        13 47 01  10.1  90.2 -5.4     -59.7    25   1  1    400  04 18 13
04 19 43  ---          13 48 01  10.3  90.3 -5.4     -59.7    60   F  1    997

04 19 59  1910+052     13 48 18  10.3  89.9 -5.4     -59.8    14   1  1    997  04 19 43
04 20 59  ---          13 49 18  10.5  90.0 -5.4     -59.8    60   F  1   1507

04 21 31  J1907+0127   13 49 49   9.9  94.2 -5.3     -59.1    27   1  1   1507  04 20 59
04 22 31  ---          13 50 50  10.1  94.3 -5.3     -59.1    60   F  1   2118

04 23 00  SS433        13 51 19  11.0  90.7 -5.3     -59.7    25   1  1   2118  04 22 31
04 24 00  ---          13 52 19  11.2  90.8 -5.3     -59.7    60   F  1   2715

04 24 17  1910+052     13 52 36  11.2  90.5 -5.3     -59.8    14   1  1   2715  04 24 00
04 25 17  ---          13 53 36  11.4  90.6 -5.3     -59.8    60   F  1   3225

04 25 48  J1907+0127   13 54 08  10.8  94.8 -5.2     -59.1    27   1  1   3225  04 25 17
04 26 48  ---          13 55 08  11.0  94.9 -5.2     -59.0    60   F  1   3835

04 27 18  SS433        13 55 37  11.9  91.3 -5.3     -59.7    25   1  1   3835  04 26 48
04 28 18  ---          13 56 38  12.2  91.4 -5.3     -59.7    60   F  1   4432

04 28 34  1910+052     13 56 54  12.1  91.0 -5.3     -59.8    14   1  1   4432  04 28 18
04 29 34  ---          13 57 54  12.4  91.1 -5.3     -59.8    60   F  1   4942

04 30 06  J1907+0127   13 58 26  11.7  95.3 -5.1     -59.0    27   1  1   4942  04 29 34
04 31 06  ---          13 59 26  12.0  95.5 -5.1     -59.0    60   F  1   5553

04 31 35  SS433        13 59 56  12.9  91.8 -5.2     -59.7    25   1  1   5553  04 31 06
04 32 35  ---          14 00 56  13.1  92.0 -5.2     -59.7    60   F  1   6150

04 32 52  1910+052     14 01 12  13.1  91.6 -5.2     -59.7    14   1  1   6150  04 32 35
04 33 52  ---          14 02 13  13.3  91.7 -5.2     -59.7    60   F  1   6660

04 34 24  J1907+0127   14 02 44  12.7  95.9 -5.1     -58.9    27   1  1   6660  04 33 52
04 35 24  ---          14 03 44  12.9  96.0 -5.1     -58.9    60   F  1   7270
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

04 35 53  SS433        14 04 14  13.8  92.4 -5.1     -59.6    25   1  1   7270  04 35 24
04 58 53  ---          14 27 18  18.7  95.4 -4.7     -59.3  1380   F  1  16667

05 00 53  SS433        14 29 18  19.2  95.7 -4.7     -59.3   117   1  2  16667  05 00 33
05 11 33  ---          14 40 00  21.5  97.1 -4.5     -59.0   640   R  1  14133

05 26 17  J1907+0127   14 54 47  23.7 103.2 -4.2     -56.9   878   1  2  14133  05 25 57
05 26 57  ---          14 55 27  23.8 103.3 -4.2     -56.9    40   R  1  13733

05 27 26  SS433        14 55 56  24.9  99.4 -4.3     -58.4    25   1  2  13733  05 26 57
05 28 26  ---          14 56 56  25.1  99.5 -4.2     -58.4    60   R  1  13139

05 28 43  1910+052     14 57 13  25.1  99.1 -4.3     -58.6    14   1  2  13139  05 28 26
05 29 43  ---          14 58 13  25.3  99.3 -4.2     -58.5    60   R  1  12629

05 30 14  J1907+0127   14 58 44  24.5 103.8 -4.1     -56.7    26   1  2  12629  05 29 43
05 31 14  ---          14 59 44  24.7 103.9 -4.1     -56.7    60   R  1  12020

05 31 43  SS433        15 00 14  25.8 100.0 -4.2     -58.3    25   1  2  12020  05 31 14
05 32 43  ---          15 01 14  26.0 100.2 -4.2     -58.2    60   R  1  11426

05 33 00  1910+052     15 01 30  26.0  99.7 -4.2     -58.4    14   1  2  11426  05 32 43
05 34 00  ---          15 02 31  26.2  99.9 -4.2     -58.4    60   R  1  10916

05 34 31  J1907+0127   15 03 02  25.4 104.4 -4.1     -56.5    26   1  2  10916  05 34 00
05 35 31  ---          15 04 02  25.6 104.6 -4.1     -56.4    60   R  1  10307

05 36 00  SS433        15 04 31  26.7 100.6 -4.1     -58.1    24   1  2  10307  05 35 31
05 37 00  ---          15 05 31  26.9 100.8 -4.1     -58.0    60   R  1   9713

05 37 17  1910+052     15 05 48  26.9 100.4 -4.1     -58.2    14   1  2   9713  05 37 00
05 38 17  ---          15 06 48  27.1 100.5 -4.1     -58.2    60   R  1   9203

05 38 48  J1907+0127   15 07 19  26.3 105.1 -4.0     -56.2    26   1  2   9203  05 38 17
05 39 48  ---          15 08 20  26.5 105.2 -4.0     -56.1    60   R  1   8595

05 40 17  SS433        15 08 49  27.6 101.3 -4.1     -57.9    24   1  2   8595  05 39 48
05 41 17  ---          15 09 49  27.8 101.4 -4.0     -57.8    60   R  1   8001

05 41 34  1910+052     15 10 06  27.8 101.0 -4.0     -58.0    14   1  2   8001  05 41 17
05 42 34  ---          15 11 06  28.0 101.1 -4.0     -58.0    60   R  1   7491
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

05 43 05  J1907+0127   15 11 37  27.2 105.7 -3.9     -55.9    26   1  2   7491  05 42 34
05 44 05  ---          15 12 37  27.4 105.9 -3.9     -55.9    60   R  1   6883

05 46 05  SS433        15 14 38  28.8 102.1 -4.0     -57.6   115   1  3   6883  05 45 45
06 19 45  ---          15 48 23  35.8 107.6 -3.4     -55.4  2020   F  1   6717

06 22 45  SS433        15 51 24  36.4 108.2 -3.3     -55.2   177   1  4   6717  06 22 25
07 06 25  ---          16 35 11  45.1 116.9 -2.6     -50.4  2620   R  1  10883

07 09 25  SS433        16 38 11  45.7 117.6 -2.6     -50.0   177   1  4  10883  07 09 05
07 31 05  ---          16 59 55  49.8 122.9 -2.2     -46.5  1300   R  1   2083

07 33 05  J2101+0341   17 01 55  27.6 103.0 -4.0     -57.2    74   1  5   2083  07 32 45
07 38 15  =2059+034    17 07 06  28.7 103.8 -3.9     -56.9   310   F  1    117

07 39 02  J2025+0316   17 07 53  36.1 110.5 -3.3     -53.9    30   1  5    117  07 38 15
07 43 52  =2022+031    17 12 44  37.1 111.3 -3.2     -53.4   290   F  1   2366

07 46 52  J1907+0127   17 15 45  50.7 132.5 -1.9     -39.4   151   1  5   2366  07 46 32
07 47 32  ---          17 16 25  50.8 132.7 -1.8     -39.2    40   F  1   2766

07 47 41  SS433        17 16 34  52.7 127.6 -1.9     -43.2     3   1  5   2766  07 47 32
07 48 41  ---          17 17 34  52.9 127.9 -1.9     -43.0    60   F  1   3227

07 48 44  1910+052     17 17 37  52.9 127.2 -1.9     -43.5     0   1  5   3227  07 48 41
07 49 44  ---          17 18 37  53.1 127.5 -1.9     -43.2    60   F  1   3646

07 49 54  J1907+0127   17 18 47  51.1 133.5 -1.8     -38.7     4   1  5   3646  07 49 44
07 50 54  ---          17 19 47  51.3 133.8 -1.8     -38.4    60   F  1   4112

07 51 03  SS433        17 19 56  53.3 128.6 -1.9     -42.4     3   1  5   4112  07 50 54
07 52 03  ---          17 20 57  53.4 128.9 -1.8     -42.2    60   F  1   4574

07 52 06  1910+052     17 20 59  53.5 128.3 -1.9     -42.7     0   1  5   4574  07 52 03
07 53 06  ---          17 22 00  53.6 128.6 -1.8     -42.5    60   F  1   4992

07 53 16  J1907+0127   17 22 10  51.7 134.5 -1.8     -37.9     4   1  5   4992  07 53 06
07 54 16  ---          17 23 10  51.8 134.8 -1.7     -37.6    60   F  1   5459

07 54 25  SS433        17 23 19  53.8 129.7 -1.8     -41.7     3   1  5   5459  07 54 16
07 55 25  ---          17 24 19  54.0 130.0 -1.8     -41.4    60   F  1   5920
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

07 55 28  1910+052     17 24 22  54.0 129.3 -1.8     -42.0     0   1  5   5920  07 55 25
07 56 28  ---          17 25 22  54.2 129.6 -1.8     -41.7    60   F  1   6339

07 56 38  J1907+0127   17 25 32  52.2 135.6 -1.7     -37.0     4   1  5   6339  07 56 28
07 57 38  ---          17 26 32  52.3 135.9 -1.7     -36.8    60   F  1   6806

07 57 47  SS433        17 26 42  54.4 130.8 -1.8     -40.9     3   1  5   6806  07 57 38
07 58 47  ---          17 27 42  54.5 131.1 -1.7     -40.6    60   F  1   7267

07 58 50  1910+052     17 27 45  54.6 130.4 -1.8     -41.2     0   1  5   7267  07 58 47
07 59 50  ---          17 28 45  54.8 130.7 -1.7     -40.9    60   F  1   7686

08 00 00  J1907+0127   17 28 55  52.7 136.7 -1.6     -36.2     4   1  5   7686  07 59 50
08 01 00  ---          17 29 55  52.8 137.0 -1.6     -35.9    60   F  1   8153

08 02 00  SS433        17 30 55  55.1 132.2 -1.7     -39.8    54   1  6   8153  08 01 00
08 34 40  ---          18 03 41  59.7 144.6 -1.1     -30.0  1960   R  1  13580

08 37 40  SS433        18 06 41  60.1 145.9 -1.1     -29.0   177   1  7  13580  08 37 20
09 21 20  ---          18 50 28  63.9 167.8 -0.4     -10.5  2620   F  1   4020

09 24 20  J1907+0127   18 53 29  60.6 173.0 -0.2      -6.0   172   1  7   4020  09 24 00
09 25 00  ---          18 54 09  60.7 173.3 -0.2      -5.7    40   F  1   4420

09 25 10  SS433        18 54 18  64.0 170.0 -0.3      -8.6     1   1  7   4420  09 25 00
09 26 10  ---          18 55 18  64.1 170.5 -0.3      -8.2    60   F  1   4882

09 26 12  1910+052     18 55 21  64.3 169.9 -0.3      -8.8     0   1  7   4882  09 26 10
09 27 12  ---          18 56 21  64.4 170.4 -0.3      -8.3    60   F  1   5301

09 27 23  J1907+0127   18 56 32  60.7 174.5 -0.2      -4.7     1   1  7   5301  09 27 12
09 28 23  ---          18 57 32  60.7 175.0 -0.2      -4.3    60   F  1   5768

09 28 32  SS433        18 57 41  64.1 171.9 -0.2      -7.0     1   1  7   5768  09 28 23
09 29 32  ---          18 58 41  64.2 172.5 -0.2      -6.5    60   F  1   6231

09 29 35  1910+052     18 58 44  64.4 171.8 -0.2      -7.1     0   1  7   6231  09 29 32
09 30 35  ---          18 59 44  64.5 172.4 -0.2      -6.6    60   F  1   6649

09 30 45  J1907+0127   18 59 54  60.8 176.3 -0.1      -3.2     1   1  7   6649  09 30 35
09 31 45  ---          19 00 55  60.8 176.8 -0.1      -2.8    60   F  1   7117
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

09 31 54  SS433        19 01 04  64.2 173.8 -0.2      -5.3     0   1  7   7117  09 31 45
09 32 54  ---          19 02 04  64.2 174.4 -0.2      -4.8    60   F  1   7580

09 32 57  1910+052     19 02 07  64.5 173.7 -0.2      -5.4     0   1  7   7580  09 32 54
09 33 57  ---          19 03 07  64.6 174.3 -0.2      -4.9    60   F  1   7998

09 34 07  J1907+0127   19 03 17  60.8 178.0 -0.1      -1.7     1   1  7   7998  09 33 57
09 35 07  ---          19 04 17  60.8 178.5  0.0      -1.3    60   F  1   8466

09 35 17  SS433        19 04 27  64.3 175.7 -0.1      -3.7     0   1  7   8466  09 35 07
09 36 17  ---          19 05 27  64.3 176.3 -0.1      -3.2    60   F  1   8928

09 36 19  1910+052     19 05 30  64.6 175.7 -0.1      -3.7     0   1  7   8928  09 36 17
09 37 19  ---          19 06 30  64.6 176.3 -0.1      -3.2    60   F  1   9347

09 37 30  J1907+0127   19 06 40  60.8 179.7  0.0      -0.2     1   1  7   9347  09 37 19
09 38 30  ---          19 07 40  60.8 180.2  0.0       0.2    60   F  1   9815

09 38 39  SS433        19 07 50  64.3 177.7 -0.1      -2.0     0   1  8   9815  09 38 30
10 00 19  ---          19 29 33  64.0 190.1  0.3       8.7  1300   R  1  16656

10 03 19  SS433        19 32 34  63.9 191.8  0.3      10.2   177   1  9  16656  10 02 59
10 46 59  ---          20 16 21  60.2 213.8  1.1      28.7  2620   F  1    944

10 48 59  J2101+0341   20 18 21  61.2 157.1 -0.7     -19.6    80   1  9    944  10 48 39
10 54 09  =2059+034    20 23 32  61.6 159.7 -0.6     -17.4   310   F  1   3144

10 54 28  J2025+0316   20 23 51  62.6 179.3  0.0      -0.6     4   1  9   3144  10 54 09
10 59 18  =2022+031    20 28 42  62.6 181.9  0.1       1.6   290   F  1   5204

11 02 18  J1907+0127   20 31 42  54.6 218.5  1.4      32.4   154   1  9   5204  11 01 58
11 02 58  ---          20 32 22  54.5 218.7  1.4      32.6    40   F  1   5604

11 03 07  SS433        20 32 32  58.1 220.5  1.3      34.1     0   1  9   5604  11 02 58
11 04 07  ---          20 33 32  57.9 220.9  1.4      34.5    60   F  1   6066

11 04 10  1910+052     20 33 35  58.4 220.9  1.3      34.4     0   1  9   6066  11 04 07
11 05 10  ---          20 34 35  58.2 221.3  1.4      34.7    60   F  1   6485

11 05 20  J1907+0127   20 34 45  54.2 219.6  1.5      33.2     0   1  9   6485  11 05 10
11 06 20  ---          20 35 45  54.1 219.9  1.5      33.5    60   F  1   6953
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

11 06 30  SS433        20 35 55  57.6 221.8  1.4      35.2     0   1  9   6953  11 06 20
11 07 30  ---          20 36 55  57.5 222.2  1.4      35.5    60   F  1   7416

11 07 32  1910+052     20 36 58  57.9 222.2  1.4      35.5     0   1  9   7416  11 07 30
11 08 32  ---          20 37 58  57.7 222.5  1.4      35.8    60   F  1   7834

11 08 43  J1907+0127   20 38 08  53.7 220.8  1.5      34.2     0   1  9   7834  11 08 32
11 09 43  ---          20 39 08  53.6 221.1  1.5      34.5    60   F  1   8303

11 09 52  SS433        20 39 18  57.1 223.1  1.5      36.2     0   1  9   8303  11 09 43
11 10 52  ---          20 40 18  57.0 223.5  1.5      36.5    60   F  1   8765

11 10 55  1910+052     20 40 21  57.4 223.4  1.5      36.5     0   1  9   8765  11 10 52
11 11 55  ---          20 41 21  57.2 223.8  1.5      36.7    60   F  1   9184

11 12 05  J1907+0127   20 41 31  53.3 221.9  1.6      35.1     0   1  9   9184  11 11 55
11 13 05  ---          20 42 31  53.1 222.3  1.6      35.4    60   F  1   9652

11 13 14  SS433        20 42 41  56.6 224.3  1.5      37.1     0   1  9   9652  11 13 05
11 14 14  ---          20 43 41  56.5 224.7  1.5      37.4    60   F  1  10114

11 14 17  1910+052     20 43 44  56.9 224.7  1.5      37.4     0   1  9  10114  11 14 14
11 15 17  ---          20 44 44  56.7 225.0  1.5      37.7    60   F  1  10533

11 15 27  J1907+0127   20 44 54  52.8 223.1  1.6      36.0     0   1  9  10533  11 15 17
11 16 27  ---          20 45 54  52.6 223.4  1.6      36.3    60   F  1  11001

11 16 37  SS433        20 46 04  56.1 225.5  1.6      38.1     0   1  9  11001  11 16 27
11 27 17  ---          20 56 45  54.4 229.2  1.7      40.8   640   F  1  15330

11 30 17  SS433        20 59 46  53.9 230.1  1.8      41.5   177   1 10  15330  11 29 57
12 13 57  ---          21 43 33  46.1 242.0  2.5      49.7  2620   R  1   2270

12 16 57  SS433        21 46 34  45.5 242.7  2.6      50.1   177   1 11   2270  12 16 37
13 00 37  ---          22 30 21  36.8 251.5  3.3      55.0  2620   F  1  15330

13 03 37  SS433        22 33 21  36.2 252.0  3.4      55.2   177   1 12  15330  13 03 17
13 36 17  ---          23 06 07  29.4 257.4  3.9      57.4  1960   R  1   6670

13 36 19  SS433        23 06 09  29.4 257.4  3.9      57.4     0   1 12   6670  13 36 17
13 46 59  ---          23 16 50  27.2 259.0  4.1      58.0   640   R  1   2390
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The anomalous equatorial emission region of SS433
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  28 May 2000   Day 149 ---

13 47 56  J2101+0341   23 17 48  48.1 236.8  2.3      46.2    13   1 13   2390  13 46 59
13 53 26  =2059+034    23 23 19  47.1 238.2  2.4      47.1   330   F  1    191

13 54 27  3C454.3      23 24 20  73.9 207.3  0.5      24.3     5   1 13    191  13 53 26
13 59 57  ---          23 29 51  73.4 211.5  0.6      27.9   330   F  1   2799


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v18cm-128-4-2.set
   Matches group v20cm_2 in /vlbi/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    8         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=  2400.00  2400.00  2400.00  2400.00
   Net SB=        U        U        U        U
   Pol.  =     RCP      LCP      RCP      LCP 
   BBC   =        1        2        3        4
   BBC SB=        L        L        L        L
   IF    =       A        C        A        C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   8  Setup file default.  Used pcal sets:   1
   LO sum=   1654.99  1654.99  1662.99  1662.99
   BBC fr=    745.01   745.01   737.01   737.01
   Bandwd=     8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=    10    10  6010  6010     0     0     0     0
    PCALFR2=    10    10  6010  6010     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- The anomalous equatorial emission region of SS433
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SS433             19 09 21.270093   * 19 11 49.555000     19 11 50.822732 
                     04 53 53.11612    * 04 58 56.94900      04 58 57.36735 
                     From catalog imbedded in main SCHED input file.

 * J1907+0127        19 04 39.789145   * 19 07 11.996900     19 07 13.278556 
                     01 22 24.61197    * 01 27 08.97400      01 27 10.17349 
                     From catalog imbedded in main SCHED input file.

 * 1910+052          19 10 26.308007   * 19 12 54.247000     19 12 55.511280 
                     05 12 51.18616    * 05 17 59.52000      05 17 59.86322 
                     From catalog imbedded in main SCHED input file.

   J1407+2827        14 04 45.615152   * 14 07 00.394411     14 07 01.690587 
 * 1404+286          28 41 29.23491    * 28 27 14.68994      28 27 18.47054 
   J1407+28          /vlbi/sched/catalogs/sources.vlba
   OQ208             USNO - Ref Frame 1998-6, Eubanks June 1998

 * J2025+0316        20 22 38.865422   * 20 25 09.631300     20 25 10.581725 
 + 2022+031          03 06 55.77275    * 03 16 44.49300      03 16 44.84923 
   J2025+03          /vlbi/sched/catalogs/sources.vlba
                     JVAS - Browne et al. 1998, mnras, 293, 257;    S8.4GHz=   406 mJy

 * J2101+0341        20 59 08.011544   * 21 01 38.834164     21 01 39.599826 
 + 2059+034          03 29 41.48334    * 03 41 31.32060      03 41 31.18902 
   J2101+03          /vlbi/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998

   J2253+1608        22 51 29.520100   * 22 53 57.748300     22 53 57.934083 
   2251+158          15 52 54.35016    * 16 08 53.56300      16 08 47.73213 
 * 3C454.3           /vlbi/sched/catalogs/sources.vlba
   J2253+16          JVAS - Browne et al. 1998, mnras, 293, 257;    S8.4GHz= 10503 mJy



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SS433              130.6
   J1907+0127         133.5
   1910+052           130.2
   1404+286           120.4
   J2025+0316         115.5
   2022+031           115.5
   J2101+0341         107.1
   2059+034           107.1
   3C454.3             76.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

