  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Phase-referencing of B1152+199
 Exp. Code:  GA036   


Schedule Version:       3.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Saghar Asadi

Address:  Stockholm University
          Department of Astronomy
          106 91 Stockholm
          Sweden

Phone:    +46855378502
EMAIL:    saghar.asadi@astro.su.se
Fax:      N/A
Phone during observation: +46706755341

Observing mode: Phase-referencing of B1152+199 at 3.6cm (1 Gb/s)

Notes:    Schedule by Eskil Varenius, varenius@chalmers.se
          Obsphone above goes to Eskil.
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

 Next scan frequencies:  8351.25  8351.25  8383.25  8383.25  8415.25  8415.25  8447.25  8447.25
 Next BBC frequencies:    751.25   751.25   783.25   783.25   815.25   815.25   847.25   847.25
 Next scan bandwidths:     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00

20 06 22  J1158+1821   05 46 36   6.6  72.6 -6.2     -59.9     0        0   20 06 22
20 07 12  ---          05 47 36   6.8  72.8 -6.2     -59.9    50        6   20 06 23

20 07 41  B1152+199    05 47 56   8.2  72.0 -6.1     -60.3    19        6   20 07 41
20 11 41  ---          05 51 56   9.0  72.5 -6.1     -60.6   240       37   20 07 42

20 12 20  J1158+1821   05 52 35   7.8  73.4 -6.1     -60.3    28       37   20 12 20
20 13 10  ---          05 53 35   8.0  73.5 -6.1     -60.3    50       44   20 12 21

20 13 39  B1152+199    05 53 54   9.4  72.7 -6.0     -60.7    19       44   20 13 39
20 17 39  ---          05 57 55  10.2  73.2 -6.0     -61.0   240       75   20 13 40

20 18 18  J1158+1821   05 58 34   9.1  74.1 -6.0     -60.6    28       75   20 18 18
20 19 08  ---          05 59 34   9.3  74.2 -6.0     -60.7    50       81   20 18 19

20 19 37  B1152+199    05 59 53  10.6  73.4 -5.9     -61.1    19       81   20 19 37
20 23 37  ---          06 03 54  11.4  73.9 -5.9     -61.3   240      112   20 19 38

20 24 16  J1158+1821   06 04 32  10.3  74.8 -5.9     -61.0    28      112   20 24 16
20 25 06  ---          06 05 33  10.5  74.9 -5.9     -61.0    50      119   20 24 17

20 25 35  B1152+199    06 05 52  11.8  74.1 -5.8     -61.4    19      119   20 25 35
20 29 35  ---          06 09 53  12.7  74.6 -5.8     -61.7   240      149   20 25 36

20 30 04  J1158+1821   06 10 21  11.5  75.4 -5.8     -61.3    18      149   20 30 04
20 31 04  ---          06 11 21  11.7  75.6 -5.8     -61.3    60      157   20 30 05

20 32 02  J1224+2122   06 12 20   8.0  69.9 -6.2     -60.1    43      157   20 32 02
20 33 52  ---          06 14 20   8.4  70.1 -6.2     -60.3   110      171   20 32 03

20 34 42  J1158+1821   06 15 01  12.5  76.0 -5.7     -61.5    35      171   20 34 42
20 35 32  ---          06 16 01  12.7  76.1 -5.7     -61.6    50      178   20 34 43

20 36 01  B1152+199    06 16 20  14.0  75.3 -5.7     -62.1    18      178   20 36 01
20 40 01  ---          06 20 20  14.9  75.8 -5.6     -62.3   240      209   20 36 02

20 40 39  J1158+1821   06 20 59  13.7  76.7 -5.6     -61.9    28      209   20 40 39
20 41 29  ---          06 21 59  14.0  76.8 -5.6     -61.9    50      215   20 40 40

20 41 58  B1152+199    06 22 18  15.3  76.0 -5.6     -62.4    18      215   20 41 58
20 45 58  ---          06 26 18  16.1  76.4 -5.5     -62.6   240      246   20 41 59
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

20 46 37  J1158+1821   06 26 57  15.0  77.4 -5.5     -62.2    28      246   20 46 37
20 47 27  ---          06 27 57  15.2  77.5 -5.5     -62.2    50      252   20 46 38

20 47 56  B1152+199    06 28 16  16.5  76.7 -5.5     -62.7    19      252   20 47 56
20 51 56  ---          06 32 17  17.3  77.1 -5.4     -62.9   240      283   20 47 57

20 52 34  J1158+1821   06 32 56  16.3  78.1 -5.4     -62.4    28      283   20 52 34
20 53 24  ---          06 33 56  16.5  78.2 -5.4     -62.5    50      290   20 52 35

20 53 54  B1152+199    06 34 15  17.8  77.3 -5.4     -63.0    19      290   20 53 54
20 57 54  ---          06 38 16  18.6  77.8 -5.3     -63.2   240      321   20 53 55

20 58 32  J1158+1821   06 38 55  17.5  78.7 -5.3     -62.7    28      321   20 58 32
20 59 22  ---          06 39 55  17.7  78.8 -5.3     -62.8    50      327   20 58 33

20 59 51  B1152+199    06 40 14  19.0  78.0 -5.3     -63.3    19      327   20 59 51
21 03 51  ---          06 44 15  19.9  78.5 -5.2     -63.5   240      358   20 59 52

21 04 30  J1158+1821   06 44 53  18.8  79.4 -5.2     -63.0    28      358   21 04 30
21 05 20  ---          06 45 53  19.0  79.5 -5.2     -63.0    50      365   21 04 31

21 05 49  B1152+199    06 46 13  20.3  78.7 -5.2     -63.6    19      365   21 05 49
21 09 49  ---          06 50 13  21.1  79.1 -5.1     -63.7   240      395   21 05 50

21 10 28  J1158+1821   06 50 52  20.0  80.1 -5.1     -63.2    28      395   21 10 28
21 11 18  ---          06 51 52  20.3  80.2 -5.1     -63.2    50      402   21 10 29

21 11 47  B1152+199    06 52 11  21.5  79.3 -5.1     -63.8    19      402   21 11 47
21 15 47  ---          06 56 12  22.4  79.8 -5.0     -64.0   240      433   21 11 48

21 16 25  J1158+1821   06 56 50  21.3  80.8 -5.0     -63.4    28      433   21 16 25
21 17 15  ---          06 57 51  21.5  80.9 -5.0     -63.5    50      439   21 16 26

21 17 44  B1152+199    06 58 10  22.8  80.0 -5.0     -64.1    19      439   21 17 44
21 21 44  ---          07 02 10  23.7  80.5 -4.9     -64.2   240      470   21 17 45

21 22 23  J1158+1821   07 02 49  22.6  81.5 -4.9     -63.7    28      470   21 22 23
21 23 13  ---          07 03 49  22.8  81.6 -4.9     -63.7    50      477   21 22 24

21 23 41  B1152+199    07 04 08  24.1  80.7 -4.9     -64.3    18      477   21 23 41
21 27 41  ---          07 08 09  24.9  81.1 -4.8     -64.5   240      508   21 23 42

21 28 20  J1158+1821   07 08 47  23.8  82.1 -4.8     -63.8    28      508   21 28 20
21 29 10  ---          07 09 48  24.1  82.3 -4.8     -63.9    50      514   21 28 21
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

21 29 39  B1152+199    07 10 06  25.3  81.3 -4.8     -64.5    18      514   21 29 39
21 33 39  ---          07 14 07  26.2  81.8 -4.7     -64.7   240      545   21 29 40

21 34 07  J1158+1821   07 14 36  25.1  82.8 -4.7     -64.0    18      545   21 34 07
21 35 07  ---          07 15 36  25.3  82.9 -4.7     -64.1    60      553   21 34 08

21 36 03  J1224+2122   07 16 31  21.2  77.1 -5.2     -64.2    39      553   21 36 03
21 37 53  ---          07 18 32  21.6  77.3 -5.1     -64.3   110      567   21 36 04

21 38 49  J1158+1821   07 19 18  26.1  83.3 -4.7     -64.2    39      567   21 38 49
21 39 39  ---          07 20 18  26.3  83.5 -4.6     -64.2    50      573   21 38 50

21 40 07  B1152+199    07 20 36  27.6  82.5 -4.6     -64.9    18      573   21 40 07
21 44 07  ---          07 24 37  28.4  83.0 -4.5     -65.0   240      604   21 40 08

21 44 46  J1158+1821   07 25 16  27.4  84.0 -4.6     -64.3    28      604   21 44 46
21 45 36  ---          07 26 16  27.6  84.2 -4.5     -64.3    50      611   21 44 47

21 46 04  B1152+199    07 26 35  28.9  83.2 -4.5     -65.1    18      611   21 46 04
21 50 04  ---          07 30 35  29.7  83.7 -4.4     -65.2   240      642   21 46 05

21 50 43  J1158+1821   07 31 14  28.6  84.7 -4.5     -64.5    28      642   21 50 43
21 51 33  ---          07 32 14  28.9  84.8 -4.4     -64.5    50      648   21 50 44

21 52 01  B1152+199    07 32 33  30.1  83.9 -4.4     -65.2    18      648   21 52 01
21 56 01  ---          07 36 33  31.0  84.3 -4.3     -65.3   240      679   21 52 02

21 56 40  J1158+1821   07 37 12  29.9  85.4 -4.4     -64.6    28      679   21 56 40
21 57 30  ---          07 38 12  30.1  85.5 -4.3     -64.6    50      685   21 56 41

21 57 58  B1152+199    07 38 31  31.4  84.6 -4.3     -65.4    18      685   21 57 58
22 01 58  ---          07 42 31  32.3  85.0 -4.2     -65.5   240      716   21 57 59

22 02 37  J1158+1821   07 43 10  31.2  86.1 -4.3     -64.7    28      716   22 02 37
22 03 27  ---          07 44 10  31.4  86.3 -4.2     -64.7    50      723   22 02 38

22 03 56  B1152+199    07 44 29  32.7  85.3 -4.2     -65.5    18      723   22 03 56
22 07 56  ---          07 48 29  33.5  85.7 -4.1     -65.6   240      754   22 03 57

22 08 33  J1158+1821   07 49 07  32.5  86.8 -4.2     -64.8    27      754   22 08 33
22 09 23  ---          07 50 07  32.7  87.0 -4.2     -64.8    50      760   22 08 34

22 09 51  B1152+199    07 50 25  34.0  85.9 -4.1     -65.6    18      760   22 09 51
22 13 51  ---          07 54 26  34.8  86.4 -4.0     -65.7   240      791   22 09 52
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

22 14 29  J1158+1821   07 55 04  33.8  87.6 -4.1     -64.9    27      791   22 14 29
22 15 19  ---          07 56 04  34.0  87.7 -4.1     -64.9    50      797   22 14 30

22 15 47  B1152+199    07 56 22  35.2  86.6 -4.0     -65.7    18      797   22 15 47
22 19 47  ---          08 00 23  36.1  87.1 -3.9     -65.8   240      828   22 15 48

22 20 24  J1158+1821   08 01 00  35.0  88.3 -4.0     -64.9    27      828   22 20 24
22 21 14  ---          08 02 00  35.3  88.4 -4.0     -64.9    50      835   22 20 25

22 21 42  B1152+199    08 02 18  36.5  87.4 -3.9     -65.8    18      835   22 21 42
22 25 42  ---          08 06 19  37.4  87.8 -3.8     -65.9   240      866   22 21 43

22 26 19  J1158+1821   08 06 56  36.3  89.0 -3.9     -65.0    27      866   22 26 19
22 27 09  ---          08 07 56  36.5  89.1 -3.9     -65.0    50      872   22 26 20

22 27 37  B1152+199    08 08 14  37.8  88.1 -3.8     -65.9    18      872   22 27 37
22 31 37  ---          08 12 15  38.6  88.6 -3.7     -65.9   240      903   22 27 38

22 32 05  J1158+1821   08 12 42  37.6  89.7 -3.8     -65.0    17      903   22 32 05
22 33 05  ---          08 13 43  37.8  89.9 -3.8     -65.0    60      911   22 32 06

22 34 01  J1224+2122   08 14 39  33.5  83.4 -4.2     -66.6    40      911   22 34 01
22 35 51  ---          08 16 39  33.9  83.7 -4.2     -66.6   110      925   22 34 02

22 36 48  J1158+1821   08 17 27  38.6  90.3 -3.7     -65.0    40      925   22 36 48
22 37 38  ---          08 18 27  38.8  90.5 -3.7     -65.0    50      931   22 36 49

22 38 06  B1152+199    08 18 45  40.0  89.4 -3.6     -65.9    17      931   22 38 06
22 42 06  ---          08 22 45  40.9  89.9 -3.6     -66.0   240      962   22 38 07

22 42 43  J1158+1821   08 23 22  39.8  91.1 -3.6     -65.0    27      962   22 42 43
22 43 33  ---          08 24 23  40.1  91.2 -3.6     -64.9    50      969   22 42 44

22 44 00  B1152+199    08 24 40  41.3  90.1 -3.5     -66.0    17      969   22 44 00
22 48 00  ---          08 28 41  42.2  90.6 -3.5     -65.9   240     1000   22 44 01

22 48 37  J1158+1821   08 29 18  41.1  91.9 -3.5     -64.9    27     1000   22 48 37
22 49 27  ---          08 30 18  41.3  92.0 -3.5     -64.9    50     1006   22 48 38

22 49 55  B1152+199    08 30 36  42.6  90.9 -3.4     -65.9    17     1006   22 49 55
22 53 55  ---          08 34 36  43.5  91.4 -3.4     -65.9   240     1037   22 49 56

22 54 32  J1158+1821   08 35 13  42.4  92.7 -3.4     -64.8    27     1037   22 54 32
22 55 22  ---          08 36 14  42.6  92.8 -3.4     -64.8    50     1043   22 54 33
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

22 55 49  B1152+199    08 36 31  43.9  91.7 -3.3     -65.9    17     1043   22 55 49
22 59 49  ---          08 40 32  44.7  92.2 -3.3     -65.9   240     1074   22 55 50

23 00 26  J1158+1821   08 41 09  43.7  93.5 -3.3     -64.7    26     1074   23 00 26
23 01 16  ---          08 42 09  43.9  93.7 -3.3     -64.7    50     1081   23 00 27

23 01 43  B1152+199    08 42 26  45.1  92.5 -3.2     -65.8    17     1081   23 01 43
23 05 43  ---          08 46 27  46.0  93.0 -3.2     -65.8   240     1112   23 01 44

23 06 20  J1158+1821   08 47 04  44.9  94.4 -3.2     -64.6    26     1112   23 06 20
23 07 10  ---          08 48 04  45.2  94.5 -3.2     -64.6    50     1118   23 06 21

23 07 37  B1152+199    08 48 21  46.4  93.3 -3.1     -65.7    17     1118   23 07 37
23 11 37  ---          08 52 22  47.3  93.9 -3.1     -65.7   240     1149   23 07 38

23 12 14  J1158+1821   08 52 59  46.2  95.2 -3.1     -64.5    26     1149   23 12 14
23 13 04  ---          08 53 59  46.4  95.4 -3.1     -64.4    50     1156   23 12 15

23 13 31  B1152+199    08 54 16  47.7  94.1 -3.0     -65.6    17     1156   23 13 31
23 17 31  ---          08 58 17  48.5  94.7 -3.0     -65.5   240     1186   23 13 32

23 18 08  J1158+1821   08 58 53  47.5  96.1 -3.0     -64.3    26     1186   23 18 08
23 18 58  ---          08 59 53  47.7  96.3 -3.0     -64.3    50     1193   23 18 09

23 19 25  B1152+199    09 00 11  48.9  95.0 -2.9     -65.5    17     1193   23 19 25
23 23 25  ---          09 04 11  49.8  95.6 -2.9     -65.3   240     1224   23 19 26

23 24 02  J1158+1821   09 04 48  48.7  97.0 -2.9     -64.1    26     1224   23 24 02
23 24 52  ---          09 05 48  48.9  97.2 -2.9     -64.0    50     1230   23 24 03

23 25 19  B1152+199    09 06 05  50.2  95.9 -2.8     -65.3    17     1230   23 25 19
23 29 19  ---          09 10 06  51.1  96.5 -2.8     -65.1   240     1261   23 25 20

23 29 48  J1158+1821   09 10 36  50.0  97.9 -2.8     -63.8    19     1261   23 29 48
23 30 48  ---          09 11 36  50.2  98.1 -2.8     -63.8    60     1269   23 29 49

23 31 45  J1224+2122   09 12 33  45.9  90.3 -3.2     -67.4    40     1269   23 31 45
23 33 35  ---          09 14 33  46.4  90.5 -3.2     -67.4   110     1283   23 31 46

23 34 33  J1158+1821   09 15 21  51.0  98.7 -2.7     -63.6    41     1283   23 34 33
23 35 23  ---          09 16 21  51.2  98.9 -2.7     -63.5    50     1289   23 34 34

23 36 09  B1152+199    09 16 57  52.5  97.6 -2.7     -64.8    36     1289   23 36 09
23 40 09  ---          09 20 58  53.4  98.3 -2.6     -64.6   240     1320   23 36 10
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  31 May 2015   Day 151 ---

23 40 45  J1158+1821   09 21 34  52.3  99.8 -2.6     -63.2    26     1320   23 40 45
23 41 35  ---          09 22 34  52.5 100.0 -2.6     -63.2    50     1327   23 40 46

23 42 02  B1152+199    09 22 51  53.8  98.6 -2.6     -64.5    16     1327   23 42 02
23 46 02  ---          09 26 52  54.6  99.3 -2.5     -64.3   240     1358   23 42 03

23 46 38  J1158+1821   09 27 28  53.5 100.9 -2.5     -62.9    26     1358   23 46 38
23 47 28  ---          09 28 28  53.8 101.0 -2.5     -62.8    50     1364   23 46 39

23 47 55  B1152+199    09 28 45  55.0  99.6 -2.5     -64.2    16     1364   23 47 55
23 51 55  ---          09 32 46  55.9 100.4 -2.4     -63.9   240     1395   23 47 56

23 52 31  J1158+1821   09 33 22  54.8 102.0 -2.4     -62.4    26     1395   23 52 31
23 53 21  ---          09 34 22  55.0 102.1 -2.4     -62.4    50     1402   23 52 32

23 53 48  B1152+199    09 34 39  56.3 100.7 -2.4     -63.8    16     1402   23 53 48
23 57 48  ---          09 38 40  57.1 101.5 -2.3     -63.5   240     1432   23 53 49

23 58 24  J1158+1821   09 39 16  56.0 103.1 -2.3     -62.0    26     1432   23 58 24
23 59 14  ---          09 40 16  56.2 103.3 -2.3     -61.9    50     1439   23 58 25

 --- Start: Sun  31 May 2015   Day 151 -- Stop: Mon   1 Jun 2015   Day 152 ---

23 59 41  B1152+199    09 40 33  57.5 101.9 -2.3     -63.3    16     1439   23 59 41
00 03 41  ---          09 44 33  58.4 102.7 -2.2     -63.0   240     1470   23 59 42

00 04 17  J1158+1821   09 45 10  57.3 104.3 -2.2     -61.4    26     1470   00 04 17
00 05 07  ---          09 46 10  57.5 104.5 -2.2     -61.3    50     1476   00 04 18

00 05 33  B1152+199    09 46 26  58.8 103.0 -2.2     -62.8    16     1476   00 05 33
00 09 33  ---          09 50 27  59.6 103.9 -2.1     -62.4   240     1507   00 05 34

00 10 09  J1158+1821   09 51 03  58.5 105.6 -2.1     -60.8    26     1507   00 10 09
00 10 59  ---          09 52 03  58.7 105.8 -2.1     -60.7    50     1514   00 10 10

00 11 26  B1152+199    09 52 20  60.0 104.3 -2.1     -62.2    16     1514   00 11 26
00 15 26  ---          09 56 20  60.8 105.2 -2.0     -61.8   240     1545   00 11 27

00 16 02  J1158+1821   09 56 56  59.7 106.9 -2.0     -60.1    26     1545   00 16 02
00 16 52  ---          09 57 57  59.9 107.2 -2.0     -60.0    50     1551   00 16 03

00 17 18  B1152+199    09 58 13  61.2 105.6 -2.0     -61.6    16     1551   00 17 18
00 21 18  ---          10 02 14  62.1 106.6 -1.9     -61.1   240     1582   00 17 19
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

00 21 54  J1158+1821   10 02 50  60.9 108.3 -1.9     -59.3    25     1582   00 21 54
00 22 44  ---          10 03 50  61.1 108.6 -1.9     -59.2    50     1588   00 21 55

00 23 10  B1152+199    10 04 06  62.4 107.0 -1.9     -60.8    16     1588   00 23 10
00 27 10  ---          10 08 07  63.3 108.1 -1.8     -60.3   240     1619   00 23 11

00 28 05  J1224+2122   10 09 02  58.0  98.7 -2.3     -65.9    36     1619   00 28 05
00 29 25  ---          10 10 32  58.4  99.0 -2.3     -65.8    80     1630   00 28 06

00 29 55  J1158+1821   10 10 52  62.5 110.4 -1.8     -58.1    13     1630   00 29 55
00 30 55  ---          10 11 52  62.7 110.7 -1.8     -58.0    60     1637   00 29 56

00 31 07  B1152+199    10 12 04  64.1 109.1 -1.7     -59.6     1     1637   00 31 07
00 35 07  ---          10 16 05  64.9 110.2 -1.7     -59.0   240     1668   00 31 08

00 35 18  J1158+1821   10 16 17  63.6 112.0 -1.7     -57.2     1     1668   00 35 18
00 36 18  ---          10 17 17  63.8 112.2 -1.7     -57.0    60     1676   00 35 19

00 36 30  B1152+199    10 17 28  65.2 110.6 -1.6     -58.7     1     1676   00 36 30
00 40 30  ---          10 21 29  66.0 111.8 -1.6     -58.0   240     1707   00 36 31

00 40 42  J1158+1821   10 21 41  64.7 113.6 -1.6     -56.2     1     1707   00 40 42
00 41 42  ---          10 22 41  64.9 113.9 -1.6     -56.0    60     1715   00 40 43

00 41 53  B1152+199    10 22 52  66.2 112.3 -1.6     -57.7     1     1715   00 41 53
00 45 53  ---          10 26 53  67.0 113.6 -1.5     -56.8   240     1746   00 41 54

00 46 04  J1158+1821   10 27 04  65.8 115.3 -1.5     -55.0     1     1746   00 46 04
00 47 04  ---          10 28 04  65.9 115.6 -1.5     -54.8    60     1753   00 46 05

00 47 15  B1152+199    10 28 15  67.3 114.0 -1.5     -56.5     0     1753   00 47 15
00 51 15  ---          10 32 16  68.1 115.4 -1.4     -55.6   240     1784   00 47 16

00 51 26  J1158+1821   10 32 27  66.8 117.1 -1.4     -53.7     0     1784   00 51 26
00 52 26  ---          10 33 27  67.0 117.5 -1.4     -53.5    60     1792   00 51 27

00 52 37  B1152+199    10 33 38  68.4 115.9 -1.4     -55.2     0     1792   00 52 37
00 56 37  ---          10 37 39  69.1 117.4 -1.3     -54.2   240     1823   00 52 38

00 56 48  J1158+1821   10 37 50  67.8 119.1 -1.4     -52.3     0     1823   00 56 48
00 57 48  ---          10 38 50  68.0 119.5 -1.3     -52.0    60     1831   00 56 49

00 57 59  B1152+199    10 39 01  69.4 117.9 -1.3     -53.8     0     1831   00 57 59
01 01 59  ---          10 43 02  70.1 119.6 -1.2     -52.6   240     1861   00 58 00
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

01 02 10  J1158+1821   10 43 13  68.8 121.3 -1.3     -50.7     0     1861   01 02 10
01 03 10  ---          10 44 13  69.0 121.7 -1.2     -50.4    60     1869   01 02 11

01 03 21  B1152+199    10 44 24  70.4 120.2 -1.2     -52.1     0     1869   01 03 21
01 07 21  ---          10 48 25  71.1 121.9 -1.1     -50.8   240     1900   01 03 22

01 07 32  J1158+1821   10 48 36  69.8 123.6 -1.2     -49.0     0     1900   01 07 32
01 08 32  ---          10 49 36  70.0 124.1 -1.2     -48.6    60     1908   01 07 33

01 08 43  B1152+199    10 49 47  71.4 122.6 -1.1     -50.3     0     1908   01 08 43
01 12 43  ---          10 53 47  72.1 124.5 -1.0     -48.8   240     1939   01 08 44

01 12 54  J1158+1821   10 53 58  70.7 126.1 -1.1     -47.0     0     1939   01 12 54
01 13 54  ---          10 54 59  70.9 126.6 -1.1     -46.6    60     1946   01 12 55

01 14 05  B1152+199    10 55 10  72.4 125.2 -1.0     -48.2     0     1946   01 14 05
01 18 05  ---          10 59 10  73.0 127.4 -0.9     -46.5   240     1977   01 14 06

01 18 27  J1224+2122   10 59 32  68.6 110.7 -1.4     -59.8     2     1977   01 18 27
01 20 27  ---          11 01 33  69.0 111.3 -1.4     -59.3   120     1993   01 18 28

01 20 49  J1158+1821   11 01 54  72.1 130.3 -1.0     -43.7     0     1993   01 20 49
01 21 49  ---          11 02 54  72.2 130.9 -0.9     -43.3    60     2001   01 20 50

01 22 00  B1152+199    11 03 05  73.7 129.7 -0.9     -44.7     0     2001   01 22 00
01 26 00  ---          11 07 06  74.4 132.1 -0.8     -42.6   240     2031   01 22 01

01 26 11  J1158+1821   11 07 17  72.9 133.4 -0.9     -41.1     0     2031   01 26 11
01 27 11  ---          11 08 17  73.1 134.0 -0.8     -40.6    60     2039   01 26 12

01 27 22  B1152+199    11 08 28  74.6 133.0 -0.8     -41.9     0     2039   01 27 22
01 31 22  ---          11 12 29  75.2 135.8 -0.7     -39.6   240     2070   01 27 23

01 31 33  J1158+1821   11 12 40  73.8 136.9 -0.8     -38.3     0     2070   01 31 33
01 32 33  ---          11 13 40  73.9 137.5 -0.8     -37.7    60     2078   01 31 34

01 32 44  B1152+199    11 13 51  75.4 136.8 -0.7     -38.7     0     2078   01 32 44
01 36 44  ---          11 17 52  76.0 139.8 -0.6     -36.1   240     2109   01 32 45

01 36 55  J1158+1821   11 18 03  74.5 140.6 -0.7     -35.1     0     2109   01 36 55
01 37 55  ---          11 19 03  74.7 141.3 -0.7     -34.5    60     2116   01 36 56

01 38 06  B1152+199    11 19 14  76.2 140.9 -0.6     -35.2     0     2116   01 38 06
01 42 06  ---          11 23 15  76.7 144.2 -0.5     -32.3   240     2147   01 38 07
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

01 42 17  J1158+1821   11 23 26  75.2 144.7 -0.6     -31.6     0     2147   01 42 17
01 43 17  ---          11 24 26  75.3 145.5 -0.6     -30.9    60     2155   01 42 18

01 43 28  B1152+199    11 24 37  76.9 145.4 -0.5     -31.2     0     2155   01 43 28
01 47 28  ---          11 28 37  77.3 149.1 -0.5     -28.0   240     2186   01 43 29

01 47 39  J1158+1821   11 28 48  75.9 149.2 -0.5     -27.7     0     2186   01 47 39
01 48 39  ---          11 29 49  76.0 150.0 -0.5     -26.9    60     2194   01 47 40

01 48 50  B1152+199    11 30 00  77.5 150.4 -0.4     -26.8     0     2194   01 48 50
01 52 50  ---          11 34 00  77.9 154.4 -0.4     -23.2   240     2225   01 48 51

01 53 01  J1158+1821   11 34 11  76.4 154.0 -0.4     -23.4     0     2225   01 53 01
01 54 01  ---          11 35 12  76.5 154.9 -0.4     -22.6    60     2232   01 53 02

01 54 12  B1152+199    11 35 23  78.0 155.9 -0.3     -21.9     0     2232   01 54 12
01 58 12  ---          11 39 23  78.3 160.2 -0.3     -18.0   240     2263   01 54 13

01 58 23  J1158+1821   11 39 34  76.9 159.1 -0.3     -18.8     0     2263   01 58 23
01 59 23  ---          11 40 34  76.9 160.1 -0.3     -17.9    60     2271   01 58 24

01 59 34  B1152+199    11 40 45  78.4 161.7 -0.3     -16.7     0     2271   01 59 34
02 03 34  ---          11 44 46  78.6 166.3 -0.2     -12.5   240     2302   01 59 35

02 03 45  J1158+1821   11 44 57  77.2 164.6 -0.2     -13.9     0     2302   02 03 45
02 04 45  ---          11 45 57  77.3 165.6 -0.2     -13.0    60     2310   02 03 46

02 04 56  B1152+199    11 46 08  78.7 167.9 -0.2     -11.0     0     2310   02 04 56
02 08 56  ---          11 50 09  78.9 172.7 -0.1      -6.6   240     2341   02 04 57

02 09 28  J1224+2122   11 50 42  77.8 137.9 -0.6     -38.3     0     2341   02 09 28
02 11 28  ---          11 52 42  78.1 139.7 -0.5     -36.7   120     2356   02 09 29

02 12 00  J1158+1821   11 53 14  77.6 173.5 -0.1      -5.9     0     2356   02 12 00
02 13 00  ---          11 54 14  77.6 174.6 -0.1      -4.9    60     2364   02 12 01

02 13 11  B1152+199    11 54 25  78.9 177.9 -0.0      -1.9     0     2364   02 13 11
02 17 11  ---          11 58 26  78.9 182.9  0.0       2.6   240     2395   02 13 12

02 17 22  J1158+1821   11 58 37  77.6 179.4 -0.0      -0.5     0     2395   02 17 22
02 18 22  ---          11 59 37  77.6 180.5  0.0       0.5    60     2402   02 17 23

02 18 33  B1152+199    11 59 48  78.9 184.5  0.1       4.1     0     2402   02 18 33
02 22 33  ---          12 03 49  78.8 189.4  0.1       8.6   240     2433   02 18 34
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

02 22 44  J1158+1821   12 04 00  77.6 185.4  0.1       4.9     0     2433   02 22 44
02 23 44  ---          12 05 00  77.6 186.5  0.1       5.9    60     2441   02 22 45

02 23 55  B1152+199    12 05 11  78.8 191.0  0.2      10.1     0     2441   02 23 55
02 27 55  ---          12 09 12  78.6 195.7  0.2      14.3   240     2472   02 23 56

02 28 06  J1158+1821   12 09 23  77.4 191.2  0.2      10.2     0     2472   02 28 06
02 29 06  ---          12 10 23  77.4 192.3  0.2      11.1    60     2480   02 28 07

02 29 18  B1152+199    12 10 34  78.5 197.3  0.2      15.8     0     2480   02 29 18
02 33 18  ---          12 14 35  78.2 201.8  0.3      19.8   240     2511   02 29 19

02 33 29  J1158+1821   12 14 47  77.1 196.9  0.3      15.3     0     2511   02 33 29
02 34 29  ---          12 15 47  77.1 197.9  0.3      16.2    60     2518   02 33 30

02 34 41  B1152+199    12 15 58  78.1 203.2  0.3      21.1     0     2518   02 34 41
02 38 41  ---          12 19 59  77.7 207.4  0.4      24.8   240     2549   02 34 42

02 38 52  J1158+1821   12 20 11  76.8 202.3  0.4      20.1     0     2549   02 38 52
02 39 52  ---          12 21 11  76.7 203.3  0.4      21.0    60     2557   02 38 53

02 40 04  B1152+199    12 21 22  77.6 208.8  0.4      26.1     0     2557   02 40 04
02 44 04  ---          12 25 23  77.1 212.6  0.5      29.5   240     2588   02 40 05

02 44 15  J1158+1821   12 25 35  76.3 207.4  0.4      24.7     0     2588   02 44 15
02 45 15  ---          12 26 35  76.2 208.3  0.5      25.5    60     2596   02 44 16

02 45 27  B1152+199    12 26 47  77.0 213.8  0.5      30.6     0     2596   02 45 27
02 49 27  ---          12 30 47  76.4 217.3  0.6      33.6   240     2627   02 45 28

02 49 39  J1158+1821   12 30 59  75.7 212.1  0.5      28.8     0     2627   02 49 39
02 50 39  ---          12 31 59  75.6 213.0  0.5      29.6    60     2634   02 49 40

02 50 51  B1152+199    12 32 11  76.3 218.5  0.6      34.6     0     2634   02 50 51
02 54 51  ---          12 36 12  75.7 221.6  0.7      37.4   240     2665   02 50 52

02 55 02  J1158+1821   12 36 23  75.0 216.5  0.6      32.6     0     2665   02 55 02
02 56 02  ---          12 37 23  74.9 217.3  0.6      33.3    60     2673   02 55 03

02 56 14  B1152+199    12 37 35  75.5 222.7  0.7      38.2     0     2673   02 56 14
03 00 14  ---          12 41 36  74.9 225.5  0.8      40.7   240     2704   02 56 15

03 00 46  J1224+2122   12 42 08  80.0 202.5  0.3      20.7     8     2704   03 00 46
03 02 46  ---          12 44 09  79.8 205.0  0.3      23.0   120     2719   03 00 47
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

03 03 16  J1158+1821   12 44 39  73.9 222.5  0.8      37.7    10     2719   03 03 16
03 04 16  ---          12 45 39  73.8 223.2  0.8      38.3    60     2727   03 03 17

03 04 28  B1152+199    12 45 50  74.2 228.3  0.8      43.0     0     2727   03 04 28
03 08 28  ---          12 49 51  73.6 230.8  0.9      45.0   240     2758   03 04 29

03 08 39  J1158+1821   12 50 02  73.1 226.0  0.8      40.7     0     2758   03 08 39
03 09 39  ---          12 51 02  72.9 226.6  0.9      41.2    60     2766   03 08 40

03 09 50  B1152+199    12 51 14  73.4 231.6  0.9      45.7     0     2766   03 09 50
03 13 50  ---          12 55 15  72.7 233.8  1.0      47.5   240     2797   03 09 51

03 14 02  J1158+1821   12 55 26  72.2 229.2  0.9      43.3     0     2797   03 14 02
03 15 02  ---          12 56 26  72.1 229.7  1.0      43.8    60     2804   03 14 03

03 15 13  B1152+199    12 56 37  72.4 234.5  1.0      48.1     0     2804   03 15 13
03 19 13  ---          13 00 38  71.7 236.6  1.1      49.6   240     2835   03 15 14

03 19 24  J1158+1821   13 00 49  71.3 232.1  1.0      45.6     0     2835   03 19 24
03 20 24  ---          13 01 50  71.2 232.6  1.0      46.1    60     2843   03 19 25

03 20 36  B1152+199    13 02 01  71.5 237.2  1.1      50.2     0     2843   03 20 36
03 24 36  ---          13 06 02  70.7 239.1  1.2      51.6   240     2874   03 20 37

03 24 47  J1158+1821   13 06 13  70.4 234.8  1.1      47.8     0     2874   03 24 47
03 25 47  ---          13 07 13  70.2 235.3  1.1      48.1    60     2882   03 24 48

03 25 59  B1152+199    13 07 25  70.5 239.7  1.2      52.0     0     2882   03 25 59
03 29 59  ---          13 11 25  69.7 241.4  1.3      53.3   240     2913   03 26 00

03 30 10  J1158+1821   13 11 37  69.4 237.2  1.2      49.6     0     2913   03 30 10
03 31 10  ---          13 12 37  69.3 237.7  1.2      50.0    60     2920   03 30 11

03 31 21  B1152+199    13 12 48  69.5 241.9  1.3      53.7     0     2920   03 31 21
03 35 21  ---          13 16 49  68.7 243.5  1.3      54.8   240     2951   03 31 22

03 35 32  J1158+1821   13 17 00  68.5 239.5  1.3      51.3     0     2951   03 35 32
03 36 32  ---          13 18 00  68.3 239.9  1.3      51.6    60     2959   03 35 33

03 36 44  B1152+199    13 18 11  68.4 244.0  1.4      55.1     1     2959   03 36 44
03 40 44  ---          13 22 12  67.7 245.4  1.4      56.1   240     2990   03 36 45

03 40 55  J1158+1821   13 22 23  67.4 241.6  1.4      52.9     1     2990   03 40 55
03 41 55  ---          13 23 23  67.3 242.0  1.4      53.1    60     2998   03 40 56
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

03 42 06  B1152+199    13 23 35  67.4 245.9  1.5      56.4     1     2998   03 42 06
03 46 06  ---          13 27 35  66.6 247.2  1.5      57.3   240     3029   03 42 07

03 46 17  J1158+1821   13 27 46  66.4 243.5  1.5      54.2     1     3029   03 46 17
03 47 17  ---          13 28 47  66.2 243.9  1.5      54.5    60     3036   03 46 18

03 47 28  B1152+199    13 28 58  66.3 247.6  1.5      57.6     1     3036   03 47 28
03 51 28  ---          13 32 58  65.5 248.8  1.6      58.4   240     3067   03 47 29

03 51 51  J1224+2122   13 33 21  72.2 242.4  1.1      54.9     2     3067   03 51 51
03 53 51  ---          13 35 21  71.8 243.3  1.2      55.6   120     3083   03 51 52

03 54 14  J1158+1821   13 35 44  64.9 246.2  1.6      56.0     1     3083   03 54 14
03 55 14  ---          13 36 45  64.7 246.5  1.6      56.2    60     3090   03 54 15

03 55 25  B1152+199    13 36 56  64.7 250.0  1.7      59.1     1     3090   03 55 25
03 59 25  ---          13 40 56  63.9 251.1  1.7      59.8   240     3121   03 55 26

03 59 35  J1158+1821   13 41 07  63.8 247.8  1.7      57.0     1     3121   03 59 35
04 00 35  ---          13 42 07  63.6 248.1  1.7      57.2    60     3129   03 59 36

04 00 46  B1152+199    13 42 18  63.6 251.5  1.8      60.0     1     3129   04 00 46
04 04 46  ---          13 46 19  62.8 252.5  1.8      60.6   240     3160   04 00 47

04 04 57  J1158+1821   13 46 29  62.7 249.3  1.8      58.0     1     3160   04 04 57
04 05 57  ---          13 47 30  62.5 249.6  1.8      58.1    60     3168   04 04 58

04 06 08  B1152+199    13 47 40  62.5 252.8  1.9      60.8     1     3168   04 06 08
04 10 08  ---          13 51 41  61.7 253.8  1.9      61.3   240     3199   04 06 09

04 10 18  J1158+1821   13 51 52  61.6 250.7  1.9      58.8     0     3199   04 10 18
04 11 18  ---          13 52 52  61.4 251.0  1.9      59.0    60     3206   04 10 19

04 11 29  B1152+199    13 53 02  61.4 254.1  1.9      61.5     0     3206   04 11 29
04 15 29  ---          13 57 03  60.6 255.1  2.0      61.9   240     3237   04 11 30

04 15 39  J1158+1821   13 57 13  60.5 252.1  2.0      59.6     0     3237   04 15 39
04 16 39  ---          13 58 14  60.3 252.3  2.0      59.7    60     3245   04 15 40

04 16 50  B1152+199    13 58 24  60.3 255.4  2.0      62.1     0     3245   04 16 50
04 20 50  ---          14 02 25  59.5 256.3  2.1      62.5   240     3276   04 16 51

04 21 00  J1158+1821   14 02 35  59.4 253.4  2.1      60.3     1     3276   04 21 00
04 22 00  ---          14 03 35  59.2 253.6  2.1      60.4    60     3284   04 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

04 22 11  B1152+199    14 03 46  59.2 256.5  2.1      62.6     1     3284   04 22 11
04 26 11  ---          14 07 47  58.3 257.4  2.2      63.0   240     3315   04 22 12

04 26 21  J1158+1821   14 07 57  58.3 254.6  2.1      60.9     1     3315   04 26 21
04 27 21  ---          14 08 58  58.1 254.8  2.2      61.0    60     3322   04 26 22

04 27 32  B1152+199    14 09 08  58.1 257.6  2.2      63.1     1     3322   04 27 32
04 31 32  ---          14 13 09  57.2 258.4  2.3      63.5   240     3353   04 27 33

04 31 43  J1158+1821   14 13 20  57.2 255.7  2.2      61.4     1     3353   04 31 43
04 32 43  ---          14 14 20  57.0 255.9  2.3      61.5    60     3361   04 31 44

04 32 54  B1152+199    14 14 31  56.9 258.7  2.3      63.6     1     3361   04 32 54
04 36 54  ---          14 18 32  56.1 259.5  2.4      63.9   240     3392   04 32 55

04 37 05  J1158+1821   14 18 43  56.1 256.8  2.3      61.9     1     3392   04 37 05
04 38 05  ---          14 19 43  55.9 257.0  2.3      62.0    60     3400   04 37 06

04 38 16  B1152+199    14 19 54  55.8 259.7  2.4      64.0     1     3400   04 38 16
04 42 16  ---          14 23 55  54.9 260.4  2.5      64.2   240     3430   04 38 17

04 42 39  J1224+2122   14 24 18  61.9 257.7  2.0      64.5     1     3430   04 42 39
04 44 39  ---          14 26 18  61.4 258.2  2.0      64.7   120     3446   04 42 40

04 45 02  J1158+1821   14 26 41  54.4 258.4  2.5      62.6     1     3446   04 45 02
04 46 02  ---          14 27 41  54.2 258.6  2.5      62.6    60     3454   04 45 03

04 46 14  B1152+199    14 27 53  54.1 261.1  2.5      64.5     2     3454   04 46 14
04 50 14  ---          14 31 54  53.2 261.8  2.6      64.7   240     3485   04 46 15

04 50 26  J1158+1821   14 32 05  53.3 259.4  2.5      63.0     2     3485   04 50 26
04 51 26  ---          14 33 06  53.1 259.6  2.6      63.0    60     3492   04 50 27

04 51 37  B1152+199    14 33 18  52.9 262.1  2.6      64.8     2     3492   04 51 37
04 55 37  ---          14 37 18  52.1 262.7  2.7      64.9   240     3523   04 51 38

04 55 50  J1158+1821   14 37 31  52.1 260.3  2.6      63.3     3     3523   04 55 50
04 56 50  ---          14 38 31  51.9 260.5  2.7      63.4    60     3531   04 55 51

04 57 02  B1152+199    14 38 43  51.8 262.9  2.7      65.0     3     3531   04 57 02
05 01 02  ---          14 42 44  50.9 263.6  2.8      65.2   240     3562   04 57 03

05 01 15  J1158+1821   14 42 57  51.0 261.3  2.7      63.6     3     3562   05 01 15
05 02 15  ---          14 43 57  50.8 261.4  2.7      63.6    60     3570   05 01 16
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Phase-referencing of B1152+199
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   1 Jun 2015   Day 152 ---

05 02 28  B1152+199    14 44 10  50.6 263.8  2.8      65.2     3     3570   05 02 28
05 06 28  ---          14 48 11  49.8 264.4  2.9      65.4   240     3600   05 02 29

05 06 42  J1158+1821   14 48 24  49.8 262.2  2.8      63.9     4     3600   05 06 42
05 07 42  ---          14 49 25  49.6 262.3  2.8      63.9    60     3608   05 06 43

05 07 56  B1152+199    14 49 38  49.5 264.6  2.9      65.4     4     3608   05 07 56
05 11 56  ---          14 53 39  48.6 265.2  3.0      65.5   240     3639   05 07 57

05 12 10  J1158+1821   14 53 54  48.6 263.0  2.9      64.1     5     3639   05 12 10
05 13 10  ---          14 54 54  48.4 263.2  2.9      64.1    60     3647   05 12 11

05 13 25  B1152+199    14 55 09  48.3 265.5  3.0      65.6     5     3647   05 13 25
05 17 25  ---          14 59 09  47.4 266.0  3.1      65.7   240     3678   05 13 26

05 17 41  J1158+1821   14 59 25  47.5 263.9  3.0      64.3     6     3678   05 17 41
05 18 41  ---          15 00 25  47.2 264.1  3.0      64.3    60     3686   05 17 42

05 18 57  B1152+199    15 00 42  47.1 266.3  3.1      65.7     7     3686   05 18 57
05 22 57  ---          15 04 42  46.2 266.8  3.1      65.8   240     3716   05 18 58

05 23 15  J1158+1821   15 05 00  46.3 264.7  3.1      64.5     9     3716   05 23 15
05 24 15  ---          15 06 00  46.1 264.9  3.1      64.5    60     3724   05 23 16

05 24 33  B1152+199    15 06 19  45.9 267.1  3.2      65.8     9     3724   05 24 33
05 28 33  ---          15 10 19  45.0 267.6  3.2      65.8   240     3755   05 24 34

05 28 56  J1224+2122   15 10 42  52.0 265.9  2.8      67.1     1     3755   05 28 56
05 29 56  ---          15 11 42  51.8 266.0  2.8      67.1    60     3763   05 28 57


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess215.X1024glob
   Matching groups in /opt/sched/sched_11.4/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    6         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = off
   LO sum=   8351.25  8351.25  8383.25  8383.25  8415.25  8415.25  8447.25  8447.25
   BBC fr=    751.25   751.25   783.25   783.25   815.25   815.25   847.25   847.25
   Bandwd=     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     791.25    791.25    823.25    823.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20  21  22

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * B1152+199         11 52 43.941355   * 11 55 18.328885     11 56 06.135474       0.00
                     19 56 23.25440    * 19 39 41.60530      19 34 35.87753        0.00
                     From catalog imbedded in main SCHED input file.

 * J1158+1821        11 55 46.237132   * 11 58 20.284700     11 59 08.021652       0.00
                     18 38 31.16817    * 18 21 49.25400      18 16 43.14995        0.00
                     From catalog imbedded in main SCHED input file.

 * J1224+2122        12 22 23.408715   * 12 24 54.458400     12 25 41.395725       0.00
                     21 39 23.03739    * 21 22 46.38900      21 17 43.94948        0.00
                     From catalog imbedded in main SCHED input file.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  B1152+199  sess215.X1024glob     1 2 3 4 5 8 9 10 11 12 13        11.000   880.596
  J1158+1821 sess215.X1024glob     1 2 3 4 5 8 9 10 11 12 13         2.636   207.933
  J1224+2122 sess215.X1024glob     1 2 3 4 5 8 9 10 11 12 13         0.572    43.264


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   B1152+199          100.5
   J1158+1821         101.7
   J1224+2122         105.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

