  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Global 7mm VLBI observations of Cygnus A
 Exp. Code:  gb075c  


Schedule Version:       1.00
Processed by SCHED version:  11.30  Version 11.3 update 1.  April 14, 2014

PI:       Biagina Boccardi

Address:  Max Planck Institute for Radioastronomy
          Auf dem Huegel 69
          Bonn, 53121
           Germany

Phone:    +49 (0)228 525 366
EMAIL:    bboccardi@mpifr-bonn.mpg.de
Fax:      +49-2257-301-106
Phone during observation: +49-2257-301-155

Observing mode: 1024-32-2

Notes:
 
 
 


COVER LETTER:

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

 Next scan frequencies:  43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
 Next BBC frequencies:     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

03 34 00  CYG-A        13 07 34  10.7  48.6 -6.9     -58.5     0        0   03 34 00
03 38 00  ---          13 11 35  11.3  49.0 -6.8     -59.1   240       31   03 34 01

03 43 00  CYG-A        13 16 36  12.1  49.5 -6.7     -59.8   294       31   03 43 00
03 55 00  ---          13 28 38  14.1  50.7 -6.5     -61.5   720      124   03 43 01

03 56 00  CYG-A        13 29 38  14.3  50.8 -6.5     -61.6    54      124   03 56 00
04 00 00  ---          13 33 39  14.9  51.1 -6.4     -62.2   240      155   03 56 01

04 17 00  2013+370     13 50 41  13.4  54.5 -6.4     -61.6  1003      155   04 17 00
04 19 00  ---          13 52 42  13.8  54.6 -6.4     -61.8   120      170   04 17 01

04 21 00  CYG-A        13 54 42  18.5  53.0 -6.1     -65.1   103      170   04 21 00
04 33 00  ---          14 06 44  20.6  54.0 -5.9     -66.8   720      263   04 21 01

04 34 00  CYG-A        14 07 44  20.8  54.0 -5.9     -66.9    54      263   04 34 00
04 38 00  ---          14 11 45  21.5  54.4 -5.8     -67.4   240      294   04 34 01

04 39 00  2013+370     14 12 45  17.4  56.5 -6.1     -64.3    44      294   04 39 00
04 41 00  ---          14 14 45  17.7  56.7 -6.0     -64.6   120      309   04 39 01

04 43 00  CYG-A        14 16 46  22.4  54.7 -5.7     -68.1   103      309   04 43 00
04 55 00  ---          14 28 48  24.5  55.6 -5.5     -69.7   720      402   04 43 01

04 56 00  CYG-A        14 29 48  24.7  55.7 -5.5     -69.8    54      402   04 56 00
05 00 00  ---          14 33 48  25.4  56.0 -5.4     -70.4   240      433   04 56 01

05 01 00  2013+370     14 34 49  21.4  58.4 -5.7     -67.0    44      433   05 01 00
05 03 00  ---          14 36 49  21.7  58.6 -5.7     -67.3   120      448   05 01 01

05 05 00  CYG-A        14 38 49  26.3  56.3 -5.4     -71.0   104      448   05 05 00
05 17 00  ---          14 50 51  28.4  57.1 -5.2     -72.6   720      541   05 05 01

05 18 00  CYG-A        14 51 51  28.6  57.2 -5.1     -72.8    54      541   05 18 00
05 22 00  ---          14 55 52  29.3  57.5 -5.1     -73.3   240      572   05 18 01

05 23 00  2013+370     14 56 52  25.4  60.2 -5.3     -69.7    44      572   05 23 00
05 25 00  ---          14 58 53  25.8  60.4 -5.3     -69.9   120      587   05 23 01

05 27 00  CYG-A        15 00 53  30.3  57.8 -5.0     -74.0   104      587   05 27 00
05 39 00  ---          15 12 55  32.4  58.5 -4.8     -75.6   720      680   05 27 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

05 40 00  CYG-A        15 13 55  32.6  58.5 -4.8     -75.7    54      680   05 40 00
05 44 00  ---          15 17 56  33.4  58.7 -4.7     -76.2   240      711   05 40 01

05 46 00  BLLAC        15 19 56  12.9  48.1 -6.7     -60.1    71      711   05 46 00
05 49 00  ---          15 22 56  13.4  48.4 -6.7     -60.5   180      734   05 46 01

05 55 00  2013+370     15 28 57  31.5  62.5 -4.8     -73.4   318      734   05 55 00
05 57 00  ---          15 30 58  31.9  62.6 -4.8     -73.7   120      750   05 55 01

05 59 00  CYG-A        15 32 58  36.1  59.5 -4.5     -78.3   104      750   05 59 00
06 11 00  ---          15 45 00  38.4  60.1 -4.3     -79.9   720      842   05 59 01

06 12 00  CYG-A        15 46 00  38.6  60.1 -4.2     -80.0    54      842   06 12 00
06 16 00  ---          15 50 01  39.3  60.3 -4.2     -80.6   240      873   06 12 01

06 17 00  2013+370     15 51 01  35.7  63.9 -4.4     -76.0    45      873   06 17 00
06 19 00  ---          15 53 01  36.1  64.0 -4.4     -76.2   120      889   06 17 01

06 20 00  CYG-A        15 54 02  40.1  60.4 -4.1     -81.1    45      889   06 20 00
06 32 00  ---          16 06 04  42.3  60.8 -3.9     -82.8   720      982   06 20 01

06 33 00  CYG-A        16 07 04  42.5  60.9 -3.9     -83.0    54      982   06 33 00
06 37 00  ---          16 11 04  43.3  61.0 -3.8     -83.6   240     1013   06 33 01

06 38 00  2013+370     16 12 05  39.8  65.1 -4.1     -78.5    45     1013   06 38 00
06 40 00  ---          16 14 05  40.2  65.2 -4.0     -78.7   120     1028   06 38 01

06 41 00  CYG-A        16 15 05  44.0  61.1 -3.7     -84.1    45     1028   06 41 00
06 53 00  ---          16 27 07  46.3  61.4 -3.5     -85.9   720     1121   06 41 01

06 54 00  CYG-A        16 28 07  46.5  61.4 -3.5     -86.0    54     1121   06 54 00
06 58 00  ---          16 32 08  47.2  61.5 -3.5     -86.6   240     1152   06 54 01

06 59 00  2013+370     16 33 08  43.9  66.1 -3.7     -81.0    45     1152   06 59 00
07 01 00  ---          16 35 08  44.3  66.1 -3.7     -81.2   120     1167   06 59 01

07 02 00  CYG-A        16 36 08  48.0  61.5 -3.4     -87.3    45     1167   07 02 00
07 14 00  ---          16 48 10  50.3  61.6 -3.2     -89.1   720     1260   07 02 01

07 15 00  CYG-A        16 49 11  50.5  61.6 -3.2     -89.3    54     1260   07 15 00
07 19 00  ---          16 53 11  51.2  61.7 -3.1     -89.9   240     1291   07 15 01

07 20 00  2013+370     16 54 11  48.1  66.9 -3.4     -83.6    45     1291   07 20 00
07 22 00  ---          16 56 12  48.5  66.9 -3.3     -83.9   120     1306   07 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

07 23 00  CYG-A        16 57 12  52.0  61.6 -3.0     -90.6    45     1306   07 23 00
07 35 00  ---          17 09 14  54.3  61.5 -2.8     -92.7   720     1399   07 23 01

07 36 00  CYG-A        17 10 14  54.4  61.5 -2.8     -92.8    54     1399   07 36 00
07 40 00  ---          17 14 15  55.2  61.5 -2.8     -93.6   240     1430   07 36 01

07 42 00  BLLAC        17 16 15  32.8  56.7 -4.8     -76.6    68     1430   07 42 00
07 45 00  ---          17 19 16  33.4  56.8 -4.7     -77.0   180     1453   07 42 01

07 47 00  CYG-A        17 21 16  56.5  61.3 -2.6     -94.8    67     1453   07 47 00
07 59 00  ---          17 33 18  58.8  60.8 -2.4     -97.2   720     1546   07 47 01

08 00 00  CYG-A        17 34 18  59.0  60.8 -2.4     -97.4    54     1546   08 00 00
08 04 00  ---          17 38 19  59.7  60.6 -2.4     -98.2   240     1577   08 00 01

08 05 00  2013+370     17 39 19  57.1  67.7 -2.6     -89.8    46     1577   08 05 00
08 07 00  ---          17 41 19  57.5  67.7 -2.6     -90.1   120     1592   08 05 01

08 08 00  CYG-A        17 42 19  60.5  60.4 -2.3     -99.1    46     1592   08 08 00
08 20 00  ---          17 54 21  62.7  59.5 -2.1    -101.8   720     1685   08 08 01

08 21 00  CYG-A        17 55 21  62.9  59.4 -2.1    -102.0    54     1685   08 21 00
08 25 00  ---          17 59 22  63.7  59.0 -2.0    -103.0   240     1716   08 21 01

08 26 00  2013+370     18 00 22  61.3  67.5 -2.3     -93.1    46     1716   08 26 00
08 28 00  ---          18 02 23  61.7  67.5 -2.2     -93.5   120     1731   08 26 01

08 29 00  CYG-A        18 03 23  64.4  58.6 -1.9    -104.0    46     1731   08 29 00
08 41 00  ---          18 15 25  66.6  57.1 -1.7    -107.4   720     1824   08 29 01

08 42 00  CYG-A        18 16 25  66.8  57.0 -1.7    -107.7    54     1824   08 42 00
08 46 00  ---          18 20 26  67.5  56.4 -1.7    -108.9   240     1855   08 42 01

08 47 00  2013+370     18 21 26  65.4  66.7 -1.9     -97.1    45     1855   08 47 00
08 49 00  ---          18 23 26  65.8  66.6 -1.9     -97.5   120     1870   08 47 01

08 50 00  CYG-A        18 24 26  68.2  55.7 -1.6    -110.1    45     1870   08 50 00
09 02 00  ---          18 36 28  70.3  53.3 -1.4    -114.4   720     1963   08 50 01

09 03 00  CYG-A        18 37 28  70.5  53.0 -1.4    -114.8    54     1963   09 03 00
09 07 00  ---          18 41 29  71.2  52.0 -1.3    -116.4   240     1994   09 03 01

09 08 00  2013+370     18 42 29  69.6  64.9 -1.6    -101.9    43     1994   09 08 00
09 10 00  ---          18 44 29  70.0  64.6 -1.5    -102.4   120     2010   09 08 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

09 11 00  CYG-A        18 45 30  71.8  50.9 -1.2    -118.1    43     2010   09 11 00
09 23 00  ---          18 57 32  73.8  47.0 -1.0    -123.8   720     2102   09 11 01

09 24 00  CYG-A        18 58 32  74.0  46.6 -1.0    -124.4    54     2102   09 24 00
09 28 00  ---          19 02 32  74.6  45.0 -1.0    -126.6   240     2133   09 24 01

09 31 00  BLLAC        19 05 33  52.9  59.0 -3.0     -93.5   128     2133   09 31 00
09 34 00  ---          19 08 33  53.4  59.0 -2.9     -94.1   180     2156   09 31 01

09 37 00  2013+370     19 11 34  75.1  59.4 -1.1    -111.5   130     2156   09 37 00
09 39 00  ---          19 13 34  75.5  58.8 -1.0    -112.4   120     2172   09 37 01

09 40 00  CYG-A        19 14 34  76.3  39.1 -0.8    -134.2    38     2172   09 40 00
09 52 00  ---          19 26 36  77.8  31.4 -0.6    -143.7   720     2265   09 40 01

09 53 00  CYG-A        19 27 37  77.9  30.7 -0.5    -144.6    54     2265   09 53 00
09 57 00  ---          19 31 37  78.3  27.6 -0.5    -148.2   240     2296   09 53 01

09 58 00  2013+370     19 32 37  78.8  50.9 -0.7    -123.1    35     2296   09 58 00
10 00 00  ---          19 34 38  79.2  49.7 -0.7    -124.5   120     2311   09 58 01

10 01 00  CYG-A        19 35 38  78.7  24.3 -0.4    -152.1    34     2311   10 01 00
10 13 00  ---          19 47 40  79.6  13.0 -0.2    -165.2   720     2404   10 01 01

10 14 00  CYG-A        19 48 40  79.6  12.0 -0.2    -166.3    54     2404   10 14 00
10 18 00  ---          19 52 41  79.8   7.8 -0.1    -171.1   240     2435   10 14 01

10 19 00  2013+370     19 53 41  81.9  33.6 -0.4    -143.2    33     2435   10 19 00
10 21 00  ---          19 55 41  82.2  31.3 -0.3    -145.9   120     2450   10 19 01

10 22 00  CYG-A        19 56 41  79.8   3.6 -0.1    -175.9    33     2450   10 22 00
10 34 00  ---          20 08 43  79.7  -9.2  0.1     169.5   720     2543   10 22 01

10 35 00  CYG-A        20 09 43  79.7 -10.3  0.2     168.3    54     2543   10 35 00
10 39 00  ---          20 13 44  79.5 -14.4  0.2     163.6   240     2574   10 35 01

10 40 00  2013+370     20 14 44  83.4   2.3 -0.0    -177.5    39     2574   10 40 00
10 42 00  ---          20 16 45  83.4  -1.2  0.0     178.7   120     2589   10 40 01

10 43 00  CYG-A        20 17 45  79.2 -18.3  0.3     159.1    40     2589   10 43 00
10 55 00  ---          20 29 47  78.2 -28.7  0.5     147.0   720     2682   10 43 01

10 56 00  CYG-A        20 30 47  78.1 -29.4  0.5     146.1    54     2682   10 56 00
11 00 00  ---          20 34 48  77.7 -32.4  0.6     142.5   240     2713   10 56 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

11 03 00  BLLAC        20 37 48  69.3  49.7 -1.4    -117.5   113     2713   11 03 00
11 06 00  ---          20 40 49  69.8  48.9 -1.4    -118.7   180     2736   11 03 01

11 09 00  CYG-A        20 43 49  76.5 -38.1  0.7     135.4   111     2736   11 09 00
11 21 00  ---          20 55 51  74.8 -44.3  0.9     127.5   720     2829   11 09 01

11 23 00  2013+370     20 57 51  79.1 -49.9  0.7     124.3   103     2829   11 23 00
11 25 00  ---          20 59 52  78.8 -51.0  0.7     122.8   120     2844   11 23 01

11 27 00  CYG-A        21 01 52  73.9 -46.7  1.0     124.2   103     2844   11 27 00
11 39 00  ---          21 13 54  72.0 -50.8  1.2     118.4   720     2937   11 27 01

11 40 00  2013+370     21 14 54  76.2 -57.6  1.0     114.1    43     2937   11 40 00
11 42 00  ---          21 16 54  75.8 -58.3  1.0     113.2   120     2953   11 40 01

11 43 00  CYG-A        21 17 55  71.3 -51.9  1.3     116.7    43     2953   11 43 00
11 55 00  ---          21 29 57  69.2 -54.6  1.5     112.1   720     3045   11 43 01

11 56 00  2013+370     21 30 57  73.2 -61.9  1.2     107.5    44     3045   11 56 00
11 58 00  ---          21 32 57  72.8 -62.3  1.3     106.9   120     3061   11 56 01

12 00 00  CYG-A        21 34 57  68.3 -55.6  1.6     110.4   104     3061   12 00 00
12 06 00  ---          21 40 58  67.2 -56.6  1.7     108.5   360     3107   12 00 01

12 07 00  2013+370     21 41 59  71.1 -63.9  1.4     104.0    44     3107   12 07 00
12 09 00  ---          21 43 59  70.7 -64.2  1.5     103.5   120     3123   12 07 01

12 10 00  CYG-A        21 44 59  66.5 -57.2  1.7     107.3    44     3123   12 10 00
12 22 00  ---          21 57 01  64.3 -58.7  1.9     104.0   720     3215   12 10 01

12 23 00  2013+370     21 58 01  67.9 -65.8  1.7      99.8    45     3215   12 23 00
12 25 00  ---          22 00 02  67.5 -65.9  1.7      99.4   120     3231   12 23 01

12 26 00  CYG-A        22 01 02  63.6 -59.1  2.0     102.9    45     3231   12 26 00
12 30 00  ---          22 05 02  62.9 -59.4  2.1     102.0   240     3262   12 26 01

12 31 00  2013+370     22 06 02  66.4 -66.4  1.8      98.0    45     3262   12 31 00
12 33 00  ---          22 08 03  66.0 -66.5  1.9      97.6   120     3277   12 31 01

12 34 00  CYG-A        22 09 03  62.1 -59.8  2.2     101.0    45     3277   12 34 00
12 46 00  ---          22 21 05  59.9 -60.5  2.4      98.4   720     3370   12 34 01

12 47 00  2013+370     22 22 05  63.2 -67.2  2.1      94.8    45     3370   12 47 00
12 49 00  ---          22 24 05  62.8 -67.3  2.1      94.5   120     3385   12 47 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

12 50 00  CYG-A        22 25 06  59.1 -60.8  2.4      97.5    45     3385   12 50 00
13 02 00  ---          22 37 08  56.8 -61.2  2.6      95.2   720     3478   12 50 01

13 03 00  2013+370     22 38 08  60.0 -67.6  2.4      92.1    45     3478   13 03 00
13 05 00  ---          22 40 08  59.6 -67.7  2.4      91.7   120     3494   13 03 01

13 06 00  CYG-A        22 41 08  56.1 -61.3  2.7      94.4    45     3494   13 06 00
13 18 00  ---          22 53 10  53.8 -61.6  2.9      92.3   720     3586   13 06 01

13 19 00  2013+370     22 54 10  56.8 -67.7  2.6      89.6    46     3586   13 19 00
13 21 00  ---          22 56 11  56.4 -67.7  2.7      89.3   120     3602   13 19 01

13 22 00  CYG-A        22 57 11  53.1 -61.6  3.0      91.6    46     3602   13 22 00
13 34 00  ---          23 09 13  50.8 -61.7  3.2      89.6   720     3695   13 22 01

13 35 00  2013+370     23 10 13  53.6 -67.6  2.9      87.3    46     3695   13 35 00
13 37 00  ---          23 12 13  53.2 -67.5  2.9      87.0   120     3710   13 35 01

13 38 00  CYG-A        23 13 14  50.0 -61.6  3.2      88.9    46     3710   13 38 00
13 50 00  ---          23 25 15  47.7 -61.5  3.4      87.1   720     3803   13 38 01

13 51 00  BLLAC        23 26 16  69.7 -49.0  1.4     118.5     9     3803   13 51 00
13 54 00  ---          23 29 16  69.2 -49.7  1.4     117.3   180     3826   13 51 01

13 55 00  2013+370     23 30 16  49.6 -67.1  3.2      84.6    14     3826   13 55 00
13 57 00  ---          23 32 17  49.2 -67.0  3.3      84.3   120     3841   13 55 01

13 58 00  CYG-A        23 33 17  46.2 -61.4  3.6      85.8    46     3841   13 58 00
14 10 00  ---          23 45 19  44.0 -61.1  3.8      84.1   720     3934   13 58 01

14 11 00  2013+370     23 46 19  46.5 -66.6  3.5      82.6    47     3934   14 11 00
14 13 00  ---          23 48 19  46.1 -66.5  3.5      82.3   120     3950   14 11 01

14 14 00  CYG-A        23 49 19  43.2 -61.0  3.8      83.5    47     3950   14 14 00
14 26 00  ---          00 01 21  40.9 -60.6  4.0      81.8   720     4042   14 14 01

14 27 00  2013+370     00 02 22  43.3 -65.9  3.8      80.6    47     4042   14 27 00
14 29 00  ---          00 04 22  42.9 -65.8  3.8      80.4   120     4058   14 27 01

14 30 00  CYG-A        00 05 22  40.2 -60.4  4.1      81.2    47     4058   14 30 00
14 42 00  ---          00 17 24  37.9 -60.0  4.3      79.6   720     4151   14 30 01

14 43 00  2013+370     00 18 24  40.2 -65.1  4.0      78.7    47     4151   14 43 00
14 45 00  ---          00 20 25  39.8 -65.0  4.1      78.4   120     4166   14 43 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

14 46 00  CYG-A        00 21 25  37.2 -59.8  4.4      79.0    47     4166   14 46 00
14 58 00  ---          00 33 27  35.0 -59.2  4.6      77.4   720     4259   14 46 01

14 59 00  BLLAC        00 34 27  57.8 -58.1  2.5      98.8     7     4259   14 59 00
15 02 00  ---          00 37 27  57.2 -58.2  2.6      98.2   180     4282   14 59 01

15 03 00  CYG-A        00 38 27  34.0 -58.9  4.6      76.7     6     4282   15 03 00
15 15 00  ---          00 50 29  31.8 -58.3  4.8      75.1   720     4375   15 03 01

15 16 00  2013+370     00 51 30  33.7 -63.3  4.6      74.8    48     4375   15 16 00
15 18 00  ---          00 53 30  33.4 -63.1  4.6      74.6   120     4390   15 16 01

15 19 00  CYG-A        00 54 30  31.1 -58.0  4.9      74.6    48     4390   15 19 00
15 31 00  ---          01 06 32  28.9 -57.3  5.1      73.0   720     4483   15 19 01

15 32 00  2013+370     01 07 32  30.7 -62.2  4.9      72.9    48     4483   15 32 00
15 34 00  ---          01 09 33  30.3 -62.1  4.9      72.7   120     4498   15 32 01

15 35 00  CYG-A        01 10 33  28.2 -57.1  5.2      72.5    48     4498   15 35 00
15 47 00  ---          01 22 35  26.0 -56.3  5.4      70.9   720     4591   15 35 01

15 48 00  2013+370     01 23 35  27.6 -61.1  5.1      71.1    48     4591   15 48 00
15 50 00  ---          01 25 35  27.3 -60.9  5.2      70.8   120     4607   15 48 01

15 51 00  CYG-A        01 26 35  25.3 -56.0  5.4      70.3    48     4607   15 51 00
16 03 00  ---          01 38 37  23.2 -55.1  5.6      68.7   720     4699   15 51 01

16 04 00  BLLAC        01 39 37  45.8 -59.1  3.6      87.0     7     4699   16 04 00
16 07 00  ---          01 42 38  45.2 -59.0  3.7      86.5   180     4723   16 04 01

16 08 00  CYG-A        01 43 38  22.3 -54.7  5.7      68.1     7     4723   16 08 00
16 20 00  ---          01 55 40  20.2 -53.8  5.9      66.4   720     4815   16 08 01

16 21 00  2013+370     01 56 40  21.5 -58.5  5.7      67.1    49     4815   16 21 00
16 23 00  ---          01 58 41  21.1 -58.3  5.7      66.9   120     4831   16 21 01

16 24 00  CYG-A        01 59 41  19.5 -53.5  6.0      65.9    49     4831   16 24 00
16 36 00  ---          02 11 43  17.4 -52.4  6.2      64.2   720     4923   16 24 01

16 37 00  2013+370     02 12 43  18.6 -57.1  5.9      65.2    49     4923   16 37 00
16 39 00  ---          02 14 43  18.2 -56.9  6.0      64.9   120     4939   16 37 01

16 40 00  CYG-A        02 15 43  16.8 -52.1  6.3      63.7    49     4939   16 40 00
16 52 00  ---          02 27 45  14.7 -51.0  6.5      62.0   720     5032   16 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Global 7mm VLBI observations of Cygnus A
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat  30 May 2015   Day 150 ---

16 53 00  2013+370     02 28 46  15.7 -55.7  6.2      63.2    49     5032   16 53 00
16 55 00  ---          02 30 46  15.3 -55.5  6.2      62.9   120     5047   16 53 01

16 56 00  CYG-A        02 31 46  14.1 -50.6  6.5      61.5    49     5047   16 56 00
17 08 00  ---          02 43 48  12.1 -49.5  6.7      59.8   720     5140   16 56 01

17 09 00  BLLAC        02 44 48  33.9 -56.9  4.7      77.4     9     5140   17 09 00
17 12 00  ---          02 47 49  33.3 -56.8  4.7      76.9   180     5163   17 09 01

17 13 00  CYG-A        02 48 49  11.3 -49.0  6.8      59.0     9     5163   17 13 00
17 25 00  ---          03 00 51   9.3 -47.8  7.0      57.3   720     5256   17 13 01

17 26 00  2013+370     03 01 51   9.9 -52.4  6.8      58.9    49     5256   17 26 00
17 28 00  ---          03 03 51   9.6 -52.2  6.8      58.6   120     5271   17 26 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: /home/bboccardi/SCHED/setups/sess215QGglob.setini
   Matching groups in /home/bboccardi/SCHED/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:    6         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   9  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43114.25  43114.25  43146.25  43146.25  43178.25  43178.25  43210.25  43210.25
   BBC fr=     714.25    714.25    746.25    746.25    778.25    778.25    810.25    810.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.25    754.25    786.25    786.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   9  10  11  12  13  14  15  16  17  18

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J1959+4044        19 57 44.453094   * 19 59 28.368821     20 00 01.808078     167.68
 * CYG-A             40 35 46.31273    * 40 44 02.04732      40 46 32.26396      120.15
   CYGNUS-A          /home/bboccardi/SCHED/catalogs/sources.vlba
   J1959+40          rfc_2012b Petrov, 2012, unpublished 3 observations
   1957+405
   1957+404

   J2015+3710        20 13 37.014489   * 20 15 28.729775     20 16 04.428858       0.16
 * 2013+370          37 01 44.45943    * 37 10 59.51531      37 13 47.83264        0.16
                     /home/bboccardi/SCHED/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 282 observations

   J2202+4216        22 00 39.362504   * 22 02 43.291371     22 03 22.344030       0.14
 * BLLAC             42 02 08.59073    * 42 16 39.97987      42 20 58.91182        0.10
   2200+420          /home/bboccardi/SCHED/catalogs/sources.vlba
   J2202+42          rfc_2012b Petrov, 2012, unpublished 59418 observations
   VR422201



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  CYG-A      /sess215QGglob.setini 1 2 3 4 5 6 9                    13.667   868.267
  2013+370   /sess215QGglob.setini 1 2 3 4 5 6 9                     1.867   116.733
  BLLAC      /sess215QGglob.setini 1 2 3 4 5 6 9                     0.650    37.700


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   CYG-A              100.4
   2013+370           100.2
   BLLAC               79.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

