  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg079d  


Schedule Version:       1.10
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez, Andrei Lobanov

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

 ---------- K-band VLBI scans. Space segment 01: 1641+399 ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00

12 00 00  1641+399     19 55 26  50.2 -63.2  3.2      87.9     0        0   12 00 00
12 10 00  ---          20 05 28  48.3 -63.1  3.4      86.4   600       39   12 00 01

12 10 30  1641+399     20 05 58  48.2 -63.0  3.4      86.4    24       39   12 10 30
12 20 00  ---          20 15 30  46.4 -62.8  3.5      85.0   570       75   12 10 31

12 20 30  1641+399     20 16 00  46.3 -62.8  3.5      84.9    24       75   12 20 30
12 30 00  ---          20 25 31  44.5 -62.6  3.7      83.6   570      112   12 20 31

12 30 30  1641+399     20 26 01  44.4 -62.6  3.7      83.5    24      112   12 30 30
12 40 00  ---          20 35 33  42.6 -62.2  3.9      82.2   570      149   12 30 31

12 40 30  1641+399     20 36 03  42.5 -62.2  3.9      82.1    24      149   12 40 30
12 50 00  ---          20 45 34  40.7 -61.9  4.0      80.9   570      185   12 40 31

12 50 30  1641+399     20 46 05  40.6 -61.8  4.0      80.8    24      185   12 50 30
13 00 00  ---          20 55 36  38.8 -61.4  4.2      79.5   570      222   12 50 31

13 04 00  3C454.3      20 59 37  60.1 112.2 -1.9     -56.1   109      222   13 04 00
13 06 00  ---          21 01 37  60.5 112.7 -1.9     -55.8   120      230   13 04 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

13 06 30  3C454.3      21 02 07  60.6 112.8 -1.9     -55.7    24      230   13 06 30
13 10 00  ---          21 05 38  61.2 113.8 -1.8     -55.1   210      243   13 06 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

13 10 30  3C454.3      21 06 08  61.3 114.0 -1.8     -55.0    24      243   13 10 30
13 12 30  ---          21 08 08  61.7 114.5 -1.8     -54.6   120      251   13 10 31

13 15 00  1641+399     21 10 39  35.9 -60.7  4.5      77.6    17      251   13 15 00
13 18 30  ---          21 14 09  35.3 -60.5  4.5      77.1   210      265   13 15 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

13 19 00  1641+399     21 14 39  35.2 -60.5  4.5      77.0    24      265   13 19 00
13 24 30  ---          21 20 10  34.1 -60.2  4.6      76.3   330      286   13 19 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

13 25 30  1641+399     21 21 10  34.0 -60.2  4.6      76.2    54      286   13 25 30
13 33 30  ---          21 29 12  32.5 -59.7  4.8      75.2   480      317   13 25 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

13 34 30  1641+399     21 30 12  32.3 -59.6  4.8      75.0    54      317   13 34 30
13 38 00  ---          21 33 42  31.6 -59.4  4.8      74.6   210      330   13 34 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

13 38 30  1641+399     21 34 12  31.5 -59.4  4.8      74.5    24      330   13 38 30
13 44 00  ---          21 39 43  30.5 -59.1  4.9      73.8   330      352   13 38 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

13 45 30  1641+399     21 41 14  30.2 -59.0  5.0      73.6    84      352   13 45 30
13 54 30  ---          21 50 15  28.6 -58.4  5.1      72.5   540      386   13 45 31

13 55 00  1641+399     21 50 45  28.5 -58.4  5.1      72.4    24      386   13 55 00
14 03 30  ---          21 59 17  26.9 -57.8  5.3      71.3   510      419   13 55 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

14 04 30  1641+399     22 00 17  26.8 -57.7  5.3      71.2    54      419   14 04 30
14 08 00  ---          22 03 47  26.1 -57.5  5.3      70.7   210      433   14 04 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

14 08 30  1641+399     22 04 17  26.0 -57.4  5.3      70.6    24      433   14 08 30
14 14 00  ---          22 09 48  25.0 -57.0  5.4      69.9   330      454   14 08 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

14 15 00  1641+399     22 10 48  24.8 -57.0  5.5      69.8    54      454   14 15 00
14 23 30  ---          22 19 20  23.3 -56.3  5.6      68.7   510      487   14 15 01

14 24 00  1641+399     22 19 50  23.2 -56.3  5.6      68.6    24      487   14 24 00
14 33 30  ---          22 29 21  21.5 -55.5  5.8      67.4   570      524   14 24 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

14 34 00  1641+399     22 29 52  21.4 -55.5  5.8      67.3    24      524   14 34 00
14 43 30  ---          22 39 23  19.8 -54.7  5.9      66.1   570      560   14 34 01

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

14 45 00  1641+399     22 40 53  19.5 -54.6  6.0      65.9    84      560   14 45 00
14 48 30  ---          22 44 24  18.9 -54.3  6.0      65.4   210      574   14 45 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

14 49 00  1641+399     22 44 54  18.8 -54.3  6.0      65.3    24      574   14 49 00
14 54 30  ---          22 50 25  17.8 -53.8  6.1      64.6   330      595   14 49 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

14 55 30  1641+399     22 51 25  17.7 -53.7  6.1      64.5    54      595   14 55 30
15 04 00  ---          22 59 56  16.2 -53.0  6.3      63.3   510      628   14 55 31

15 04 30  1641+399     23 00 27  16.1 -52.9  6.3      63.3    24      628   15 04 30
15 14 00  ---          23 09 58  14.5 -52.0  6.4      62.0   570      665   15 04 31

15 14 30  1641+399     23 10 28  14.4 -52.0  6.4      61.9    24      665   15 14 30
15 24 00  ---          23 20 00  12.8 -51.1  6.6      60.6   570      701   15 14 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

15 28 00  3C454.3      23 24 00  74.1 206.5  0.5      23.6    49      701   15 28 00
15 30 00  ---          23 26 01  73.9 208.1  0.5      25.0   120      709   15 28 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

15 30 30  3C454.3      23 26 31  73.9 208.5  0.5      25.3    24      709   15 30 30
15 34 00  ---          23 30 01  73.5 211.2  0.6      27.7   210      723   15 30 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

15 34 30  3C454.3      23 30 31  73.4 211.6  0.6      28.0    24      723   15 34 30
15 37 00  ---          23 33 02  73.2 213.4  0.6      29.6   150      732   15 34 31

15 38 00  1641+399     23 34 02  10.5 310.3  6.8      58.6   -72      732   15 39 12
15 47 30  ---          23 43 34   8.9 311.3  7.0      57.3   498      764   15 38 01

15 48 00  1641+399     23 44 04   8.8 311.3  7.0      57.2    24      764   15 48 00
15 57 30  ---          23 53 35   7.3 312.4  7.2      55.8   570      801   15 48 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

15 58 00  1641+399     23 54 05   7.2 312.4  7.2      55.7    24      801   15 58 00
16 06 00  ---          00 02 07   6.0 313.3  7.3      54.6   480      832   15 58 01

16 06 30  1641+399     00 02 37   5.9 313.4  7.3      54.5    24      832   16 06 30
16 19 00  ---          00 15 09   3.9 314.8  7.5  H   52.6     0      880   16 06 31

 ---------- K-band VLBI scans. Space segment 02: 1641+399 ----------

16 20 00  1641+399     00 16 09   3.8 314.9  7.5  H   52.5    54      880   16 20 00
16 30 00  ---          00 26 11   2.3 316.1  7.7  H   50.9     0      919   16 20 01

 ---------- VLBA scans on PA calibrator, good also as FF ----------

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

17 21 00  3C454.3      01 17 19  54.5 254.3  2.4      59.6  2930      919   17 21 00
17 23 00  ---          01 19 19  54.1 254.7  2.4      59.8   120      927   17 21 01

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

17 23 30  3C454.3      01 19 49  54.0 254.8  2.4      59.9    24      927   17 23 30
17 27 00  ---          01 23 20  53.2 255.5  2.5      60.2   210      940   17 23 31

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

17 27 30  3C454.3      01 23 50  53.1 255.6  2.5      60.2    24      940   17 27 30
17 30 00  ---          01 26 20  52.6 256.1  2.5      60.5   150      950   17 27 31

 ---------- VLBA on calibrators until end of the experiment ----------

17 30 30  3C84         01 26 51  64.7 416.6 -1.9    -106.3   -92      950   17 32 02
17 40 00  ---          01 36 22  66.4 415.2 -1.7    -109.1   478      981   17 30 31

17 40 30  NRAO150      01 36 52  56.5 402.1 -2.4    -113.6     3      981   17 40 30
17 50 00  ---          01 46 24  57.9 400.9 -2.2    -116.4   570     1017   17 40 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

17 50 30  3C84         01 46 54  68.2 413.4 -1.6    -112.5     2     1017   17 50 30
18 00 00  ---          01 56 25  69.8 411.4 -1.4    -116.0   570     1054   17 50 31

18 00 30  NRAO150      01 56 55  59.4 399.4 -2.1    -119.8     1     1054   18 00 30
18 10 00  ---          02 06 27  60.6 397.8 -1.9    -123.0   570     1091   18 00 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

18 10 30  3C84         02 06 57  71.6 408.6 -1.2    -120.4     1     1091   18 10 30
18 20 00  ---          02 16 29  73.1 405.4 -1.1    -125.0   570     1128   18 10 31

18 20 30  NRAO150      02 16 59  62.0 395.9 -1.7    -126.7     0     1128   18 20 30
18 30 00  ---          02 26 30  63.2 393.8 -1.6    -130.4   570     1164   18 20 31

 ---------- VLBA on calibrators until end of the experiment ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

18 30 30  3C84         02 27 00  74.6 401.0 -0.9    -131.0    -1     1164   18 30 31
18 40 00  ---          02 36 32  75.9 396.2 -0.7    -137.3   569     1201   18 30 31

18 40 30  NRAO150      02 37 02  64.4 391.3 -1.4    -134.7    -1     1201   18 40 31
18 50 00  ---          02 46 34  65.4 388.7 -1.2    -138.9   569     1238   18 40 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

18 50 30  3C84         02 47 04  77.1 389.6 -0.6    -145.4    -1     1238   18 50 31
19 00 00  ---          02 56 35  78.0 382.4 -0.4    -154.0   569     1274   18 50 31

19 00 30  NRAO150      02 57 05  66.5 385.6 -1.1    -143.8    -1     1274   19 00 31
19 10 00  ---          03 06 37  67.3 382.4 -0.9    -148.6   569     1311   19 00 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

19 10 30  3C84         03 07 07  78.7 373.3 -0.2    -164.7    -1     1311   19 10 31
19 20 00  ---          03 16 39  79.0 364.1 -0.1    -175.2   569     1348   19 10 31

19 20 30  NRAO150      03 17 09  68.1 378.6 -0.7    -154.2     0     1348   19 20 30
19 30 00  ---          03 26 40  68.7 374.8 -0.6    -159.5   570     1384   19 20 31

 ---------- VLBA on calibrators until end of the experiment ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

19 30 30  3C84         03 27 10  79.0 353.8  0.1     172.9     2     1384   19 30 30
19 40 00  ---          03 36 42  78.6 344.8  0.3     162.5   570     1421   19 30 31

19 40 30  NRAO150      03 37 12  69.2 370.4 -0.4    -165.7     3     1421   19 40 30
19 50 00  ---          03 46 43  69.5 366.3 -0.2    -171.4   570     1458   19 40 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

19 50 30  3C84         03 47 14  77.8 335.9  0.4     152.0     1     1458   19 50 30
20 00 00  ---          03 56 45  76.9 329.0  0.6     143.7   570     1494   19 50 31

20 00 30  NRAO150      03 57 15  69.6 361.6 -0.1    -177.9    -1     1494   20 00 31
20 10 00  ---          04 06 47  69.6 357.3  0.1     176.2   569     1531   20 00 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

20 10 30  3C84         04 07 17  75.6 322.7  0.8     135.8    -2     1531   20 10 32
20 20 00  ---          04 16 48  74.3 318.0  0.9     129.7   568     1568   20 10 31

20 20 30  NRAO150      04 17 18  69.4 352.6  0.3     169.8    -2     1568   20 20 32
20 30 00  ---          04 26 50  69.1 348.4  0.4     164.1   568     1604   20 20 31

 ---------- VLBA on calibrators until end of the experiment ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

20 30 30  3C84         04 27 20  72.7 313.9  1.1     124.0    -2     1604   20 30 32
20 40 00  ---          04 36 52  71.2 310.8  1.3     119.5   568     1641   20 30 31

20 40 30  NRAO150      04 37 22  68.5 344.1  0.6     158.0    -2     1641   20 40 32
20 50 00  ---          04 46 53  67.9 340.4  0.8     152.8   568     1677   20 40 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

20 50 30  3C84         04 47 23  69.5 308.1  1.4     115.2    -1     1677   20 50 31
21 00 00  ---          04 56 55  67.8 306.2  1.6     111.8   569     1714   20 50 31

21 00 30  NRAO150      04 57 25  67.1 336.7  0.9     147.2     0     1714   21 00 30
21 10 00  ---          05 06 57  66.2 333.6  1.1     142.6   570     1751   21 00 31

 Next scan frequencies:  43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
 Next BBC frequencies:     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25

21 10 30  3C84         05 07 27  66.0 304.4  1.8     108.5     1     1751   21 10 30
21 20 00  ---          05 16 58  64.3 303.2  1.9     105.8   570     1787   21 10 31

21 20 30  NRAO150      05 17 28  65.1 330.5  1.3     137.7     3     1787   21 20 30
21 30 00  ---          05 27 00  64.1 328.0  1.4     133.6   570     1824   21 20 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   4 May 2016   Day 125 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00

21 30 30  3C84         05 27 30  62.4 302.1  2.1     103.0     4     1824   21 30 30
21 40 00  ---          05 37 02  60.6 301.3  2.3     100.8   570     1861   21 30 31

21 40 30  NRAO150      05 37 32  62.9 325.6  1.6     129.3     5     1861   21 40 30
21 50 00  ---          05 47 03  61.7 323.6  1.8     125.8   570     1898   21 40 31

 Next scan frequencies:  15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00

21 50 30  3C84         05 47 33  58.7 300.7  2.4      98.5     6     1898   21 50 30
21 55 00  ---          05 52 04  57.9 300.5  2.5      97.5   270     1915   21 50 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg079d_freq.dat:
     v1cm_b3

   Setup group:    8         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   2  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22236.00  22236.00  22236.00  22236.00  22268.00  22268.00  22268.00  22268.00
   BBC fr=     736.00    736.00    736.00    736.00    768.00    768.00    768.00    768.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     735.99    735.99    768.01    768.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   2   3   4   5   6   7   8   9  10  11

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg079d_freq.dat:
     v7mm_c8

   Setup group:   46         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  29  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43130.25  43130.25  43130.25  43130.25  43162.25  43162.25  43162.25  43162.25
   BBC fr=     730.25    730.25    730.25    730.25    762.25    762.25    762.25    762.25
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     730.25    730.25    762.25    762.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  29  30  31  32  33  34  35  36  37  38

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg079d_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   36         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U         L         L         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  39  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15337.00  15337.00  15369.00  15369.00  15369.00  15369.00
   BBC fr=     737.00    737.00    737.00    737.00    769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00     16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     736.99    736.99    769.01    769.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  39  40  41  42  43  44  45  46  47  48

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 52.931641       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 47.83533        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

   0316+413          03 16 29.567283   * 03 19 48.160114     03 20 51.478442       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 00.64304        0.00
 * 3C84              ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

   0355+508          03 55 45.261370   * 03 59 29.747271     04 00 41.281703       0.00
   J0359+5057        50 49 20.28584    * 50 57 50.16179      51 00 24.99723        0.00
 * NRAO150           ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 19270 observations, RA-AO3-04, RA-AO2-1

 * 0552+398          05 52 01.407174   * 05 55 30.805616     05 56 37.626233       0.00
   J0555+3948        39 48 21.94579    * 39 48 49.16494      39 48 49.71446        0.00
                     ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 392026 observations, RA-AO3-04, RA-AO2-

 * 0642+449          06 42 53.021453   * 06 46 32.026000     06 47 41.964830       0.00
   J0646+4451        44 54 30.82735    * 44 51 16.59010      44 50 08.47437        0.00
                     ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 129725 observations, RA-AO3-04, RA-AO2-

 * 1641+399          16 41 17.606226   * 16 42 58.809963     16 43 33.055616       0.00
   J1642+3948        39 54 10.81479    * 39 48 36.99385      39 46 48.81080        0.00
   3C345             ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 51938 observations, RA-AO3-04, RA-AO3-0

   2251+158          22 51 29.519741   * 22 53 57.747940     22 54 45.464296       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 13 57.99014        0.00
 * 3C454.3           ./gg079d_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO3-04, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            15                                3.192     0.000
  3C84       ra1cm2.set            2                                 0.792    33.749
             ra2cm2.set            39                                0.708    31.047
             ra7mm2.set            29                                0.633    27.862
  NRAO150    ra1cm2.set            2                                 0.792    34.789
             ra2cm2.set            39                                0.633    27.793
             ra7mm2.set            29                                0.633    27.943
  0552+398   ra1cm2.set            16 17 18 19 20 21 22 23 24  +     3.008   112.002
  0642+449   ra1cm2.set            16 17 18 19 20 21 22 23 24  +     3.008   121.492
  1641+399   ra1cm2.set            1 2 12 16 18 19 20 21 22 23 +     9.317   815.607
             ra2cm2.set            39                                0.233     8.400
             ra7mm2.set            29 49                             1.358    16.175
  3C454.3    ra1cm2.set            2                                 0.117     5.250
             ra2cm2.set            39                                0.100     4.169
             ra7mm2.set            29                                0.175     7.875


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              77.6
   3C84                26.3
   NRAO150             37.6
   0552+398            47.0
   0642+449            57.3
   1641+399           117.9
   3C454.3             56.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

