!*  Schedule for VLBA_FD   *!
!*  Experiment GV016    *!
!* Schedule Version:       1.01 *!
!* Processed by SCHED version: Release of 02 July 2002 *!
!* PI:       Rene Vermeulen *!
!* Address:  ASTRON/NFRA *!
!*           P.O. Box 2 *!
!*           NL-7990 AA Dwingeloo *!
!*           The Netherlands *!
!* Phone:    +31 (521) 595 262 *!
!* EMAIL:    rvermeulen@nfra.nl *!
!* Fax:      +31 (521) 597 332 *!
!* Phone during observation: as above or +31 (528) 232612 (home) *!
!* Observing mode: 128 Mb/s, 4x 8 MHz BBC: RCP+LCP OH1665+7 and OH1720 lines *!
!* Notes:    PHASE CAL must be OFF *!
!*  *!
!*  *!
!*  *!
!*  Start at 23h27m00s     Mon, 2002 Nov 18  Day of year  322   *!
program=GV016   
autoallocate=off
autoreverse=off

!* The first scan is preceeded by a setup scan *!
!* that ends at the start time of the first scan  *!
!* ========= New tape starts at: 23h31m00s ========= *!

!* --- Scan from 23h31m00s to 23h42m00s   Mon, 2002 Nov 18 --- *!
sname='3C454.3'  ra=22h53m57.747931s  dec= 16d08'53.56097"  qual=999  calib=' '
maxcaltime= 120
fe=(1,20cm),(3,20cm)
fexfer=(2,norm)
noise=(1,low-s),(2,low-s),(3,low-s),(4,low-s)
synth=( 1,15.4),( 2, 2.4),( 3,15.4)
logging=STANDARD
nchan= 4
format=VLBA1:4
barrel=roll_off
ifdistr=(1,0),(2,0),(3,0),(4,0)
baseband=(1,1),(2,2),(3,3),(4,4)
ifchan=(1,A),(2,C),(3,A),(4,C)
sideband=(1,L),(2,L),(3,L),(4,L)
bits=(1,2),(2,2),(3,2),(4,2)
period=(1,1),(2,1),(3,1),(4,1)
level=(1,-1),(2,-1),(3,-1),(4,-1)
azcolim=   0.00  elcolim=   0.00
bbsynth=( 1,746.39),( 2,746.39),( 3,692.52),( 4,692.52)
bbfilter=(1,8M),(2,8M),(3,8M),(4,8M)
pcal=OFF
pcalxbit1=(1,S1),(2,S2),(3,S3),(4,S4),(5,OFF),(6,OFF),(7,OFF),(8,OFF)
pcalxbit2=(1,M1),(2,M2),(3,M3),(4,M4),(5,OFF),(6,OFF),(7,OFF),(8,OFF)
pcalxfreq1=(1,0),(2,0),(3,0),(4,0),(5,0),(6,0),(7,0),(8,0)
pcalxfreq2=(1,0),(2,0),(3,0),(4,0),(5,0),(6,0),(7,0),(8,0)
samplerate=16M
track=(1,2),(2,18),(3,3),(4,19)
tape=(2,STOP)    write=(2,off) 
tape=( 1,STOP)   write=( 1,off) head=( 1,-319)
  date = 2002Nov18
stop=23h31m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-319) 
stop=23h42m00s   !NEXT!

!* --- Scan from 23h46m00s to 00h19m00s   Mon, 2002 Nov 18 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-319)
stop=23h46m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-319) 
date=2002Nov19
stop=00h19m00s   !NEXT!

!* --- Scan from 00h23m00s to 00h34m00s   Tue, 2002 Nov 19 --- *!
sname='3C454.3'  ra=22h53m57.747931s  dec= 16d08'53.56097"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,  31)
stop=00h23m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  31) 
stop=00h34m00s   !NEXT!

!* --- Scan from 00h38m00s to 00h49m00s   Tue, 2002 Nov 19 --- *!
sname='3C84'  ra=03h19m48.160092s  dec= 41d30'42.10384"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,  31)
stop=00h38m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  31) 
stop=00h49m00s   !NEXT!

!* --- Scan from 00h52m00s to 01h14m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,  31)
stop=00h52m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  31) 
stop=01h14m00s   !NEXT!

!* --- Scan from 01h16m00s to 02h00m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-271)
stop=01h16m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-271) 
stop=02h00m00s   !NEXT!

!* --- Scan from 02h02m00s to 02h46m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,  79)
stop=02h02m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1,  79) 
stop=02h46m00s   !NEXT!

!* --- Scan from 02h49m00s to 03h22m00s   Tue, 2002 Nov 19 --- *!
sname='3C84'  ra=03h19m48.160092s  dec= 41d30'42.10384"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-223)
stop=02h49m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-223) 
stop=03h22m00s   !NEXT!

!* --- Scan from 03h25m00s to 03h36m00s   Tue, 2002 Nov 19 --- *!
sname='DA193'  ra=05h55m30.805609s  dec= 39d48'49.16500"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-223)
stop=03h25m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-223) 
stop=03h36m00s   !NEXT!

!* --- Scan from 03h39m00s to 04h23m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, 127)
stop=03h39m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 127) 
stop=04h23m00s   !NEXT!

!* --- Scan from 04h25m00s to 05h09m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-175)
stop=04h25m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-175) 
stop=05h09m00s   !NEXT!

!* --- Scan from 05h11m00s to 05h55m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, 175)
stop=05h11m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 175) 
stop=05h55m00s   !NEXT!

!* --- Scan from 05h57m00s to 06h41m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1,-127)
stop=05h57m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1,-127) 
stop=06h41m00s   !NEXT!

!* --- Scan from 06h43m00s to 07h27m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, 223)
stop=06h43m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 223) 
stop=07h27m00s   !NEXT!

!* --- Scan from 07h29m00s to 08h13m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, -79)
stop=07h29m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -79) 
stop=08h13m00s   !NEXT!

!* --- Scan from 08h15m00s to 08h59m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, 271)
stop=08h15m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 271) 
stop=08h59m00s   !NEXT!

!* --- Scan from 09h01m00s to 09h45m00s   Tue, 2002 Nov 19 --- *!
sname='NGC1052'  ra=02h41m04.798288s  dec=-08d15'20.75075"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, -31)
stop=09h01m00s   !NEXT!        
qual=  0
tape=( 1,+RUN)   write=( 1,on)  head=( 1, -31) 
stop=09h45m00s   !NEXT!

!* --- Scan from 09h48m00s to 10h32m00s   Tue, 2002 Nov 19 --- *!
sname='3C84'  ra=03h19m48.160092s  dec= 41d30'42.10384"  qual=999  calib=' '
tape=( 1,STOP)   write=( 1,off) head=( 1, 319)
stop=09h48m00s   !NEXT!        
qual=  0
tape=( 1,-RUN)   write=( 1,on)  head=( 1, 319) 
stop=10h32m00s   !NEXT!

!* =====  UNLOADING DRIVE 1 ==== *!
tape=(1,STOP)    write=(1,off)   dur=0s 
stop=10h32m05s  !NEXT! 
tape=(1,UNLOAD)  stop=10h32m07s
  !NEXT! 
  stop=10h32m11s   !QUIT!
