  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: T Tau S, simultaneous with Chandra
 Exp. Code:  GG049A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       Manuel Guedel                                                   

Address:  Institute of Astronomy                                          
          SEC 7                                                           
          ETHZ                                                            
          Switzerland                                                     

Phone:    ++41-1-632 71 29                                                
EMAIL:    guedel@astro.phys.ethz.ch                                       
Fax:                                                                      
Phone during observation: ++41-1-632 71 29                                

Observing mode: Continuum                                                 

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

 Next scan frequencies:  8399.49  8399.49  8415.49  8415.49
 Next BBC frequencies:    799.49   799.49   815.49   815.49
 Next scan bandwidths:     16.00    16.00    16.00    16.00

03 34 00  TTAUS        22 46 46  14.9  75.8 -5.6     -62.3     0   1  1      0  03 34 00
03 37 00  ---          22 49 46  15.5  76.2 -5.5     -62.4   180   F  1   2400

03 37 00  J0431+1731   22 49 46  12.5  76.9 -5.7     -61.5   -12   1  1   2400  03 37 00
03 39 00  ---          22 51 47  12.9  77.1 -5.7     -61.6   108   F  1   4000

03 39 00  TTAUS        22 51 47  15.9  76.4 -5.5     -62.6   -12   1  1   4000  03 39 00
03 42 40  ---          22 55 27  16.7  76.8 -5.4     -62.7   208   F  1   6933

03 42 40  J0431+1731   22 55 27  13.7  77.5 -5.6     -61.8   -12   1  1   6933  03 42 40
03 44 40  ---          22 57 27  14.1  77.8 -5.6     -61.9   108   F  1   8533

03 44 40  TTAUS        22 57 27  17.1  77.0 -5.4     -62.8   -12   1  1   8533  03 44 40
03 48 20  ---          23 01 08  17.9  77.5 -5.4     -63.0   208   F  1  11467

03 48 20  J0431+1731   23 01 08  14.9  78.2 -5.5     -62.0   -12   1  1  11467  03 48 20
03 50 20  ---          23 03 08  15.3  78.4 -5.5     -62.1   108   F  1  13067

03 50 20  TTAUS        23 03 08  18.3  77.7 -5.3     -63.1   -12   1  1  13067  03 50 20
03 54 00  ---          23 06 49  19.1  78.1 -5.3     -63.3   208   F  1  16000

03 54 00  J0431+1731   23 06 49  16.1  78.8 -5.4     -62.3   -12   1  1  16000  03 54 00
03 56 00  ---          23 08 49  16.5  79.1 -5.4     -62.4   108   F  1  17600

03 56 40  J0403+2600   23 09 29  26.3  74.0 -4.9     -67.0    14   1  2  17600  03 56 40
04 01 40  ---          23 14 30  27.4  74.5 -4.8     -67.3   300   R  1  13600

04 01 40  J0431+1731   23 14 30  17.7  79.7 -5.3     -62.6   -25   1  2  13600  04 01 40
04 03 40  ---          23 16 31  18.1  79.9 -5.3     -62.7    95   R  1  12000

04 03 40  TTAUS        23 16 31  21.1  79.2 -5.1     -63.7   -12   1  2  12000  04 03 40
04 06 40  ---          23 19 31  21.8  79.5 -5.0     -63.9   168   R  1   9600

04 06 40  J0431+1731   23 19 31  18.8  80.3 -5.2     -62.8   -12   1  2   9600  04 06 40
04 08 40  ---          23 21 31  19.2  80.5 -5.2     -62.9   108   R  1   8000

04 08 40  TTAUS        23 21 31  22.2  79.7 -5.0     -64.0   -12   1  2   8000  04 08 40
04 11 40  ---          23 24 32  22.8  80.1 -5.0     -64.1   168   R  1   5600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

04 11 40  J0431+1731   23 24 32  19.8  80.9 -5.1     -63.0   -12   1  2   5600  04 11 40
04 13 40  ---          23 26 32  20.3  81.1 -5.1     -63.1   108   R  1   4000

04 13 40  TTAUS        23 26 32  23.3  80.3 -4.9     -64.2   -12   1  2   4000  04 13 40
04 16 40  ---          23 29 33  23.9  80.6 -4.9     -64.3   168   R  1   1600

04 16 40  J0431+1731   23 29 33  20.9  81.4 -5.0     -63.2   -12   1  2   1600  04 16 40
04 18 40  ---          23 31 33  21.3  81.7 -5.0     -63.2   108   R  1      0

04 21 20  J0555+3948   23 34 14  15.3  52.5 -6.4     -62.6   135   1  3      0  04 21 20
04 25 20  =0552+398    23 38 14  16.0  52.8 -6.3     -63.2   240   F  1   3200

04 25 20  J0403+2600   23 38 14  32.3  76.8 -4.4     -68.8   -39   1  3   3200  04 25 20
04 28 20  ---          23 41 15  32.9  77.1 -4.4     -68.9   141   F  1   5600

04 28 20  J0431+1731   23 41 15  23.4  82.8 -4.8     -63.5   -25   1  3   5600  04 28 20
04 30 20  ---          23 43 15  23.8  83.0 -4.8     -63.6    95   F  1   7200

04 30 20  TTAUS        23 43 15  26.8  82.2 -4.6     -64.8   -12   1  3   7200  04 30 20
04 33 50  ---          23 46 46  27.6  82.6 -4.6     -64.9   198   F  1  10000

04 33 50  J0431+1731   23 46 46  24.6  83.4 -4.8     -63.7   -12   1  3  10000  04 33 50
04 35 50  ---          23 48 46  25.0  83.7 -4.7     -63.7   108   F  1  11600

04 35 50  TTAUS        23 48 46  28.0  82.8 -4.6     -64.9   -12   1  3  11600  04 35 50
04 39 20  ---          23 52 16  28.7  83.2 -4.5     -65.0   198   F  1  14400

04 39 20  J0431+1731   23 52 16  25.8  84.1 -4.7     -63.8   -12   1  3  14400  04 39 20
04 41 20  ---          23 54 17  26.2  84.3 -4.6     -63.9   108   F  1  16000

04 41 20  J0403+2600   23 54 17  35.7  78.3 -4.2     -69.7   -25   1  3  16000  04 41 20
04 43 20  ---          23 56 17  36.1  78.5 -4.1     -69.8    95   F  1  17600

04 44 00  J0431+1731   23 56 57  26.8  84.6 -4.6     -63.9    15   1  4  17600  04 44 00
04 46 00  ---          23 58 58  27.2  84.9 -4.6     -64.0   120   R  1  16000

04 46 00  TTAUS        23 58 58  30.2  83.9 -4.4     -65.2   -12   1  4  16000  04 46 00
04 49 40  ---          00 02 38  31.0  84.4 -4.3     -65.3   208   R  1  13067

04 49 40  J0431+1731   00 02 38  28.0  85.3 -4.5     -64.1   -12   1  4  13067  04 49 40
04 51 40  ---          00 04 38  28.4  85.5 -4.5     -64.1   108   R  1  11467
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

04 51 40  TTAUS        00 04 38  31.4  84.6 -4.3     -65.4   -12   1  4  11467  04 51 40
04 55 20  ---          00 08 19  32.2  85.0 -4.2     -65.5   208   R  1   8533

04 55 20  J0431+1731   00 08 19  29.2  86.0 -4.4     -64.2   -12   1  4   8533  04 55 20
04 57 20  ---          00 10 19  29.6  86.2 -4.4     -64.2   108   R  1   6933

04 57 20  TTAUS        00 10 19  32.6  85.3 -4.2     -65.5   -12   1  4   6933  04 57 20
05 01 00  ---          00 14 00  33.4  85.7 -4.1     -65.6   208   R  1   4000

05 01 00  J0431+1731   00 14 00  30.4  86.6 -4.3     -64.3   -12   1  4   4000  05 01 00
05 03 00  ---          00 16 00  30.8  86.9 -4.3     -64.3   108   R  1   2400

05 03 00  J0403+2600   00 16 00  40.3  80.4 -3.8     -70.8   -25   1  4   2400  05 03 00
05 06 00  ---          00 19 01  40.9  80.7 -3.7     -70.9   155   R  1      0

05 16 40  J0431+1731   00 29 43  33.8  88.6 -4.0     -64.4   620   1  5      0  05 16 40
05 18 40  ---          00 31 43  34.2  88.8 -4.0     -64.4   120   F  1   1600

05 18 40  TTAUS        00 31 43  37.2  87.8 -3.8     -65.8   -12   1  5   1600  05 18 40
05 22 20  ---          00 35 24  38.0  88.2 -3.8     -65.9   208   F  1   4533

05 22 20  J0431+1731   00 35 24  35.0  89.3 -3.9     -64.5   -12   1  5   4533  05 22 20
05 24 20  ---          00 37 24  35.4  89.5 -3.9     -64.5   108   F  1   6133

05 24 20  TTAUS        00 37 24  38.4  88.5 -3.7     -65.9   -12   1  5   6133  05 24 20
05 28 00  ---          00 41 04  39.2  88.9 -3.7     -65.9   208   F  1   9067

05 28 00  J0431+1731   00 41 04  36.2  90.0 -3.9     -64.5   -12   1  5   9067  05 28 00
05 30 00  ---          00 43 05  36.7  90.2 -3.8     -64.5   108   F  1  10667

05 30 00  TTAUS        00 43 05  39.6  89.2 -3.7     -65.9   -12   1  5  10667  05 30 00
05 33 40  ---          00 46 45  40.4  89.6 -3.6     -65.9   208   F  1  13600

05 33 40  J0431+1731   00 46 45  37.5  90.7 -3.8     -64.5   -12   1  5  13600  05 33 40
05 35 40  ---          00 48 46  37.9  91.0 -3.7     -64.5   108   F  1  15200

05 35 40  J0403+2600   00 48 46  47.3  83.7 -3.2     -72.1   -25   1  5  15200  05 35 40
05 38 40  ---          00 51 46  47.9  84.0 -3.2     -72.2   155   F  1  17600

05 39 20  J0431+1731   00 52 26  38.7  91.5 -3.7     -64.4    16   1  6  17600  05 39 20
05 41 20  ---          00 54 27  39.1  91.7 -3.6     -64.4   120   R  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

05 41 20  TTAUS        00 54 27  42.1  90.6 -3.5     -65.9   -12   1  6  16000  05 41 20
05 44 20  ---          00 57 27  42.7  91.0 -3.4     -65.9   168   R  1  13600

05 44 20  J0431+1731   00 57 27  39.8  92.1 -3.6     -64.4   -12   1  6  13600  05 44 20
05 46 20  ---          00 59 27  40.2  92.4 -3.5     -64.4   108   R  1  12000

05 46 20  TTAUS        00 59 27  43.2  91.3 -3.4     -65.9   -12   1  6  12000  05 46 20
05 49 20  ---          01 02 28  43.8  91.7 -3.3     -65.9   168   R  1   9600

05 49 20  J0431+1731   01 02 28  40.8  92.8 -3.5     -64.3   -12   1  6   9600  05 49 20
05 51 20  ---          01 04 28  41.3  93.1 -3.5     -64.3   108   R  1   8000

05 51 20  TTAUS        01 04 28  44.2  92.0 -3.3     -65.9   -12   1  6   8000  05 51 20
05 54 20  ---          01 07 29  44.9  92.4 -3.2     -65.8   168   R  1   5600

05 54 20  J0431+1731   01 07 29  41.9  93.5 -3.4     -64.2   -12   1  6   5600  05 54 20
05 56 20  ---          01 09 29  42.3  93.8 -3.4     -64.2   108   R  1   4000

05 56 20  J0555+3948   01 09 29  32.4  59.6 -4.8     -75.1   -29   1  6   4000  05 56 20
06 01 20  =0552+398    01 14 30  33.3  59.9 -4.7     -75.7   271   R  1      0

06 02 00  J0403+2600   01 15 10  52.9  86.5 -2.8     -72.9    -5   1  7      0  06 02 00
06 05 00  ---          01 18 11  53.6  86.8 -2.8     -72.9   175   F  1   2400

06 05 00  J0431+1731   01 18 11  44.2  95.0 -3.2     -64.0   -25   1  7   2400  06 05 00
06 07 00  ---          01 20 11  44.6  95.3 -3.2     -64.0    95   F  1   4000

06 07 00  TTAUS        01 20 11  47.6  94.1 -3.0     -65.6   -12   1  7   4000  06 07 00
06 10 40  ---          01 23 51  48.4  94.7 -3.0     -65.5   208   F  1   6933

06 10 40  J0431+1731   01 23 51  45.4  95.9 -3.1     -63.9   -12   1  7   6933  06 10 40
06 12 40  ---          01 25 52  45.8  96.2 -3.1     -63.8   108   F  1   8533

06 12 40  TTAUS        01 25 52  48.8  95.0 -2.9     -65.5   -12   1  7   8533  06 12 40
06 16 20  ---          01 29 32  49.6  95.5 -2.9     -65.3   208   F  1  11467

06 16 20  J0431+1731   01 29 32  46.6  96.7 -3.0     -63.7   -12   1  7  11467  06 16 20
06 18 20  ---          01 31 33  47.1  97.0 -3.0     -63.6   108   F  1  13067

06 18 20  TTAUS        01 31 33  50.1  95.8 -2.8     -65.3   -12   1  7  13067  06 18 20
06 22 00  ---          01 35 13  50.8  96.4 -2.8     -65.1   208   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

06 22 00  J0431+1731   01 35 13  47.8  97.6 -2.9     -63.4   -12   1  7  16000  06 22 00
06 24 00  ---          01 37 14  48.3  97.9 -2.9     -63.3   108   F  1  17600

06 24 40  J0403+2600   01 37 54  57.8  89.1 -2.4     -73.2    15   1  8  17600  06 24 40
06 27 40  ---          01 40 54  58.4  89.5 -2.4     -73.2   180   R  1  15200

06 27 40  J0431+1731   01 40 54  49.1  98.5 -2.9     -63.2   -25   1  8  15200  06 27 40
06 29 40  ---          01 42 55  49.5  98.9 -2.8     -63.1    95   R  1  13600

06 29 40  TTAUS        01 42 55  52.5  97.6 -2.7     -64.8   -12   1  8  13600  06 29 40
06 33 20  ---          01 46 35  53.3  98.3 -2.6     -64.6   208   R  1  10667

06 33 20  J0431+1731   01 46 35  50.3  99.5 -2.8     -62.9   -12   1  8  10667  06 33 20
06 35 20  ---          01 48 36  50.7  99.8 -2.7     -62.8   108   R  1   9067

06 35 20  TTAUS        01 48 36  53.7  98.6 -2.6     -64.5   -12   1  8   9067  06 35 20
06 39 00  ---          01 52 16  54.5  99.2 -2.5     -64.3   208   R  1   6133

06 39 00  J0431+1731   01 52 16  51.5 100.5 -2.7     -62.5   -12   1  8   6133  06 39 00
06 41 00  ---          01 54 16  51.9 100.8 -2.6     -62.4   108   R  1   4533

06 41 00  TTAUS        01 54 16  54.9  99.6 -2.5     -64.2   -12   1  8   4533  06 41 00
06 44 40  ---          01 57 57  55.7 100.2 -2.4     -64.0   208   R  1   1600

06 44 40  J0431+1731   01 57 57  52.7 101.5 -2.6     -62.2   -12   1  8   1600  06 44 40
06 46 40  ---          01 59 57  53.1 101.9 -2.5     -62.0   108   R  1      0

06 47 20  J0403+2600   02 00 38  62.7  92.1 -2.0     -73.1    15   1  9      0  06 47 20
06 50 20  ---          02 03 38  63.3  92.5 -2.0     -73.0   180   F  1   2400

06 50 20  J0431+1731   02 03 38  53.9 102.5 -2.5     -61.7   -25   1  9   2400  06 50 20
06 52 20  ---          02 05 38  54.3 102.9 -2.4     -61.6    95   F  1   4000

06 52 20  TTAUS        02 05 38  57.3 101.7 -2.3     -63.4   -12   1  9   4000  06 52 20
06 55 20  ---          02 08 39  57.9 102.3 -2.2     -63.1   168   F  1   6400

06 55 20  J0431+1731   02 08 39  54.9 103.5 -2.4     -61.3   -12   1  9   6400  06 55 20
06 57 20  ---          02 10 39  55.3 103.9 -2.4     -61.1   108   F  1   8000

06 57 20  TTAUS        02 10 39  58.4 102.7 -2.2     -63.0   -12   1  9   8000  06 57 20
07 00 20  ---          02 13 40  59.0 103.3 -2.1     -62.7   168   F  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

07 00 20  J0431+1731   02 13 40  56.0 104.5 -2.3     -60.9   -12   1  9  10400  07 00 20
07 02 20  ---          02 15 40  56.4 105.0 -2.3     -60.7   108   F  1  12000

07 02 20  TTAUS        02 15 40  59.4 103.8 -2.1     -62.5   -12   1  9  12000  07 02 20
07 05 20  ---          02 18 40  60.0 104.4 -2.1     -62.2   168   F  1  14400

07 05 20  J0431+1731   02 18 40  57.0 105.6 -2.2     -60.4   -12   1  9  14400  07 05 20
07 07 20  ---          02 20 41  57.4 106.0 -2.2     -60.1   108   F  1  16000

07 07 20  J0357+2319   02 20 41  67.3 102.8 -1.6     -66.0   -26   1  9  16000  07 07 20
07 09 20  ---          02 22 41  67.7 103.3 -1.6     -65.8    94   F  1  17600

07 09 20  J0403+2600   02 22 41  67.4  95.6 -1.7     -72.3   -11   1 10  17600  07 09 20
07 11 20  ---          02 24 41  67.9  95.9 -1.6     -72.2   109   R  1  16000

07 11 20  J0431+1731   02 24 41  58.2 106.9 -2.1     -59.7   -25   1 10  16000  07 11 20
07 13 20  ---          02 26 42  58.7 107.4 -2.1     -59.4    95   R  1  14400

07 13 20  TTAUS        02 26 42  61.7 106.2 -1.9     -61.2   -12   1 10  14400  07 13 20
07 17 00  ---          02 30 22  62.5 107.1 -1.9     -60.7   208   R  1  11467

07 17 00  J0431+1731   02 30 22  59.4 108.3 -2.0     -59.0   -12   1 10  11467  07 17 00
07 19 00  ---          02 32 23  59.8 108.8 -2.0     -58.7   108   R  1   9867

07 19 00  TTAUS        02 32 23  62.9 107.6 -1.8     -60.5   -12   1 10   9867  07 19 00
07 22 40  ---          02 36 03  63.6 108.6 -1.8     -59.9   208   R  1   6933

07 22 40  J0431+1731   02 36 03  60.6 109.7 -1.9     -58.2   -12   1 10   6933  07 22 40
07 24 40  ---          02 38 04  61.0 110.2 -1.9     -57.9   108   R  1   5333

07 24 40  TTAUS        02 38 04  64.0 109.1 -1.7     -59.6   -12   1 10   5333  07 24 40
07 28 20  ---          02 41 44  64.8 110.2 -1.7     -59.0   208   R  1   2400

07 28 20  J0431+1731   02 41 44  61.7 111.2 -1.8     -57.3   -12   1 10   2400  07 28 20
07 30 20  ---          02 43 45  62.1 111.7 -1.8     -56.9   108   R  1    800

07 30 20  J0403+2600   02 43 45  71.9  99.9 -1.3     -70.6   -26   1 11    800  07 30 20
07 33 20  ---          02 46 45  72.6 100.6 -1.3     -70.2   154   F  1   1600

07 33 20  J0431+1731   02 46 45  62.7 112.6 -1.8     -56.4   -26   1 11   1600  07 33 20
07 35 20  ---          02 48 45  63.1 113.2 -1.7     -56.1    94   F  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

07 35 20  TTAUS        02 48 45  66.2 112.3 -1.6     -57.7   -12   1 11   3200  07 35 20
07 39 00  ---          02 52 26  66.9 113.4 -1.5     -56.9   208   F  1   6133

07 39 00  J0431+1731   02 52 26  63.8 114.3 -1.7     -55.3   -12   1 11   6133  07 39 00
07 41 00  ---          02 54 26  64.2 114.9 -1.6     -54.9   108   F  1   7733

07 41 00  TTAUS        02 54 26  67.3 114.1 -1.5     -56.5   -12   1 11   7733  07 41 00
07 44 40  ---          02 58 07  68.0 115.4 -1.4     -55.6   208   F  1  10667

07 44 40  J0431+1731   02 58 07  64.9 116.1 -1.6     -54.1   -12   1 11  10667  07 44 40
07 46 40  ---          03 00 07  65.3 116.8 -1.5     -53.7   108   F  1  12267

07 46 40  TTAUS        03 00 07  68.4 116.1 -1.4     -55.1   -12   1 11  12267  07 46 40
07 50 20  ---          03 03 48  69.1 117.5 -1.3     -54.1   208   F  1  15200

07 50 20  J0431+1731   03 03 48  66.0 118.0 -1.5     -52.8   -12   1 11  15200  07 50 20
07 52 20  ---          03 05 48  66.4 118.8 -1.4     -52.3   108   F  1  16800

07 54 20  J0555+3948   03 07 49  54.8  63.2 -2.8     -91.8    77   1 12  16800  07 54 20
07 58 20  =0552+398    03 11 49  55.6  63.1 -2.7     -92.5   240   R  1  15200

07 58 20  J0403+2600   03 11 49  77.8 109.0 -0.9     -64.8   -50   1 12  15200  07 58 20
08 01 20  ---          03 14 50  78.4 110.4 -0.8     -63.8   130   R  1  12800

08 01 20  J0431+1731   03 14 50  68.1 122.2 -1.3     -49.7   -27   1 12  12800  08 01 20
08 03 20  ---          03 16 50  68.4 123.1 -1.3     -49.1    93   R  1  11200

08 03 20  TTAUS        03 16 50  71.5 123.1 -1.1     -49.9   -12   1 12  11200  08 03 20
08 06 20  ---          03 19 50  72.1 124.6 -1.0     -48.7   168   R  1   8800

08 06 20  J0431+1731   03 19 50  69.0 124.4 -1.2     -48.1   -12   1 12   8800  08 06 20
08 08 20  ---          03 21 51  69.3 125.3 -1.2     -47.4   108   R  1   7200

08 08 20  TTAUS        03 21 51  72.4 125.6 -1.0     -47.9   -12   1 12   7200  08 08 20
08 11 20  ---          03 24 51  73.0 127.2 -1.0     -46.6   168   R  1   4800

08 11 20  J0431+1731   03 24 51  69.9 126.7 -1.1     -46.3   -12   1 12   4800  08 11 20
08 13 20  ---          03 26 52  70.2 127.7 -1.1     -45.6   108   R  1   3200

08 13 20  TTAUS        03 26 52  73.3 128.4 -0.9     -45.7   -12   1 12   3200  08 13 20
08 16 20  ---          03 29 52  73.8 130.1 -0.9     -44.3   168   R  1    800
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

08 16 20  J0431+1731   03 29 52  70.7 129.2 -1.0     -44.4   -12   1 13    800  08 16 20
08 18 20  ---          03 31 52  71.0 130.2 -1.0     -43.5   108   F  1    800

08 18 20  TTAUS        03 31 52  74.1 131.4 -0.8     -43.3   -12   1 13    800  08 18 20
08 21 20  ---          03 34 53  74.6 133.3 -0.8     -41.6   168   F  1   3200

08 21 20  J0431+1731   03 34 53  71.5 131.9 -1.0     -42.2   -12   1 13   3200  08 21 20
08 23 20  ---          03 36 53  71.8 133.0 -0.9     -41.3   108   F  1   4800

08 23 20  J0403+2600   03 36 53  82.6 126.9 -0.4     -50.0   -27   1 13   4800  08 23 20
08 26 20  ---          03 39 54  83.1 130.5 -0.4     -46.8   153   F  1   7200

08 26 20  J0431+1731   03 39 54  72.3 134.8 -0.9     -39.8   -28   1 13   7200  08 26 20
08 28 20  ---          03 41 54  72.6 136.0 -0.8     -38.8    92   F  1   8800

08 28 20  TTAUS        03 41 54  75.7 138.3 -0.7     -37.4   -12   1 13   8800  08 28 20
08 31 35  ---          03 45 10  76.1 140.8 -0.6     -35.2   183   F  1  11400

08 31 35  J0431+1731   03 45 10  73.1 138.1 -0.8     -37.1   -12   1 13  11400  08 31 35
08 33 35  ---          03 47 10  73.4 139.4 -0.8     -35.9   108   F  1  13000

08 33 35  TTAUS        03 47 10  76.4 142.4 -0.6     -33.8   -12   1 13  13000  08 33 35
08 36 50  ---          03 50 25  76.8 145.2 -0.5     -31.4   183   F  1  15600

08 36 50  J0431+1731   03 50 25  73.8 141.7 -0.7     -34.0   -12   1 13  15600  08 36 50
08 38 50  ---          03 52 26  74.1 143.1 -0.7     -32.8   108   F  1  17200

08 38 50  TTAUS        03 52 26  77.0 147.0 -0.5     -29.8   -12   1 14  17200  08 38 50
08 42 05  ---          03 55 41  77.4 150.1 -0.4     -27.1   183   R  1  14600

08 42 05  J0431+1731   03 55 41  74.5 145.6 -0.6     -30.7   -12   1 14  14600  08 42 05
08 44 05  ---          03 57 42  74.7 147.1 -0.6     -29.3   108   R  1  13000

08 44 05  TTAUS        03 57 42  77.6 152.0 -0.4     -25.3   -12   1 14  13000  08 44 05
08 47 20  ---          04 00 57  77.9 155.4 -0.4     -22.4   183   R  1  10400

08 47 20  J0431+1731   04 00 57  75.1 149.8 -0.5     -27.0   -12   1 14  10400  08 47 20
08 49 20  ---          04 02 58  75.3 151.4 -0.5     -25.6   108   R  1   8800

08 49 20  J0403+2600   04 02 58  85.4 179.0  0.0      -1.0   -26   1 14   8800  08 49 20
08 52 20  ---          04 05 58  85.3 187.3  0.0       7.0   154   R  1   6400
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

08 52 20  J0431+1731   04 05 58  75.6 154.0 -0.4     -23.3   -28   1 14   6400  08 52 20
08 54 20  ---          04 07 58  75.8 155.8 -0.4     -21.7    92   R  1   4800

08 54 20  TTAUS        04 07 58  78.5 163.0 -0.2     -15.5   -11   1 14   4800  08 54 20
08 57 35  ---          04 11 14  78.6 166.8 -0.2     -12.1   184   R  1   2200

08 57 35  J0431+1731   04 11 14  76.1 158.8 -0.3     -19.0   -11   1 14   2200  08 57 35
08 59 35  ---          04 13 14  76.2 160.7 -0.3     -17.3   109   R  1    600

-----------  Tape Change ------------

08 59 35  TTAUS        04 13 14  78.7 169.1 -0.1      -9.9   -12   2  1    600  08 59 35
09 02 50  ---          04 16 30  78.8 173.0 -0.1      -6.4   183   F  1   2000

09 02 50  J0431+1731   04 16 30  76.4 163.9 -0.3     -14.5   -12   2  1   2000  09 02 50
09 04 50  ---          04 18 30  76.5 165.9 -0.2     -12.7   108   F  1   3600

09 04 50  TTAUS        04 18 30  78.9 175.5 -0.1      -4.1   -12   2  1   3600  09 04 50
09 08 05  ---          04 21 46  78.9 179.4  0.0      -0.5   183   F  1   6200

09 08 05  J0431+1731   04 21 46  76.7 169.2 -0.2      -9.8   -13   2  1   6200  09 08 05
09 10 05  ---          04 23 46  76.8 171.2 -0.1      -7.9   107   F  1   7800

09 10 05  TTAUS        04 23 46  78.9 181.9  0.0       1.7   -13   2  1   7800  09 10 05
09 13 20  ---          04 27 01  78.9 185.9  0.1       5.4   182   F  1  10400

09 13 20  J0431+1731   04 27 01  76.8 174.6 -0.1      -4.9   -14   2  1  10400  09 13 20
09 15 20  ---          04 29 02  76.9 176.7 -0.1      -3.0   106   F  1  12000

09 15 20  J0403+2600   04 29 02  82.7 232.3  0.4      49.3   -43   2  1  12000  09 15 20
09 18 20  ---          04 32 02  82.2 235.6  0.5      52.1   137   F  1  14400

09 18 20  J0431+1731   04 32 02  76.9 179.9  0.0      -0.1   -43   2  1  14400  09 18 20
09 20 20  ---          04 34 03  76.9 182.0  0.0       1.8    77   F  1  16000

09 20 20  TTAUS        04 34 03  78.6 194.2  0.2      13.0   -14   2  2  16000  09 20 20
09 23 35  ---          04 37 18  78.4 198.0  0.3      16.3   181   R  1  16600

09 23 35  J0431+1731   04 37 18  76.8 185.4  0.1       4.9   -14   2  2  16600  09 23 35
09 25 35  ---          04 39 18  76.8 187.5  0.1       6.7   106   R  1  15000

09 25 35  TTAUS        04 39 18  78.3 200.2  0.3      18.4   -14   2  2  15000  09 25 35
09 28 50  ---          04 42 34  78.0 203.7  0.3      21.5   181   R  1  12400
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

09 28 50  J0431+1731   04 42 34  76.7 190.8  0.2       9.8   -15   2  2  12400  09 28 50
09 30 50  ---          04 44 34  76.6 192.9  0.2      11.6   105   R  1  10800

09 30 50  TTAUS        04 44 34  77.8 205.8  0.4      23.4   -15   2  2  10800  09 30 50
09 34 05  ---          04 47 50  77.5 209.0  0.4      26.3   180   R  1   8200

09 34 05  J0431+1731   04 47 50  76.4 196.1  0.3      14.5   -15   2  2   8200  09 34 05
09 36 05  ---          04 49 50  76.3 198.1  0.3      16.2   105   R  1   6600

09 36 05  TTAUS        04 49 50  77.3 211.0  0.5      28.0   -15   2  2   6600  09 36 05
09 39 20  ---          04 53 06  76.9 214.0  0.5      30.7   180   R  1   4000

09 39 20  J0431+1731   04 53 06  76.1 201.2  0.3      19.0   -15   2  2   4000  09 39 20
09 41 20  ---          04 55 06  75.9 203.0  0.4      20.7   105   R  1   2400

09 41 20  J0403+2600   04 55 06  77.7 251.1  0.9      64.9   -38   2  2   2400  09 41 20
09 44 20  ---          04 58 07  77.1 252.4  0.9      65.9   142   R  1      0

09 44 20  J0431+1731   04 58 07  75.6 205.7  0.4      23.1   -37   2  3      0  09 44 20
09 46 20  ---          05 00 07  75.4 207.5  0.5      24.6    83   F  1   1600

09 46 20  TTAUS        05 00 07  76.0 219.9  0.6      35.8   -14   2  3   1600  09 46 20
09 49 35  ---          05 03 22  75.5 222.4  0.7      38.0   181   F  1   4200

09 49 35  J0431+1731   05 03 22  75.1 210.2  0.5      27.0   -14   2  3   4200  09 49 35
09 51 35  ---          05 05 23  74.9 211.9  0.6      28.4   106   F  1   5800

09 51 35  TTAUS        05 05 23  75.2 223.8  0.7      39.2   -14   2  3   5800  09 51 35
09 54 50  ---          05 08 38  74.7 226.1  0.8      41.1   181   F  1   8400

09 54 50  J0431+1731   05 08 38  74.5 214.4  0.6      30.7   -14   2  3   8400  09 54 50
09 56 50  ---          05 10 39  74.2 215.9  0.6      32.0   106   F  1  10000

09 56 50  TTAUS        05 10 39  74.4 227.4  0.8      42.2   -14   2  3  10000  09 56 50
10 00 05  ---          05 13 54  73.9 229.5  0.9      43.9   181   F  1  12600

10 00 05  J0431+1731   05 13 54  73.8 218.3  0.7      34.0   -13   2  3  12600  10 00 05
10 02 05  ---          05 15 54  73.6 219.7  0.7      35.2   107   F  1  14200

10 02 05  TTAUS        05 15 54  73.6 230.7  0.9      44.9   -13   2  3  14200  10 02 05
10 05 20  ---          05 19 10  73.0 232.5  0.9      46.4   182   F  1  16800
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

10 05 20  J0431+1731   05 19 10  73.1 221.9  0.8      37.0   -13   2  4  16800  10 05 20
10 07 20  ---          05 21 10  72.8 223.2  0.8      38.1   107   R  1  16800

10 07 20  J0403+2600   05 21 10  72.3 259.7  1.3      70.4   -30   2  4  16800  10 07 20
10 10 20  ---          05 24 11  71.6 260.4  1.3      70.7   150   R  1  14400

10 10 20  J0431+1731   05 24 11  72.4 225.0  0.9      39.7   -30   2  4  14400  10 10 20
10 12 20  ---          05 26 11  72.0 226.2  0.9      40.7    90   R  1  12800

10 12 20  TTAUS        05 26 11  71.8 236.2  1.1      49.4   -13   2  4  12800  10 12 20
10 15 35  ---          05 29 27  71.2 237.8  1.1      50.6   182   R  1  10200

10 15 35  J0431+1731   05 29 27  71.5 228.1  1.0      42.2   -12   2  4  10200  10 15 35
10 17 35  ---          05 31 27  71.2 229.2  1.0      43.1   108   R  1   8600

10 17 35  TTAUS        05 31 27  70.8 238.7  1.2      51.3   -12   2  4   8600  10 17 35
10 20 50  ---          05 34 43  70.2 240.1  1.2      52.3   183   R  1   6000

10 20 50  J0431+1731   05 34 43  70.7 230.9  1.0      44.5   -12   2  4   6000  10 20 50
10 22 50  ---          05 36 43  70.3 231.9  1.1      45.3   108   R  1   4400

10 22 50  TTAUS        05 36 43  69.9 240.9  1.2      53.0   -12   2  4   4400  10 22 50
10 26 05  ---          05 39 58  69.2 242.3  1.3      53.9   183   R  1   1800

10 26 05  J0431+1731   05 39 58  69.8 233.5  1.1      46.5   -12   2  4   1800  10 26 05
10 28 05  ---          05 41 59  69.4 234.5  1.2      47.2   108   R  1    200

10 28 05  TTAUS        05 41 59  68.9 243.0  1.3      54.5   -12   2  5    200  10 28 05
10 31 20  ---          05 45 14  68.2 244.2  1.4      55.3   183   F  1   2800

10 31 20  J0431+1731   05 45 14  68.9 235.9  1.2      48.4   -12   2  5   2800  10 31 20
10 33 20  ---          05 47 15  68.5 236.8  1.3      49.0   108   F  1   4400

10 33 20  J0403+2600   05 47 15  66.7 265.0  1.7      72.5   -25   2  5   4400  10 33 20
10 36 20  ---          05 50 15  66.1 265.5  1.8      72.6   155   F  1   6800

10 36 20  J0431+1731   05 50 15  67.9 238.0  1.3      50.0   -24   2  5   6800  10 36 20
10 38 20  ---          05 52 15  67.6 238.9  1.3      50.6    96   F  1   8400

10 38 20  TTAUS        05 52 15  66.9 246.7  1.5      57.0   -11   2  5   8400  10 38 20
10 41 35  ---          05 55 31  66.2 247.7  1.6      57.6   184   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

10 41 35  J0431+1731   05 55 31  67.0 240.1  1.4      51.5   -11   2  5  11000  10 41 35
10 43 35  ---          05 57 31  66.6 240.9  1.4      52.0   109   F  1  12600

10 43 35  TTAUS        05 57 31  65.8 248.3  1.6      58.0   -11   2  5  12600  10 43 35
10 46 50  ---          06 00 47  65.2 249.3  1.6      58.6   184   F  1  15200

10 46 50  J0431+1731   06 00 47  66.0 242.0  1.5      52.9   -11   2  5  15200  10 46 50
10 48 50  ---          06 02 47  65.6 242.7  1.5      53.3   109   F  1  16800

10 48 50  TTAUS        06 02 47  64.8 249.9  1.7      59.0   -11   2  6  16800  10 48 50
10 52 05  ---          06 06 03  64.1 250.8  1.7      59.6   184   R  1  15800

10 52 05  J0431+1731   06 06 03  65.0 243.8  1.6      54.1   -11   2  6  15800  10 52 05
10 54 05  ---          06 08 03  64.6 244.5  1.6      54.5   109   R  1  14200

10 54 05  TTAUS        06 08 03  63.7 251.3  1.8      59.9   -11   2  6  14200  10 54 05
10 57 20  ---          06 11 19  63.0 252.2  1.8      60.4   184   R  1  11600

10 57 20  J0431+1731   06 11 19  64.0 245.5  1.7      55.2   -10   2  6  11600  10 57 20
10 59 20  ---          06 13 19  63.6 246.1  1.7      55.6   110   R  1  10000

10 59 20  J0403+2600   06 13 19  61.1 268.9  2.2      73.2   -21   2  6  10000  10 59 20
11 02 20  ---          06 16 19  60.5 269.3  2.2      73.2   159   R  1   7600

11 02 20  J0431+1731   06 16 19  63.0 247.0  1.7      56.2   -21   2  6   7600  11 02 20
11 04 20  ---          06 18 20  62.6 247.6  1.8      56.6    99   R  1   6000

11 04 20  TTAUS        06 18 20  61.6 253.9  1.9      61.3   -10   2  6   6000  11 04 20
11 07 35  ---          06 21 35  60.9 254.7  2.0      61.7   185   R  1   3400

11 07 35  J0431+1731   06 21 35  61.9 248.5  1.8      57.1   -10   2  6   3400  11 07 35
11 09 35  ---          06 23 36  61.5 249.1  1.9      57.4   110   R  1   1800

11 09 35  TTAUS        06 23 36  60.5 255.1  2.0      61.9   -10   2  7   1800  11 09 35
11 12 50  ---          06 26 51  59.8 255.8  2.1      62.3   185   F  1    800

11 12 50  J0431+1731   06 26 51  60.9 249.9  1.9      58.0   -10   2  7    800  11 12 50
11 14 50  ---          06 28 51  60.5 250.5  1.9      58.3   110   F  1   2400

11 14 50  TTAUS        06 28 51  59.4 256.3  2.1      62.5   -10   2  7   2400  11 14 50
11 18 05  ---          06 32 07  58.7 257.0  2.2      62.8   185   F  1   5000
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

11 18 05  J0431+1731   06 32 07  59.8 251.3  2.0      58.7   -10   2  7   5000  11 18 05
11 20 05  ---          06 34 07  59.4 251.8  2.0      59.0   110   F  1   6600

11 20 05  TTAUS        06 34 07  58.3 257.4  2.2      63.0   -10   2  7   6600  11 20 05
11 23 20  ---          06 37 23  57.6 258.0  2.3      63.3   185   F  1   9200

11 23 20  J0431+1731   06 37 23  58.7 252.5  2.1      59.4   -10   2  7   9200  11 23 20
11 25 20  ---          06 39 23  58.3 253.0  2.1      59.6   110   F  1  10800

11 25 20  J0403+2600   06 39 23  55.5 272.2  2.6      73.1   -19   2  7  10800  11 25 20
11 28 20  ---          06 42 24  54.9 272.5  2.7      73.0   161   F  1  13200

11 28 20  J0431+1731   06 42 24  57.7 253.7  2.2      60.0   -19   2  7  13200  11 28 20
11 30 20  ---          06 44 24  57.3 254.1  2.2      60.2   101   F  1  14800

11 30 20  TTAUS        06 44 24  56.1 259.4  2.4      63.8    -9   2  7  14800  11 30 20
11 33 20  ---          06 47 24  55.5 259.9  2.4      64.0   171   F  1  17200

11 33 20  J0431+1731   06 47 24  56.6 254.8  2.3      60.5    -9   2  8  17200  11 33 20
11 35 20  ---          06 49 25  56.2 255.2  2.3      60.7   111   R  1  15600

11 35 20  TTAUS        06 49 25  55.1 260.3  2.5      64.2    -9   2  8  15600  11 35 20
11 38 20  ---          06 52 25  54.4 260.8  2.5      64.3   171   R  1  13200

11 38 20  J0431+1731   06 52 25  55.6 255.8  2.3      61.0    -9   2  8  13200  11 38 20
11 40 20  ---          06 54 26  55.2 256.2  2.4      61.2   111   R  1  11600

11 40 20  TTAUS        06 54 26  54.0 261.2  2.5      64.5    -9   2  8  11600  11 40 20
11 43 20  ---          06 57 26  53.4 261.7  2.6      64.6   171   R  1   9200

11 43 20  J0431+1731   06 57 26  54.6 256.8  2.4      61.5    -9   2  8   9200  11 43 20
11 45 20  ---          06 59 26  54.1 257.2  2.5      61.6   111   R  1   7600

11 45 20  TTAUS        06 59 26  52.9 262.0  2.6      64.7    -9   2  8   7600  11 45 20
11 48 20  ---          07 02 27  52.3 262.5  2.7      64.9   171   R  1   5200

11 48 20  J0431+1731   07 02 27  53.5 257.8  2.5      61.9    -9   2  8   5200  11 48 20
11 50 20  ---          07 04 27  53.1 258.2  2.5      62.0   111   R  1   3600

11 52 20  J0555+3948   07 06 28  72.9 307.4  1.2     117.1    74   2  8   3600  11 52 20
11 56 20  =0552+398    07 10 28  72.3 306.2  1.2     115.4   240   R  1    400
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

11 56 20  J0403+2600   07 10 28  48.8 275.6  3.1      72.3   -53   2  9    400  11 56 20
11 59 20  ---          07 13 29  48.2 275.9  3.2      72.2   127   F  1   2800

11 59 20  J0431+1731   07 13 29  51.2 259.8  2.7      62.6   -17   2  9   2800  11 59 20
12 01 20  ---          07 15 29  50.7 260.1  2.7      62.8   103   F  1   4400

12 01 20  TTAUS        07 15 29  49.5 264.6  2.9      65.4    -9   2  9   4400  12 01 20
12 04 35  ---          07 18 45  48.8 265.1  2.9      65.5   186   F  1   7000

12 04 35  J0431+1731   07 18 45  50.1 260.7  2.8      62.9    -9   2  9   7000  12 04 35
12 06 35  ---          07 20 45  49.6 261.0  2.8      63.0   111   F  1   8600

12 06 35  TTAUS        07 20 45  48.4 265.3  3.0      65.5    -9   2  9   8600  12 06 35
12 09 50  ---          07 24 00  47.7 265.8  3.0      65.6   186   F  1  11200

12 09 50  J0431+1731   07 24 00  48.9 261.6  2.9      63.2    -9   2  9  11200  12 09 50
12 11 50  ---          07 26 01  48.5 261.9  2.9      63.3   111   F  1  12800

12 11 50  TTAUS        07 26 01  47.2 266.1  3.1      65.6    -9   2  9  12800  12 11 50
12 15 05  ---          07 29 16  46.5 266.6  3.1      65.7   186   F  1  15400

12 15 05  J0431+1731   07 29 16  47.8 262.4  3.0      63.4    -9   2  9  15400  12 15 05
12 17 05  ---          07 31 17  47.4 262.7  3.0      63.5   111   F  1  17000

12 17 05  J0403+2600   07 31 17  44.4 277.7  3.5      71.6   -16   2 10  17000  12 17 05
12 20 05  ---          07 34 17  43.8 278.0  3.5      71.5   164   R  1  15800

12 20 05  J0431+1731   07 34 17  46.7 263.2  3.0      63.6   -16   2 10  15800  12 20 05
12 22 05  ---          07 36 17  46.3 263.5  3.1      63.7   104   R  1  14200

12 22 05  TTAUS        07 36 17  45.0 267.5  3.2      65.8    -9   2 10  14200  12 22 05
12 25 05  ---          07 39 18  44.4 268.0  3.3      65.8   171   R  1  11800

12 25 05  J0431+1731   07 39 18  45.7 264.0  3.1      63.8    -9   2 10  11800  12 25 05
12 27 05  ---          07 41 18  45.2 264.3  3.2      63.9   111   R  1  10200

12 27 05  TTAUS        07 41 18  44.0 268.2  3.3      65.9    -9   2 10  10200  12 27 05
12 30 05  ---          07 44 19  43.3 268.6  3.4      65.9   171   R  1   7800

12 30 05  J0431+1731   07 44 19  44.6 264.7  3.2      64.0    -9   2 10   7800  12 30 05
12 32 05  ---          07 46 19  44.2 265.0  3.2      64.0   111   R  1   6200
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

12 32 05  TTAUS        07 46 19  42.9 268.9  3.4      65.9    -9   2 10   6200  12 32 05
12 35 05  ---          07 49 20  42.2 269.3  3.5      65.9   171   R  1   3800

12 35 05  J0431+1731   07 49 20  43.5 265.4  3.3      64.1    -9   2 10   3800  12 35 05
12 37 05  ---          07 51 20  43.1 265.7  3.3      64.1   111   R  1   2200

12 37 05  TTAUS        07 51 20  41.8 269.5  3.5      65.9    -9   2 11   2200  12 37 05
12 40 05  ---          07 54 20  41.2 269.9  3.5      65.9   171   F  1    200

12 40 05  J0431+1731   07 54 20  42.5 266.2  3.4      64.2    -9   2 11    200  12 40 05
12 42 05  ---          07 56 21  42.0 266.4  3.4      64.2   111   F  1   1800

12 42 05  J0403+2600   07 56 21  39.1 280.1  3.9      70.5   -15   2 11   1800  12 42 05
12 45 05  ---          07 59 21  38.4 280.4  3.9      70.3   165   F  1   4200

12 45 05  J0431+1731   07 59 21  41.4 266.8  3.5      64.3   -15   2 11   4200  12 45 05
12 47 05  ---          08 01 22  40.9 267.1  3.5      64.3   105   F  1   5800

12 47 05  TTAUS        08 01 22  39.6 270.8  3.7      65.9    -9   2 11   5800  12 47 05
12 50 20  ---          08 04 37  38.9 271.2  3.7      65.9   186   F  1   8400

12 50 20  J0431+1731   08 04 37  40.2 267.6  3.5      64.4    -9   2 11   8400  12 50 20
12 52 20  ---          08 06 37  39.8 267.8  3.6      64.4   111   F  1  10000

12 52 20  TTAUS        08 06 37  38.5 271.5  3.7      65.9    -9   2 11  10000  12 52 20
12 55 35  ---          08 09 53  37.8 271.9  3.8      65.9   186   F  1  12600

12 55 35  J0431+1731   08 09 53  39.1 268.3  3.6      64.4    -9   2 11  12600  12 55 35
12 57 35  ---          08 11 53  38.7 268.5  3.7      64.4   111   F  1  14200

12 57 35  TTAUS        08 11 53  37.4 272.1  3.8      65.8    -9   2 11  14200  12 57 35
13 00 50  ---          08 15 09  36.7 272.5  3.9      65.8   186   F  1  16800

13 00 50  J0431+1731   08 15 09  38.0 269.0  3.7      64.5    -9   2 12  16800  13 00 50
13 02 50  ---          08 17 09  37.5 269.2  3.7      64.5   111   R  1  16800

13 02 50  TTAUS        08 17 09  36.3 272.7  3.9      65.8    -9   2 12  16800  13 02 50
13 06 05  ---          08 20 25  35.5 273.1  4.0      65.7   186   R  1  14200

13 06 05  J0431+1731   08 20 25  36.8 269.6  3.8      64.5    -9   2 12  14200  13 06 05
13 08 05  ---          08 22 25  36.4 269.9  3.8      64.5   111   R  1  12600
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

13 08 05  J0403+2600   08 22 25  33.6 282.6  4.3      69.1   -14   2 12  12600  13 08 05
13 11 05  ---          08 25 26  32.9 282.9  4.4      68.9   166   R  1  10200

13 11 05  J0431+1731   08 25 26  35.8 270.3  3.9      64.5   -14   2 12  10200  13 11 05
13 13 05  ---          08 27 26  35.3 270.5  3.9      64.5   106   R  1   8600

13 13 05  TTAUS        08 27 26  34.0 274.0  4.1      65.6    -9   2 12   8600  13 13 05
13 16 20  ---          08 30 41  33.3 274.3  4.1      65.6   186   R  1   6000

13 16 20  J0431+1731   08 30 41  34.6 270.9  4.0      64.5    -9   2 12   6000  13 16 20
13 18 20  ---          08 32 42  34.2 271.2  4.0      64.4   111   R  1   4400

13 18 20  TTAUS        08 32 42  32.9 274.6  4.2      65.5    -9   2 12   4400  13 18 20
13 21 35  ---          08 35 57  32.2 275.0  4.2      65.5   186   R  1   1800

13 21 35  J0431+1731   08 35 57  33.5 271.6  4.1      64.4    -9   2 12   1800  13 21 35
13 23 35  ---          08 37 58  33.1 271.8  4.1      64.4   111   R  1    200

13 23 35  J0403+2600   08 37 58  30.3 284.1  4.6      68.2   -14   2 13    200  13 23 35
13 26 35  ---          08 40 58  29.7 284.4  4.6      68.0   166   F  1   2600

13 26 35  J0431+1731   08 40 58  32.4 272.2  4.1      64.4   -14   2 13   2600  13 26 35
13 28 35  ---          08 42 58  32.0 272.5  4.2      64.4   106   F  1   4200

13 28 35  TTAUS        08 42 58  30.7 275.8  4.3      65.3    -9   2 13   4200  13 28 35
13 31 35  ---          08 45 59  30.1 276.1  4.4      65.2   171   F  1   6600

13 31 35  J0431+1731   08 45 59  31.3 272.8  4.2      64.3    -9   2 13   6600  13 31 35
13 33 35  ---          08 47 59  30.9 273.1  4.3      64.3   111   F  1   8200

13 33 35  TTAUS        08 47 59  29.6 276.3  4.4      65.2    -9   2 13   8200  13 33 35
13 35 35  ---          08 50 00  29.2 276.6  4.5      65.1   111   F  1   9800

13 35 35  J0431+1731   08 50 00  30.5 273.3  4.3      64.3    -9   2 13   9800  13 35 35
13 37 35  ---          08 52 00  30.1 273.5  4.3      64.2   111   F  1  11400

13 37 35  J0555+3948   08 52 00  53.2 296.8  2.9      90.4   -52   2 13  11400  13 37 35
13 41 35  =0552+398    08 56 01  52.5 296.8  3.0      89.8   188   F  1  14600

13 41 35  J0403+2600   08 56 01  26.6 285.9  4.9      67.1   -58   2 13  14600  13 41 35
13 44 05  ---          08 58 31  26.1 286.1  4.9      66.9    92   F  1  16600
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               T Tau S, simultaneous with Chandra
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 Oct 2003   Day 297 ---

13 44 05  J0431+1731   08 58 31  28.7 274.3  4.4      64.1   -14   2 14  16600  13 44 05
13 46 05  ---          09 00 31  28.2 274.6  4.5      64.1   106   R  1  17000

13 46 05  TTAUS        09 00 31  27.0 277.8  4.6      64.8    -9   2 14  17000  13 46 05
13 49 05  ---          09 03 32  26.3 278.1  4.7      64.7   171   R  1  14600

13 49 05  J0431+1731   09 03 32  27.6 274.9  4.5      64.0    -9   2 14  14600  13 49 05
13 51 05  ---          09 05 32  27.2 275.2  4.6      64.0   111   R  1  13000

13 51 05  TTAUS        09 05 32  25.9 278.3  4.7      64.6    -9   2 14  13000  13 51 05
13 54 05  ---          09 08 33  25.3 278.7  4.8      64.5   171   R  1  10600

13 54 05  J0431+1731   09 08 33  26.5 275.5  4.6      63.9    -9   2 14  10600  13 54 05
13 56 05  ---          09 10 33  26.1 275.7  4.6      63.9   111   R  1   9000


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v4cm.set
   Matches group v4cm_3 in /homes/kester/Work/apps/chandra/ttaus/freq_cormac.dat

   Setup group:    9         Station: VLBA              Total bit rate:  256
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=    8399.49   8399.49   8415.49   8415.49
   BBC fr=     799.49    799.49    815.49    815.49
   Bandwd=     16.000    16.000    16.000    16.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510 13510 13510     0     0     0     0
    PCALFR2=   510   510 13510 13510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- T Tau S, simultaneous with Chandra
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * TTAUS             04 19 04.243788   * 04 21 59.426300     04 22 12.859645 
                     19 25 04.35304    * 19 32 05.73000      19 32 43.71196 
                     From catalog imbedded in main SCHED input file.

 * J0431+1731        04 29 04.186277   * 04 31 57.379800     04 32 10.637319 
                     17 25 14.39409    * 17 31 35.79200      17 32 11.27473 
                     From catalog imbedded in main SCHED input file.

 * J0357+2319        03 54 23.254633   * 03 57 21.608800     03 57 35.343656 
                     23 11 17.31305    * 23 19 53.85900      23 20 38.15787 
                     From catalog imbedded in main SCHED input file.

 * J0403+2600        04 00 03.595169   * 04 03 05.586400     04 03 19.581631 
                     25 51 46.48815    * 26 00 01.50200      26 00 43.65846 
                     From catalog imbedded in main SCHED input file.

 * J0555+3948        05 52 01.407166   * 05 55 30.805609     05 55 46.480484 
   0552+398          39 48 21.94585    * 39 48 49.16500      39 48 51.80569 
   DA193             /aux/pc176a/ksmith/software/sched/catalogs/sources.vlba
   J0555+39          ICRF - Ext.1 Source - 1998 IERS Annual Report



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   TTAUS              143.3
   J0431+1731         141.1
   J0357+2319         148.2
   J0403+2600         146.1
   J0555+3948         119.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

