  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
 Exp. Code:  GB067   


Schedule Version:       1.00                                              
Processed by SCHED version:   6.05  June 2006                             

PI:       M. Bietenholz                                                   

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 512-16-2-ul 6cm                                      

Notes:    Fringe finder  : 3C84                                           
          Pol. Calibrator: 3C84                                           
          Amplitude check: 3C66A                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  25 Oct 2008   Day 299 ---

 Next scan frequencies:  4958.49  4958.49  4958.49  4958.49  4974.49  4974.49
                         4974.49  4974.49  4990.49  4990.49  4990.49  4990.49
                         5006.49  5006.49  5006.49  5006.49
 Next BBC frequencies:    858.49   858.49   858.49   858.49   874.49   874.49
                          874.49   874.49   890.49   890.49   890.49   890.49
                          906.49   906.49   906.49   906.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00     8.00     8.00

23 04 20  3C66A        18 27 21   2.5  39.8 -7.9  H  -48.9     0   1  1      0  23 04 20
23 05 30  ---          18 28 31   2.7  39.9 -7.9  H  -49.1     0   F  1      5  23 04 38

23 05 30  SN1986J      18 28 31   2.2  40.5 -7.9  D  -49.1    -7   1  1      5  23 05 30
23 07 30  ---          18 30 32   2.5  40.7 -7.9  H  -49.4     0   F  1     12  23 05 30

23 07 30  3C66A        18 30 32   2.9  40.1 -7.9  H  -49.4    -7   1  1     12  23 07 30
23 08 40  ---          18 31 42   3.1  40.3 -7.9     -49.6     0   F  1     17  23 07 30

23 08 40  SN1986J      18 31 42   2.7  40.8 -7.9  H  -49.6    -7   1  1     17  23 08 40
23 10 40  ---          18 33 42   2.9  41.1 -7.8     -49.9     0   F  1     25  23 08 40

23 10 40  3C66A        18 33 42   3.4  40.5 -7.8     -49.9    -7   1  1     25  23 10 40
23 11 50  ---          18 34 52   3.5  40.7 -7.8     -50.1    63   F  1     29  23 10 40

23 11 50  SN1986J      18 34 52   3.1  41.2 -7.8     -50.1    -7   1  1     29  23 11 50
23 13 50  ---          18 36 53   3.4  41.4 -7.8     -50.4   113   F  1     37  23 11 50

23 13 50  3C66A        18 36 53   3.8  40.9 -7.8     -50.5    -7   1  1     37  23 13 50
23 15 00  ---          18 38 03   4.0  41.0 -7.8     -50.6    63   F  1     41  23 13 50

23 15 00  SN1986J      18 38 03   3.6  41.6 -7.8     -50.6    -7   1  1     41  23 15 00
23 17 00  ---          18 40 03   3.9  41.8 -7.7     -51.0   113   F  1     49  23 15 00

23 17 00  3C66A        18 40 03   4.3  41.3 -7.7     -51.0    -7   1  1     49  23 17 00
23 18 10  ---          18 41 13   4.4  41.4 -7.7     -51.2    63   F  1     54  23 17 00

23 20 30  3C66A        18 43 34   4.8  41.7 -7.7     -51.5   134   1  1     54  23 20 30
23 21 40  ---          18 44 44   4.9  41.8 -7.6     -51.7    70   F  1     58  23 20 48

23 21 40  SN1986J      18 44 44   4.5  42.4 -7.6     -51.7    -7   1  1     58  23 21 40
23 23 40  ---          18 46 44   4.8  42.6 -7.6     -52.0   113   F  1     66  23 21 40
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  25 Oct 2008   Day 299 ---

23 23 40  3C66A        18 46 44   5.2  42.0 -7.6     -52.0    -7   1  1     66  23 23 40
23 24 50  ---          18 47 55   5.4  42.2 -7.6     -52.2    63   F  1     70  23 23 40

23 24 50  SN1986J      18 47 55   5.0  42.7 -7.6     -52.2    -7   1  1     70  23 24 50
23 26 50  ---          18 49 55   5.3  43.0 -7.6     -52.5   113   F  1     78  23 24 50

23 26 50  3C66A        18 49 55   5.7  42.4 -7.6     -52.6    -7   1  1     78  23 26 50
23 28 00  ---          18 51 05   5.9  42.5 -7.5     -52.7    63   F  1     83  23 26 50

23 28 00  SN1986J      18 51 05   5.5  43.1 -7.5     -52.7    -7   1  1     83  23 28 00
23 30 00  ---          18 53 05   5.7  43.3 -7.5     -53.0   113   F  1     90  23 28 00

23 30 00  3C66A        18 53 05   6.1  42.7 -7.5     -53.1    -7   1  1     90  23 30 00
23 31 10  ---          18 54 16   6.3  42.9 -7.5     -53.2    63   F  1     95  23 30 00

23 31 10  SN1986J      18 54 16   5.9  43.4 -7.5     -53.2    -7   1  1     95  23 31 10
23 33 10  ---          18 56 16   6.2  43.7 -7.4     -53.5   113   F  1    103  23 31 10

23 33 10  3C66A        18 56 16   6.6  43.1 -7.4     -53.6    -7   1  1    103  23 33 10
23 34 20  ---          18 57 26   6.8  43.2 -7.4     -53.8    63   F  1    107  23 33 10

23 34 20  SN1986J      18 57 26   6.4  43.8 -7.4     -53.7    -7   1  1    107  23 34 20
23 36 20  ---          18 59 26   6.7  44.0 -7.4     -54.0   113   F  1    115  23 34 20

23 36 20  3C66A        18 59 26   7.1  43.4 -7.4     -54.1    -7   1  1    115  23 36 20
23 37 30  ---          19 00 37   7.3  43.5 -7.4     -54.3    63   F  1    119  23 36 20

23 39 50  3C66A        19 02 57   7.6  43.8 -7.3     -54.6   134   1  1    119  23 39 50
23 41 00  ---          19 04 07   7.8  43.9 -7.3     -54.8    70   F  1    124  23 40 08

23 41 00  SN1986J      19 04 07   7.4  44.5 -7.3     -54.7    -6   1  1    124  23 41 00
23 43 00  ---          19 06 08   7.7  44.7 -7.3     -55.1   114   F  1    132  23 41 00

23 43 00  3C66A        19 06 08   8.1  44.1 -7.3     -55.1    -6   1  1    132  23 43 00
23 44 10  ---          19 07 18   8.3  44.3 -7.3     -55.3    64   F  1    136  23 43 00

23 44 10  SN1986J      19 07 18   7.9  44.9 -7.3     -55.2    -6   1  1    136  23 44 10
23 46 10  ---          19 09 18   8.2  45.1 -7.2     -55.5   114   F  1    144  23 44 10

23 46 10  3C66A        19 09 18   8.6  44.5 -7.2     -55.6    -6   1  1    144  23 46 10
23 47 20  ---          19 10 28   8.7  44.6 -7.2     -55.8    64   F  1    148  23 46 10
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  25 Oct 2008   Day 299 ---

23 47 20  SN1986J      19 10 28   8.4  45.2 -7.2     -55.7    -6   1  1    148  23 47 20
23 49 20  ---          19 12 29   8.7  45.4 -7.2     -56.0   114   F  1    156  23 47 20

23 49 20  3C66A        19 12 29   9.0  44.8 -7.2     -56.1    -6   1  1    156  23 49 20
23 50 30  ---          19 13 39   9.2  44.9 -7.2     -56.3    64   F  1    161  23 49 20

23 50 30  SN1986J      19 13 39   8.8  45.5 -7.2     -56.2    -6   1  1    161  23 50 30
23 52 30  ---          19 15 39   9.2  45.7 -7.1     -56.5   114   F  1    168  23 50 30

23 52 30  3C66A        19 15 39   9.5  45.1 -7.1     -56.6    -6   1  1    168  23 52 30
23 53 40  ---          19 16 49   9.7  45.2 -7.1     -56.8    64   F  1    173  23 52 30

23 53 40  SN1986J      19 16 49   9.3  45.9 -7.1     -56.7    -6   1  1    173  23 53 40
23 55 40  ---          19 18 50   9.6  46.1 -7.1     -57.0   114   F  1    181  23 53 40

23 55 40  3C66A        19 18 50  10.0  45.4 -7.1     -57.1    -6   1  1    181  23 55 40
23 56 50  ---          19 20 00  10.2  45.6 -7.1     -57.3    64   F  1    185  23 55 40

 --- Start: Sat  25 Oct 2008   Day 299 -- Stop: Sun  26 Oct 2008   Day 300 ---

23 59 10  3C66A        19 22 20  10.5  45.8 -7.0     -57.6   134   1  1    185  23 59 10
00 00 20  ---          19 23 30  10.7  45.9 -7.0     -57.8    70   F  1    190  23 59 28

00 00 20  SN1986J      19 23 30  10.4  46.5 -7.0     -57.7    -6   1  1    190  00 00 20
00 02 20  ---          19 25 31  10.7  46.7 -7.0     -58.0   114   F  1    197  00 00 20

00 02 20  3C66A        19 25 31  11.0  46.1 -7.0     -58.1    -6   1  1    197  00 02 20
00 03 30  ---          19 26 41  11.2  46.2 -6.9     -58.3    64   F  1    202  00 02 20

00 03 30  SN1986J      19 26 41  10.9  46.8 -6.9     -58.2    -6   1  1    202  00 03 30
00 05 30  ---          19 28 41  11.2  47.0 -6.9     -58.5   114   F  1    210  00 03 30

00 05 30  3C66A        19 28 41  11.5  46.4 -6.9     -58.6    -6   1  1    210  00 05 30
00 06 40  ---          19 29 51  11.7  46.5 -6.9     -58.8    64   F  1    214  00 05 30

00 06 40  SN1986J      19 29 51  11.4  47.2 -6.9     -58.7    -6   1  1    214  00 06 40
00 08 40  ---          19 31 52  11.7  47.4 -6.9     -59.0   114   F  1    222  00 06 40

00 08 40  3C66A        19 31 52  12.0  46.7 -6.9     -59.1    -6   1  1    222  00 08 40
00 09 50  ---          19 33 02  12.2  46.8 -6.8     -59.2    64   F  1    226  00 08 40

00 09 50  SN1986J      19 33 02  11.9  47.5 -6.8     -59.1    -6   1  1    226  00 09 50
00 11 50  ---          19 35 02  12.2  47.7 -6.8     -59.4   114   F  1    234  00 09 50
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

00 11 50  3C66A        19 35 02  12.5  47.0 -6.8     -59.5    -6   1  1    234  00 11 50
00 13 00  ---          19 36 12  12.7  47.1 -6.8     -59.7    64   F  1    239  00 11 50

00 13 00  SN1986J      19 36 12  12.4  47.8 -6.8     -59.6    -6   1  1    239  00 13 00
00 15 00  ---          19 38 13  12.7  48.0 -6.7     -59.9   114   F  1    246  00 13 00

00 15 00  3C66A        19 38 13  13.0  47.3 -6.8     -60.0    -6   1  1    246  00 15 00
00 16 10  ---          19 39 23  13.2  47.4 -6.7     -60.2    64   F  1    251  00 15 00

00 18 30  3C66A        19 41 43  13.6  47.7 -6.7     -60.5   134   1  1    251  00 18 30
00 19 40  ---          19 42 54  13.8  47.8 -6.7     -60.7    70   F  1    255  00 18 48

00 19 40  SN1986J      19 42 54  13.4  48.4 -6.7     -60.6    -6   1  1    255  00 19 40
00 21 40  ---          19 44 54  13.8  48.6 -6.6     -60.9   114   F  1    263  00 19 40

00 21 40  3C66A        19 44 54  14.1  47.9 -6.6     -61.0    -6   1  1    263  00 21 40
00 22 50  ---          19 46 04  14.3  48.1 -6.6     -61.2    64   F  1    268  00 21 40

00 22 50  SN1986J      19 46 04  14.0  48.7 -6.6     -61.0    -6   1  1    268  00 22 50
00 24 50  ---          19 48 04  14.3  48.9 -6.6     -61.3   114   F  1    275  00 22 50

00 24 50  3C66A        19 48 04  14.6  48.2 -6.6     -61.5    -6   1  1    275  00 24 50
00 26 00  ---          19 49 15  14.8  48.3 -6.6     -61.7    64   F  1    280  00 24 50

00 26 00  SN1986J      19 49 15  14.5  49.0 -6.6     -61.5    -6   1  1    280  00 26 00
00 28 00  ---          19 51 15  14.8  49.2 -6.5     -61.8   114   F  1    288  00 26 00

00 28 00  3C66A        19 51 15  15.1  48.5 -6.5     -61.9    -6   1  1    288  00 28 00
00 29 10  ---          19 52 25  15.3  48.6 -6.5     -62.1    64   F  1    292  00 28 00

00 29 10  SN1986J      19 52 25  15.0  49.3 -6.5     -62.0    -6   1  1    292  00 29 10
00 31 10  ---          19 54 25  15.3  49.5 -6.5     -62.3   114   F  1    300  00 29 10

00 31 10  3C66A        19 54 25  15.6  48.8 -6.5     -62.4    -6   1  1    300  00 31 10
00 32 20  ---          19 55 36  15.8  48.9 -6.5     -62.6    64   F  1    304  00 31 10

00 32 20  SN1986J      19 55 36  15.5  49.6 -6.5     -62.4    -6   1  1    304  00 32 20
00 34 20  ---          19 57 36  15.8  49.7 -6.4     -62.7   114   F  1    312  00 32 20

00 34 20  3C66A        19 57 36  16.1  49.1 -6.4     -62.9    -6   1  1    312  00 34 20
00 35 30  ---          19 58 46  16.3  49.2 -6.4     -63.1    64   F  1    317  00 34 20
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

00 37 50  3C66A        20 01 07  16.7  49.4 -6.4     -63.4   134   1  1    317  00 37 50
00 39 00  ---          20 02 17  16.9  49.5 -6.3     -63.6    70   F  1    321  00 38 08

00 39 00  SN1986J      20 02 17  16.6  50.1 -6.3     -63.4    -6   1  1    321  00 39 00
00 41 00  ---          20 04 17  16.9  50.3 -6.3     -63.7   114   F  1    329  00 39 00

00 41 00  3C66A        20 04 17  17.2  49.6 -6.3     -63.9    -6   1  1    329  00 41 00
00 42 10  ---          20 05 27  17.4  49.7 -6.3     -64.0    64   F  1    334  00 41 00

00 42 10  SN1986J      20 05 27  17.1  50.4 -6.3     -63.9    -6   1  1    334  00 42 10
00 44 10  ---          20 07 28  17.5  50.6 -6.3     -64.1   114   F  1    341  00 42 10

00 44 10  3C66A        20 07 28  17.7  49.9 -6.3     -64.3    -6   1  1    341  00 44 10
00 45 20  ---          20 08 38  17.9  50.0 -6.2     -64.5    64   F  1    346  00 44 10

00 45 20  SN1986J      20 08 38  17.7  50.7 -6.2     -64.3    -6   1  1    346  00 45 20
00 47 20  ---          20 10 38  18.0  50.9 -6.2     -64.6   114   F  1    354  00 45 20

00 47 20  3C66A        20 10 38  18.3  50.2 -6.2     -64.8    -6   1  1    354  00 47 20
00 48 30  ---          20 11 48  18.5  50.3 -6.2     -65.0    64   F  1    358  00 47 20

00 48 30  SN1986J      20 11 48  18.2  51.0 -6.2     -64.8    -6   1  1    358  00 48 30
00 50 30  ---          20 13 49  18.5  51.1 -6.2     -65.1   114   F  1    366  00 48 30

00 50 30  3C66A        20 13 49  18.8  50.4 -6.2     -65.2    -6   1  1    366  00 50 30
00 51 40  ---          20 14 59  19.0  50.5 -6.1     -65.4    64   F  1    370  00 50 30

00 51 40  SN1986J      20 14 59  18.7  51.2 -6.1     -65.2    -6   1  1    370  00 51 40
00 53 40  ---          20 16 59  19.1  51.4 -6.1     -65.5   114   F  1    378  00 51 40

00 53 40  3C66A        20 16 59  19.3  50.7 -6.1     -65.7    -6   1  1    378  00 53 40
00 54 50  ---          20 18 09  19.5  50.8 -6.1     -65.9    64   F  1    383  00 53 40

00 57 10  3C66A        20 20 30  19.9  51.0 -6.0     -66.2   134   1  1    383  00 57 10
00 58 20  ---          20 21 40  20.1  51.1 -6.0     -66.4    70   F  1    387  00 57 28

00 58 20  SN1986J      20 21 40  19.8  51.8 -6.0     -66.2    -6   1  1    387  00 58 20
01 00 20  ---          20 23 40  20.2  51.9 -6.0     -66.4   114   F  1    395  00 58 20

01 00 20  3C66A        20 23 40  20.4  51.2 -6.0     -66.7    -6   1  1    395  01 00 20
01 01 30  ---          20 24 50  20.6  51.3 -6.0     -66.8    64   F  1    399  01 00 20
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

01 01 30  SN1986J      20 24 50  20.4  52.0 -6.0     -66.6    -6   1  1    399  01 01 30
01 03 30  ---          20 26 51  20.7  52.2 -5.9     -66.9   114   F  1    407  01 01 30

01 03 30  3C66A        20 26 51  21.0  51.5 -5.9     -67.1    -6   1  1    407  01 03 30
01 04 40  ---          20 28 01  21.2  51.5 -5.9     -67.3    64   F  1    412  01 03 30

01 04 40  SN1986J      20 28 01  20.9  52.2 -5.9     -67.1    -6   1  1    412  01 04 40
01 06 40  ---          20 30 01  21.3  52.4 -5.9     -67.3   114   F  1    419  01 04 40

01 06 40  3C66A        20 30 01  21.5  51.7 -5.9     -67.6    -6   1  1    419  01 06 40
01 07 50  ---          20 31 11  21.7  51.8 -5.9     -67.7    64   F  1    424  01 06 40

01 07 50  SN1986J      20 31 11  21.5  52.5 -5.9     -67.5    -6   1  1    424  01 07 50
01 09 50  ---          20 33 12  21.8  52.6 -5.8     -67.8   114   F  1    432  01 07 50

01 09 50  3C66A        20 33 12  22.0  51.9 -5.8     -68.0    -6   1  1    432  01 09 50
01 11 00  ---          20 34 22  22.2  52.0 -5.8     -68.2    64   F  1    436  01 09 50

01 11 00  SN1986J      20 34 22  22.0  52.7 -5.8     -68.0    -6   1  1    436  01 11 00
01 13 00  ---          20 36 22  22.3  52.9 -5.8     -68.2   114   F  1    444  01 11 00

01 13 00  3C66A        20 36 22  22.6  52.2 -5.8     -68.5    -6   1  1    444  01 13 00
01 14 10  ---          20 37 33  22.8  52.2 -5.8     -68.7    64   F  1    448  01 13 00

01 16 30  3C66A        20 39 53  23.2  52.4 -5.7     -69.0   133   1  1    448  01 16 30
01 17 40  ---          20 41 03  23.4  52.5 -5.7     -69.2    70   F  1    453  01 16 48

01 17 40  SN1986J      20 41 03  23.2  53.2 -5.7     -68.9    -6   1  1    453  01 17 40
01 19 40  ---          20 43 03  23.5  53.4 -5.7     -69.2   114   F  1    461  01 17 40

01 19 40  3C66A        20 43 03  23.7  52.6 -5.7     -69.4    -6   1  1    461  01 19 40
01 20 50  ---          20 44 14  23.9  52.7 -5.7     -69.6    64   F  1    465  01 19 40

01 20 50  SN1986J      20 44 14  23.7  53.5 -5.6     -69.3    -6   1  1    465  01 20 50
01 22 50  ---          20 46 14  24.0  53.6 -5.6     -69.6   114   F  1    473  01 20 50

01 22 50  3C66A        20 46 14  24.3  52.9 -5.6     -69.9    -6   1  1    473  01 22 50
01 24 00  ---          20 47 24  24.5  52.9 -5.6     -70.1    64   F  1    477  01 22 50

01 24 00  SN1986J      20 47 24  24.2  53.7 -5.6     -69.8    -6   1  1    477  01 24 00
01 26 00  ---          20 49 24  24.6  53.8 -5.6     -70.1   114   F  1    485  01 24 00
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

01 26 00  3C66A        20 49 24  24.8  53.1 -5.6     -70.3    -6   1  1    485  01 26 00
01 27 10  ---          20 50 35  25.0  53.2 -5.5     -70.5    64   F  1    490  01 26 00

01 27 10  SN1986J      20 50 35  24.8  53.9 -5.5     -70.2    -6   1  1    490  01 27 10
01 29 10  ---          20 52 35  25.1  54.0 -5.5     -70.5   114   F  1    497  01 27 10

01 29 10  3C66A        20 52 35  25.4  53.3 -5.5     -70.8    -6   1  1    497  01 29 10
01 30 20  ---          20 53 45  25.6  53.4 -5.5     -71.0    64   F  1    502  01 29 10

01 30 20  SN1986J      20 53 45  25.4  54.1 -5.5     -70.7    -6   1  1    502  01 30 20
01 32 20  ---          20 55 46  25.7  54.2 -5.5     -70.9   114   F  1    510  01 30 20

01 32 20  3C66A        20 55 46  25.9  53.5 -5.5     -71.3    -6   1  1    510  01 32 20
01 33 30  ---          20 56 56  26.1  53.6 -5.4     -71.4    64   F  1    514  01 32 20

01 35 50  3C66A        20 59 16  26.5  53.7 -5.4     -71.7   133   1  1    514  01 35 50
01 37 00  ---          21 00 26  26.7  53.8 -5.4     -71.9    70   F  1    519  01 36 08

01 37 00  SN1986J      21 00 26  26.5  54.6 -5.4     -71.6    -6   1  1    519  01 37 00
01 39 00  ---          21 02 27  26.9  54.7 -5.3     -71.9   114   F  1    526  01 37 00

01 39 00  3C66A        21 02 27  27.1  53.9 -5.3     -72.2    -6   1  1    526  01 39 00
01 40 10  ---          21 03 37  27.3  54.0 -5.3     -72.4    64   F  1    531  01 39 00

01 40 10  SN1986J      21 03 37  27.1  54.8 -5.3     -72.0    -6   1  1    531  01 40 10
01 42 10  ---          21 05 37  27.4  54.9 -5.3     -72.3   114   F  1    539  01 40 10

01 42 10  3C66A        21 05 37  27.6  54.1 -5.3     -72.7    -6   1  1    539  01 42 10
01 43 20  ---          21 06 47  27.8  54.2 -5.3     -72.8    64   F  1    543  01 42 10

01 43 20  SN1986J      21 06 47  27.6  55.0 -5.3     -72.5    -6   1  1    543  01 43 20
01 45 20  ---          21 08 48  28.0  55.1 -5.2     -72.8   114   F  1    551  01 43 20

01 45 20  3C66A        21 08 48  28.2  54.3 -5.2     -73.1    -6   1  1    551  01 45 20
01 46 30  ---          21 09 58  28.4  54.4 -5.2     -73.3    64   F  1    555  01 45 20

01 46 30  SN1986J      21 09 58  28.2  55.2 -5.2     -72.9    -6   1  1    555  01 46 30
01 48 30  ---          21 11 58  28.5  55.3 -5.2     -73.2   114   F  1    563  01 46 30

01 48 30  3C66A        21 11 58  28.7  54.5 -5.2     -73.6    -6   1  1    563  01 48 30
01 49 40  ---          21 13 08  28.9  54.6 -5.2     -73.7    64   F  1    568  01 48 30
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

01 49 40  SN1986J      21 13 08  28.8  55.4 -5.2     -73.4    -6   1  1    568  01 49 40
01 51 40  ---          21 15 09  29.1  55.5 -5.1     -73.7   114   F  1    575  01 49 40

01 51 40  3C66A        21 15 09  29.3  54.7 -5.1     -74.0    -6   1  1    575  01 51 40
01 52 50  ---          21 16 19  29.5  54.8 -5.1     -74.2    64   F  1    580  01 51 40

01 55 10  3C66A        21 18 39  29.9  54.9 -5.1     -74.5   133   1  1    580  01 55 10
01 56 20  ---          21 19 49  30.1  55.0 -5.1     -74.7    70   F  1    584  01 55 28

01 56 20  SN1986J      21 19 49  29.9  55.7 -5.1     -74.3    -6   1  1    584  01 56 20
01 58 20  ---          21 21 50  30.3  55.9 -5.0     -74.6   114   F  1    592  01 56 20

01 58 20  3C66A        21 21 50  30.5  55.1 -5.0     -75.0    -6   1  1    592  01 58 20
01 59 30  ---          21 23 00  30.7  55.1 -5.0     -75.1    64   F  1    597  01 58 20

01 59 30  SN1986J      21 23 00  30.5  55.9 -5.0     -74.7    -6   1  1    597  01 59 30
02 01 30  ---          21 25 00  30.9  56.0 -5.0     -75.0   114   F  1    604  01 59 30

02 01 30  3C66A        21 25 00  31.0  55.2 -5.0     -75.4    -6   1  1    604  02 01 30
02 02 40  ---          21 26 11  31.2  55.3 -5.0     -75.6    64   F  1    609  02 01 30

02 02 40  SN1986J      21 26 11  31.1  56.1 -4.9     -75.2    -6   1  1    609  02 02 40
02 04 40  ---          21 28 11  31.4  56.2 -4.9     -75.5   114   F  1    617  02 02 40

02 04 40  3C66A        21 28 11  31.6  55.4 -4.9     -75.9    -6   1  1    617  02 04 40
02 05 50  ---          21 29 21  31.8  55.5 -4.9     -76.0    64   F  1    621  02 04 40

02 05 50  SN1986J      21 29 21  31.6  56.3 -4.9     -75.6    -6   1  1    621  02 05 50
02 07 50  ---          21 31 21  32.0  56.4 -4.9     -75.9   114   F  1    629  02 05 50

02 07 50  3C66A        21 31 21  32.1  55.6 -4.9     -76.3    -6   1  1    629  02 07 50
02 09 00  ---          21 32 32  32.4  55.6 -4.8     -76.5    64   F  1    634  02 07 50

02 09 00  SN1986J      21 32 32  32.2  56.4 -4.8     -76.1    -6   1  1    634  02 09 00
02 11 00  ---          21 34 32  32.6  56.6 -4.8     -76.4   114   F  1    641  02 09 00

02 11 00  3C66A        21 34 32  32.7  55.7 -4.8     -76.8    -6   1  1    641  02 11 00
02 12 10  ---          21 35 42  32.9  55.8 -4.8     -77.0    64   F  1    646  02 11 00

02 14 30  3C66A        21 38 02  33.3  55.9 -4.8     -77.3   133   1  1    646  02 14 30
02 15 40  ---          21 39 13  33.5  56.0 -4.7     -77.5    70   F  1    650  02 14 48
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

02 15 40  SN1986J      21 39 13  33.4  56.8 -4.7     -77.0    -6   1  1    650  02 15 40
02 17 40  ---          21 41 13  33.8  56.9 -4.7     -77.3   114   F  1    658  02 15 40

02 17 40  3C66A        21 41 13  33.9  56.1 -4.7     -77.7    -6   1  1    658  02 17 40
02 18 50  ---          21 42 23  34.1  56.1 -4.7     -77.9    64   F  1    663  02 17 40

02 18 50  SN1986J      21 42 23  34.0  56.9 -4.7     -77.5    -6   1  1    663  02 18 50
02 20 50  ---          21 44 23  34.3  57.0 -4.6     -77.8   114   F  1    670  02 18 50

02 20 50  3C66A        21 44 23  34.5  56.2 -4.6     -78.2    -6   1  1    670  02 20 50
02 22 00  ---          21 45 34  34.7  56.3 -4.6     -78.4    64   F  1    675  02 20 50

02 22 00  SN1986J      21 45 34  34.6  57.1 -4.6     -77.9    -6   1  1    675  02 22 00
02 24 00  ---          21 47 34  34.9  57.2 -4.6     -78.2   114   F  1    683  02 22 00

02 24 00  3C66A        21 47 34  35.0  56.3 -4.6     -78.7    -6   1  1    683  02 24 00
02 25 10  ---          21 48 44  35.2  56.4 -4.6     -78.8    64   F  1    687  02 24 00

02 25 10  SN1986J      21 48 44  35.1  57.2 -4.6     -78.4    -6   1  1    687  02 25 10
02 27 10  ---          21 50 45  35.5  57.3 -4.5     -78.7   114   F  1    695  02 25 10

02 27 10  3C66A        21 50 45  35.6  56.5 -4.5     -79.1    -6   1  1    695  02 27 10
02 28 20  ---          21 51 55  35.8  56.5 -4.5     -79.3    64   F  1    699  02 27 10

02 28 20  SN1986J      21 51 55  35.7  57.4 -4.5     -78.8    -6   1  1    699  02 28 20
02 30 20  ---          21 53 55  36.1  57.5 -4.5     -79.1   114   F  1    707  02 28 20

02 30 20  3C66A        21 53 55  36.2  56.6 -4.5     -79.6    -6   1  1    707  02 30 20
02 31 30  ---          21 55 05  36.4  56.7 -4.5     -79.8    64   F  1    712  02 30 20

02 33 50  3C66A        21 57 26  36.8  56.8 -4.4     -80.1   133   1  1    712  02 33 50
02 35 00  ---          21 58 36  37.0  56.8 -4.4     -80.3    70   F  1    716  02 34 08

02 35 00  SN1986J      21 58 36  36.9  57.7 -4.4     -79.8    -6   1  1    716  02 35 00
02 37 00  ---          22 00 36  37.3  57.7 -4.4     -80.1   114   F  1    724  02 35 00

02 37 00  3C66A        22 00 36  37.4  56.9 -4.4     -80.6    -6   1  1    724  02 37 00
02 38 10  ---          22 01 46  37.6  56.9 -4.4     -80.8    64   F  1    728  02 37 00

02 38 10  SN1986J      22 01 46  37.5  57.8 -4.4     -80.2    -6   1  1    728  02 38 10
02 40 10  ---          22 03 47  37.9  57.9 -4.3     -80.5   114   F  1    736  02 38 10
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

02 40 10  3C66A        22 03 47  37.9  57.0 -4.3     -81.1    -6   1  1    736  02 40 10
02 41 20  ---          22 04 57  38.2  57.0 -4.3     -81.2    64   F  1    741  02 40 10

02 41 20  SN1986J      22 04 57  38.1  57.9 -4.3     -80.7    -6   1  1    741  02 41 20
02 43 20  ---          22 06 57  38.4  58.0 -4.3     -81.0   114   F  1    748  02 41 20

02 43 20  3C66A        22 06 57  38.5  57.1 -4.3     -81.5    -6   1  1    748  02 43 20
02 44 30  ---          22 08 07  38.7  57.1 -4.3     -81.7    64   F  1    753  02 43 20

02 44 30  SN1986J      22 08 07  38.7  58.0 -4.2     -81.2    -6   1  1    753  02 44 30
02 46 30  ---          22 10 08  39.0  58.1 -4.2     -81.5   114   F  1    761  02 44 30

02 46 30  3C66A        22 10 08  39.1  57.2 -4.2     -82.0    -6   1  1    761  02 46 30
02 47 40  ---          22 11 18  39.3  57.2 -4.2     -82.2    64   F  1    765  02 46 30

02 47 40  SN1986J      22 11 18  39.2  58.1 -4.2     -81.6    -6   1  1    765  02 47 40
02 49 40  ---          22 13 18  39.6  58.2 -4.2     -81.9   114   F  1    773  02 47 40

02 49 40  3C66A        22 13 18  39.7  57.3 -4.2     -82.5    -6   1  1    773  02 49 40
02 50 50  ---          22 14 28  39.9  57.3 -4.1     -82.7    64   F  1    777  02 49 40

02 53 10  3C66A        22 16 49  40.3  57.4 -4.1     -83.0   133   1  1    777  02 53 10
02 54 20  ---          22 17 59  40.5  57.4 -4.1     -83.2    70   F  1    782  02 53 28

02 54 20  SN1986J      22 17 59  40.5  58.4 -4.1     -82.6    -6   1  1    782  02 54 20
02 56 20  ---          22 19 59  40.8  58.4 -4.1     -82.9   114   F  1    790  02 54 20

02 56 20  3C66A        22 19 59  40.9  57.5 -4.1     -83.5    -6   1  1    790  02 56 20
02 57 30  ---          22 21 10  41.1  57.5 -4.0     -83.7    64   F  1    794  02 56 20

02 57 30  SN1986J      22 21 10  41.0  58.5 -4.0     -83.1    -6   1  1    794  02 57 30
02 59 30  ---          22 23 10  41.4  58.5 -4.0     -83.4   114   F  1    802  02 57 30

02 59 30  3C66A        22 23 10  41.5  57.6 -4.0     -84.0    -6   1  1    802  02 59 30
03 00 40  ---          22 24 20  41.7  57.6 -4.0     -84.2    64   F  1    806  02 59 30

03 00 40  SN1986J      22 24 20  41.6  58.6 -4.0     -83.6    -6   1  1    806  03 00 40
03 02 40  ---          22 26 20  42.0  58.6 -3.9     -83.9   114   F  1    814  03 00 40

03 02 40  3C66A        22 26 20  42.0  57.7 -3.9     -84.5    -6   1  1    814  03 02 40
03 03 50  ---          22 27 31  42.2  57.7 -3.9     -84.7    64   F  1    819  03 02 40
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

03 03 50  SN1986J      22 27 31  42.2  58.6 -3.9     -84.0    -6   1  1    819  03 03 50
03 05 50  ---          22 29 31  42.6  58.7 -3.9     -84.3   114   F  1    826  03 03 50

03 05 50  3C66A        22 29 31  42.6  57.7 -3.9     -85.0    -6   1  1    826  03 05 50
03 07 00  ---          22 30 41  42.8  57.8 -3.9     -85.1    64   F  1    831  03 05 50

03 07 00  SN1986J      22 30 41  42.8  58.7 -3.9     -84.5    -6   1  1    831  03 07 00
03 09 00  ---          22 32 41  43.2  58.8 -3.8     -84.8   114   F  1    839  03 07 00

03 09 00  3C66A        22 32 41  43.2  57.8 -3.8     -85.5    -6   1  1    839  03 09 00
03 10 10  ---          22 33 52  43.4  57.8 -3.8     -85.6    64   F  1    843  03 09 00

03 12 30  3C66A        22 36 12  43.8  57.9 -3.8     -86.0   133   1  1    843  03 12 30
03 13 40  ---          22 37 22  44.0  57.9 -3.8     -86.2    70   F  1    848  03 12 48

03 13 40  SN1986J      22 37 22  44.0  58.9 -3.8     -85.5    -6   1  1    848  03 13 40
03 15 40  ---          22 39 22  44.4  58.9 -3.7     -85.9   114   F  1    855  03 13 40

03 15 40  3C66A        22 39 22  44.4  57.9 -3.7     -86.5    -6   1  1    855  03 15 40
03 16 50  ---          22 40 33  44.6  57.9 -3.7     -86.7    64   F  1    860  03 15 40

03 16 50  SN1986J      22 40 33  44.6  58.9 -3.7     -86.0    -6   1  1    860  03 16 50
03 18 50  ---          22 42 33  45.0  59.0 -3.7     -86.4   114   F  1    868  03 16 50

03 18 50  3C66A        22 42 33  45.0  58.0 -3.7     -87.0    -6   1  1    868  03 18 50
03 20 00  ---          22 43 43  45.2  58.0 -3.7     -87.2    64   F  1    872  03 18 50

03 20 00  SN1986J      22 43 43  45.2  59.0 -3.7     -86.5    -6   1  1    872  03 20 00
03 22 00  ---          22 45 44  45.6  59.0 -3.6     -86.9   114   F  1    880  03 20 00

03 22 00  3C66A        22 45 44  45.6  58.0 -3.6     -87.5    -6   1  1    880  03 22 00
03 23 10  ---          22 46 54  45.8  58.0 -3.6     -87.7    64   F  1    884  03 22 00

03 23 10  SN1986J      22 46 54  45.8  59.0 -3.6     -87.0    -6   1  1    884  03 23 10
03 25 10  ---          22 48 54  46.1  59.1 -3.6     -87.4   114   F  1    892  03 23 10

03 25 10  3C66A        22 48 54  46.1  58.0 -3.6     -88.1    -6   1  1    892  03 25 10
03 26 20  ---          22 50 04  46.4  58.0 -3.6     -88.3    64   F  1    897  03 25 10

03 26 20  SN1986J      22 50 04  46.4  59.1 -3.6     -87.5    -6   1  1    897  03 26 20
03 28 20  ---          22 52 05  46.7  59.1 -3.5     -87.9   114   F  1    904  03 26 20
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

03 28 20  3C66A        22 52 05  46.7  58.1 -3.5     -88.6    -6   1  1    904  03 28 20
03 29 30  ---          22 53 15  46.9  58.1 -3.5     -88.8    64   F  1    909  03 28 20

03 31 50  3C66A        22 55 35  47.4  58.1 -3.5     -89.2   133   1  1    909  03 31 50
03 33 00  ---          22 56 45  47.6  58.1 -3.4     -89.4    70   F  1    913  03 32 08

03 33 00  SN1986J      22 56 45  47.6  59.1 -3.4     -88.6    -6   1  1    913  03 33 00
03 35 00  ---          22 58 46  48.0  59.1 -3.4     -89.0   114   F  1    921  03 33 00

03 35 00  3C66A        22 58 46  47.9  58.1 -3.4     -89.7    -6   1  1    921  03 35 00
03 36 10  ---          22 59 56  48.2  58.1 -3.4     -89.9    64   F  1    926  03 35 00

03 36 10  SN1986J      22 59 56  48.2  59.1 -3.4     -89.2    -6   1  1    926  03 36 10
03 38 10  ---          23 01 56  48.5  59.2 -3.4     -89.5   114   F  1    933  03 36 10

03 38 10  3C66A        23 01 56  48.5  58.1 -3.4     -90.3    -6   1  1    933  03 38 10
03 39 20  ---          23 03 06  48.7  58.1 -3.3     -90.5    64   F  1    938  03 38 10

03 39 20  SN1986J      23 03 06  48.8  59.2 -3.3     -89.7    -6   1  1    938  03 39 20
03 41 20  ---          23 05 07  49.1  59.2 -3.3     -90.0   114   F  1    946  03 39 20

03 41 20  3C66A        23 05 07  49.1  58.1 -3.3     -90.8    -6   1  1    946  03 41 20
03 42 30  ---          23 06 17  49.3  58.1 -3.3     -91.0    64   F  1    950  03 41 20

03 42 30  SN1986J      23 06 17  49.4  59.2 -3.3     -90.2    -6   1  1    950  03 42 30
03 44 30  ---          23 08 17  49.7  59.2 -3.2     -90.6   114   F  1    958  03 42 30

03 44 30  3C66A        23 08 17  49.7  58.1 -3.2     -91.4    -6   1  1    958  03 44 30
03 45 40  ---          23 09 27  49.9  58.1 -3.2     -91.6    64   F  1    963  03 44 30

03 45 40  SN1986J      23 09 27  49.9  59.1 -3.2     -90.8    -6   1  1    963  03 45 40
03 47 40  ---          23 11 28  50.3  59.1 -3.2     -91.1   114   F  1    970  03 45 40

03 47 40  3C66A        23 11 28  50.3  58.0 -3.2     -91.9    -6   1  1    970  03 47 40
03 48 50  ---          23 12 38  50.5  58.0 -3.2     -92.1    64   F  1    975  03 47 40

03 51 10  3C66A        23 14 58  50.9  58.0 -3.1     -92.6   133   1  1    975  03 51 10
03 52 20  ---          23 16 09  51.1  58.0 -3.1     -92.8    70   F  1    979  03 51 28

03 52 20  SN1986J      23 16 09  51.2  59.1 -3.1     -91.9    -6   1  1    979  03 52 20
03 54 20  ---          23 18 09  51.5  59.1 -3.1     -92.3   114   F  1    987  03 52 20
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

03 54 20  3C66A        23 18 09  51.5  58.0 -3.1     -93.1    -6   1  1    987  03 54 20
03 55 30  ---          23 19 19  51.7  57.9 -3.1     -93.3    64   F  1    992  03 54 20

03 55 30  SN1986J      23 19 19  51.8  59.1 -3.1     -92.5    -6   1  1    992  03 55 30
03 57 30  ---          23 21 19  52.1  59.0 -3.0     -92.8   114   F  1    999  03 55 30

03 57 30  3C66A        23 21 19  52.1  57.9 -3.0     -93.7    -6   1  1    999  03 57 30
03 58 40  ---          23 22 30  52.3  57.9 -3.0     -93.9    64   F  1   1004  03 57 30

03 58 40  SN1986J      23 22 30  52.3  59.0 -3.0     -93.1    -6   1  1   1004  03 58 40
04 00 40  ---          23 24 30  52.7  59.0 -3.0     -93.4   114   F  1   1012  03 58 40

04 00 40  3C66A        23 24 30  52.6  57.8 -3.0     -94.3    -6   1  1   1012  04 00 40
04 01 50  ---          23 25 40  52.9  57.8 -3.0     -94.5    64   F  1   1016  04 00 40

04 01 50  SN1986J      23 25 40  52.9  59.0 -3.0     -93.6    -6   1  1   1016  04 01 50
04 03 50  ---          23 27 40  53.3  58.9 -2.9     -94.0   114   F  1   1024  04 01 50

04 03 50  3C66A        23 27 40  53.2  57.8 -2.9     -94.9    -6   1  1   1024  04 03 50
04 05 00  ---          23 28 51  53.4  57.7 -2.9     -95.1    64   F  1   1028  04 03 50

04 05 00  SN1986J      23 28 51  53.5  58.9 -2.9     -94.2    -7   1  1   1028  04 05 00
04 07 00  ---          23 30 51  53.9  58.8 -2.9     -94.6   113   F  1   1036  04 05 00

04 07 00  3C66A        23 30 51  53.8  57.7 -2.9     -95.5    -7   1  1   1036  04 07 00
04 08 10  ---          23 32 01  54.0  57.6 -2.9     -95.8    63   F  1   1041  04 07 00

04 10 30  3C66A        23 34 22  54.4  57.6 -2.8     -96.2   133   1  1   1041  04 10 30
04 11 40  ---          23 35 32  54.6  57.5 -2.8     -96.4    70   F  1   1045  04 10 48

04 11 40  SN1986J      23 35 32  54.7  58.7 -2.8     -95.5    -7   1  1   1045  04 11 40
04 13 40  ---          23 37 32  55.1  58.7 -2.8     -95.9   113   F  1   1053  04 11 40

04 13 40  3C66A        23 37 32  55.0  57.4 -2.8     -96.9    -7   1  1   1053  04 13 40
04 14 50  ---          23 38 42  55.2  57.4 -2.7     -97.1    63   F  1   1057  04 13 40

04 14 50  SN1986J      23 38 42  55.3  58.6 -2.7     -96.1    -7   1  1   1057  04 14 50
04 16 50  ---          23 40 43  55.7  58.5 -2.7     -96.5   113   F  1   1065  04 14 50

04 16 50  3C66A        23 40 43  55.6  57.3 -2.7     -97.5    -7   1  1   1065  04 16 50
04 18 00  ---          23 41 53  55.8  57.3 -2.7     -97.7    63   F  1   1070  04 16 50
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

04 18 00  SN1986J      23 41 53  55.9  58.5 -2.7     -96.7    -7   1  1   1070  04 18 00
04 20 00  ---          23 43 53  56.3  58.4 -2.7     -97.1   113   F  1   1077  04 18 00

04 20 00  3C66A        23 43 53  56.2  57.2 -2.7     -98.2    -7   1  1   1077  04 20 00
04 21 10  ---          23 45 03  56.4  57.1 -2.6     -98.4    63   F  1   1082  04 20 00

04 21 10  SN1986J      23 45 03  56.5  58.4 -2.6     -97.4    -7   1  1   1082  04 21 10
04 23 10  ---          23 47 04  56.9  58.3 -2.6     -97.8   113   F  1   1090  04 21 10

04 23 10  3C66A        23 47 04  56.7  57.0 -2.6     -98.8    -7   1  1   1090  04 23 10
04 24 20  ---          23 48 14  56.9  57.0 -2.6     -99.1    63   F  1   1094  04 23 10

04 24 20  SN1986J      23 48 14  57.1  58.2 -2.6     -98.0    -7   1  1   1094  04 24 20
04 26 20  ---          23 50 14  57.4  58.1 -2.5     -98.5   113   F  1   1102  04 24 20

04 26 20  3C66A        23 50 14  57.3  56.8 -2.6     -99.5    -7   1  1   1102  04 26 20
04 27 30  ---          23 51 24  57.5  56.8 -2.5     -99.8    63   F  1   1106  04 26 20

04 29 50  3C66A        23 53 45  57.9  56.6 -2.5    -100.3   133   1  1   1106  04 29 50
04 31 00  ---          23 54 55  58.1  56.6 -2.5    -100.5    70   F  1   1111  04 30 08

04 31 00  SN1986J      23 54 55  58.3  57.9 -2.5     -99.5    -7   1  1   1111  04 31 00
04 33 00  ---          23 56 55  58.7  57.8 -2.4     -99.9   113   F  1   1119  04 31 00

04 33 00  3C66A        23 56 55  58.5  56.4 -2.4    -101.0    -7   1  1   1119  04 33 00
04 34 10  ---          23 58 05  58.7  56.4 -2.4    -101.3    63   F  1   1123  04 33 00

04 34 10  SN1986J      23 58 05  58.9  57.7 -2.4    -100.2    -7   1  1   1123  04 34 10
04 36 10  ---          00 00 06  59.2  57.6 -2.4    -100.6   113   F  1   1131  04 34 10

04 36 10  3C66A        00 00 06  59.1  56.2 -2.4    -101.7    -7   1  1   1131  04 36 10
04 37 20  ---          00 01 16  59.3  56.1 -2.4    -102.0    63   F  1   1135  04 36 10

04 37 20  SN1986J      00 01 16  59.4  57.5 -2.4    -100.9    -7   1  1   1135  04 37 20
04 39 20  ---          00 03 16  59.8  57.3 -2.3    -101.3   113   F  1   1143  04 37 20

04 39 20  3C66A        00 03 16  59.6  56.0 -2.3    -102.5    -7   1  1   1143  04 39 20
04 40 30  ---          00 04 26  59.8  55.9 -2.3    -102.8    63   F  1   1148  04 39 20

04 40 30  SN1986J      00 04 26  60.0  57.2 -2.3    -101.6    -7   1  1   1148  04 40 30
04 42 30  ---          00 06 27  60.4  57.1 -2.3    -102.1   113   F  1   1155  04 40 30
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

04 42 30  3C66A        00 06 27  60.2  55.7 -2.3    -103.2    -7   1  1   1155  04 42 30
04 43 40  ---          00 07 37  60.4  55.6 -2.3    -103.5    63   F  1   1160  04 42 30

04 43 40  SN1986J      00 07 37  60.6  57.0 -2.3    -102.4    -7   1  1   1160  04 43 40
04 45 40  ---          00 09 37  61.0  56.8 -2.2    -102.8   113   F  1   1168  04 43 40

04 45 40  3C66A        00 09 37  60.8  55.4 -2.2    -104.0    -7   1  1   1168  04 45 40
04 46 50  ---          00 10 47  61.0  55.3 -2.2    -104.3    63   F  1   1172  04 45 40

04 49 10  3C66A        00 13 08  61.4  55.1 -2.2    -104.9   133   1  1   1172  04 49 10
04 50 20  ---          00 14 18  61.6  55.0 -2.1    -105.2    70   F  1   1177  04 49 28

04 50 20  SN1986J      00 14 18  61.8  56.4 -2.1    -104.0    -7   1  1   1177  04 50 20
04 52 20  ---          00 16 18  62.2  56.2 -2.1    -104.5   113   F  1   1184  04 50 20

04 52 20  3C66A        00 16 18  61.9  54.8 -2.1    -105.7    -7   1  1   1184  04 52 20
04 53 30  ---          00 17 29  62.2  54.7 -2.1    -106.1    63   F  1   1189  04 52 20

04 53 30  SN1986J      00 17 29  62.4  56.1 -2.1    -104.8    -7   1  1   1189  04 53 30
04 55 30  ---          00 19 29  62.7  55.9 -2.1    -105.3   113   F  1   1197  04 53 30

04 55 30  3C66A        00 19 29  62.5  54.4 -2.1    -106.6    -7   1  1   1197  04 55 30
04 56 40  ---          00 20 39  62.7  54.3 -2.0    -106.9    63   F  1   1201  04 55 30

04 56 40  SN1986J      00 20 39  62.9  55.8 -2.0    -105.6    -7   1  1   1201  04 56 40
04 58 40  ---          00 22 39  63.3  55.5 -2.0    -106.2   113   F  1   1209  04 56 40

04 58 40  3C66A        00 22 39  63.1  54.1 -2.0    -107.5    -7   1  1   1209  04 58 40
04 59 50  ---          00 23 50  63.3  53.9 -2.0    -107.8    63   F  1   1213  04 58 40

04 59 50  SN1986J      00 23 50  63.5  55.4 -2.0    -106.5    -7   1  1   1213  04 59 50
05 01 50  ---          00 25 50  63.9  55.2 -2.0    -107.0   113   F  1   1221  04 59 50

05 01 50  3C66A        00 25 50  63.6  53.7 -2.0    -108.4    -7   1  1   1221  05 01 50
05 03 00  ---          00 27 00  63.8  53.5 -1.9    -108.7    63   F  1   1226  05 01 50

05 03 00  SN1986J      00 27 00  64.1  55.0 -1.9    -107.4    -7   1  1   1226  05 03 00
05 05 00  ---          00 29 00  64.4  54.8 -1.9    -107.9   113   F  1   1233  05 03 00

05 05 00  3C66A        00 29 00  64.2  53.2 -1.9    -109.3    -7   1  1   1233  05 05 00
05 06 10  ---          00 30 11  64.4  53.1 -1.9    -109.6    63   F  1   1238  05 05 00
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

05 08 30  3C66A        00 32 31  64.8  52.7 -1.8    -110.3   133   1  1   1238  05 08 30
05 09 40  ---          00 33 41  65.0  52.6 -1.8    -110.7    70   F  1   1243  05 08 48

05 09 40  SN1986J      00 33 41  65.2  54.1 -1.8    -109.3    -7   1  1   1243  05 09 40
05 11 40  ---          00 35 42  65.6  53.8 -1.8    -109.9   113   F  1   1250  05 09 40

05 11 40  3C66A        00 35 42  65.3  52.3 -1.8    -111.3    -7   1  1   1250  05 11 40
05 12 50  ---          00 36 52  65.5  52.1 -1.8    -111.7    63   F  1   1255  05 11 40

05 12 50  SN1986J      00 36 52  65.8  53.6 -1.8    -110.3    -7   1  1   1255  05 12 50
05 14 50  ---          00 38 52  66.1  53.3 -1.7    -110.9   113   F  1   1263  05 12 50

05 14 50  3C66A        00 38 52  65.8  51.7 -1.7    -112.3    -7   1  1   1263  05 14 50
05 16 00  ---          00 40 02  66.0  51.5 -1.7    -112.7    63   F  1   1267  05 14 50

05 16 00  SN1986J      00 40 02  66.3  53.1 -1.7    -111.3    -7   1  1   1267  05 16 00
05 18 00  ---          00 42 03  66.7  52.8 -1.7    -111.9   113   F  1   1275  05 16 00

05 18 00  3C66A        00 42 03  66.4  51.2 -1.7    -113.4    -7   1  1   1275  05 18 00
05 19 10  ---          00 43 13  66.6  51.0 -1.7    -113.8    63   F  1   1279  05 18 00

05 19 10  SN1986J      00 43 13  66.9  52.6 -1.7    -112.3    -7   1  1   1279  05 19 10
05 21 10  ---          00 45 13  67.2  52.2 -1.6    -113.0   113   F  1   1287  05 19 10

05 21 10  3C66A        00 45 13  66.9  50.6 -1.6    -114.5    -7   1  1   1287  05 21 10
05 22 20  ---          00 46 23  67.1  50.4 -1.6    -114.9    63   F  1   1292  05 21 10

05 22 20  SN1986J      00 46 23  67.4  52.0 -1.6    -113.4    -7   1  1   1292  05 22 20
05 24 20  ---          00 48 24  67.8  51.6 -1.6    -114.1   113   F  1   1299  05 22 20

05 24 20  3C66A        00 48 24  67.4  50.0 -1.6    -115.6    -7   1  1   1299  05 24 20
05 25 30  ---          00 49 34  67.6  49.7 -1.6    -116.0    63   F  1   1304  05 24 20

05 27 50  3C66A        00 51 54  68.0  49.2 -1.5    -116.9   134   1  1   1304  05 27 50
05 29 00  ---          00 53 04  68.2  48.9 -1.5    -117.3    70   F  1   1308  05 28 08

05 29 00  SN1986J      00 53 04  68.5  50.6 -1.5    -115.8    -7   1  1   1308  05 29 00
05 31 00  ---          00 55 05  68.9  50.2 -1.5    -116.6   113   F  1   1316  05 29 00

05 31 00  3C66A        00 55 05  68.5  48.5 -1.5    -118.1    -7   1  1   1316  05 31 00
05 32 10  ---          00 56 15  68.7  48.2 -1.5    -118.6    63   F  1   1321  05 31 00
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

05 32 10  SN1986J      00 56 15  69.1  49.9 -1.4    -117.0    -7   1  1   1321  05 32 10
05 34 10  ---          00 58 15  69.4  49.4 -1.4    -117.8   113   F  1   1328  05 32 10

05 34 10  3C66A        00 58 15  69.0  47.7 -1.4    -119.4    -7   1  1   1328  05 34 10
05 35 20  ---          00 59 25  69.2  47.4 -1.4    -119.8    63   F  1   1333  05 34 10

05 35 20  SN1986J      00 59 25  69.6  49.1 -1.4    -118.3    -7   1  1   1333  05 35 20
05 37 20  ---          01 01 26  69.9  48.6 -1.4    -119.1   113   F  1   1341  05 35 20

05 37 20  3C66A        01 01 26  69.5  46.9 -1.4    -120.7    -7   1  1   1341  05 37 20
05 38 30  ---          01 02 36  69.7  46.6 -1.3    -121.2    63   F  1   1345  05 37 20

05 38 30  SN1986J      01 02 36  70.1  48.3 -1.3    -119.6    -7   1  1   1345  05 38 30
05 40 30  ---          01 04 36  70.4  47.8 -1.3    -120.4   113   F  1   1353  05 38 30

05 40 30  3C66A        01 04 36  70.0  46.0 -1.3    -122.0    -7   1  1   1353  05 40 30
05 41 40  ---          01 05 46  70.2  45.7 -1.3    -122.6    63   F  1   1357  05 40 30

05 41 40  SN1986J      01 05 46  70.6  47.4 -1.3    -120.9    -7   1  1   1357  05 41 40
05 43 40  ---          01 07 47  70.9  46.8 -1.3    -121.8   113   F  1   1365  05 41 40

05 43 40  3C66A        01 07 47  70.5  45.1 -1.3    -123.5    -7   1  1   1365  05 43 40
05 44 50  ---          01 08 57  70.7  44.7 -1.2    -124.0    63   F  1   1370  05 43 40

05 47 10  3C66A        01 11 17  71.0  44.0 -1.2    -125.1   134   1  1   1370  05 47 10
05 48 20  ---          01 12 28  71.2  43.6 -1.2    -125.7    70   F  1   1374  05 47 28

05 48 20  SN1986J      01 12 28  71.6  45.4 -1.2    -124.0    -7   1  1   1374  05 48 20
05 50 20  ---          01 14 28  71.9  44.7 -1.1    -125.0   113   F  1   1382  05 48 20

05 50 20  3C66A        01 14 28  71.5  42.9 -1.1    -126.6    -7   1  1   1382  05 50 20
05 51 30  ---          01 15 38  71.7  42.5 -1.1    -127.2    63   F  1   1386  05 50 20

05 51 30  SN1986J      01 15 38  72.1  44.3 -1.1    -125.6    -7   1  1   1386  05 51 30
05 53 30  ---          01 17 38  72.4  43.6 -1.1    -126.6   113   F  1   1394  05 51 30

05 53 30  3C66A        01 17 38  72.0  41.8 -1.1    -128.2    -7   1  1   1394  05 53 30
05 54 40  ---          01 18 49  72.1  41.4 -1.1    -128.9    63   F  1   1399  05 53 30

05 54 40  SN1986J      01 18 49  72.6  43.2 -1.1    -127.2    -7   1  1   1399  05 54 40
05 56 40  ---          01 20 49  72.9  42.4 -1.0    -128.3   113   F  1   1406  05 54 40
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

05 56 40  3C66A        01 20 49  72.4  40.6 -1.0    -129.9    -7   1  1   1406  05 56 40
05 57 50  ---          01 21 59  72.6  40.2 -1.0    -130.6    63   F  1   1411  05 56 40

05 57 50  SN1986J      01 21 59  73.1  41.9 -1.0    -128.9    -7   1  1   1411  05 57 50
05 59 50  ---          01 23 59  73.3  41.1 -1.0    -130.0   113   F  1   1419  05 57 50

05 59 50  3C66A        01 23 59  72.9  39.3 -1.0    -131.7    -7   1  1   1419  05 59 50
06 01 00  ---          01 25 10  73.0  38.9 -1.0    -132.4    63   F  1   1423  05 59 50

06 01 00  SN1986J      01 25 10  73.5  40.6 -1.0    -130.7    -7   1  1   1423  06 01 00
06 03 00  ---          01 27 10  73.8  39.8 -0.9    -131.9   113   F  1   1431  06 01 00

06 03 00  3C66A        01 27 10  73.3  38.0 -0.9    -133.5    -7   1  1   1431  06 03 00
06 04 10  ---          01 28 20  73.4  37.5 -0.9    -134.2    63   F  1   1435  06 03 00

06 07 10  3C84         01 31 21  65.6  56.0 -1.8    -107.7   158   1  1   1435  06 07 10
06 08 50  ---          01 33 01  65.9  55.7 -1.8    -108.2   100   F  1   1442  06 07 28

06 11 10  3C66A        01 35 21  74.3  34.1 -0.8    -138.6   117   1  1   1442  06 11 10
06 14 10  ---          01 38 22  74.7  32.6 -0.7    -140.7   180   F  1   1453  06 11 28

06 14 10  SN1986J      01 38 22  75.2  34.2 -0.7    -139.1    -7   1  1   1453  06 14 10
06 16 10  ---          01 40 22  75.5  33.1 -0.7    -140.5   113   F  1   1461  06 14 10

06 16 10  3C66A        01 40 22  74.9  31.5 -0.7    -142.0    -7   1  1   1461  06 16 10
06 17 20  ---          01 41 32  75.0  30.8 -0.7    -142.9    63   F  1   1466  06 16 10

06 17 20  SN1986J      01 41 32  75.6  32.4 -0.7    -141.3    -7   1  1   1466  06 17 20
06 19 20  ---          01 43 33  75.8  31.3 -0.7    -142.8   113   F  1   1473  06 17 20

06 19 20  3C66A        01 43 33  75.3  29.7 -0.7    -144.3    -7   1  1   1473  06 19 20
06 20 30  ---          01 44 43  75.4  29.0 -0.6    -145.2    63   F  1   1478  06 19 20

06 20 30  SN1986J      01 44 43  76.0  30.5 -0.6    -143.7    -7   1  1   1478  06 20 30
06 22 30  ---          01 46 43  76.2  29.3 -0.6    -145.3   113   F  1   1486  06 20 30

06 22 30  3C66A        01 46 43  75.6  27.8 -0.6    -146.7    -7   1  1   1486  06 22 30
06 23 40  ---          01 47 53  75.7  27.0 -0.6    -147.6    63   F  1   1490  06 22 30

06 23 40  SN1986J      01 47 53  76.3  28.5 -0.6    -146.2    -7   1  1   1490  06 23 40
06 25 40  ---          01 49 54  76.5  27.2 -0.6    -147.8   113   F  1   1498  06 23 40
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

06 25 40  3C66A        01 49 54  75.9  25.8 -0.6    -149.2    -7   1  1   1498  06 25 40
06 26 50  ---          01 51 04  76.0  25.0 -0.5    -150.1    63   F  1   1502  06 25 40

06 26 50  SN1986J      01 51 04  76.6  26.4 -0.5    -148.8    -7   1  1   1502  06 26 50
06 28 50  ---          01 53 04  76.8  25.0 -0.5    -150.5   113   F  1   1510  06 26 50

06 28 50  3C66A        01 53 04  76.2  23.7 -0.5    -151.8    -7   1  1   1510  06 28 50
06 30 00  ---          01 54 14  76.3  22.9 -0.5    -152.7    63   F  1   1515  06 28 50

06 32 20  3C66A        01 56 35  76.5  21.3 -0.4    -154.7   133   1  1   1515  06 32 20
06 33 30  ---          01 57 45  76.6  20.4 -0.4    -155.7    70   F  1   1519  06 32 38

06 33 30  SN1986J      01 57 45  77.2  21.6 -0.4    -154.6    -7   1  1   1519  06 33 30
06 35 30  ---          01 59 45  77.4  20.1 -0.4    -156.4   113   F  1   1527  06 33 30

06 35 30  3C66A        01 59 45  76.7  19.0 -0.4    -157.5    -7   1  1   1527  06 35 30
06 36 40  ---          02 00 56  76.8  18.1 -0.4    -158.5    63   F  1   1532  06 35 30

06 36 40  SN1986J      02 00 56  77.4  19.2 -0.4    -157.5    -7   1  1   1532  06 36 40
06 38 40  ---          02 02 56  77.6  17.6 -0.3    -159.4   113   F  1   1539  06 36 40

06 38 40  3C66A        02 02 56  76.9  16.6 -0.3    -160.3    -7   1  1   1539  06 38 40
06 39 50  ---          02 04 06  77.0  15.7 -0.3    -161.4    63   F  1   1544  06 38 40

06 39 50  SN1986J      02 04 06  77.7  16.6 -0.3    -160.5    -7   1  1   1544  06 39 50
06 41 50  ---          02 06 06  77.8  15.0 -0.3    -162.5   113   F  1   1552  06 39 50

06 41 50  3C66A        02 06 06  77.1  14.2 -0.3    -163.3    -7   1  1   1552  06 41 50
06 43 00  ---          02 07 17  77.2  13.2 -0.3    -164.4    63   F  1   1556  06 41 50

06 43 00  SN1986J      02 07 17  77.8  14.0 -0.3    -163.6    -7   1  1   1556  06 43 00
06 45 00  ---          02 09 17  77.9  12.3 -0.2    -165.6   113   F  1   1564  06 43 00

06 45 00  3C66A        02 09 17  77.2  11.6 -0.2    -166.3    -7   1  1   1564  06 45 00
06 46 10  ---          02 10 27  77.3  10.7 -0.2    -167.4    63   F  1   1568  06 45 00

06 46 10  SN1986J      02 10 27  78.0  11.3 -0.2    -166.8    -7   1  1   1568  06 46 10
06 48 10  ---          02 12 27  78.1   9.6 -0.2    -168.8   113   F  1   1576  06 46 10

06 48 10  3C66A        02 12 27  77.4   9.1 -0.2    -169.3    -7   1  1   1576  06 48 10
06 49 20  ---          02 13 38  77.4   8.1 -0.2    -170.5    63   F  1   1581  06 48 10
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

06 51 40  3C66A        02 15 58  77.5   6.1 -0.1    -172.8   133   1  1   1581  06 51 40
06 52 50  ---          02 17 08  77.5   5.2 -0.1    -173.9    70   F  1   1585  06 51 58

06 52 50  SN1986J      02 17 08  78.2   5.4 -0.1    -173.7    -7   1  1   1585  06 52 50
06 54 50  ---          02 19 09  78.2   3.6 -0.1    -175.8   113   F  1   1593  06 52 50

06 54 50  3C66A        02 19 09  77.5   3.5 -0.1    -175.9    -7   1  1   1593  06 54 50
06 56 00  ---          02 20 19  77.5   2.5  0.0    -177.1    63   F  1   1597  06 54 50

06 56 00  SN1986J      02 20 19  78.2   2.5  0.0    -177.0    -7   1  1   1597  06 56 00
06 58 00  ---          02 22 19  78.3   0.7  0.0    -179.2   113   F  1   1605  06 56 00

06 58 00  3C66A        02 22 19  77.6   0.8  0.0    -179.1    -7   1  1   1605  06 58 00
06 59 10  ---          02 23 29  77.6  -0.2  0.0     179.8    63   F  1   1610  06 58 00

06 59 10  SN1986J      02 23 29  78.3  -0.3  0.0     179.6    -7   1  1   1610  06 59 10
07 01 10  ---          02 25 30  78.2  -2.2  0.0     177.5   113   F  1   1617  06 59 10

07 01 10  3C66A        02 25 30  77.5  -1.9  0.0     177.8    -7   1  1   1617  07 01 10
07 02 20  ---          02 26 40  77.5  -2.9  0.1     176.6    63   F  1   1622  07 01 10

07 02 20  SN1986J      02 26 40  78.2  -3.2  0.1     176.3    -7   1  1   1622  07 02 20
07 04 20  ---          02 28 40  78.2  -5.0  0.1     174.1   113   F  1   1630  07 02 20

07 04 20  3C66A        02 28 40  77.5  -4.6  0.1     174.6    -7   1  1   1630  07 04 20
07 05 30  ---          02 29 50  77.5  -5.6  0.1     173.5    63   F  1   1634  07 04 20

07 05 30  SN1986J      02 29 50  78.2  -6.1  0.1     172.9    -7   1  1   1634  07 05 30
07 07 30  ---          02 31 51  78.1  -7.9  0.1     170.8   113   F  1   1642  07 05 30

07 07 30  3C66A        02 31 51  77.4  -7.2  0.1     171.5    -7   1  1   1642  07 07 30
07 08 40  ---          02 33 01  77.4  -8.2  0.2     170.3    63   F  1   1646  07 07 30

07 11 00  3C66A        02 35 21  77.3 -10.1  0.2     168.1   133   1  1   1646  07 11 00
07 12 10  ---          02 36 31  77.3 -11.1  0.2     166.9    70   F  1   1651  07 11 18

07 12 10  SN1986J      02 36 31  78.0 -11.9  0.2     166.0    -7   1  1   1651  07 12 10
07 14 10  ---          02 38 32  77.9 -13.7  0.3     164.0   113   F  1   1659  07 12 10

07 14 10  3C66A        02 38 32  77.2 -12.7  0.3     165.0    -7   1  1   1659  07 14 10
07 15 20  ---          02 39 42  77.1 -13.6  0.3     163.9    63   F  1   1663  07 14 10
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

07 15 20  SN1986J      02 39 42  77.8 -14.6  0.3     162.9    -7   1  1   1663  07 15 20
07 17 20  ---          02 41 42  77.7 -16.3  0.3     160.9   113   F  1   1671  07 15 20

07 17 20  3C66A        02 41 42  77.0 -15.2  0.3     162.1    -7   1  1   1671  07 17 20
07 18 30  ---          02 42 52  77.0 -16.1  0.3     161.0    63   F  1   1675  07 17 20

07 18 30  SN1986J      02 42 52  77.6 -17.2  0.3     159.8    -7   1  1   1675  07 18 30
07 20 30  ---          02 44 53  77.5 -18.8  0.4     157.9   113   F  1   1683  07 18 30

07 20 30  3C66A        02 44 53  76.8 -17.6  0.4     159.2    -7   1  1   1683  07 20 30
07 21 40  ---          02 46 03  76.8 -18.5  0.4     158.1    63   F  1   1688  07 20 30

07 21 40  SN1986J      02 46 03  77.4 -19.8  0.4     156.8    -7   1  1   1688  07 21 40
07 23 40  ---          02 48 03  77.2 -21.3  0.4     155.0   113   F  1   1695  07 21 40

07 23 40  3C66A        02 48 03  76.6 -19.9  0.4     156.3    -7   1  1   1695  07 23 40
07 24 50  ---          02 49 13  76.5 -20.8  0.4     155.3    63   F  1   1700  07 23 40

07 24 50  SN1986J      02 49 13  77.2 -22.2  0.4     153.9    -7   1  1   1700  07 24 50
07 26 50  ---          02 51 14  77.0 -23.7  0.5     152.1   113   F  1   1708  07 24 50

07 26 50  3C66A        02 51 14  76.4 -22.2  0.5     153.6    -7   1  1   1708  07 26 50
07 28 00  ---          02 52 24  76.3 -23.0  0.5     152.6    63   F  1   1712  07 26 50

07 30 20  3C66A        02 54 44  76.1 -24.5  0.5     150.7   133   1  1   1712  07 30 20
07 31 30  ---          02 55 55  76.0 -25.3  0.5     149.8    70   F  1   1717  07 30 38

07 31 30  SN1986J      02 55 55  76.6 -26.9  0.5     148.2    -7   1  1   1717  07 31 30
07 33 30  ---          02 57 55  76.4 -28.3  0.6     146.5   113   F  1   1724  07 31 30

07 33 30  3C66A        02 57 55  75.8 -26.6  0.6     148.2    -7   1  1   1724  07 33 30
07 34 40  ---          02 59 05  75.7 -27.3  0.6     147.3    63   F  1   1729  07 33 30

07 34 40  SN1986J      02 59 05  76.2 -29.0  0.6     145.6    -7   1  1   1729  07 34 40
07 36 40  ---          03 01 05  76.0 -30.3  0.6     144.0   113   F  1   1737  07 34 40

07 36 40  3C66A        03 01 05  75.5 -28.6  0.6     145.7    -7   1  1   1737  07 36 40
07 37 50  ---          03 02 16  75.3 -29.3  0.7     144.9    63   F  1   1741  07 36 40

07 37 50  SN1986J      03 02 16  75.9 -31.0  0.7     143.1    -7   1  1   1741  07 37 50
07 39 50  ---          03 04 16  75.7 -32.2  0.7     141.6   113   F  1   1749  07 37 50
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

07 39 50  3C66A        03 04 16  75.1 -30.4  0.7     143.4    -7   1  1   1749  07 39 50
07 41 00  ---          03 05 26  75.0 -31.1  0.7     142.5    63   F  1   1753  07 39 50

07 41 00  SN1986J      03 05 26  75.5 -32.9  0.7     140.8    -7   1  1   1753  07 41 00
07 43 00  ---          03 07 26  75.3 -34.0  0.7     139.4   113   F  1   1761  07 41 00

07 43 00  3C66A        03 07 26  74.8 -32.2  0.7     141.1    -7   1  1   1761  07 43 00
07 44 10  ---          03 08 37  74.6 -32.8  0.8     140.3    63   F  1   1766  07 43 00

07 44 10  SN1986J      03 08 37  75.1 -34.6  0.8     138.5    -7   1  1   1766  07 44 10
07 46 10  ---          03 10 37  74.9 -35.7  0.8     137.2   113   F  1   1773  07 44 10

07 46 10  3C66A        03 10 37  74.4 -33.9  0.8     139.0    -7   1  1   1773  07 46 10
07 47 20  ---          03 11 47  74.3 -34.4  0.8     138.2    63   F  1   1778  07 46 10

07 49 40  3C66A        03 14 08  74.0 -35.6  0.8     136.7   134   1  1   1778  07 49 40
07 50 50  ---          03 15 18  73.8 -36.2  0.9     136.0    70   F  1   1782  07 49 58

07 50 50  SN1986J      03 15 18  74.3 -38.0  0.9     134.1    -7   1  1   1782  07 50 50
07 52 50  ---          03 17 18  74.0 -39.0  0.9     132.9   113   F  1   1790  07 50 50

07 52 50  3C66A        03 17 18  73.6 -37.1  0.9     134.7    -7   1  1   1790  07 52 50
07 54 00  ---          03 18 28  73.4 -37.6  0.9     134.0    63   F  1   1795  07 52 50

07 54 00  SN1986J      03 18 28  73.9 -39.5  0.9     132.2    -7   1  1   1795  07 54 00
07 56 00  ---          03 20 29  73.6 -40.4  1.0     131.0   113   F  1   1802  07 54 00

07 56 00  3C66A        03 20 29  73.1 -38.5  1.0     132.9    -7   1  1   1802  07 56 00
07 57 10  ---          03 21 39  73.0 -39.0  1.0     132.2    63   F  1   1807  07 56 00

07 57 10  SN1986J      03 21 39  73.4 -40.9  1.0     130.4    -7   1  1   1807  07 57 10
07 59 10  ---          03 23 39  73.1 -41.7  1.0     129.2   113   F  1   1815  07 57 10

07 59 10  3C66A        03 23 39  72.7 -39.8  1.0     131.1    -7   1  1   1815  07 59 10
08 00 20  ---          03 24 49  72.5 -40.3  1.0     130.4    63   F  1   1819  07 59 10

08 00 20  SN1986J      03 24 49  73.0 -42.2  1.0     128.6    -7   1  1   1819  08 00 20
08 02 20  ---          03 26 50  72.7 -42.9  1.1     127.5   113   F  1   1827  08 00 20

08 02 20  3C66A        03 26 50  72.3 -41.0  1.1     129.3    -7   1  1   1827  08 02 20
08 03 30  ---          03 28 00  72.1 -41.5  1.1     128.7    63   F  1   1832  08 02 20
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

08 03 30  SN1986J      03 28 00  72.5 -43.4  1.1     126.9    -7   1  1   1832  08 03 30
08 05 30  ---          03 30 00  72.2 -44.1  1.1     125.9   113   F  1   1839  08 03 30

08 05 30  3C66A        03 30 00  71.8 -42.2  1.1     127.7    -7   1  1   1839  08 05 30
08 06 40  ---          03 31 10  71.6 -42.6  1.1     127.1    63   F  1   1844  08 05 30

08 09 40  3C84         03 34 11  78.7 -13.3  0.2     164.7   154   1  1   1844  08 09 40
08 11 20  ---          03 35 51  78.7 -14.8  0.3     162.9   100   F  1   1850  08 09 58

08 13 40  3C66A        03 38 11  70.6 -44.9  1.2     123.7   114   1  1   1850  08 13 40
08 16 40  ---          03 41 12  70.1 -45.8  1.3     122.4   180   F  1   1862  08 13 58

08 16 40  SN1986J      03 41 12  70.5 -47.6  1.3     120.6    -7   1  1   1862  08 16 40
08 18 40  ---          03 43 12  70.2 -48.2  1.3     119.8   113   F  1   1870  08 16 40

08 18 40  3C66A        03 43 12  69.8 -46.4  1.3     121.5    -7   1  1   1870  08 18 40
08 19 50  ---          03 44 22  69.6 -46.7  1.4     121.0    63   F  1   1874  08 18 40

08 19 50  SN1986J      03 44 22  70.0 -48.5  1.4     119.3    -7   1  1   1874  08 19 50
08 21 50  ---          03 46 23  69.7 -49.0  1.4     118.4   113   F  1   1882  08 19 50

08 21 50  3C66A        03 46 23  69.3 -47.2  1.4     120.1    -7   1  1   1882  08 21 50
08 23 00  ---          03 47 33  69.1 -47.5  1.4     119.7    63   F  1   1886  08 21 50

08 23 00  SN1986J      03 47 33  69.5 -49.3  1.4     118.0    -7   1  1   1886  08 23 00
08 25 00  ---          03 49 33  69.1 -49.8  1.4     117.2   113   F  1   1894  08 23 00

08 25 00  3C66A        03 49 33  68.8 -48.0  1.4     118.9    -7   1  1   1894  08 25 00
08 26 10  ---          03 50 44  68.6 -48.3  1.5     118.4    63   F  1   1899  08 25 00

08 26 10  SN1986J      03 50 44  68.9 -50.1  1.5     116.7    -7   1  1   1899  08 26 10
08 28 10  ---          03 52 44  68.6 -50.5  1.5     116.0   113   F  1   1906  08 26 10

08 28 10  3C66A        03 52 44  68.3 -48.8  1.5     117.6    -7   1  1   1906  08 28 10
08 29 20  ---          03 53 54  68.1 -49.0  1.5     117.2    63   F  1   1911  08 28 10

08 29 20  SN1986J      03 53 54  68.4 -50.8  1.5     115.5    -7   1  1   1911  08 29 20
08 31 20  ---          03 55 54  68.1 -51.2  1.5     114.8   113   F  1   1919  08 29 20

08 31 20  3C66A        03 55 54  67.8 -49.5  1.5     116.4    -7   1  1   1919  08 31 20
08 32 30  ---          03 57 05  67.6 -49.7  1.6     116.0    63   F  1   1923  08 31 20
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

08 34 50  3C66A        03 59 25  67.2 -50.2  1.6     115.1   134   1  1   1923  08 34 50
08 36 00  ---          04 00 35  67.0 -50.4  1.6     114.7    70   F  1   1928  08 35 08

08 36 00  SN1986J      04 00 35  67.3 -52.1  1.6     113.2    -7   1  1   1928  08 36 00
08 38 00  ---          04 02 35  66.9 -52.5  1.7     112.5   113   F  1   1935  08 36 00

08 38 00  3C66A        04 02 35  66.7 -50.8  1.7     114.0    -7   1  1   1935  08 38 00
08 39 10  ---          04 03 46  66.5 -51.0  1.7     113.6    63   F  1   1940  08 38 00

08 39 10  SN1986J      04 03 46  66.7 -52.7  1.7     112.1    -7   1  1   1940  08 39 10
08 41 10  ---          04 05 46  66.4 -53.1  1.7     111.4   113   F  1   1948  08 39 10

08 41 10  3C66A        04 05 46  66.2 -51.4  1.7     113.0    -7   1  1   1948  08 41 10
08 42 20  ---          04 06 56  66.0 -51.6  1.7     112.6    63   F  1   1952  08 41 10

08 42 20  SN1986J      04 06 56  66.2 -53.2  1.7     111.1    -7   1  1   1952  08 42 20
08 44 20  ---          04 08 56  65.9 -53.6  1.8     110.4   113   F  1   1960  08 42 20

08 44 20  3C66A        04 08 56  65.6 -52.0  1.8     111.9    -7   1  1   1960  08 44 20
08 45 30  ---          04 10 07  65.4 -52.1  1.8     111.6    63   F  1   1964  08 44 20

08 45 30  SN1986J      04 10 07  65.7 -53.8  1.8     110.1    -7   1  1   1964  08 45 30
08 47 30  ---          04 12 07  65.3 -54.1  1.8     109.4   113   F  1   1972  08 45 30

08 47 30  3C66A        04 12 07  65.1 -52.5  1.8     110.9    -7   1  1   1972  08 47 30
08 48 40  ---          04 13 17  64.9 -52.6  1.8     110.6    63   F  1   1977  08 47 30

08 48 40  SN1986J      04 13 17  65.1 -54.2  1.8     109.1    -7   1  1   1977  08 48 40
08 50 40  ---          04 15 18  64.7 -54.5  1.9     108.5   113   F  1   1984  08 48 40

08 50 40  3C66A        04 15 18  64.5 -52.9  1.9     109.9    -7   1  1   1984  08 50 40
08 51 50  ---          04 16 28  64.3 -53.1  1.9     109.6    63   F  1   1989  08 50 40

08 54 10  3C66A        04 18 48  63.9 -53.4  1.9     108.9   133   1  1   1989  08 54 10
08 55 20  ---          04 19 58  63.7 -53.6  1.9     108.6    70   F  1   1993  08 54 28

08 55 20  SN1986J      04 19 58  63.9 -55.1  1.9     107.2    -7   1  1   1993  08 55 20
08 57 20  ---          04 21 59  63.6 -55.4  2.0     106.6   113   F  1   2001  08 55 20

08 57 20  3C66A        04 21 59  63.4 -53.8  2.0     108.0    -7   1  1   2001  08 57 20
08 58 30  ---          04 23 09  63.2 -54.0  2.0     107.7    63   F  1   2006  08 57 20
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

08 58 30  SN1986J      04 23 09  63.4 -55.5  2.0     106.3    -7   1  1   2006  08 58 30
09 00 30  ---          04 25 09  63.0 -55.7  2.0     105.7   113   F  1   2013  08 58 30

09 00 30  3C66A        04 25 09  62.8 -54.2  2.0     107.1    -7   1  1   2013  09 00 30
09 01 40  ---          04 26 19  62.6 -54.4  2.1     106.8    63   F  1   2018  09 00 30

09 01 40  SN1986J      04 26 19  62.8 -55.9  2.1     105.4    -7   1  1   2018  09 01 40
09 03 40  ---          04 28 20  62.4 -56.1  2.1     104.9   113   F  1   2026  09 01 40

09 03 40  3C66A        04 28 20  62.3 -54.6  2.1     106.2    -7   1  1   2026  09 03 40
09 04 50  ---          04 29 30  62.1 -54.7  2.1     105.9    63   F  1   2030  09 03 40

09 04 50  SN1986J      04 29 30  62.2 -56.2  2.1     104.6    -7   1  1   2030  09 04 50
09 06 50  ---          04 31 30  61.9 -56.4  2.1     104.1   113   F  1   2038  09 04 50

09 06 50  3C66A        04 31 30  61.7 -54.9  2.1     105.4    -7   1  1   2038  09 06 50
09 08 00  ---          04 32 40  61.5 -55.0  2.2     105.1    63   F  1   2042  09 06 50

09 08 00  SN1986J      04 32 40  61.7 -56.5  2.2     103.8    -7   1  1   2042  09 08 00
09 10 00  ---          04 34 41  61.3 -56.7  2.2     103.3   113   F  1   2050  09 08 00

09 10 00  3C66A        04 34 41  61.2 -55.2  2.2     104.6    -7   1  1   2050  09 10 00
09 11 10  ---          04 35 51  61.0 -55.3  2.2     104.3    63   F  1   2055  09 10 00

09 13 30  3C66A        04 38 11  60.5 -55.6  2.2     103.7   133   1  1   2055  09 13 30
09 14 40  ---          04 39 21  60.3 -55.7  2.3     103.4    70   F  1   2059  09 13 48

09 14 40  SN1986J      04 39 21  60.5 -57.1  2.3     102.2    -7   1  1   2059  09 14 40
09 16 40  ---          04 41 22  60.1 -57.2  2.3     101.7   113   F  1   2067  09 14 40

09 16 40  3C66A        04 41 22  60.0 -55.8  2.3     102.9    -7   1  1   2067  09 16 40
09 17 50  ---          04 42 32  59.8 -55.9  2.3     102.6    63   F  1   2071  09 16 40

09 17 50  SN1986J      04 42 32  59.9 -57.3  2.3     101.4    -7   1  1   2071  09 17 50
09 19 50  ---          04 44 32  59.5 -57.4  2.4     101.0   113   F  1   2079  09 17 50

09 19 50  3C66A        04 44 32  59.4 -56.1  2.4     102.2    -7   1  1   2079  09 19 50
09 21 00  ---          04 45 43  59.2 -56.2  2.4     101.9    63   F  1   2084  09 19 50

09 21 00  SN1986J      04 45 43  59.3 -57.5  2.4     100.7    -7   1  1   2084  09 21 00
09 23 00  ---          04 47 43  58.9 -57.7  2.4     100.3   113   F  1   2091  09 21 00
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

09 23 00  3C66A        04 47 43  58.8 -56.3  2.4     101.4    -7   1  1   2091  09 23 00
09 24 10  ---          04 48 53  58.6 -56.4  2.4     101.2    63   F  1   2096  09 23 00

09 24 10  SN1986J      04 48 53  58.7 -57.7  2.4     100.0    -7   1  1   2096  09 24 10
09 26 10  ---          04 50 53  58.4 -57.8  2.5      99.6   113   F  1   2104  09 24 10

09 26 10  3C66A        04 50 53  58.3 -56.5  2.5     100.7    -7   1  1   2104  09 26 10
09 27 20  ---          04 52 04  58.1 -56.6  2.5     100.4    63   F  1   2108  09 26 10

09 27 20  SN1986J      04 52 04  58.2 -57.9  2.5      99.3    -7   1  1   2108  09 27 20
09 29 20  ---          04 54 04  57.8 -58.0  2.5      98.9   113   F  1   2116  09 27 20

09 29 20  3C66A        04 54 04  57.7 -56.7  2.5     100.0    -7   1  1   2116  09 29 20
09 30 30  ---          04 55 14  57.5 -56.8  2.5      99.7    63   F  1   2121  09 29 20

09 32 50  3C66A        04 57 34  57.1 -56.9  2.6      99.2   133   1  1   2121  09 32 50
09 34 00  ---          04 58 45  56.9 -57.0  2.6      99.0    70   F  1   2125  09 33 08

09 34 00  SN1986J      04 58 45  56.9 -58.3  2.6      97.9    -7   1  1   2125  09 34 00
09 36 00  ---          05 00 45  56.6 -58.4  2.6      97.5   113   F  1   2133  09 34 00

09 36 00  3C66A        05 00 45  56.5 -57.1  2.6      98.6    -7   1  1   2133  09 36 00
09 37 10  ---          05 01 55  56.3 -57.1  2.6      98.3    63   F  1   2137  09 36 00

09 37 10  SN1986J      05 01 55  56.4 -58.4  2.6      97.2    -7   1  1   2137  09 37 10
09 39 10  ---          05 03 55  56.0 -58.5  2.7      96.8   113   F  1   2145  09 37 10

09 39 10  3C66A        05 03 55  55.9 -57.2  2.7      97.9    -7   1  1   2145  09 39 10
09 40 20  ---          05 05 06  55.7 -57.3  2.7      97.6    63   F  1   2150  09 39 10

09 40 20  SN1986J      05 05 06  55.8 -58.5  2.7      96.6    -7   1  1   2150  09 40 20
09 42 20  ---          05 07 06  55.4 -58.6  2.7      96.2   113   F  1   2157  09 40 20

09 42 20  3C66A        05 07 06  55.3 -57.4  2.7      97.2    -7   1  1   2157  09 42 20
09 43 30  ---          05 08 16  55.1 -57.4  2.8      97.0    63   F  1   2162  09 42 20

09 43 30  SN1986J      05 08 16  55.2 -58.6  2.8      96.0    -7   1  1   2162  09 43 30
09 45 30  ---          05 10 17  54.8 -58.7  2.8      95.6   113   F  1   2170  09 43 30

09 45 30  3C66A        05 10 17  54.8 -57.5  2.8      96.6    -7   1  1   2170  09 45 30
09 46 40  ---          05 11 27  54.6 -57.5  2.8      96.4    63   F  1   2174  09 45 30
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

09 46 40  SN1986J      05 11 27  54.6 -58.7  2.8      95.3    -7   1  1   2174  09 46 40
09 48 40  ---          05 13 27  54.2 -58.8  2.8      95.0   113   F  1   2182  09 46 40

09 48 40  3C66A        05 13 27  54.2 -57.6  2.8      96.0    -7   1  1   2182  09 48 40
09 49 50  ---          05 14 37  54.0 -57.6  2.9      95.7    63   F  1   2186  09 48 40

09 52 10  3C66A        05 16 58  53.6 -57.7  2.9      95.3   133   1  1   2186  09 52 10
09 53 20  ---          05 18 08  53.3 -57.7  2.9      95.0    70   F  1   2191  09 52 28

09 53 20  SN1986J      05 18 08  53.4 -58.9  2.9      94.1    -7   1  1   2191  09 53 20
09 55 20  ---          05 20 08  53.0 -59.0  3.0      93.7   113   F  1   2199  09 53 20

09 55 20  3C66A        05 20 08  53.0 -57.8  2.9      94.7    -6   1  1   2199  09 55 20
09 56 30  ---          05 21 18  52.8 -57.8  3.0      94.4    64   F  1   2203  09 55 20

09 56 30  SN1986J      05 21 18  52.8 -59.0  3.0      93.5    -6   1  1   2203  09 56 30
09 58 30  ---          05 23 19  52.4 -59.0  3.0      93.1   114   F  1   2211  09 56 30

09 58 30  3C66A        05 23 19  52.4 -57.9  3.0      94.1    -6   1  1   2211  09 58 30
09 59 40  ---          05 24 29  52.2 -57.9  3.0      93.8    64   F  1   2215  09 58 30

09 59 40  SN1986J      05 24 29  52.2 -59.0  3.0      92.9    -6   1  1   2215  09 59 40
10 01 40  ---          05 26 29  51.8 -59.1  3.1      92.6   114   F  1   2223  09 59 40

10 01 40  3C66A        05 26 29  51.8 -57.9  3.1      93.5    -6   1  1   2223  10 01 40
10 02 50  ---          05 27 39  51.6 -57.9  3.1      93.3    64   F  1   2228  10 01 40

10 02 50  SN1986J      05 27 39  51.6 -59.1  3.1      92.3    -6   1  1   2228  10 02 50
10 04 50  ---          05 29 40  51.3 -59.1  3.1      92.0   114   F  1   2235  10 02 50

10 04 50  3C66A        05 29 40  51.2 -58.0  3.1      92.9    -6   1  1   2235  10 04 50
10 06 00  ---          05 30 50  51.0 -58.0  3.1      92.7    64   F  1   2240  10 04 50

10 06 00  SN1986J      05 30 50  51.0 -59.1  3.1      91.8    -6   1  1   2240  10 06 00
10 08 00  ---          05 32 50  50.7 -59.1  3.2      91.4   114   F  1   2248  10 06 00

10 08 00  3C66A        05 32 50  50.7 -58.0  3.2      92.3    -6   1  1   2248  10 08 00
10 09 10  ---          05 34 00  50.5 -58.0  3.2      92.1    64   F  1   2252  10 08 00

10 11 30  3C66A        05 36 21  50.0 -58.1  3.2      91.7   133   1  1   2252  10 11 30
10 12 40  ---          05 37 31  49.8 -58.1  3.2      91.5    70   F  1   2257  10 11 48
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

10 12 40  SN1986J      05 37 31  49.8 -59.2  3.2      90.6    -6   1  1   2257  10 12 40
10 14 40  ---          05 39 31  49.4 -59.2  3.3      90.3   114   F  1   2264  10 12 40

10 14 40  3C66A        05 39 31  49.4 -58.1  3.3      91.1    -6   1  1   2264  10 14 40
10 15 50  ---          05 40 42  49.2 -58.1  3.3      90.9    64   F  1   2269  10 14 40

10 15 50  SN1986J      05 40 42  49.2 -59.2  3.3      90.1    -6   1  1   2269  10 15 50
10 17 50  ---          05 42 42  48.8 -59.2  3.3      89.8   114   F  1   2277  10 15 50

10 17 50  3C66A        05 42 42  48.9 -58.1  3.3      90.6    -6   1  1   2277  10 17 50
10 19 00  ---          05 43 52  48.7 -58.1  3.3      90.4    64   F  1   2281  10 17 50

10 19 00  SN1986J      05 43 52  48.6 -59.2  3.3      89.6    -6   1  1   2281  10 19 00
10 21 00  ---          05 45 52  48.3 -59.1  3.4      89.2   114   F  1   2289  10 19 00

10 21 00  3C66A        05 45 52  48.3 -58.1  3.4      90.0    -6   1  1   2289  10 21 00
10 22 10  ---          05 47 03  48.1 -58.1  3.4      89.8    64   F  1   2293  10 21 00

10 22 10  SN1986J      05 47 03  48.0 -59.1  3.4      89.0    -6   1  1   2293  10 22 10
10 24 10  ---          05 49 03  47.7 -59.1  3.4      88.7   114   F  1   2301  10 22 10

10 24 10  3C66A        05 49 03  47.7 -58.1  3.4      89.5    -6   1  1   2301  10 24 10
10 25 20  ---          05 50 13  47.5 -58.1  3.4      89.3    64   F  1   2306  10 24 10

10 25 20  SN1986J      05 50 13  47.5 -59.1  3.5      88.5    -6   1  1   2306  10 25 20
10 27 20  ---          05 52 13  47.1 -59.1  3.5      88.2   114   F  1   2313  10 25 20

10 27 20  3C66A        05 52 13  47.1 -58.1  3.5      89.0    -6   1  1   2313  10 27 20
10 28 30  ---          05 53 24  46.9 -58.1  3.5      88.8    64   F  1   2318  10 27 20

10 30 50  3C66A        05 55 44  46.5 -58.1  3.5      88.4   133   1  1   2318  10 30 50
10 32 00  ---          05 56 54  46.3 -58.0  3.6      88.2    70   F  1   2322  10 31 08

10 32 00  SN1986J      05 56 54  46.2 -59.1  3.6      87.4    -6   1  1   2322  10 32 00
10 34 00  ---          05 58 55  45.9 -59.0  3.6      87.1   114   F  1   2330  10 32 00

10 34 00  3C66A        05 58 55  45.9 -58.0  3.6      87.9    -6   1  1   2330  10 34 00
10 35 10  ---          06 00 05  45.7 -58.0  3.6      87.7    64   F  1   2335  10 34 00

10 35 10  SN1986J      06 00 05  45.6 -59.0  3.6      86.9    -6   1  1   2335  10 35 10
10 37 10  ---          06 02 05  45.3 -59.0  3.6      86.6   114   F  1   2342  10 35 10
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

10 37 10  3C66A        06 02 05  45.3 -58.0  3.6      87.3    -6   1  1   2342  10 37 10
10 38 20  ---          06 03 15  45.1 -58.0  3.7      87.1    64   F  1   2347  10 37 10

10 38 20  SN1986J      06 03 15  45.0 -59.0  3.7      86.4    -6   1  1   2347  10 38 20
10 40 20  ---          06 05 16  44.7 -58.9  3.7      86.1   114   F  1   2355  10 38 20

10 40 20  3C66A        06 05 16  44.7 -58.0  3.7      86.8    -6   1  1   2355  10 40 20
10 41 30  ---          06 06 26  44.5 -57.9  3.7      86.6    64   F  1   2359  10 40 20

10 41 30  SN1986J      06 06 26  44.5 -58.9  3.7      85.9    -6   1  1   2359  10 41 30
10 43 30  ---          06 08 26  44.1 -58.9  3.8      85.6   114   F  1   2367  10 41 30

10 43 30  3C66A        06 08 26  44.2 -57.9  3.8      86.3    -6   1  1   2367  10 43 30
10 44 40  ---          06 09 36  44.0 -57.9  3.8      86.1    64   F  1   2371  10 43 30

10 44 40  SN1986J      06 09 36  43.9 -58.9  3.8      85.4    -6   1  1   2371  10 44 40
10 46 40  ---          06 11 37  43.5 -58.8  3.8      85.1   114   F  1   2379  10 44 40

10 46 40  3C66A        06 11 37  43.6 -57.8  3.8      85.8    -6   1  1   2379  10 46 40
10 47 50  ---          06 12 47  43.4 -57.8  3.8      85.6    64   F  1   2384  10 46 40

10 50 10  3C66A        06 15 07  43.0 -57.8  3.9      85.3   133   1  1   2384  10 50 10
10 51 20  ---          06 16 17  42.7 -57.8  3.9      85.1    70   F  1   2388  10 50 28

10 51 20  SN1986J      06 16 17  42.6 -58.7  3.9      84.4    -6   1  1   2388  10 51 20
10 53 20  ---          06 18 18  42.3 -58.7  3.9      84.1   114   F  1   2396  10 51 20

10 53 20  3C66A        06 18 18  42.4 -57.7  3.9      84.8    -6   1  1   2396  10 53 20
10 54 30  ---          06 19 28  42.2 -57.7  3.9      84.6    64   F  1   2400  10 53 20

10 54 30  SN1986J      06 19 28  42.1 -58.6  3.9      83.9    -6   1  1   2400  10 54 30
10 56 30  ---          06 21 28  41.7 -58.6  4.0      83.6   114   F  1   2408  10 54 30

10 56 30  3C66A        06 21 28  41.8 -57.6  4.0      84.3    -6   1  1   2408  10 56 30
10 57 40  ---          06 22 38  41.6 -57.6  4.0      84.1    64   F  1   2413  10 56 30

10 57 40  SN1986J      06 22 38  41.5 -58.5  4.0      83.5    -6   1  1   2413  10 57 40
10 59 40  ---          06 24 39  41.1 -58.5  4.0      83.2   114   F  1   2420  10 57 40

10 59 40  3C66A        06 24 39  41.2 -57.6  4.0      83.8    -6   1  1   2420  10 59 40
11 00 50  ---          06 25 49  41.0 -57.5  4.0      83.6    64   F  1   2425  10 59 40
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

11 00 50  SN1986J      06 25 49  40.9 -58.4  4.0      83.0    -6   1  1   2425  11 00 50
11 02 50  ---          06 27 49  40.5 -58.4  4.1      82.7   114   F  1   2433  11 00 50

11 02 50  3C66A        06 27 49  40.6 -57.5  4.1      83.3    -6   1  1   2433  11 02 50
11 04 00  ---          06 28 59  40.4 -57.4  4.1      83.1    64   F  1   2437  11 02 50

11 04 00  SN1986J      06 28 59  40.3 -58.3  4.1      82.5    -6   1  1   2437  11 04 00
11 06 00  ---          06 31 00  40.0 -58.3  4.1      82.2   114   F  1   2445  11 04 00

11 06 00  3C66A        06 31 00  40.1 -57.4  4.1      82.8    -6   1  1   2445  11 06 00
11 07 10  ---          06 32 10  39.9 -57.3  4.1      82.6    64   F  1   2450  11 06 00

11 09 30  3C66A        06 34 30  39.4 -57.3  4.2      82.3   133   1  1   2450  11 09 30
11 10 40  ---          06 35 41  39.2 -57.2  4.2      82.1    70   F  1   2454  11 09 48

11 10 40  SN1986J      06 35 41  39.1 -58.1  4.2      81.5    -6   1  1   2454  11 10 40
11 12 40  ---          06 37 41  38.7 -58.1  4.2      81.2   114   F  1   2462  11 10 40

11 12 40  3C66A        06 37 41  38.9 -57.2  4.2      81.8    -6   1  1   2462  11 12 40
11 13 50  ---          06 38 51  38.6 -57.1  4.3      81.6    64   F  1   2466  11 12 40

11 13 50  SN1986J      06 38 51  38.5 -58.0  4.3      81.1    -6   1  1   2466  11 13 50
11 15 50  ---          06 40 51  38.2 -57.9  4.3      80.8   114   F  1   2474  11 13 50

11 15 50  3C66A        06 40 51  38.3 -57.1  4.3      81.3    -6   1  1   2474  11 15 50
11 17 00  ---          06 42 02  38.1 -57.0  4.3      81.2    64   F  1   2479  11 15 50

11 17 00  SN1986J      06 42 02  37.9 -57.9  4.3      80.6    -6   1  1   2479  11 17 00
11 19 00  ---          06 44 02  37.6 -57.8  4.3      80.3   114   F  1   2486  11 17 00

11 19 00  3C66A        06 44 02  37.7 -56.9  4.3      80.9    -6   1  1   2486  11 19 00
11 20 10  ---          06 45 12  37.5 -56.9  4.4      80.7    64   F  1   2491  11 19 00

11 20 10  SN1986J      06 45 12  37.4 -57.8  4.4      80.1    -6   1  1   2491  11 20 10
11 22 10  ---          06 47 12  37.0 -57.7  4.4      79.8   114   F  1   2499  11 20 10

11 22 10  3C66A        06 47 12  37.1 -56.8  4.4      80.4    -6   1  1   2499  11 22 10
11 23 20  ---          06 48 23  36.9 -56.8  4.4      80.2    64   F  1   2503  11 22 10

11 23 20  SN1986J      06 48 23  36.8 -57.6  4.4      79.7    -6   1  1   2503  11 23 20
11 25 20  ---          06 50 23  36.4 -57.6  4.5      79.4   114   F  1   2511  11 23 20
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

11 25 20  3C66A        06 50 23  36.6 -56.7  4.5      79.9    -6   1  1   2511  11 25 20
11 26 30  ---          06 51 33  36.4 -56.7  4.5      79.8    64   F  1   2515  11 25 20

11 29 30  3C84         06 54 34  46.1 -60.3  3.6      86.5   154   1  1   2515  11 29 30
11 31 10  ---          06 56 14  45.8 -60.2  3.6      86.3   100   F  1   2522  11 29 48

11 33 30  3C66A        06 58 34  35.1 -56.4  4.6      78.7   113   1  1   2522  11 33 30
11 36 30  ---          07 01 35  34.6 -56.2  4.6      78.3   180   F  1   2533  11 33 48

11 36 30  SN1986J      07 01 35  34.4 -57.1  4.6      77.8    -6   1  1   2533  11 36 30
11 38 30  ---          07 03 35  34.0 -57.0  4.7      77.5   114   F  1   2541  11 36 30

11 38 30  3C66A        07 03 35  34.2 -56.1  4.7      78.0    -6   1  1   2541  11 38 30
11 39 40  ---          07 04 45  34.0 -56.1  4.7      77.8    64   F  1   2546  11 38 30

11 39 40  SN1986J      07 04 45  33.8 -56.9  4.7      77.3    -6   1  1   2546  11 39 40
11 41 40  ---          07 06 46  33.5 -56.8  4.7      77.1   114   F  1   2553  11 39 40

11 41 40  3C66A        07 06 46  33.6 -56.0  4.7      77.5    -6   1  1   2553  11 41 40
11 42 50  ---          07 07 56  33.4 -55.9  4.7      77.4    64   F  1   2558  11 41 40

11 42 50  SN1986J      07 07 56  33.2 -56.7  4.7      76.9    -6   1  1   2558  11 42 50
11 44 50  ---          07 09 56  32.9 -56.6  4.8      76.6   114   F  1   2566  11 42 50

11 44 50  3C66A        07 09 56  33.1 -55.8  4.8      77.1    -6   1  1   2566  11 44 50
11 46 00  ---          07 11 06  32.9 -55.8  4.8      76.9    64   F  1   2570  11 44 50

11 46 00  SN1986J      07 11 06  32.7 -56.6  4.8      76.5    -6   1  1   2570  11 46 00
11 48 00  ---          07 13 07  32.3 -56.5  4.8      76.2   114   F  1   2578  11 46 00

11 48 00  3C66A        07 13 07  32.5 -55.7  4.8      76.6    -6   1  1   2578  11 48 00
11 49 10  ---          07 14 17  32.3 -55.6  4.9      76.5    64   F  1   2582  11 48 00

11 49 10  SN1986J      07 14 17  32.1 -56.4  4.9      76.0    -6   1  1   2582  11 49 10
11 51 10  ---          07 16 17  31.7 -56.3  4.9      75.7   114   F  1   2590  11 49 10

11 51 10  3C66A        07 16 17  31.9 -55.5  4.9      76.2    -6   1  1   2590  11 51 10
11 52 20  ---          07 17 27  31.7 -55.5  4.9      76.0    64   F  1   2595  11 51 10

11 54 40  3C66A        07 19 48  31.3 -55.3  4.9      75.7   133   1  1   2595  11 54 40
11 55 50  ---          07 20 58  31.1 -55.3  5.0      75.5    70   F  1   2599  11 54 58
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

11 55 50  SN1986J      07 20 58  30.9 -56.1  5.0      75.1    -6   1  1   2599  11 55 50
11 57 50  ---          07 22 58  30.6 -55.9  5.0      74.8   114   F  1   2607  11 55 50

11 57 50  3C66A        07 22 58  30.8 -55.2  5.0      75.2    -6   1  1   2607  11 57 50
11 59 00  ---          07 24 08  30.6 -55.1  5.0      75.0    64   F  1   2611  11 57 50

11 59 00  SN1986J      07 24 08  30.3 -55.9  5.0      74.6    -6   1  1   2611  11 59 00
12 01 00  ---          07 26 09  30.0 -55.8  5.1      74.3   114   F  1   2619  11 59 00

12 01 00  3C66A        07 26 09  30.2 -55.0  5.0      74.8    -6   1  1   2619  12 01 00
12 02 10  ---          07 27 19  30.0 -54.9  5.1      74.6    64   F  1   2624  12 01 00

12 02 10  SN1986J      07 27 19  29.8 -55.7  5.1      74.2    -6   1  1   2624  12 02 10
12 04 10  ---          07 29 19  29.4 -55.6  5.1      73.9   114   F  1   2631  12 02 10

12 04 10  3C66A        07 29 19  29.6 -54.8  5.1      74.3    -6   1  1   2631  12 04 10
12 05 20  ---          07 30 30  29.4 -54.7  5.1      74.1    64   F  1   2636  12 04 10

12 05 20  SN1986J      07 30 30  29.2 -55.5  5.1      73.7    -6   1  1   2636  12 05 20
12 07 20  ---          07 32 30  28.9 -55.4  5.2      73.5   114   F  1   2644  12 05 20

12 07 20  3C66A        07 32 30  29.1 -54.6  5.2      73.8    -6   1  1   2644  12 07 20
12 08 30  ---          07 33 40  28.9 -54.6  5.2      73.7    64   F  1   2648  12 07 20

12 08 30  SN1986J      07 33 40  28.7 -55.3  5.2      73.3    -6   1  1   2648  12 08 30
12 10 30  ---          07 35 40  28.3 -55.2  5.2      73.0   114   F  1   2656  12 08 30

12 10 30  3C66A        07 35 40  28.5 -54.4  5.2      73.4    -6   1  1   2656  12 10 30
12 11 40  ---          07 36 51  28.3 -54.4  5.2      73.2    64   F  1   2660  12 10 30

12 14 00  3C66A        07 39 11  27.9 -54.2  5.3      72.9   133   1  1   2660  12 14 00
12 15 10  ---          07 40 21  27.7 -54.2  5.3      72.7    70   F  1   2665  12 14 18

12 15 10  SN1986J      07 40 21  27.5 -54.9  5.3      72.4    -6   1  1   2665  12 15 10
12 17 10  ---          07 42 21  27.1 -54.8  5.3      72.1   114   F  1   2673  12 15 10

12 17 10  3C66A        07 42 21  27.4 -54.0  5.3      72.4    -6   1  1   2673  12 17 10
12 18 20  ---          07 43 32  27.2 -54.0  5.3      72.3    64   F  1   2677  12 17 10

12 18 20  SN1986J      07 43 32  26.9 -54.7  5.3      71.9    -6   1  1   2677  12 18 20
12 20 20  ---          07 45 32  26.6 -54.6  5.4      71.6   114   F  1   2685  12 18 20
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

12 20 20  3C66A        07 45 32  26.8 -53.8  5.4      72.0    -6   1  1   2685  12 20 20
12 21 30  ---          07 46 42  26.6 -53.8  5.4      71.8    64   F  1   2690  12 20 20

12 21 30  SN1986J      07 46 42  26.4 -54.5  5.4      71.5    -6   1  1   2690  12 21 30
12 23 30  ---          07 48 42  26.0 -54.4  5.4      71.2   114   F  1   2697  12 21 30

12 23 30  3C66A        07 48 42  26.3 -53.6  5.4      71.5    -6   1  1   2697  12 23 30
12 24 40  ---          07 49 53  26.1 -53.6  5.4      71.4    64   F  1   2702  12 23 30

12 24 40  SN1986J      07 49 53  25.8 -54.3  5.4      71.0    -6   1  1   2702  12 24 40
12 26 40  ---          07 51 53  25.5 -54.2  5.5      70.8   114   F  1   2710  12 24 40

12 26 40  3C66A        07 51 53  25.7 -53.4  5.5      71.1    -6   1  1   2710  12 26 40
12 27 50  ---          07 53 03  25.5 -53.3  5.5      70.9    64   F  1   2714  12 26 40

12 27 50  SN1986J      07 53 03  25.3 -54.1  5.5      70.6    -6   1  1   2714  12 27 50
12 29 50  ---          07 55 04  24.9 -53.9  5.5      70.3   114   F  1   2722  12 27 50

12 29 50  3C66A        07 55 04  25.2 -53.2  5.5      70.6    -6   1  1   2722  12 29 50
12 31 00  ---          07 56 14  25.0 -53.1  5.5      70.5    64   F  1   2726  12 29 50

12 33 20  3C66A        07 58 34  24.6 -53.0  5.6      70.1   133   1  1   2726  12 33 20
12 34 30  ---          07 59 44  24.4 -52.9  5.6      70.0    70   F  1   2731  12 33 38

12 34 30  SN1986J      07 59 44  24.1 -53.6  5.6      69.7    -6   1  1   2731  12 34 30
12 36 30  ---          08 01 45  23.7 -53.5  5.6      69.4   114   F  1   2739  12 34 30

12 36 30  3C66A        08 01 45  24.0 -52.8  5.6      69.7    -6   1  1   2739  12 36 30
12 37 40  ---          08 02 55  23.8 -52.7  5.7      69.5    64   F  1   2743  12 36 30

12 37 40  SN1986J      08 02 55  23.5 -53.4  5.7      69.2    -6   1  1   2743  12 37 40
12 39 40  ---          08 04 55  23.2 -53.2  5.7      68.9   114   F  1   2751  12 37 40

12 39 40  3C66A        08 04 55  23.5 -52.5  5.7      69.2    -6   1  1   2751  12 39 40
12 40 50  ---          08 06 05  23.3 -52.5  5.7      69.1    64   F  1   2755  12 39 40

12 40 50  SN1986J      08 06 05  23.0 -53.2  5.7      68.8    -6   1  1   2755  12 40 50
12 42 50  ---          08 08 06  22.6 -53.0  5.7      68.5   114   F  1   2763  12 40 50

12 42 50  3C66A        08 08 06  22.9 -52.3  5.7      68.8    -6   1  1   2763  12 42 50
12 44 00  ---          08 09 16  22.7 -52.2  5.8      68.6    64   F  1   2768  12 42 50
Schedule for VLBA_FD   (Code Fd )                                   Page  35
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

12 44 00  SN1986J      08 09 16  22.4 -52.9  5.8      68.3    -6   1  1   2768  12 44 00
12 46 00  ---          08 11 16  22.1 -52.8  5.8      68.0   114   F  1   2775  12 44 00

12 46 00  3C66A        08 11 16  22.4 -52.1  5.8      68.3    -6   1  1   2775  12 46 00
12 47 10  ---          08 12 26  22.2 -52.0  5.8      68.2    64   F  1   2780  12 46 00

12 47 10  SN1986J      08 12 26  21.9 -52.7  5.8      67.9    -6   1  1   2780  12 47 10
12 49 10  ---          08 14 27  21.6 -52.5  5.9      67.6   114   F  1   2788  12 47 10

12 49 10  3C66A        08 14 27  21.9 -51.8  5.9      67.9    -6   1  1   2788  12 49 10
12 50 20  ---          08 15 37  21.7 -51.8  5.9      67.7    64   F  1   2792  12 49 10

12 52 40  3C66A        08 17 57  21.3 -51.6  5.9      67.4   133   1  1   2792  12 52 40
12 53 50  ---          08 19 07  21.1 -51.5  5.9      67.2    70   F  1   2797  12 52 58

12 53 50  SN1986J      08 19 07  20.8 -52.2  5.9      66.9    -6   1  1   2797  12 53 50
12 55 50  ---          08 21 08  20.4 -52.0  6.0      66.7   114   F  1   2804  12 53 50

12 55 50  3C66A        08 21 08  20.7 -51.3  6.0      66.9    -6   1  1   2804  12 55 50
12 57 00  ---          08 22 18  20.5 -51.3  6.0      66.7    64   F  1   2809  12 55 50

12 57 00  SN1986J      08 22 18  20.2 -51.9  6.0      66.5    -6   1  1   2809  12 57 00
12 59 00  ---          08 24 18  19.9 -51.8  6.0      66.2   114   F  1   2817  12 57 00

12 59 00  3C66A        08 24 18  20.2 -51.1  6.0      66.5    -6   1  1   2817  12 59 00
13 00 10  ---          08 25 29  20.0 -51.0  6.0      66.3    64   F  1   2821  12 59 00

13 00 10  SN1986J      08 25 29  19.7 -51.7  6.0      66.0    -6   1  1   2821  13 00 10
13 02 10  ---          08 27 29  19.4 -51.5  6.1      65.8   114   F  1   2829  13 00 10

13 02 10  3C66A        08 27 29  19.7 -50.9  6.1      66.0    -6   1  1   2829  13 02 10
13 03 20  ---          08 28 39  19.5 -50.8  6.1      65.8    64   F  1   2833  13 02 10

13 03 20  SN1986J      08 28 39  19.2 -51.4  6.1      65.6    -6   1  1   2833  13 03 20
13 05 20  ---          08 30 39  18.8 -51.3  6.1      65.3   114   F  1   2841  13 03 20

13 05 20  3C66A        08 30 39  19.1 -50.6  6.1      65.5    -6   1  1   2841  13 05 20
13 06 30  ---          08 31 50  18.9 -50.5  6.1      65.4    64   F  1   2846  13 05 20

13 06 30  SN1986J      08 31 50  18.6 -51.2  6.1      65.1    -6   1  1   2846  13 06 30
13 08 30  ---          08 33 50  18.3 -51.0  6.2      64.8   114   F  1   2853  13 06 30
Schedule for VLBA_FD   (Code Fd )                                   Page  36
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

13 08 30  3C66A        08 33 50  18.6 -50.3  6.2      65.1    -6   1  1   2853  13 08 30
13 09 40  ---          08 35 00  18.4 -50.2  6.2      64.9    64   F  1   2858  13 08 30

13 12 00  3C66A        08 37 20  18.0 -50.1  6.2      64.6   134   1  1   2858  13 12 00
13 13 10  ---          08 38 31  17.8 -50.0  6.3      64.4    70   F  1   2862  13 12 18

13 13 10  SN1986J      08 38 31  17.5 -50.6  6.3      64.2    -6   1  1   2862  13 13 10
13 15 10  ---          08 40 31  17.2 -50.4  6.3      63.9   114   F  1   2870  13 13 10

13 15 10  3C66A        08 40 31  17.5 -49.8  6.3      64.1    -6   1  1   2870  13 15 10
13 16 20  ---          08 41 41  17.3 -49.7  6.3      63.9    64   F  1   2875  13 15 10

13 16 20  SN1986J      08 41 41  17.0 -50.3  6.3      63.7    -6   1  1   2875  13 16 20
13 18 20  ---          08 43 42  16.6 -50.2  6.3      63.4   114   F  1   2882  13 16 20

13 18 20  3C66A        08 43 42  17.0 -49.5  6.3      63.6    -6   1  1   2882  13 18 20
13 19 30  ---          08 44 52  16.8 -49.4  6.4      63.5    64   F  1   2887  13 18 20

13 19 30  SN1986J      08 44 52  16.5 -50.1  6.4      63.3    -6   1  1   2887  13 19 30
13 21 30  ---          08 46 52  16.1 -49.9  6.4      63.0   114   F  1   2895  13 19 30

13 21 30  3C66A        08 46 52  16.5 -49.3  6.4      63.2    -6   1  1   2895  13 21 30
13 22 40  ---          08 48 02  16.3 -49.2  6.4      63.0    64   F  1   2899  13 21 30

13 22 40  SN1986J      08 48 02  15.9 -49.8  6.4      62.8    -6   1  1   2899  13 22 40
13 24 40  ---          08 50 03  15.6 -49.6  6.4      62.5   114   F  1   2907  13 22 40

13 24 40  3C66A        08 50 03  15.9 -49.0  6.4      62.7    -6   1  1   2907  13 24 40
13 25 50  ---          08 51 13  15.8 -48.9  6.5      62.5    64   F  1   2911  13 24 40

13 25 50  SN1986J      08 51 13  15.4 -49.5  6.5      62.4    -6   1  1   2911  13 25 50
13 27 50  ---          08 53 13  15.1 -49.3  6.5      62.1   114   F  1   2919  13 25 50

13 27 50  3C66A        08 53 13  15.4 -48.7  6.5      62.3    -6   1  1   2919  13 27 50
13 29 00  ---          08 54 23  15.2 -48.6  6.5      62.1    64   F  1   2924  13 27 50

13 31 20  3C66A        08 56 44  14.9 -48.4  6.6      61.7   134   1  1   2924  13 31 20
13 32 30  ---          08 57 54  14.7 -48.3  6.6      61.6    70   F  1   2928  13 31 38

13 32 30  SN1986J      08 57 54  14.3 -48.9  6.6      61.4    -6   1  1   2928  13 32 30
13 34 30  ---          08 59 54  14.0 -48.7  6.6      61.1   114   F  1   2936  13 32 30
Schedule for VLBA_FD   (Code Fd )                                   Page  37
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

13 34 30  3C66A        08 59 54  14.4 -48.1  6.6      61.3    -6   1  1   2936  13 34 30
13 35 40  ---          09 01 04  14.2 -48.0  6.6      61.1    64   F  1   2940  13 34 30

13 35 40  SN1986J      09 01 04  13.8 -48.6  6.6      60.9    -6   1  1   2940  13 35 40
13 37 40  ---          09 03 05  13.5 -48.4  6.7      60.6   114   F  1   2948  13 35 40

13 37 40  3C66A        09 03 05  13.9 -47.8  6.7      60.8    -6   1  1   2948  13 37 40
13 38 50  ---          09 04 15  13.7 -47.7  6.7      60.6    64   F  1   2953  13 37 40

13 38 50  SN1986J      09 04 15  13.3 -48.3  6.7      60.5    -6   1  1   2953  13 38 50
13 40 50  ---          09 06 15  13.0 -48.1  6.7      60.2   114   F  1   2960  13 38 50

13 40 50  3C66A        09 06 15  13.3 -47.5  6.7      60.3    -6   1  1   2960  13 40 50
13 42 00  ---          09 07 25  13.2 -47.4  6.7      60.1    64   F  1   2965  13 40 50

13 42 00  SN1986J      09 07 25  12.8 -48.0  6.7      60.0    -6   1  1   2965  13 42 00
13 44 00  ---          09 09 26  12.5 -47.8  6.8      59.7   114   F  1   2973  13 42 00

13 44 00  3C66A        09 09 26  12.8 -47.2  6.8      59.8    -6   1  1   2973  13 44 00
13 45 10  ---          09 10 36  12.7 -47.1  6.8      59.7    64   F  1   2977  13 44 00

13 45 10  SN1986J      09 10 36  12.3 -47.7  6.8      59.5    -6   1  1   2977  13 45 10
13 47 10  ---          09 12 36  12.0 -47.5  6.8      59.2   114   F  1   2985  13 45 10

13 47 10  3C66A        09 12 36  12.3 -46.9  6.8      59.4    -6   1  1   2985  13 47 10
13 48 20  ---          09 13 46  12.2 -46.8  6.8      59.2    64   F  1   2989  13 47 10

13 50 40  3C66A        09 16 07  11.8 -46.6  6.9      58.8   134   1  1   2989  13 50 40
13 51 50  ---          09 17 17  11.6 -46.5  6.9      58.7    70   F  1   2994  13 50 58

13 51 50  SN1986J      09 17 17  11.2 -47.1  6.9      58.5    -6   1  1   2994  13 51 50
13 53 50  ---          09 19 17  10.9 -46.9  6.9      58.2   114   F  1   3002  13 51 50

13 53 50  3C66A        09 19 17  11.3 -46.3  6.9      58.4    -7   1  1   3002  13 53 50
13 55 00  ---          09 20 28  11.1 -46.2  7.0      58.2    63   F  1   3006  13 53 50

13 55 00  SN1986J      09 20 28  10.7 -46.8  7.0      58.0    -7   1  1   3006  13 55 00
13 57 00  ---          09 22 28  10.4 -46.6  7.0      57.7   113   F  1   3014  13 55 00

13 57 00  3C66A        09 22 28  10.8 -46.0  7.0      57.9    -7   1  1   3014  13 57 00
13 58 10  ---          09 23 38  10.6 -45.8  7.0      57.7    63   F  1   3019  13 57 00
Schedule for VLBA_FD   (Code Fd )                                   Page  38
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

13 58 10  SN1986J      09 23 38  10.2 -46.4  7.0      57.6    -7   1  1   3019  13 58 10
14 00 10  ---          09 25 38   9.9 -46.2  7.0      57.3   113   F  1   3026  13 58 10

14 00 10  3C66A        09 25 38  10.3 -45.6  7.0      57.4    -7   1  1   3026  14 00 10
14 01 20  ---          09 26 49  10.1 -45.5  7.1      57.2    63   F  1   3031  14 00 10

14 01 20  SN1986J      09 26 49   9.7 -46.1  7.1      57.1    -7   1  1   3031  14 01 20
14 03 20  ---          09 28 49   9.4 -45.9  7.1      56.8   113   F  1   3039  14 01 20

14 03 20  3C66A        09 28 49   9.8 -45.3  7.1      56.9    -7   1  1   3039  14 03 20
14 04 30  ---          09 29 59   9.6 -45.2  7.1      56.7    63   F  1   3043  14 03 20

14 04 30  SN1986J      09 29 59   9.2 -45.8  7.1      56.6    -7   1  1   3043  14 04 30
14 06 30  ---          09 31 59   8.9 -45.6  7.1      56.3   113   F  1   3051  14 04 30

14 06 30  3C66A        09 31 59   9.3 -45.0  7.1      56.4    -7   1  1   3051  14 06 30
14 07 40  ---          09 33 10   9.2 -44.9  7.2      56.2    63   F  1   3055  14 06 30

14 09 50  3C66A        09 35 20   8.8 -44.7  7.2      55.9   124   1  1   3055  14 09 50
14 11 00  ---          09 36 30   8.7 -44.5  7.2      55.7    70   F  1   3060  14 10 08

14 11 00  SN1986J      09 36 30   8.2 -45.1  7.2      55.6    -7   1  1   3060  14 11 00
14 13 00  ---          09 38 30   7.9 -44.9  7.3      55.3   113   F  1   3068  14 11 00

14 13 00  3C66A        09 38 30   8.4 -44.3  7.3      55.4    -7   1  1   3068  14 13 00
14 14 10  ---          09 39 41   8.2 -44.2  7.3      55.2    63   F  1   3072  14 13 00

14 14 10  SN1986J      09 39 41   7.8 -44.8  7.3      55.1    -7   1  1   3072  14 14 10
14 16 10  ---          09 41 41   7.5 -44.6  7.3      54.8   113   F  1   3080  14 14 10

14 16 10  3C66A        09 41 41   7.9 -44.0  7.3      54.9    -7   1  1   3080  14 16 10
14 17 20  ---          09 42 51   7.7 -43.9  7.3      54.7    63   F  1   3084  14 16 10

14 17 20  SN1986J      09 42 51   7.3 -44.4  7.3      54.6    -7   1  1   3084  14 17 20
14 19 20  ---          09 44 52   7.0 -44.2  7.4      54.3   113   F  1   3092  14 17 20

14 19 20  3C66A        09 44 52   7.4 -43.7  7.4      54.4    -7   1  1   3092  14 19 20
14 20 30  ---          09 46 02   7.2 -43.5  7.4      54.2    63   F  1   3097  14 19 20

14 20 30  SN1986J      09 46 02   6.8 -44.1  7.4      54.1    -7   1  1   3097  14 20 30
14 22 30  ---          09 48 02   6.5 -43.9  7.4      53.8   113   F  1   3104  14 20 30
Schedule for VLBA_FD   (Code Fd )                                   Page  39
               10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  26 Oct 2008   Day 300 ---

14 22 30  3C66A        09 48 02   6.9 -43.3  7.4      53.9    -7   1  1   3104  14 22 30
14 23 40  ---          09 49 12   6.8 -43.2  7.4      53.7    63   F  1   3109  14 22 30

14 23 40  SN1986J      09 49 12   6.3 -43.7  7.4      53.6    -7   1  1   3109  14 23 40
14 25 40  ---          09 51 13   6.0 -43.5  7.5      53.3   113   F  1   3117  14 23 40

14 25 40  3C66A        09 51 13   6.5 -43.0  7.5      53.4    -7   1  1   3117  14 25 40
14 26 50  ---          09 52 23   6.3 -42.8  7.5      53.2    63   F  1   3121  14 25 40

14 26 50  SN1986J      09 52 23   5.9 -43.4  7.5      53.1    -7   1  1   3121  14 26 50
14 28 50  ---          09 54 23   5.6 -43.2  7.5      52.8   113   F  1   3129  14 26 50

14 28 50  3C66A        09 54 23   6.0 -42.6  7.5      52.9    -7   1  1   3129  14 28 50
14 30 00  ---          09 55 33   5.8 -42.5  7.5      52.7    63   F  1   3133  14 28 50


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v6cm-512-16-2.set
   Matches group v6cm_2 in /usr/local/sched/catalogs/freq.dat

   Setup group:    4         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels: 16                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
             4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
                   5         6         5         6         7         8         7         8
   BBC SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:  15  Setup file default.  Used pcal sets:   1
   LO sum=    4958.49   4958.49   4958.49   4958.49   4974.49   4974.49   4974.49   4974.49
              4990.49   4990.49   4990.49   4990.49   5006.49   5006.49   5006.49   5006.49
   BBC fr=     858.49    858.49    858.49    858.49    874.49    874.49    874.49    874.49
               890.49    890.49    890.49    890.49    906.49    906.49    906.49    906.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000
                8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S9    S11   S13   S15
    PCALXB2=   S2    S4    S6    S8    S10   S12   S14   S16
    PCALFR1=   490   510   490   510   490   510   490   510
    PCALFR2=   490   510   490   510   490   510   490   510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27, 66, 74, 82, 90, 67, 75, 83, 91
    barrel=roll_off 
 SOURCE LIST -- 10TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SN1986J           02 19 22.592220   * 02 22 31.320000     02 23 06.932618       0.00
                     42 06 18.95870    * 42 19 57.28200      42 22 33.34650        0.00
                     From catalog imbedded in main SCHED input file.
                        9.033 scan hours,    819.591 baseline hours above horizon.

 * 3C66A             02 19 29.982891   * 02 22 39.611477     02 23 15.401461       0.00
                     42 48 29.80879    * 43 02 07.79928      43 04 43.73859        0.00
                     From catalog imbedded in main SCHED input file.
                        6.442 scan hours,    550.410 baseline hours above horizon.

 * 3C84              03 16 29.567269   * 03 19 48.160100     03 20 25.545676       0.00
                     41 19 51.91887    * 41 30 42.10600      41 32 45.57942        0.00
                     From catalog imbedded in main SCHED input file.
                        0.111 scan hours,      8.965 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1986J            149.9
   3C66A              149.2
   3C84               146.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

