  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
 Exp. Code:  GB072   


Schedule Version:       1.00
Processed by SCHED version:  10.00  Release Sept. 15, 2011

PI:       Norbert Bartel

Address:  York University
          Toronto, ON M3J 1P3
          Canada
 

Phone:    +1-416-736-5424 (work)
EMAIL:    bartel@yorku.ca
Fax:      +1-416-736-5516
Phone during observation: +1-416-483-9068 (home)

Observing mode: VLBA 512-16-2-ul 6cm

Notes:    Fringe finder  : OQ208, OJ287, 3C273
          Pol. Calibrator: OQ208, OJ287
          Amplitude check: OQ208, OJ287
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

 Next scan frequencies:  4942.49  4942.49  4942.49  4942.49  4974.49  4974.49
                         4974.49  4974.49  5006.49  5006.49  5006.49  5006.49
                         5038.49  5038.49  5038.49  5038.49
 Next BBC frequencies:    842.49   842.49   842.49   842.49   874.49   874.49
                          874.49   874.49   906.49   906.49   906.49   906.49
                          938.49   938.49   938.49   938.49
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00

08 35 00  OJ287        03 52 47  22.0  79.0 -5.0     -64.1     0        0   08 34 55
08 38 00  ---          03 55 47  22.6  79.3 -5.0     -64.2   180       12   08 34 55

10 29 10  J1215+17     05 47 15   2.6  71.9 -6.5  H  -58.7  6622       12   10 29 05
10 30 20  ---          05 48 25   2.9  72.1 -6.5  H  -58.8     0       17   10 29 05

10 33 40  J1215+17     05 51 46   3.6  72.5 -6.4  H  -59.0   194       17   10 33 40
10 35 00  ---          05 53 06   3.8  72.7 -6.4  H  -59.1     0       22   10 33 40

10 35 00  SN1979C      05 53 06   1.6  72.6 -6.5  D  -58.6   -11       22   No stop 
10 38 20  ---          05 56 27   2.3  73.1 -6.5  H  -58.8     0       35   10 35 00

10 39 10  J1215+17     05 57 17   4.7  73.2 -6.3     -59.4    38       35   10 39 05
10 40 20  ---          05 58 27   4.9  73.3 -6.3     -59.5    70       40   10 39 05

10 40 20  SN1979C      05 58 27   2.7  73.3 -6.4  H  -58.9   -12       40   No stop 
10 43 40  ---          06 01 48   3.4  73.7 -6.4  H  -59.1     0       53   10 40 20

10 43 40  J1215+17     06 01 48   5.6  73.7 -6.2     -59.7   -12       53   No stop 
10 45 00  ---          06 03 08   5.9  73.9 -6.2     -59.7    68       58   10 43 40

10 45 00  SN1979C      06 03 08   3.7  73.9 -6.3  H  -59.2   -12       58   No stop 
10 48 20  ---          06 06 28   4.4  74.3 -6.3     -59.4     0       71   10 45 00

10 49 10  J1215+17     06 07 19   6.8  74.4 -6.1     -60.0    38       71   10 49 05
10 50 20  ---          06 08 29   7.0  74.5 -6.1     -60.1    70       75   10 49 05

10 50 20  SN1979C      06 08 29   4.8  74.5 -6.3     -59.5   -12       75   No stop 
10 53 40  ---          06 11 49   5.5  75.0 -6.2     -59.7   188       88   10 50 20

10 53 40  J1215+17     06 11 49   7.7  74.9 -6.1     -60.2   -12       88   No stop 
10 55 00  ---          06 13 10   8.0  75.1 -6.0     -60.3    68       94   10 53 40
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

10 55 00  SN1979C      06 13 10   5.8  75.1 -6.2     -59.8   -12       94   No stop 
10 58 20  ---          06 16 30   6.5  75.5 -6.1     -59.9   188      106   10 55 00

10 59 10  J1215+17     06 17 20   8.8  75.6 -6.0     -60.5    38      106   10 59 05
11 00 20  ---          06 18 30   9.1  75.7 -6.0     -60.6    70      111   10 59 05

11 00 20  SN1979C      06 18 30   6.9  75.8 -6.1     -60.1   -12      111   No stop 
11 03 40  ---          06 21 51   7.6  76.2 -6.0     -60.2   188      124   11 00 20

11 03 40  J1215+17     06 21 51   9.8  76.1 -5.9     -60.8   -12      124   No stop 
11 05 00  ---          06 23 11  10.1  76.3 -5.9     -60.9    68      129   11 03 40

11 05 00  SN1979C      06 23 11   7.9  76.3 -6.0     -60.3   -12      129   No stop 
11 08 20  ---          06 26 32   8.6  76.7 -6.0     -60.5   188      142   11 05 00

11 09 10  J1215+17     06 27 22  10.9  76.8 -5.8     -61.1    38      142   11 09 05
11 10 20  ---          06 28 32  11.2  76.9 -5.8     -61.1    70      147   11 09 05

11 10 20  SN1979C      06 28 32   9.0  77.0 -5.9     -60.6   -12      147   No stop 
11 13 40  ---          06 31 53   9.7  77.4 -5.9     -60.7   188      160   11 10 20

11 13 40  J1215+17     06 31 53  11.9  77.3 -5.7     -61.3   -12      160   No stop 
11 15 00  ---          06 33 13  12.2  77.5 -5.7     -61.4    68      165   11 13 40

11 15 00  SN1979C      06 33 13  10.0  77.5 -5.8     -60.8   -12      165   No stop 
11 18 20  ---          06 36 33  10.7  77.9 -5.8     -60.9   188      178   11 15 00

11 19 10  J1215+17     06 37 23  13.0  78.0 -5.6     -61.6    38      178   11 19 05
11 20 20  ---          06 38 34  13.3  78.1 -5.6     -61.6    70      183   11 19 05

11 20 20  SN1979C      06 38 34  11.1  78.2 -5.8     -61.0   -12      183   No stop 
11 23 40  ---          06 41 54  11.8  78.6 -5.7     -61.2   188      196   11 20 20

11 23 40  J1215+17     06 41 54  14.0  78.5 -5.6     -61.8   -12      196   No stop 
11 25 00  ---          06 43 14  14.3  78.6 -5.5     -61.8    68      201   11 23 40

11 25 00  SN1979C      06 43 14  12.1  78.7 -5.7     -61.2   -12      201   No stop 
11 28 20  ---          06 46 35  12.8  79.1 -5.6     -61.4   188      214   11 25 00

11 29 10  J1215+17     06 47 25  15.2  79.1 -5.5     -62.0    38      214   11 29 05
11 30 20  ---          06 48 35  15.4  79.3 -5.5     -62.0    70      219   11 29 05

11 30 20  SN1979C      06 48 35  13.2  79.4 -5.6     -61.5   -12      219   No stop 
11 33 40  ---          06 51 56  13.9  79.7 -5.5     -61.6   188      232   11 30 20
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

11 33 40  J1215+17     06 51 56  16.1  79.7 -5.4     -62.2   -12      232   No stop 
11 35 00  ---          06 53 16  16.4  79.8 -5.4     -62.2    68      237   11 33 40

11 35 00  SN1979C      06 53 16  14.2  79.9 -5.5     -61.7   -12      237   No stop 
11 38 20  ---          06 56 37  14.9  80.3 -5.4     -61.8   188      250   11 35 00

11 39 10  J1215+17     06 57 27  17.3  80.3 -5.3     -62.4    38      250   11 39 05
11 40 20  ---          06 58 37  17.5  80.4 -5.3     -62.4    70      254   11 39 05

11 40 20  SN1979C      06 58 37  15.3  80.5 -5.4     -61.9   -12      254   No stop 
11 43 40  ---          07 01 58  16.0  80.9 -5.4     -62.0   188      267   11 40 20

11 43 40  J1215+17     07 01 58  18.2  80.8 -5.2     -62.6   -12      267   No stop 
11 45 00  ---          07 03 18  18.5  81.0 -5.2     -62.6    68      273   11 43 40

11 45 00  SN1979C      07 03 18  16.3  81.1 -5.3     -62.0   -12      273   No stop 
11 48 20  ---          07 06 38  17.0  81.5 -5.3     -62.1   188      285   11 45 00

11 49 10  J1215+17     07 07 28  19.4  81.5 -5.1     -62.8    38      285   11 49 05
11 50 20  ---          07 08 39  19.7  81.6 -5.1     -62.8    70      290   11 49 05

11 50 20  SN1979C      07 08 39  17.5  81.7 -5.2     -62.2   -12      290   No stop 
11 53 40  ---          07 11 59  18.2  82.1 -5.2     -62.3   188      303   11 50 20

11 53 40  J1215+17     07 11 59  20.4  82.0 -5.1     -62.9   -12      303   No stop 
11 55 00  ---          07 13 19  20.7  82.1 -5.0     -62.9    68      308   11 53 40

11 55 00  SN1979C      07 13 19  18.5  82.3 -5.2     -62.3   -12      308   No stop 
11 58 20  ---          07 16 40  19.2  82.7 -5.1     -62.4   188      321   11 55 00

11 59 10  J1215+17     07 17 30  21.5  82.6 -5.0     -63.1    38      321   11 59 05
12 00 20  ---          07 18 40  21.8  82.8 -4.9     -63.1    70      326   11 59 05

12 00 20  SN1979C      07 18 40  19.6  82.9 -5.1     -62.5   -12      326   No stop 
12 03 40  ---          07 22 01  20.3  83.3 -5.0     -62.6   188      339   12 00 20

12 03 40  J1215+17     07 22 01  22.5  83.2 -4.9     -63.2   -12      339   No stop 
12 05 00  ---          07 23 21  22.8  83.3 -4.9     -63.2    68      344   12 03 40

12 05 00  SN1979C      07 23 21  20.6  83.4 -5.0     -62.6   -12      344   No stop 
12 08 20  ---          07 26 42  21.3  83.8 -4.9     -62.7   188      357   12 05 00

12 09 10  J1215+17     07 27 32  23.7  83.8 -4.8     -63.3    38      357   12 09 05
12 10 20  ---          07 28 42  23.9  83.9 -4.8     -63.4    70      362   12 09 05
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

12 10 20  SN1979C      07 28 42  21.7  84.1 -4.9     -62.8   -12      362   No stop 
12 13 40  ---          07 32 02  22.5  84.5 -4.9     -62.8   188      375   12 10 20

12 13 40  J1215+17     07 32 02  24.6  84.3 -4.7     -63.5   -12      375   No stop 
12 15 00  ---          07 33 23  24.9  84.5 -4.7     -63.5    68      380   12 13 40

12 15 00  SN1979C      07 33 23  22.7  84.6 -4.8     -62.9   -12      380   No stop 
12 18 20  ---          07 36 43  23.5  85.0 -4.8     -62.9   188      393   12 15 00

12 19 10  J1215+17     07 37 33  25.8  85.0 -4.6     -63.6    38      393   12 19 05
12 20 20  ---          07 38 44  26.1  85.1 -4.6     -63.6    70      398   12 19 05

12 20 20  SN1979C      07 38 44  23.9  85.3 -4.7     -63.0   -12      398   No stop 
12 23 40  ---          07 42 04  24.6  85.7 -4.7     -63.0   188      411   12 20 20

12 23 40  J1215+17     07 42 04  26.8  85.5 -4.6     -63.7   -12      411   No stop 
12 25 00  ---          07 43 24  27.1  85.7 -4.5     -63.7    68      416   12 23 40

12 25 00  SN1979C      07 43 24  24.9  85.8 -4.7     -63.1   -12      416   No stop 
12 28 20  ---          07 46 45  25.6  86.2 -4.6     -63.1   188      429   12 25 00

12 29 10  J1215+17     07 47 35  28.0  86.2 -4.5     -63.8    38      429   12 29 05
12 30 20  ---          07 48 45  28.2  86.3 -4.4     -63.8    70      434   12 29 05

12 30 20  SN1979C      07 48 45  26.0  86.5 -4.6     -63.2   -12      434   No stop 
12 33 40  ---          07 52 06  26.8  86.9 -4.5     -63.2   188      446   12 30 20

12 33 40  J1215+17     07 52 06  28.9  86.7 -4.4     -63.8   -12      446   No stop 
12 35 00  ---          07 53 26  29.2  86.9 -4.4     -63.9    68      452   12 33 40

12 35 00  SN1979C      07 53 26  27.0  87.0 -4.5     -63.2   -12      452   No stop 
12 38 20  ---          07 56 47  27.8  87.5 -4.4     -63.3   188      464   12 35 00

12 39 10  J1215+17     07 57 37  30.1  87.4 -4.3     -63.9    38      464   12 39 05
12 40 20  ---          07 58 47  30.4  87.5 -4.3     -63.9    70      469   12 39 05

12 40 20  SN1979C      07 58 47  28.2  87.7 -4.4     -63.3   -12      469   No stop 
12 43 40  ---          08 02 07  28.9  88.1 -4.4     -63.3   188      482   12 40 20

12 43 40  J1215+17     08 02 07  31.1  87.9 -4.2     -64.0   -12      482   No stop 
12 45 00  ---          08 03 28  31.4  88.1 -4.2     -64.0    68      487   12 43 40

12 45 00  SN1979C      08 03 28  29.2  88.3 -4.3     -63.3   -12      487   No stop 
12 48 20  ---          08 06 48  29.9  88.7 -4.3     -63.3   188      500   12 45 00
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

12 49 10  J1215+17     08 07 38  32.3  88.6 -4.1     -64.0    38      500   12 49 05
12 50 20  ---          08 08 48  32.5  88.8 -4.1     -64.0    70      505   12 49 05

12 50 20  SN1979C      08 08 48  30.3  88.9 -4.2     -63.4   -12      505   No stop 
12 53 40  ---          08 12 09  31.1  89.4 -4.2     -63.4   188      518   12 50 20

12 53 40  J1215+17     08 12 09  33.3  89.2 -4.1     -64.0   -12      518   No stop 
12 55 00  ---          08 13 29  33.5  89.3 -4.0     -64.0    68      523   12 53 40

12 55 00  SN1979C      08 13 29  31.4  89.5 -4.2     -63.4   -12      523   No stop 
12 58 20  ---          08 16 50  32.1  90.0 -4.1     -63.4   188      536   12 55 00

12 59 10  J1215+17     08 17 40  34.4  89.9 -4.0     -64.0    38      536   12 59 05
13 00 20  ---          08 18 50  34.7  90.0 -3.9     -64.0    70      541   12 59 05

13 00 20  SN1979C      08 18 50  32.5  90.2 -4.1     -63.4   -12      541   No stop 
13 03 40  ---          08 22 11  33.2  90.6 -4.0     -63.4   188      554   13 00 20

13 03 40  J1215+17     08 22 11  35.4  90.5 -3.9     -64.0   -12      554   No stop 
13 05 00  ---          08 23 31  35.7  90.6 -3.9     -64.0    68      559   13 03 40

13 05 00  SN1979C      08 23 31  33.5  90.8 -4.0     -63.4   -12      559   No stop 
13 08 20  ---          08 26 51  34.2  91.2 -3.9     -63.3   188      572   13 05 00

13 09 10  J1215+17     08 27 42  36.6  91.2 -3.8     -64.0    38      572   13 09 05
13 10 20  ---          08 28 52  36.9  91.3 -3.8     -64.0    70      577   13 09 05

13 10 20  SN1979C      08 28 52  34.7  91.5 -3.9     -63.3   -12      577   No stop 
13 13 40  ---          08 32 12  35.4  92.0 -3.9     -63.3   188      590   13 10 20

13 13 40  J1215+17     08 32 12  37.6  91.8 -3.7     -64.0   -12      590   No stop 
13 15 00  ---          08 33 33  37.9  91.9 -3.7     -64.0    68      595   13 13 40

13 15 00  SN1979C      08 33 33  35.7  92.1 -3.8     -63.3   -12      595   No stop 
13 17 50  ---          08 36 23  36.3  92.5 -3.8     -63.3   158      606   13 15 00

13 18 40  J1215+17     08 37 13  38.7  92.4 -3.6     -63.9    38      606   13 18 35
13 20 30  ---          08 39 03  39.0  92.7 -3.6     -63.9   110      613   13 18 35

13 20 30  SN1979C      08 39 03  36.9  92.9 -3.7     -63.2   -12      613   No stop 
13 23 10  ---          08 41 44  37.4  93.2 -3.7     -63.2   148      624   13 20 30

13 23 10  J1215+17     08 41 44  39.6  93.0 -3.6     -63.9   -12      624   No stop 
13 25 00  ---          08 43 34  40.0  93.3 -3.5     -63.8    98      631   13 23 10
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

13 25 00  SN1979C      08 43 34  37.8  93.5 -3.7     -63.2   -12      631   No stop 
13 27 50  ---          08 46 25  38.4  93.9 -3.6     -63.1   158      642   13 25 00

13 28 40  J1215+17     08 47 15  40.8  93.8 -3.5     -63.8    38      642   13 28 35
13 30 30  ---          08 49 05  41.2  94.1 -3.4     -63.7   110      649   13 28 35

13 30 30  SN1979C      08 49 05  39.0  94.3 -3.6     -63.1   -12      649   No stop 
13 33 10  ---          08 51 46  39.6  94.6 -3.5     -63.0   148      659   13 30 30

13 33 10  J1215+17     08 51 46  41.8  94.4 -3.4     -63.7   -12      659   No stop 
13 35 00  ---          08 53 36  42.2  94.7 -3.4     -63.6    98      666   13 33 10

13 35 00  SN1979C      08 53 36  40.0  94.9 -3.5     -63.0   -12      666   No stop 
13 37 50  ---          08 56 26  40.6  95.3 -3.5     -62.9   158      677   13 35 00

13 38 40  J1215+17     08 57 16  43.0  95.2 -3.3     -63.5    38      677   13 38 35
13 40 30  ---          08 59 07  43.3  95.5 -3.3     -63.5   110      685   13 38 35

13 40 30  SN1979C      08 59 07  41.2  95.7 -3.4     -62.8   -12      685   No stop 
13 43 10  ---          09 01 47  41.7  96.1 -3.4     -62.7   148      695   13 40 30

13 43 10  J1215+17     09 01 47  43.9  95.9 -3.2     -63.4   -12      695   No stop 
13 45 00  ---          09 03 37  44.3  96.2 -3.2     -63.4    98      702   13 43 10

13 45 00  SN1979C      09 03 37  42.1  96.4 -3.3     -62.7   -12      702   No stop 
13 47 50  ---          09 06 28  42.7  96.8 -3.3     -62.6   158      713   13 45 00

13 48 40  J1215+17     09 07 18  45.1  96.7 -3.1     -63.2    38      713   13 48 35
13 50 30  ---          09 09 08  45.5  97.0 -3.1     -63.2   110      721   13 48 35

13 50 30  SN1979C      09 09 08  43.3  97.2 -3.2     -62.5   -12      721   No stop 
13 53 10  ---          09 11 49  43.9  97.6 -3.2     -62.4   148      731   13 50 30

13 53 10  J1215+17     09 11 49  46.1  97.4 -3.1     -63.1   -12      731   No stop 
13 55 00  ---          09 13 39  46.5  97.7 -3.0     -63.0    98      738   13 53 10

13 55 00  SN1979C      09 13 39  44.3  97.9 -3.2     -62.3   -12      738   No stop 
13 57 50  ---          09 16 30  44.9  98.3 -3.1     -62.2   158      749   13 55 00

13 58 40  J1215+17     09 17 20  47.2  98.3 -3.0     -62.8    38      749   13 58 35
14 00 30  ---          09 19 10  47.6  98.6 -2.9     -62.7   110      756   13 58 35

14 00 30  SN1979C      09 19 10  45.4  98.8 -3.1     -62.1   -12      756   No stop 
14 03 10  ---          09 21 50  46.0  99.2 -3.0     -61.9   148      767   14 00 30
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

14 03 10  J1215+17     09 21 50  48.2  99.0 -2.9     -62.6   -12      767   No stop 
14 05 00  ---          09 23 41  48.6  99.3 -2.9     -62.5    98      774   14 03 10

14 10 10  3C273        09 28 52  38.6 114.9 -3.0     -51.4   280      774   14 10 05
14 11 30  ---          09 30 12  38.8 115.1 -3.0     -51.2    80      779   14 10 05

14 11 30  J1215+17     09 30 12  50.0 100.5 -2.8     -62.1   -30      779   No stop 
14 18 30  ---          09 37 13  51.5 101.7 -2.6     -61.7   390      806   14 11 30

14 18 30  SN1979C      09 37 13  49.3 101.8 -2.8     -61.0   -12      806   No stop 
14 21 40  ---          09 40 23  49.9 102.4 -2.7     -60.8   178      819   14 18 30

14 21 40  J1215+17     09 40 23  52.1 102.3 -2.6     -61.5   -12      819   No stop 
14 25 00  ---          09 43 44  52.8 102.9 -2.5     -61.2   188      832   14 21 40

14 25 00  SN1979C      09 43 44  50.6 103.0 -2.7     -60.6   -12      832   No stop 
14 28 00  ---          09 46 45  51.3 103.6 -2.6     -60.3   168      843   14 25 00

14 28 50  J1215+17     09 47 35  53.6 103.7 -2.5     -60.9    38      843   14 28 45
14 31 30  ---          09 50 15  54.2 104.2 -2.4     -60.6   160      854   14 28 45

14 31 30  SN1979C      09 50 15  52.0 104.2 -2.6     -60.0   -12      854   No stop 
14 34 30  ---          09 53 16  52.6 104.8 -2.5     -59.8   168      865   14 31 30

14 34 30  J1215+17     09 53 16  54.8 104.8 -2.4     -60.4   -12      865   No stop 
14 37 30  ---          09 56 16  55.4 105.4 -2.3     -60.1   168      877   14 34 30

14 37 30  SN1979C      09 56 16  53.2 105.4 -2.5     -59.5   -12      877   No stop 
14 40 30  ---          09 59 17  53.9 106.1 -2.4     -59.2   168      889   14 37 30

14 41 20  J1215+17     10 00 07  56.2 106.2 -2.3     -59.7    38      889   14 41 15
14 42 50  ---          10 01 37  56.5 106.6 -2.2     -59.5    90      895   14 41 15

14 42 50  SN1979C      10 01 37  54.3 106.6 -2.4     -59.0   -12      895   No stop 
14 45 40  ---          10 04 27  54.9 107.2 -2.3     -58.7   158      906   14 42 50

14 45 40  J1215+17     10 04 27  57.1 107.2 -2.2     -59.2   -12      906   No stop 
14 47 30  ---          10 06 18  57.5 107.6 -2.2     -59.0    98      913   14 45 40

14 47 30  SN1979C      10 06 18  55.3 107.6 -2.3     -58.5   -12      913   No stop 
14 50 30  ---          10 09 18  55.9 108.2 -2.2     -58.1   168      924   14 47 30

14 51 20  J1215+17     10 10 08  58.3 108.5 -2.1     -58.5    38      924   14 51 15
14 52 50  ---          10 11 39  58.6 108.9 -2.1     -58.3    90      931   14 51 15
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

14 52 50  SN1979C      10 11 39  56.4 108.8 -2.2     -57.8   -12      931   No stop 
14 55 40  ---          10 14 29  57.0 109.4 -2.2     -57.5   158      942   14 52 50

14 55 40  J1215+17     10 14 29  59.2 109.6 -2.0     -57.9   -12      942   No stop 
14 57 30  ---          10 16 19  59.5 110.0 -2.0     -57.6    98      949   14 55 40

14 57 30  SN1979C      10 16 19  57.3 109.9 -2.1     -57.2   -12      949   No stop 
15 00 30  ---          10 19 20  58.0 110.6 -2.1     -56.8   168      960   14 57 30

15 01 20  J1215+17     10 20 10  60.3 111.0 -1.9     -57.0    38      960   15 01 15
15 02 50  ---          10 21 40  60.6 111.4 -1.9     -56.8    90      966   15 01 15

15 02 50  SN1979C      10 21 40  58.4 111.2 -2.0     -56.4   -12      966   No stop 
15 05 40  ---          10 24 31  59.0 111.9 -2.0     -56.0   158      977   15 02 50

15 05 40  J1215+17     10 24 31  61.2 112.2 -1.9     -56.3   -12      977   No stop 
15 07 30  ---          10 26 21  61.6 112.7 -1.8     -56.0    98      984   15 05 40

15 07 30  SN1979C      10 26 21  59.4 112.4 -2.0     -55.7   -12      984   No stop 
15 10 30  ---          10 29 21  60.0 113.2 -1.9     -55.2   168      996   15 07 30

15 11 20  J1215+17     10 30 12  62.3 113.8 -1.8     -55.3    38      996   15 11 15
15 12 50  ---          10 31 42  62.6 114.3 -1.7     -55.0    90     1002   15 11 15

15 12 50  SN1979C      10 31 42  60.4 113.9 -1.9     -54.8   -12     1002   No stop 
15 15 40  ---          10 34 32  61.0 114.7 -1.8     -54.3   158     1013   15 12 50

15 15 40  J1215+17     10 34 32  63.2 115.1 -1.7     -54.5   -12     1013   No stop 
15 17 30  ---          10 36 23  63.5 115.7 -1.7     -54.1    98     1020   15 15 40

15 17 30  SN1979C      10 36 23  61.3 115.2 -1.8     -54.0   -12     1020   No stop 
15 20 30  ---          10 39 23  61.9 116.1 -1.7     -53.4   168     1032   15 17 30

15 21 20  J1215+17     10 40 13  64.3 116.9 -1.6     -53.3    38     1032   15 21 15
15 22 50  ---          10 41 44  64.6 117.4 -1.6     -52.9    90     1038   15 21 15

15 22 50  SN1979C      10 41 44  62.4 116.9 -1.7     -52.9   -12     1038   No stop 
15 25 40  ---          10 44 34  62.9 117.8 -1.7     -52.3   158     1049   15 22 50

15 25 40  J1215+17     10 44 34  65.1 118.4 -1.5     -52.3   -12     1049   No stop 
15 27 30  ---          10 46 24  65.4 119.1 -1.5     -51.8    98     1056   15 25 40

15 27 30  SN1979C      10 46 24  63.3 118.4 -1.6     -51.9   -12     1056   No stop 
15 30 30  ---          10 49 25  63.8 119.4 -1.6     -51.2   168     1068   15 27 30
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

15 31 20  J1215+17     10 50 15  66.2 120.5 -1.4     -50.8    38     1068   15 31 15
15 32 50  ---          10 51 45  66.4 121.0 -1.4     -50.4    90     1074   15 31 15

15 32 50  SN1979C      10 51 45  64.3 120.2 -1.5     -50.6   -12     1074   No stop 
15 35 40  ---          10 54 36  64.8 121.2 -1.5     -49.9   158     1085   15 32 50

15 35 40  J1215+17     10 54 36  67.0 122.1 -1.4     -49.6   -12     1085   No stop 
15 37 30  ---          10 56 26  67.3 122.9 -1.3     -49.0    98     1092   15 35 40

15 37 30  SN1979C      10 56 26  65.1 121.9 -1.5     -49.4   -12     1092   No stop 
15 40 30  ---          10 59 26  65.7 123.0 -1.4     -48.6   168     1103   15 37 30

15 41 20  J1215+17     11 00 17  68.0 124.5 -1.3     -47.8    38     1103   15 41 15
15 42 50  ---          11 01 47  68.2 125.1 -1.2     -47.3    90     1110   15 41 15

15 42 50  SN1979C      11 01 47  66.1 123.9 -1.4     -47.9   -12     1110   No stop 
15 45 40  ---          11 04 37  66.6 125.1 -1.3     -47.0   158     1121   15 42 50

15 45 40  J1215+17     11 04 37  68.7 126.4 -1.2     -46.4   -12     1121   No stop 
15 47 30  ---          11 06 28  69.1 127.2 -1.2     -45.7    98     1128   15 45 40

15 47 30  SN1979C      11 06 28  66.9 125.9 -1.3     -46.4   -12     1128   No stop 
15 50 30  ---          11 09 28  67.4 127.2 -1.2     -45.4   168     1139   15 47 30

15 51 20  J1215+17     11 10 18  69.7 129.1 -1.1     -44.3    38     1139   15 51 15
15 52 50  ---          11 11 48  70.0 129.8 -1.1     -43.7    90     1145   15 51 15

15 52 50  SN1979C      11 11 48  67.8 128.2 -1.2     -44.6   -12     1145   No stop 
15 55 40  ---          11 14 39  68.3 129.5 -1.1     -43.6   158     1156   15 52 50

15 55 40  J1215+17     11 14 39  70.4 131.3 -1.0     -42.5   -12     1156   No stop 
15 57 30  ---          11 16 29  70.7 132.3 -1.0     -41.7    98     1163   15 55 40

15 57 30  SN1979C      11 16 29  68.6 130.4 -1.1     -42.9   -12     1163   No stop 
16 00 50  ---          11 19 50  69.2 132.0 -1.1     -41.6   188     1176   15 57 30

16 01 40  J1215+17     11 20 40  71.4 134.6 -0.9     -39.8    38     1176   16 01 35
16 02 50  ---          11 21 50  71.5 135.3 -0.9     -39.2    70     1181   16 01 35

16 02 50  SN1979C      11 21 50  69.5 133.1 -1.0     -40.8   -12     1181   No stop 
16 06 10  ---          11 25 11  70.0 134.9 -1.0     -39.3   188     1194   16 02 50

16 06 10  J1215+17     11 25 11  72.0 137.3 -0.8     -37.6   -12     1194   No stop 
16 07 30  ---          11 26 31  72.2 138.1 -0.8     -36.9    68     1199   16 06 10
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

16 07 30  SN1979C      11 26 31  70.2 135.6 -1.0     -38.7   -12     1199   No stop 
16 10 50  ---          11 29 51  70.7 137.5 -0.9     -37.2   188     1212   16 07 30

16 11 40  J1215+17     11 30 42  72.8 140.8 -0.7     -34.6    38     1212   16 11 35
16 12 50  ---          11 31 52  73.0 141.6 -0.7     -33.9    70     1217   16 11 35

16 12 50  SN1979C      11 31 52  71.0 138.7 -0.9     -36.2   -12     1217   No stop 
16 16 10  ---          11 35 12  71.4 140.7 -0.8     -34.5   188     1230   16 12 50

16 16 10  J1215+17     11 35 12  73.4 143.9 -0.7     -32.0   -12     1230   No stop 
16 17 30  ---          11 36 33  73.6 144.9 -0.7     -31.1    68     1235   16 16 10

16 17 30  SN1979C      11 36 33  71.6 141.5 -0.8     -33.8   -12     1235   No stop 
16 20 50  ---          11 39 53  72.1 143.7 -0.7     -31.9   188     1248   16 17 30

16 21 40  J1215+17     11 40 43  74.1 148.0 -0.6     -28.4    38     1248   16 21 35
16 22 50  ---          11 41 53  74.2 148.9 -0.6     -27.7    70     1253   16 21 35

16 22 50  SN1979C      11 41 53  72.3 145.1 -0.7     -30.8   -12     1253   No stop 
16 26 10  ---          11 45 14  72.7 147.4 -0.6     -28.8   188     1266   16 22 50

16 26 10  J1215+17     11 45 14  74.6 151.6 -0.5     -25.3   -12     1266   No stop 
16 27 30  ---          11 46 34  74.7 152.7 -0.5     -24.4    68     1271   16 26 10

16 27 30  SN1979C      11 46 34  72.9 148.3 -0.6     -28.0   -12     1271   No stop 
16 30 30  ---          11 49 35  73.2 150.5 -0.6     -26.1   168     1282   16 27 30

16 31 00  J1215+17     11 50 05  75.0 155.6 -0.4     -21.8    18     1282   16 30 55
16 32 20  ---          11 51 25  75.1 156.8 -0.4     -20.8    80     1288   16 30 55

16 32 20  SN1979C      11 51 25  73.4 151.9 -0.5     -24.9   -11     1288   No stop 
16 35 20  ---          11 54 25  73.7 154.3 -0.5     -22.8   169     1300   16 32 20

16 35 20  J1215+17     11 54 25  75.4 159.5 -0.4     -18.4   -12     1300   No stop 
16 36 40  ---          11 55 46  75.5 160.7 -0.3     -17.3    68     1305   16 35 20

16 36 40  SN1979C      11 55 46  73.8 155.3 -0.5     -21.9   -12     1305   No stop 
16 39 40  ---          11 58 46  74.1 157.8 -0.4     -19.8   168     1316   16 36 40

16 39 40  J1215+17     11 58 46  75.7 163.4 -0.3     -14.8   -12     1316   No stop 
16 41 00  ---          12 00 06  75.8 164.7 -0.3     -13.7    68     1322   16 39 40

16 41 00  SN1979C      12 00 06  74.2 158.9 -0.4     -18.8   -12     1322   No stop 
16 44 00  ---          12 03 07  74.4 161.4 -0.3     -16.5   168     1333   16 41 00
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

16 44 30  J1215+17     12 03 37  75.9 168.1 -0.2     -10.7    18     1333   16 44 25
16 45 50  ---          12 04 57  76.0 169.4 -0.2      -9.6    80     1339   16 44 25

16 45 50  SN1979C      12 04 57  74.5 163.0 -0.3     -15.1   -12     1339   No stop 
16 48 50  ---          12 07 58  74.7 165.6 -0.3     -12.8   168     1350   16 45 50

16 48 50  J1215+17     12 07 58  76.1 172.3 -0.1      -6.9   -13     1350   No stop 
16 50 10  ---          12 09 18  76.1 173.6 -0.1      -5.7    67     1355   16 48 50

16 50 10  SN1979C      12 09 18  74.7 166.8 -0.2     -11.7   -13     1355   No stop 
16 53 10  ---          12 12 18  74.9 169.6 -0.2      -9.3   167     1367   16 50 10

16 53 10  J1215+17     12 12 18  76.2 176.6 -0.1      -3.0   -13     1367   No stop 
16 54 30  ---          12 13 39  76.2 178.0  0.0      -1.8    67     1372   16 53 10

16 55 40  OQ208        12 14 49  65.4  88.1 -1.9     -77.8    -2     1372   16 55 35
16 58 40  ---          12 17 49  66.1  88.4 -1.8     -77.9   178     1384   16 55 35

16 58 40  J1215+17     12 17 49  76.2 182.2  0.0       1.9   -75     1384   No stop 
17 02 00  ---          12 21 10  76.2 185.5  0.1       5.0   125     1397   16 58 40

17 02 00  SN1979C      12 21 10  75.1 177.7  0.0      -2.0   -13     1397   No stop 
17 05 00  ---          12 24 10  75.1 180.6  0.0       0.5   167     1409   17 02 00

17 05 30  J1215+17     12 24 40  76.1 189.0  0.2       8.1    16     1409   17 05 25
17 06 50  ---          12 26 01  76.0 190.3  0.2       9.2    80     1414   17 05 25

17 06 50  SN1979C      12 26 01  75.1 182.3  0.0       2.0   -13     1414   No stop 
17 09 50  ---          12 29 01  75.0 185.1  0.1       4.5   167     1426   17 06 50

17 09 50  J1215+17     12 29 01  75.9 193.2  0.2      11.9   -14     1426   No stop 
17 11 10  ---          12 30 21  75.8 194.5  0.2      13.0    66     1431   17 09 50

17 11 10  SN1979C      12 30 21  75.0 186.3  0.1       5.7   -14     1431   No stop 
17 14 10  ---          12 33 22  74.9 189.1  0.2       8.1   166     1442   17 11 10

17 14 10  J1215+17     12 33 22  75.6 197.3  0.3      15.5   -14     1442   No stop 
17 15 30  ---          12 34 42  75.5 198.5  0.3      16.6    66     1448   17 14 10

17 15 30  SN1979C      12 34 42  74.9 190.3  0.2       9.2   -14     1448   No stop 
17 18 30  ---          12 37 43  74.7 193.0  0.2      11.6   166     1459   17 15 30

17 19 00  J1215+17     12 38 13  75.3 201.7  0.4      19.4    16     1459   17 18 55
17 20 20  ---          12 39 33  75.2 202.9  0.4      20.5    80     1465   17 18 55
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

17 20 20  SN1979C      12 39 33  74.7 194.7  0.3      13.1   -14     1465   No stop 
17 23 20  ---          12 42 33  74.5 197.3  0.3      15.4   166     1476   17 20 20

17 23 20  J1215+17     12 42 33  74.9 205.5  0.4      22.8   -14     1476   No stop 
17 24 40  ---          12 43 54  74.8 206.6  0.5      23.7    66     1482   17 23 20

17 24 40  SN1979C      12 43 54  74.4 198.5  0.3      16.4   -14     1482   No stop 
17 27 40  ---          12 46 54  74.2 201.0  0.4      18.7   166     1493   17 24 40

17 27 40  J1215+17     12 46 54  74.5 209.1  0.5      25.9   -14     1493   No stop 
17 29 00  ---          12 48 14  74.3 210.1  0.5      26.8    66     1498   17 27 40

17 29 00  SN1979C      12 48 14  74.1 202.1  0.4      19.7   -14     1498   No stop 
17 32 00  ---          12 51 15  73.8 204.6  0.5      21.8   166     1510   17 29 00

17 32 30  J1215+17     12 51 45  73.9 212.9  0.6      29.2    16     1510   17 32 25
17 33 50  ---          12 53 05  73.8 213.9  0.6      30.1    80     1515   17 32 25

17 33 50  SN1979C      12 53 05  73.6 206.0  0.5      23.1   -13     1515   No stop 
17 36 50  ---          12 56 06  73.3 208.4  0.5      25.1   167     1527   17 33 50

17 36 50  J1215+17     12 56 06  73.4 216.0  0.7      31.9   -13     1527   No stop 
17 38 10  ---          12 57 26  73.2 217.0  0.7      32.7    67     1532   17 36 50

17 38 10  SN1979C      12 57 26  73.2 209.4  0.6      26.0   -13     1532   No stop 
17 41 10  ---          13 00 26  72.9 211.6  0.6      27.9   167     1544   17 38 10

17 41 10  J1215+17     13 00 26  72.8 219.0  0.7      34.5   -13     1544   No stop 
17 42 30  ---          13 01 46  72.7 219.9  0.8      35.2    67     1549   17 41 10

17 42 30  SN1979C      13 01 46  72.7 212.5  0.6      28.7   -13     1549   No stop 
17 45 30  ---          13 04 47  72.4 214.6  0.7      30.5   167     1561   17 42 30

17 46 00  J1215+17     13 05 17  72.2 222.2  0.8      37.1    17     1561   17 45 55
17 47 20  ---          13 06 37  72.0 223.0  0.8      37.8    80     1566   17 45 55

17 47 20  SN1979C      13 06 37  72.1 215.9  0.7      31.6   -13     1566   No stop 
17 50 20  ---          13 09 38  71.7 217.8  0.8      33.3   167     1578   17 47 20

17 50 20  J1215+17     13 09 38  71.5 224.8  0.9      39.3   -13     1578   No stop 
17 51 40  ---          13 10 58  71.3 225.6  0.9      39.9    67     1583   17 50 20

17 51 40  SN1979C      13 10 58  71.6 218.7  0.8      34.0   -13     1583   No stop 
17 54 40  ---          13 13 58  71.2 220.6  0.8      35.5   167     1594   17 51 40
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

17 54 40  J1215+17     13 13 58  70.8 227.3  1.0      41.3   -13     1594   No stop 
17 56 00  ---          13 15 19  70.6 228.0  1.0      41.9    67     1600   17 54 40

17 56 00  SN1979C      13 15 19  71.0 221.4  0.9      36.2   -13     1600   No stop 
17 59 00  ---          13 18 19  70.5 223.1  0.9      37.7   167     1611   17 56 00

17 59 30  J1215+17     13 18 49  70.1 229.8  1.1      43.4    18     1611   17 59 25
18 00 50  ---          13 20 09  69.8 230.5  1.1      43.9    80     1617   17 59 25

18 00 50  SN1979C      13 20 09  70.3 224.2  0.9      38.5   -12     1617   No stop 
18 03 50  ---          13 23 10  69.8 225.8  1.0      39.9   168     1628   18 00 50

18 03 50  J1215+17     13 23 10  69.3 232.0  1.1      45.1   -12     1628   No stop 
18 05 10  ---          13 24 30  69.1 232.6  1.1      45.6    68     1633   18 03 50

18 05 10  SN1979C      13 24 30  69.6 226.5  1.0      40.4   -12     1633   No stop 
18 08 10  ---          13 27 31  69.1 228.1  1.1      41.7   168     1645   18 05 10

18 08 10  J1215+17     13 27 31  68.6 234.0  1.2      46.6   -12     1645   No stop 
18 09 30  ---          13 28 51  68.4 234.6  1.2      47.1    68     1650   18 08 10

18 09 30  SN1979C      13 28 51  68.9 228.7  1.1      42.2   -12     1650   No stop 
18 12 30  ---          13 31 51  68.4 230.2  1.1      43.4   168     1662   18 09 30

18 13 00  J1215+17     13 32 21  67.7 236.1  1.3      48.3    18     1662   18 12 55
18 14 20  ---          13 33 42  67.5 236.6  1.3      48.7    80     1667   18 12 55

18 14 20  SN1979C      13 33 42  68.1 231.0  1.2      44.0   -12     1667   No stop 
18 17 20  ---          13 36 42  67.6 232.4  1.2      45.1   168     1679   18 14 20

18 17 20  J1215+17     13 36 42  67.0 237.9  1.4      49.6   -12     1679   No stop 
18 18 40  ---          13 38 02  66.7 238.4  1.4      50.0    68     1684   18 17 20

18 18 40  SN1979C      13 38 02  67.4 233.0  1.2      45.6   -12     1684   No stop 
18 21 40  ---          13 41 03  66.9 234.3  1.3      46.5   168     1696   18 18 40

18 21 40  J1215+17     13 41 03  66.2 239.5  1.4      50.8   -12     1696   No stop 
18 23 00  ---          13 42 23  65.9 240.0  1.4      51.2    68     1701   18 21 40

18 23 00  SN1979C      13 42 23  66.6 234.9  1.3      47.0   -12     1701   No stop 
18 26 00  ---          13 45 24  66.1 236.1  1.4      47.9   168     1712   18 23 00

18 26 30  J1215+17     13 45 54  65.3 241.3  1.5      52.0    19     1712   18 26 25
18 27 50  ---          13 47 14  65.0 241.8  1.5      52.4    80     1718   18 26 25
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

18 27 50  SN1979C      13 47 14  65.8 236.8  1.4      48.4   -11     1718   No stop 
18 30 50  ---          13 50 14  65.2 237.9  1.4      49.3   169     1730   18 27 50

18 30 50  J1215+17     13 50 14  64.4 242.8  1.6      53.1   -11     1730   No stop 
18 32 10  ---          13 51 35  64.2 243.2  1.6      53.4    69     1735   18 30 50

18 32 10  SN1979C      13 51 35  65.0 238.4  1.5      49.6   -11     1735   No stop 
18 35 10  ---          13 54 35  64.4 239.5  1.5      50.4   169     1746   18 32 10

18 35 10  J1215+17     13 54 35  63.6 244.2  1.6      54.0   -11     1746   No stop 
18 36 30  ---          13 55 55  63.3 244.6  1.7      54.3    69     1752   18 35 10

18 36 30  SN1979C      13 55 55  64.2 240.0  1.5      50.7   -11     1752   No stop 
18 39 30  ---          13 58 56  63.6 241.0  1.6      51.5   169     1763   18 36 30

18 40 00  J1215+17     13 59 26  62.6 245.7  1.7      55.0    19     1763   18 39 55
18 41 20  ---          14 00 46  62.4 246.1  1.8      55.3    80     1769   18 39 55

18 41 20  SN1979C      14 00 46  63.3 241.6  1.6      51.9   -11     1769   No stop 
18 44 20  ---          14 03 47  62.7 242.6  1.7      52.5   169     1780   18 41 20

18 44 20  J1215+17     14 03 47  61.8 246.9  1.8      55.8   -11     1780   No stop 
18 45 40  ---          14 05 07  61.5 247.3  1.8      56.0    69     1785   18 44 20

18 45 40  SN1979C      14 05 07  62.4 243.0  1.7      52.8   -11     1785   No stop 
18 48 40  ---          14 08 07  61.8 244.0  1.7      53.4   169     1797   18 45 40

18 48 40  J1215+17     14 08 07  60.9 248.2  1.9      56.6   -11     1797   No stop 
18 50 00  ---          14 09 28  60.7 248.5  1.9      56.8    69     1802   18 48 40

18 50 00  SN1979C      14 09 28  61.6 244.4  1.8      53.7   -11     1802   No stop 
18 53 00  ---          14 12 28  61.0 245.3  1.8      54.3   169     1814   18 50 00

18 53 30  J1215+17     14 12 58  60.0 249.4  2.0      57.3    19     1814   18 53 25
18 54 50  ---          14 14 18  59.7 249.8  2.0      57.5    80     1819   18 53 25

18 54 50  SN1979C      14 14 18  60.6 245.8  1.8      54.6   -11     1819   No stop 
18 57 50  ---          14 17 19  60.0 246.6  1.9      55.1   169     1831   18 54 50

18 57 50  J1215+17     14 17 19  59.1 250.5  2.0      58.0   -11     1831   No stop 
18 59 10  ---          14 18 39  58.8 250.9  2.0      58.1    69     1836   18 57 50

18 59 10  SN1979C      14 18 39  59.8 247.0  1.9      55.4   -11     1836   No stop 
19 02 10  ---          14 21 40  59.2 247.8  2.0      55.9   169     1848   18 59 10
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

19 02 10  J1215+17     14 21 40  58.2 251.6  2.1      58.5   -11     1848   No stop 
19 03 30  ---          14 23 00  57.9 251.9  2.1      58.7    69     1853   19 02 10

19 03 30  SN1979C      14 23 00  58.9 248.2  2.0      56.1   -11     1853   No stop 
19 06 30  ---          14 26 00  58.3 248.9  2.0      56.5   169     1864   19 03 30

19 07 00  J1215+17     14 26 30  57.2 252.7  2.2      59.1    20     1864   19 06 55
19 08 20  ---          14 27 51  56.9 253.0  2.2      59.3    80     1870   19 06 55

19 08 20  SN1979C      14 27 51  57.9 249.4  2.1      56.8   -10     1870   No stop 
19 11 20  ---          14 30 51  57.3 250.1  2.1      57.2   170     1881   19 08 20

19 11 20  J1215+17     14 30 51  56.3 253.7  2.3      59.6   -10     1881   No stop 
19 12 40  ---          14 32 11  56.0 254.0  2.3      59.8    70     1887   19 11 20

19 12 40  SN1979C      14 32 11  57.1 250.4  2.1      57.4   -10     1887   No stop 
19 15 40  ---          14 35 12  56.5 251.2  2.2      57.8   170     1898   19 12 40

19 15 40  J1215+17     14 35 12  55.4 254.6  2.3      60.1   -10     1898   No stop 
19 17 00  ---          14 36 32  55.1 254.9  2.3      60.2    70     1903   19 15 40

19 17 00  SN1979C      14 36 32  56.2 251.5  2.2      57.9   -10     1903   No stop 
19 20 00  ---          14 39 32  55.6 252.1  2.3      58.3   170     1915   19 17 00

19 20 30  J1215+17     14 40 03  54.4 255.6  2.4      60.5    20     1915   19 20 25
19 21 50  ---          14 41 23  54.1 255.9  2.4      60.7    80     1921   19 20 25

19 21 50  SN1979C      14 41 23  55.2 252.6  2.3      58.5   -10     1921   No stop 
19 24 50  ---          14 44 23  54.6 253.2  2.3      58.8   170     1932   19 21 50

19 24 50  J1215+17     14 44 23  53.5 256.5  2.5      60.9   -10     1932   No stop 
19 26 10  ---          14 45 43  53.2 256.7  2.5      61.0    70     1937   19 24 50

19 26 10  SN1979C      14 45 43  54.3 253.5  2.4      59.0   -10     1937   No stop 
19 29 10  ---          14 48 44  53.7 254.1  2.4      59.3   170     1949   19 26 10

19 29 10  J1215+17     14 48 44  52.6 257.3  2.6      61.3   -10     1949   No stop 
19 30 30  ---          14 50 04  52.3 257.6  2.6      61.4    70     1954   19 29 10

19 30 30  SN1979C      14 50 04  53.4 254.4  2.4      59.4   -10     1954   No stop 
19 33 30  ---          14 53 05  52.8 255.0  2.5      59.7   170     1966   19 30 30

19 34 00  J1215+17     14 53 35  51.6 258.2  2.6      61.6    20     1966   19 33 55
19 35 20  ---          14 54 55  51.3 258.4  2.7      61.7    80     1971   19 33 55
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

19 35 20  SN1979C      14 54 55  52.4 255.4  2.5      59.9   -10     1971   No stop 
19 38 20  ---          14 57 55  51.8 256.0  2.6      60.1   170     1983   19 35 20

19 38 20  J1215+17     14 57 55  50.6 259.0  2.7      61.9   -10     1983   No stop 
19 39 40  ---          14 59 16  50.4 259.2  2.7      62.0    70     1988   19 38 20

19 39 40  SN1979C      14 59 16  51.5 256.2  2.6      60.2   -10     1988   No stop 
19 42 40  ---          15 02 16  50.9 256.8  2.6      60.5   170     2000   19 39 40

19 42 40  J1215+17     15 02 16  49.7 259.7  2.8      62.2   -10     2000   No stop 
19 44 00  ---          15 03 36  49.4 260.0  2.8      62.3    70     2005   19 42 40

19 44 00  SN1979C      15 03 36  50.6 257.0  2.7      60.6   -10     2005   No stop 
19 47 00  ---          15 06 37  49.9 257.6  2.7      60.8   170     2016   19 44 00

19 47 30  J1215+17     15 07 07  48.7 260.6  2.9      62.5    20     2016   19 47 25
19 48 50  ---          15 08 27  48.4 260.8  2.9      62.6    80     2022   19 47 25

19 48 50  SN1979C      15 08 27  49.6 257.9  2.7      60.9   -10     2022   No stop 
19 51 50  ---          15 11 28  48.9 258.5  2.8      61.1   170     2033   19 48 50

19 51 50  J1215+17     15 11 28  47.8 261.3  2.9      62.7   -10     2033   No stop 
19 53 10  ---          15 12 48  47.5 261.5  3.0      62.8    70     2039   19 51 50

19 53 10  SN1979C      15 12 48  48.6 258.7  2.8      61.2   -10     2039   No stop 
19 56 10  ---          15 15 48  48.0 259.2  2.9      61.4   170     2050   19 53 10

19 56 10  J1215+17     15 15 48  46.9 262.0  3.0      62.9   -10     2050   No stop 
19 57 30  ---          15 17 09  46.6 262.2  3.0      63.0    70     2055   19 56 10

19 57 30  SN1979C      15 17 09  47.7 259.5  2.9      61.5   -10     2055   No stop 
20 00 30  ---          15 20 09  47.1 260.0  2.9      61.7   170     2067   19 57 30

20 01 00  J1215+17     15 20 39  45.8 262.8  3.1      63.1    20     2067   20 00 55
20 02 20  ---          15 21 59  45.5 263.0  3.1      63.2    80     2072   20 00 55

20 02 20  SN1979C      15 21 59  46.7 260.3  3.0      61.8   -10     2072   No stop 
20 05 20  ---          15 25 00  46.1 260.8  3.0      61.9   170     2084   20 02 20

20 05 20  J1215+17     15 25 00  44.9 263.4  3.2      63.3   -10     2084   No stop 
20 06 40  ---          15 26 20  44.6 263.6  3.2      63.3    70     2089   20 05 20

20 06 40  SN1979C      15 26 20  45.8 261.0  3.0      62.0   -10     2089   No stop 
20 09 40  ---          15 29 21  45.1 261.5  3.1      62.1   170     2101   20 06 40
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

20 09 40  J1215+17     15 29 21  44.0 264.1  3.2      63.4   -10     2101   No stop 
20 11 00  ---          15 30 41  43.7 264.3  3.3      63.4    70     2106   20 09 40

20 11 00  SN1979C      15 30 41  44.9 261.7  3.1      62.2   -10     2106   No stop 
20 14 00  ---          15 33 41  44.2 262.2  3.2      62.3   170     2118   20 11 00

20 14 30  J1215+17     15 34 11  42.9 264.8  3.3      63.5    20     2118   20 14 25
20 15 50  ---          15 35 32  42.6 265.0  3.3      63.6    80     2123   20 14 25

20 15 50  SN1979C      15 35 32  43.8 262.4  3.2      62.4   -10     2123   No stop 
20 18 50  ---          15 38 32  43.2 262.9  3.2      62.5   170     2135   20 15 50

20 18 50  J1215+17     15 38 32  42.0 265.4  3.4      63.7   -10     2135   No stop 
20 20 10  ---          15 39 52  41.7 265.6  3.4      63.7    70     2140   20 18 50

20 20 10  SN1979C      15 39 52  42.9 263.1  3.3      62.6   -10     2140   No stop 
20 23 10  ---          15 42 53  42.3 263.6  3.3      62.7   170     2151   20 20 10

20 23 10  J1215+17     15 42 53  41.1 266.0  3.5      63.7   -10     2151   No stop 
20 24 30  ---          15 44 13  40.8 266.2  3.5      63.8    70     2157   20 23 10

20 24 30  SN1979C      15 44 13  42.0 263.8  3.3      62.7   -10     2157   No stop 
20 27 30  ---          15 47 14  41.3 264.2  3.4      62.8   170     2168   20 24 30

20 28 00  J1215+17     15 47 44  40.0 266.7  3.5      63.8    20     2168   20 27 55
20 29 20  ---          15 49 04  39.7 266.9  3.6      63.9    80     2174   20 27 55

20 29 20  SN1979C      15 49 04  40.9 264.5  3.4      62.8   -10     2174   No stop 
20 32 20  ---          15 52 04  40.3 264.9  3.5      62.9   170     2185   20 29 20

20 32 20  J1215+17     15 52 04  39.1 267.3  3.6      63.9   -10     2185   No stop 
20 33 40  ---          15 53 25  38.8 267.5  3.6      63.9    70     2191   20 32 20

20 33 40  SN1979C      15 53 25  40.0 265.1  3.5      63.0   -10     2191   No stop 
20 36 40  ---          15 56 25  39.4 265.5  3.5      63.0   170     2202   20 33 40

20 36 40  J1215+17     15 56 25  38.2 267.9  3.7      63.9   -10     2202   No stop 
20 38 00  ---          15 57 45  37.9 268.1  3.7      64.0    70     2207   20 36 40

20 38 00  SN1979C      15 57 45  39.1 265.7  3.6      63.1   -10     2207   No stop 
20 41 00  ---          16 00 46  38.4 266.1  3.6      63.1   170     2219   20 38 00

20 41 30  J1215+17     16 01 16  37.1 268.5  3.8      64.0    20     2219   20 41 25
20 42 50  ---          16 02 36  36.8 268.7  3.8      64.0    80     2224   20 41 25
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

20 42 50  SN1979C      16 02 36  38.0 266.4  3.7      63.1   -10     2224   No stop 
20 45 50  ---          16 05 37  37.4 266.8  3.7      63.2   170     2236   20 42 50

20 45 50  J1215+17     16 05 37  36.2 269.1  3.8      64.0   -10     2236   No stop 
20 47 10  ---          16 06 57  35.9 269.3  3.9      64.0    70     2241   20 45 50

20 47 10  SN1979C      16 06 57  37.1 267.0  3.7      63.2   -10     2241   No stop 
20 50 10  ---          16 09 57  36.4 267.4  3.8      63.3   170     2253   20 47 10

20 50 10  J1215+17     16 09 57  35.2 269.7  3.9      64.0   -10     2253   No stop 
20 51 30  ---          16 11 18  35.0 269.8  3.9      64.0    70     2258   20 50 10

20 51 30  SN1979C      16 11 18  36.2 267.6  3.8      63.3   -10     2258   No stop 
20 54 30  ---          16 14 18  35.5 268.0  3.8      63.3   170     2270   20 51 30

20 54 30  J1215+17     16 14 18  34.3 270.2  4.0      64.0   -10     2270   No stop 
20 55 50  ---          16 15 38  34.0 270.4  4.0      64.0    70     2275   20 54 30

20 55 50  SN1979C      16 15 38  35.2 268.1  3.9      63.3   -10     2275   No stop 
20 58 40  ---          16 18 29  34.6 268.5  3.9      63.3   160     2286   20 55 50

20 58 40  J1215+17     16 18 29  33.4 270.7  4.0      64.0   -10     2286   No stop 
21 00 00  ---          16 19 49  33.1 270.9  4.1      64.0    70     2291   20 58 40

21 00 00  SN1979C      16 19 49  34.3 268.7  3.9      63.3   -10     2291   No stop 
21 03 00  ---          16 22 49  33.7 269.1  4.0      63.4   170     2302   21 00 00

21 03 30  J1215+17     16 23 19  32.4 271.3  4.1      64.0    20     2302   21 03 25
21 04 50  ---          16 24 40  32.1 271.5  4.1      64.0    80     2308   21 03 25

21 04 50  SN1979C      16 24 40  33.3 269.3  4.0      63.4   -10     2308   No stop 
21 07 50  ---          16 27 40  32.6 269.7  4.1      63.4   170     2320   21 04 50

21 07 50  J1215+17     16 27 40  31.4 271.9  4.2      64.0   -10     2320   No stop 
21 09 10  ---          16 29 00  31.1 272.0  4.2      64.0    70     2325   21 07 50

21 09 10  SN1979C      16 29 00  32.4 269.9  4.1      63.4   -10     2325   No stop 
21 12 10  ---          16 32 01  31.7 270.3  4.1      63.4   170     2336   21 09 10

21 12 10  J1215+17     16 32 01  30.5 272.4  4.3      63.9   -10     2336   No stop 
21 13 30  ---          16 33 21  30.2 272.6  4.3      63.9    70     2341   21 12 10

21 13 30  SN1979C      16 33 21  31.4 270.4  4.2      63.4   -10     2341   No stop 
21 16 30  ---          16 36 22  30.8 270.8  4.2      63.4   170     2353   21 13 30
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

21 17 00  J1215+17     16 36 52  29.5 273.0  4.4      63.9    20     2353   21 16 55
21 18 20  ---          16 38 12  29.2 273.2  4.4      63.8    80     2359   21 16 55

21 18 20  SN1979C      16 38 12  30.4 271.0  4.2      63.4   -10     2359   No stop 
21 21 20  ---          16 41 12  29.7 271.4  4.3      63.3   170     2370   21 18 20

21 21 20  J1215+17     16 41 12  28.5 273.5  4.4      63.8   -10     2370   No stop 
21 22 40  ---          16 42 33  28.2 273.7  4.4      63.8    70     2375   21 21 20

21 22 40  SN1979C      16 42 33  29.4 271.6  4.3      63.3   -10     2375   No stop 
21 25 40  ---          16 45 33  28.8 272.0  4.4      63.3   170     2387   21 22 40

21 25 40  J1215+17     16 45 33  27.6 274.0  4.5      63.7   -10     2387   No stop 
21 27 00  ---          16 46 53  27.3 274.2  4.5      63.7    70     2392   21 25 40

21 27 00  SN1979C      16 46 53  28.5 272.1  4.4      63.3   -10     2392   No stop 
21 30 00  ---          16 49 54  27.9 272.5  4.4      63.3   170     2404   21 27 00

21 30 30  J1215+17     16 50 24  26.6 274.6  4.6      63.6    20     2404   21 30 25
21 31 50  ---          16 51 44  26.3 274.8  4.6      63.6    80     2409   21 30 25

21 31 50  SN1979C      16 51 44  27.5 272.7  4.5      63.2   -10     2409   No stop 
21 34 50  ---          16 54 45  26.8 273.1  4.5      63.2   170     2421   21 31 50

21 34 50  J1215+17     16 54 45  25.6 275.1  4.7      63.6   -10     2421   No stop 
21 36 10  ---          16 56 05  25.3 275.3  4.7      63.5    70     2426   21 34 50

21 36 10  SN1979C      16 56 05  26.5 273.2  4.5      63.2   -10     2426   No stop 
21 39 10  ---          16 59 05  25.9 273.6  4.6      63.1   170     2438   21 36 10

21 39 10  J1215+17     16 59 05  24.7 275.6  4.7      63.5   -10     2438   No stop 
21 40 30  ---          17 00 26  24.4 275.8  4.7      63.4    70     2443   21 39 10

21 40 30  SN1979C      17 00 26  25.6 273.8  4.6      63.1   -10     2443   No stop 
21 43 30  ---          17 03 26  25.0 274.1  4.7      63.1   170     2454   21 40 30

21 44 00  J1215+17     17 03 56  23.7 276.2  4.8      63.3    20     2454   21 43 55
21 45 20  ---          17 05 16  23.4 276.4  4.8      63.3    80     2460   21 43 55

21 45 20  SN1979C      17 05 16  24.6 274.3  4.7      63.0   -10     2460   No stop 
21 48 20  ---          17 08 17  23.9 274.7  4.7      63.0   170     2471   21 45 20

21 48 20  J1215+17     17 08 17  22.7 276.7  4.9      63.2   -10     2471   No stop 
21 49 40  ---          17 09 37  22.4 276.9  4.9      63.2    70     2477   21 48 20
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

21 49 40  SN1979C      17 09 37  23.6 274.9  4.8      63.0   -10     2477   No stop 
21 52 40  ---          17 12 38  23.0 275.2  4.8      62.9   170     2488   21 49 40

21 52 40  J1215+17     17 12 38  21.8 277.2  4.9      63.1   -10     2488   No stop 
21 54 00  ---          17 13 58  21.5 277.4  5.0      63.1    70     2493   21 52 40

21 54 00  SN1979C      17 13 58  22.7 275.4  4.8      62.9   -10     2493   No stop 
21 57 00  ---          17 16 58  22.1 275.7  4.9      62.8   170     2505   21 54 00

21 57 30  J1215+17     17 17 28  20.8 277.8  5.0      63.0    20     2505   21 57 25
21 58 50  ---          17 18 49  20.5 278.0  5.1      62.9    80     2510   21 57 25

21 58 50  SN1979C      17 18 49  21.7 276.0  4.9      62.8   -10     2510   No stop 
22 01 50  ---          17 21 49  21.0 276.3  5.0      62.7   170     2522   21 58 50

22 01 50  J1215+17     17 21 49  19.8 278.3  5.1      62.8   -10     2522   No stop 
22 03 10  ---          17 23 09  19.6 278.5  5.1      62.8    70     2527   22 01 50

22 03 10  SN1979C      17 23 09  20.7 276.5  5.0      62.6   -10     2527   No stop 
22 06 10  ---          17 26 10  20.1 276.8  5.0      62.6   170     2539   22 03 10

22 06 10  J1215+17     17 26 10  18.9 278.8  5.2      62.7   -10     2539   No stop 
22 07 30  ---          17 27 30  18.6 279.0  5.2      62.6    70     2544   22 06 10

22 07 30  SN1979C      17 27 30  19.8 277.0  5.1      62.5   -10     2544   No stop 
22 10 30  ---          17 30 30  19.2 277.3  5.1      62.4   170     2556   22 07 30

22 11 00  J1215+17     17 31 01  17.9 279.4  5.3      62.5    20     2556   22 10 55
22 12 20  ---          17 32 21  17.6 279.5  5.3      62.5    80     2561   22 10 55

22 12 20  SN1979C      17 32 21  18.8 277.6  5.1      62.4   -10     2561   No stop 
22 15 20  ---          17 35 21  18.1 277.9  5.2      62.3   170     2573   22 12 20

22 15 20  J1215+17     17 35 21  17.0 279.9  5.3      62.3   -10     2573   No stop 
22 16 40  ---          17 36 42  16.7 280.0  5.4      62.3    70     2578   22 15 20

22 16 40  SN1979C      17 36 42  17.8 278.1  5.2      62.3   -10     2578   No stop 
22 19 40  ---          17 39 42  17.2 278.4  5.3      62.2   170     2590   22 16 40

22 19 40  J1215+17     17 39 42  16.0 280.4  5.4      62.2   -10     2590   No stop 
22 21 00  ---          17 41 02  15.8 280.5  5.4      62.1    70     2595   22 19 40

22 21 00  SN1979C      17 41 02  16.9 278.6  5.3      62.1   -10     2595   No stop 
22 24 00  ---          17 44 03  16.3 278.9  5.3      62.0   170     2606   22 21 00
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

22 24 30  J1215+17     17 44 33  15.0 280.9  5.5      62.0    20     2606   22 24 25
22 25 50  ---          17 45 53  14.7 281.1  5.5      61.9    80     2612   22 24 25

22 25 50  SN1979C      17 45 53  15.9 279.2  5.4      61.9   -10     2612   No stop 
22 28 50  ---          17 48 54  15.2 279.5  5.4      61.8   170     2623   22 25 50

22 28 50  J1215+17     17 48 54  14.1 281.4  5.6      61.8   -10     2623   No stop 
22 30 10  ---          17 50 14  13.8 281.6  5.6      61.7    70     2629   22 28 50

22 30 10  SN1979C      17 50 14  15.0 279.7  5.4      61.8   -10     2629   No stop 
22 33 10  ---          17 53 14  14.3 280.0  5.5      61.7   170     2640   22 30 10

22 33 10  J1215+17     17 53 14  13.2 282.0  5.6      61.6   -10     2640   No stop 
22 34 30  ---          17 54 34  12.9 282.1  5.6      61.5    70     2645   22 33 10

22 34 30  SN1979C      17 54 34  14.0 280.2  5.5      61.6   -10     2645   No stop 
22 37 30  ---          17 57 35  13.4 280.5  5.6      61.5   170     2657   22 34 30

22 38 00  J1215+17     17 58 05  12.2 282.5  5.7      61.4    20     2657   22 37 55
22 39 20  ---          17 59 25  11.9 282.7  5.7      61.3    80     2662   22 37 55

22 39 20  SN1979C      17 59 25  13.0 280.7  5.6      61.4   -10     2662   No stop 
22 42 20  ---          18 02 26  12.4 281.1  5.6      61.3   170     2674   22 39 20

22 42 20  J1215+17     18 02 26  11.3 283.0  5.8      61.1   -10     2674   No stop 
22 43 40  ---          18 03 46  11.0 283.2  5.8      61.1    70     2679   22 42 20

22 43 40  SN1979C      18 03 46  12.1 281.3  5.7      61.2   -10     2679   No stop 
22 46 40  ---          18 06 46  11.5 281.6  5.7      61.1   170     2691   22 43 40

22 46 40  J1215+17     18 06 46  10.3 283.5  5.9      60.9   -10     2691   No stop 
22 48 00  ---          18 08 07  10.1 283.7  5.9      60.9    70     2696   22 46 40

22 48 00  SN1979C      18 08 07  11.2 281.8  5.7      61.1   -10     2696   No stop 
22 50 30  ---          18 10 37  10.7 282.1  5.8      60.9   140     2706   22 48 00

22 51 00  J1215+17     18 11 07   9.4 284.1  5.9      60.7    20     2706   22 50 55
22 52 20  ---          18 12 27   9.2 284.2  5.9      60.6    80     2711   22 50 55

22 52 20  SN1979C      18 12 27  10.3 282.3  5.8      60.9   -10     2711   No stop 
22 54 50  ---          18 14 58   9.7 282.6  5.9      60.7   140     2721   22 52 20

22 54 50  J1215+17     18 14 58   8.6 284.5  6.0      60.5   -10     2721   No stop 
22 56 10  ---          18 16 18   8.4 284.7  6.0      60.4    70     2726   22 54 50
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2011   Day 298 ---

22 56 10  SN1979C      18 16 18   9.5 282.8  5.9      60.7   -10     2726   No stop 
22 58 40  ---          18 18 48   8.9 283.1  5.9      60.6   140     2736   22 56 10

22 58 40  J1215+17     18 18 48   7.8 285.0  6.1      60.3   -10     2736   No stop 
23 00 00  ---          18 20 09   7.6 285.1  6.1      60.2    70     2741   22 58 40


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: globGbps.6cm
   Matching groups in /usr/local/sched/catalogs/freq.dat:
     v6cm_2

   Setup group:   12         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:4           Bits per sample: 1         Sample rate: 32.000
   Number of channels: 16    DBE type:                  Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
             4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
                   5         6         5         6         7         8         7         8
   BBC SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on these setups were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4942.49   4942.49   4942.49   4942.49   4974.49   4974.49   4974.49   4974.49
              5006.49   5006.49   5006.49   5006.49   5038.49   5038.49   5038.49   5038.49
   BBC fr=     842.49    842.49    842.49    842.49    874.49    874.49    874.49    874.49
               906.49    906.49    906.49    906.49    938.49    938.49    938.49    938.49
   Bandwd=     16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000
               16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000
    Matching frequency sets:   1   2   3   4   5   6   7   8   9  20

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S9    S11   S13   S15
    PCALXB2=   S2    S4    S6    S8    S10   S12   S14   S16
    PCALFR1=   490   510   490   510   490   510   490   510
    PCALFR2=   490   510   490   510   490   510   490   510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27, 66, 74, 82, 90, 67, 75, 83, 91
    barrel=roll_off 
 SOURCES USED IN RECORDING SCANS --                         11th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SN1979C           12 20 26.708149   * 12 22 58.666427     12 23 34.258856       0.00
                     16 04 29.46765    * 15 47 51.95179      15 43 54.62585        0.00
                     From catalog imbedded in main SCHED input file.
                        8.994 scan and    665.198 baseline hours in setup: globGbps.6cm
                     Frequency sets (dups not shown):   1 10 11 12 13 14 15 16 17 18 19

 * 3C273             12 26 33.246145   * 12 29 06.700041     12 29 42.737584       0.00
                     02 19 43.30589    * 02 03 08.59840      01 59 14.55075        0.00
                     From catalog imbedded in main SCHED input file.
                        0.022 scan and      3.400 baseline hours in setup: globGbps.6cm
                     Frequency sets (dups not shown):   1 10 11 12 13 14 15 16 18 19

 * J1215+17          12 12 31.449683   * 12 15 03.979124     12 15 39.719922       0.00
                     17 11 18.14600    * 16 54 37.95736      16 50 39.48527        0.00
                     From catalog imbedded in main SCHED input file.
                        4.267 scan and    315.053 baseline hours in setup: globGbps.6cm
                     Frequency sets (dups not shown):   1 10 11 12 13 14 15 16 17 18 19

 * OQ208             14 04 45.615152   * 14 07 00.394411     14 07 31.518027       0.00
                     28 41 29.23491    * 28 27 14.68994      28 23 54.84502        0.00
                     From catalog imbedded in main SCHED input file.
                        0.050 scan and      2.531 baseline hours in setup: globGbps.6cm
                     Frequency sets (dups not shown):   1 18

 * OJ287             08 51 57.250620   * 08 54 48.874931     08 55 30.167405       0.00
                     20 17 58.41739    * 20 06 30.64084      20 03 41.25723        0.00
                     From catalog imbedded in main SCHED input file.
                        0.050 scan and      6.800 baseline hours in setup: globGbps.6cm
                     Frequency sets (dups not shown):   1 10 11 12 13 14 15 16 17



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1979C             36.5
   3C273               26.3
   J1215+17            38.6
   OQ208               40.6
   OJ287               81.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

