  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
 Exp. Code:  GB074   


Schedule Version:       1.40
Processed by SCHED version:  11.40  Beta release 11.4.   June 17, 2014

PI:       M. Bietenholz

Address:  York University
          Toronto, ON M3J 1P3
          Canada
 

Phone:    +27-12-301-3100 (work)
EMAIL:    michael@yorku.ca
Fax:      +1-416-736-5516
Phone during observation: +27-76-882-3872 (cell)

Observing mode: VLBA 512-16-2-ul 6cm

Notes:    ***** single version tying in Jb ********
          Fringe finder  : 3C84
          Pol. Calibrator: 3C84
          Amplitude check: 3C66A

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  22 Oct 2014   Day 295 ---

 Next scan frequencies:  4924.75  4924.75  5003.25  5003.25
 Next BBC frequencies:    824.75   824.75   903.25   903.25
 Next scan bandwidths:     64.00    64.00    64.00    64.00

16 00 00  3C84         11 08 15   2.7 -41.9  7.8  H   50.2     0        0   16 00 00
16 04 00  ---          11 12 15   2.1 -41.5  7.9  D   49.6     0       31   16 00 00

23 16 10  3C66A        18 25 36   2.2  39.5 -8.0  D  -48.5 25916       31   23 16 10
23 17 20  ---          18 26 46   2.4  39.6 -7.9  H  -48.7     0       40   23 16 10

23 19 50  3C66A        18 29 17   2.7  39.9 -7.9  H  -49.1   144       40   23 19 50
23 21 00  ---          18 30 27   2.9  40.1 -7.9  H  -49.3     0       49   23 19 50

23 21 00  SN1986J      18 30 27   2.4  40.6 -7.9  H  -49.3    -9       49   23 21 09
23 23 00  ---          18 32 27   2.7  40.9 -7.9  H  -49.7     0       63   23 21 09

23 23 00  3C66A        18 32 27   3.2  40.3 -7.9     -49.7    -9       63   23 23 09
23 24 10  ---          18 33 38   3.3  40.4 -7.8     -49.9    61       71   23 23 09

23 24 10  SN1986J      18 33 38   2.9  41.0 -7.8     -49.9    -9       71   23 24 19
23 26 10  ---          18 35 38   3.2  41.2 -7.8     -50.2   111       85   23 24 19

23 26 10  3C66A        18 35 38   3.6  40.7 -7.8     -50.2    -9       85   23 26 19
23 27 20  ---          18 36 48   3.8  40.8 -7.8     -50.4    61       93   23 26 19

23 27 20  SN1986J      18 36 48   3.3  41.4 -7.8     -50.4    -9       93   23 27 29
23 29 20  ---          18 38 48   3.6  41.6 -7.7     -50.7   111      108   23 27 29

23 29 50  3C66A        18 39 19   4.1  41.1 -7.7     -50.8    21      108   23 29 50
23 31 20  ---          18 40 49   4.3  41.3 -7.7     -51.0    90      119   23 29 50

23 31 20  SN1986J      18 40 49   3.9  41.8 -7.7     -51.0    -9      119   23 31 29
23 33 20  ---          18 42 49   4.2  42.1 -7.7     -51.3   111      133   23 31 29

23 33 20  3C66A        18 42 49   4.6  41.5 -7.7     -51.4    -9      133   23 33 29
23 34 30  ---          18 43 59   4.8  41.6 -7.7     -51.5    61      141   23 33 29

23 34 30  SN1986J      18 43 59   4.4  42.2 -7.7     -51.5    -9      141   23 34 39
23 36 30  ---          18 46 00   4.7  42.4 -7.6     -51.8   111      156   23 34 39

23 36 30  3C66A        18 46 00   5.1  41.9 -7.6     -51.9    -9      156   23 36 39
23 37 40  ---          18 47 10   5.2  42.0 -7.6     -52.1    61      163   23 36 39

23 37 40  SN1986J      18 47 10   4.8  42.6 -7.6     -52.0    -9      163   23 37 49
23 39 40  ---          18 49 10   5.1  42.8 -7.6     -52.3   111      178   23 37 49
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  22 Oct 2014   Day 295 ---

23 40 10  3C66A        18 49 40   5.6  42.3 -7.6     -52.5    21      178   23 40 10
23 41 20  ---          18 50 50   5.8  42.4 -7.5     -52.6    70      187   23 40 10

23 41 20  SN1986J      18 50 50   5.4  43.0 -7.5     -52.6    -9      187   23 41 29
23 43 20  ---          18 52 51   5.7  43.2 -7.5     -52.9   111      201   23 41 29

23 43 20  3C66A        18 52 51   6.1  42.6 -7.5     -53.0    -9      201   23 43 29
23 44 30  ---          18 54 01   6.2  42.8 -7.5     -53.2    61      209   23 43 29

23 44 30  SN1986J      18 54 01   5.8  43.3 -7.5     -53.1    -9      209   23 44 39
23 46 30  ---          18 56 01   6.1  43.6 -7.5     -53.4   111      223   23 44 39

23 46 30  3C66A        18 56 01   6.5  43.0 -7.5     -53.5    -9      223   23 46 39
23 47 40  ---          18 57 11   6.7  43.1 -7.4     -53.7    61      231   23 46 39

23 47 40  SN1986J      18 57 11   6.3  43.7 -7.4     -53.6    -8      231   23 47 48
23 49 40  ---          18 59 12   6.6  43.9 -7.4     -53.9   112      246   23 47 48

23 50 00  3C66A        18 59 32   7.1  43.4 -7.4     -54.0    11      246   23 50 00
23 51 10  ---          19 00 42   7.2  43.5 -7.4     -54.2    70      255   23 50 00

23 51 30  SN1986J      19 01 02   6.9  44.1 -7.4     -54.2    12      255   23 51 30
23 53 10  ---          19 02 42   7.1  44.3 -7.3     -54.5   100      267   23 51 30

23 53 10  3C66A        19 02 42   7.5  43.7 -7.3     -54.5    -9      267   23 53 19
23 54 20  ---          19 03 53   7.7  43.8 -7.3     -54.7    61      275   23 53 19

23 54 20  SN1986J      19 03 53   7.3  44.4 -7.3     -54.7    -8      275   23 54 28
23 55 20  ---          19 04 53   7.5  44.5 -7.3     -54.8    52      282   23 54 28

23 56 30  3C66A        19 06 03   8.0  44.1 -7.3     -55.0    61      282   23 56 30
23 59 50  ---          19 09 23   8.5  44.4 -7.2     -55.6   200      308   23 56 30

 --- Thu  23 Oct 2014   Day 296 ---

00 00 20  SN1986J      19 09 54   8.2  45.1 -7.2     -55.6    22      308   00 00 20
00 02 20  ---          19 11 54   8.5  45.3 -7.2     -55.9   120      323   00 00 20

00 02 50  3C66A        19 12 24   9.0  44.7 -7.2     -56.0    22      323   00 02 50
00 04 20  ---          19 13 54   9.2  44.9 -7.2     -56.3    90      335   00 02 50

00 04 20  SN1986J      19 13 54   8.8  45.5 -7.2     -56.2    -8      335   00 04 28
00 06 20  ---          19 15 55   9.1  45.7 -7.1     -56.5   112      349   00 04 28
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

00 06 20  3C66A        19 15 55   9.5  45.1 -7.1     -56.6    -8      349   00 06 28
00 07 30  ---          19 17 05   9.7  45.2 -7.1     -56.8    62      357   00 06 28

00 07 30  SN1986J      19 17 05   9.3  45.8 -7.1     -56.7    -8      357   00 07 38
00 09 30  ---          19 19 05   9.6  46.0 -7.1     -57.0   112      372   00 07 38

00 09 30  3C66A        19 19 05  10.0  45.4 -7.1     -57.1    -8      372   00 09 38
00 10 40  ---          19 20 15  10.2  45.5 -7.1     -57.2    62      380   00 09 38

00 10 40  SN1986J      19 20 15   9.8  46.1 -7.1     -57.2    -8      380   00 10 48
00 12 40  ---          19 22 16  10.1  46.3 -7.0     -57.5   112      394   00 10 48

00 13 10  3C66A        19 22 46  10.6  45.8 -7.0     -57.6    22      394   00 13 10
00 14 20  ---          19 23 56  10.7  45.9 -7.0     -57.8    70      403   00 13 10

00 14 20  SN1986J      19 23 56  10.4  46.5 -7.0     -57.7    -8      403   00 14 28
00 16 20  ---          19 25 56  10.7  46.7 -7.0     -58.0   112      418   00 14 28

00 16 20  3C66A        19 25 56  11.1  46.1 -7.0     -58.1    -8      418   00 16 28
00 17 30  ---          19 27 06  11.2  46.2 -6.9     -58.3    62      425   00 16 28

00 17 30  SN1986J      19 27 06  10.9  46.8 -6.9     -58.2    -8      425   00 17 38
00 19 30  ---          19 29 07  11.2  47.0 -6.9     -58.5   112      440   00 17 38

00 19 30  3C66A        19 29 07  11.5  46.4 -6.9     -58.6    -8      440   00 19 38
00 20 40  ---          19 30 17  11.7  46.5 -6.9     -58.8    62      448   00 19 38

00 20 40  SN1986J      19 30 17  11.4  47.1 -6.9     -58.7    -8      448   00 20 48
00 22 40  ---          19 32 17  11.7  47.3 -6.9     -59.0   112      462   00 20 48

00 23 10  3C66A        19 32 47  12.1  46.8 -6.8     -59.1    22      462   00 23 10
00 24 40  ---          19 34 18  12.4  46.9 -6.8     -59.4    90      474   00 23 10

00 24 40  SN1986J      19 34 18  12.0  47.5 -6.8     -59.3    -8      474   00 24 48
00 26 40  ---          19 36 18  12.3  47.7 -6.8     -59.6   112      488   00 24 48

00 26 40  3C66A        19 36 18  12.7  47.1 -6.8     -59.7    -8      488   00 26 48
00 27 50  ---          19 37 28  12.9  47.2 -6.8     -59.8    62      496   00 26 48

00 27 50  SN1986J      19 37 28  12.5  47.8 -6.8     -59.7    -8      496   00 27 58
00 29 50  ---          19 39 28  12.8  48.0 -6.7     -60.0   112      511   00 27 58

00 29 50  3C66A        19 39 28  13.2  47.4 -6.7     -60.1    -8      511   00 29 58
00 31 00  ---          19 40 39  13.4  47.5 -6.7     -60.3    62      519   00 29 58
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

00 31 00  SN1986J      19 40 39  13.0  48.1 -6.7     -60.2    -8      519   00 31 08
00 33 00  ---          19 42 39  13.4  48.3 -6.7     -60.5   112      533   00 31 08

00 33 30  3C66A        19 43 09  13.8  47.7 -6.7     -60.7    22      533   00 33 30
00 34 40  ---          19 44 19  13.9  47.8 -6.7     -60.9    70      542   00 33 30

00 34 40  SN1986J      19 44 19  13.6  48.5 -6.7     -60.7    -8      542   00 34 48
00 36 40  ---          19 46 20  13.9  48.7 -6.6     -61.0   112      557   00 34 48

00 36 40  3C66A        19 46 20  14.3  48.0 -6.6     -61.2    -8      557   00 36 48
00 37 50  ---          19 47 30  14.4  48.1 -6.6     -61.3    62      565   00 36 48

00 37 50  SN1986J      19 47 30  14.1  48.8 -6.6     -61.2    -8      565   00 37 58
00 39 50  ---          19 49 30  14.5  49.0 -6.6     -61.5   112      579   00 37 58

00 39 50  3C66A        19 49 30  14.8  48.3 -6.6     -61.6    -8      579   00 39 58
00 41 00  ---          19 50 40  15.0  48.4 -6.5     -61.8    62      587   00 39 58

00 41 00  SN1986J      19 50 40  14.6  49.1 -6.5     -61.7    -8      587   00 41 08
00 43 00  ---          19 52 41  15.0  49.2 -6.5     -62.0   112      601   00 41 08

00 43 30  3C66A        19 53 11  15.4  48.6 -6.5     -62.2    22      601   00 43 30
00 45 00  ---          19 54 41  15.6  48.8 -6.5     -62.4    90      613   00 43 30

00 45 00  SN1986J      19 54 41  15.3  49.4 -6.5     -62.3    -8      613   00 45 08
00 47 00  ---          19 56 41  15.6  49.6 -6.4     -62.5   112      627   00 45 08

00 47 00  3C66A        19 56 41  15.9  48.9 -6.4     -62.7    -8      627   00 47 08
00 48 10  ---          19 57 51  16.1  49.0 -6.4     -62.9    62      635   00 47 08

00 48 10  SN1986J      19 57 51  15.8  49.7 -6.4     -62.7    -8      635   00 48 18
00 50 10  ---          19 59 52  16.2  49.9 -6.4     -63.0   112      650   00 48 18

00 50 10  3C66A        19 59 52  16.4  49.2 -6.4     -63.2    -8      650   00 50 18
00 51 20  ---          20 01 02  16.6  49.3 -6.4     -63.3    62      658   00 50 18

00 51 20  SN1986J      20 01 02  16.3  50.0 -6.4     -63.2    -8      658   00 51 28
00 53 20  ---          20 03 02  16.7  50.2 -6.3     -63.5   112      672   00 51 28

00 53 50  3C66A        20 03 32  17.0  49.5 -6.3     -63.7    22      672   00 53 50
00 55 00  ---          20 04 43  17.2  49.6 -6.3     -63.9    70      681   00 53 50

00 55 00  SN1986J      20 04 43  17.0  50.3 -6.3     -63.7    -8      681   00 55 08
00 57 00  ---          20 06 43  17.3  50.5 -6.3     -64.0   112      696   00 55 08
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

00 57 00  3C66A        20 06 43  17.6  49.8 -6.3     -64.2    -8      696   00 57 08
00 58 10  ---          20 07 53  17.8  49.9 -6.3     -64.3    62      704   00 57 08

00 58 10  SN1986J      20 07 53  17.5  50.6 -6.3     -64.2    -8      704   00 58 18
01 00 10  ---          20 09 53  17.8  50.7 -6.2     -64.4   112      718   00 58 18

01 00 10  3C66A        20 09 53  18.1  50.1 -6.2     -64.6    -8      718   01 00 18
01 01 20  ---          20 11 04  18.3  50.2 -6.2     -64.8    62      726   01 00 18

01 01 20  SN1986J      20 11 04  18.0  50.8 -6.2     -64.6    -8      726   01 01 28
01 03 20  ---          20 13 04  18.3  51.0 -6.2     -64.9   112      741   01 01 28

01 03 50  3C66A        20 13 34  18.7  50.4 -6.2     -65.2    22      741   01 03 50
01 05 20  ---          20 15 04  18.9  50.5 -6.1     -65.4    90      752   01 03 50

01 05 20  SN1986J      20 15 04  18.7  51.2 -6.1     -65.2    -8      752   01 05 28
01 07 20  ---          20 17 05  19.0  51.3 -6.1     -65.5   112      767   01 05 28

01 07 20  3C66A        20 17 05  19.3  50.6 -6.1     -65.7    -8      767   01 07 28
01 08 30  ---          20 18 15  19.5  50.7 -6.1     -65.8    62      775   01 07 28

01 08 30  SN1986J      20 18 15  19.2  51.4 -6.1     -65.6    -8      775   01 08 38
01 10 30  ---          20 20 15  19.5  51.6 -6.1     -65.9   112      789   01 08 38

01 10 30  3C66A        20 20 15  19.8  50.9 -6.1     -66.1    -8      789   01 10 38
01 11 40  ---          20 21 25  20.0  51.0 -6.0     -66.3    62      797   01 10 38

01 11 40  SN1986J      20 21 25  19.7  51.7 -6.0     -66.1    -8      797   01 11 48
01 13 40  ---          20 23 26  20.1  51.8 -6.0     -66.4   112      811   01 11 48

01 14 10  3C66A        20 23 56  20.4  51.2 -6.0     -66.7    22      811   01 14 10
01 15 20  ---          20 25 06  20.6  51.3 -6.0     -66.8    70      820   01 14 10

01 15 20  SN1986J      20 25 06  20.4  52.0 -6.0     -66.6    -8      820   01 15 28
01 17 20  ---          20 27 06  20.7  52.1 -5.9     -66.9   112      835   01 15 28

01 17 20  3C66A        20 27 06  21.0  51.4 -5.9     -67.1    -8      835   01 17 28
01 18 30  ---          20 28 16  21.2  51.5 -5.9     -67.3    62      843   01 17 28

01 18 30  SN1986J      20 28 16  20.9  52.2 -5.9     -67.1    -8      843   01 18 38
01 20 30  ---          20 30 17  21.2  52.4 -5.9     -67.3   112      857   01 18 38

01 20 30  3C66A        20 30 17  21.5  51.7 -5.9     -67.6    -8      857   01 20 38
01 21 40  ---          20 31 27  21.7  51.7 -5.9     -67.7    62      865   01 20 38
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

01 21 40  SN1986J      20 31 27  21.4  52.5 -5.9     -67.5    -8      865   01 21 48
01 23 40  ---          20 33 27  21.8  52.6 -5.8     -67.8   112      880   01 21 48

01 24 10  3C84         20 33 57  12.0  48.5 -6.8     -59.5     3      880   01 24 10
01 27 10  ---          20 36 58  12.5  48.8 -6.7     -59.9   180      903   01 24 10

01 27 40  3C66A        20 37 28  22.7  52.2 -5.8     -68.6     2      903   01 27 40
01 31 40  ---          20 41 29  23.4  52.5 -5.7     -69.2   240      934   01 27 40

01 32 10  SN1986J      20 41 59  23.3  53.2 -5.7     -69.0    22      934   01 32 10
01 34 10  ---          20 43 59  23.6  53.4 -5.7     -69.3   120      949   01 32 10

01 34 40  3C66A        20 44 29  23.9  52.7 -5.7     -69.6    22      949   01 34 40
01 36 10  ---          20 45 59  24.2  52.8 -5.6     -69.8    90      961   01 34 40

01 36 10  SN1986J      20 45 59  23.9  53.5 -5.6     -69.5    -8      961   01 36 18
01 38 10  ---          20 48 00  24.3  53.7 -5.6     -69.8   112      975   01 36 18

01 38 10  3C66A        20 48 00  24.5  52.9 -5.6     -70.1    -8      975   01 38 18
01 39 20  ---          20 49 10  24.7  53.0 -5.6     -70.3    62      983   01 38 18

01 39 20  SN1986J      20 49 10  24.5  53.7 -5.6     -70.0    -8      983   01 39 28
01 41 20  ---          20 51 10  24.8  53.9 -5.5     -70.3   112      998   01 39 28

01 41 20  3C66A        20 51 10  25.1  53.1 -5.5     -70.6    -8      998   01 41 28
01 42 30  ---          20 52 20  25.3  53.2 -5.5     -70.7    62     1006   01 41 28

01 42 30  SN1986J      20 52 20  25.0  54.0 -5.5     -70.4    -8     1006   01 42 38
01 44 30  ---          20 54 21  25.4  54.1 -5.5     -70.7   112     1020   01 42 38

01 44 50  3C66A        20 54 41  25.7  53.4 -5.5     -71.1    12     1020   01 44 50
01 46 00  ---          20 55 51  25.9  53.5 -5.5     -71.2    70     1029   01 44 50

01 46 00  SN1986J      20 55 51  25.7  54.2 -5.5     -70.9    -8     1029   01 46 08
01 48 00  ---          20 57 51  26.0  54.3 -5.4     -71.2   112     1044   01 46 08

01 48 00  3C66A        20 57 51  26.2  53.6 -5.4     -71.5    -8     1044   01 48 08
01 49 10  ---          20 59 01  26.4  53.7 -5.4     -71.7    62     1052   01 48 08

01 49 10  SN1986J      20 59 01  26.2  54.4 -5.4     -71.4    -8     1052   01 49 18
01 51 10  ---          21 01 02  26.6  54.5 -5.4     -71.6   112     1066   01 49 18

01 51 10  3C66A        21 01 02  26.8  53.8 -5.4     -72.0    -8     1066   01 51 18
01 52 20  ---          21 02 12  27.0  53.9 -5.4     -72.1    62     1074   01 51 18
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

01 52 20  SN1986J      21 02 12  26.8  54.6 -5.4     -71.8    -8     1074   01 52 28
01 54 20  ---          21 04 12  27.1  54.7 -5.3     -72.1   112     1088   01 52 28

01 54 50  3C66A        21 04 42  27.4  54.0 -5.3     -72.5    22     1088   01 54 50
01 56 20  ---          21 06 13  27.7  54.1 -5.3     -72.7    90     1100   01 54 50

01 56 20  SN1986J      21 06 13  27.5  54.9 -5.3     -72.4    -8     1100   01 56 28
01 58 20  ---          21 08 13  27.8  55.0 -5.3     -72.6   112     1114   01 56 28

01 58 20  3C66A        21 08 13  28.0  54.2 -5.3     -73.0    -8     1114   01 58 28
01 59 30  ---          21 09 23  28.2  54.3 -5.2     -73.1    62     1122   01 58 28

01 59 30  SN1986J      21 09 23  28.0  55.1 -5.2     -72.8    -8     1122   01 59 38
02 01 30  ---          21 11 23  28.4  55.2 -5.2     -73.1   112     1137   01 59 38

02 01 30  3C66A        21 11 23  28.6  54.4 -5.2     -73.4    -8     1137   02 01 38
02 02 40  ---          21 12 34  28.8  54.5 -5.2     -73.6    62     1145   02 01 38

02 02 40  SN1986J      21 12 34  28.6  55.3 -5.2     -73.3    -8     1145   02 02 48
02 04 40  ---          21 14 34  28.9  55.4 -5.1     -73.5   112     1159   02 02 48

02 05 00  3C66A        21 14 54  29.2  54.6 -5.1     -73.9    12     1159   02 05 00
02 06 10  ---          21 16 04  29.4  54.7 -5.1     -74.1    70     1168   02 05 00

02 06 10  SN1986J      21 16 04  29.2  55.5 -5.1     -73.7    -8     1168   02 06 18
02 08 10  ---          21 18 05  29.6  55.6 -5.1     -74.0   112     1183   02 06 18

02 08 10  3C66A        21 18 05  29.7  54.8 -5.1     -74.4    -8     1183   02 08 18
02 09 20  ---          21 19 15  29.9  54.9 -5.1     -74.6    62     1191   02 08 18

02 09 20  SN1986J      21 19 15  29.8  55.7 -5.1     -74.2    -8     1191   02 09 28
02 11 20  ---          21 21 15  30.1  55.8 -5.0     -74.5   112     1205   02 09 28

02 11 20  3C66A        21 21 15  30.3  55.0 -5.0     -74.8    -8     1205   02 11 28
02 12 30  ---          21 22 25  30.5  55.1 -5.0     -75.0    62     1213   02 11 28

02 12 30  SN1986J      21 22 25  30.3  55.8 -5.0     -74.6    -8     1213   02 12 38
02 14 30  ---          21 24 26  30.7  56.0 -5.0     -74.9   112     1228   02 12 38

02 15 00  3C66A        21 24 56  30.9  55.2 -5.0     -75.4    22     1228   02 15 00
02 16 30  ---          21 26 26  31.2  55.3 -5.0     -75.6    90     1239   02 15 00

02 16 30  SN1986J      21 26 26  31.1  56.1 -5.0     -75.2    -8     1239   02 16 38
02 18 30  ---          21 28 26  31.4  56.2 -4.9     -75.5   112     1254   02 16 38
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

02 18 30  3C66A        21 28 26  31.6  55.4 -4.9     -75.9    -8     1254   02 18 38
02 19 40  ---          21 29 36  31.8  55.4 -4.9     -76.0    62     1262   02 18 38

02 19 40  SN1986J      21 29 36  31.6  56.2 -4.9     -75.6    -8     1262   02 19 48
02 21 40  ---          21 31 37  32.0  56.4 -4.9     -75.9   112     1276   02 19 48

02 21 40  3C66A        21 31 37  32.1  55.5 -4.9     -76.3    -8     1276   02 21 48
02 22 50  ---          21 32 47  32.3  55.6 -4.8     -76.5    62     1284   02 21 48

02 22 50  SN1986J      21 32 47  32.2  56.4 -4.8     -76.1    -8     1284   02 22 58
02 24 50  ---          21 34 47  32.6  56.5 -4.8     -76.4   112     1298   02 22 58

02 25 10  3C66A        21 35 07  32.7  55.7 -4.8     -76.8    12     1298   02 25 10
02 26 20  ---          21 36 18  33.0  55.8 -4.8     -77.0    70     1307   02 25 10

02 26 20  SN1986J      21 36 18  32.8  56.6 -4.8     -76.6    -8     1307   02 26 28
02 28 20  ---          21 38 18  33.2  56.7 -4.8     -76.9   112     1322   02 26 28

02 28 20  3C66A        21 38 18  33.3  55.9 -4.8     -77.3    -8     1322   02 28 28
02 29 30  ---          21 39 28  33.5  55.9 -4.7     -77.5    62     1330   02 28 28

02 29 30  SN1986J      21 39 28  33.4  56.8 -4.7     -77.0    -8     1330   02 29 38
02 31 30  ---          21 41 28  33.8  56.9 -4.7     -77.3   112     1344   02 29 38

02 31 30  3C66A        21 41 28  33.9  56.0 -4.7     -77.7    -8     1344   02 31 38
02 32 40  ---          21 42 39  34.1  56.1 -4.7     -77.9    62     1352   02 31 38

02 32 40  SN1986J      21 42 39  34.0  56.9 -4.7     -77.5    -8     1352   02 32 48
02 34 40  ---          21 44 39  34.3  57.0 -4.6     -77.8   112     1367   02 32 48

02 35 10  3C66A        21 45 09  34.5  56.2 -4.6     -78.3    22     1367   02 35 10
02 36 40  ---          21 46 39  34.8  56.3 -4.6     -78.5    90     1378   02 35 10

02 36 40  SN1986J      21 46 39  34.7  57.1 -4.6     -78.0    -8     1378   02 36 48
02 38 40  ---          21 48 40  35.1  57.2 -4.6     -78.3   112     1393   02 36 48

02 38 40  3C66A        21 48 40  35.2  56.3 -4.6     -78.8    -8     1393   02 38 48
02 39 50  ---          21 49 50  35.4  56.4 -4.6     -79.0    62     1401   02 38 48

02 39 50  SN1986J      21 49 50  35.3  57.2 -4.6     -78.5    -8     1401   02 39 58
02 41 50  ---          21 51 50  35.6  57.3 -4.5     -78.8   112     1415   02 39 58

02 41 50  3C66A        21 51 50  35.7  56.5 -4.5     -79.3    -8     1415   02 41 58
02 43 00  ---          21 53 00  35.9  56.5 -4.5     -79.4    62     1423   02 41 58
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

02 43 00  SN1986J      21 53 00  35.8  57.4 -4.5     -78.9    -8     1423   02 43 08
02 45 00  ---          21 55 01  36.2  57.5 -4.5     -79.2   112     1437   02 43 08

02 45 20  3C66A        21 55 21  36.4  56.6 -4.5     -79.8    12     1437   02 45 20
02 46 30  ---          21 56 31  36.6  56.7 -4.5     -79.9    70     1447   02 45 20

02 46 30  SN1986J      21 56 31  36.5  57.5 -4.4     -79.4    -8     1447   02 46 38
02 48 30  ---          21 58 31  36.8  57.6 -4.4     -79.7   112     1461   02 46 38

02 48 30  3C66A        21 58 31  36.9  56.7 -4.4     -80.2    -8     1461   02 48 38
02 49 40  ---          21 59 41  37.1  56.8 -4.4     -80.4    62     1469   02 48 38

02 49 40  SN1986J      21 59 41  37.1  57.7 -4.4     -79.9    -8     1469   02 49 48
02 51 40  ---          22 01 42  37.4  57.7 -4.4     -80.2   112     1483   02 49 48

02 51 40  3C66A        22 01 42  37.5  56.9 -4.4     -80.7    -8     1483   02 51 48
02 52 50  ---          22 02 52  37.7  56.9 -4.3     -80.9    62     1491   02 51 48

02 52 50  SN1986J      22 02 52  37.6  57.8 -4.3     -80.4    -8     1491   02 52 58
02 54 50  ---          22 04 52  38.0  57.9 -4.3     -80.7   112     1506   02 52 58

02 55 20  3C66A        22 05 22  38.2  57.0 -4.3     -81.3    22     1506   02 55 20
02 56 50  ---          22 06 53  38.4  57.1 -4.3     -81.5    90     1517   02 55 20

02 56 50  SN1986J      22 06 53  38.4  57.9 -4.3     -80.9    -8     1517   02 56 58
02 58 50  ---          22 08 53  38.7  58.0 -4.2     -81.2   112     1532   02 56 58

02 58 50  3C66A        22 08 53  38.8  57.1 -4.2     -81.8    -8     1532   02 58 58
03 00 00  ---          22 10 03  39.0  57.2 -4.2     -82.0    62     1540   02 58 58

03 00 00  SN1986J      22 10 03  38.9  58.1 -4.2     -81.4    -8     1540   03 00 08
03 02 00  ---          22 12 03  39.3  58.1 -4.2     -81.7   112     1554   03 00 08

03 02 00  3C66A        22 12 03  39.4  57.2 -4.2     -82.3    -8     1554   03 02 08
03 03 10  ---          22 13 14  39.6  57.3 -4.2     -82.4    62     1562   03 02 08

03 03 10  SN1986J      22 13 14  39.5  58.2 -4.2     -81.9    -8     1562   03 03 18
03 05 10  ---          22 15 14  39.9  58.2 -4.1     -82.2   112     1577   03 03 18

03 05 30  3C66A        22 15 34  40.0  57.3 -4.1     -82.8    12     1577   03 05 30
03 06 40  ---          22 16 44  40.2  57.4 -4.1     -83.0    70     1586   03 05 30

03 06 40  SN1986J      22 16 44  40.2  58.3 -4.1     -82.4    -8     1586   03 06 48
03 08 40  ---          22 18 44  40.5  58.4 -4.1     -82.7   112     1600   03 06 48
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

03 08 40  3C66A        22 18 44  40.6  57.4 -4.1     -83.3    -8     1600   03 08 48
03 09 50  ---          22 19 55  40.8  57.5 -4.1     -83.4    62     1608   03 08 48

03 09 50  SN1986J      22 19 55  40.7  58.4 -4.1     -82.9    -8     1608   03 09 58
03 11 50  ---          22 21 55  41.1  58.4 -4.0     -83.2   112     1622   03 09 58

03 11 50  3C66A        22 21 55  41.2  57.5 -4.0     -83.8    -8     1622   03 11 58
03 13 00  ---          22 23 05  41.4  57.5 -4.0     -83.9    62     1630   03 11 58

03 13 00  SN1986J      22 23 05  41.3  58.5 -4.0     -83.3    -8     1630   03 13 08
03 15 00  ---          22 25 06  41.7  58.5 -4.0     -83.6   112     1645   03 13 08

03 15 30  3C66A        22 25 36  41.8  57.6 -4.0     -84.3    22     1645   03 15 30
03 17 00  ---          22 27 06  42.1  57.6 -3.9     -84.6    90     1656   03 15 30

03 17 00  SN1986J      22 27 06  42.1  58.6 -3.9     -83.9    -8     1656   03 17 08
03 19 00  ---          22 29 06  42.4  58.6 -3.9     -84.2   112     1671   03 17 08

03 19 00  3C66A        22 29 06  42.5  57.7 -3.9     -84.9    -8     1671   03 19 08
03 20 10  ---          22 30 16  42.7  57.7 -3.9     -85.0    62     1679   03 19 08

03 20 10  SN1986J      22 30 16  42.6  58.7 -3.9     -84.4    -8     1679   03 20 18
03 22 10  ---          22 32 17  43.0  58.7 -3.9     -84.7   112     1693   03 20 18

03 22 10  3C66A        22 32 17  43.0  57.8 -3.9     -85.4    -8     1693   03 22 18
03 23 20  ---          22 33 27  43.3  57.8 -3.8     -85.5    62     1701   03 22 18

03 23 20  SN1986J      22 33 27  43.2  58.7 -3.8     -84.9    -8     1701   03 23 28
03 25 20  ---          22 35 27  43.6  58.8 -3.8     -85.2   112     1716   03 23 28

03 25 40  3C66A        22 35 47  43.7  57.8 -3.8     -85.9    12     1716   03 25 40
03 26 50  ---          22 36 57  43.9  57.8 -3.8     -86.1    70     1725   03 25 40

03 26 50  SN1986J      22 36 57  43.9  58.8 -3.8     -85.4    -8     1725   03 26 58
03 28 50  ---          22 38 58  44.2  58.9 -3.7     -85.8   112     1739   03 26 58

03 28 50  3C66A        22 38 58  44.3  57.9 -3.7     -86.4    -8     1739   03 28 58
03 30 00  ---          22 40 08  44.5  57.9 -3.7     -86.6    62     1747   03 28 58

03 30 00  SN1986J      22 40 08  44.5  58.9 -3.7     -85.9    -8     1747   03 30 08
03 32 00  ---          22 42 08  44.8  58.9 -3.7     -86.3   112     1762   03 30 08

03 32 00  3C66A        22 42 08  44.8  57.9 -3.7     -86.9    -8     1762   03 32 08
03 33 10  ---          22 43 19  45.1  57.9 -3.7     -87.1    62     1770   03 32 08
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

03 33 10  SN1986J      22 43 19  45.0  58.9 -3.7     -86.4    -8     1770   03 33 18
03 35 10  ---          22 45 19  45.4  59.0 -3.6     -86.8   112     1784   03 33 18

03 35 40  3C66A        22 45 49  45.5  58.0 -3.6     -87.5    22     1784   03 35 40
03 37 10  ---          22 47 19  45.8  58.0 -3.6     -87.8    90     1796   03 35 40

03 37 40  3C84         22 47 49  35.2  58.3 -4.6     -78.0     1     1796   03 37 40
03 40 40  ---          22 50 50  35.8  58.4 -4.5     -78.4   180     1819   03 37 40

03 41 10  3C66A        22 51 20  46.5  58.0 -3.5     -88.4     1     1819   03 41 10
03 42 40  ---          22 52 50  46.8  58.0 -3.5     -88.7    90     1830   03 41 10

03 42 40  SN1986J      22 52 50  46.8  59.1 -3.5     -88.0    -8     1830   03 42 48
03 44 40  ---          22 54 50  47.2  59.1 -3.5     -88.3   112     1845   03 42 48

03 44 40  3C66A        22 54 50  47.2  58.0 -3.5     -89.0    -8     1845   03 44 48
03 45 50  ---          22 56 01  47.4  58.0 -3.5     -89.2    62     1853   03 44 48

03 45 50  SN1986J      22 56 01  47.4  59.1 -3.5     -88.5    -8     1853   03 45 58
03 47 50  ---          22 58 01  47.8  59.1 -3.4     -88.8   112     1867   03 45 58

03 47 50  3C66A        22 58 01  47.7  58.1 -3.4     -89.5    -8     1867   03 47 58
03 49 00  ---          22 59 11  48.0  58.1 -3.4     -89.7    62     1875   03 47 58

03 49 00  SN1986J      22 59 11  48.0  59.1 -3.4     -89.0    -8     1875   03 49 08
03 51 00  ---          23 01 11  48.3  59.1 -3.4     -89.3   112     1890   03 49 08

03 51 20  3C66A        23 01 32  48.4  58.1 -3.4     -90.1    12     1890   03 51 20
03 52 30  ---          23 02 42  48.6  58.1 -3.3     -90.3    70     1899   03 51 20

03 52 30  SN1986J      23 02 42  48.6  59.1 -3.3     -89.6    -8     1899   03 52 38
03 54 30  ---          23 04 42  49.0  59.1 -3.3     -89.9   112     1913   03 52 38

03 54 30  3C66A        23 04 42  49.0  58.0 -3.3     -90.7    -8     1913   03 54 38
03 55 40  ---          23 05 52  49.2  58.0 -3.3     -90.9    62     1921   03 54 38

03 55 40  SN1986J      23 05 52  49.2  59.1 -3.3     -90.1    -8     1921   03 55 48
03 57 40  ---          23 07 53  49.6  59.1 -3.3     -90.4   112     1936   03 55 48

03 57 40  3C66A        23 07 53  49.5  58.0 -3.3     -91.2    -8     1936   03 57 48
03 58 50  ---          23 09 03  49.8  58.0 -3.2     -91.5    62     1943   03 57 48

03 58 50  SN1986J      23 09 03  49.8  59.1 -3.2     -90.6    -8     1943   03 58 58
04 00 50  ---          23 11 03  50.2  59.1 -3.2     -91.0   112     1958   03 58 58
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

04 01 20  3C66A        23 11 33  50.2  58.0 -3.2     -91.9    22     1958   04 01 20
04 02 50  ---          23 13 03  50.5  58.0 -3.2     -92.2    90     1970   04 01 20

04 02 50  SN1986J      23 13 03  50.5  59.1 -3.2     -91.3    -8     1970   04 02 58
04 04 50  ---          23 15 04  50.9  59.1 -3.1     -91.7   112     1984   04 02 58

04 04 50  3C66A        23 15 04  50.8  58.0 -3.1     -92.5    -8     1984   04 04 58
04 06 00  ---          23 16 14  51.1  58.0 -3.1     -92.7    62     1992   04 04 58

04 06 00  SN1986J      23 16 14  51.1  59.1 -3.1     -91.9    -8     1992   04 06 08
04 08 00  ---          23 18 14  51.5  59.0 -3.1     -92.2   112     2006   04 06 08

04 08 00  3C66A        23 18 14  51.4  57.9 -3.1     -93.1    -8     2006   04 08 08
04 09 10  ---          23 19 24  51.6  57.9 -3.1     -93.3    62     2014   04 08 08

04 09 10  SN1986J      23 19 24  51.7  59.0 -3.1     -92.5    -8     2014   04 09 18
04 11 10  ---          23 21 25  52.1  59.0 -3.0     -92.8   112     2029   04 09 18

04 11 30  3C66A        23 21 45  52.1  57.9 -3.0     -93.8    12     2029   04 11 30
04 12 40  ---          23 22 55  52.3  57.8 -3.0     -94.0    70     2038   04 11 30

04 12 40  SN1986J      23 22 55  52.3  59.0 -3.0     -93.1    -8     2038   04 12 48
04 14 40  ---          23 24 55  52.7  58.9 -3.0     -93.5   112     2052   04 12 48

04 14 40  3C66A        23 24 55  52.6  57.8 -3.0     -94.3    -8     2052   04 14 48
04 15 50  ---          23 26 06  52.9  57.8 -3.0     -94.6    62     2060   04 14 48

04 15 50  SN1986J      23 26 06  52.9  58.9 -3.0     -93.7    -8     2060   04 15 58
04 17 50  ---          23 28 06  53.3  58.9 -2.9     -94.0   112     2075   04 15 58

04 17 50  3C66A        23 28 06  53.2  57.7 -2.9     -95.0    -8     2075   04 17 58
04 19 00  ---          23 29 16  53.4  57.7 -2.9     -95.2    62     2083   04 17 58

04 19 00  SN1986J      23 29 16  53.5  58.9 -2.9     -94.3    -9     2083   04 19 09
04 21 00  ---          23 31 16  53.9  58.8 -2.9     -94.6   111     2097   04 19 09

04 21 30  3C66A        23 31 46  53.9  57.6 -2.9     -95.7    21     2097   04 21 30
04 23 00  ---          23 33 17  54.2  57.6 -2.8     -96.0    90     2109   04 21 30

04 23 00  SN1986J      23 33 17  54.3  58.8 -2.8     -95.0    -9     2109   04 23 09
04 25 00  ---          23 35 17  54.6  58.7 -2.8     -95.4   111     2123   04 23 09

04 25 00  3C66A        23 35 17  54.5  57.5 -2.8     -96.4    -9     2123   04 25 09
04 26 10  ---          23 36 27  54.7  57.5 -2.8     -96.6    61     2131   04 25 09
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

04 26 10  SN1986J      23 36 27  54.8  58.7 -2.8     -95.6    -9     2131   04 26 19
04 28 10  ---          23 38 28  55.2  58.6 -2.8     -96.0   111     2145   04 26 19

04 28 10  3C66A        23 38 28  55.1  57.4 -2.8     -97.0    -9     2145   04 28 19
04 29 20  ---          23 39 38  55.3  57.3 -2.7     -97.2    61     2153   04 28 19

04 29 20  SN1986J      23 39 38  55.4  58.6 -2.7     -96.3    -9     2153   04 29 29
04 31 20  ---          23 41 38  55.8  58.5 -2.7     -96.7   111     2167   04 29 29

04 31 40  3C66A        23 41 58  55.7  57.2 -2.7     -97.7    11     2167   04 31 40
04 32 50  ---          23 43 08  56.0  57.2 -2.7     -98.0    70     2176   04 31 40

04 32 50  SN1986J      23 43 08  56.1  58.4 -2.7     -97.0    -9     2176   04 32 59
04 34 50  ---          23 45 09  56.4  58.3 -2.6     -97.4   111     2190   04 32 59

04 34 50  3C66A        23 45 09  56.3  57.1 -2.6     -98.4    -9     2190   04 34 59
04 36 00  ---          23 46 19  56.5  57.0 -2.6     -98.6    61     2198   04 34 59

04 36 00  SN1986J      23 46 19  56.6  58.3 -2.6     -97.6    -9     2198   04 36 09
04 38 00  ---          23 48 19  57.0  58.2 -2.6     -98.0   111     2213   04 36 09

04 38 00  3C66A        23 48 19  56.9  56.9 -2.6     -99.1    -9     2213   04 38 09
04 39 10  ---          23 49 29  57.1  56.9 -2.6     -99.3    61     2220   04 38 09

04 39 10  SN1986J      23 49 29  57.2  58.1 -2.6     -98.3    -9     2220   04 39 19
04 41 10  ---          23 51 30  57.6  58.0 -2.5     -98.7   111     2235   04 39 19

04 41 40  3C66A        23 52 00  57.5  56.7 -2.5     -99.9    21     2235   04 41 40
04 43 10  ---          23 53 30  57.8  56.6 -2.5    -100.2    90     2246   04 41 40

04 43 10  SN1986J      23 53 30  58.0  57.9 -2.5     -99.1    -9     2246   04 43 19
04 45 10  ---          23 55 30  58.3  57.8 -2.5     -99.5   111     2261   04 43 19

04 45 10  3C66A        23 55 30  58.2  56.5 -2.5    -100.6    -9     2261   04 45 19
04 46 20  ---          23 56 41  58.4  56.4 -2.4    -100.9    61     2269   04 45 19

04 46 20  SN1986J      23 56 41  58.5  57.7 -2.4     -99.8    -9     2269   04 46 29
04 48 20  ---          23 58 41  58.9  57.6 -2.4    -100.2   111     2283   04 46 29

04 48 20  3C66A        23 58 41  58.7  56.3 -2.4    -101.4    -9     2283   04 48 29
04 49 30  ---          23 59 51  59.0  56.2 -2.4    -101.6    61     2291   04 48 29

04 49 30  SN1986J      23 59 51  59.1  57.5 -2.4    -100.5    -9     2291   04 49 39
04 51 30  ---          00 01 51  59.5  57.4 -2.4    -101.0   111     2305   04 49 39
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

04 51 50  3C66A        00 02 11  59.4  56.0 -2.4    -102.2    11     2305   04 51 50
04 53 00  ---          00 03 22  59.6  56.0 -2.3    -102.4    70     2314   04 51 50

04 53 00  SN1986J      00 03 22  59.8  57.3 -2.3    -101.3    -9     2314   04 53 09
04 55 00  ---          00 05 22  60.1  57.2 -2.3    -101.8   111     2328   04 53 09

04 55 00  3C66A        00 05 22  59.9  55.8 -2.3    -102.9    -9     2328   04 55 09
04 56 10  ---          00 06 32  60.1  55.7 -2.3    -103.2    61     2336   04 55 09

04 56 10  SN1986J      00 06 32  60.3  57.1 -2.3    -102.0    -9     2336   04 56 19
04 58 10  ---          00 08 32  60.7  56.9 -2.2    -102.5   111     2350   04 56 19

04 58 10  3C66A        00 08 32  60.5  55.5 -2.3    -103.7    -9     2350   04 58 19
04 59 20  ---          00 09 43  60.7  55.4 -2.2    -104.0    61     2358   04 58 19

04 59 20  SN1986J      00 09 43  60.9  56.8 -2.2    -102.8    -9     2358   04 59 29
05 01 20  ---          00 11 43  61.3  56.6 -2.2    -103.3   111     2373   04 59 29

05 01 50  3C66A        00 12 13  61.2  55.2 -2.2    -104.6    21     2373   05 01 50
05 03 20  ---          00 13 43  61.4  55.0 -2.2    -105.0    90     2384   05 01 50

05 03 20  SN1986J      00 13 43  61.6  56.5 -2.2    -103.8    -9     2384   05 03 29
05 05 20  ---          00 15 44  62.0  56.3 -2.1    -104.3   111     2398   05 03 29

05 05 20  3C66A        00 15 44  61.8  54.8 -2.1    -105.5    -9     2398   05 05 29
05 06 30  ---          00 16 54  62.0  54.7 -2.1    -105.8    61     2406   05 05 29

05 06 30  SN1986J      00 16 54  62.2  56.2 -2.1    -104.6    -9     2406   05 06 39
05 08 30  ---          00 18 54  62.5  55.9 -2.1    -105.1   111     2421   05 06 39

05 08 30  3C66A        00 18 54  62.3  54.5 -2.1    -106.4    -9     2421   05 08 39
05 09 40  ---          00 20 04  62.5  54.4 -2.1    -106.7    61     2428   05 08 39

05 09 40  SN1986J      00 20 04  62.8  55.8 -2.1    -105.4    -9     2428   05 09 49
05 11 40  ---          00 22 05  63.1  55.6 -2.0    -106.0   111     2443   05 09 49

05 12 00  3C66A        00 22 25  62.9  54.1 -2.0    -107.3    11     2443   05 12 00
05 13 10  ---          00 23 35  63.1  54.0 -2.0    -107.7    70     2452   05 12 00

05 13 10  SN1986J      00 23 35  63.4  55.4 -2.0    -106.4    -9     2452   05 13 19
05 15 10  ---          00 25 35  63.7  55.2 -2.0    -106.9   111     2466   05 13 19

05 15 10  3C66A        00 25 35  63.5  53.7 -2.0    -108.2    -9     2466   05 15 19
05 16 20  ---          00 26 45  63.7  53.6 -1.9    -108.6    61     2474   05 15 19
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

05 16 20  SN1986J      00 26 45  63.9  55.1 -1.9    -107.2    -9     2474   05 16 29
05 18 20  ---          00 28 46  64.3  54.8 -1.9    -107.8   111     2488   05 16 29

05 18 20  3C66A        00 28 46  64.0  53.3 -1.9    -109.1    -9     2488   05 18 29
05 19 30  ---          00 29 56  64.2  53.1 -1.9    -109.5    61     2496   05 18 29

05 19 30  SN1986J      00 29 56  64.5  54.6 -1.9    -108.1    -9     2496   05 19 39
05 21 30  ---          00 31 56  64.8  54.4 -1.9    -108.7   111     2510   05 19 39

05 22 00  3C66A        00 32 26  64.7  52.8 -1.9    -110.2    21     2510   05 22 00
05 23 30  ---          00 33 57  64.9  52.5 -1.8    -110.7    90     2522   05 22 00

05 23 30  SN1986J      00 33 57  65.2  54.1 -1.8    -109.3    -9     2522   05 23 39
05 25 30  ---          00 35 57  65.5  53.8 -1.8    -109.9   111     2536   05 23 39

05 25 30  3C66A        00 35 57  65.3  52.2 -1.8    -111.3    -9     2536   05 25 39
05 26 40  ---          00 37 07  65.5  52.0 -1.8    -111.7    61     2544   05 25 39

05 26 40  SN1986J      00 37 07  65.8  53.6 -1.8    -110.3    -9     2544   05 26 49
05 28 40  ---          00 39 07  66.1  53.3 -1.7    -110.9   111     2558   05 26 49

05 28 40  3C66A        00 39 07  65.8  51.7 -1.7    -112.4    -9     2558   05 28 49
05 29 50  ---          00 40 18  66.0  51.5 -1.7    -112.7    61     2566   05 28 49

05 29 50  SN1986J      00 40 18  66.3  53.1 -1.7    -111.3    -9     2566   05 29 59
05 31 50  ---          00 42 18  66.6  52.7 -1.7    -112.0   111     2581   05 29 59

05 32 10  3C66A        00 42 38  66.4  51.1 -1.7    -113.5    11     2581   05 32 10
05 33 20  ---          00 43 48  66.6  50.9 -1.7    -113.9    70     2590   05 32 10

05 33 20  SN1986J      00 43 48  66.9  52.5 -1.7    -112.5    -9     2590   05 33 29
05 35 20  ---          00 45 49  67.2  52.1 -1.6    -113.1   111     2604   05 33 29

05 35 20  3C66A        00 45 49  66.9  50.5 -1.6    -114.6    -9     2604   05 35 29
05 36 30  ---          00 46 59  67.1  50.3 -1.6    -115.0    61     2612   05 35 29

05 36 30  SN1986J      00 46 59  67.4  51.9 -1.6    -113.5    -9     2612   05 36 39
05 38 30  ---          00 48 59  67.8  51.5 -1.6    -114.2   111     2626   05 36 39

05 38 30  3C66A        00 48 59  67.5  49.9 -1.6    -115.7    -9     2626   05 38 39
05 39 40  ---          00 50 09  67.6  49.6 -1.6    -116.2    61     2634   05 38 39

05 39 40  SN1986J      00 50 09  68.0  51.3 -1.6    -114.7    -9     2634   05 39 49
05 41 40  ---          00 52 10  68.3  50.8 -1.5    -115.4   111     2648   05 39 49
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

05 42 10  3C66A        00 52 40  68.1  49.1 -1.5    -117.1    21     2648   05 42 10
05 43 40  ---          00 54 10  68.3  48.7 -1.5    -117.7    90     2660   05 42 10

05 44 10  3C84         00 54 40  58.8  59.3 -2.4     -98.6     3     2660   05 44 10
05 47 10  ---          00 57 41  59.4  59.1 -2.4     -99.2   180     2683   05 44 10

05 47 40  3C66A        00 58 11  68.9  47.8 -1.4    -119.2     3     2683   05 47 40
05 48 50  ---          00 59 21  69.1  47.5 -1.4    -119.7    70     2692   05 47 40

05 48 50  SN1986J      00 59 21  69.5  49.2 -1.4    -118.1    -9     2692   05 48 59
05 50 50  ---          01 01 21  69.8  48.7 -1.4    -119.0   111     2706   05 48 59

05 50 50  3C66A        01 01 21  69.4  47.0 -1.4    -120.5    -9     2706   05 50 59
05 52 00  ---          01 02 31  69.6  46.6 -1.4    -121.0    61     2714   05 50 59

05 52 00  SN1986J      01 02 31  70.0  48.4 -1.3    -119.4    -9     2714   05 52 09
05 54 00  ---          01 04 32  70.3  47.8 -1.3    -120.3   111     2729   05 52 09

05 54 00  3C66A        01 04 32  69.9  46.1 -1.3    -121.9    -9     2729   05 54 09
05 55 10  ---          01 05 42  70.1  45.8 -1.3    -122.4    61     2736   05 54 09

05 55 10  SN1986J      01 05 42  70.5  47.5 -1.3    -120.8    -9     2736   05 55 19
05 57 10  ---          01 07 42  70.8  46.9 -1.3    -121.7   111     2751   05 55 19

05 57 30  3C66A        01 08 02  70.5  45.1 -1.3    -123.5    11     2751   05 57 30
05 58 40  ---          01 09 12  70.7  44.7 -1.2    -124.0    70     2760   05 57 30

05 58 40  SN1986J      01 09 12  71.1  46.5 -1.2    -122.4    -9     2760   05 58 49
06 00 40  ---          01 11 13  71.4  45.8 -1.2    -123.3   111     2774   05 58 49

06 00 40  3C66A        01 11 13  71.0  44.1 -1.2    -124.9    -9     2774   06 00 49
06 01 50  ---          01 12 23  71.1  43.7 -1.2    -125.5    61     2782   06 00 49

06 01 50  SN1986J      01 12 23  71.6  45.5 -1.2    -123.8    -9     2782   06 01 59
06 03 50  ---          01 14 23  71.9  44.8 -1.2    -124.8   111     2796   06 01 59

06 03 50  3C66A        01 14 23  71.4  43.0 -1.2    -126.5    -9     2796   06 03 59
06 05 00  ---          01 15 33  71.6  42.6 -1.1    -127.0    61     2804   06 03 59

06 05 00  SN1986J      01 15 33  72.0  44.4 -1.1    -125.4    -9     2804   06 05 09
06 07 00  ---          01 17 34  72.3  43.7 -1.1    -126.4   111     2818   06 05 09

06 07 30  3C66A        01 18 04  72.0  41.7 -1.1    -128.3    21     2818   06 07 30
06 08 40  ---          01 19 14  72.1  41.3 -1.1    -128.9    70     2827   06 07 30
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

06 08 40  SN1986J      01 19 14  72.6  43.1 -1.1    -127.3    -9     2827   06 08 49
06 10 40  ---          01 21 14  72.9  42.3 -1.0    -128.3   111     2842   06 08 49

06 10 40  3C66A        01 21 14  72.4  40.5 -1.0    -130.0    -9     2842   06 10 49
06 11 50  ---          01 22 25  72.6  40.1 -1.0    -130.6    61     2849   06 10 49

06 11 50  SN1986J      01 22 25  73.0  41.8 -1.0    -129.0    -9     2849   06 11 59
06 13 50  ---          01 24 25  73.3  41.0 -1.0    -130.1   111     2864   06 11 59

06 13 50  3C66A        01 24 25  72.9  39.3 -1.0    -131.8    -9     2864   06 13 59
06 15 00  ---          01 25 35  73.0  38.8 -1.0    -132.4    61     2872   06 13 59

06 15 00  SN1986J      01 25 35  73.5  40.5 -1.0    -130.8    -9     2872   06 15 09
06 17 00  ---          01 27 35  73.8  39.7 -0.9    -131.9   111     2886   06 15 09

06 17 20  3C66A        01 27 55  73.3  37.8 -0.9    -133.8    11     2886   06 17 20
06 18 30  ---          01 29 06  73.5  37.2 -0.9    -134.5    70     2895   06 17 20

06 18 30  SN1986J      01 29 06  74.0  39.0 -0.9    -132.8    -9     2895   06 18 39
06 20 30  ---          01 31 06  74.3  38.1 -0.9    -134.1   111     2909   06 18 39

06 20 30  3C66A        01 31 06  73.7  36.3 -0.9    -135.7    -9     2909   06 20 39
06 21 40  ---          01 32 16  73.9  35.8 -0.9    -136.4    61     2917   06 20 39

06 21 40  SN1986J      01 32 16  74.4  37.5 -0.9    -134.8    -9     2917   06 21 49
06 23 40  ---          01 34 17  74.7  36.5 -0.8    -136.1   111     2931   06 21 49

06 23 40  3C66A        01 34 17  74.1  34.8 -0.8    -137.7    -9     2931   06 23 49
06 24 50  ---          01 35 27  74.3  34.2 -0.8    -138.5    61     2939   06 23 49

06 24 50  SN1986J      01 35 27  74.8  35.9 -0.8    -136.9    -9     2939   06 24 59
06 26 50  ---          01 37 27  75.1  34.9 -0.8    -138.2   111     2954   06 24 59

06 27 20  3C66A        01 37 57  74.6  32.9 -0.8    -140.2    21     2954   06 27 20
06 28 30  ---          01 39 07  74.7  32.3 -0.7    -141.0    70     2963   06 27 20

06 28 30  SN1986J      01 39 07  75.3  34.0 -0.7    -139.4    -9     2963   06 28 39
06 30 30  ---          01 41 08  75.5  32.8 -0.7    -140.8   111     2977   06 28 39

06 30 30  3C66A        01 41 08  74.9  31.2 -0.7    -142.4    -9     2977   06 30 39
06 31 40  ---          01 42 18  75.1  30.6 -0.7    -143.2    61     2985   06 30 39

06 31 40  SN1986J      01 42 18  75.6  32.2 -0.7    -141.7    -9     2985   06 31 49
06 33 40  ---          01 44 18  75.9  31.0 -0.7    -143.2   111     2999   06 31 49
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

06 33 40  3C66A        01 44 18  75.3  29.4 -0.7    -144.7    -9     2999   06 33 49
06 34 50  ---          01 45 28  75.4  28.7 -0.6    -145.5    61     3007   06 33 49

06 34 50  SN1986J      01 45 28  76.0  30.3 -0.6    -144.0    -9     3007   06 34 59
06 36 50  ---          01 47 29  76.2  29.0 -0.6    -145.6   111     3021   06 34 59

06 37 10  3C66A        01 47 49  75.6  27.3 -0.6    -147.3    11     3021   06 37 10
06 38 20  ---          01 48 59  75.8  26.6 -0.6    -148.2    70     3030   06 37 10

06 38 20  SN1986J      01 48 59  76.4  28.0 -0.6    -146.8    -9     3030   06 38 29
06 40 20  ---          01 50 59  76.6  26.7 -0.5    -148.4   111     3045   06 38 29

06 40 20  3C66A        01 50 59  75.9  25.3 -0.5    -149.8    -9     3045   06 40 29
06 41 30  ---          01 52 09  76.0  24.5 -0.5    -150.7    61     3052   06 40 29

06 41 30  SN1986J      01 52 09  76.7  25.9 -0.5    -149.4    -9     3052   06 41 39
06 43 30  ---          01 54 10  76.9  24.5 -0.5    -151.1   111     3067   06 41 39

06 43 30  3C66A        01 54 10  76.2  23.2 -0.5    -152.4    -9     3067   06 43 39
06 44 40  ---          01 55 20  76.3  22.4 -0.5    -153.4    61     3075   06 43 39

06 44 40  SN1986J      01 55 20  77.0  23.6 -0.5    -152.1    -9     3075   06 44 49
06 46 40  ---          01 57 20  77.1  22.2 -0.4    -153.9   111     3089   06 44 49

06 47 10  3C66A        01 57 50  76.5  20.6 -0.4    -155.5    21     3089   06 47 10
06 48 20  ---          01 59 01  76.6  19.8 -0.4    -156.5    70     3098   06 47 10

06 48 20  SN1986J      01 59 01  77.3  20.9 -0.4    -155.4    -9     3098   06 48 29
06 50 20  ---          02 01 01  77.4  19.4 -0.4    -157.3   111     3112   06 48 29

06 50 20  3C66A        02 01 01  76.7  18.3 -0.4    -158.3    -9     3112   06 50 29
06 51 30  ---          02 02 11  76.8  17.4 -0.4    -159.3    61     3120   06 50 29

06 51 30  SN1986J      02 02 11  77.5  18.5 -0.4    -158.4    -9     3120   06 51 39
06 53 30  ---          02 04 11  77.6  16.8 -0.3    -160.3   111     3134   06 51 39

06 53 30  3C66A        02 04 11  76.9  15.9 -0.3    -161.2    -9     3134   06 53 39
06 54 40  ---          02 05 22  77.0  15.0 -0.3    -162.2    61     3142   06 53 39

06 54 40  SN1986J      02 05 22  77.7  15.9 -0.3    -161.4    -9     3142   06 54 49
06 56 40  ---          02 07 22  77.8  14.2 -0.3    -163.4   111     3156   06 54 49

06 57 00  3C66A        02 07 42  77.1  13.2 -0.3    -164.4    11     3156   06 57 00
06 58 10  ---          02 08 52  77.2  12.2 -0.2    -165.5    70     3165   06 57 00
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

06 58 10  SN1986J      02 08 52  77.9  13.0 -0.2    -164.9    -9     3165   06 58 19
07 00 10  ---          02 10 53  78.0  11.2 -0.2    -166.9   111     3180   06 58 19

07 00 10  3C66A        02 10 53  77.3  10.6 -0.2    -167.4    -9     3180   07 00 19
07 01 20  ---          02 12 03  77.3   9.7 -0.2    -168.6    61     3188   07 00 19

07 01 20  SN1986J      02 12 03  78.0  10.2 -0.2    -168.1    -9     3188   07 01 29
07 03 20  ---          02 14 03  78.1   8.5 -0.2    -170.1   111     3202   07 01 29

07 03 20  3C66A        02 14 03  77.4   8.0 -0.2    -170.5    -9     3202   07 03 29
07 04 30  ---          02 15 13  77.4   7.1 -0.1    -171.7    61     3210   07 03 29

07 04 30  SN1986J      02 15 13  78.1   7.4 -0.1    -171.3    -9     3210   07 04 39
07 06 30  ---          02 17 14  78.2   5.7 -0.1    -173.4   111     3224   07 04 39

07 07 00  3C66A        02 17 44  77.5   5.0 -0.1    -174.1    21     3224   07 07 00
07 08 10  ---          02 18 54  77.5   4.0 -0.1    -175.3    70     3233   07 07 00

07 08 10  SN1986J      02 18 54  78.2   4.2 -0.1    -175.2    -9     3233   07 08 19
07 10 10  ---          02 20 54  78.2   2.3  0.0    -177.3   111     3247   07 08 19

07 10 10  3C66A        02 20 54  77.5   2.3  0.0    -177.3    -9     3247   07 10 19
07 11 20  ---          02 22 04  77.5   1.3  0.0    -178.4    61     3255   07 10 19

07 11 20  SN1986J      02 22 04  78.2   1.3  0.0    -178.5    -9     3255   07 11 29
07 13 20  ---          02 24 05  78.2  -0.5  0.0     179.4   111     3270   07 11 29

07 13 20  3C66A        02 24 05  77.5  -0.4  0.0     179.6    -9     3270   07 13 29
07 14 30  ---          02 25 15  77.5  -1.4  0.0     178.4    61     3277   07 13 29

07 14 30  SN1986J      02 25 15  78.2  -1.6  0.0     178.2    -9     3277   07 14 39
07 16 30  ---          02 27 15  78.2  -3.4  0.1     176.0   111     3292   07 14 39

07 16 50  3C66A        02 27 35  77.5  -3.3  0.1     176.1    11     3292   07 16 50
07 18 00  ---          02 28 45  77.5  -4.3  0.1     174.9    70     3301   07 16 50

07 18 00  SN1986J      02 28 45  78.2  -4.7  0.1     174.5    -9     3301   07 18 09
07 20 00  ---          02 30 46  78.1  -6.5  0.1     172.4   111     3315   07 18 09

07 20 00  3C66A        02 30 46  77.5  -6.0  0.1     172.9    -9     3315   07 20 09
07 21 10  ---          02 31 56  77.4  -7.0  0.1     171.8    61     3323   07 20 09

07 21 10  SN1986J      02 31 56  78.1  -7.6  0.1     171.2    -9     3323   07 21 19
07 23 10  ---          02 33 56  78.1  -9.3  0.2     169.1   111     3337   07 21 19
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

07 23 10  3C66A        02 33 56  77.4  -8.6  0.2     169.8    -9     3337   07 23 19
07 24 20  ---          02 35 06  77.3  -9.6  0.2     168.7    61     3345   07 23 19

07 24 20  SN1986J      02 35 06  78.0 -10.4  0.2     167.9    -9     3345   07 24 29
07 26 20  ---          02 37 07  77.9 -12.1  0.2     165.9   111     3359   07 24 29

07 26 50  3C66A        02 37 37  77.2 -11.6  0.2     166.3    21     3359   07 26 50
07 28 00  ---          02 38 47  77.2 -12.5  0.3     165.2    70     3368   07 26 50

07 28 00  SN1986J      02 38 47  77.8 -13.5  0.3     164.2    -9     3368   07 28 09
07 30 00  ---          02 40 47  77.7 -15.2  0.3     162.2   111     3383   07 28 09

07 30 00  3C66A        02 40 47  77.1 -14.1  0.3     163.3    -9     3383   07 30 09
07 31 10  ---          02 41 58  77.0 -15.0  0.3     162.2    61     3391   07 30 09

07 31 10  SN1986J      02 41 58  77.7 -16.2  0.3     161.1    -9     3391   07 31 19
07 33 10  ---          02 43 58  77.5 -17.8  0.3     159.2   111     3405   07 31 19

07 33 10  3C66A        02 43 58  76.9 -16.6  0.3     160.4    -9     3405   07 33 19
07 34 20  ---          02 45 08  76.8 -17.5  0.4     159.3    61     3413   07 33 19

07 34 20  SN1986J      02 45 08  77.5 -18.7  0.4     158.1    -9     3413   07 34 29
07 36 20  ---          02 47 08  77.3 -20.3  0.4     156.2   111     3427   07 34 29

07 36 40  3C66A        02 47 29  76.7 -19.2  0.4     157.2    11     3427   07 36 40
07 37 50  ---          02 48 39  76.6 -20.0  0.4     156.2    70     3436   07 36 40

07 37 50  SN1986J      02 48 39  77.2 -21.4  0.4     154.8    -9     3436   07 37 59
07 39 50  ---          02 50 39  77.0 -22.9  0.5     153.0   111     3450   07 37 59

07 39 50  3C66A        02 50 39  76.4 -21.5  0.5     154.5    -9     3450   07 39 59
07 41 00  ---          02 51 49  76.3 -22.3  0.5     153.5    61     3458   07 39 59

07 41 00  SN1986J      02 51 49  76.9 -23.8  0.5     152.0    -9     3458   07 41 09
07 43 00  ---          02 53 50  76.8 -25.2  0.5     150.3   111     3472   07 41 09

07 43 00  3C66A        02 53 50  76.2 -23.6  0.5     151.8    -9     3472   07 43 09
07 44 10  ---          02 55 00  76.1 -24.4  0.5     150.8    61     3480   07 43 09

07 44 10  SN1986J      02 55 00  76.7 -26.0  0.5     149.3    -9     3480   07 44 19
07 46 10  ---          02 57 00  76.5 -27.4  0.6     147.6   111     3495   07 44 19

07 46 40  3C66A        02 57 30  75.8 -26.0  0.6     148.8    21     3495   07 46 40
07 48 10  ---          02 59 00  75.7 -27.0  0.6     147.7    90     3506   07 46 40
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

07 48 40  3C84         02 59 30  78.3  20.0 -0.4    -156.9   -11     3506   07 48 51
07 51 40  ---          03 02 31  78.5  17.4 -0.3    -159.9   169     3528   07 48 51

07 52 10  3C66A        03 03 01  75.3 -29.4  0.7     144.6   -11     3528   07 52 21
07 52 40  ---          03 03 31  75.2 -29.7  0.7     144.3    19     3530   07 52 21

07 53 10  3C66A        03 04 01  75.2 -30.0  0.7     143.9    24     3530   07 53 10
07 54 40  ---          03 05 31  75.0 -30.9  0.7     142.8    90     3542   07 53 10

07 54 40  SN1986J      03 05 31  75.5 -32.6  0.7     141.1    -9     3542   07 54 49
07 56 40  ---          03 07 32  75.3 -33.8  0.7     139.6   111     3556   07 54 49

07 56 40  3C66A        03 07 32  74.8 -32.0  0.7     141.4    -9     3556   07 56 49
07 57 50  ---          03 08 42  74.6 -32.6  0.8     140.6    61     3564   07 56 49

07 57 50  SN1986J      03 08 42  75.2 -34.4  0.8     138.8    -9     3564   07 57 59
07 59 50  ---          03 10 42  74.9 -35.5  0.8     137.4   111     3578   07 57 59

07 59 50  3C66A        03 10 42  74.4 -33.6  0.8     139.2    -9     3578   07 59 59
08 01 00  ---          03 11 53  74.3 -34.2  0.8     138.5    61     3586   07 59 59

08 01 00  SN1986J      03 11 53  74.8 -36.1  0.8     136.7    -9     3586   08 01 09
08 03 00  ---          03 13 53  74.5 -37.1  0.8     135.3   111     3601   08 01 09

08 03 20  3C66A        03 14 13  74.0 -35.4  0.8     137.0    11     3601   08 03 20
08 04 30  ---          03 15 23  73.8 -36.0  0.9     136.2    70     3610   08 03 20

08 04 30  SN1986J      03 15 23  74.3 -37.8  0.9     134.4    -9     3610   08 04 39
08 06 30  ---          03 17 23  74.1 -38.8  0.9     133.1   111     3624   08 04 39

08 06 30  3C66A        03 17 23  73.6 -36.9  0.9     135.0    -9     3624   08 06 39
08 07 40  ---          03 18 34  73.4 -37.4  0.9     134.3    61     3632   08 06 39

08 07 40  SN1986J      03 18 34  73.9 -39.3  0.9     132.4    -9     3632   08 07 49
08 09 40  ---          03 20 34  73.6 -40.2  1.0     131.3   111     3646   08 07 49

08 09 40  3C66A        03 20 34  73.2 -38.3  0.9     133.1    -9     3646   08 09 49
08 10 50  ---          03 21 44  73.0 -38.8  1.0     132.4    61     3654   08 09 49

08 10 50  SN1986J      03 21 44  73.5 -40.7  1.0     130.6    -9     3654   08 10 59
08 12 50  ---          03 23 44  73.2 -41.5  1.0     129.4   111     3668   08 10 59

08 13 20  3C66A        03 24 15  72.7 -39.8  1.0     131.0    21     3668   08 13 20
08 14 50  ---          03 25 45  72.5 -40.4  1.0     130.2    90     3680   08 13 20
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

08 14 50  SN1986J      03 25 45  72.9 -42.3  1.0     128.3    -9     3680   08 14 59
08 16 50  ---          03 27 45  72.6 -43.1  1.1     127.3   111     3694   08 14 59

08 16 50  3C66A        03 27 45  72.2 -41.2  1.1     129.1    -9     3694   08 16 59
08 18 00  ---          03 28 55  72.0 -41.6  1.1     128.5    61     3702   08 16 59

08 18 00  SN1986J      03 28 55  72.4 -43.5  1.1     126.7    -9     3702   08 18 09
08 20 00  ---          03 30 56  72.1 -44.2  1.1     125.6   111     3716   08 18 09

08 20 00  3C66A        03 30 56  71.7 -42.3  1.1     127.5    -9     3716   08 20 09
08 21 10  ---          03 32 06  71.6 -42.8  1.1     126.9    61     3724   08 20 09

08 21 10  SN1986J      03 32 06  71.9 -44.6  1.1     125.1    -9     3724   08 21 19
08 23 10  ---          03 34 06  71.6 -45.3  1.2     124.1   111     3738   08 21 19

08 23 30  3C66A        03 34 26  71.2 -43.6  1.2     125.7    11     3738   08 23 30
08 24 40  ---          03 35 36  71.0 -43.9  1.2     125.2    70     3747   08 23 30

08 24 40  SN1986J      03 35 36  71.4 -45.8  1.2     123.4    -9     3747   08 24 49
08 26 40  ---          03 37 37  71.1 -46.4  1.2     122.4   111     3762   08 24 49

08 26 40  3C66A        03 37 37  70.7 -44.6  1.2     124.2    -9     3762   08 26 49
08 27 50  ---          03 38 47  70.6 -44.9  1.3     123.7    61     3770   08 26 49

08 27 50  SN1986J      03 38 47  70.9 -46.8  1.3     121.9    -9     3770   08 27 59
08 29 50  ---          03 40 47  70.6 -47.3  1.3     121.0   111     3784   08 27 59

08 29 50  3C66A        03 40 47  70.2 -45.5  1.3     122.8    -9     3784   08 29 59
08 31 00  ---          03 41 57  70.1 -45.9  1.3     122.2    61     3792   08 29 59

08 31 00  SN1986J      03 41 57  70.4 -47.7  1.3     120.5    -9     3792   08 31 09
08 33 00  ---          03 43 58  70.1 -48.2  1.3     119.7   111     3806   08 31 09

08 33 30  3C66A        03 44 28  69.7 -46.6  1.3     121.2    21     3806   08 33 30
08 35 00  ---          03 45 58  69.4 -47.0  1.4     120.5    90     3818   08 33 30

08 35 00  SN1986J      03 45 58  69.8 -48.8  1.4     118.8    -9     3818   08 35 09
08 37 00  ---          03 47 58  69.4 -49.3  1.4     118.0   111     3832   08 35 09

08 37 00  3C66A        03 47 58  69.1 -47.5  1.4     119.7    -9     3832   08 37 09
08 38 10  ---          03 49 09  68.9 -47.8  1.4     119.2    61     3840   08 37 09

08 38 10  SN1986J      03 49 09  69.3 -49.5  1.4     117.5    -9     3840   08 38 19
08 40 10  ---          03 51 09  68.9 -50.0  1.5     116.8   111     3854   08 38 19
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

08 40 10  3C66A        03 51 09  68.6 -48.3  1.5     118.4    -9     3854   08 40 19
08 41 20  ---          03 52 19  68.4 -48.5  1.5     118.0    61     3862   08 40 19

08 41 20  SN1986J      03 52 19  68.7 -50.3  1.5     116.3    -9     3862   08 41 29
08 43 20  ---          03 54 19  68.4 -50.7  1.5     115.6   111     3876   08 41 29

08 43 40  3C66A        03 54 40  68.1 -49.1  1.5     117.1    11     3876   08 43 40
08 44 50  ---          03 55 50  67.9 -49.3  1.5     116.6    70     3885   08 43 40

08 44 50  SN1986J      03 55 50  68.1 -51.1  1.5     115.0    -9     3885   08 44 59
08 46 50  ---          03 57 50  67.8 -51.5  1.6     114.3   111     3900   08 44 59

08 46 50  3C66A        03 57 50  67.5 -49.8  1.6     115.9    -9     3900   08 46 59
08 48 00  ---          03 59 00  67.3 -50.0  1.6     115.5    61     3907   08 46 59

08 48 00  SN1986J      03 59 00  67.6 -51.7  1.6     113.9    -9     3907   08 48 09
08 50 00  ---          04 01 01  67.3 -52.1  1.6     113.2   111     3922   08 48 09

08 50 00  3C66A        04 01 01  67.0 -50.4  1.6     114.8    -9     3922   08 50 09
08 51 10  ---          04 02 11  66.8 -50.6  1.6     114.4    61     3930   08 50 09

08 51 10  SN1986J      04 02 11  67.1 -52.3  1.6     112.8    -9     3930   08 51 19
08 53 10  ---          04 04 11  66.7 -52.7  1.7     112.1   111     3944   08 51 19

08 53 40  3C66A        04 04 41  66.4 -51.1  1.7     113.5    21     3944   08 53 40
08 55 10  ---          04 06 11  66.1 -51.4  1.7     113.0    90     3956   08 53 40

08 55 10  SN1986J      04 06 11  66.4 -53.0  1.7     111.5    -9     3956   08 55 19
08 57 10  ---          04 08 12  66.0 -53.3  1.7     110.8   111     3970   08 55 19

08 57 10  3C66A        04 08 12  65.8 -51.7  1.7     112.3    -9     3970   08 57 19
08 58 20  ---          04 09 22  65.6 -51.9  1.8     112.0    61     3978   08 57 19

08 58 20  SN1986J      04 09 22  65.8 -53.5  1.8     110.5    -9     3978   08 58 29
09 00 20  ---          04 11 22  65.5 -53.8  1.8     109.8   111     3992   08 58 29

09 00 20  3C66A        04 11 22  65.3 -52.2  1.8     111.3    -9     3992   09 00 29
09 01 30  ---          04 12 32  65.1 -52.4  1.8     111.0    61     4000   09 00 29

09 01 30  SN1986J      04 12 32  65.3 -54.0  1.8     109.5    -9     4000   09 01 39
09 03 30  ---          04 14 33  64.9 -54.3  1.9     108.9   111     4014   09 01 39

09 03 50  3C66A        04 14 53  64.7 -52.8  1.9     110.2    11     4014   09 03 50
09 05 00  ---          04 16 03  64.5 -52.9  1.9     109.9    70     4023   09 03 50
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

09 05 00  SN1986J      04 16 03  64.7 -54.5  1.9     108.4    -9     4023   09 05 09
09 07 00  ---          04 18 03  64.3 -54.8  1.9     107.9   111     4037   09 05 09

09 07 00  3C66A        04 18 03  64.1 -53.2  1.9     109.3    -9     4037   09 07 09
09 08 10  ---          04 19 14  63.9 -53.4  1.9     108.9    61     4045   09 07 09

09 08 10  SN1986J      04 19 14  64.1 -54.9  1.9     107.5    -9     4045   09 08 19
09 10 10  ---          04 21 14  63.8 -55.2  2.0     107.0   111     4060   09 08 19

09 10 10  3C66A        04 21 14  63.6 -53.6  2.0     108.4    -9     4060   09 10 19
09 11 20  ---          04 22 24  63.4 -53.8  2.0     108.0    61     4067   09 10 19

09 11 20  SN1986J      04 22 24  63.6 -55.3  2.0     106.6    -9     4067   09 11 29
09 13 20  ---          04 24 24  63.2 -55.5  2.0     106.1   111     4082   09 11 29

09 13 50  3C66A        04 24 54  62.9 -54.1  2.0     107.3    21     4082   09 13 50
09 15 20  ---          04 26 25  62.7 -54.3  2.0     106.9    90     4093   09 13 50

09 15 20  SN1986J      04 26 25  62.8 -55.8  2.0     105.6    -9     4093   09 15 29
09 17 20  ---          04 28 25  62.5 -56.0  2.1     105.0   111     4108   09 15 29

09 17 20  3C66A        04 28 25  62.3 -54.5  2.1     106.4    -9     4108   09 17 29
09 18 30  ---          04 29 35  62.1 -54.6  2.1     106.1    61     4116   09 17 29

09 18 30  SN1986J      04 29 35  62.3 -56.1  2.1     104.7    -9     4116   09 18 39
09 20 30  ---          04 31 36  61.9 -56.3  2.1     104.2   111     4130   09 18 39

09 20 30  3C66A        04 31 36  61.8 -54.8  2.1     105.5    -9     4130   09 20 39
09 21 40  ---          04 32 46  61.6 -55.0  2.2     105.2    61     4138   09 20 39

09 21 40  SN1986J      04 32 46  61.7 -56.4  2.2     103.9    -9     4138   09 21 49
09 23 40  ---          04 34 46  61.4 -56.6  2.2     103.4   111     4152   09 21 49

09 24 00  3C66A        04 35 06  61.1 -55.2  2.2     104.6    11     4152   09 24 00
09 25 10  ---          04 36 16  60.9 -55.3  2.2     104.3    70     4161   09 24 00

09 25 10  SN1986J      04 36 16  61.1 -56.7  2.2     103.1    -9     4161   09 25 19
09 27 10  ---          04 38 17  60.7 -56.9  2.2     102.6   111     4175   09 25 19

09 27 10  3C66A        04 38 17  60.6 -55.5  2.2     103.8    -9     4175   09 27 19
09 28 20  ---          04 39 27  60.4 -55.6  2.3     103.5    61     4183   09 27 19

09 28 20  SN1986J      04 39 27  60.5 -57.0  2.3     102.3    -9     4183   09 28 29
09 30 20  ---          04 41 27  60.1 -57.1  2.3     101.8   111     4197   09 28 29
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

09 30 20  3C66A        04 41 27  60.0 -55.8  2.3     103.0    -9     4197   09 30 29
09 31 30  ---          04 42 37  59.8 -55.9  2.3     102.8    61     4205   09 30 29

09 31 30  SN1986J      04 42 37  59.9 -57.2  2.3     101.5    -9     4205   09 31 39
09 33 30  ---          04 44 38  59.6 -57.4  2.4     101.1   111     4220   09 31 39

09 34 00  3C66A        04 45 08  59.4 -56.0  2.4     102.2    21     4220   09 34 00
09 35 30  ---          04 46 38  59.1 -56.2  2.4     101.8    90     4231   09 34 00

09 35 30  SN1986J      04 46 38  59.2 -57.5  2.4     100.6    -9     4231   09 35 39
09 37 30  ---          04 48 38  58.8 -57.6  2.4     100.2   111     4245   09 35 39

09 37 30  3C66A        04 48 38  58.7 -56.3  2.4     101.3    -9     4245   09 37 39
09 38 40  ---          04 49 49  58.5 -56.4  2.4     101.1    61     4253   09 37 39

09 38 40  SN1986J      04 49 49  58.6 -57.7  2.4      99.9    -9     4253   09 38 49
09 40 40  ---          04 51 49  58.3 -57.8  2.5      99.5   111     4268   09 38 49

09 40 40  3C66A        04 51 49  58.2 -56.5  2.5     100.6    -9     4268   09 40 49
09 41 50  ---          04 52 59  58.0 -56.6  2.5     100.4    61     4275   09 40 49

09 41 50  SN1986J      04 52 59  58.1 -57.9  2.5      99.2    -9     4275   09 41 59
09 43 50  ---          04 54 59  57.7 -58.0  2.5      98.8   111     4290   09 41 59

09 44 10  3C66A        04 55 19  57.5 -56.7  2.5      99.8    11     4290   09 44 10
09 45 20  ---          04 56 30  57.3 -56.8  2.5      99.6    70     4299   09 44 10

09 45 20  SN1986J      04 56 30  57.4 -58.1  2.5      98.5    -9     4299   09 45 29
09 47 20  ---          04 58 30  57.0 -58.2  2.6      98.1   111     4313   09 45 29

09 47 20  3C66A        04 58 30  57.0 -56.9  2.6      99.2    -9     4313   09 47 29
09 48 30  ---          04 59 40  56.8 -57.0  2.6      98.9    61     4321   09 47 29

09 48 30  SN1986J      04 59 40  56.8 -58.2  2.6      97.8    -9     4321   09 48 39
09 50 30  ---          05 01 41  56.5 -58.3  2.6      97.4   111     4335   09 48 39

09 50 30  3C66A        05 01 41  56.4 -57.1  2.6      98.5    -9     4335   09 50 39
09 51 40  ---          05 02 51  56.2 -57.1  2.7      98.2    61     4343   09 50 39

09 51 40  SN1986J      05 02 51  56.3 -58.4  2.7      97.2    -9     4343   09 51 49
09 53 40  ---          05 04 51  55.9 -58.5  2.7      96.8   111     4357   09 51 49

09 54 10  3C66A        05 05 21  55.7 -57.2  2.7      97.7    21     4357   09 54 10
09 56 10  ---          05 07 21  55.4 -57.3  2.7      97.3   120     4373   09 54 10
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

09 56 40  3C84         05 07 52  65.9 -55.6  1.8     108.3     1     4373   09 56 40
10 00 00  ---          05 11 12  65.3 -56.1  1.8     107.4   200     4399   09 56 40

10 00 30  3C66A        05 11 42  54.6 -57.5  2.8      96.4     1     4399   10 00 30
10 02 00  ---          05 13 12  54.3 -57.5  2.8      96.1    90     4410   10 00 30

10 02 00  SN1986J      05 13 12  54.4 -58.7  2.8      95.1    -9     4410   10 02 09
10 04 00  ---          05 15 13  54.0 -58.8  2.9      94.7   111     4425   10 02 09

10 04 00  3C66A        05 15 13  53.9 -57.6  2.9      95.7    -9     4425   10 04 09
10 05 10  ---          05 16 23  53.7 -57.6  2.9      95.5    61     4432   10 04 09

10 05 10  SN1986J      05 16 23  53.8 -58.8  2.9      94.5    -9     4432   10 05 19
10 07 10  ---          05 18 23  53.4 -58.9  2.9      94.1   111     4447   10 05 19

10 07 10  3C66A        05 18 23  53.4 -57.7  2.9      95.1    -9     4447   10 07 19
10 08 20  ---          05 19 33  53.2 -57.7  2.9      94.9    61     4455   10 07 19

10 08 20  SN1986J      05 19 33  53.2 -58.9  2.9      93.9    -9     4455   10 08 29
10 10 20  ---          05 21 34  52.8 -58.9  3.0      93.5   111     4469   10 08 29

10 10 40  3C66A        05 21 54  52.7 -57.8  3.0      94.4    12     4469   10 10 40
10 11 50  ---          05 23 04  52.5 -57.8  3.0      94.2    70     4478   10 10 40

10 11 50  SN1986J      05 23 04  52.5 -59.0  3.0      93.3    -8     4478   10 11 58
10 13 50  ---          05 25 04  52.2 -59.0  3.0      92.9   112     4492   10 11 58

10 13 50  3C66A        05 25 04  52.2 -57.9  3.0      93.8    -8     4492   10 13 58
10 15 00  ---          05 26 15  51.9 -57.9  3.0      93.6    62     4500   10 13 58

10 15 00  SN1986J      05 26 15  52.0 -59.0  3.0      92.7    -8     4500   10 15 08
10 17 00  ---          05 28 15  51.6 -59.0  3.1      92.3   112     4515   10 15 08

10 17 00  3C66A        05 28 15  51.6 -57.9  3.1      93.3    -8     4515   10 17 08
10 18 10  ---          05 29 25  51.4 -57.9  3.1      93.0    62     4523   10 17 08

10 18 10  SN1986J      05 29 25  51.4 -59.1  3.1      92.1    -8     4523   10 18 18
10 20 10  ---          05 31 25  51.0 -59.1  3.1      91.8   112     4537   10 18 18

10 20 40  3C66A        05 31 55  50.9 -58.0  3.1      92.6    22     4537   10 20 40
10 22 10  ---          05 33 26  50.6 -58.0  3.2      92.3    90     4549   10 20 40

10 22 10  SN1986J      05 33 26  50.6 -59.1  3.2      91.4    -8     4549   10 22 18
10 24 10  ---          05 35 26  50.3 -59.1  3.2      91.1   112     4563   10 22 18
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

10 24 10  3C66A        05 35 26  50.3 -58.0  3.2      91.9    -8     4563   10 24 18
10 25 20  ---          05 36 36  50.0 -58.0  3.2      91.7    62     4571   10 24 18

10 25 20  SN1986J      05 36 36  50.0 -59.1  3.2      90.9    -8     4571   10 25 28
10 27 20  ---          05 38 37  49.7 -59.1  3.3      90.5   112     4586   10 25 28

10 27 20  3C66A        05 38 37  49.7 -58.0  3.2      91.4    -8     4586   10 27 28
10 28 30  ---          05 39 47  49.5 -58.0  3.3      91.2    62     4594   10 27 28

10 28 30  SN1986J      05 39 47  49.5 -59.1  3.3      90.3    -8     4594   10 28 38
10 30 30  ---          05 41 47  49.1 -59.1  3.3      90.0   112     4608   10 28 38

10 30 50  3C66A        05 42 07  49.0 -58.0  3.3      90.8    12     4608   10 30 50
10 32 00  ---          05 43 17  48.8 -58.1  3.3      90.6    70     4617   10 30 50

10 32 00  SN1986J      05 43 17  48.8 -59.1  3.3      89.7    -8     4617   10 32 08
10 34 00  ---          05 45 18  48.4 -59.1  3.4      89.4   112     4631   10 32 08

10 34 00  3C66A        05 45 18  48.5 -58.1  3.4      90.2    -8     4631   10 34 08
10 35 10  ---          05 46 28  48.2 -58.1  3.4      90.0    62     4639   10 34 08

10 35 10  SN1986J      05 46 28  48.2 -59.1  3.4      89.2    -8     4639   10 35 18
10 37 10  ---          05 48 28  47.8 -59.1  3.4      88.9   112     4654   10 35 18

10 37 10  3C66A        05 48 28  47.9 -58.1  3.4      89.7    -8     4654   10 37 18
10 38 20  ---          05 49 38  47.7 -58.1  3.4      89.5    62     4662   10 37 18

10 38 20  SN1986J      05 49 38  47.6 -59.1  3.4      88.7    -8     4662   10 38 28
10 40 20  ---          05 51 39  47.3 -59.1  3.5      88.4   112     4676   10 38 28

10 40 50  3C66A        05 52 09  47.2 -58.0  3.5      89.1    22     4676   10 40 50
10 42 20  ---          05 53 39  46.9 -58.0  3.5      88.8    90     4688   10 40 50

10 42 20  SN1986J      05 53 39  46.9 -59.1  3.5      88.0    -8     4688   10 42 28
10 44 20  ---          05 55 39  46.5 -59.0  3.5      87.7   112     4702   10 42 28

10 44 20  3C66A        05 55 39  46.6 -58.0  3.5      88.5    -8     4702   10 44 28
10 45 30  ---          05 56 50  46.4 -58.0  3.6      88.3    62     4710   10 44 28

10 45 30  SN1986J      05 56 50  46.3 -59.0  3.6      87.5    -8     4710   10 45 38
10 47 30  ---          05 58 50  45.9 -59.0  3.6      87.2   112     4725   10 45 38

10 47 30  3C66A        05 58 50  46.0 -58.0  3.6      88.0    -8     4725   10 47 38
10 48 40  ---          06 00 00  45.8 -58.0  3.6      87.8    62     4733   10 47 38
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

10 48 40  SN1986J      06 00 00  45.7 -59.0  3.6      87.0    -8     4733   10 48 48
10 50 40  ---          06 02 00  45.4 -59.0  3.6      86.7   112     4747   10 48 48

10 51 00  3C66A        06 02 20  45.4 -58.0  3.6      87.4    12     4747   10 51 00
10 52 10  ---          06 03 31  45.1 -57.9  3.7      87.2    70     4756   10 51 00

10 52 10  SN1986J      06 03 31  45.1 -58.9  3.7      86.5    -8     4756   10 52 18
10 54 10  ---          06 05 31  44.7 -58.9  3.7      86.2   112     4771   10 52 18

10 54 10  3C66A        06 05 31  44.8 -57.9  3.7      86.9    -8     4771   10 54 18
10 55 20  ---          06 06 41  44.6 -57.9  3.7      86.7    62     4779   10 54 18

10 55 20  SN1986J      06 06 41  44.5 -58.9  3.7      86.0    -8     4779   10 55 28
10 57 20  ---          06 08 41  44.1 -58.8  3.8      85.7   112     4793   10 55 28

10 57 20  3C66A        06 08 41  44.2 -57.9  3.8      86.4    -8     4793   10 57 28
10 58 30  ---          06 09 52  44.0 -57.9  3.8      86.2    62     4801   10 57 28

10 58 30  SN1986J      06 09 52  43.9 -58.8  3.8      85.5    -8     4801   10 58 38
11 00 30  ---          06 11 52  43.5 -58.8  3.8      85.2   112     4815   10 58 38

11 01 00  3C66A        06 12 22  43.5 -57.8  3.8      85.8    22     4815   11 01 00
11 02 30  ---          06 13 52  43.3 -57.8  3.8      85.5    90     4827   11 01 00

11 02 30  SN1986J      06 13 52  43.2 -58.7  3.8      84.9    -8     4827   11 02 38
11 04 30  ---          06 15 53  42.8 -58.7  3.9      84.6   112     4841   11 02 38

11 04 30  3C66A        06 15 53  42.9 -57.7  3.9      85.2    -8     4841   11 04 38
11 05 40  ---          06 17 03  42.7 -57.7  3.9      85.0    62     4849   11 04 38

11 05 40  SN1986J      06 17 03  42.6 -58.7  3.9      84.4    -8     4849   11 05 48
11 07 40  ---          06 19 03  42.2 -58.6  3.9      84.1   112     4864   11 05 48

11 07 40  3C66A        06 19 03  42.3 -57.7  3.9      84.7    -8     4864   11 07 48
11 08 50  ---          06 20 13  42.1 -57.6  3.9      84.5    62     4872   11 07 48

11 08 50  SN1986J      06 20 13  42.0 -58.6  3.9      83.9    -8     4872   11 08 58
11 10 50  ---          06 22 14  41.6 -58.5  4.0      83.6   112     4886   11 08 58

11 11 10  3C66A        06 22 34  41.7 -57.6  4.0      84.2    12     4886   11 11 10
11 12 20  ---          06 23 44  41.5 -57.6  4.0      84.0    70     4895   11 11 10

11 12 20  SN1986J      06 23 44  41.4 -58.5  4.0      83.4    -8     4895   11 12 28
11 14 20  ---          06 25 44  41.0 -58.4  4.0      83.1   112     4910   11 12 28
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

11 14 20  3C66A        06 25 44  41.1 -57.5  4.0      83.7    -8     4910   11 14 28
11 15 30  ---          06 26 54  40.9 -57.5  4.1      83.5    62     4918   11 14 28

11 15 30  SN1986J      06 26 54  40.8 -58.4  4.1      82.9    -8     4918   11 15 38
11 17 30  ---          06 28 55  40.4 -58.3  4.1      82.6   112     4932   11 15 38

11 17 30  3C66A        06 28 55  40.5 -57.4  4.1      83.2    -8     4932   11 17 38
11 18 40  ---          06 30 05  40.3 -57.4  4.1      83.0    62     4940   11 17 38

11 18 40  SN1986J      06 30 05  40.2 -58.3  4.1      82.4    -8     4940   11 18 48
11 20 40  ---          06 32 05  39.8 -58.2  4.1      82.1   112     4955   11 18 48

11 21 10  3C66A        06 32 35  39.9 -57.3  4.1      82.7    22     4955   11 21 10
11 22 40  ---          06 34 06  39.6 -57.3  4.2      82.4    90     4966   11 21 10

11 22 40  SN1986J      06 34 06  39.5 -58.2  4.2      81.8    -8     4966   11 22 48
11 24 40  ---          06 36 06  39.1 -58.1  4.2      81.5   112     4981   11 22 48

11 24 40  3C66A        06 36 06  39.2 -57.2  4.2      82.1    -8     4981   11 24 48
11 25 50  ---          06 37 16  39.0 -57.2  4.2      81.9    62     4989   11 24 48

11 25 50  SN1986J      06 37 16  38.9 -58.1  4.2      81.4    -8     4989   11 25 58
11 27 50  ---          06 39 16  38.5 -58.0  4.3      81.1   112     5003   11 25 58

11 27 50  3C66A        06 39 16  38.6 -57.1  4.3      81.6    -8     5003   11 27 58
11 29 00  ---          06 40 27  38.4 -57.1  4.3      81.5    62     5011   11 27 58

11 29 00  SN1986J      06 40 27  38.3 -57.9  4.3      80.9    -8     5011   11 29 08
11 31 00  ---          06 42 27  37.9 -57.9  4.3      80.6   112     5025   11 29 08

11 31 20  3C66A        06 42 47  38.0 -57.0  4.3      81.1    12     5025   11 31 20
11 32 30  ---          06 43 57  37.8 -56.9  4.3      80.9    70     5034   11 31 20

11 32 30  SN1986J      06 43 57  37.7 -57.8  4.3      80.4    -8     5034   11 32 38
11 34 30  ---          06 45 58  37.3 -57.7  4.4      80.1   112     5049   11 32 38

11 34 30  3C66A        06 45 58  37.4 -56.9  4.4      80.7    -8     5049   11 34 38
11 35 40  ---          06 47 08  37.2 -56.8  4.4      80.5    62     5057   11 34 38

11 35 40  SN1986J      06 47 08  37.1 -57.7  4.4      79.9    -8     5057   11 35 48
11 37 40  ---          06 49 08  36.7 -57.6  4.4      79.6   112     5071   11 35 48

11 37 40  3C66A        06 49 08  36.9 -56.7  4.4      80.2    -8     5071   11 37 48
11 38 50  ---          06 50 18  36.7 -56.7  4.4      80.0    62     5079   11 37 48
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

11 38 50  SN1986J      06 50 18  36.5 -57.5  4.4      79.5    -8     5079   11 38 58
11 40 50  ---          06 52 19  36.1 -57.5  4.5      79.2   112     5094   11 38 58

11 41 20  3C66A        06 52 49  36.2 -56.6  4.5      79.6    22     5094   11 41 20
11 42 50  ---          06 54 19  35.9 -56.5  4.5      79.4    90     5105   11 41 20

11 42 50  SN1986J      06 54 19  35.8 -57.4  4.5      78.9    -8     5105   11 42 58
11 44 50  ---          06 56 19  35.4 -57.3  4.5      78.6   112     5120   11 42 58

11 44 50  3C66A        06 56 19  35.6 -56.4  4.5      79.1    -8     5120   11 44 58
11 46 00  ---          06 57 29  35.4 -56.4  4.6      79.0    62     5128   11 44 58

11 46 00  SN1986J      06 57 29  35.2 -57.2  4.6      78.4    -8     5128   11 46 08
11 48 00  ---          06 59 30  34.8 -57.1  4.6      78.2   112     5142   11 46 08

11 48 00  3C66A        06 59 30  35.0 -56.3  4.6      78.7    -8     5142   11 48 08
11 49 10  ---          07 00 40  34.8 -56.3  4.6      78.5    62     5150   11 48 08

11 49 10  SN1986J      07 00 40  34.6 -57.1  4.6      78.0    -8     5150   11 49 18
11 51 10  ---          07 02 40  34.3 -57.0  4.7      77.7   112     5164   11 49 18

11 51 30  3C66A        07 03 00  34.4 -56.1  4.7      78.2    12     5164   11 51 30
11 52 40  ---          07 04 11  34.2 -56.1  4.7      78.0    70     5173   11 51 30

11 52 40  SN1986J      07 04 11  34.0 -56.9  4.7      77.5    -8     5173   11 52 48
11 54 40  ---          07 06 11  33.6 -56.8  4.7      77.2   112     5188   11 52 48

11 54 40  3C66A        07 06 11  33.8 -56.0  4.7      77.7    -8     5188   11 54 48
11 55 50  ---          07 07 21  33.6 -55.9  4.7      77.5    62     5196   11 54 48

11 55 50  SN1986J      07 07 21  33.4 -56.8  4.7      77.0    -8     5196   11 55 58
11 57 50  ---          07 09 21  33.1 -56.7  4.8      76.8   112     5210   11 55 58

11 57 50  3C66A        07 09 21  33.2 -55.9  4.8      77.2    -8     5210   11 57 58
11 59 00  ---          07 10 32  33.0 -55.8  4.8      77.1    62     5218   11 57 58

11 59 00  SN1986J      07 10 32  32.9 -56.6  4.8      76.6    -8     5218   11 59 08
12 01 00  ---          07 12 32  32.5 -56.5  4.8      76.3   112     5233   11 59 08

12 01 30  3C66A        07 13 02  32.6 -55.7  4.8      76.7    22     5233   12 01 30
12 03 00  ---          07 14 32  32.3 -55.6  4.8      76.5    90     5244   12 01 30

12 03 30  3C84         07 15 02  42.4 -59.8  3.9      83.5     2     5244   12 03 30
12 06 30  ---          07 18 03  41.8 -59.7  4.0      83.1   180     5268   12 03 30
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

12 07 00  3C66A        07 18 33  31.6 -55.4  4.9      75.9     2     5268   12 07 00
12 08 30  ---          07 20 03  31.4 -55.3  4.9      75.7    90     5279   12 07 00

12 08 30  SN1986J      07 20 03  31.1 -56.1  4.9      75.3    -8     5279   12 08 38
12 10 30  ---          07 22 04  30.8 -56.0  5.0      75.0   112     5294   12 08 38

12 10 30  3C66A        07 22 04  31.0 -55.2  5.0      75.4    -8     5294   12 10 38
12 11 40  ---          07 23 14  30.8 -55.1  5.0      75.2    62     5302   12 10 38

12 11 40  SN1986J      07 23 14  30.6 -55.9  5.0      74.8    -8     5302   12 11 48
12 13 40  ---          07 25 14  30.2 -55.8  5.0      74.5   112     5316   12 11 48

12 13 40  3C66A        07 25 14  30.4 -55.0  5.0      75.0    -8     5316   12 13 48
12 14 50  ---          07 26 24  30.2 -55.0  5.0      74.8    62     5324   12 13 48

12 14 50  SN1986J      07 26 24  30.0 -55.7  5.0      74.4    -8     5324   12 14 58
12 16 50  ---          07 28 25  29.7 -55.6  5.1      74.1   112     5338   12 14 58

12 17 10  3C66A        07 28 45  29.8 -54.8  5.1      74.5    12     5338   12 17 10
12 18 20  ---          07 29 55  29.6 -54.8  5.1      74.3    70     5347   12 17 10

12 18 20  SN1986J      07 29 55  29.4 -55.5  5.1      73.9    -8     5347   12 18 28
12 20 20  ---          07 31 55  29.0 -55.4  5.1      73.6   112     5362   12 18 28

12 20 20  3C66A        07 31 55  29.3 -54.7  5.1      74.0    -8     5362   12 20 28
12 21 30  ---          07 33 05  29.1 -54.6  5.2      73.8    62     5370   12 20 28

12 21 30  SN1986J      07 33 05  28.8 -55.3  5.2      73.4    -8     5370   12 21 38
12 23 30  ---          07 35 06  28.5 -55.2  5.2      73.2   112     5384   12 21 38

12 23 30  3C66A        07 35 06  28.7 -54.5  5.2      73.5    -8     5384   12 23 38
12 24 40  ---          07 36 16  28.5 -54.4  5.2      73.4    62     5392   12 23 38

12 24 40  SN1986J      07 36 16  28.3 -55.2  5.2      73.0    -8     5392   12 24 48
12 26 40  ---          07 38 16  27.9 -55.0  5.2      72.7   112     5407   12 24 48

12 27 10  3C66A        07 38 46  28.1 -54.3  5.3      73.0    22     5407   12 27 10
12 28 40  ---          07 40 16  27.8 -54.2  5.3      72.8    90     5418   12 27 10

12 28 40  SN1986J      07 40 16  27.6 -54.9  5.3      72.4    -8     5418   12 28 48
12 30 40  ---          07 42 17  27.2 -54.8  5.3      72.2   112     5433   12 28 48

12 30 40  3C66A        07 42 17  27.4 -54.0  5.3      72.5    -8     5433   12 30 48
12 31 50  ---          07 43 27  27.2 -54.0  5.3      72.4    62     5441   12 30 48
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

12 31 50  SN1986J      07 43 27  27.0 -54.7  5.3      72.0    -8     5441   12 31 58
12 33 50  ---          07 45 27  26.7 -54.6  5.4      71.7   112     5455   12 31 58

12 33 50  3C66A        07 45 27  26.9 -53.8  5.4      72.1    -8     5455   12 33 58
12 35 00  ---          07 46 38  26.7 -53.8  5.4      71.9    62     5463   12 33 58

12 35 00  SN1986J      07 46 38  26.4 -54.5  5.4      71.6    -8     5463   12 35 08
12 37 00  ---          07 48 38  26.1 -54.4  5.4      71.3   112     5478   12 35 08

12 37 20  3C66A        07 48 58  26.3 -53.6  5.4      71.6    12     5478   12 37 20
12 38 30  ---          07 50 08  26.1 -53.5  5.4      71.4    70     5487   12 37 20

12 38 30  SN1986J      07 50 08  25.8 -54.3  5.4      71.1    -8     5487   12 38 38
12 40 30  ---          07 52 08  25.5 -54.1  5.5      70.8   112     5501   12 38 38

12 40 30  3C66A        07 52 08  25.7 -53.4  5.5      71.1    -8     5501   12 40 38
12 41 40  ---          07 53 19  25.5 -53.3  5.5      71.0    62     5509   12 40 38

12 41 40  SN1986J      07 53 19  25.3 -54.1  5.5      70.6    -8     5509   12 41 48
12 43 40  ---          07 55 19  24.9 -53.9  5.5      70.3   112     5523   12 41 48

12 43 40  3C66A        07 55 19  25.2 -53.2  5.5      70.7    -8     5523   12 43 48
12 44 50  ---          07 56 29  25.0 -53.1  5.5      70.5    62     5531   12 43 48

12 44 50  SN1986J      07 56 29  24.7 -53.8  5.5      70.2    -8     5531   12 44 58
12 46 50  ---          07 58 29  24.4 -53.7  5.6      69.9   112     5546   12 44 58

12 47 20  3C66A        07 59 00  24.6 -53.0  5.6      70.1    22     5546   12 47 20
12 48 50  ---          08 00 30  24.3 -52.8  5.6      69.9    90     5557   12 47 20

12 48 50  SN1986J      08 00 30  24.0 -53.6  5.6      69.6    -8     5557   12 48 58
12 50 50  ---          08 02 30  23.7 -53.4  5.7      69.3   112     5572   12 48 58

12 50 50  3C66A        08 02 30  24.0 -52.7  5.6      69.6    -8     5572   12 50 58
12 52 00  ---          08 03 40  23.8 -52.6  5.7      69.5    62     5580   12 50 58

12 52 00  SN1986J      08 03 40  23.5 -53.3  5.7      69.2    -8     5580   12 52 08
12 54 00  ---          08 05 41  23.1 -53.2  5.7      68.9   112     5594   12 52 08

12 54 00  3C66A        08 05 41  23.4 -52.5  5.7      69.2    -8     5594   12 54 08
12 55 10  ---          08 06 51  23.2 -52.4  5.7      69.0    62     5602   12 54 08

12 55 10  SN1986J      08 06 51  22.9 -53.1  5.7      68.7    -8     5602   12 55 18
12 57 10  ---          08 08 51  22.6 -53.0  5.8      68.4   112     5617   12 55 18
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

12 57 30  3C66A        08 09 11  22.8 -52.2  5.8      68.7    12     5617   12 57 30
12 58 40  ---          08 10 21  22.6 -52.2  5.8      68.5    70     5626   12 57 30

12 58 40  SN1986J      08 10 21  22.3 -52.8  5.8      68.2    -8     5626   12 58 48
13 00 40  ---          08 12 22  22.0 -52.7  5.8      67.9   112     5640   12 58 48

13 00 40  3C66A        08 12 22  22.3 -52.0  5.8      68.2    -8     5640   13 00 48
13 01 50  ---          08 13 32  22.1 -51.9  5.8      68.1    62     5648   13 00 48

13 01 50  SN1986J      08 13 32  21.8 -52.6  5.8      67.8    -8     5648   13 01 58
13 03 50  ---          08 15 32  21.4 -52.5  5.9      67.5   112     5662   13 01 58

13 03 50  3C66A        08 15 32  21.7 -51.8  5.9      67.8    -8     5662   13 03 58
13 05 00  ---          08 16 42  21.5 -51.7  5.9      67.6    62     5670   13 03 58

13 05 00  SN1986J      08 16 42  21.2 -52.4  5.9      67.3    -8     5670   13 05 08
13 07 00  ---          08 18 43  20.9 -52.2  5.9      67.1   112     5685   13 05 08

13 07 30  3C66A        08 19 13  21.1 -51.5  5.9      67.3    22     5685   13 07 30
13 09 00  ---          08 20 43  20.9 -51.4  6.0      67.0    90     5697   13 07 30

13 09 00  SN1986J      08 20 43  20.6 -52.1  6.0      66.8    -8     5697   13 09 08
13 11 00  ---          08 22 43  20.2 -51.9  6.0      66.5   112     5711   13 09 08

13 11 00  3C66A        08 22 43  20.5 -51.2  6.0      66.7    -8     5711   13 11 08
13 12 10  ---          08 23 54  20.3 -51.1  6.0      66.6    62     5719   13 11 08

13 12 10  SN1986J      08 23 54  20.0 -51.8  6.0      66.3    -8     5719   13 12 18
13 14 10  ---          08 25 54  19.7 -51.7  6.0      66.0   112     5733   13 12 18

13 14 10  3C66A        08 25 54  20.0 -51.0  6.0      66.3    -8     5733   13 14 18
13 15 20  ---          08 27 04  19.8 -50.9  6.1      66.1    62     5741   13 14 18

13 15 20  SN1986J      08 27 04  19.5 -51.6  6.1      65.9    -8     5741   13 15 28
13 17 20  ---          08 29 04  19.2 -51.4  6.1      65.6   112     5756   13 15 28

13 17 40  3C66A        08 29 25  19.4 -50.7  6.1      65.8    12     5756   13 17 40
13 18 50  ---          08 30 35  19.2 -50.6  6.1      65.6    70     5765   13 17 40

13 18 50  SN1986J      08 30 35  18.9 -51.3  6.1      65.4    -8     5765   13 18 58
13 20 50  ---          08 32 35  18.6 -51.1  6.2      65.1   112     5779   13 18 58

13 20 50  3C66A        08 32 35  18.9 -50.5  6.1      65.3    -8     5779   13 20 58
13 22 00  ---          08 33 45  18.7 -50.4  6.2      65.2    62     5787   13 20 58
Schedule for VLBA_FD   (Code Fd )                                   Page  35
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

13 22 00  SN1986J      08 33 45  18.4 -51.0  6.2      64.9    -8     5787   13 22 08
13 24 00  ---          08 35 46  18.0 -50.9  6.2      64.6   112     5802   13 22 08

13 24 00  3C66A        08 35 46  18.4 -50.2  6.2      64.9    -8     5802   13 24 08
13 25 10  ---          08 36 56  18.2 -50.1  6.2      64.7    62     5810   13 24 08

13 25 10  SN1986J      08 36 56  17.8 -50.8  6.2      64.5    -8     5810   13 25 18
13 27 10  ---          08 38 56  17.5 -50.6  6.3      64.2   112     5824   13 25 18

13 27 40  3C66A        08 39 26  17.8 -49.9  6.3      64.3    22     5824   13 27 40
13 29 10  ---          08 40 56  17.5 -49.8  6.3      64.1    90     5836   13 27 40

13 29 10  SN1986J      08 40 56  17.2 -50.4  6.3      63.9    -8     5836   13 29 18
13 31 10  ---          08 42 57  16.8 -50.2  6.3      63.6   112     5850   13 29 18

13 31 10  3C66A        08 42 57  17.2 -49.6  6.3      63.8    -8     5850   13 31 18
13 32 20  ---          08 44 07  17.0 -49.5  6.3      63.6    62     5858   13 31 18

13 32 20  SN1986J      08 44 07  16.6 -50.1  6.3      63.4    -8     5858   13 32 28
13 34 20  ---          08 46 07  16.3 -50.0  6.4      63.1   112     5872   13 32 28

13 34 20  3C66A        08 46 07  16.7 -49.3  6.4      63.4    -8     5872   13 34 28
13 35 30  ---          08 47 17  16.5 -49.2  6.4      63.2    62     5880   13 34 28

13 35 30  SN1986J      08 47 17  16.1 -49.9  6.4      63.0    -8     5880   13 35 38
13 37 30  ---          08 49 18  15.8 -49.7  6.4      62.7   112     5895   13 35 38

13 37 50  3C66A        08 49 38  16.1 -49.0  6.4      62.8    12     5895   13 37 50
13 39 00  ---          08 50 48  15.9 -48.9  6.5      62.7    70     5904   13 37 50

13 39 00  SN1986J      08 50 48  15.6 -49.6  6.5      62.5    -8     5904   13 39 08
13 41 00  ---          08 52 48  15.2 -49.4  6.5      62.2   112     5918   13 39 08

13 41 00  3C66A        08 52 48  15.6 -48.7  6.5      62.4    -8     5918   13 41 08
13 42 10  ---          08 53 59  15.4 -48.6  6.5      62.2    62     5926   13 41 08

13 42 10  SN1986J      08 53 59  15.0 -49.3  6.5      62.0    -8     5926   13 42 18
13 44 10  ---          08 55 59  14.7 -49.1  6.5      61.7   112     5941   13 42 18

13 44 10  3C66A        08 55 59  15.1 -48.5  6.5      61.9    -8     5941   13 44 18
13 45 20  ---          08 57 09  14.9 -48.4  6.6      61.7    62     5949   13 44 18

13 45 20  SN1986J      08 57 09  14.5 -49.0  6.6      61.6    -8     5949   13 45 28
13 47 20  ---          08 59 09  14.2 -48.8  6.6      61.3   112     5963   13 45 28
Schedule for VLBA_FD   (Code Fd )                                   Page  36
               11th epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  23 Oct 2014   Day 296 ---

13 47 50  3C66A        08 59 39  14.5 -48.1  6.6      61.4    22     5963   13 47 50
13 49 10  ---          09 01 00  14.3 -48.0  6.6      61.2    80     5973   13 47 50

13 49 40  SN1986J      09 01 30  13.8 -48.6  6.6      60.9    22     5973   13 49 40
13 51 30  ---          09 03 20  13.5 -48.4  6.7      60.6   110     5988   13 49 40

13 51 30  3C66A        09 03 20  13.9 -47.8  6.7      60.8    -8     5988   13 51 38
13 52 50  ---          09 04 40  13.7 -47.7  6.7      60.6    72     5997   13 51 38

13 52 50  SN1986J      09 04 40  13.3 -48.3  6.7      60.4    -8     5997   13 52 58
13 54 30  ---          09 06 21  13.0 -48.1  6.7      60.2    92     6009   13 52 58

13 55 00  3C66A        09 06 51  13.3 -47.5  6.7      60.3    22     6009   13 55 00
13 56 30  ---          09 08 21  13.1 -47.3  6.7      60.1    90     6020   13 55 00

13 57 00  3C84         09 08 51  21.8 -53.6  5.8      67.8     5     6020   13 57 00
14 00 00  ---          09 11 51  21.3 -53.4  5.9      67.3   180     6044   13 57 00


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess314.C1024glob
   Matching groups in /users/cwalker/files/sched_beta/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    4         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.1      4.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   1  Setup file default.  Used with PCAL = off
   LO sum=   4924.75  4924.75  5003.25  5003.25
   BBC fr=    824.75   824.75   903.25   903.25
   Bandwd=     64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     848.75    848.75    927.25    927.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   1   2   3   4   5   6   7   8  20  21

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SN1986J           02 19 22.592220   * 02 22 31.320000     02 23 29.863290       0.00
                     42 06 18.95870    * 42 19 57.28200      42 23 58.93503        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C66A             02 19 29.982891   * 02 22 39.611477     02 23 38.458151       0.00
                     42 48 29.80879    * 43 02 07.79928      43 06 09.26285        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C84              03 16 29.567269   * 03 19 48.160100     03 20 49.418728       0.00
                     41 19 51.91887    * 41 30 42.10600      41 33 48.48926        0.00
                     From catalog imbedded in main SCHED input file.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  SN1986J    sess314.C1024glob     1 9 10 11 12 13 16 17 18 19 +    12.369  1225.744
  3C66A      sess314.C1024glob     1 9 10 11 12 13 16 17 18 19 +     7.903   733.885
  3C84       sess314.C1024glob     1 9 10 11 12 13 16 17 18 19 +     0.572    52.750

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * J0244+6228        02 41 00.673388   * 02 44 57.696708     02 46 12.315376       0.52
   0241+622          62 15 27.54317    * 62 28 06.51568      62 31 45.29606        0.21
   J0244+62          /users/cwalker/files/sched_beta/catalogs/sources.vlba
                     GSFC 2011B astro solution        95 Observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1986J            148.1
   3C66A              147.4
   3C84               143.9
   J0244+6228         127.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

