  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron Imaging of high-redshift quasars
 Exp. Code:  eg094b  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Leonid Gurvits

Address:  Joint Institute for VLBI in Europe
          Oude Hoogeveensedijk 4
          7991 PD Dwingeloo, The Netherlands
 

Phone:    +31 521 596 514
EMAIL:    lgurvits@jive.eu
Fax:      +31 521 596 539
Phone during observation: +31 521 596 514

Observing mode: L-band, dual-pol

Notes:    L-band, Radioastron-compatible frequency setup
          P-CAL is ON, Tsys is ON, auto-level (AGC) is ON
          Mk5 raw data should be transferred to JIVE first,
          from JIVE raw data should be e-transferred to ASC/Moscow

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

 ---------- C/L-band VLBI scans. Ground segment 01 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00
 Next scan bandwidths:     16.00    16.00    16.00    16.00

00 00 00  2215+020     19 27 22  40.7 116.4 -2.9     -50.5     0        0   00 00 00
00 05 00  ---          19 32 23  41.7 117.5 -2.8     -49.8   300       10   00 00 01

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

00 05 30  2215+020     19 32 53  41.8 117.6 -2.8     -49.8    24       10   00 05 30
00 10 30  ---          19 37 53  42.7 118.7 -2.7     -49.1   300       19   00 05 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 11 00  2215+020     19 38 24  42.8 118.8 -2.7     -49.0    24       19   00 11 00
00 16 00  ---          19 43 24  43.7 119.9 -2.6     -48.3   300       29   00 11 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

00 16 30  2215+020     19 43 54  43.8 120.0 -2.6     -48.2    24       29   00 16 30
00 21 30  ---          19 48 55  44.8 121.2 -2.5     -47.4   300       39   00 16 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 22 00  2215+020     19 49 25  44.9 121.3 -2.5     -47.4    24       39   00 22 00
00 27 00  ---          19 54 26  45.8 122.5 -2.4     -46.6   300       48   00 22 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

00 27 30  2215+020     19 54 56  45.9 122.7 -2.4     -46.5    24       48   00 27 30
00 32 30  ---          19 59 57  46.8 123.9 -2.3     -45.6   300       58   00 27 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 33 00  2215+020     20 00 27  46.9 124.0 -2.3     -45.5    24       58   00 33 00
00 38 00  ---          20 05 28  47.7 125.4 -2.2     -44.6   300       68   00 33 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

00 38 30  2215+020     20 05 58  47.8 125.5 -2.2     -44.5    24       68   00 38 30
00 43 30  ---          20 10 59  48.7 126.8 -2.1     -43.6   300       77   00 38 55
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 44 00  2215+020     20 11 29  48.8 127.0 -2.1     -43.5    24       77   00 44 00
00 49 00  ---          20 16 30  49.6 128.4 -2.0     -42.5   300       87   00 44 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

00 49 30  2215+020     20 17 00  49.7 128.5 -2.0     -42.4    24       87   00 49 30
00 54 30  ---          20 22 01  50.6 130.0 -1.9     -41.3   300       97   00 49 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

00 55 00  2215+020     20 22 31  50.6 130.1 -1.9     -41.2    24       97   00 55 00
01 00 00  ---          20 27 32  51.5 131.6 -1.9     -40.1   300      106   00 55 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

01 00 30  2215+020     20 28 02  51.5 131.8 -1.8     -39.9    24      106   01 00 30
01 05 30  ---          20 33 02  52.3 133.4 -1.8     -38.8   300      116   01 00 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

01 06 00  2215+020     20 33 33  52.4 133.5 -1.8     -38.6    24      116   01 06 00
01 11 00  ---          20 38 33  53.2 135.2 -1.7     -37.4   300      126   01 06 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

01 11 30  2215+020     20 39 03  53.3 135.3 -1.7     -37.3    24      126   01 11 30
01 16 30  ---          20 44 04  54.0 137.0 -1.6     -36.0   300      135   01 11 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

01 17 20  2251+158     20 44 54  57.1 108.5 -2.2     -58.2    22      135   01 17 20
01 24 00  ---          20 51 35  58.4 110.1 -2.1     -57.3   400      148   01 17 45

 ---------- L-band VLBI scans. Space segment 01 ----------

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

01 25 00  2215+020     20 52 36  55.2 140.0 -1.4     -33.6    31      148   01 25 00
01 42 30  ---          21 10 09  57.5 146.8 -1.1     -28.1  1050      182   01 25 25

01 43 00  2215+020     21 10 39  57.5 147.0 -1.1     -27.9    24      182   01 43 00
02 00 00  ---          21 27 41  59.3 154.4 -0.8     -21.8  1020      215   01 43 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

02 00 30  2215+020     21 28 11  59.4 154.6 -0.8     -21.6    24      215   02 00 30
02 17 30  ---          21 45 14  60.7 162.7 -0.6     -14.8  1020      248   02 00 31

02 18 00  2215+020     21 45 44  60.7 163.0 -0.5     -14.6    24      248   02 18 00
02 35 00  ---          22 02 47  61.5 171.7 -0.3      -7.2  1020      281   02 18 01

 ---------- C/L-band VLBI VLBA only scans. Ground segment 02 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 36 00  2215+020     22 03 47  61.6 172.2 -0.2      -6.7    54      281   02 36 00
02 41 00  ---          22 08 48  61.7 174.8 -0.2      -4.5   300      290   02 36 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

02 41 30  2215+020     22 09 18  61.7 175.1 -0.2      -4.2    24      290   02 41 30
02 46 30  ---          22 14 19  61.8 177.7 -0.1      -2.0   300      300   02 41 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 47 00  2215+020     22 14 49  61.8 178.0 -0.1      -1.7    24      300   02 47 00
02 52 00  ---          22 19 50  61.8 180.6  0.0       0.5   300      309   02 47 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

02 52 30  2215+020     22 20 20  61.8 180.9  0.0       0.8    24      309   02 52 30
02 57 30  ---          22 25 21  61.7 183.5  0.1       3.0   300      319   02 52 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

02 58 00  2215+020     22 25 51  61.7 183.8  0.1       3.3    24      319   02 58 00
03 03 00  ---          22 30 52  61.6 186.4  0.2       5.5   300      329   02 58 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

03 03 30  2215+020     22 31 22  61.6 186.7  0.2       5.8    24      329   03 03 30
03 08 30  ---          22 36 23  61.5 189.3  0.3       8.0   300      338   03 03 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

03 09 00  2215+020     22 36 53  61.5 189.6  0.3       8.2    24      338   03 09 00
03 14 00  ---          22 41 54  61.3 192.1  0.4      10.4   300      348   03 09 25
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

03 14 30  2215+020     22 42 24  61.2 192.4  0.4      10.7    24      348   03 14 30
03 19 30  ---          22 47 24  61.0 194.9  0.5      12.8   300      358   03 14 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

03 20 00  2215+020     22 47 55  61.0 195.2  0.5      13.0    24      358   03 20 00
03 25 00  ---          22 52 55  60.6 197.7  0.6      15.2   300      367   03 20 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

03 25 30  2215+020     22 53 25  60.6 197.9  0.6      15.4    24      367   03 25 30
03 30 30  ---          22 58 26  60.3 200.4  0.7      17.4   300      377   03 25 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

03 31 00  2215+020     22 58 56  60.2 200.6  0.7      17.6    24      377   03 31 00
03 36 00  ---          23 03 57  59.8 203.0  0.8      19.6   300      387   03 31 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

03 36 30  2215+020     23 04 27  59.8 203.2  0.8      19.8    24      387   03 36 30
03 41 30  ---          23 09 28  59.3 205.5  0.8      21.8   300      396   03 36 55

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

03 42 00  2215+020     23 09 58  59.3 205.7  0.9      22.0    24      396   03 42 00
03 47 00  ---          23 14 59  58.8 208.0  0.9      23.8   300      406   03 42 25

 Next scan frequencies:  1668.00  1668.00  1668.00  1668.00
 Next BBC frequencies:    732.00   732.00   732.00   732.00

03 47 30  2215+020     23 15 29  58.8 208.2  0.9      24.0    24      406   03 47 30
03 52 30  ---          23 20 30  58.2 210.4  1.0      25.8   300      416   03 47 55

 ---------- L-band VLBI VLBA+ only scans. Ground segment 02 ----------

03 53 20  2251+158     23 21 20  74.4 204.3  0.4      21.7    10      416   03 53 20
03 57 40  ---          23 25 41  74.0 207.8  0.5      24.7   260      424   03 53 21

03 58 30  2215+020     23 26 31  57.5 212.9  1.1      27.9    10      424   03 58 30
04 03 30  ---          23 31 32  56.9 214.9  1.2      29.5   300      434   03 58 31

04 04 00  2215+020     23 32 02  56.9 215.1  1.2      29.7    24      434   04 04 00
04 09 00  ---          23 37 03  56.2 217.1  1.3      31.3   300      443   04 04 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

04 09 30  2215+020     23 37 33  56.2 217.3  1.3      31.4    24      443   04 09 30
04 14 30  ---          23 42 34  55.5 219.2  1.4      33.0   300      453   04 09 31

04 15 00  2215+020     23 43 04  55.4 219.4  1.4      33.1    24      453   04 15 00
04 20 00  ---          23 48 04  54.7 221.2  1.5      34.5   300      463   04 15 01

04 20 30  2215+020     23 48 34  54.7 221.3  1.5      34.7    24      463   04 20 30
04 25 30  ---          23 53 35  54.0 223.1  1.6      36.0   300      472   04 20 31

04 26 00  2215+020     23 54 05  53.9 223.3  1.6      36.2    24      472   04 26 00
04 31 00  ---          23 59 06  53.1 225.0  1.7      37.5   300      482   04 26 01

04 31 30  2215+020     23 59 36  53.1 225.1  1.7      37.6    24      482   04 31 30
04 36 30  ---          00 04 37  52.3 226.7  1.8      38.8   300      492   04 31 31

04 37 00  2215+020     00 05 07  52.2 226.9  1.8      39.0    24      492   04 37 00
04 42 00  ---          00 10 08  51.4 228.5  1.9      40.1   300      501   04 37 01

04 42 30  2215+020     00 10 38  51.3 228.6  1.9      40.3    24      501   04 42 30
04 47 30  ---          00 15 39  50.5 230.1  1.9      41.4   300      511   04 42 31

04 48 00  2215+020     00 16 09  50.4 230.3  2.0      41.5    24      511   04 48 00
04 53 00  ---          00 21 10  49.6 231.7  2.0      42.5   300      521   04 48 01

04 53 30  2215+020     00 21 40  49.5 231.9  2.1      42.6    24      521   04 53 30
04 58 30  ---          00 26 41  48.6 233.3  2.1      43.6   300      530   04 53 31

04 59 00  2215+020     00 27 11  48.6 233.4  2.1      43.7    24      530   04 59 00
05 04 00  ---          00 32 12  47.7 234.7  2.2      44.7   300      540   04 59 01

05 04 30  2215+020     00 32 42  47.6 234.9  2.2      44.8    24      540   05 04 30
05 09 30  ---          00 37 43  46.7 236.2  2.3      45.7   300      550   05 04 31

05 10 00  2215+020     00 38 13  46.6 236.3  2.3      45.8    24      550   05 10 00
05 15 00  ---          00 43 13  45.7 237.5  2.4      46.6   300      559   05 10 01

05 15 30  2215+020     00 43 44  45.6 237.7  2.4      46.7    24      559   05 15 30
05 20 30  ---          00 48 44  44.7 238.9  2.5      47.5   300      569   05 15 31

05 21 00  2215+020     00 49 14  44.6 239.0  2.5      47.6    24      569   05 21 00
05 26 00  ---          00 54 15  43.7 240.2  2.6      48.3   300      579   05 21 01

05 26 30  2215+020     00 54 45  43.6 240.3  2.6      48.4    24      579   05 26 30
05 31 30  ---          00 59 46  42.6 241.4  2.7      49.1   300      588   05 26 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

05 32 00  2215+020     01 00 16  42.5 241.5  2.7      49.2    24      588   05 32 00
05 37 00  ---          01 05 17  41.6 242.6  2.8      49.9   300      598   05 32 01

05 37 30  2215+020     01 05 47  41.5 242.7  2.8      49.9    24      598   05 37 30
05 42 30  ---          01 10 48  40.5 243.8  2.9      50.6   300      608   05 37 31

05 43 00  2215+020     01 11 18  40.4 243.9  2.9      50.7    24      608   05 43 00
05 48 00  ---          01 16 19  39.5 244.9  3.0      51.3   300      617   05 43 01

05 48 30  2215+020     01 16 49  39.4 245.0  3.0      51.3    24      617   05 48 30
05 53 30  ---          01 21 50  38.4 246.0  3.1      51.9   300      627   05 48 31

05 54 00  2215+020     01 22 20  38.3 246.1  3.1      51.9    24      627   05 54 00
05 59 00  ---          01 27 21  37.3 247.1  3.1      52.5   300      637   05 54 01

05 59 30  2215+020     01 27 51  37.2 247.2  3.2      52.5    24      637   05 59 30
06 04 30  ---          01 32 52  36.2 248.1  3.2      53.1   300      646   05 59 31

 ---------- L-band VLBI scans. Space segment 02 ----------

06 10 00  2215+020     01 38 22  35.1 249.1  3.3      53.6   324      646   06 10 00
06 27 30  ---          01 55 55  31.5 252.2  3.6      55.1  1050      680   06 10 01

06 28 00  2215+020     01 56 25  31.4 252.3  3.6      55.1    24      680   06 28 00
06 45 00  ---          02 13 28  27.9 255.0  3.9      56.3  1020      713   06 28 01

06 45 30  2215+020     02 13 58  27.8 255.1  3.9      56.3    24      713   06 45 30
07 02 30  ---          02 31 01  24.2 257.7  4.2      57.3  1020      746   06 45 31

07 03 00  2215+020     02 31 31  24.1 257.8  4.2      57.3    24      746   07 03 00
07 20 00  ---          02 48 34  20.5 260.2  4.5      58.1  1020      779   07 03 01

 ---------- L-band VLBI VLBA+ only scans. Ground segment 03 ----------

07 21 00  2251+158     02 49 34  34.9 269.1  3.9      63.6    24      779   07 21 00
07 31 10  ---          02 59 46  32.7 270.4  4.1      63.7   610      798   07 21 01

07 32 00  2215+020     03 00 36  18.0 261.9  4.7      58.5    13      798   07 32 00
07 37 00  ---          03 05 37  16.9 262.6  4.8      58.7   300      808   07 32 01

07 37 30  2215+020     03 06 07  16.8 262.7  4.8      58.7    24      808   07 37 30
07 42 30  ---          03 11 08  15.7 263.3  4.9      58.8   300      818   07 37 31

07 43 00  2215+020     03 11 38  15.6 263.4  4.9      58.8    24      818   07 43 00
07 48 00  ---          03 16 39  14.6 264.1  5.0      58.9   300      827   07 43 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron Imaging of high-redshift quasars
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Oct 2016   Day 301 ---

07 48 30  2215+020     03 17 09  14.5 264.2  5.0      59.0    24      827   07 48 30
07 53 30  ---          03 22 09  13.4 264.8  5.1      59.1   300      837   07 48 31

07 54 00  2215+020     03 22 40  13.3 264.9  5.1      59.1    24      837   07 54 00
07 59 00  ---          03 27 40  12.2 265.5  5.2      59.2   300      847   07 54 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra6cm2.set
   Matching groups in ./eg094b_freq.dat:
     vc_d

   Setup group:    2         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   1  Setup file default.  Used with PCAL = 1MHz
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     736.01    736.01    735.99    735.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   1   2   3   4   5   6   7   8   9  20

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 


 ======== Setup file: ra18cm2.set
   Matching groups in ./eg094b_freq.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:   30         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         L         U         U
   IF SB =         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         L         L
   IF    =        A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  10  Setup file default.  Used with PCAL = 1MHz
   LO sum=   1668.00  1668.00  1668.00  1668.00
   BBC fr=    732.00   732.00   732.00   732.00
   Bandwd=     16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     731.99    731.99    732.01    732.01
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  10  11  12  13  14  15  16  17  18  19

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 32.808792       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 14.78603        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 1934-638          04 20 04.230487   * 19 39 25.024972     04 20 47.461629       0.00
                    -63 49 48.04871    *-63 42 45.62440     -63 40 21.75670        0.00
                     From catalog imbedded in main SCHED input file.
                     ATCA flux calibrator

 * 2215+020          22 15 15.584186   * 22 17 48.237927     22 18 39.727739       0.00
   J2217+0220        02 05 08.96683    * 02 20 10.71214      02 25 23.50610        0.00
                     ./eg094b_sources.radioastron
                     AGN, HIGHz, rfc_2013d Petrov, 2013, unpublished 383 observations, RA-AO3-04, RA-

 * 2251+158          22 51 29.519741   * 22 53 57.747940     22 54 48.149055       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 14 27.30715        0.00
   3C454.3           ./eg094b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO3-04, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra18cm2.set           21                                4.242     0.000
  1934-638   ra6cm2.set            23                                0.083     0.000
  2215+020   ra6cm2.set            1 22 23 24 28 31 32 35 36 3 +    13.683   588.274
             ra18cm2.set           10 25 26 27 29 30 46 47          13.717   157.283
  2251+158   ra6cm2.set            1 22 23 24 28 31 32 35 36 3 +     0.661    31.933
             ra18cm2.set           10 25 26 27 29 30 46              0.536     3.081

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 2145+067          21 45 36.078473   * 21 48 05.458671     21 48 55.746824       0.00
   J2148+0657        06 43 40.90449    * 06 57 38.60409      07 02 32.72502        0.00
                     ./eg094b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 104350 observations, RA-AO3-04, RA-AO2-



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              98.6
   1934-638            99.3
   2145+067           116.0
   2215+020           122.2
   2251+158           133.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

