  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg081a  


Schedule Version:       1.50
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   8 Oct 2016   Day 282 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

20 00 00  3C418        14 15 44  20.1  41.4 -6.4     -65.7     0        0   20 00 00
20 09 30  ---          14 25 16  21.4  42.0 -6.2     -67.3   570       73   20 00 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

20 10 00  3C418        14 25 46  21.5  42.0 -6.2     -67.4    24       73   20 10 00
20 17 50  ---          14 33 37  22.7  42.5 -6.1     -68.8   470      134   20 10 01

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

20 18 20  3C418        14 34 07  22.7  42.6 -6.1     -68.9    24      134   20 18 20
20 29 30  ---          14 45 19  24.4  43.2 -5.9     -70.8   670      220   20 18 21

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

20 30 00  3C418        14 45 49  24.4  43.3 -5.9     -70.9    24      220   20 30 00
20 39 30  ---          14 55 21  25.9  43.8 -5.7     -72.5   570      294   20 30 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

20 40 00  3C418        14 55 51  25.9  43.8 -5.7     -72.6    24      294   20 40 00
20 47 50  ---          15 03 42  27.1  44.2 -5.6     -74.0   470      354   20 40 01

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

20 48 20  3C418        15 04 12  27.2  44.2 -5.6     -74.0    24      354   20 48 20
20 59 30  ---          15 15 24  28.9  44.7 -5.4     -76.0   670      441   20 48 21

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

21 00 00  3C418        15 15 54  28.9  44.7 -5.4     -76.1    24      441   21 00 00
21 09 30  ---          15 25 26  30.4  45.1 -5.2     -77.7   570      514   21 00 01

21 10 00  3C418        15 25 56  30.5  45.2 -5.2     -77.8    24      514   21 10 00
21 23 30  ---          15 39 28  32.5  45.6 -5.0     -80.2   810      618   21 10 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   8 Oct 2016   Day 282 ---

 ---------- K-band VLBI scans. VLBA calibrator scans ----------

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

21 25 00  3C418        15 40 58  32.8  45.7 -5.0     -80.5    84      618   21 25 00
21 37 30  ---          15 53 30  34.7  46.0 -4.8     -82.8   750      715   21 25 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

21 38 00  3C418        15 54 00  34.8  46.0 -4.8     -82.8    24      715   21 38 00
21 45 30  ---          16 01 32  35.9  46.2 -4.6     -84.2   450      773   21 38 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

21 46 00  3C418        16 02 02  36.0  46.2 -4.6     -84.3    24      773   21 46 00
21 54 30  ---          16 10 33  37.4  46.3 -4.5     -85.9   510      839   21 46 01

 ---------- K-band VLBI scans. VLBA calibrator scans ----------

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

21 55 00  3C418        16 11 03  37.4  46.3 -4.5     -86.0    24      839   21 55 00
22 07 30  ---          16 23 35  39.4  46.5 -4.3     -88.4   750      935   21 55 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

22 08 00  3C418        16 24 05  39.5  46.5 -4.3     -88.5    24      935   22 08 00
22 15 30  ---          16 31 37  40.6  46.5 -4.1     -89.9   450      993   22 08 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

22 16 00  3C418        16 32 07  40.7  46.5 -4.1     -90.0    24      993   22 16 00
22 24 30  ---          16 40 38  42.0  46.5 -4.0     -91.7   510     1059   22 16 01

 ---------- K-band  VLBI scans.  Ground segment 03: 2251+158 with EVN+VLBA+GB+Hh ----------

22 26 00  2251+158     16 42 08   5.6  74.4 -6.2     -59.7    10     1059   22 26 00
22 36 00  ---          16 52 10   7.6  75.6 -6.0     -60.2   600     1136   22 26 01

22 36 30  2251+158     16 52 40   7.7  75.7 -6.0     -60.3    24     1136   22 36 30
22 46 00  ---          17 02 12   9.7  76.8 -5.9     -60.8   570     1210   22 36 31

22 47 40  2136+141     17 03 52  25.2  87.6 -4.6     -62.6    62     1210   22 47 40
22 55 30  ---          17 11 43  26.9  88.6 -4.5     -62.7   470     1270   22 47 41
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   8 Oct 2016   Day 282 ---

22 57 40  2251+158     17 13 53  12.2  78.2 -5.7     -61.3    92     1270   22 57 40
23 06 00  ---          17 22 15  14.0  79.2 -5.5     -61.7   500     1335   22 57 41

23 07 40  2251+158     17 23 55  14.3  79.4 -5.5     -61.7    94     1335   23 07 40
23 16 00  ---          17 32 16  16.1  80.4 -5.4     -62.1   500     1399   23 07 41

23 16 30  2251+158     17 32 47  16.2  80.4 -5.4     -62.1    24     1399   Stopped 
23 17 30  ---          17 33 47  16.4  80.5 -5.4     -62.1    60     1399           

23 17 40  2251+158     17 33 57  16.4  80.5 -5.3     -62.1     4     1399   23 17 40
23 26 30  ---          17 42 48  18.3  81.6 -5.2     -62.4   530     1467   23 17 41

23 31 00  2251+158     17 47 19  19.3  82.1 -5.1     -62.6   264     1467   23 31 00
23 37 00  ---          17 53 20  20.6  82.8 -5.0     -62.8   360     1514   23 31 01

23 39 30  2136+141     17 55 50  36.4  94.3 -3.7     -62.4   112     1514   23 39 30
23 45 40  ---          18 02 01  37.7  95.2 -3.6     -62.2   370     1561   23 39 31

23 48 10  2251+158     18 04 32  23.0  84.1 -4.8     -63.1   112     1561   23 48 10
23 56 30  ---          18 12 53  24.7  85.1 -4.7     -63.2   500     1626   23 48 11

 --- Start: Sat   8 Oct 2016   Day 282 -- Stop: Sun   9 Oct 2016   Day 283 ---

23 59 00  2331+073     18 15 24  12.6  88.4 -5.3     -60.2   117     1626   23 59 00
00 05 10  ---          18 21 35  13.9  89.2 -5.2     -60.2   370     1673   23 59 01

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

00 08 40  2251+158     18 25 05  27.4  86.6 -4.5     -63.5   177     1673   00 08 40
00 17 00  ---          18 33 26  29.2  87.6 -4.4     -63.6   500     1738   00 08 41

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

00 18 40  2251+158     18 35 07  29.5  87.8 -4.3     -63.6    94     1738   00 18 40
00 27 00  ---          18 43 28  31.3  88.8 -4.2     -63.6   500     1802   00 18 41

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

00 28 40  2251+158     18 45 08  31.7  89.1 -4.2     -63.6    94     1802   00 28 40
00 37 00  ---          18 53 30  33.5  90.1 -4.0     -63.7   500     1867   00 28 41

00 41 00  2251+158     18 57 30  34.3  90.6 -4.0     -63.7   234     1867   00 41 00
00 47 00  ---          19 03 31  35.6  91.4 -3.9     -63.6   360     1913   00 41 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

00 48 40  2251+158     19 05 12  36.0  91.6 -3.8     -63.6    94     1913   00 48 40
00 57 00  ---          19 13 33  37.8  92.7 -3.7     -63.5   500     1977   00 48 41

00 58 40  2251+158     19 15 13  38.1  93.0 -3.7     -63.5    94     1977   00 58 40
01 07 00  ---          19 23 35  39.9  94.1 -3.5     -63.4   500     2042   00 58 41

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 12 50  2136+141     19 29 26  56.0 111.0 -2.2     -56.0   312     2042   01 12 50
01 19 10  ---          19 35 47  57.3 112.6 -2.1     -55.1   380     2091   01 12 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 20 50  2136+141     19 37 27  57.6 113.0 -2.0     -54.9    94     2091   01 20 50
01 27 10  ---          19 43 48  58.9 114.7 -1.9     -53.8   380     2140   01 20 51

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 27 30  2251+158     19 44 08  44.3  97.1 -3.2     -62.8   -17     2140   01 27 47
01 37 00  ---          19 53 40  46.4  98.6 -3.0     -62.4   553     2211   01 27 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 38 40  2251+158     19 55 20  46.7  98.9 -3.0     -62.3    94     2211   01 38 40
01 47 00  ---          20 03 41  48.5 100.3 -2.9     -61.9   500     2275   01 38 41

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 48 40  2251+158     20 05 22  48.8 100.6 -2.8     -61.8    94     2275   01 48 40
01 57 00  ---          20 13 43  50.6 102.1 -2.7     -61.2   500     2340   01 48 41

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 58 40  2251+158     20 15 23  51.0 102.4 -2.7     -61.1    94     2340   01 58 40
02 07 00  ---          20 23 45  52.7 104.0 -2.5     -60.4   500     2404   01 58 41

 ---------- K-band VLBI scans. Space segment 03: 2251+158 with VLA+VLBA+EVN+GB ----------

02 15 00  2251+158     20 31 46  54.4 105.6 -2.4     -59.7   473     2404   02 15 00
02 23 50  ---          20 40 37  56.2 107.5 -2.2     -58.7   530     2472   02 15 01

02 25 30  2251+158     20 42 18  56.5 107.9 -2.2     -58.5    94     2472   02 25 30
02 33 50  ---          20 50 39  58.2 109.8 -2.1     -57.5   500     2537   02 25 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

02 35 30  2251+158     20 52 19  58.6 110.2 -2.0     -57.2    94     2537   02 35 30
02 43 50  ---          21 00 41  60.3 112.4 -1.9     -55.9   500     2601   02 35 31

02 45 30  2251+158     21 02 21  60.6 112.9 -1.9     -55.7    94     2601   02 45 30
02 53 50  ---          21 10 42  62.2 115.3 -1.7     -54.1   500     2666   02 45 31

02 55 30  2251+158     21 12 23  62.6 115.8 -1.7     -53.8    94     2666   02 55 30
03 03 50  ---          21 20 44  64.2 118.5 -1.6     -52.0   500     2730   02 55 31

03 05 30  2251+158     21 22 24  64.5 119.1 -1.5     -51.6    94     2730   03 05 30
03 15 00  ---          21 31 56  66.2 122.6 -1.4     -49.0   570     2803   03 05 31

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

03 17 10  2251+158     21 34 06  66.6 123.4 -1.3     -48.4   124     2803   03 17 10
03 25 20  ---          21 42 17  68.1 126.9 -1.2     -45.8   490     2867   03 17 11

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

03 26 40  2251+158     21 43 38  68.3 127.5 -1.2     -45.3    74     2867   03 26 40
03 35 20  ---          21 52 19  69.7 131.7 -1.0     -42.0   520     2934   03 26 41

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 37 50  2136+141     21 54 49  73.5 192.9  0.2      11.4   100     2934   03 37 50
03 44 00  ---          22 01 00  73.1 197.9  0.4      15.9   370     2981   03 37 51

03 49 20  2251+158     22 06 21  71.8 139.7 -0.8     -35.4   269     2981   03 49 20
03 56 00  ---          22 13 02  72.7 144.1 -0.7     -31.7   400     3033   03 49 21

03 58 30  2331+073     22 15 33  60.5 136.9 -1.3     -36.4   117     3033   03 58 30
04 04 40  ---          22 21 44  61.4 139.4 -1.2     -34.4   370     3080   03 58 31

04 06 20  2251+158     22 23 24  73.9 151.7 -0.5     -25.1    68     3080   04 06 20
04 15 50  ---          22 32 56  74.8 159.6 -0.4     -18.2   570     3154   04 06 21

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

04 28 10  2251+158     22 45 18  75.4 170.9 -0.2      -8.2   733     3154   04 28 10
04 36 20  ---          22 53 29  75.6 178.7 -0.0      -1.1   490     3217   04 28 11
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

04 37 40  2251+158     22 54 49  75.6 180.0  0.0       0.0    74     3217   04 37 40
04 46 20  ---          23 03 31  75.5 188.4  0.1       7.5   520     3284   04 37 41

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

04 48 50  2136+141     23 06 01  64.5 235.6  1.4      47.1   109     3284   04 48 50
04 55 00  ---          23 12 12  63.3 237.8  1.5      48.8   370     3332   04 48 51

04 57 30  2251+158     23 14 43  74.9 198.6  0.3      16.7   113     3332   04 57 30
05 05 30  ---          23 22 44  74.3 205.5  0.5      22.7   480     3393   04 57 31

05 08 00  2331+073     23 25 14  67.0 173.8 -0.2      -5.4   119     3393   05 08 00
05 14 10  ---          23 31 25  67.1 177.7 -0.1      -2.0   370     3441   05 08 01

05 15 50  2251+158     23 33 06  73.2 213.4  0.6      29.6    67     3441   05 15 50
05 23 50  ---          23 41 07  72.1 218.9  0.8      34.3   480     3503   05 15 51

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

05 28 30  2251+158     23 45 48  71.5 221.8  0.8      36.7   274     3503   05 28 30
05 36 40  ---          23 53 59  70.3 226.5  1.0      40.6   490     3566   05 28 31

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

05 38 00  2251+158     23 55 19  70.0 227.2  1.0      41.2    74     3566   05 38 00
05 46 40  ---          00 04 01  68.6 231.6  1.2      44.6   520     3633   05 38 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 48 20  2251+158     00 05 41  68.3 232.4  1.2      45.2    94     3633   05 48 20
05 56 20  ---          00 13 42  66.9 235.8  1.3      47.9   480     3695   05 48 21

05 58 00  2251+158     00 15 23  66.6 236.5  1.3      48.4    94     3695   05 58 00
06 06 00  ---          00 23 24  65.2 239.6  1.5      50.6   480     3757   05 58 01

06 07 40  2251+158     00 25 04  64.9 240.2  1.5      51.0    94     3757   06 07 40
06 15 40  ---          00 33 05  63.4 242.9  1.6      52.9   480     3819   06 07 41
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 18 30  2136+141     00 35 56  46.6 258.3  2.9      60.5   130     3819   06 18 30
06 26 50  ---          00 44 17  44.8 259.7  3.1      61.0   500     3883   06 18 31

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

06 28 30  2136+141     00 45 58  44.5 260.0  3.1      61.0    94     3883   06 28 30
06 36 50  ---          00 54 19  42.7 261.3  3.2      61.5   500     3947   06 28 31

 ---------- K-band VLBI scans. Space segment 04: 2251+158 with Y27+GBT+VLBA ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

06 45 00  2251+158     01 02 30  57.5 251.0  2.1      57.9   450     3947   06 45 00
06 53 50  ---          01 11 22  55.7 253.0  2.3      59.0   530     4016   06 45 01

06 55 30  2251+158     01 13 02  55.4 253.4  2.3      59.2    94     4016   06 55 30
07 03 50  ---          01 21 23  53.6 255.2  2.4      60.0   500     4080   06 55 31

07 05 30  2251+158     01 23 04  53.3 255.5  2.5      60.2    94     4080   07 05 30
07 15 00  ---          01 32 35  51.3 257.3  2.6      61.0   570     4154   07 05 31

07 17 10  2251+158     01 34 46  50.8 257.7  2.7      61.1   124     4154   07 17 10
07 27 10  ---          01 44 47  48.7 259.5  2.8      61.8   600     4231   07 17 11

07 31 20  2251+158     01 48 58  47.8 260.2  2.9      62.0   244     4231   07 31 20
07 38 30  ---          01 56 09  46.3 261.4  3.0      62.4   430     4286   07 31 21

07 39 50  2251+158     01 57 29  46.0 261.6  3.0      62.5    74     4286   07 39 50
07 49 50  ---          02 07 31  43.9 263.2  3.2      62.9   600     4363   07 39 51

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 51 20  2251+158     02 09 01  43.6 263.4  3.2      62.9    84     4363   07 51 20
08 01 20  ---          02 19 03  41.4 264.9  3.4      63.2   600     4441   07 51 21

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

08 03 00  2251+158     02 20 43  41.1 265.1  3.4      63.2    94     4441   08 03 00
08 12 40  ---          02 30 25  39.0 266.5  3.6      63.4   580     4516   08 03 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

08 14 20  2251+158     02 32 05  38.6 266.7  3.6      63.5    94     4516   08 14 20
08 22 10  ---          02 39 56  36.9 267.8  3.8      63.6   470     4576   08 14 21

08 23 30  2251+158     02 41 16  36.7 268.0  3.8      63.6    74     4576   08 23 30
08 31 00  ---          02 48 48  35.0 268.9  3.9      63.6   450     4634   08 23 31

 ---------- K-band VLBI scans. Space segment 05: 2251+158 with SHANGHAI+KVN+LBA+Y27+VLBA+GB ----------

08 40 00  2251+158     02 57 49  33.1 270.1  4.1      63.7   533     4634   08 40 00
08 48 50  ---          03 06 41  31.2 271.2  4.2      63.6   530     4702   08 40 01

08 50 30  2251+158     03 08 21  30.8 271.4  4.2      63.6    94     4702   08 50 30
08 58 50  ---          03 16 42  29.0 272.5  4.4      63.6   500     4767   08 50 31

09 00 30  2251+158     03 18 22  28.7 272.7  4.4      63.5    94     4767   09 00 30
09 10 00  ---          03 27 54  26.6 273.8  4.6      63.4   570     4840   09 00 31

09 12 30  2251+158     03 30 24  26.1 274.1  4.6      63.4   144     4840   09 12 30
09 18 30  ---          03 36 25  24.8 274.8  4.7      63.3   360     4886   09 12 31

09 20 30  2331+073     03 38 26  28.9 261.4  4.1      59.2   102     4886   09 20 30
09 26 40  ---          03 44 37  27.6 262.3  4.2      59.4   370     4934   09 20 31

09 30 30  2251+158     03 48 27  22.2 276.3  4.9      63.0   212     4934   09 30 30
09 38 30  ---          03 56 29  20.5 277.2  5.0      62.8   480     4996   09 30 31

09 40 30  2331+073     03 58 29  24.7 264.2  4.4      59.8   103     4996   09 40 30
09 46 40  ---          04 04 40  23.3 265.1  4.5      59.9   370     5044   09 40 31

09 50 30  2251+158     04 08 31  18.0 278.6  5.2      62.4   213     5044   09 50 30
09 58 30  ---          04 16 32  16.2 279.6  5.4      62.1   480     5105   09 50 31

10 00 30  2251+158     04 18 32  15.8 279.8  5.4      62.0   114     5105   10 00 30
10 08 30  ---          04 26 34  14.1 280.7  5.5      61.7   480     5167   10 00 31

10 10 30  2251+158     04 28 34  13.7 281.0  5.6      61.6   114     5167   10 10 30
10 18 30  ---          04 36 35  12.0 281.9  5.7      61.3   480     5229   10 10 31

10 20 30  2251+158     04 38 36  11.6 282.1  5.7      61.2   114     5229   10 20 30
10 28 30  ---          04 46 37   9.9 283.1  5.9      60.8   480     5291   10 20 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   9 Oct 2016   Day 283 ---

 ---------- K-band VLBI scans. Space segment 06: 2251+158 with VLBA+LBA+KVN+Sh ----------

10 30 00  2251+158     04 48 07   9.6 283.3  5.9      60.7    84     5291   10 30 00
10 38 50  ---          04 56 59   7.7 284.3  6.0      60.3   530     5359   10 30 01

10 40 30  2251+158     04 58 39   7.4 284.5  6.1      60.2    94     5359   10 40 30
10 48 50  ---          05 07 00   5.7 285.5  6.2      59.7   500     5424   10 40 31

10 50 30  2251+158     05 08 41   5.3 285.7  6.2      59.6    94     5424   10 50 30
11 00 00  ---          05 18 12   3.3 286.9  6.4      59.0   570     5497   10 50 31

11 02 20  2251+158     05 20 33   2.9 287.2  6.4      58.9   134     5497   11 02 20
11 09 00  ---          05 27 14   1.5 288.0  6.5  D   58.4     0     5549   11 02 21

11 11 50  2331+073     05 30 04   5.0 276.0  5.9      59.7   153     5549   11 11 50
11 19 40  ---          05 37 55   3.3 277.0  6.0  H   59.5     0     5609   11 11 51


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg081a_freq.dat:
     v1cm_b3

   Setup group:    8         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  20  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
   BBC fr=     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     759.99    759.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  20  21  22  23  24  25  26  27  28  51

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg081a_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   43         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  29  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
   BBC fr=     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     776.99    776.99    808.99    808.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  29  30  31  32  33  34  35  36  37  53

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg081a_freq.dat:
     v7mm_c8

   Setup group:   54         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  38  Setup file default.  Used with PCAL = off
   LO sum=   43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
   BBC fr=     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.00    754.00    786.00    786.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  38  39  40  41  42  43  44  45  46  54

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 30.885028       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 21.50196        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 2331+073          23 31 40.087463   * 23 34 12.828163     23 35 04.888788       0.00
   J2334+0736        07 19 52.41033    * 07 36 27.55159      07 42 08.61343        0.00
                     From catalog imbedded in main SCHED input file.
                     Calibrator; position from rfc_2013d Petrov, 2013, unpublished 207 observations

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 52.594343       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 36.62028        0.00
 * 3C286             ./gg081a_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati

   0851+202          08 51 57.250618   * 08 54 48.874930     08 55 45.160432       0.00
   J0854+2006        20 17 58.41733    * 20 06 30.64078      20 02 35.26632        0.00
 * OJ287             ./gg081a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 213710 observations, RA-AO3-04, RA-AO3-

   2037+511          20 37 07.456977   * 20 38 37.034732     20 39 08.003296       0.00
   J2038+5119        51 08 35.76950    * 51 19 12.66253      51 23 10.77548        0.00
 * 3C418             ./gg081a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 108656 observations, RA-AO3-04, RA-AO2-

 * 2136+141          21 36 37.412147   * 21 39 01.309269     21 39 50.070488       0.00
   J2139+1423        14 10 00.62094    * 14 23 35.99209      14 28 24.77234        0.00
                     ./gg081a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 52968 observations, RA-AO3-04, RA-AO2-1

 * 2251+158          22 51 29.519741   * 22 53 57.747940     22 54 48.320174       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 14 26.23315        0.00
   3C454.3           ./gg081a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO3-04, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            18                                5.050     0.000
  2331+073   ra1cm2.set            1 4 5 6 8 12 13 14 15 16 17 +     0.775    81.753
  3C286      ra1cm2.set            47                                0.511     0.000
             ra2cm2.set            49                                0.422     0.000
             ra7mm2.set            48                                0.658     0.000
  OJ287      ra1cm2.set            4 5 6 7 12 13 14 15 16 52         1.756    65.139
  3C418      ra1cm2.set            19 20 47                          1.144    27.533
             ra2cm2.set            29 49                             0.639    11.900
             ra7mm2.set            38 48                             1.050    17.567
  2136+141   ra1cm2.set            1 4 5 6 7 8 9 10 11 12 13 1 +     0.989   103.239
             ra2cm2.set            29 49                             0.244    13.444
             ra7mm2.set            38 48                             0.244    13.444
  2251+158   ra1cm2.set            1 4 5 6 7 8 9 10 11 12 13 1 +    16.711  1641.695
             ra6cm2.set            56 57 58                          0.192     0.575
             ra2cm2.set            29 49                             0.853    44.125
             ra7mm2.set            38 48                             0.872    43.583

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   1641+399          16 41 17.606226   * 16 42 58.809963     16 43 31.328223       0.00
   J1642+3948        39 54 10.81479    * 39 48 36.99385      39 47 11.00309        0.00
 * 3C345             ./gg081a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 51938 observations, RA-AO3-04, RA-AO3-0



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              91.4
   2331+073           159.0
   3C286               37.6
   OJ287               65.5
   3C345               69.1
   3C418              110.3
   2136+141           130.3
   2251+158           147.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

