  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg081b  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band,Q-band, dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  17 Oct 2016   Day 291 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

21 16 50  2230+114     16 08 16   0.7  76.6 -6.4  D  -58.8     0        0   21 16 50
21 26 20  ---          16 17 47   2.7  77.8 -6.3  H  -59.2     0       73   21 16 40

21 26 50  2230+114     16 18 18   2.8  77.9 -6.3  H  -59.3    24       73   21 26 39
21 36 20  ---          16 27 49   4.8  79.1 -6.1     -59.7     0      148   21 26 40

 ---------- K-band  VLBI scans.  EVPA calibrator 2136+141 with EVN+KVN+VLBA segment 3 ----------

21 37 43  2136+141     16 29 13  17.8  83.4 -5.2     -62.0    50      148   21 37 32
21 44 43  ---          16 36 14  19.3  84.2 -5.1     -62.1   420      204   21 37 33

21 47 00  2230+114     16 38 31   7.1  80.4 -5.9     -60.1   104      204   21 46 49
21 57 00  ---          16 48 32   9.2  81.6 -5.7     -60.4   600      283   21 46 50

21 57 30  2230+114     16 49 03   9.3  81.7 -5.7     -60.4    24      283   21 57 19
22 07 00  ---          16 58 34  11.3  82.9 -5.6     -60.7   570      357   21 57 20

22 07 30  2230+114     16 59 04  11.4  82.9 -5.6     -60.7    24      357   22 07 19
22 17 00  ---          17 08 36  13.5  84.1 -5.4     -61.0   570      432   22 07 20

22 17 30  2230+114     17 09 06  13.6  84.2 -5.4     -61.0    24      432   22 17 19
22 19 30  ---          17 11 06  14.0  84.4 -5.4     -61.0   120      449   22 17 20

 ---------- K-band VLBI scans. Space segment 02: 2230+114 with EVN+GB+Ro70+VLBA+Y27+Hh(-23:00), no KVN+Sh LBA here ----------

22 20 00  2230+114     17 11 36  14.1  84.5 -5.4     -61.0    24      449   22 19 49
22 28 50  ---          17 20 28  16.0  85.5 -5.2     -61.2   530      519   22 19 50

22 29 00  2230+114     17 20 38  16.1  85.6 -5.2     -61.2     4      519   22 28 56
22 30 00  ---          17 21 38  16.3  85.7 -5.2     -61.2    60      527   22 28 51

22 30 30  2230+114     17 22 08  16.4  85.8 -5.2     -61.2    24      527   22 30 19
22 38 50  ---          17 30 29  18.2  86.8 -5.0     -61.4   500      593   22 30 20

22 39 00  2230+114     17 30 39  18.2  86.8 -5.0     -61.4     4      593   22 38 56
22 40 00  ---          17 31 40  18.4  86.9 -5.0     -61.4    60      601   22 38 51

22 40 30  2230+114     17 32 10  18.5  87.0 -5.0     -61.4    24      601   22 40 19
22 48 50  ---          17 40 31  20.3  88.0 -4.9     -61.5   500      667   22 40 20

22 49 00  2230+114     17 40 41  20.4  88.0 -4.9     -61.5     4      667   22 48 56
22 50 00  ---          17 41 41  20.6  88.2 -4.9     -61.5    60      675   22 48 51
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  17 Oct 2016   Day 291 ---

22 50 30  2230+114     17 42 11  20.7  88.2 -4.9     -61.5    24      675   22 50 19
22 58 50  ---          17 50 33  22.5  89.3 -4.7     -61.5   500      741   22 50 20

22 59 00  2230+114     17 50 43  22.5  89.3 -4.7     -61.5     4      741   22 58 56
23 00 00  ---          17 51 43  22.7  89.4 -4.7     -61.5    60      749   22 58 51

23 00 30  2230+114     17 52 13  22.8  89.5 -4.7     -61.5    24      749   23 00 19
23 06 00  ---          17 57 44  24.0  90.2 -4.6     -61.5   330      793   23 00 20

23 06 10  2230+114     17 57 54  24.1  90.2 -4.6     -61.5     4      793   23 06 06
23 08 50  ---          18 00 34  24.6  90.6 -4.5     -61.5   160      814   23 06 01

23 09 00  2230+114     18 00 44  24.7  90.6 -4.5     -61.5     4      814   23 08 56
23 10 00  ---          18 01 44  24.9  90.7 -4.5     -61.5    60      823   23 08 51

23 10 30  2230+114     18 02 15  25.0  90.8 -4.5     -61.5    24      823   23 10 19
23 18 50  ---          18 10 36  26.8  91.9 -4.4     -61.5   500      888   23 10 20

23 19 00  2230+114     18 10 46  26.8  91.9 -4.4     -61.5     4      888   23 18 56
23 20 00  ---          18 11 46  27.0  92.0 -4.4     -61.5    60      897   23 18 51

23 20 30  2230+114     18 12 16  27.2  92.1 -4.4     -61.5    24      897   23 20 19
23 28 50  ---          18 20 38  28.9  93.2 -4.2     -61.4   500      962   23 20 20

23 29 00  2230+114     18 20 48  29.0  93.2 -4.2     -61.4     4      962   23 28 56
23 30 00  ---          18 21 48  29.2  93.3 -4.2     -61.4    60      971   23 28 51

23 30 30  2230+114     18 22 18  29.3  93.4 -4.2     -61.3    24      971   23 30 19
23 38 50  ---          18 30 39  31.1  94.5 -4.0     -61.2   500     1036   23 30 20

23 39 00  2230+114     18 30 49  31.1  94.6 -4.0     -61.2     4     1036   23 38 56
23 40 00  ---          18 31 49  31.4  94.7 -4.0     -61.2    60     1045   23 38 51

23 40 30  2230+114     18 32 19  31.5  94.8 -4.0     -61.2    24     1045   23 40 19
23 50 00  ---          18 41 51  33.5  96.1 -3.9     -60.9   570     1120   23 40 20

23 51 00  2230+114     18 42 51  33.7  96.3 -3.8     -60.9    54     1120   23 50 49
23 53 40  ---          18 45 32  34.3  96.6 -3.8     -60.8   160     1142   23 50 50

23 53 50  2230+114     18 45 42  34.3  96.7 -3.8     -60.8     4     1142   23 53 46
23 54 50  ---          18 46 42  34.5  96.8 -3.8     -60.8    60     1150   23 53 41
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Start: Mon  17 Oct 2016   Day 291 -- Stop: Tue  18 Oct 2016   Day 292 ---

23 55 20  2230+114     18 47 12  34.6  96.9 -3.8     -60.8    24     1150   23 55 09
00 03 40  ---          18 55 33  36.4  98.1 -3.6     -60.5   500     1216   23 55 10

 ---------- Ground-only VLBA+VLA27 +Ef  U,Q-band  +Ys in Q band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

00 04 40  2230+114     18 56 33  36.6  98.3 -3.6     -60.5    54     1216   00 04 29
00 05 40  ---          18 57 34  36.9  98.4 -3.6     -60.4    60     1225   00 04 30

00 05 50  2230+114     18 57 44  36.9  98.4 -3.6     -60.4     4     1225   00 05 46
00 12 25  ---          19 04 20  38.3  99.5 -3.5     -60.1   395     1276   00 05 41

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

00 13 40  2230+114     19 05 35  38.6  99.6 -3.5     -60.1    69     1276   00 13 29
00 14 40  ---          19 06 35  38.8  99.8 -3.4     -60.0    60     1285   00 13 30

00 14 50  2230+114     19 06 45  38.8  99.8 -3.4     -60.0     4     1285   00 14 46
00 23 55  ---          19 15 52  40.7 101.3 -3.3     -59.5   545     1356   00 14 41

 ----------  All ground stations in  K-band  on target source ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

00 24 55  2230+114     19 16 52  40.9 101.5 -3.3     -59.5    54     1356   00 24 44
00 25 55  ---          19 17 52  41.2 101.6 -3.3     -59.4    60     1365   00 24 45

00 26 05  2230+114     19 18 02  41.2 101.6 -3.3     -59.4     4     1365   00 26 01
00 35 35  ---          19 27 34  43.2 103.3 -3.1     -58.8   570     1439   00 25 56

 ---------- Ground-only VLBA+VL27 +Ef  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

00 36 35  2230+114     19 28 34  43.4 103.4 -3.1     -58.8    54     1439   00 36 24
00 37 35  ---          19 29 34  43.6 103.6 -3.1     -58.7    60     1448   00 36 25

00 37 45  2230+114     19 29 44  43.6 103.6 -3.1     -58.7     4     1448   00 37 41
00 44 20  ---          19 36 20  45.0 104.8 -3.0     -58.2   395     1500   00 37 36
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

00 45 20  2230+114     19 37 20  45.2 105.0 -2.9     -58.1    54     1500   00 45 09
00 46 20  ---          19 38 20  45.4 105.2 -2.9     -58.0    60     1509   00 45 10

00 46 30  2230+114     19 38 30  45.5 105.2 -2.9     -58.0     4     1509   00 46 26
00 55 35  ---          19 47 37  47.4 107.0 -2.8     -57.2   545     1580   00 46 21

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

00 55 50  2230+114     19 47 52  47.4 107.0 -2.8     -57.2     9     1580   00 55 41
00 58 30  ---          19 50 32  48.0 107.5 -2.7     -57.0   160     1601   00 55 40

 ----------  All ground stations in  K-band  on target source ----------

00 59 00  2230+114     19 51 02  48.1 107.6 -2.7     -56.9    24     1601   00 58 49
01 00 00  ---          19 52 03  48.3 107.8 -2.7     -56.8    60     1610   00 58 50

01 00 10  2230+114     19 52 13  48.3 107.9 -2.7     -56.8     4     1610   01 00 06
01 10 10  ---          20 02 14  50.3 110.0 -2.5     -55.7   600     1688   01 00 01

 ---------- Ground-only VLBA +Ef  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 11 10  2230+114     20 03 14  50.5 110.2 -2.5     -55.6    54     1688   01 10 59
01 12 10  ---          20 04 15  50.7 110.4 -2.5     -55.5    60     1697   01 11 00

01 12 20  2230+114     20 04 25  50.8 110.4 -2.5     -55.5     4     1697   01 12 16
01 18 55  ---          20 11 01  52.1 111.9 -2.4     -54.6   395     1749   01 12 11

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

01 19 55  2230+114     20 12 01  52.3 112.1 -2.4     -54.5    54     1749   01 19 44
01 20 55  ---          20 13 01  52.5 112.4 -2.3     -54.4    60     1758   01 19 45

01 21 05  2230+114     20 13 11  52.5 112.4 -2.3     -54.4     4     1758   01 21 01
01 30 10  ---          20 22 18  54.3 114.6 -2.2     -53.0   545     1829   01 20 56
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

 ----------  All ground stations in  K-band  on target source ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

01 30 40  2230+114     20 22 48  54.4 114.8 -2.2     -53.0    24     1829   01 30 29
01 31 40  ---          20 23 48  54.6 115.0 -2.2     -52.8    60     1838   01 30 30

01 31 50  2230+114     20 23 58  54.7 115.1 -2.2     -52.8     4     1838   01 31 46
01 40 10  ---          20 32 19  56.3 117.3 -2.0     -51.4   500     1903   01 31 41

01 40 40  2230+114     20 32 49  56.4 117.4 -2.0     -51.3    24     1903   01 40 29
01 41 40  ---          20 33 49  56.6 117.7 -2.0     -51.1    60     1912   01 40 30

01 41 50  2230+114     20 33 59  56.6 117.7 -2.0     -51.1     4     1912   01 41 46
01 49 00  ---          20 41 11  57.9 119.8 -1.9     -49.7   430     1968   01 41 41

01 49 30  2230+114     20 41 41  58.0 120.0 -1.9     -49.6    24     1968   01 49 19
01 52 10  ---          20 44 21  58.5 120.8 -1.8     -49.1   160     1990   01 49 20

 ---------- Ground-only VLBA+VLA27  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

01 53 10  2230+114     20 45 21  58.7 121.1 -1.8     -48.8    54     1990   01 52 59
01 54 10  ---          20 46 21  58.9 121.4 -1.8     -48.6    60     1999   01 53 00

01 54 20  2230+114     20 46 31  58.9 121.4 -1.8     -48.6     4     1999   01 54 16
02 00 55  ---          20 53 08  60.1 123.6 -1.7     -47.1   395     2050   01 54 11

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

02 01 55  2230+114     20 54 08  60.3 123.9 -1.7     -46.8    54     2050   02 01 44
02 02 55  ---          20 55 08  60.5 124.3 -1.6     -46.6    60     2060   02 01 45

02 03 05  2230+114     20 55 18  60.5 124.3 -1.6     -46.6     4     2060   02 03 01
02 12 10  ---          21 04 24  62.1 127.6 -1.5     -44.2   545     2130   02 02 56

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

02 13 10  2230+114     21 05 25  62.3 128.0 -1.5     -43.9    54     2130   02 12 59
02 14 10  ---          21 06 25  62.4 128.3 -1.5     -43.6    60     2139   02 13 00

02 14 20  2230+114     21 06 35  62.5 128.4 -1.4     -43.5     4     2139   02 14 16
02 22 40  ---          21 14 56  63.8 131.8 -1.3     -41.0   500     2204   02 14 11
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

02 23 10  2230+114     21 15 26  63.9 132.0 -1.3     -40.8    24     2204   02 22 59
02 24 10  ---          21 16 26  64.1 132.4 -1.3     -40.5    60     2213   02 23 00

02 24 20  2230+114     21 16 36  64.1 132.5 -1.3     -40.4     4     2213   02 24 16
02 32 40  ---          21 24 58  65.4 136.2 -1.1     -37.5   500     2278   02 24 11

02 33 40  2136+141     21 25 58  73.5 168.1 -0.2     -10.6    30     2278   02 33 29
02 34 40  ---          21 26 58  73.6 168.9 -0.2      -9.8    60     2288   02 33 30

02 34 50  2136+141     21 27 08  73.6 169.1 -0.2      -9.7     4     2288   02 34 46
02 39 50  ---          21 32 09  73.7 173.3 -0.1      -5.9   300     2327   02 34 41

 ---------- VLBA/EVN observing target during the VLA27 pointing  scan ----------

02 43 10  2230+114     21 35 30  66.9 141.4 -1.0     -33.3   168     2327   02 42 59
02 45 50  ---          21 38 10  67.2 142.8 -0.9     -32.1   160     2349   02 43 00

 ---------- VLBA+VLA27+EVN on source scans ----------

02 46 50  2230+114     21 39 10  67.4 143.3 -0.9     -31.7    54     2349   02 46 39
02 47 50  ---          21 40 10  67.5 143.9 -0.9     -31.2    60     2358   02 46 40

02 48 00  2230+114     21 40 20  67.5 144.0 -0.9     -31.1     4     2358   02 47 56
02 56 20  ---          21 48 42  68.5 148.8 -0.7     -27.1   500     2423   02 47 51

 ---------- VLBA scan on FF 3C454.3 in KUQ bands ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

02 56 50  2251+158     21 49 12  69.2 130.1 -1.1     -43.2     9     2423   02 56 41
02 57 50  ---          21 50 12  69.4 130.6 -1.1     -42.8    60     2432   02 56 40

02 58 00  2251+158     21 50 22  69.4 130.7 -1.1     -42.8     4     2432   02 57 56
03 03 00  ---          21 55 23  70.2 133.3 -1.0     -40.7   300     2471   02 57 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

03 03 30  2251+158     21 55 53  70.3 133.6 -1.0     -40.5    24     2471   03 03 19
03 04 30  ---          21 56 53  70.5 134.2 -1.0     -40.0    60     2480   03 03 20

03 04 40  2251+158     21 57 03  70.5 134.2 -1.0     -39.9     4     2480   03 04 36
03 11 40  ---          22 04 04  71.5 138.3 -0.8     -36.6   420     2535   03 04 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

03 12 10  2251+158     22 04 34  71.6 138.6 -0.8     -36.3    24     2535   03 11 59
03 13 10  ---          22 05 34  71.7 139.2 -0.8     -35.8    60     2544   03 12 00

03 13 20  2251+158     22 05 44  71.8 139.3 -0.8     -35.7     4     2544   03 13 16
03 19 20  ---          22 11 45  72.6 143.2 -0.7     -32.4   360     2591   03 13 11

 ---------- VLBA/EVN observing target during the VLA27 pointing  scan ----------

03 19 50  2230+114     22 12 16  70.6 164.2 -0.4     -13.8     7     2591   03 19 43
03 22 30  ---          22 14 56  70.7 166.2 -0.3     -12.1   160     2612   03 19 40

03 23 10  2230+114     22 15 36  70.7 166.7 -0.3     -11.7    34     2612   03 22 59
03 24 10  ---          22 16 36  70.8 167.4 -0.3     -11.1    60     2621   03 23 00

03 24 20  2230+114     22 16 46  70.8 167.5 -0.3     -11.0     4     2621   03 24 16
03 33 10  ---          22 25 38  71.1 174.1 -0.1      -5.2   530     2690   03 24 11

03 33 20  2230+114     22 25 48  71.1 174.2 -0.1      -5.1     4     2690   03 33 16
03 34 20  ---          22 26 48  71.1 175.0 -0.1      -4.4    60     2698   03 33 11

 ---------- K-band VLBI scans. Space segment 03: 2230+114 with VLA+VLBA+EVN+GB ----------

03 35 00  2230+114     22 27 28  71.1 175.5 -0.1      -4.0    34     2698   03 34 49
03 43 50  ---          22 36 19  71.2 182.2  0.0       1.9   530     2768   03 34 50

03 44 00  2230+114     22 36 29  71.2 182.3  0.1       2.0     4     2768   03 43 56
03 45 00  ---          22 37 30  71.2 183.1  0.1       2.7    60     2776   03 43 51

03 45 30  2230+114     22 38 00  71.2 183.4  0.1       3.0    24     2776   03 45 19
03 53 50  ---          22 46 21  70.9 189.7  0.2       8.5   500     2842   03 45 20

03 54 00  2230+114     22 46 31  70.9 189.8  0.2       8.6     4     2842   03 53 56
03 55 00  ---          22 47 31  70.9 190.6  0.2       9.3    60     2850   03 53 51

03 55 30  2230+114     22 48 01  70.9 191.0  0.2       9.6    24     2850   03 55 19
04 03 50  ---          22 56 23  70.5 197.0  0.4      14.9   500     2916   03 55 20

04 04 00  2230+114     22 56 33  70.4 197.1  0.4      15.0     4     2916   04 03 56
04 05 00  ---          22 57 33  70.4 197.8  0.4      15.6    60     2924   04 03 51

04 05 30  2230+114     22 58 03  70.3 198.2  0.4      15.9    24     2924   04 05 19
04 13 50  ---          23 06 24  69.7 203.8  0.5      20.8   500     2990   04 05 20
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

04 14 00  2230+114     23 06 34  69.7 204.0  0.6      20.9     4     2990   04 13 56
04 15 00  ---          23 07 35  69.6 204.6  0.6      21.5    60     2999   04 13 51

04 15 30  2230+114     23 08 05  69.5 204.9  0.6      21.8    24     2999   04 15 19
04 23 50  ---          23 16 26  68.7 210.2  0.7      26.2   500     3064   04 15 20

04 24 00  2230+114     23 16 36  68.7 210.3  0.7      26.3     4     3064   04 23 56
04 25 00  ---          23 17 36  68.6 210.9  0.7      26.8    60     3073   04 23 51

04 25 30  2230+114     23 18 06  68.5 211.2  0.7      27.1    24     3073   04 25 19
04 33 50  ---          23 26 28  67.5 216.0  0.9      31.1   500     3138   04 25 20

04 34 00  2230+114     23 26 38  67.5 216.1  0.9      31.2     4     3138   04 33 56
04 35 00  ---          23 27 38  67.4 216.6  0.9      31.6    60     3147   04 33 51

04 35 30  2230+114     23 28 08  67.3 216.9  0.9      31.8    24     3147   04 35 19
04 43 50  ---          23 36 29  66.2 221.2  1.1      35.4   500     3212   04 35 20

04 44 00  2230+114     23 36 39  66.2 221.3  1.1      35.4     4     3212   04 43 56
04 45 00  ---          23 37 40  66.0 221.8  1.1      35.8    60     3221   04 43 51

04 45 30  2230+114     23 38 10  66.0 222.0  1.1      36.0    24     3221   04 45 19
04 55 00  ---          23 47 41  64.5 226.4  1.2      39.5   570     3296   04 45 20

04 55 40  2230+114     23 48 21  64.4 226.7  1.2      39.8    34     3296   04 55 29
04 58 20  ---          23 51 02  64.0 227.9  1.3      40.7   160     3318   04 55 30

04 58 50  2230+114     23 51 32  63.9 228.1  1.3      40.8    24     3318   04 58 39
05 07 40  ---          00 00 23  62.5 231.6  1.4      43.6   530     3387   04 58 40

05 07 50  2230+114     00 00 33  62.4 231.7  1.5      43.6     4     3387   05 07 46
05 08 50  ---          00 01 33  62.3 232.1  1.5      43.9    60     3396   05 07 41

05 09 20  2230+114     00 02 04  62.2 232.3  1.5      44.0    24     3396   05 09 09
05 17 40  ---          00 10 25  60.7 235.3  1.6      46.3   500     3461   05 09 10

05 17 50  2230+114     00 10 35  60.7 235.3  1.6      46.3     4     3461   05 17 46
05 18 50  ---          00 11 35  60.5 235.7  1.6      46.6    60     3470   05 17 41

05 19 20  2230+114     00 12 05  60.4 235.8  1.6      46.7    24     3470   05 19 09
05 27 40  ---          00 20 27  58.9 238.6  1.8      48.6   500     3535   05 19 10

05 27 50  2230+114     00 20 37  58.9 238.6  1.8      48.6     4     3535   05 27 46
05 28 50  ---          00 21 37  58.7 238.9  1.8      48.9    60     3544   05 27 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

05 29 20  2230+114     00 22 07  58.6 239.1  1.8      49.0    24     3544   05 29 09
05 37 40  ---          00 30 28  57.1 241.6  2.0      50.6   500     3610   05 29 10

05 37 50  2230+114     00 30 38  57.0 241.6  2.0      50.7     4     3610   05 37 46
05 38 50  ---          00 31 38  56.8 241.9  2.0      50.9    60     3618   05 37 41

 ---------- Ground-only VLBA+VLA27  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

05 39 50  2230+114     00 32 39  56.6 242.2  2.0      51.0    54     3618   05 39 39
05 40 50  ---          00 33 39  56.4 242.5  2.0      51.2    60     3627   05 39 40

05 41 00  2230+114     00 33 49  56.4 242.5  2.0      51.2     4     3627   05 40 56
05 47 00  ---          00 39 50  55.3 244.1  2.1      52.3   360     3674   05 40 51

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

05 48 00  2230+114     00 40 50  55.1 244.4  2.1      52.4    54     3674   05 47 49
05 49 00  ---          00 41 50  54.9 244.7  2.1      52.6    60     3683   05 47 50

05 49 10  2230+114     00 42 00  54.8 244.7  2.1      52.6     4     3683   05 49 06
05 58 15  ---          00 51 07  53.0 247.0  2.3      54.0   545     3754   05 49 01

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

05 58 45  2230+114     00 51 37  53.0 247.1  2.3      54.1    24     3754   05 58 34
06 02 55  ---          00 55 47  52.1 248.1  2.4      54.6   250     3787   05 58 35

06 03 05  2230+114     00 55 57  52.1 248.1  2.4      54.7     4     3787   06 03 01
06 12 25  ---          01 05 19  50.2 250.2  2.5      55.8   560     3860   06 02 56

06 12 35  2230+114     01 05 29  50.2 250.2  2.5      55.8     4     3860   06 12 31
06 13 35  ---          01 06 29  50.0 250.4  2.6      55.9    60     3868   06 12 26

06 13 45  2230+114     01 06 39  49.9 250.5  2.6      55.9     4     3868   Stopped 
06 14 45  ---          01 07 39  49.7 250.7  2.6      56.1    60     3868           

06 15 15  2230+114     01 08 09  49.6 250.8  2.6      56.1    24     3868   06 15 04
06 24 45  ---          01 17 41  47.7 252.7  2.7      57.1   570     3943   06 15 05

06 25 45  2136+141     01 18 41  37.5 264.9  3.6      62.3    32     3943   06 25 34
06 26 45  ---          01 19 41  37.3 265.1  3.7      62.3    60     3952   06 25 35
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

06 27 15  2136+141     01 20 11  37.2 265.2  3.7      62.3    24     3952   06 27 04
06 32 15  ---          01 25 12  36.1 265.9  3.8      62.4   300     3992   06 27 05

06 33 15  2230+114     01 26 12  45.9 254.4  2.9      57.8    32     3992   06 33 04
06 34 15  ---          01 27 12  45.7 254.6  2.9      57.9    60     4001   06 33 05

06 34 25  2230+114     01 27 22  45.7 254.6  2.9      57.9     4     4001   06 34 21
06 43 55  ---          01 36 54  43.7 256.3  3.1      58.7   570     4075   06 34 16

 ---------- Ground-only VLBA+VLA27  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

06 44 55  2230+114     01 37 54  43.5 256.5  3.1      58.7    54     4075   06 44 44
06 45 55  ---          01 38 54  43.3 256.7  3.1      58.8    60     4084   06 44 45

06 46 05  2230+114     01 39 04  43.2 256.7  3.1      58.8     4     4084   06 46 01
06 52 40  ---          01 45 40  41.9 257.8  3.2      59.2   395     4136   06 45 56

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

06 53 40  2230+114     01 46 41  41.6 258.0  3.2      59.3    54     4136   06 53 29
06 54 40  ---          01 47 41  41.4 258.2  3.2      59.4    60     4145   06 53 30

06 54 50  2230+114     01 47 51  41.4 258.2  3.2      59.4     4     4145   06 54 46
07 07 00  ---          02 00 03  38.8 260.2  3.4      60.0   730     4240   06 54 41

 ---------- VLBA observing during the VLA27 pointing  scan ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

07 07 00  2230+114     02 00 03  38.8 260.2  3.4      60.0    -6     4240   07 07 06
07 09 40  ---          02 02 43  38.3 260.6  3.5      60.1   154     4259   07 07 01

 ----------  All ground stations in  K-band  on target source ----------

07 10 10  2230+114     02 03 13  38.2 260.7  3.5      60.2    24     4259   07 09 59
07 11 10  ---          02 04 14  37.9 260.8  3.5      60.2    60     4269   07 10 00

07 11 20  2230+114     02 04 24  37.9 260.8  3.5      60.2     4     4269   07 11 16
07 21 20  ---          02 14 25  35.8 262.3  3.7      60.6   600     4346   07 11 11
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

 ---------- Ground-only VLBA+VLA  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 22 20  2230+114     02 15 25  35.6 262.5  3.7      60.6    54     4346   07 22 09
07 23 20  ---          02 16 26  35.3 262.6  3.7      60.7    60     4356   07 22 10

07 23 30  2230+114     02 16 36  35.3 262.7  3.7      60.7     4     4356   07 23 26
07 30 05  ---          02 23 12  33.9 263.6  3.8      60.9   395     4407   07 23 21

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

07 31 05  2230+114     02 24 12  33.7 263.8  3.8      60.9    54     4407   07 30 54
07 32 05  ---          02 25 12  33.5 263.9  3.9      60.9    60     4416   07 30 55

07 32 15  2230+114     02 25 22  33.4 263.9  3.9      60.9     4     4416   07 32 11
07 41 20  ---          02 34 28  31.5 265.2  4.0      61.2   545     4487   07 32 06

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

07 41 50  2230+114     02 34 59  31.4 265.3  4.0      61.2    24     4487   07 41 39
07 44 30  ---          02 37 39  30.8 265.6  4.1      61.2   160     4509   07 41 40

 ----------  All ground stations in  K-band  on target source ----------

07 44 40  2230+114     02 37 49  30.8 265.7  4.1      61.2     4     4509   07 44 36
07 45 40  ---          02 38 49  30.5 265.8  4.1      61.2    60     4517   07 44 31

07 45 50  2230+114     02 38 59  30.5 265.8  4.1      61.3     4     4517   07 45 46
07 53 00  ---          02 46 10  29.0 266.8  4.2      61.4   430     4573   07 45 41

 ---------- Ground-only VLBA+VLA27  U,Q-band scans on target source ----------

 Next scan frequencies:  15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
 Next BBC frequencies:     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00

07 54 00  2230+114     02 47 11  28.8 266.9  4.2      61.4    54     4573   07 53 49
07 55 00  ---          02 48 11  28.5 267.1  4.2      61.4    60     4582   07 53 50

07 55 10  2230+114     02 48 21  28.5 267.1  4.2      61.4     4     4582   07 55 06
08 01 45  ---          02 54 57  27.1 268.0  4.4      61.5   395     4633   07 55 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

 Next scan frequencies:  43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
 Next BBC frequencies:     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00

08 02 45  2230+114     02 55 57  26.9 268.1  4.4      61.5    54     4633   08 02 34
08 03 45  ---          02 56 57  26.7 268.2  4.4      61.5    60     4643   08 02 35

08 03 55  2230+114     02 57 07  26.6 268.3  4.4      61.5     4     4643   08 03 51
08 13 00  ---          03 06 14  24.7 269.4  4.5      61.5   545     4713   08 03 46

 ----------  All ground stations in  K-band  on target source ----------

 Next scan frequencies:  22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
 Next BBC frequencies:     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00

08 13 30  2230+114     03 06 44  24.6 269.5  4.6      61.5    24     4713   08 13 19
08 14 30  ---          03 07 44  24.3 269.6  4.6      61.5    60     4723   08 13 20

08 14 40  2230+114     03 07 54  24.3 269.6  4.6      61.5     4     4723   08 14 36
08 23 00  ---          03 16 15  22.5 270.7  4.7      61.5   500     4787   08 14 31

08 23 30  2230+114     03 16 45  22.4 270.8  4.7      61.5    24     4787   08 23 19
08 24 30  ---          03 17 46  22.2 270.9  4.7      61.5    60     4797   08 23 20

08 24 40  2230+114     03 17 56  22.1 270.9  4.7      61.5     4     4797   08 24 36
08 33 00  ---          03 26 17  20.3 272.0  4.9      61.5   500     4862   08 24 31

08 34 20  2230+114     03 27 37  20.1 272.1  4.9      61.5    74     4862   08 34 09
08 37 30  ---          03 30 48  19.4 272.5  5.0      61.4   190     4887   08 34 10

08 38 30  2230+114     03 31 48  19.2 272.7  5.0      61.4    54     4887   08 38 19
08 39 30  ---          03 32 48  18.9 272.8  5.0      61.4    60     4897   08 38 20

 ---------- K-band VLBI scans. Space segment 04: 2230+114 with Y27(-9:00)+VLBA+LBA+KVN+Sh ----------

08 40 00  2230+114     03 33 18  18.8 272.8  5.0      61.4    24     4897   08 39 49
08 48 50  ---          03 42 10  16.9 273.9  5.1      61.3   530     4966   08 39 50

08 49 00  2230+114     03 42 20  16.9 274.0  5.1      61.3     4     4966   08 48 56
08 50 00  ---          03 43 20  16.7 274.1  5.2      61.3    60     4974   08 48 51

08 50 30  2230+114     03 43 50  16.6 274.1  5.2      61.3    24     4974   08 50 19
08 58 50  ---          03 52 11  14.8 275.2  5.3      61.1   500     5040   08 50 20

08 59 00  2230+114     03 52 21  14.7 275.2  5.3      61.1     4     5040   08 58 56
09 00 00  ---          03 53 21  14.5 275.3  5.3      61.1    60     5049   08 58 51
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  18 Oct 2016   Day 292 ---

09 00 30  2230+114     03 53 51  14.4 275.4  5.3      61.1    24     5049   09 00 19
09 08 50  ---          04 02 13  12.6 276.4  5.5      60.9   500     5114   09 00 20

09 09 00  2230+114     04 02 23  12.6 276.4  5.5      60.9     4     5114   09 08 56
09 10 00  ---          04 03 23  12.4 276.5  5.5      60.9    60     5123   09 08 51

09 10 30  2230+114     04 03 53  12.3 276.6  5.5      60.8    24     5123   09 10 19
09 18 50  ---          04 12 15  10.5 277.6  5.6      60.6   500     5188   09 10 20

09 19 00  2230+114     04 12 25  10.5 277.6  5.6      60.6     4     5188   09 18 56
09 20 00  ---          04 13 25  10.2 277.8  5.7      60.6    60     5197   09 18 51

09 20 30  2230+114     04 13 55  10.1 277.8  5.7      60.6    24     5197   09 20 19
09 28 50  ---          04 22 16   8.4 278.8  5.8      60.3   500     5263   09 20 20

09 29 00  2230+114     04 22 26   8.3 278.9  5.8      60.3     4     5263   09 28 56
09 30 00  ---          04 23 26   8.1 279.0  5.8      60.3    60     5271   09 28 51

09 30 30  2230+114     04 23 56   8.0 279.0  5.8      60.2    24     5271   09 30 19
09 38 50  ---          04 32 18   6.2 280.1  6.0      59.9   500     5337   09 30 20

09 39 00  2230+114     04 32 28   6.2 280.1  6.0      59.9     4     5337   09 38 56
09 40 00  ---          04 33 28   6.0 280.2  6.0      59.9    60     5345   09 38 51

09 40 30  2230+114     04 33 58   5.9 280.3  6.0      59.9    24     5345   09 40 19
09 48 50  ---          04 42 19   4.1 281.3  6.1      59.5   500     5411   09 40 20

09 49 00  2230+114     04 42 29   4.1 281.3  6.2      59.5     4     5411   09 48 56
09 50 00  ---          04 43 30   3.9 281.5  6.2      59.5    60     5419   09 48 51

09 50 30  2230+114     04 44 00   3.8 281.5  6.2      59.5    24     5419   09 50 19
09 58 50  ---          04 52 21   2.0 282.6  6.3  D   59.1     0     5485   09 50 20


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg081b_freq.dat:
     v1cm_b3

   Setup group:    8         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  20  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22220.00  22220.00  22252.00  22252.00  22284.00  22284.00  22316.00  22316.00
   BBC fr=     720.00    720.00    752.00    752.00    784.00    784.00    816.00    816.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     759.99    759.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  20  21  22  23  24  25  26  27  28  55

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg081b_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   46         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  35  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15337.00  15337.00  15369.00  15369.00  15401.00  15401.00  15433.00  15433.00
   BBC fr=     737.00    737.00    769.00    769.00    801.00    801.00    833.00    833.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     776.99    776.99    808.99    808.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  35  36  37  38  39  40  41  42  43  56

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg081b_freq.dat:
     v7mm_c8

   Setup group:   59         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  46  Setup file default.  Used with PCAL = off
   LO sum=   43114.00  43114.00  43146.00  43146.00  43178.00  43178.00  43210.00  43210.00
   BBC fr=     714.00    714.00    746.00    746.00    778.00    778.00    810.00    810.00
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     754.00    754.00    786.00    786.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  46  47  48  49  50  51  52  53  54  57

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 31.676268       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 18.22736        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 52.609697       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 34.41572        0.00
 * 3C286             ./gg081b_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati

 * 0316+413          03 16 29.567283   * 03 19 48.160114     03 20 56.362032       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 10.36045        0.00
   3C84              ./gg081b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

 * 0748+126          07 48 05.060493   * 07 50 52.045731     07 51 47.529372       0.00
   J0750+1231        12 38 45.47747    * 12 31 04.82815      12 28 24.72088        0.00
                     ./gg081b_sources.radioastron
                     AGN, MASIV, rfc_2013d Petrov, 2013, unpublished 26051 observations, RA-AO3-04, R

 * 1921-293          19 21 42.234129   * 19 24 51.055956     19 25 53.565583       0.00
   J1924-2914       -29 20 26.35404    *-29 14 30.12114     -29 12 23.78367        0.00
                     ./gg081b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 45960 observations, RA-AO3-04, RA-AO2-1

 * 2136+141          21 36 37.412147   * 21 39 01.309269     21 39 49.929363       0.00
   J2139+1423        14 10 00.62094    * 14 23 35.99209      14 28 25.01652        0.00
                     ./gg081b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 52968 observations, RA-AO3-04, RA-AO2-1

 * 2230+114          22 30 07.803947   * 22 32 36.408905     22 33 26.843297       0.00
   J2232+1143        11 28 22.81067    * 11 43 50.90395      11 49 14.08660        0.00
   CTA102            ./gg081b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 5100 observations, RA-AO3-04, RA-AO2-12

 * 2251+158          22 51 29.519741   * 22 53 57.747940     22 54 48.229805       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 14 26.76997        0.00
   3C454.3           ./gg081b_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO3-04, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            18                                5.258     0.000
  3C286      ra1cm2.set            29                                0.292     0.000
             ra2cm2.set            31                                0.258     0.000
             ra7mm2.set            30                                0.362     0.000
  0316+413   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 19 33        0.500    32.555
  0748+126   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 33           5.306   182.989
  1921-293   ra1cm2.set            62 63 64 65                       0.114     0.683
  2136+141   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 13 14  +     0.483    52.186
  2230+114   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 13 14  +    15.356  1568.299
             ra6cm2.set            66 67 68 69                       0.336     2.017
             ra2cm2.set            31 34 35                          1.001    52.798
             ra7mm2.set            30 44 45 46 58 59                 1.396    99.330
  2251+158   ra1cm2.set            1 2 3 4 5 6 7 8 9 10 13 14  +     0.200    18.999
             ra2cm2.set            31 35                             0.100     5.500
             ra7mm2.set            30 46                             0.133     7.333


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              95.0
   3C286               40.1
   0316+413           140.3
   0748+126            87.6
   1921-293            83.7
   2136+141           122.9
   2230+114           135.9
   2251+158           141.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

