  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Confirming the detection of a dark matter substructure with Global VLBI
 Exp. Code:  gs038a  


Schedule Version:       2.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Cristiana Spingola

Address:  University of Groningen - Kapteyn Astronomical Institute
          Landleven 12
          9747AD Groningen
          the Netherlands

Phone:    +31 633380186
EMAIL:    spingola@astro.rug.nl
Fax:
Phone during observation:

Observing mode: 18cm 2048-8-2

Notes:
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

 Next scan frequencies:  1504.25  1504.25  1568.25  1568.25  1632.25  1632.25  1696.25  1696.25
 Next BBC frequencies:    895.75   895.75   831.75   831.75   767.75   767.75   703.75   703.75
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

10 30 00  J0720+473    06 10 55  68.3  33.6 -1.2    -135.1     0        0   10 30 00
10 33 00  ---          06 13 55  68.7  32.6 -1.1    -136.5   180       46   10 30 01

10 33 00  B0712+472    06 13 55  69.5  32.0 -1.1    -137.9   -10       46   10 33 10
10 36 30  ---          06 17 26  69.9  30.8 -1.0    -139.7   200       98   10 33 01

10 37 00  J0720+473    06 17 56  69.1  31.2 -1.1    -138.6    20       98   10 37 00
10 38 30  ---          06 19 26  69.3  30.7 -1.0    -139.3    90      121   10 37 01

10 38 30  B0712+472    06 19 26  70.1  30.0 -1.0    -140.8   -10      121   10 38 40
10 42 00  ---          06 22 57  70.5  28.6 -0.9    -142.8   200      173   10 38 31

10 42 30  J0720+473    06 23 27  69.7  29.2 -1.0    -141.5    20      173   10 42 30
10 44 00  ---          06 24 57  69.9  28.6 -0.9    -142.3    90      196   10 42 31

10 44 00  B0712+472    06 24 57  70.7  27.8 -0.9    -143.9   -10      196   10 44 10
10 47 30  ---          06 28 28  71.0  26.3 -0.8    -146.0   200      247   10 44 01

10 48 00  J0720+473    06 28 58  70.3  27.1 -0.9    -144.5    20      247   10 48 00
10 49 30  ---          06 30 28  70.4  26.4 -0.9    -145.4    90      271   10 48 01

10 49 30  B0712+472    06 30 28  71.2  25.4 -0.8    -147.2   -10      271   10 49 40
10 53 00  ---          06 33 59  71.5  23.8 -0.7    -149.3   200      322   10 49 31

10 53 30  J0720+473    06 34 29  70.8  24.7 -0.8    -147.7    20      322   10 53 30
10 55 00  ---          06 35 59  70.9  24.1 -0.8    -148.6    90      345   10 53 31

10 55 00  B0712+472    06 35 59  71.7  22.9 -0.7    -150.6   -10      345   10 55 10
10 58 30  ---          06 39 30  72.0  21.2 -0.6    -152.8   200      397   10 55 01

10 59 00  J0720+473    06 40 00  71.3  22.3 -0.7    -151.1    21      397   10 59 00
11 00 30  ---          06 41 30  71.4  21.6 -0.7    -152.0    90      420   10 59 01

11 00 30  B0712+472    06 41 30  72.1  20.2 -0.6    -154.1    -9      420   11 00 39
11 04 00  ---          06 45 00  72.4  18.4 -0.5    -156.5   201      472   11 00 31

11 04 30  J0720+473    06 45 31  71.7  19.7 -0.6    -154.6    21      472   11 04 30
11 06 00  ---          06 47 01  71.8  18.9 -0.6    -155.5    90      495   11 04 31

11 11 00  DA193        06 52 02  75.5 -47.1  0.9     124.9   247      495   11 11 00
11 20 00  ---          07 01 03  74.0 -50.6  1.1     120.0   540      634   11 11 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

11 20 00  J0720+473    07 01 03  72.6  11.6 -0.3    -165.1   -52      634   11 20 52
11 24 30  ---          07 05 34  72.8   9.2 -0.3    -168.3   218      690   11 20 01

11 24 30  B0712+472    07 05 34  73.4   7.0 -0.2    -171.1    -9      690   11 24 39
11 28 00  ---          07 09 04  73.4   4.9 -0.1    -173.8   201      742   11 24 31

11 28 30  J0720+473    07 09 34  72.9   6.9 -0.2    -171.2    21      742   11 28 30
11 30 00  ---          07 11 05  72.9   6.1 -0.2    -172.3    90      765   11 28 31

11 30 00  B0712+472    07 11 05  73.5   3.7 -0.1    -175.3   -10      765   11 30 10
11 33 30  ---          07 14 35  73.5   1.6 -0.0    -177.9   200      817   11 30 01

11 34 00  J0720+473    07 15 05  73.0   3.8 -0.1    -175.2    20      817   11 34 00
11 35 30  ---          07 16 36  73.0   2.9 -0.1    -176.3    90      840   11 34 01

11 35 30  B0712+472    07 16 36  73.5   0.4 -0.0    -179.5   -10      840   11 35 40
11 39 00  ---          07 20 06  73.5  -1.7  0.0     177.9   200      891   11 35 31

11 39 30  J0720+473    07 20 36  73.0   0.6 -0.0    -179.3    20      891   11 39 30
11 41 00  ---          07 22 07  73.0  -0.3  0.0     179.6    90      915   11 39 31

11 41 00  B0712+472    07 22 07  73.5  -2.9  0.1     176.4   -10      915   11 41 10
11 44 30  ---          07 25 37  73.4  -5.0  0.1     173.7   200      966   11 41 01

11 45 00  J0720+473    07 26 07  73.0  -2.6  0.1     176.7    20      966   11 45 00
11 46 30  ---          07 27 37  73.0  -3.5  0.1     175.6    90      989   11 45 01

11 46 30  B0712+472    07 27 37  73.4  -6.2  0.2     172.2   -10      989   11 46 40
11 50 00  ---          07 31 08  73.3  -8.2  0.2     169.6   200     1041   11 46 31

11 50 30  J0720+473    07 31 38  72.9  -5.8  0.2     172.6    20     1041   11 50 30
11 52 00  ---          07 33 08  72.9  -6.6  0.2     171.5    90     1064   11 50 31

11 52 00  B0712+472    07 33 08  73.2  -9.4  0.3     168.1   -10     1064   11 52 10
11 55 30  ---          07 36 39  73.1 -11.4  0.3     165.5   200     1116   11 52 01

11 56 00  J0720+473    07 37 09  72.8  -8.9  0.3     168.6    20     1116   11 56 00
11 57 30  ---          07 38 39  72.7  -9.7  0.3     167.6    90     1139   11 56 01

11 57 30  B0712+472    07 38 39  73.0 -12.5  0.4     164.1   -10     1139   11 57 40
12 01 00  ---          07 42 10  72.8 -14.5  0.4     161.6   200     1190   11 57 31

12 01 30  J0720+473    07 42 40  72.6 -11.9  0.4     164.7    20     1190   12 01 30
12 03 00  ---          07 44 10  72.5 -12.7  0.4     163.7    90     1213   12 01 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

12 03 00  B0712+472    07 44 10  72.7 -15.6  0.4     160.2   -10     1213   12 03 10
12 06 30  ---          07 47 41  72.5 -17.4  0.5     157.8   200     1265   12 03 01

12 07 00  J0720+473    07 48 11  72.3 -14.9  0.4     160.9    20     1265   12 07 00
12 08 30  ---          07 49 41  72.2 -15.7  0.5     159.9    90     1288   12 07 01

12 08 30  B0712+472    07 49 41  72.4 -18.5  0.5     156.4   -10     1288   12 08 40
12 12 00  ---          07 53 12  72.1 -20.2  0.6     154.1   200     1340   12 08 31

12 12 30  J0720+473    07 53 42  72.0 -17.7  0.5     157.2    20     1340   12 12 30
12 14 00  ---          07 55 12  71.9 -18.4  0.6     156.2    90     1363   12 12 31

12 14 00  B0712+472    07 55 12  72.0 -21.2  0.6     152.8   -10     1363   12 14 10
12 17 30  ---          07 58 43  71.7 -22.9  0.7     150.5   200     1414   12 14 01

12 18 00  J0720+473    07 59 13  71.6 -20.4  0.6     153.6    20     1414   12 18 00
12 19 30  ---          08 00 43  71.5 -21.1  0.7     152.6    90     1438   12 18 01

12 19 30  B0712+472    08 00 43  71.5 -23.9  0.7     149.3   -10     1438   12 19 40
12 23 00  ---          08 04 13  71.2 -25.4  0.8     147.1   200     1489   12 19 31

12 23 30  J0720+473    08 04 44  71.1 -23.0  0.7     150.1    20     1489   12 23 30
12 25 00  ---          08 06 14  71.0 -23.6  0.7     149.2    90     1512   12 23 31

12 25 00  B0712+472    08 06 14  71.0 -26.3  0.8     145.9   -10     1512   12 25 10
12 28 30  ---          08 09 44  70.7 -27.8  0.9     143.9   200     1564   12 25 01

12 29 00  J0720+473    08 10 14  70.6 -25.4  0.8     146.8    20     1564   12 29 00
12 30 30  ---          08 11 45  70.5 -26.0  0.8     146.0    90     1587   12 29 01

12 35 30  4C39.25      08 16 45  73.2  55.5 -1.2    -114.3   233     1587   12 35 30
12 42 30  ---          08 23 47  74.4  53.3 -1.1    -117.4   420     1695   12 35 31

12 42 30  B0712+472    08 23 47  69.1 -33.1  1.1     136.3   -70     1695   12 43 40
12 46 00  ---          08 27 17  68.7 -34.3  1.2     134.5   140     1731   12 42 31

12 46 30  J0720+473    08 27 47  68.8 -32.1  1.1     137.3    20     1731   12 46 30
12 48 00  ---          08 29 18  68.7 -32.6  1.1     136.5    90     1755   12 46 31

12 48 00  B0712+472    08 29 18  68.5 -35.0  1.2     133.6   -10     1755   12 48 10
12 51 30  ---          08 32 48  68.0 -36.1  1.3     131.9   200     1806   12 48 01

12 52 00  J0720+473    08 33 18  68.2 -33.9  1.2     134.6    21     1806   12 52 00
12 53 30  ---          08 34 48  68.0 -34.4  1.2     133.8    90     1829   12 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

12 53 30  B0712+472    08 34 48  67.8 -36.7  1.3     131.0    -9     1829   12 53 39
12 57 00  ---          08 38 19  67.3 -37.7  1.4     129.4   201     1881   12 53 31

12 57 30  J0720+473    08 38 49  67.5 -35.6  1.3     132.0    21     1881   12 57 30
12 59 00  ---          08 40 19  67.3 -36.1  1.3     131.3    90     1904   12 57 31

12 59 00  B0712+472    08 40 19  67.1 -38.2  1.4     128.5    -9     1904   12 59 09
13 02 30  ---          08 43 50  66.6 -39.2  1.4     127.0   201     1956   12 59 01

13 03 00  J0720+473    08 44 20  66.8 -37.2  1.4     129.5    21     1956   13 03 00
13 04 30  ---          08 45 50  66.6 -37.6  1.4     128.9    90     1979   13 03 01

13 04 30  B0712+472    08 45 50  66.3 -39.7  1.5     126.2    -9     1979   13 04 39
13 08 00  ---          08 49 21  65.8 -40.5  1.5     124.8   201     2031   13 04 31

13 08 30  J0720+473    08 49 51  66.1 -38.6  1.5     127.2    21     2031   13 08 30
13 10 00  ---          08 51 21  65.9 -39.0  1.5     126.6    90     2054   13 08 31

13 10 00  B0712+472    08 51 21  65.5 -41.0  1.6     124.0    -9     2054   13 10 09
13 13 30  ---          08 54 52  65.0 -41.8  1.6     122.6   201     2106   13 10 01

13 14 00  J0720+473    08 55 22  65.3 -40.0  1.6     125.0    21     2106   13 14 00
13 15 30  ---          08 56 52  65.1 -40.3  1.6     124.4    90     2129   13 14 01

13 15 30  B0712+472    08 56 52  64.8 -42.2  1.7     121.9    -9     2129   13 15 39
13 19 00  ---          09 00 23  64.3 -42.9  1.7     120.6   201     2181   13 15 31

13 19 30  J0720+473    09 00 53  64.5 -41.2  1.7     122.8    21     2181   13 19 30
13 21 00  ---          09 02 23  64.3 -41.5  1.7     122.3    90     2204   13 19 31

13 21 00  B0712+472    09 02 23  64.0 -43.3  1.8     119.8    -9     2204   13 21 09
13 24 30  ---          09 05 54  63.4 -44.0  1.8     118.6   201     2256   13 21 01

13 25 00  J0720+473    09 06 24  63.8 -42.3  1.7     120.8    21     2256   13 25 00
13 26 30  ---          09 07 54  63.5 -42.6  1.8     120.3    90     2279   13 25 01

13 26 30  B0712+472    09 07 54  63.1 -44.3  1.8     117.9    -9     2279   13 26 39
13 30 00  ---          09 11 24  62.6 -44.9  1.9     116.7   201     2331   13 26 31

13 30 30  J0720+473    09 11 55  62.9 -43.4  1.8     118.9    21     2331   13 30 30
13 32 00  ---          09 13 25  62.7 -43.6  1.9     118.3    90     2354   13 30 31

13 32 00  B0712+472    09 13 25  62.3 -45.3  1.9     116.1    -9     2354   13 32 09
13 35 30  ---          09 16 55  61.8 -45.8  2.0     115.0   201     2406   13 32 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

13 36 00  J0720+473    09 17 25  62.1 -44.3  1.9     117.0    21     2406   13 36 00
13 37 30  ---          09 18 56  61.9 -44.5  2.0     116.5    90     2429   13 36 01

13 37 30  B0712+472    09 18 56  61.4 -46.1  2.0     114.3    -9     2429   13 37 39
13 41 00  ---          09 22 26  60.9 -46.6  2.1     113.3   201     2481   13 37 31

13 41 30  J0720+473    09 22 56  61.3 -45.2  2.0     115.2    21     2481   13 41 30
13 43 00  ---          09 24 27  61.1 -45.4  2.0     114.7    90     2504   13 41 31

13 43 00  B0712+472    09 24 27  60.6 -46.9  2.1     112.6    -9     2504   13 43 09
13 46 30  ---          09 27 57  60.0 -47.3  2.2     111.6   201     2556   13 43 01

13 47 00  J0720+473    09 28 27  60.4 -45.9  2.1     113.5    21     2556   13 47 00
13 48 30  ---          09 29 57  60.2 -46.2  2.1     113.1    90     2579   13 47 01

13 48 30  B0712+472    09 29 57  59.7 -47.6  2.2     111.0    -9     2579   13 48 39
13 52 00  ---          09 33 28  59.2 -48.0  2.3     110.0   201     2631   13 48 31

13 52 30  J0720+473    09 33 58  59.6 -46.7  2.2     111.9    21     2631   13 52 30
13 55 00  ---          09 36 29  59.2 -47.0  2.2     111.1   150     2669   13 52 31

14 00 00  DA193        09 41 29  43.9 -62.4  3.7      83.2   264     2669   14 00 00
14 10 00  ---          09 51 31  42.0 -62.1  3.9      81.9   600     2824   14 00 01

14 10 00  J0720+473    09 51 31  56.8 -48.5  2.5     107.0   -37     2824   14 10 37
14 14 00  ---          09 55 32  56.1 -48.9  2.6     106.0   203     2876   14 10 01

14 14 00  B0712+472    09 55 32  55.6 -50.0  2.6     104.3    -9     2876   14 14 09
14 17 30  ---          09 59 02  55.0 -50.3  2.7     103.4   201     2928   14 14 01

14 18 00  J0720+473    09 59 32  55.5 -49.2  2.6     105.0    21     2928   14 18 00
14 19 30  ---          10 01 03  55.3 -49.3  2.7     104.6    90     2951   14 18 01

14 19 30  B0712+472    10 01 03  54.7 -50.4  2.7     102.9    -9     2951   14 19 39
14 23 00  ---          10 04 33  54.1 -50.7  2.8     102.1   201     3003   14 19 31

14 23 30  J0720+473    10 05 03  54.6 -49.6  2.7     103.7    21     3003   14 23 30
14 25 00  ---          10 06 33  54.4 -49.7  2.7     103.3    90     3026   14 23 31

14 25 00  B0712+472    10 06 33  53.7 -50.8  2.8     101.6    -9     3026   14 25 09
14 28 30  ---          10 10 04  53.2 -51.0  2.9     100.8   201     3078   14 25 01

14 29 00  J0720+473    10 10 34  53.7 -50.0  2.8     102.4    21     3078   14 29 00
14 31 00  ---          10 12 34  53.4 -50.1  2.8     101.9   120     3109   14 29 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

14 31 00  B0712+472    10 12 34  52.7 -51.1  2.9     100.3    -9     3109   14 31 09
14 34 30  ---          10 16 05  52.1 -51.3  3.0      99.5   201     3161   14 31 01

14 35 00  J0720+473    10 16 35  52.7 -50.3  2.9     101.0    21     3161   14 35 00
14 36 30  ---          10 18 05  52.4 -50.4  2.9     100.6    90     3184   14 35 01

14 36 30  B0712+472    10 18 05  51.8 -51.4  3.0      99.1    -9     3184   14 36 39
14 40 00  ---          10 21 36  51.2 -51.5  3.1      98.3   201     3236   14 36 31

14 40 30  J0720+473    10 22 06  51.8 -50.6  3.0      99.7    21     3236   14 40 30
14 42 00  ---          10 23 36  51.5 -50.6  3.0      99.4    90     3259   14 40 31

14 42 00  B0712+472    10 23 36  50.9 -51.6  3.1      97.9    -9     3259   14 42 09
14 44 30  ---          10 26 07  50.5 -51.7  3.1      97.4   141     3295   14 42 01

14 44 30  J0720+473    10 26 07  51.1 -50.8  3.1      98.9    -9     3295   14 44 39
14 46 30  ---          10 28 07  50.8 -50.8  3.1      98.4   111     3324   14 44 31

14 46 30  B0712+472    10 28 07  50.1 -51.7  3.2      96.9    -9     3324   14 46 39
14 50 00  ---          10 31 38  49.5 -51.8  3.2      96.2   201     3376   14 46 31

14 50 30  J0720+473    10 32 08  50.1 -51.0  3.2      97.6    21     3376   14 50 30
14 52 00  ---          10 33 38  49.9 -51.0  3.2      97.3    90     3399   14 50 31

14 52 00  B0712+472    10 33 38  49.2 -51.9  3.3      95.8    -9     3399   14 52 09
14 55 30  ---          10 37 08  48.6 -52.0  3.3      95.1   201     3451   14 52 01

14 56 00  J0720+473    10 37 39  49.2 -51.2  3.3      96.4    21     3451   14 56 00
14 57 30  ---          10 39 09  48.9 -51.2  3.3      96.1    90     3474   14 56 01

14 57 30  B0712+472    10 39 09  48.3 -52.0  3.4      94.7    -9     3474   14 57 39
15 00 30  ---          10 42 09  47.7 -52.1  3.4      94.1   171     3518   14 57 31

15 01 00  J0720+473    10 42 39  48.3 -51.3  3.4      95.4    21     3518   15 01 00
15 02 00  ---          10 43 40  48.2 -51.3  3.4      95.2    60     3533   15 01 01

15 07 00  4C39.25      10 48 40  71.5 -57.7  1.3     110.7   245     3533   15 07 00
15 17 00  ---          10 58 42  69.7 -59.6  1.5     107.3   600     3688   15 07 01

15 17 00  J0720+473    10 58 42  45.6 -51.6  3.6      92.2   -56     3688   15 17 56
15 18 30  ---          11 00 12  45.4 -51.6  3.6      92.0    34     3697   15 17 01

15 18 30  B0712+472    11 00 12  44.7 -52.3  3.7      90.7    -9     3697   15 18 39
15 23 00  ---          11 04 43  43.9 -52.3  3.8      89.8   261     3764   15 18 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

15 23 30  J0720+473    11 05 13  44.6 -51.6  3.7      91.0    21     3764   15 23 30
15 25 00  ---          11 06 43  44.3 -51.6  3.8      90.7    90     3787   15 23 31

15 25 00  B0712+472    11 06 43  43.6 -52.3  3.8      89.5    -9     3787   15 25 09
15 28 30  ---          11 10 14  43.0 -52.3  3.9      88.8   201     3839   15 25 01

15 29 00  J0720+473    11 10 44  43.6 -51.6  3.8      90.0    21     3839   15 29 00
15 30 30  ---          11 12 14  43.4 -51.6  3.8      89.7    90     3862   15 29 01

15 30 30  B0712+472    11 12 14  42.6 -52.2  3.9      88.5    -9     3862   15 30 39
15 34 00  ---          11 15 45  42.0 -52.2  4.0      87.8   201     3914   15 30 31

15 34 30  J0720+473    11 16 15  42.7 -51.6  3.9      89.0    21     3914   15 34 30
15 36 00  ---          11 17 45  42.4 -51.6  3.9      88.7    90     3937   15 34 31

15 36 00  B0712+472    11 17 45  41.7 -52.2  4.0      87.5    -9     3937   15 36 09
15 39 30  ---          11 21 16  41.1 -52.2  4.1      86.9   201     3989   15 36 01

15 40 00  J0720+473    11 21 46  41.8 -51.6  4.0      88.0    21     3989   15 40 00
15 41 30  ---          11 23 16  41.5 -51.6  4.0      87.7    90     4012   15 40 01

15 41 30  B0712+472    11 23 16  40.8 -52.1  4.1      86.5    -9     4012   15 41 39
15 45 00  ---          11 26 47  40.2 -52.1  4.2      85.9   201     4064   15 41 31

15 45 30  J0720+473    11 27 17  40.8 -51.5  4.1      87.0    21     4064   15 45 30
15 47 00  ---          11 28 47  40.6 -51.5  4.1      86.7    90     4087   15 45 31

15 47 00  B0712+472    11 28 47  39.8 -52.1  4.2      85.6   -10     4087   15 47 10
15 50 30  ---          11 32 18  39.2 -52.0  4.2      85.0   200     4138   15 47 01

15 51 00  J0720+473    11 32 48  39.9 -51.4  4.2      86.0    21     4138   15 51 00
15 52 30  ---          11 34 18  39.7 -51.4  4.2      85.8    90     4162   15 51 01

15 52 30  B0712+472    11 34 18  38.9 -52.0  4.3      84.6   -10     4162   15 52 40
15 56 00  ---          11 37 48  38.3 -51.9  4.3      84.0   200     4213   15 52 31

15 56 30  J0720+473    11 38 18  39.0 -51.3  4.3      85.1    21     4213   15 56 30
15 58 00  ---          11 39 49  38.7 -51.3  4.3      84.8    90     4236   15 56 31

16 03 00  DA193        11 44 50  21.1 -55.3  5.8      67.1   259     4236   16 03 00
16 11 00  ---          11 52 51  19.7 -54.7  5.9      66.0   480     4360   16 03 01

16 11 00  B0712+472    11 52 51  35.8 -51.5  4.6      81.5   -39     4360   16 11 39
16 14 30  ---          11 56 21  35.2 -51.4  4.7      80.9   171     4404   16 11 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

16 15 00  J0720+473    11 56 52  35.9 -50.9  4.6      81.9    20     4404   16 15 00
16 16 30  ---          11 58 22  35.6 -50.9  4.6      81.7    90     4427   16 15 01

16 16 30  B0712+472    11 58 22  34.8 -51.3  4.7      80.6   -10     4427   16 16 40
16 20 00  ---          12 01 52  34.2 -51.2  4.7      80.0   200     4479   16 16 31

16 20 30  J0720+473    12 02 22  35.0 -50.7  4.7      81.0    20     4479   16 20 30
16 22 00  ---          12 03 53  34.7 -50.7  4.7      80.7    90     4502   16 20 31

16 22 00  B0712+472    12 03 53  33.9 -51.1  4.8      79.7   -10     4502   16 22 10
16 25 30  ---          12 07 23  33.3 -51.0  4.8      79.1   200     4554   16 22 01

16 26 00  J0720+473    12 07 53  34.0 -50.5  4.8      80.1    20     4554   16 26 00
16 27 30  ---          12 09 24  33.8 -50.5  4.8      79.8    90     4577   16 26 01

16 27 30  B0712+472    12 09 24  33.0 -50.9  4.9      78.8   -10     4577   16 27 40
16 31 00  ---          12 12 54  32.4 -50.7  4.9      78.2   200     4628   16 27 31

16 31 30  J0720+473    12 13 24  33.1 -50.3  4.9      79.2    20     4628   16 31 30
16 33 00  ---          12 14 54  32.9 -50.3  4.9      78.9    90     4651   16 31 31

16 33 00  B0712+472    12 14 54  32.1 -50.7  5.0      77.9   -10     4651   16 33 10
16 36 30  ---          12 18 25  31.5 -50.5  5.0      77.4   200     4703   16 33 01

16 37 00  J0720+473    12 18 55  32.2 -50.1  5.0      78.3    20     4703   16 37 00
16 38 30  ---          12 20 25  32.0 -50.1  5.0      78.0    90     4726   16 37 01

16 38 30  B0712+472    12 20 25  31.1 -50.4  5.1      77.0   -10     4726   16 38 40
16 42 00  ---          12 23 56  30.6 -50.3  5.1      76.5   200     4778   16 38 31

16 42 30  J0720+473    12 24 26  31.3 -49.9  5.0      77.4    20     4778   16 42 30
16 44 00  ---          12 25 56  31.1 -49.8  5.1      77.1    90     4801   16 42 31

16 44 00  B0712+472    12 25 56  30.2 -50.2  5.1      76.2   -10     4801   16 44 10
16 47 30  ---          12 29 27  29.7 -50.0  5.2      75.6   200     4852   16 44 01

16 48 00  J0720+473    12 29 57  30.4 -49.6  5.1      76.5    20     4852   16 48 00
16 49 30  ---          12 31 27  30.1 -49.6  5.2      76.2    90     4876   16 48 01

16 49 30  B0712+472    12 31 27  29.3 -49.9  5.2      75.3   -10     4876   16 49 40
16 53 00  ---          12 34 58  28.7 -49.7  5.3      74.7   200     4927   16 49 31

16 53 30  J0720+473    12 35 28  29.5 -49.4  5.2      75.6    20     4927   16 53 30
16 55 00  ---          12 36 58  29.2 -49.3  5.3      75.3    90     4950   16 53 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Confirming the detection of a dark matter substructure with Global VLBI
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2016   Day 304 ---

17 00 00  4C39.25      12 41 59  49.8 -64.4  3.2      86.7   250     4950   17 00 00
17 08 00  ---          12 50 00  48.3 -64.3  3.4      85.5   480     5074   17 00 01

17 08 00  B0712+472    12 50 00  26.3 -48.9  5.5      72.3   -51     5074   17 08 51
17 11 30  ---          12 53 31  25.7 -48.7  5.6      71.8   159     5115   17 08 01

17 12 00  J0720+473    12 54 01  26.5 -48.4  5.5      72.6    20     5115   17 12 00
17 13 30  ---          12 55 31  26.2 -48.3  5.6      72.4    90     5138   17 12 01

17 13 30  B0712+472    12 55 31  25.4 -48.6  5.6      71.5   -10     5138   17 13 40
17 17 00  ---          12 59 02  24.8 -48.4  5.7      70.9   200     5190   17 13 31

17 17 30  J0720+473    12 59 32  25.6 -48.1  5.6      71.7    20     5190   17 17 30
17 19 00  ---          13 01 02  25.4 -48.0  5.7      71.5    90     5213   17 17 31

17 19 00  B0712+472    13 01 02  24.5 -48.3  5.7      70.6   -10     5213   17 19 10
17 22 30  ---          13 04 33  23.9 -48.0  5.8      70.1   200     5264   17 19 01

17 23 00  J0720+473    13 05 03  24.7 -47.8  5.7      70.9    20     5264   17 23 00
17 24 30  ---          13 06 33  24.5 -47.7  5.7      70.6    90     5288   17 23 01

17 24 30  B0712+472    13 06 33  23.6 -47.9  5.8      69.7   -10     5288   17 24 40
17 28 00  ---          13 10 04  23.1 -47.7  5.9      69.2   200     5339   17 24 31

17 28 30  J0720+473    13 10 34  23.8 -47.4  5.8      70.0    20     5339   17 28 30
17 30 00  ---          13 12 04  23.6 -47.3  5.8      69.7    90     5362   17 28 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess316.L2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.
    ****** Only  511.50 of  512.00 MHz total bandwidth is within the IFs
           in the setup file before any FREQ or DOPPLER shifts.

   Setup group:    2         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   1  Setup file default.  Used with PCAL = off
   LO sum=   1504.25  1504.25  1568.25  1568.25  1632.25  1632.25  1696.25  1696.25
   BBC fr=    895.75   895.75   831.75   831.75   767.75   767.75   703.75   703.75
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     807.75    807.75    743.75    743.75
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   1   2   3   4   5   6   7   8   9  10

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * B0712+472         07 12 21.530378   * 07 16 03.640000     07 17 18.082272       0.00
                     47 14 08.95037    * 47 08 50.15000      47 06 43.37609        0.00
                     From catalog imbedded in main SCHED input file.

 * J0720+473         07 16 38.668004   * 07 20 21.497762     07 21 36.128656       0.00
                     47 43 20.65409    * 47 37 44.12483      47 35 31.26295        0.00
                     From catalog imbedded in main SCHED input file.

   0552+398          05 52 01.407169   * 05 55 30.805611     05 56 41.783482       0.00
   J0555+3948        39 48 21.94581    * 39 48 49.16496      39 48 41.88529        0.00
 * DA193             /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J0555+39          GSFC 2015a astro solution, unpublished 394383 observations.

 * 4C39.25           09 23 55.319215   * 09 27 03.013936     09 28 04.729288       0.30
   J0927+3902        39 15 23.56645    * 39 02 20.85186      38 57 45.56833        0.16
   0923+392          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J0927+39          GSFC 2015a astro solution, unpublished 245753 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  B0712+472  sess316.L2048glob     1 11                              3.433   167.811
  J0720+473  sess316.L2048glob     1 11                              1.717    88.337
  DA193      sess316.L2048glob     1 11                              0.450    23.417
  4C39.25    sess316.L2048glob     1 11                              0.417    22.917


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   B0712+472          111.0
   J0720+473          110.3
   DA193              126.4
   4C39.25             86.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

