  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron AGN polarization imaging
 Exp. Code:  gg083a  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Jose L. Gomez

Address:  Instituto de Astrofisica de Andalucia-CSIC
          Glorieta de la Astronomia
          E-18008 Granada, Spain
 

Phone:    +79165452842
EMAIL:    jlgomez@iaa.es, alobanov@mpifr-bonn.mpg.de
Fax:
Phone during observation: +79165452842

Observing mode: K-band,Q-band,U-band dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is ON
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Oct 2017   Day 281 ---

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

19 51 15  2200+420     14 06 01   1.8  40.1 -8.0  D  -48.6     0        0   19 51 15
20 00 45  ---          14 15 32   3.1  41.3 -7.8     -50.2     0      147   19 51 05

 ---------- K-band VLBI scans. Ground  segment 01: 2200+420 with EVN+KVN ----------

20 01 00  2200+420     14 15 47   3.2  41.3 -7.8     -50.2     9      147   20 00 51
20 10 30  ---          14 25 19   4.6  42.4 -7.6     -51.7   570      296   20 00 50

20 11 00  2200+420     14 25 49   4.6  42.5 -7.6     -51.8    24      296   20 10 49
20 15 00  ---          14 29 49   5.2  42.9 -7.6     -52.5   240      361   20 10 50

 ---------- K-band VLBI scans. Ground  segment 01: 2200+420 with EVN+KVN ----------

20 15 00  2200+420     14 29 49   5.2  42.9 -7.6     -52.5    -6      361   20 15 06
20 21 00  ---          14 35 50   6.1  43.6 -7.5     -53.4   354      452   20 15 01

 ---------- K-band VLBI scans. Ground  segment 02 : full array on 2200+420 ----------

20 21 30  2200+420     14 36 21   6.2  43.6 -7.5     -53.5    24      452   20 21 19
20 31 00  ---          14 45 52   7.6  44.7 -7.3     -55.0   570      602   20 21 20

20 31 30  2200+420     14 46 22   7.7  44.7 -7.3     -55.0    24      602   20 31 19
20 41 00  ---          14 55 54   9.1  45.7 -7.1     -56.5   570      751   20 31 20

20 41 30  2200+420     14 56 24   9.2  45.8 -7.1     -56.6    24      751   20 41 19
20 51 00  ---          15 05 55  10.7  46.7 -7.0     -58.0   570      901   20 41 20

20 51 15  2200+420     15 06 10  10.7  46.8 -7.0     -58.0     9      901   20 51 06
21 01 00  ---          15 15 57  12.3  47.7 -6.8     -59.5   585     1054   20 51 05

21 01 30  2200+420     15 16 27  12.3  47.8 -6.8     -59.6    24     1054   21 01 19
21 11 00  ---          15 25 59  13.9  48.7 -6.6     -61.0   570     1204   21 01 20

21 11 15  2200+420     15 26 14  13.9  48.7 -6.6     -61.0     9     1204   21 11 06
21 14 15  ---          15 29 14  14.4  49.0 -6.6     -61.5   180     1252   21 11 05

 ---------- K-band VLBI scans. Space segment 03: 2200+420 with EVN+KVN+VLBA+VLA ----------

21 15 00  2200+420     15 29 59  14.5  49.0 -6.6     -61.6    39     1252   21 14 49
21 16 00  ---          15 30 59  14.7  49.1 -6.5     -61.7    60     1271   21 14 50
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Oct 2017   Day 281 ---

21 16 10  2200+420     15 31 09  14.7  49.1 -6.5     -61.7     4     1271   21 16 06
21 19 55  ---          15 34 55  15.3  49.5 -6.5     -62.3   225     1330   21 16 01

21 20 05  2200+420     15 35 05  15.4  49.5 -6.5     -62.3     4     1330   21 20 01
21 21 05  ---          15 36 05  15.5  49.6 -6.5     -62.5    60     1346   21 19 56

21 21 15  2200+420     15 36 15  15.5  49.6 -6.5     -62.5     4     1346   21 21 11
21 25 00  ---          15 40 01  16.2  49.9 -6.4     -63.0   225     1405   21 21 06

21 25 30  2200+420     15 40 31  16.2  50.0 -6.4     -63.1    24     1405   21 25 19
21 26 30  ---          15 41 31  16.4  50.1 -6.4     -63.2    60     1423   21 25 20

21 26 40  2200+420     15 41 41  16.4  50.1 -6.4     -63.3     4     1423   21 26 36
21 30 10  ---          15 45 12  17.0  50.4 -6.3     -63.8   210     1479   21 26 31

21 30 20  2200+420     15 45 22  17.1  50.4 -6.3     -63.8     4     1479   21 30 16
21 31 20  ---          15 46 22  17.2  50.5 -6.3     -63.9    60     1495   21 30 11

21 31 30  2200+420     15 46 32  17.2  50.5 -6.3     -64.0     4     1495   21 31 26
21 35 00  ---          15 50 03  17.8  50.8 -6.2     -64.5   210     1550   21 31 21

21 35 30  2200+420     15 50 33  17.9  50.8 -6.2     -64.5    24     1550   21 35 19
21 36 30  ---          15 51 33  18.1  50.9 -6.2     -64.7    60     1569   21 35 20

21 36 40  2200+420     15 51 43  18.1  50.9 -6.2     -64.7     4     1569   21 36 36
21 40 10  ---          15 55 13  18.7  51.2 -6.1     -65.2   210     1624   21 36 31

21 40 20  2200+420     15 55 23  18.7  51.2 -6.1     -65.2     4     1624   21 40 16
21 41 20  ---          15 56 24  18.9  51.3 -6.1     -65.4    60     1640   21 40 11

21 41 30  2200+420     15 56 34  18.9  51.3 -6.1     -65.4     4     1640   21 41 26
21 45 00  ---          16 00 04  19.5  51.6 -6.1     -65.9   210     1695   21 41 21

21 45 30  2200+420     16 00 34  19.6  51.6 -6.0     -66.0    24     1695   21 45 19
21 46 30  ---          16 01 34  19.8  51.7 -6.0     -66.1    60     1714   21 45 20

21 46 40  2200+420     16 01 45  19.8  51.7 -6.0     -66.1     4     1714   21 46 36
21 50 10  ---          16 05 15  20.4  52.0 -6.0     -66.6   210     1769   21 46 31

21 50 20  2200+420     16 05 25  20.4  52.0 -6.0     -66.6     4     1769   21 50 16
21 51 20  ---          16 06 25  20.6  52.1 -6.0     -66.8    60     1785   21 50 11

21 51 30  2200+420     16 06 35  20.6  52.1 -5.9     -66.8     4     1785   21 51 26
21 55 00  ---          16 10 06  21.2  52.4 -5.9     -67.3   210     1840   21 51 21
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Oct 2017   Day 281 ---

21 55 30  2200+420     16 10 36  21.3  52.4 -5.9     -67.4    24     1840   21 55 19
21 56 30  ---          16 11 36  21.5  52.5 -5.9     -67.5    60     1859   21 55 20

21 56 40  2200+420     16 11 46  21.5  52.5 -5.9     -67.5     4     1859   21 56 36
22 00 10  ---          16 15 17  22.1  52.8 -5.8     -68.0   210     1914   21 56 31

22 00 20  2200+420     16 15 27  22.1  52.8 -5.8     -68.1     4     1914   22 00 16
22 01 20  ---          16 16 27  22.3  52.9 -5.8     -68.2    60     1930   22 00 11

22 01 30  2200+420     16 16 37  22.3  52.9 -5.8     -68.2     4     1930   22 01 26
22 05 00  ---          16 20 08  22.9  53.1 -5.7     -68.7   210     1985   22 01 21

22 05 30  2200+420     16 20 38  23.0  53.2 -5.7     -68.8    24     1985   22 05 19
22 06 30  ---          16 21 38  23.2  53.2 -5.7     -68.9    60     2004   22 05 20

22 06 40  2200+420     16 21 48  23.2  53.3 -5.7     -68.9     4     2004   22 06 36
22 10 10  ---          16 25 18  23.8  53.5 -5.6     -69.4   210     2059   22 06 31

22 10 20  2200+420     16 25 28  23.8  53.5 -5.6     -69.5     4     2059   22 10 16
22 11 20  ---          16 26 29  24.0  53.6 -5.6     -69.6    60     2075   22 10 11

22 11 30  2200+420     16 26 39  24.1  53.6 -5.6     -69.6     4     2075   22 11 26
22 15 00  ---          16 30 09  24.7  53.8 -5.6     -70.1   210     2130   22 11 21

22 15 30  2200+420     16 30 39  24.7  53.9 -5.5     -70.2    24     2130   22 15 19
22 16 30  ---          16 31 39  24.9  54.0 -5.5     -70.3    60     2149   22 15 20

22 16 40  2200+420     16 31 49  25.0  54.0 -5.5     -70.3     4     2149   22 16 36
22 20 10  ---          16 35 20  25.6  54.2 -5.5     -70.8   210     2204   22 16 31

22 20 20  2200+420     16 35 30  25.6  54.2 -5.5     -70.9     4     2204   22 20 16
22 21 20  ---          16 36 30  25.8  54.3 -5.4     -71.0    60     2220   22 20 11

22 21 30  2200+420     16 36 40  25.8  54.3 -5.4     -71.0     4     2220   22 21 26
22 25 00  ---          16 40 11  26.4  54.5 -5.4     -71.5   210     2275   22 21 21

 ---------- K-band VLBI scans. Ground segment 03: 2200+420 with EVN+KVN+VLBA+VLA ----------

22 25 30  2200+420     16 40 41  26.5  54.6 -5.4     -71.6    24     2275   22 25 19
22 26 30  ---          16 41 41  26.7  54.6 -5.4     -71.7    60     2294   22 25 20

22 26 40  2200+420     16 41 51  26.7  54.6 -5.4     -71.7     4     2294   22 26 36
22 30 00  ---          16 45 12  27.3  54.8 -5.3     -72.2   200     2346   22 26 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Oct 2017   Day 281 ---

22 30 10  2200+420     16 45 22  27.3  54.9 -5.3     -72.2     4     2346   22 30 06
22 31 10  ---          16 46 22  27.5  54.9 -5.3     -72.4    60     2363   22 30 01

22 31 20  2200+420     16 46 32  27.5  54.9 -5.3     -72.4     4     2363   22 31 16
22 35 00  ---          16 50 12  28.2  55.2 -5.2     -72.9   220     2421   22 31 11

22 35 30  2200+420     16 50 43  28.3  55.2 -5.2     -73.0    24     2421   22 35 19
22 36 30  ---          16 51 43  28.4  55.3 -5.2     -73.1    60     2439   22 35 20

22 36 40  2200+420     16 51 53  28.5  55.3 -5.2     -73.1     4     2439   22 36 36
22 40 00  ---          16 55 13  29.1  55.5 -5.1     -73.6   200     2491   22 36 31

22 40 10  2200+420     16 55 23  29.1  55.5 -5.1     -73.6     4     2491   22 40 06
22 41 10  ---          16 56 23  29.3  55.5 -5.1     -73.8    60     2508   22 40 01

22 41 20  2200+420     16 56 33  29.3  55.5 -5.1     -73.8     4     2508   22 41 16
22 45 00  ---          17 00 14  29.9  55.8 -5.1     -74.3   220     2566   22 41 11

22 45 30  2200+420     17 00 44  30.0  55.8 -5.0     -74.4    24     2566   22 45 19
22 46 30  ---          17 01 44  30.2  55.8 -5.0     -74.5    60     2584   22 45 20

22 46 40  2200+420     17 01 54  30.2  55.9 -5.0     -74.5     4     2584   22 46 36
22 50 00  ---          17 05 15  30.8  56.0 -5.0     -75.0   200     2636   22 46 31

22 50 10  2200+420     17 05 25  30.9  56.1 -5.0     -75.0     4     2636   22 50 06
22 51 10  ---          17 06 25  31.1  56.1 -5.0     -75.2    60     2653   22 50 01

22 51 20  2200+420     17 06 35  31.1  56.1 -4.9     -75.2     4     2653   22 51 16
22 55 00  ---          17 10 16  31.7  56.3 -4.9     -75.7   220     2711   22 51 11

22 55 10  2200+420     17 10 26  31.8  56.3 -4.9     -75.7     4     2711   22 55 06
22 56 10  ---          17 11 26  31.9  56.4 -4.9     -75.9    60     2727   22 55 01

22 56 20  2200+420     17 11 36  32.0  56.4 -4.9     -75.9     4     2727   22 56 16
23 00 00  ---          17 15 17  32.6  56.6 -4.8     -76.4   220     2785   22 56 11

 ---------- K-band VLBI scans. Ground segment 03 cont.: 2200+420 with EVN+KVN+VLBA+VLA ----------

23 02 30  2200+420     17 17 47  33.1  56.7 -4.8     -76.8   144     2785   23 02 19
23 03 30  ---          17 18 47  33.3  56.8 -4.7     -76.9    60     2803   23 02 20

23 03 40  2200+420     17 18 57  33.3  56.8 -4.7     -76.9     4     2803   23 03 36
23 07 20  ---          17 22 38  34.0  56.9 -4.7     -77.5   220     2861   23 03 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   8 Oct 2017   Day 281 ---

23 07 30  2200+420     17 22 48  34.0  57.0 -4.7     -77.5     4     2861   23 07 26
23 08 30  ---          17 23 48  34.2  57.0 -4.7     -77.6    60     2877   23 07 21

23 08 40  2200+420     17 23 58  34.2  57.0 -4.7     -77.6     4     2877   23 08 36
23 12 20  ---          17 27 39  34.9  57.2 -4.6     -78.2   220     2935   23 08 31

23 12 30  2200+420     17 27 49  34.9  57.2 -4.6     -78.2     4     2935   23 12 26
23 13 30  ---          17 28 49  35.1  57.2 -4.6     -78.3    60     2952   23 12 21

23 13 40  2200+420     17 28 59  35.1  57.2 -4.6     -78.4     4     2952   23 13 36
23 17 00  ---          17 32 19  35.7  57.4 -4.5     -78.8   200     3004   23 13 31

23 17 10  2200+420     17 32 29  35.7  57.4 -4.5     -78.9     4     3004   23 17 06
23 18 10  ---          17 33 30  35.9  57.4 -4.5     -79.0    60     3021   23 17 01

23 18 20  2200+420     17 33 40  36.0  57.5 -4.5     -79.0     4     3021   23 18 16
23 21 40  ---          17 37 00  36.6  57.6 -4.4     -79.5   200     3073   23 18 11

23 22 40  2200+420     17 38 00  36.7  57.6 -4.4     -79.6    54     3073   23 22 29
23 23 40  ---          17 39 00  36.9  57.7 -4.4     -79.8    60     3091   23 22 30

23 23 50  2200+420     17 39 10  37.0  57.7 -4.4     -79.8     4     3091   23 23 46
23 27 30  ---          17 42 51  37.6  57.8 -4.3     -80.3   220     3149   23 23 41

23 27 40  2200+420     17 43 01  37.7  57.8 -4.3     -80.4     4     3149   23 27 36
23 28 40  ---          17 44 01  37.8  57.9 -4.3     -80.5    60     3166   23 27 31

23 28 50  2200+420     17 44 11  37.9  57.9 -4.3     -80.5     4     3166   23 28 46
23 32 00  ---          17 47 22  38.4  58.0 -4.3     -81.0   190     3216   23 28 41

23 33 00  2200+420     17 48 22  38.6  58.0 -4.3     -81.1    54     3216   23 32 49
23 43 00  ---          17 58 24  40.5  58.4 -4.1     -82.6   600     3373   23 32 50

23 43 30  2200+420     17 58 54  40.6  58.4 -4.1     -82.7    24     3373   23 43 19
23 53 30  ---          18 08 55  42.4  58.7 -3.9     -84.2   600     3530   23 43 20

 --- Start: Sun   8 Oct 2017   Day 281 -- Stop: Mon   9 Oct 2017   Day 282 ---

23 54 00  2200+420     18 09 25  42.5  58.7 -3.9     -84.3    24     3530   23 53 49
00 04 00  ---          18 19 27  44.3  58.9 -3.7     -85.8   600     3688   23 53 50

00 04 30  2200+420     18 19 57  44.4  58.9 -3.7     -85.9    24     3688   00 04 19
00 11 30  ---          18 26 58  45.7  59.0 -3.6     -87.0   420     3799   00 04 20
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

00 12 20  2200+420     18 27 48  45.9  59.0 -3.6     -87.1    44     3799   00 12 09
00 13 20  ---          18 28 49  46.1  59.1 -3.6     -87.3    60     3817   00 12 10

00 13 30  2200+420     18 28 59  46.1  59.1 -3.6     -87.3     4     3817   00 13 26
00 17 10  ---          18 32 39  46.8  59.1 -3.5     -87.9   220     3875   00 13 21

00 17 20  2200+420     18 32 49  46.8  59.1 -3.5     -87.9     4     3875   00 17 16
00 18 20  ---          18 33 49  47.0  59.1 -3.5     -88.1    60     3891   00 17 11

00 18 30  2200+420     18 33 59  47.0  59.1 -3.5     -88.1     4     3891   00 18 26
00 22 30  ---          18 38 00  47.8  59.1 -3.4     -88.8   240     3954   00 18 21

00 23 30  2200+420     18 39 00  47.9  59.2 -3.4     -88.9    54     3954   00 23 19
00 24 30  ---          18 40 00  48.1  59.2 -3.4     -89.1    60     3973   00 23 20

00 24 40  2200+420     18 40 10  48.2  59.2 -3.4     -89.1     4     3973   00 24 36
00 28 40  ---          18 44 11  48.9  59.2 -3.3     -89.8   240     4035   00 24 31

00 28 50  2200+420     18 44 21  48.9  59.2 -3.3     -89.8     4     4035   00 28 46
00 29 50  ---          18 45 21  49.1  59.2 -3.3     -90.0    60     4052   00 28 41

00 30 00  2200+420     18 45 31  49.1  59.2 -3.3     -90.0     4     4052   00 29 56
00 34 00  ---          18 49 32  49.9  59.2 -3.2     -90.7   240     4115   00 29 51

00 35 00  2200+420     18 50 32  50.1  59.2 -3.2     -90.9    54     4115   00 34 49
00 36 00  ---          18 51 32  50.3  59.2 -3.2     -91.0    60     4133   00 34 50

00 36 10  2200+420     18 51 42  50.3  59.2 -3.2     -91.1     4     4133   00 36 06
00 40 10  ---          18 55 43  51.0  59.1 -3.1     -91.8   240     4196   00 36 01

00 40 20  2200+420     18 55 53  51.1  59.1 -3.1     -91.8     4     4196   00 40 16
00 41 20  ---          18 56 53  51.2  59.1 -3.1     -92.0    60     4212   00 40 11

00 41 30  2200+420     18 57 03  51.3  59.1 -3.1     -92.0     4     4212   00 41 26
00 44 50  ---          19 00 24  51.9  59.1 -3.1     -92.6   200     4265   00 41 21

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

00 45 50  2200+420     19 01 24  52.1  59.1 -3.0     -92.8    54     4265   00 45 39
00 46 50  ---          19 02 24  52.3  59.0 -3.0     -93.0    60     4283   00 45 40

00 47 00  2200+420     19 02 34  52.3  59.0 -3.0     -93.0     4     4283   00 46 56
00 55 20  ---          19 10 55  53.8  58.9 -2.9     -94.5   500     4413   00 46 51
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

00 57 00  2200+420     19 12 36  54.1  58.8 -2.8     -94.8    94     4413   00 56 49
01 05 50  ---          19 21 27  55.8  58.5 -2.7     -96.6   530     4552   00 56 50

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

01 06 50  2200+420     19 22 27  56.0  58.5 -2.7     -96.8    54     4552   01 06 39
01 07 50  ---          19 23 28  56.1  58.5 -2.7     -97.0    60     4571   01 06 40

01 08 00  2200+420     19 23 38  56.2  58.5 -2.7     -97.0     4     4571   01 07 56
01 12 00  ---          19 27 38  56.9  58.3 -2.6     -97.8   240     4634   01 07 51

01 12 10  2200+420     19 27 48  56.9  58.3 -2.6     -97.9     4     4634   01 12 06
01 13 10  ---          19 28 48  57.1  58.2 -2.6     -98.1    60     4650   01 12 01

01 13 20  2200+420     19 28 58  57.1  58.2 -2.6     -98.1     4     4650   01 13 16
01 17 20  ---          19 32 59  57.9  58.0 -2.5     -99.0   240     4713   01 13 11

01 18 20  2200+420     19 33 59  58.1  58.0 -2.5     -99.2    54     4713   01 18 09
01 19 20  ---          19 34 59  58.2  57.9 -2.5     -99.4    60     4731   01 18 10

01 19 30  2200+420     19 35 09  58.3  57.9 -2.5     -99.4     4     4731   01 19 26
01 22 50  ---          19 38 30  58.9  57.7 -2.4    -100.2   200     4784   01 19 21

01 23 00  2200+420     19 38 40  58.9  57.7 -2.4    -100.2     4     4784   01 22 56
01 24 00  ---          19 39 40  59.1  57.6 -2.4    -100.4    60     4800   01 22 51

01 24 10  2200+420     19 39 50  59.1  57.6 -2.4    -100.5     4     4800   01 24 06
01 27 30  ---          19 43 11  59.7  57.4 -2.3    -101.2   200     4853   01 24 01

01 28 00  2200+420     19 43 41  59.8  57.3 -2.3    -101.3    24     4853   01 27 49
01 34 40  ---          19 50 22  61.0  56.8 -2.2    -102.9   400     4959   01 27 50

 ---------- K-band VLBI scans. Space segment 04: 2200+420 with EVN+KVN+VLBA+VLA ----------

01 35 00  2200+420     19 50 42  61.1  56.8 -2.2    -103.0    14     4959   01 34 49
01 36 00  ---          19 51 42  61.3  56.7 -2.2    -103.2    60     4977   01 34 50

01 36 10  2200+420     19 51 52  61.3  56.7 -2.2    -103.3     4     4977   01 36 06
01 39 55  ---          19 55 38  62.0  56.3 -2.1    -104.2   225     5036   01 36 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

01 40 05  2200+420     19 55 48  62.0  56.3 -2.1    -104.3     4     5036   01 40 01
01 41 05  ---          19 56 48  62.2  56.2 -2.1    -104.5    60     5053   01 39 56

01 41 15  2200+420     19 56 58  62.2  56.2 -2.1    -104.6     4     5053   01 41 11
01 45 00  ---          20 00 44  62.9  55.8 -2.0    -105.5   225     5112   01 41 06

01 45 30  2200+420     20 01 14  63.0  55.8 -2.0    -105.7    24     5112   01 45 19
01 46 30  ---          20 02 14  63.2  55.7 -2.0    -105.9    60     5130   01 45 20

01 46 40  2200+420     20 02 24  63.2  55.6 -2.0    -106.0     4     5130   01 46 36
01 50 10  ---          20 05 55  63.8  55.2 -2.0    -107.0   210     5185   01 46 31

01 50 20  2200+420     20 06 05  63.8  55.2 -2.0    -107.0     4     5185   01 50 16
01 51 20  ---          20 07 05  64.0  55.1 -1.9    -107.3    60     5201   01 50 11

01 51 30  2200+420     20 07 15  64.0  55.1 -1.9    -107.3     4     5201   01 51 26
01 55 00  ---          20 10 45  64.7  54.6 -1.9    -108.3   210     5257   01 51 21

01 55 30  2200+420     20 11 15  64.7  54.5 -1.9    -108.5    24     5257   01 55 19
01 56 30  ---          20 12 16  64.9  54.4 -1.9    -108.8    60     5275   01 55 20

01 56 40  2200+420     20 12 26  64.9  54.4 -1.9    -108.8     4     5275   01 56 36
02 00 10  ---          20 15 56  65.6  53.9 -1.8    -109.9   210     5330   01 56 31

02 00 20  2200+420     20 16 06  65.6  53.8 -1.8    -109.9     4     5330   02 00 16
02 01 20  ---          20 17 06  65.8  53.7 -1.8    -110.2    60     5347   02 00 11

02 01 30  2200+420     20 17 16  65.8  53.6 -1.8    -110.3     4     5347   02 01 26
02 05 00  ---          20 20 47  66.4  53.1 -1.7    -111.4   210     5402   02 01 21

02 05 30  2200+420     20 21 17  66.5  53.0 -1.7    -111.6    24     5402   02 05 19
02 06 30  ---          20 22 17  66.7  52.8 -1.7    -111.9    60     5420   02 05 20

02 06 40  2200+420     20 22 27  66.7  52.8 -1.7    -111.9     4     5420   02 06 36
02 10 10  ---          20 25 58  67.3  52.2 -1.6    -113.1   210     5475   02 06 31

02 10 20  2200+420     20 26 08  67.3  52.1 -1.6    -113.2     4     5475   02 10 16
02 11 20  ---          20 27 08  67.5  51.9 -1.6    -113.5    60     5492   02 10 11

02 11 30  2200+420     20 27 18  67.5  51.9 -1.6    -113.6     4     5492   02 11 26
02 15 00  ---          20 30 49  68.1  51.2 -1.5    -114.8   210     5547   02 11 21

02 15 30  2200+420     20 31 19  68.2  51.1 -1.5    -115.0    24     5547   02 15 19
02 16 30  ---          20 32 19  68.4  50.9 -1.5    -115.4    60     5565   02 15 20
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

02 16 40  2200+420     20 32 29  68.4  50.8 -1.5    -115.4     4     5565   02 16 36
02 20 10  ---          20 35 59  69.0  50.1 -1.5    -116.8   210     5620   02 16 31

02 20 20  2200+420     20 36 09  69.0  50.0 -1.5    -116.8     4     5620   02 20 16
02 21 20  ---          20 37 10  69.2  49.8 -1.4    -117.2    60     5637   02 20 11

02 21 30  2200+420     20 37 20  69.2  49.7 -1.4    -117.3     4     5637   02 21 26
02 25 00  ---          20 40 50  69.8  48.9 -1.4    -118.7   210     5692   02 21 21

02 25 30  2200+420     20 41 20  69.8  48.7 -1.4    -118.9    24     5692   02 25 19
02 26 30  ---          20 42 20  70.0  48.5 -1.4    -119.3    60     5710   02 25 20

02 26 40  2200+420     20 42 31  70.0  48.4 -1.3    -119.4     4     5710   02 26 36
02 30 10  ---          20 46 01  70.6  47.5 -1.3    -120.9   210     5765   02 26 31

02 30 20  2200+420     20 46 11  70.6  47.4 -1.3    -120.9     4     5765   02 30 16
02 31 20  ---          20 47 11  70.8  47.1 -1.3    -121.4    60     5782   02 30 11

02 31 30  2200+420     20 47 21  70.8  47.1 -1.3    -121.5     4     5782   02 31 26
02 35 00  ---          20 50 52  71.3  46.0 -1.2    -123.1   210     5837   02 31 21

 ---------- K-band VLBI scans. Ground segment 04: 2200+420 with EVN+KVN+VLBA+VLA ----------

02 35 10  2200+420     20 51 02  71.4  46.0 -1.2    -123.1     4     5837   02 35 06
02 38 50  ---          20 54 43  71.9  44.8 -1.1    -124.9   220     5895   02 35 01

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

02 40 00  2200+420     20 55 53  72.1  44.4 -1.1    -125.5    64     5895   02 39 49
02 41 00  ---          20 56 53  72.3  44.0 -1.1    -126.0    60     5913   02 39 50

02 41 10  2200+420     20 57 03  72.3  43.9 -1.1    -126.1     4     5913   02 41 06
02 49 30  ---          21 05 24  73.5  40.7 -1.0    -130.6   500     6043   02 41 01

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

02 50 30  2200+420     21 06 24  73.6  40.3 -1.0    -131.2    54     6043   02 50 19
03 00 00  ---          21 15 56  74.9  35.7 -0.8    -137.1   570     6192   02 50 20
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

03 01 00  2200+420     21 16 56  75.0  35.2 -0.8    -137.8    54     6192   03 00 49
03 02 00  ---          21 17 56  75.2  34.7 -0.8    -138.5    60     6211   03 00 50

03 02 10  2200+420     21 18 06  75.2  34.6 -0.8    -138.6     4     6211   03 02 06
03 05 40  ---          21 21 37  75.6  32.6 -0.7    -141.1   210     6266   03 02 01

03 05 50  2200+420     21 21 47  75.6  32.5 -0.7    -141.2     4     6266   03 05 46
03 06 50  ---          21 22 47  75.7  31.9 -0.7    -142.0    60     6282   03 05 41

03 07 00  2200+420     21 22 57  75.7  31.8 -0.7    -142.1     4     6282   03 06 56
03 10 30  ---          21 26 28  76.1  29.7 -0.6    -144.8   210     6337   03 06 51

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

03 12 00  2200+420     21 27 58  76.3  28.7 -0.6    -145.9    84     6337   03 11 49
03 13 00  ---          21 28 58  76.4  28.1 -0.6    -146.7    60     6356   03 11 50

03 13 10  2200+420     21 29 08  76.4  28.0 -0.6    -146.9     4     6356   03 13 06
03 21 30  ---          21 37 30  77.2  22.1 -0.4    -154.0   500     6486   03 13 01

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

03 22 30  2200+420     21 38 30  77.2  21.3 -0.4    -154.9    54     6486   03 22 19
03 32 00  ---          21 48 01  77.9  13.7 -0.3    -164.0   570     6635   03 22 20

 ---------- K-band VLBI scans. Ground segment 04: NRAO150 with EVN+KVN+VLBA+VLA ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

03 36 00  NRAO150      21 52 02  22.0  42.7 -6.1     -68.1   122     6635   03 35 49
03 39 40  ---          21 55 42  22.6  42.9 -6.1     -68.7   220     6695   03 35 50

 ---------- K-band VLBI scans. Ground  segment 04: NRAO150 with EVN+KVN ----------

03 40 40  NRAO150      21 56 43  22.7  43.0 -6.1     -68.9    54     6695   03 40 29
03 41 40  ---          21 57 43  22.9  43.1 -6.1     -69.0    60     6713   03 40 30

03 41 50  NRAO150      21 57 53  22.9  43.1 -6.0     -69.1     4     6713   03 41 46
03 46 50  ---          22 02 54  23.6  43.4 -6.0     -69.9   300     6791   03 41 41
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- Q-band VLBI scans. Ground  segment 04: NRAO150 with VLBA+VLA ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

03 47 50  NRAO150      22 03 54  23.8  43.4 -5.9     -70.1    54     6791   03 47 39
03 52 50  ---          22 08 55  24.5  43.7 -5.9     -70.9   300     6871   03 47 40

 ---------- U-band VLBI scans. Ground  segment 04 : NRAO150 with VLBA+VLA ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

03 53 50  NRAO150      22 09 55  24.7  43.8 -5.8     -71.1    54     6871   03 53 39
03 54 50  ---          22 10 55  24.8  43.8 -5.8     -71.3    60     6890   03 53 40

03 55 00  NRAO150      22 11 05  24.9  43.8 -5.8     -71.3     4     6890   03 54 56
04 00 00  ---          22 16 06  25.6  44.1 -5.7     -72.2   300     6968   03 54 51

 ---------- U-band VLBI scans. Ground  segment 04 : 3C454.3 with VLBA+VLA ----------

04 10 00  3C454.3      22 26 07  74.2 153.9 -0.5     -23.2   498     6968   04 09 49
04 13 40  ---          22 29 48  74.5 156.9 -0.4     -20.6   220     7028   04 09 50

 ---------- U-band VLBI scans. Ground  segment 04 : 3C454.3 with VLBA+VLA ----------

04 14 40  3C454.3      22 30 48  74.6 157.8 -0.4     -19.8    54     7028   04 14 29
04 15 40  ---          22 31 48  74.7 158.6 -0.4     -19.1    60     7046   04 14 30

04 15 50  3C454.3      22 31 58  74.7 158.8 -0.4     -18.9     4     7046   04 15 46
04 20 50  ---          22 36 59  75.0 163.2 -0.3     -15.0   300     7124   04 15 41

 ---------- Q-band VLBI scans. Ground  segment 04: 3C454.3 with VLBA+VLA ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

04 21 50  3C454.3      22 37 59  75.1 164.1 -0.3     -14.2    54     7124   04 21 39
04 26 50  ---          22 43 00  75.4 168.7 -0.2     -10.1   300     7204   04 21 40
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- K-band VLBI scans. Ground  segment 04: 3C454.3 with EVN+KVN ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

04 27 50  3C454.3      22 44 00  75.4 169.6 -0.2      -9.3    54     7204   04 27 39
04 28 50  ---          22 45 01  75.4 170.6 -0.2      -8.4    60     7223   04 27 40

04 29 00  3C454.3      22 45 11  75.4 170.7 -0.2      -8.3     4     7223   04 28 56
04 34 00  ---          22 50 11  75.6 175.5 -0.1      -4.0   300     7301   04 28 51

 ---------- K-band VLBI scans. Ground  segment 04 : 2200+420 with VLBA ----------

04 36 00  2200+420     22 52 12  74.8 323.6  0.8     136.3     7     7301   04 35 53
04 39 40  ---          22 55 52  74.3 321.8  0.9     134.0   220     7359   04 35 50

04 39 50  2200+420     22 56 02  74.3 321.8  0.9     133.9     4     7359   04 39 46
04 40 50  ---          22 57 03  74.1 321.3  0.9     133.3    60     7376   04 39 41

04 41 00  2200+420     22 57 13  74.1 321.2  0.9     133.2     4     7376   04 40 56
04 45 00  ---          23 01 13  73.5 319.4  1.0     130.8   240     7439   04 40 51

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

04 46 00  2200+420     23 02 13  73.4 319.0  1.0     130.2    54     7439   04 45 49
04 47 00  ---          23 03 14  73.3 318.6  1.0     129.6    60     7457   04 45 50

04 47 10  2200+420     23 03 24  73.2 318.5  1.0     129.5     4     7457   04 47 06
04 55 30  ---          23 11 45  72.0 315.4  1.1     125.1   500     7587   04 47 01

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

04 56 30  2200+420     23 12 45  71.9 315.1  1.2     124.7    54     7587   04 56 19
05 05 30  ---          23 21 47  70.5 312.3  1.3     120.5   540     7729   04 56 20
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- K-band VLBI scans. Ground  segment 04 : 3C84 with VLBA+VLA+EVN+KVN ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

05 09 00  3C84         23 25 17  42.1 419.7 -3.9     -83.3   126     7729   05 08 49
05 12 40  ---          23 28 58  42.8 419.8 -3.9     -83.8   220     7788   05 08 50

 ---------- K-band VLBI scans. Ground  segment 04: 3C84 with VLBA+VLA+EVN+KVN ----------

05 12 50  3C84         23 29 08  42.8 419.8 -3.9     -83.9     4     7788   05 12 46
05 13 50  ---          23 30 08  43.0 419.9 -3.8     -84.0    60     7805   05 12 41

05 14 00  3C84         23 30 18  43.0 419.9 -3.8     -84.0     4     7805   05 13 56
05 19 00  ---          23 35 19  44.0 420.0 -3.8     -84.8   300     7883   05 13 51

 ---------- Q-band VLBI scans. Ground  segment 04: 3C84 with VLBA+VLA ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

05 20 00  3C84         23 36 19  44.1 420.0 -3.7     -84.9    54     7883   05 19 49
05 25 00  ---          23 41 20  45.1 420.1 -3.7     -85.7   300     7963   05 19 50

05 25 10  3C84         23 41 30  45.1 420.1 -3.7     -85.7     4     7963   05 25 06
05 29 40  ---          23 46 01  46.0 420.2 -3.6     -86.4   270     8034   05 25 01

 ---------- U-band VLBI scans. Ground  segment 04 : 3C84 with VLBA+VLA ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

05 30 40  3C84         23 47 01  46.1 420.2 -3.6     -86.6    54     8034   05 30 29
05 31 40  ---          23 48 01  46.3 420.2 -3.5     -86.7    60     8052   05 30 30

05 31 50  3C84         23 48 11  46.4 420.2 -3.5     -86.7     4     8052   05 31 46
05 37 40  ---          23 54 02  47.5 420.3 -3.4     -87.7   350     8143   05 31 41

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

05 41 00  2200+420     23 57 22  64.4 305.2  1.9     108.0   110     8143   05 40 49
05 44 40  ---          00 01 03  63.8 304.8  2.0     106.9   220     8203   05 40 50

 ---------- K-band VLBI scans. Space segment 05: 2200+420 with EVN+KVN ----------

05 45 00  2200+420     00 01 23  63.7 304.7  2.0     106.9    14     8203   05 44 49
05 46 00  ---          00 02 23  63.6 304.6  2.0     106.6    60     8221   05 44 50
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

05 46 10  2200+420     00 02 33  63.5 304.6  2.0     106.5     4     8221   05 46 06
05 49 55  ---          00 06 19  62.9 304.2  2.0     105.5   225     8280   05 46 01

05 50 05  2200+420     00 06 29  62.8 304.2  2.1     105.5     4     8280   05 50 01
05 51 05  ---          00 07 29  62.7 304.0  2.1     105.2    60     8297   05 49 56

05 51 15  2200+420     00 07 39  62.6 304.0  2.1     105.2     4     8297   05 51 11
05 55 00  ---          00 11 25  62.0 303.6  2.1     104.2   225     8356   05 51 06

05 55 30  2200+420     00 11 55  61.9 303.6  2.1     104.1    24     8356   05 55 19
05 56 30  ---          00 12 55  61.7 303.5  2.2     103.8    60     8374   05 55 20

05 56 40  2200+420     00 13 05  61.7 303.5  2.2     103.8     4     8374   05 56 36
06 00 10  ---          00 16 36  61.0 303.2  2.2     102.9   210     8429   05 56 31

06 00 20  2200+420     00 16 46  61.0 303.2  2.2     102.9     4     8429   06 00 16
06 01 20  ---          00 17 46  60.8 303.1  2.2     102.6    60     8446   06 00 11

06 01 30  2200+420     00 17 56  60.8 303.1  2.2     102.6     4     8446   06 01 26
06 05 00  ---          00 21 26  60.2 302.8  2.3     101.8   210     8501   06 01 21

06 05 30  2200+420     00 21 56  60.1 302.8  2.3     101.6    24     8501   06 05 19
06 06 30  ---          00 22 57  59.9 302.7  2.3     101.4    60     8519   06 05 20

06 06 40  2200+420     00 23 07  59.8 302.7  2.3     101.4     4     8519   06 06 36
06 10 10  ---          00 26 37  59.2 302.4  2.4     100.6   210     8574   06 06 31

06 10 20  2200+420     00 26 47  59.2 302.4  2.4     100.5     4     8574   06 10 16
06 11 20  ---          00 27 47  59.0 302.3  2.4     100.3    60     8591   06 10 11

06 11 30  2200+420     00 27 57  59.0 302.3  2.4     100.3     4     8591   06 11 26
06 15 00  ---          00 31 28  58.3 302.1  2.5      99.5   210     8646   06 11 21

06 15 30  2200+420     00 31 58  58.2 302.1  2.5      99.4    24     8646   06 15 19
06 16 30  ---          00 32 58  58.1 302.0  2.5      99.2    60     8664   06 15 20

06 16 40  2200+420     00 33 08  58.0 302.0  2.5      99.1     4     8664   06 16 36
06 20 10  ---          00 36 39  57.4 301.8  2.6      98.4   210     8719   06 16 31

06 20 20  2200+420     00 36 49  57.4 301.8  2.6      98.3     4     8719   06 20 16
06 21 20  ---          00 37 49  57.2 301.8  2.6      98.1    60     8736   06 20 11

06 21 30  2200+420     00 37 59  57.1 301.8  2.6      98.1     4     8736   06 21 26
06 25 00  ---          00 41 30  56.5 301.6  2.6      97.4   210     8791   06 21 21
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

06 25 30  2200+420     00 42 00  56.4 301.6  2.6      97.3    24     8791   06 25 19
06 26 30  ---          00 43 00  56.2 301.6  2.7      97.1    60     8809   06 25 20

06 26 40  2200+420     00 43 10  56.2 301.5  2.7      97.0     4     8809   06 26 36
06 30 10  ---          00 46 41  55.5 301.4  2.7      96.3   210     8864   06 26 31

06 30 20  2200+420     00 46 51  55.5 301.4  2.7      96.3     4     8864   06 30 16
06 31 20  ---          00 47 51  55.3 301.4  2.7      96.1    60     8881   06 30 11

06 31 30  2200+420     00 48 01  55.3 301.4  2.7      96.1     4     8881   06 31 26
06 35 00  ---          00 51 31  54.7 301.3  2.8      95.4   210     8936   06 31 21

06 35 30  2200+420     00 52 01  54.6 301.2  2.8      95.3    24     8936   06 35 19
06 36 30  ---          00 53 02  54.4 301.2  2.8      95.1    60     8954   06 35 20

06 36 40  2200+420     00 53 12  54.4 301.2  2.8      95.1     4     8954   06 36 36
06 40 10  ---          00 56 42  53.7 301.1  2.9      94.4   210     9009   06 36 31

06 40 20  2200+420     00 56 52  53.7 301.1  2.9      94.4     4     9009   06 40 16
06 41 20  ---          00 57 52  53.5 301.1  2.9      94.2    60     9026   06 40 11

06 41 30  2200+420     00 58 02  53.5 301.1  2.9      94.2     4     9026   06 41 26
06 45 00  ---          01 01 33  52.8 301.0  3.0      93.5   210     9081   06 41 21

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

06 47 00  2200+420     01 03 33  52.4 301.0  3.0      93.1   114     9081   06 46 49
06 50 40  ---          01 07 14  51.8 300.9  3.1      92.5   220     9140   06 46 50

 ---------- Ground-only VLBA+VLA27  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

06 51 40  2200+420     01 08 14  51.6 300.9  3.1      92.3    54     9140   06 51 29
07 01 10  ---          01 17 46  49.8 300.8  3.2      90.6   570     9290   06 51 30

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

07 02 10  2200+420     01 18 46  49.6 300.8  3.3      90.5    54     9290   07 01 59
07 03 10  ---          01 19 46  49.5 300.8  3.3      90.3    60     9308   07 02 00

07 03 20  2200+420     01 19 56  49.4 300.8  3.3      90.3     4     9308   07 03 16
07 11 30  ---          01 28 07  47.9 300.8  3.4      88.9   490     9436   07 03 11
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

07 14 00  NRAO150      01 30 38  55.6 402.8 -2.5    -111.8    69     9436   07 13 49
07 17 40  ---          01 34 18  56.1 402.4 -2.4    -112.8   220     9495   07 13 50

 ---------- K-band VLBI scans. Ground  segment 04: NRAO150 with EVN+KVN ----------

07 18 40  NRAO150      01 35 18  56.3 402.3 -2.4    -113.1    54     9495   07 18 29
07 19 40  ---          01 36 19  56.4 402.2 -2.4    -113.4    60     9514   07 18 30

07 19 50  NRAO150      01 36 29  56.5 402.1 -2.4    -113.4     4     9514   07 19 46
07 24 50  ---          01 41 29  57.2 401.5 -2.3    -114.9   300     9592   07 19 41

 ---------- Q-band VLBI scans. Ground  segment 04: NRAO150 with VLBA+VLA ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

07 25 50  NRAO150      01 42 30  57.3 401.4 -2.3    -115.2    54     9592   07 25 39
07 30 50  ---          01 47 30  58.0 400.8 -2.2    -116.7   300     9672   07 25 40

 ---------- U-band VLBI scans. Ground  segment 04 : NRAO150 with VLBA+VLA ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

07 31 50  NRAO150      01 48 31  58.2 400.6 -2.2    -117.0    54     9672   07 31 39
07 32 50  ---          01 49 31  58.3 400.5 -2.2    -117.4    60     9690   07 31 40

07 33 00  NRAO150      01 49 41  58.3 400.5 -2.2    -117.4     4     9690   07 32 56
07 38 00  ---          01 54 42  59.0 399.8 -2.1    -119.0   300     9769   07 32 51

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

07 41 00  2200+420     01 57 42  42.5 301.3  3.9      84.2   102     9769   07 40 49
07 44 40  ---          02 01 23  41.8 301.4  4.0      83.7   220     9828   07 40 50
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- Ground-only VLBA+VLA27+Ef+Yb  Q-band on target source ----------

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

07 45 40  2200+420     02 02 23  41.6 301.4  4.0      83.5    54     9828   07 45 29
07 55 10  ---          02 11 54  39.8 301.7  4.1      82.1   570     9978   07 45 30

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on target source ----------

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

07 56 10  2200+420     02 12 55  39.7 301.8  4.2      82.0    54     9978   07 55 59
07 57 10  ---          02 13 55  39.5 301.8  4.2      81.8    60     9996   07 56 00

07 57 20  2200+420     02 14 05  39.5 301.8  4.2      81.8     4     9996   07 57 16
08 05 30  ---          02 22 16  38.0 302.1  4.3      80.6   490    10123   07 57 11

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

08 06 30  2200+420     02 23 16  37.8 302.1  4.3      80.5    54    10123   08 06 19
08 07 30  ---          02 24 16  37.6 302.2  4.3      80.3    60    10142   08 06 20

08 07 40  2200+420     02 24 27  37.6 302.2  4.3      80.3     4    10142   08 07 36
08 11 25  ---          02 28 12  36.9 302.3  4.4      79.8   225    10201   08 07 31

08 11 35  2200+420     02 28 22  36.8 302.3  4.4      79.7     4    10201   08 11 31
08 12 35  ---          02 29 22  36.7 302.4  4.4      79.6    60    10217   08 11 26

08 12 45  2200+420     02 29 32  36.6 302.4  4.4      79.6     4    10217   08 12 41
08 16 30  ---          02 33 18  36.0 302.5  4.5      79.0   225    10276   08 12 36

08 17 00  2200+420     02 33 48  35.9 302.6  4.5      78.9    24    10276   08 16 49
08 18 00  ---          02 34 48  35.7 302.6  4.5      78.8    60    10294   08 16 50

08 18 10  2200+420     02 34 58  35.6 302.6  4.5      78.8     4    10294   08 18 06
08 21 40  ---          02 38 29  35.0 302.8  4.6      78.3   210    10350   08 18 01

08 21 50  2200+420     02 38 39  35.0 302.8  4.6      78.3     4    10350   08 21 46
08 22 50  ---          02 39 39  34.8 302.8  4.6      78.1    60    10366   08 21 41

08 23 00  2200+420     02 39 49  34.8 302.8  4.6      78.1     4    10366   08 22 56
08 26 30  ---          02 43 20  34.1 303.0  4.7      77.6   210    10421   08 22 51

08 27 00  2200+420     02 43 50  34.0 303.0  4.7      77.5    24    10421   08 26 49
08 28 00  ---          02 44 50  33.9 303.1  4.7      77.4    60    10440   08 26 50
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

08 28 10  2200+420     02 45 00  33.8 303.1  4.7      77.4     4    10440   08 28 06
08 31 40  ---          02 48 30  33.2 303.3  4.8      76.9   210    10495   08 28 01

08 31 50  2200+420     02 48 40  33.2 303.3  4.8      76.8     4    10495   08 31 46
08 32 50  ---          02 49 41  33.0 303.3  4.8      76.7    60    10511   08 31 41

08 33 00  2200+420     02 49 51  33.0 303.3  4.8      76.7     4    10511   08 32 56
08 36 30  ---          02 53 21  32.3 303.5  4.8      76.2   210    10566   08 32 51

08 37 00  2200+420     02 53 51  32.2 303.5  4.8      76.1    24    10566   08 36 49
08 38 00  ---          02 54 52  32.1 303.6  4.9      76.0    60    10585   08 36 50

08 38 10  2200+420     02 55 02  32.0 303.6  4.9      75.9     4    10585   08 38 06
08 41 40  ---          02 58 32  31.4 303.8  4.9      75.5   210    10640   08 38 01

08 41 50  2200+420     02 58 42  31.4 303.8  4.9      75.4     4    10640   08 41 46
08 42 50  ---          02 59 42  31.2 303.8  4.9      75.3    60    10656   08 41 41

08 43 00  2200+420     02 59 52  31.2 303.9  4.9      75.3     4    10656   08 42 56
08 46 30  ---          03 03 23  30.5 304.1  5.0      74.8   210    10711   08 42 51

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

08 47 00  2200+420     03 03 53  30.5 304.1  5.0      74.7    24    10711   08 46 49
08 52 00  ---          03 08 54  29.6 304.4  5.1      74.0   300    10791   08 46 50

08 52 30  2200+420     03 09 24  29.5 304.4  5.1      73.9    24    10791   08 52 19
08 53 30  ---          03 10 24  29.3 304.5  5.1      73.8    60    10810   08 52 20

08 53 40  2200+420     03 10 34  29.3 304.5  5.1      73.8     4    10810   08 53 36
09 02 00  ---          03 18 55  27.8 305.0  5.3      72.6   500    10940   08 53 31

09 02 30  2200+420     03 19 26  27.7 305.0  5.3      72.5    24    10940   09 02 19
09 03 30  ---          03 20 26  27.5 305.1  5.3      72.4    60    10958   09 02 20

09 03 40  2200+420     03 20 36  27.5 305.1  5.3      72.4     4    10958   09 03 36
09 12 00  ---          03 28 57  26.0 305.6  5.4      71.2   500    11088   09 03 31

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

09 17 00  3C84         03 33 58  78.8 347.5  0.2     165.5   188    11088   09 16 49
09 20 40  ---          03 37 39  78.6 344.1  0.3     161.6   220    11147   09 16 50
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

 ---------- Ground-only VLBA+VLA27+Ef+Yb  U-band on calibrator source ----------

09 21 40  3C84         03 38 39  78.5 343.2  0.3     160.6    54    11147   09 21 29
09 22 40  ---          03 39 39  78.4 342.3  0.3     159.6    60    11166   09 21 30

09 22 50  3C84         03 39 49  78.4 342.2  0.3     159.4     4    11166   09 22 46
09 27 50  ---          03 44 50  78.1 338.0  0.4     154.4   300    11244   09 22 41

 Next scan frequencies:  43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
 Next BBC frequencies:     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25

09 28 50  3C84         03 45 50  78.0 337.1  0.4     153.5    54    11244   09 28 39
09 29 50  ---          03 46 50  77.9 336.3  0.4     152.5    60    11262   09 28 40

09 30 00  3C84         03 47 00  77.9 336.2  0.4     152.4     4    11262   09 29 56
09 34 00  ---          03 51 01  77.5 333.2  0.5     148.7   240    11325   09 29 51

 Next scan frequencies:  15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
 Next BBC frequencies:     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00

09 35 00  3C84         03 52 01  77.4 332.4  0.5     147.8    54    11325   09 34 49
09 36 00  ---          03 53 01  77.3 331.7  0.5     146.9    60    11343   09 34 50

09 36 10  3C84         03 53 11  77.3 331.6  0.5     146.8     4    11343   09 36 06
09 40 10  ---          03 57 12  76.9 328.8  0.6     143.5   240    11406   09 36 01

 ---------- K-band VLBI scans. Ground segment 05: 2200+420 with EVN+KVN+VLBA+VLA ----------

 Next scan frequencies:  22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
 Next BBC frequencies:     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00

09 44 00  2200+420     04 01 02  20.5 307.9  6.0      66.7   112    11406   09 43 50
09 47 40  ---          04 04 43  19.9 308.2  6.0      66.2   220    11465   09 43 51

09 48 10  2200+420     04 05 13  19.8 308.3  6.0      66.1    24    11465   09 47 59
09 49 10  ---          04 06 13  19.6 308.3  6.0      66.0    60    11484   09 48 00

09 49 20  2200+420     04 06 23  19.6 308.4  6.0      66.0     4    11484   09 49 16
09 53 20  ---          04 10 24  18.9 308.7  6.1      65.4   240    11547   09 49 11

09 53 30  2200+420     04 10 34  18.9 308.7  6.1      65.4     4    11547   09 53 26
09 54 30  ---          04 11 34  18.7 308.8  6.1      65.2    60    11563   09 53 21

09 54 40  2200+420     04 11 44  18.7 308.8  6.1      65.2     4    11563   09 54 36
09 58 40  ---          04 15 45  18.0 309.1  6.2      64.6   240    11626   09 54 31

09 59 10  2200+420     04 16 15  17.9 309.2  6.2      64.6    24    11626   09 58 59
10 00 10  ---          04 17 15  17.8 309.2  6.2      64.4    60    11644   09 59 00
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

10 00 20  2200+420     04 17 25  17.7 309.3  6.2      64.4     4    11644   10 00 16
10 04 20  ---          04 21 26  17.1 309.6  6.3      63.8   240    11707   10 00 11

10 04 30  2200+420     04 21 36  17.0 309.6  6.3      63.8     4    11707   10 04 26
10 05 30  ---          04 22 36  16.9 309.7  6.3      63.6    60    11724   10 04 21

10 05 40  2200+420     04 22 46  16.9 309.7  6.3      63.6     4    11724   10 05 36
10 09 40  ---          04 26 47  16.2 310.1  6.4      63.0   240    11786   10 05 31

 ---------- K-band VLBI scans. Space segment 06: 2200+420 with EVN+KVN ----------

10 10 00  2200+420     04 27 07  16.1 310.1  6.4      63.0    14    11786   10 09 49
10 11 00  ---          04 28 07  16.0 310.2  6.4      62.8    60    11805   10 09 50

10 11 10  2200+420     04 28 17  15.9 310.2  6.4      62.8     4    11805   10 11 06
10 14 55  ---          04 32 02  15.3 310.5  6.5      62.3   225    11864   10 11 01

10 15 05  2200+420     04 32 12  15.3 310.5  6.5      62.3     4    11864   10 15 01
10 16 05  ---          04 33 13  15.1 310.6  6.5      62.1    60    11880   10 14 56

10 16 15  2200+420     04 33 23  15.1 310.6  6.5      62.1     4    11880   10 16 11
10 20 00  ---          04 37 08  14.5 311.0  6.6      61.5   225    11939   10 16 06

10 20 30  2200+420     04 37 38  14.4 311.0  6.6      61.5    24    11939   10 20 19
10 21 30  ---          04 38 39  14.3 311.1  6.6      61.3    60    11958   10 20 20

10 21 40  2200+420     04 38 49  14.2 311.1  6.6      61.3     4    11958   10 21 36
10 25 10  ---          04 42 19  13.7 311.5  6.6      60.8   210    12013   10 21 31

10 25 20  2200+420     04 42 29  13.6 311.5  6.7      60.8     4    12013   10 25 16
10 26 20  ---          04 43 29  13.5 311.6  6.7      60.6    60    12029   10 25 11

10 26 30  2200+420     04 43 39  13.4 311.6  6.7      60.6     4    12029   10 26 26
10 30 00  ---          04 47 10  12.9 311.9  6.7      60.1   210    12084   10 26 21

10 30 30  2200+420     04 47 40  12.8 312.0  6.7      60.0    24    12084   10 30 19
10 31 30  ---          04 48 40  12.6 312.1  6.8      59.8    60    12103   10 30 20

10 31 40  2200+420     04 48 50  12.6 312.1  6.8      59.8     4    12103   10 31 36
10 35 10  ---          04 52 21  12.1 312.4  6.8      59.3   210    12158   10 31 31

10 35 20  2200+420     04 52 31  12.0 312.4  6.8      59.3     4    12158   10 35 16
10 36 20  ---          04 53 31  11.9 312.5  6.8      59.1    60    12174   10 35 11
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               RadioAstron AGN polarization imaging
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   9 Oct 2017   Day 282 ---

10 36 30  2200+420     04 53 41  11.8 312.5  6.8      59.1     4    12174   10 36 26
10 40 00  ---          04 57 12  11.3 312.9  6.9      58.6   210    12229   10 36 21

10 40 30  2200+420     04 57 42  11.2 312.9  6.9      58.5    24    12229   10 40 19
10 41 30  ---          04 58 42  11.1 313.0  6.9      58.4    60    12248   10 40 20

10 41 40  2200+420     04 58 52  11.0 313.0  6.9      58.3     4    12248   10 41 36
10 45 10  ---          05 02 22  10.5 313.4  7.0      57.8   210    12303   10 41 31

10 45 20  2200+420     05 02 32  10.4 313.4  7.0      57.8     4    12303   10 45 16
10 46 20  ---          05 03 33  10.3 313.5  7.0      57.6    60    12319   10 45 11

10 46 30  2200+420     05 03 43  10.3 313.5  7.0      57.6     4    12319   10 46 26
10 50 00  ---          05 07 13   9.7 313.9  7.1      57.1   210    12374   10 46 21

10 50 30  2200+420     05 07 43   9.6 313.9  7.1      57.0    24    12374   10 50 19
10 51 30  ---          05 08 43   9.5 314.0  7.1      56.9    60    12393   10 50 20

10 51 40  2200+420     05 08 53   9.5 314.1  7.1      56.8     4    12393   10 51 36
10 55 10  ---          05 12 24   8.9 314.4  7.1      56.3   210    12448   10 51 31

10 55 20  2200+420     05 12 34   8.9 314.4  7.2      56.3     4    12448   10 55 16
10 56 20  ---          05 13 34   8.7 314.5  7.2      56.1    60    12464   10 55 11

10 56 30  2200+420     05 13 44   8.7 314.6  7.2      56.1     4    12464   10 56 26
11 00 00  ---          05 17 15   8.2 314.9  7.2      55.6   210    12519   10 56 21


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gg083a_freq.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  23  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22156.00  22156.00  22220.00  22220.00  22396.00  22396.00  22460.00  22460.00
   BBC fr=     656.00    656.00    720.00    720.00    896.00    896.00    960.00    960.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     743.99    743.99    919.99    919.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  23  24  25  26  27  28  29  30  31  37

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gg083a_freq.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   37         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00  14600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     10.9     10.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  39  Setup file default.  Used with PCAL = 1MHz
   LO sum=   15273.00  15273.00  15337.00  15337.00  15401.00  15401.00  15503.00  15503.00
   BBC fr=     673.00    673.00    737.00    737.00    801.00    801.00    903.00    903.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     760.99    760.99    824.99    824.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  39  40  41  42  43  44  45  46  47  48

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gg083a_freq.dat:
     v7mm_c8

   Setup group:   49         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  49  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43063.25  43063.25  43127.25  43127.25  43191.25  43191.25  43303.25  43303.25
   BBC fr=     663.25    663.25    727.25    727.25    791.25    791.25    903.25    903.25
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     751.25    751.25    815.25    815.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  49  50  51  52  53  54  55  56  57  58

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 34.789477       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 03.68850        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

   1328+307          13 28 49.657778   * 13 31 08.288070     13 31 55.127711       0.00
   J1331+3030        30 45 58.64060    * 30 30 32.95924      30 25 19.56062        0.00
 * 3C286             ./gg083a_sources.radioastron
                     WSRT calibrator, not for 92cm, rfc_2013d Petrov, 2013, unpublished 542 observati

   0316+413          03 16 29.567283   * 03 19 48.160114     03 20 59.660736       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 21.39346        0.00
 * 3C84              ./gg083a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO3-04, RA-AO2-1

   0355+508          03 55 45.261370   * 03 59 29.747271     04 00 50.453528       0.00
   J0359+5057        50 49 20.28584    * 50 57 50.16179      51 00 34.74763        0.00
 * NRAO150           ./gg083a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 19270 observations, RA-AO3-04, RA-AO2-1

 * 2200+420          22 00 39.362504   * 22 02 43.291371     22 03 28.303492       0.00
   J2202+4216        42 02 08.59073    * 42 16 39.97987      42 22 04.96074        0.00
   BLLAC             ./gg083a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 59417 observations, RA-AO3-04, RA-AO2-1

   2251+158          22 51 29.519741   * 22 53 57.747940     22 54 50.943009       0.00
   J2253+1608        15 52 54.34791    * 16 08 53.56074      16 14 42.95221        0.00
 * 3C454.3           ./gg083a_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 40570 observations, RA-AO3-04, RA-AO2-1



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            16                                6.383     0.000
  3C286      ra1cm2.set            33                                0.322     0.000
             ra2cm2.set            34                                0.317     0.000
             ra7mm2.set            32                                0.322     0.000
  3C84       ra1cm2.set            1 2 3 4 7 9 11 23 33              0.322    47.150
             ra2cm2.set            34 38 39                          0.197    13.016
             ra7mm2.set            21 22 32 49                       0.242    16.917
  NRAO150    ra1cm2.set            1 2 3 4 5 6 7 8 9 11 12 23  +     0.589    81.892
             ra2cm2.set            34 39                             0.200    10.000
             ra7mm2.set            18 21 22 32 49                    0.333    13.083
  2200+420   ra1cm2.set            1 2 3 4 5 6 7 8 9 11 12 17  +    17.874  2530.536
             ra2cm2.set            34 38 39                          0.928    56.510
             ra7mm2.set            18 21 22 32 49                    1.081    82.250
  3C454.3    ra1cm2.set            1 2 3 4 5 6 7 8 9 11 12 17  +     0.267    23.448
             ra2cm2.set            34 39                             0.161     8.250
             ra7mm2.set            18 21 22 32 49                    0.250     6.250


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA              91.3
   3C286               37.5
   3C84               132.6
   NRAO150            121.5
   2200+420           127.1
   3C454.3            148.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

