  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: JUNO tracking
 Exp. Code:  gd023a  


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Dominic Dirkx

Address:  DELFT
 
 
 

Phone:    +31 521 596545
EMAIL:    D.Dirkx@tudelft.nl
Fax:
Phone during observation:

Observing mode:

Notes:    JUNO freq. 8403.5
          v2: sub-arrayed fringe-finders for scans 13:22:30 & 13:56:30
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

 Next scan frequencies:  8400.00  8432.00  8464.00  8496.00
 Next BBC frequencies:    800.00   832.00   864.00   896.00
 Next scan bandwidths:     32.00    32.00    32.00    32.00

08 30 00  J0237+2848   03 08 42  83.4 256.7  0.5      73.0     0        0   08 30 00
08 32 00  =0234+285    03 10 43  83.0 257.8  0.5      73.8   120        8   08 30 01

08 33 00  J0244+1320   03 11 43  71.8 200.4  0.4      17.9    11        8   08 33 00
08 35 00  =0242+131    03 13 43  71.7 201.8  0.5      19.2   120       15   08 33 01

08 36 00  J0242+1411   03 14 43  72.2 205.0  0.5      22.0    50       15   08 36 00
08 37 30  ---          03 16 14  72.1 206.1  0.5      23.0    90       21   08 36 01

08 38 00  083000       03 16 44  72.1 206.8  0.6      23.6    22       21   08 38 00
08 41 00  ---          03 19 44  71.8 209.0  0.6      25.5   180       33   08 38 01

08 42 00  J0242+1411   03 20 44  71.6 209.3  0.6      25.7    53       33   08 42 00
08 43 30  ---          03 22 15  71.5 210.3  0.6      26.6    90       39   08 42 01

08 44 30  J0244+1320   03 23 15  70.8 208.5  0.6      25.0    50       39   08 44 30
08 46 30  =0242+131    03 25 15  70.6 209.8  0.7      26.1   120       46   08 44 31

08 47 00  085000       03 25 45  71.1 213.0  0.7      29.0    20       46   08 47 00
08 50 00  ---          03 28 46  70.7 215.0  0.8      30.6   180       58   08 47 01

08 51 00  J0244+1320   03 29 46  70.1 212.7  0.7      28.6    50       58   08 51 00
08 53 00  =0242+131    03 31 46  69.8 214.0  0.8      29.6   120       66   08 51 01

08 53 30  085000       03 32 16  70.3 217.1  0.8      32.4    20       66   08 53 30
08 56 30  ---          03 35 17  69.9 218.9  0.9      33.9   180       77   08 53 31

08 57 30  J0244+1320   03 36 17  69.3 216.7  0.8      31.9    50       77   08 57 30
08 59 30  =0242+131    03 38 17  69.0 217.8  0.9      32.9   120       85   08 57 31

09 00 00  085000       03 38 47  69.4 220.9  0.9      35.6    20       85   09 00 00
09 03 00  ---          03 41 48  69.0 222.6  1.0      36.9   180       97   09 00 01

09 04 00  J0244+1320   03 42 48  68.4 220.3  0.9      34.9    50       97   09 04 00
09 06 00  =0242+131    03 44 48  68.1 221.4  1.0      35.8   120      104   09 04 01

09 06 30  091000       03 45 18  68.4 224.4  1.0      38.5    20      104   09 06 30
09 09 30  ---          03 48 19  68.0 226.0  1.1      39.7   180      116   09 06 31

09 10 30  J0244+1320   03 49 19  67.5 223.7  1.1      37.7    50      116   09 10 30
09 12 30  =0242+131    03 51 19  67.2 224.7  1.1      38.5   120      124   09 10 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

09 13 00  091000       03 51 49  67.4 227.7  1.1      41.0    20      124   09 13 00
09 16 00  ---          03 54 50  67.0 229.1  1.2      42.2   180      135   09 13 01

09 17 00  J0244+1320   03 55 50  66.5 226.9  1.2      40.2    50      135   09 17 00
09 19 00  =0242+131    03 57 50  66.1 227.8  1.2      41.0   120      143   09 17 01

09 19 30  091000       03 58 20  66.4 230.7  1.2      43.4    20      143   09 19 30
09 22 30  ---          04 01 21  65.9 232.0  1.3      44.4   180      155   09 19 31

09 23 30  J0244+1320   04 02 21  65.4 229.8  1.3      42.5    50      155   09 23 30
09 25 30  =0242+131    04 04 21  65.1 230.7  1.3      43.2   120      162   09 23 31

09 26 00  093000       04 04 52  65.3 233.4  1.4      45.5    20      162   09 26 00
09 29 00  ---          04 07 52  64.7 234.6  1.4      46.4   180      174   09 26 01

09 30 00  J0244+1320   04 08 52  64.3 232.5  1.4      44.6    50      174   09 30 00
09 32 00  =0242+131    04 10 53  64.0 233.3  1.4      45.2   120      182   09 30 01

09 32 30  093000       04 11 23  64.1 236.0  1.5      47.4    20      182   09 32 30
09 35 30  ---          04 14 23  63.6 237.1  1.5      48.2   180      193   09 32 31

09 36 30  J0244+1320   04 15 23  63.2 235.0  1.5      46.5    50      193   09 36 30
09 38 30  =0242+131    04 17 24  62.8 235.8  1.5      47.0   120      201   09 36 31

09 39 00  093000       04 17 54  62.9 238.3  1.6      49.1    20      201   09 39 00
09 42 00  ---          04 20 54  62.4 239.3  1.6      49.8   180      213   09 39 01

09 43 00  J0244+1320   04 21 54  62.0 237.4  1.6      48.2    50      213   09 43 00
09 45 00  =0242+131    04 23 55  61.7 238.0  1.6      48.6   120      220   09 43 01

09 46 00  J0242+1411   04 24 55  61.7 240.4  1.7      50.5    51      220   09 46 00
09 47 30  ---          04 26 25  61.4 240.9  1.7      50.9    90      226   09 46 01

09 48 00  095000       04 26 55  61.3 241.3  1.7      51.2    23      226   09 48 00
09 51 00  ---          04 29 56  60.7 242.2  1.8      51.8   180      238   09 48 01

09 52 00  J0242+1411   04 30 56  60.5 242.3  1.8      51.8    53      238   09 52 00
09 53 30  ---          04 32 26  60.3 242.7  1.8      52.1    90      243   09 52 01

09 54 30  J0244+1320   04 33 26  59.9 241.1  1.8      50.8    51      243   09 54 30
09 56 30  =0242+131    04 35 27  59.5 241.7  1.8      51.2   120      251   09 54 31

09 57 00  095000       04 35 57  59.5 244.0  1.9      53.0    21      251   09 57 00
10 00 00  ---          04 38 57  59.0 244.9  1.9      53.5   180      263   09 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

10 01 00  J0244+1320   04 39 57  58.7 243.1  1.9      52.1    51      263   10 01 00
10 03 00  =0242+131    04 41 58  58.3 243.6  1.9      52.4   120      271   10 01 01

10 03 30  101000       04 42 28  58.3 245.8  2.0      54.1    21      271   10 03 30
10 06 30  ---          04 45 28  57.7 246.6  2.0      54.6   180      282   10 03 31

10 07 30  J0244+1320   04 46 28  57.4 244.9  2.0      53.2    51      282   10 07 30
10 09 30  =0242+131    04 48 29  57.0 245.4  2.0      53.6   120      290   10 07 31

10 10 00  101000       04 48 59  57.0 247.5  2.1      55.2    21      290   10 10 00
10 13 00  ---          04 51 59  56.4 248.3  2.1      55.6   180      301   10 10 01

10 14 00  J0244+1320   04 52 59  56.1 246.6  2.1      54.3    51      301   10 14 00
10 16 00  =0242+131    04 55 00  55.7 247.1  2.1      54.6   120      309   10 14 01

10 16 30  101000       04 55 30  55.7 249.2  2.2      56.1    21      309   10 16 30
10 19 30  ---          04 58 30  55.1 249.9  2.2      56.5   180      321   10 16 31

10 20 30  J0244+1320   04 59 30  54.8 248.2  2.2      55.2    51      321   10 20 30
10 22 30  =0242+131    05 01 31  54.4 248.7  2.3      55.5   120      328   10 20 31

10 23 00  103000       05 02 01  54.4 250.7  2.3      57.0    21      328   10 23 00
10 26 00  ---          05 05 01  53.8 251.3  2.4      57.3   180      340   10 23 01

10 27 00  J0244+1320   05 06 02  53.5 249.7  2.3      56.1    51      340   10 27 00
10 29 00  =0242+131    05 08 02  53.1 250.2  2.4      56.3   120      348   10 27 01

10 29 30  103000       05 08 32  53.0 252.1  2.4      57.7    21      348   10 29 30
10 32 30  ---          05 11 32  52.4 252.8  2.5      58.0   180      359   10 29 31

10 33 30  J0244+1320   05 12 33  52.2 251.2  2.4      56.9    51      359   10 33 30
10 35 30  =0242+131    05 14 33  51.8 251.6  2.5      57.1   120      367   10 33 31

10 36 00  103000       05 15 03  51.7 253.5  2.5      58.4    21      367   10 36 00
10 39 00  ---          05 18 04  51.1 254.1  2.6      58.7   180      379   10 36 01

10 40 00  J0244+1320   05 19 04  50.9 252.5  2.5      57.6    51      379   10 40 00
10 42 00  =0242+131    05 21 04  50.5 253.0  2.6      57.8   120      386   10 40 01

10 42 30  105000       05 21 34  50.4 254.8  2.6      59.0    21      386   10 42 30
10 45 30  ---          05 24 35  49.7 255.4  2.7      59.3   180      398   10 42 31

10 46 30  J0244+1320   05 25 35  49.5 253.9  2.7      58.2    51      398   10 46 30
10 48 30  =0242+131    05 27 35  49.1 254.3  2.7      58.4   120      406   10 46 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

10 49 00  105000       05 28 05  49.0 256.0  2.7      59.5    21      406   10 49 00
10 52 00  ---          05 31 06  48.4 256.6  2.8      59.8   180      417   10 49 01

10 53 00  J0244+1320   05 32 06  48.2 255.1  2.8      58.8    51      417   10 53 00
10 55 00  =0242+131    05 34 06  47.8 255.5  2.8      58.9   120      425   10 53 01

10 55 30  105000       05 34 36  47.6 257.2  2.8      60.0    21      425   10 55 30
10 58 30  ---          05 37 37  47.0 257.8  2.9      60.2   180      437   10 55 31

10 59 30  J0244+1320   05 38 37  46.8 256.3  2.9      59.3    51      437   10 59 30
11 01 30  =0242+131    05 40 37  46.4 256.7  2.9      59.4   120      444   10 59 31

11 02 00  111000       05 41 07  46.3 258.4  3.0      60.5    21      444   11 02 00
11 05 00  ---          05 44 08  45.6 258.9  3.0      60.6   180      456   11 02 01

11 06 00  J0244+1320   05 45 08  45.4 257.5  3.0      59.7    51      456   11 06 00
11 08 00  =0242+131    05 47 08  45.0 257.8  3.0      59.9   120      464   11 06 01

11 08 30  111000       05 47 38  44.9 259.5  3.1      60.8    21      464   11 08 30
11 11 30  ---          05 50 39  44.3 260.0  3.1      61.0   180      475   11 08 31

11 12 30  J0244+1320   05 51 39  44.1 258.6  3.1      60.1    51      475   11 12 30
11 14 30  =0242+131    05 53 39  43.7 258.9  3.1      60.3   120      483   11 12 31

11 15 00  111000       05 54 09  43.5 260.5  3.2      61.2    21      483   11 15 00
11 18 00  ---          05 57 10  42.9 261.0  3.2      61.3   180      495   11 15 01

11 19 00  J0244+1320   05 58 10  42.7 259.7  3.2      60.5    51      495   11 19 00
11 21 00  =0242+131    06 00 10  42.3 260.0  3.2      60.6   120      502   11 19 01

11 22 00  J0242+1411   06 01 11  42.1 261.5  3.3      61.4    51      502   11 22 00
11 23 30  ---          06 02 41  41.7 261.7  3.3      61.5    90      508   11 22 01

11 24 00  113000       06 03 11  41.6 262.0  3.3      61.6    23      508   11 24 00
11 27 00  ---          06 06 11  41.0 262.4  3.4      61.7   180      520   11 24 01

11 28 00  J0242+1411   06 07 12  40.8 262.4  3.4      61.7    53      520   11 28 00
11 29 30  ---          06 08 42  40.5 262.6  3.4      61.7    90      526   11 28 01

11 30 30  J0244+1320   06 09 42  40.3 261.5  3.4      61.0    51      526   11 30 30
11 32 30  =0242+131    06 11 42  39.8 261.8  3.4      61.1   120      533   11 30 31

11 33 00  115000       06 12 12  39.7 263.3  3.5      61.9    21      533   11 33 00
11 36 00  ---          06 15 13  39.0 263.8  3.5      62.0   180      545   11 33 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

11 37 00  J0244+1320   06 16 13  38.9 262.5  3.5      61.3    51      545   11 37 00
11 39 00  =0242+131    06 18 13  38.4 262.8  3.5      61.4   120      553   11 37 01

11 39 30  115000       06 18 43  38.3 264.3  3.6      62.1    21      553   11 39 30
11 42 30  ---          06 21 44  37.6 264.7  3.6      62.2   180      564   11 39 31

11 43 30  J0244+1320   06 22 44  37.5 263.5  3.6      61.5    51      564   11 43 30
11 45 30  =0242+131    06 24 44  37.0 263.8  3.6      61.6   120      572   11 43 31

11 46 00  115000       06 25 15  36.9 265.2  3.7      62.3    21      572   11 46 00
11 49 00  ---          06 28 15  36.2 265.6  3.7      62.3   180      584   11 46 01

11 50 00  J0244+1320   06 29 15  36.1 264.4  3.7      61.7    51      584   11 50 00
11 52 00  =0242+131    06 31 16  35.6 264.7  3.8      61.7   120      591   11 50 01

11 52 30  121000       06 31 46  35.5 266.1  3.8      62.4    21      591   11 52 30
11 55 30  ---          06 34 46  34.8 266.5  3.8      62.4   180      603   11 52 31

11 56 30  J0244+1320   06 35 46  34.7 265.3  3.8      61.9    51      603   11 56 30
11 58 30  =0242+131    06 37 47  34.3 265.6  3.9      61.9   120      611   11 56 31

11 59 00  121000       06 38 17  34.1 267.0  3.9      62.5    21      611   11 59 00
12 02 00  ---          06 41 17  33.4 267.4  4.0      62.5   180      622   11 59 01

12 03 00  J0244+1320   06 42 17  33.3 266.2  3.9      62.0    51      622   12 03 00
12 05 00  =0242+131    06 44 18  32.9 266.5  4.0      62.0   120      630   12 03 01

12 05 30  121000       06 44 48  32.7 267.9  4.0      62.6    21      630   12 05 30
12 08 30  ---          06 47 48  32.0 268.3  4.1      62.6   180      642   12 05 31

12 09 30  J0244+1320   06 48 48  31.9 267.1  4.0      62.1    51      642   12 09 30
12 11 30  =0242+131    06 50 49  31.5 267.4  4.1      62.1   120      649   12 09 31

12 12 00  121000       06 51 19  31.3 268.7  4.1      62.6    21      649   12 12 00
12 15 00  ---          06 54 19  30.6 269.1  4.2      62.6   180      661   12 12 01

12 16 00  J0244+1320   06 55 19  30.5 268.0  4.2      62.1    51      661   12 16 00
12 18 00  =0242+131    06 57 20  30.1 268.2  4.2      62.2   120      669   12 16 01

12 18 30  121000       06 57 50  29.9 269.6  4.2      62.6    21      669   12 18 30
12 21 30  ---          07 00 50  29.2 269.9  4.3      62.6   180      680   12 18 31

12 22 30  J0244+1320   07 01 51  29.1 268.8  4.3      62.2    51      680   12 22 30
12 24 30  =0242+131    07 03 51  28.6 269.1  4.3      62.2   120      688   12 22 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

12 25 00  123000       07 04 21  28.5 270.4  4.3      62.6    21      688   12 25 00
12 28 00  ---          07 07 21  27.8 270.8  4.4      62.6   180      699   12 25 01

12 29 00  J0244+1320   07 08 22  27.7 269.7  4.4      62.2    51      699   12 29 00
12 31 00  =0242+131    07 10 22  27.2 269.9  4.4      62.2   120      707   12 29 01

12 31 30  123000       07 10 52  27.1 271.2  4.5      62.6    21      707   12 31 30
12 34 30  ---          07 13 52  26.4 271.6  4.5      62.6   180      719   12 31 31

12 35 30  J0244+1320   07 14 53  26.3 270.5  4.5      62.2    51      719   12 35 30
12 37 30  =0242+131    07 16 53  25.8 270.8  4.5      62.2   120      727   12 35 31

12 38 30  J0242+1411   07 17 53  25.6 272.0  4.6      62.5    52      727   12 38 30
12 40 00  ---          07 19 23  25.3 272.2  4.6      62.5    90      732   12 38 31

12 40 30  125000       07 19 53  25.1 272.3  4.6      62.6    23      732   12 40 30
12 43 30  ---          07 22 54  24.5 272.7  4.7      62.5   180      744   12 40 31

12 44 30  J0242+1411   07 23 54  24.3 272.7  4.7      62.5    53      744   12 44 30
12 46 00  ---          07 25 24  24.0 272.9  4.7      62.5    90      750   12 44 31

12 47 00  J0244+1320   07 26 25  23.8 271.9  4.7      62.1    52      750   12 47 00
12 49 00  =0242+131    07 28 25  23.4 272.2  4.7      62.1   120      757   12 47 01

12 49 30  125000       07 28 55  23.2 273.4  4.8      62.4    21      757   12 49 30
12 52 30  ---          07 31 55  22.5 273.8  4.8      62.4   180      769   12 49 31

12 53 30  J0244+1320   07 32 56  22.4 272.8  4.8      62.1    52      769   12 53 30
12 55 30  =0242+131    07 34 56  22.0 273.0  4.8      62.1   120      777   12 53 31

12 56 00  125000       07 35 26  21.8 274.2  4.9      62.3    22      777   12 56 00
12 59 00  ---          07 38 27  21.1 274.6  4.9      62.3   180      788   12 56 01

13 00 00  J0244+1320   07 39 27  21.0 273.6  4.9      62.0    52      788   13 00 00
13 02 00  =0242+131    07 41 27  20.6 273.8  4.9      62.0   120      796   13 00 01

13 02 30  125000       07 41 57  20.4 275.0  5.0      62.2    22      796   13 02 30
13 05 30  ---          07 44 58  19.8 275.4  5.0      62.2   180      808   13 02 31

13 06 30  J0244+1320   07 45 58  19.6 274.3  5.0      61.9    52      808   13 06 30
13 08 30  =0242+131    07 47 58  19.2 274.6  5.0      61.9   120      815   13 06 31

13 09 00  131000       07 48 28  19.0 275.8  5.1      62.1    22      815   13 09 00
13 12 00  ---          07 51 29  18.4 276.1  5.1      62.0   180      827   13 09 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  15 Oct 2023   Day 288 ---

13 13 00  J0244+1320   07 52 29  18.2 275.1  5.1      61.8    52      827   13 13 00
13 15 00  =0242+131    07 54 29  17.8 275.4  5.1      61.7   120      835   13 13 01

13 15 30  131000       07 54 59  17.6 276.6  5.2      61.9    22      835   13 15 30
13 18 30  ---          07 58 00  17.0 276.9  5.2      61.8   180      846   13 15 31

13 19 30  J0244+1320   07 59 00  16.8 275.9  5.2      61.6    52      846   13 19 30
13 21 30  =0242+131    08 01 00  16.4 276.2  5.2      61.6   120      854   13 19 31

13 22 30  J0237+2848   08 02 00  21.6 291.7  5.4      66.0    41      854   13 22 30
13 24 30  =0234+285    08 04 01  21.2 291.9  5.4      65.8   120      862   13 22 31

13 25 00  133000       08 04 31  15.6 277.7  5.3      61.7    11      862   13 25 00
13 28 00  ---          08 07 31  14.9 278.1  5.4      61.6   180      873   13 25 01

13 29 00  J0244+1320   08 08 31  14.8 277.1  5.4      61.4    52      873   13 29 00
13 31 00  =0242+131    08 10 32  14.3 277.3  5.4      61.3   120      881   13 29 01

13 31 30  133000       08 11 02  14.2 278.5  5.5      61.5    22      881   13 31 30
13 34 30  ---          08 14 02  13.5 278.8  5.5      61.4   180      893   13 31 31

13 35 30  J0244+1320   08 15 03  13.4 277.9  5.5      61.2    52      893   13 35 30
13 37 30  =0242+131    08 17 03  13.0 278.1  5.5      61.1   120      900   13 35 31

13 38 00  135000       08 17 33  12.8 279.3  5.6      61.2    22      900   13 38 00
13 41 00  ---          08 20 33  12.2 279.6  5.6      61.1   180      912   13 38 01

13 42 00  J0244+1320   08 21 34  12.0 278.6  5.6      61.0    52      912   13 42 00
13 44 00  =0242+131    08 23 34  11.6 278.9  5.6      60.9   120      920   13 42 01

13 56 30  J0530+1331   08 36 06  44.5 258.5  3.1      60.1   672      920   13 56 30
14 00 00  =0528+134    08 39 37  43.8 259.0  3.1      60.3   210      933   13 56 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess323.X512Rglob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    2         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       RCP       RCP       RCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        B         B         B         B 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   1  Setup file default.  Used with PCAL = off
   LO sum=   8400.00  8432.00  8464.00  8496.00
   BBC fr=    800.00   832.00   864.00   896.00
   Bandwd=     32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     808.00    840.00    872.00    904.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   1   2   3   4   5   6   7   8   9  10

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   0234+285          02 34 55.589590   * 02 37 52.405677     02 39 17.277395       0.00
 * J0237+2848        28 35 11.40773    * 28 48 08.98999      28 54 23.22629        0.00
   J0237+28          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  58420 observations.

   0235+164          02 35 52.630214   * 02 38 38.930106     02 39 58.751782       0.12
 * J0238+1636        16 24 04.01612    * 16 36 59.27454      16 43 14.15676        0.16
   J0238+16          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  64441 observations.

   0242+131          02 42 01.666226   * 02 44 45.693338     02 46 04.425785       0.14
 * J0244+1320        13 07 29.20762    * 13 20 07.22120      13 26 14.36013        0.27
                     /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,     84 observations.

   0528+134          05 28 06.759216   * 05 30 56.416746     05 32 17.247102       0.21
 * J0530+1331        13 29 42.28882    * 13 31 55.14948      13 33 05.83047        0.24
   J0530+13          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution, 138236 observations.

 * J0242+1411        02 40 04.778041   * 02 42 49.390000     02 44 08.402872       0.00
                     13 58 53.56084    * 14 11 37.10000      14 17 46.74198        0.00
                     ./sources.gd23a.coord

 * 083000            02 39 38.362979   * 02 42 23.010000     02 43 42.040147       0.00
                     14 03 20.61683    * 14 16 05.40000      14 22 15.62202        0.00
                     ./sources.gd23a.coord

 * 085000            02 39 38.521716   * 02 42 23.170000     02 43 42.200744       0.00
                     14 03 25.62434    * 14 16 10.40000      14 22 20.61827        0.00
                     ./sources.gd23a.coord

 * 091000            02 39 38.720416   * 02 42 23.370000     02 43 42.401357       0.00
                     14 03 30.63374    * 14 16 15.40000      14 22 25.61362        0.00
                     ./sources.gd23a.coord

 * 093000            02 39 38.969046   * 02 42 23.620000     02 43 42.652001       0.00
                     14 03 35.74548    * 14 16 20.50000      14 22 30.70786        0.00
                     ./sources.gd23a.coord

 * 095000            02 39 39.277642   * 02 42 23.930000     02 43 42.962661       0.00
                     14 03 40.76006    * 14 16 25.50000      14 22 35.70076        0.00
                     ./sources.gd23a.coord

 * 101000            02 39 39.676198   * 02 42 24.330000     02 43 43.363337       0.00
                     14 03 45.57887    * 14 16 30.30000      14 22 40.49166        0.00
                     ./sources.gd23a.coord

 * 103000            02 39 40.184740   * 02 42 24.840000     02 43 43.874018       0.00
                     14 03 50.00286    * 14 16 34.70000      14 22 44.88011        0.00
                     ./sources.gd23a.coord

 * 105000            02 39 40.843452   * 02 42 25.500000     02 43 44.534614       0.00
                     14 03 53.03391    * 14 16 37.70000      14 22 47.86527        0.00
                     ./sources.gd23a.coord

 * 111000            02 39 41.712769   * 02 42 26.370000     02 43 45.404919       0.00
                     14 03 52.47487    * 14 16 37.10000      14 22 47.24586        0.00
                     ./sources.gd23a.coord

 * 113000            02 39 42.673781   * 02 42 27.330000     02 43 46.364415       0.00
                     14 03 43.92010    * 14 16 28.50000      14 22 38.62472        0.00
                     ./sources.gd23a.coord

 * 115000            02 39 43.297005   * 02 42 27.950000     02 43 46.982869       0.00
                     14 03 26.84936    * 14 16 11.40000      14 22 21.51149        0.00
                     ./sources.gd23a.coord

 * 121000            02 39 43.491056   * 02 42 28.140000     02 43 47.170940       0.00
                     14 03 07.85838    * 14 15 52.40000      14 22 02.50792        0.00
                     ./sources.gd23a.coord

 * 123000            02 39 43.455100   * 02 42 28.100000     02 43 47.129020       0.00
                     14 02 49.85656    * 14 15 34.40000      14 21 44.50946        0.00
                     ./sources.gd23a.coord

 * 125000            02 39 43.279008   * 02 42 27.920000     02 43 46.947168       0.00
                     14 02 33.04815    * 14 15 17.60000      14 21 27.71408        0.00
                     ./sources.gd23a.coord

 * 131000            02 39 43.022724   * 02 42 27.660000     02 43 46.685409       0.00
                     14 02 17.43597    * 14 15 02.00000      14 21 12.12044        0.00
                     ./sources.gd23a.coord

 * 133000            02 39 42.716308   * 02 42 27.350000     02 43 46.373714       0.00
                     14 02 02.62143    * 14 14 47.20000      14 20 57.32789        0.00
                     ./sources.gd23a.coord

 * 135000            02 39 42.369774   * 02 42 27.000000     02 43 46.022076       0.00
                     14 01 48.50501    * 14 14 33.10000      14 20 43.23621        0.00
                     ./sources.gd23a.coord



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J0237+2848 sess323.X512Rglob     1                                 0.067     2.433
  J0238+1636 sess323.X512Rglob     11 12 13 14 15 17 18 19 21  +     0.092     6.050
  J0244+1320 sess323.X512Rglob     1 11 12 13 14 15 17 18 19 2 +     1.533   169.800
  J0530+1331 sess323.X512Rglob     1                                 0.058     2.418
  J0242+1411 sess323.X512Rglob     1 11 12 13 14 15 17 18 19 2 +     0.250    27.950
  083000     sess323.X512Rglob     1                                 0.050     2.250
  085000     sess323.X512Rglob     1 11                              0.150     8.250
  091000     sess323.X512Rglob     1 11                              0.150     8.250
  093000     sess323.X512Rglob     1 11                              0.150     8.250
  095000     sess323.X512Rglob     1 11                              0.100     5.500
  101000     sess323.X512Rglob     1 11                              0.150     8.250
  103000     sess323.X512Rglob     1 11 12                           0.150     9.900
  105000     sess323.X512Rglob     1 11 12 13 14 15                  0.150    15.150
  111000     sess323.X512Rglob     1 11 12 13 14 15 17 18            0.150    21.300
  113000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19         0.050     7.650
  115000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19         0.150    22.950
  121000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19         0.250    36.550
  123000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19         0.100    15.300
  125000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19         0.200    30.600
  131000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19 2 +     0.100    19.000
  133000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19 2 +     0.100    17.100
  135000     sess323.X512Rglob     1 11 12 13 14 15 17 18 19 2 +     0.100    16.200


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0237+2848         152.5
   J0238+1636         159.0
   J0244+1320         158.5
   J0530+1331         118.2
   J0242+1411         158.8
   083000             158.9
   085000             158.9
   091000             158.9
   093000             158.9
   095000             158.9
   101000             158.9
   103000             158.9
   105000             158.9
   111000             158.9
   113000             158.9
   115000             158.9
   121000             158.9
   123000             158.9
   125000             158.9
   131000             158.9
   133000             158.9
   135000             158.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

