  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GG088
 Exp. Code:  GG088   


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Stefano Giarratana

Address:  OAB
          Via Emilio Bianchi
          Merate
          Italy

Phone:    +393487994415
EMAIL:    stefano.giarratana@inaf.it
Fax:
Phone during observation:

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
          v2: LBA pre-science 6hr ftp-fringe test, VLA ~10min autophase
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

 Next scan frequencies:  4612.00  4612.00  4740.00  4740.00  4868.00  4868.00  4996.00  4996.00
 Next BBC frequencies:    512.00   512.00   640.00   640.00   768.00   768.00   896.00   896.00
 Next scan bandwidths:    128.00   128.00   128.00   128.00   128.00   128.00   128.00   128.00

18 33 20 J191142+1952  14 07 56  21.5  78.9 -5.1     -63.9     0        0   18 33 20
18 34 25  ---          14 09 01  21.7  79.0 -5.1     -64.0    65       33   18 33 21

18 34 25 J191249+1940  14 09 01  21.4  79.1 -5.1     -63.8    -8       33   18 34 33
18 35 55  ---          14 10 31  21.7  79.3 -5.1     -63.9    82       76   18 34 26

18 35 55 J191142+1952  14 10 31  22.0  79.2 -5.0     -64.0    -8       76   18 36 03
18 37 25  ---          14 12 02  22.4  79.4 -5.0     -64.1    82      118   18 35 56

18 37 25  GRB221009A   14 12 02  22.0  79.3 -5.0     -64.0    -8      118   18 37 33
18 42 00  ---          14 16 37  23.0  79.8 -5.0     -64.2   267      256   18 37 26

18 42 20 J191142+1952  14 16 57  23.4  79.9 -4.9     -64.3    12      256   18 42 20
18 43 25  ---          14 18 03  23.6  80.0 -4.9     -64.3    65      289   18 42 21

18 43 25  GRB221009A   14 18 03  23.3  80.0 -4.9     -64.2    -8      289   18 43 33
18 48 00  ---          14 22 38  24.3  80.5 -4.9     -64.4   267      427   18 43 26

18 48 20 J191142+1952  14 22 58  24.7  80.6 -4.8     -64.5    12      427   18 48 20
18 49 25  ---          14 24 04  24.9  80.7 -4.8     -64.6    65      460   18 48 21

18 50 05  J1925+2106   14 24 44  22.6  78.0 -5.0     -64.5    27      460   18 50 05
18 53 25  =1923+210    14 28 04  23.3  78.3 -5.0     -64.6   200      563   18 50 06

18 53 45 J191142+1952  14 28 24  25.8  81.2 -4.7     -64.7     7      563   18 53 45
18 55 15  ---          14 29 55  26.1  81.4 -4.7     -64.8    90      610   18 53 46

18 55 15  GRB221009A   14 29 55  25.8  81.3 -4.7     -64.7    -8      610   18 55 23
18 59 50  ---          14 34 30  26.8  81.8 -4.7     -64.9   267      747   18 55 16

19 00 05  J1925+2106   14 34 45  24.7  79.1 -4.9     -64.9     3      747   19 00 05
19 01 05  =1923+210    14 35 45  24.9  79.2 -4.9     -65.0    60      778   19 00 06

19 01 20 J191142+1952  14 36 01  27.4  82.0 -4.6     -65.0     2      778   19 01 20
19 02 30  ---          14 37 11  27.7  82.2 -4.6     -65.0    70      814   19 01 21

19 02 30  GRB221009A   14 37 11  27.4  82.1 -4.6     -65.0    -8      814   19 02 38
19 07 05  ---          14 41 46  28.3  82.6 -4.5     -65.1   267      952   19 02 31

19 07 25 J191142+1952  14 42 07  28.7  82.7 -4.5     -65.2    12      952   19 07 25
19 08 30  ---          14 43 12  29.0  82.9 -4.5     -65.2    65      985   19 07 26
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

19 08 30  J1905+1943   14 43 12  30.2  83.7 -4.4     -65.3   -11      985   19 08 41
19 10 15  ---          14 44 57  30.6  83.9 -4.4     -65.4    94     1034   19 08 31

19 10 15 J191142+1952  14 44 57  29.4  83.0 -4.5     -65.3   -10     1034   19 10 25
19 11 40  ---          14 46 22  29.7  83.2 -4.4     -65.3    75     1072   19 10 16

19 11 55  J1925+2106   14 46 37  27.2  80.4 -4.7     -65.5     2     1072   19 11 55
19 12 55  =1923+210    14 47 37  27.4  80.5 -4.7     -65.5    60     1103   19 11 56

19 13 05  GRB221009A   14 47 47  29.6  83.3 -4.4     -65.3    -2     1103   19 13 07
19 17 30  ---          14 52 13  30.6  83.8 -4.4     -65.4   263     1239   19 13 06

19 17 50 J191142+1952  14 52 33  31.0  83.9 -4.3     -65.5    12     1239   19 17 50
19 19 15  ---          14 53 58  31.3  84.1 -4.3     -65.5    85     1283   19 17 51

19 19 15  GRB221009A   14 53 58  31.0  84.0 -4.3     -65.5    -8     1283   19 19 23
19 23 50  ---          14 58 34  31.9  84.5 -4.3     -65.6   267     1420   19 19 16

19 24 05  J1925+2106   14 58 49  29.8  81.7 -4.5     -65.9     3     1420   19 24 05
19 25 05  =1923+210    14 59 49  30.0  81.8 -4.5     -66.0    60     1451   19 24 06

19 25 20 J191142+1952  15 00 04  32.6  84.8 -4.2     -65.7     2     1451   19 25 20
19 26 45  ---          15 01 30  32.9  84.9 -4.2     -65.7    85     1495   19 25 21

19 26 45  J1923+2010   15 01 30  30.6  83.3 -4.4     -65.6   -13     1495   19 26 58
19 28 20  ---          15 03 05  30.9  83.5 -4.4     -65.6    82     1537   19 26 46

19 28 40 J191142+1952  15 03 25  33.3  85.2 -4.2     -65.8     7     1537   19 28 40
19 30 10  ---          15 04 55  33.6  85.3 -4.1     -65.8    90     1583   19 28 41

19 30 10  GRB221009A   15 04 55  33.3  85.3 -4.2     -65.7    -8     1583   19 30 18
19 34 45  ---          15 09 31  34.3  85.8 -4.1     -65.8   267     1721   19 30 11

19 35 00  J1925+2106   15 09 46  32.1  82.9 -4.3     -66.3     3     1721   19 35 00
19 36 00  =1923+210    15 10 46  32.3  83.0 -4.3     -66.3    60     1752   19 35 01

19 36 10 J191142+1952  15 10 56  34.9  86.0 -4.0     -65.9    -3     1752   19 36 13
19 37 25  ---          15 12 11  35.2  86.2 -4.0     -65.9    72     1789   19 36 11

19 37 25  GRB221009A   15 12 11  34.9  86.1 -4.0     -65.9    -8     1789   19 37 33
19 42 00  ---          15 16 47  35.8  86.7 -4.0     -65.9   267     1927   19 37 26

19 42 20 J191142+1952  15 17 07  36.2  86.8 -3.9     -66.0    12     1927   19 42 20
19 43 25  ---          15 18 12  36.5  86.9 -3.9     -66.0    65     1960   19 42 21
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

19 43 40  J1925+2106   15 18 27  34.0  83.9 -4.1     -66.5     2     1960   19 43 40
19 44 40  =1923+210    15 19 28  34.2  84.0 -4.1     -66.6    60     1991   19 43 41

19 45 00 J191249+1940  15 19 48  36.5  87.2 -3.9     -65.9     8     1991   19 45 00
19 46 30  ---          15 21 18  36.8  87.3 -3.9     -65.9    90     2037   19 45 01

19 46 50 J191142+1952  15 21 38  37.2  87.3 -3.9     -66.1    12     2037   19 46 50
19 48 00  ---          15 22 48  37.5  87.4 -3.8     -66.1    70     2073   19 46 51

19 48 00  GRB221009A   15 22 48  37.1  87.4 -3.9     -66.0    -8     2073   19 48 08
19 52 35  ---          15 27 24  38.1  87.9 -3.8     -66.1   267     2211   19 48 01

19 52 50  J1925+2106   15 27 39  35.9  84.9 -4.0     -66.8     3     2211   19 52 50
19 53 50  =1923+210    15 28 39  36.2  85.0 -4.0     -66.8    60     2242   19 52 51

19 54 05 J191142+1952  15 28 54  38.8  88.2 -3.7     -66.2     2     2242   19 54 05
19 55 15  ---          15 30 04  39.0  88.3 -3.7     -66.2    70     2278   19 54 06

19 55 15  GRB221009A   15 30 04  38.7  88.3 -3.7     -66.1    -8     2278   19 55 23
19 59 50  ---          15 34 40  39.7  88.8 -3.7     -66.1   267     2416   19 55 16

20 00 10 J191142+1952  15 35 00  40.1  88.9 -3.6     -66.2    12     2416   20 00 10
20 01 15  ---          15 36 05  40.3  89.1 -3.6     -66.2    65     2449   20 00 11

20 01 15  J1905+1943   15 36 05  41.6  90.0 -3.5     -66.1   -11     2449   20 01 26
20 03 00  ---          15 37 51  42.0  90.2 -3.5     -66.1    94     2498   20 01 16

20 03 00 J191142+1952  15 37 51  40.7  89.3 -3.6     -66.2   -10     2498   20 03 10
20 04 25  ---          15 39 16  41.0  89.5 -3.6     -66.2    75     2536   20 03 01

20 04 40  J1925+2106   15 39 31  38.5  86.3 -3.8     -67.0     2     2536   20 04 40
20 05 40  =1923+210    15 40 31  38.7  86.4 -3.8     -67.0    60     2567   20 04 41

20 05 50  GRB221009A   15 40 41  41.0  89.6 -3.6     -66.1    -2     2567   20 05 52
20 10 15  ---          15 45 07  41.9  90.1 -3.5     -66.1   263     2703   20 05 51

20 10 35 J191142+1952  15 45 27  42.3  90.2 -3.5     -66.2    12     2703   20 10 35
20 12 00  ---          15 46 52  42.6  90.4 -3.4     -66.2    85     2746   20 10 36

20 12 00  GRB221009A   15 46 52  42.3  90.4 -3.5     -66.1    -8     2746   20 12 08
20 16 35  ---          15 51 28  43.3  91.0 -3.4     -66.1   267     2884   20 12 01

20 16 50  J1925+2106   15 51 43  41.1  87.7 -3.6     -67.2     3     2884   20 16 50
20 17 50  =1923+210    15 52 43  41.3  87.8 -3.6     -67.2    60     2915   20 16 51
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

20 18 05 J191142+1952  15 52 58  44.0  91.2 -3.3     -66.2     2     2915   20 18 05
20 19 30  ---          15 54 23  44.3  91.4 -3.3     -66.2    85     2959   20 18 06

20 19 30  J1923+2010   15 54 23  41.9  89.5 -3.5     -66.5   -13     2959   20 19 43
20 21 05  ---          15 55 59  42.3  89.7 -3.5     -66.5    82     3001   20 19 31

20 21 25 J191142+1952  15 56 19  44.7  91.7 -3.3     -66.2     7     3001   20 21 25
20 22 55  ---          15 57 49  45.0  91.9 -3.2     -66.2    90     3047   20 21 26

20 22 55  GRB221009A   15 57 49  44.7  91.8 -3.3     -66.1    -8     3047   20 23 03
20 27 30  ---          16 02 25  45.7  92.4 -3.2     -66.0   267     3185   20 22 56

20 27 45  J1925+2106   16 02 40  43.5  89.0 -3.4     -67.3     3     3185   20 27 45
20 28 45  =1923+210    16 03 40  43.7  89.2 -3.4     -67.3    60     3216   20 27 46

20 28 55 J191142+1952  16 03 50  46.3  92.7 -3.1     -66.1    -3     3216   20 28 58
20 30 10  ---          16 05 05  46.6  92.9 -3.1     -66.1    72     3253   20 28 56

20 30 10  GRB221009A   16 05 05  46.2  92.8 -3.2     -66.0    -8     3253   20 30 18
20 34 45  ---          16 09 41  47.2  93.4 -3.1     -65.9   267     3391   20 30 11

20 35 05 J191142+1952  16 10 01  47.6  93.5 -3.0     -66.0    12     3391   20 35 05
20 36 10  ---          16 11 06  47.8  93.7 -3.0     -66.0    65     3424   20 35 06

20 36 25  J1925+2106   16 11 21  45.3  90.1 -3.3     -67.3     2     3424   20 36 25
20 37 25  =1923+210    16 12 21  45.5  90.3 -3.2     -67.3    60     3455   20 36 26

20 37 45 J191249+1940  16 12 41  47.9  94.0 -3.0     -65.7     7     3455   20 37 45
20 39 15  ---          16 14 12  48.2  94.3 -3.0     -65.7    90     3501   20 37 46

20 39 35 J191142+1952  16 14 32  48.6  94.2 -3.0     -65.9    12     3501   20 39 35
20 40 45  ---          16 15 42  48.8  94.4 -3.0     -65.9    70     3537   20 39 36

20 44 45  3C286        16 19 43  54.1 -79.4  2.8      78.6   108     3537   20 44 45
20 48 45  ---          16 23 43  53.3 -79.1  2.9      78.4   240     3661   20 44 46

20 50 45  GRB221009A   16 25 44  50.7  95.8 -2.8     -65.5   -12     3661   20 50 57
20 55 20  ---          16 30 19  51.6  96.5 -2.7     -65.3   263     3797   20 50 46

20 55 35  J1925+2106   16 30 34  49.5  92.7 -2.9     -67.2     3     3797   20 55 35
20 56 35  =1923+210    16 31 34  49.7  92.8 -2.9     -67.1    60     3827   20 55 36

20 56 50 J191142+1952  16 31 50  52.3  96.8 -2.7     -65.3     2     3827   20 56 50
20 58 00  ---          16 33 00  52.5  97.0 -2.7     -65.3    70     3864   20 56 51
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

20 58 00  GRB221009A   16 33 00  52.2  96.9 -2.7     -65.2    -8     3864   20 58 08
21 02 35  ---          16 37 35  53.2  97.7 -2.6     -65.0   267     4001   20 58 01

21 02 55 J191142+1952  16 37 56  53.6  97.8 -2.6     -65.0    12     4001   21 02 55
21 04 00  ---          16 39 01  53.8  98.0 -2.6     -65.0    65     4035   21 02 56

21 04 00  J1905+1943   16 39 01  55.1  99.3 -2.5     -64.5   -10     4035   21 04 10
21 05 45  ---          16 40 46  55.4  99.6 -2.4     -64.3    95     4084   21 04 01

21 05 45 J191142+1952  16 40 46  54.2  98.3 -2.5     -64.9   -10     4084   21 05 55
21 07 10  ---          16 42 11  54.5  98.5 -2.5     -64.8    75     4122   21 05 46

21 07 25  J1925+2106   16 42 26  52.0  94.4 -2.7     -66.9     2     4122   21 07 25
21 08 25  =1923+210    16 43 26  52.2  94.5 -2.7     -66.9    60     4153   21 07 26

21 08 35  GRB221009A   16 43 36  54.5  98.7 -2.5     -64.7    -2     4153   21 08 37
21 13 00  ---          16 48 02  55.4  99.5 -2.4     -64.4   263     4289   21 08 36

21 13 20 J191142+1952  16 48 22  55.8  99.6 -2.4     -64.5    12     4289   21 13 20
21 14 45  ---          16 49 47  56.1  99.9 -2.4     -64.4    85     4332   21 13 21

21 14 45  GRB221009A   16 49 47  55.8  99.8 -2.4     -64.3    -8     4332   21 14 53
21 19 20  ---          16 54 23  56.8 100.6 -2.3     -64.0   267     4470   21 14 46

21 19 35  J1925+2106   16 54 38  54.6  96.3 -2.5     -66.5     3     4470   21 19 35
21 20 35  =1923+210    16 55 38  54.8  96.4 -2.5     -66.5    60     4501   21 19 36

21 20 50 J191142+1952  16 55 53  57.4 101.0 -2.3     -63.9     2     4501   21 20 50
21 22 15  ---          16 57 19  57.7 101.3 -2.3     -63.8    85     4545   21 20 51

21 22 15  J1923+2010   16 57 19  55.4  98.7 -2.4     -65.0   -13     4545   21 22 28
21 23 50  ---          16 58 54  55.7  99.0 -2.4     -64.9    82     4587   21 22 16

21 24 10 J191142+1952  16 59 14  58.1 101.7 -2.2     -63.7     7     4587   21 24 10
21 25 40  ---          17 00 44  58.4 102.0 -2.2     -63.5    90     4633   21 24 11

21 25 40  GRB221009A   17 00 44  58.1 101.9 -2.2     -63.5    -8     4633   21 25 48
21 30 15  ---          17 05 20  59.1 102.8 -2.1     -63.1   267     4771   21 25 41

21 30 30  J1925+2106   17 05 35  57.0  98.1 -2.4     -66.0     3     4771   21 30 30
21 31 30  =1923+210    17 06 35  57.2  98.3 -2.3     -65.9    60     4802   21 30 31

21 31 40 J191142+1952  17 06 45  59.7 103.2 -2.1     -63.0    -3     4802   21 31 43
21 32 55  ---          17 08 00  59.9 103.5 -2.1     -62.9    72     4839   21 31 41
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

21 32 55  GRB221009A   17 08 00  59.6 103.4 -2.1     -62.9    -8     4839   21 33 03
21 37 30  ---          17 12 36  60.6 104.4 -2.0     -62.4   267     4977   21 32 56

21 37 50 J191142+1952  17 12 56  61.0 104.6 -2.0     -62.3    12     4977   21 37 50
21 38 55  ---          17 14 01  61.2 104.8 -2.0     -62.2    65     5010   21 37 51

21 39 10  J1925+2106   17 14 16  58.8  99.7 -2.2     -65.4     2     5010   21 39 10
21 40 10  =1923+210    17 15 17  59.0  99.9 -2.2     -65.4    60     5041   21 39 11

21 40 30 J191249+1940  17 15 37  61.2 105.3 -2.0     -61.8     8     5041   21 40 30
21 42 00  ---          17 17 07  61.5 105.6 -1.9     -61.7    90     5087   21 40 31

21 42 20 J191142+1952  17 17 27  61.9 105.6 -1.9     -61.8    12     5087   21 42 20
21 43 30  ---          17 18 37  62.2 105.9 -1.9     -61.7    70     5123   21 42 21

21 43 30  GRB221009A   17 18 37  61.8 105.7 -1.9     -61.7    -8     5123   21 43 38
21 48 05  ---          17 23 13  62.8 106.9 -1.8     -61.1   267     5261   21 43 31

21 48 20  J1925+2106   17 23 28  60.7 101.5 -2.1     -64.7     3     5261   21 48 20
21 49 20  =1923+210    17 24 28  61.0 101.7 -2.0     -64.6    60     5292   21 48 21

21 49 35 J191142+1952  17 24 43  63.4 107.4 -1.8     -60.8     2     5292   21 49 35
21 50 45  ---          17 25 53  63.7 107.7 -1.8     -60.7    70     5328   21 49 36

21 50 45  GRB221009A   17 25 53  63.3 107.5 -1.8     -60.7    -8     5328   21 50 53
21 55 20  ---          17 30 29  64.3 108.7 -1.7     -60.0   267     5466   21 50 46

21 55 40 J191142+1952  17 30 49  64.7 109.0 -1.7     -59.9    12     5466   21 55 40
21 56 45  ---          17 31 54  64.9 109.3 -1.7     -59.7    65     5499   21 55 41

21 56 45  J1905+1943   17 31 54  66.0 111.4 -1.6     -58.3   -10     5499   21 56 55
21 58 30  ---          17 33 40  66.4 111.9 -1.6     -58.0    95     5548   21 56 46

21 58 30 J191142+1952  17 33 40  65.2 109.8 -1.7     -59.4   -10     5548   21 58 40
21 59 55  ---          17 35 05  65.5 110.2 -1.6     -59.2    75     5587   21 58 31

22 00 10  J1925+2106   17 35 20  63.2 104.0 -1.9     -63.5     2     5587   22 00 10
22 01 10  =1923+210    17 36 20  63.4 104.3 -1.8     -63.4    60     5618   22 00 11

22 01 20  GRB221009A   17 36 30  65.5 110.4 -1.6     -59.0    -2     5618   22 01 22
22 05 45  ---          17 40 56  66.4 111.8 -1.6     -58.1   263     5753   22 01 21

22 06 05 J191142+1952  17 41 16  66.8 112.1 -1.5     -58.0    12     5753   22 06 05
22 07 30  ---          17 42 41  67.0 112.5 -1.5     -57.7    85     5797   22 06 06
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

22 07 30  GRB221009A   17 42 41  66.7 112.3 -1.5     -57.8    -8     5797   22 07 38
22 12 05  ---          17 47 17  67.6 113.8 -1.4     -56.8   267     5934   22 07 31

22 12 20  J1925+2106   17 47 32  65.8 107.1 -1.7     -61.9     2     5934   22 12 20
22 13 20  =1923+210    17 48 32  66.0 107.3 -1.6     -61.7    60     5965   22 12 21

22 13 35 J191142+1952  17 48 47  68.2 114.6 -1.4     -56.3     2     5965   22 13 35
22 15 00  ---          17 50 12  68.5 115.1 -1.4     -56.0    85     6009   22 13 36

22 15 00  J1923+2010   17 50 12  66.4 110.6 -1.6     -59.1   -12     6009   22 15 12
22 16 35  ---          17 51 48  66.7 111.1 -1.5     -58.8    83     6052   22 15 01

22 16 55 J191142+1952  17 52 08  68.9 115.8 -1.3     -55.5     8     6052   22 16 55
22 18 25  ---          17 53 38  69.2 116.4 -1.3     -55.1    90     6098   22 16 56

22 18 25  GRB221009A   17 53 38  68.9 116.1 -1.3     -55.2    -8     6098   22 18 33
22 23 00  ---          17 58 14  69.8 117.8 -1.3     -54.0   267     6236   22 18 26

22 23 15  J1925+2106   17 58 29  68.0 110.2 -1.5     -60.0     2     6236   22 23 15
22 24 15  =1923+210    17 59 29  68.2 110.5 -1.5     -59.8    60     6267   22 23 16

22 24 25 J191142+1952  17 59 39  70.3 118.8 -1.2     -53.3    -4     6267   22 24 29
22 25 40  ---          18 00 54  70.6 119.3 -1.2     -53.0    71     6303   22 24 26

22 25 40  GRB221009A   18 00 54  70.3 118.9 -1.2     -53.2    -8     6303   22 25 48
22 30 15  ---          18 05 30  71.1 120.9 -1.1     -51.7   267     6441   22 25 41

22 30 35 J191142+1952  18 05 50  71.5 121.5 -1.1     -51.3    12     6441   22 30 35
22 31 40  ---          18 06 55  71.7 122.0 -1.1     -50.9    65     6474   22 30 36

22 31 55  J1925+2106   18 07 10  69.7 113.1 -1.3     -58.0     1     6474   22 31 55
22 32 55  =1923+210    18 08 10  69.9 113.5 -1.3     -57.8    60     6505   22 31 56

22 33 15 J191249+1940  18 08 30  71.6 122.7 -1.1     -50.3     6     6505   22 33 15
22 34 45  ---          18 10 01  71.9 123.4 -1.1     -49.7    90     6552   22 33 16

22 35 05 J191142+1952  18 10 21  72.3 123.7 -1.0     -49.6    12     6552   22 35 05
22 36 15  ---          18 11 31  72.5 124.2 -1.0     -49.2    70     6588   22 35 06

22 36 15  GRB221009A   18 11 31  72.2 123.8 -1.0     -49.5    -8     6588   22 36 23
22 40 50  ---          18 16 07  73.0 126.2 -1.0     -47.6   267     6725   22 36 16

22 41 05  J1925+2106   18 16 22  71.5 116.7 -1.2     -55.5     0     6725   22 41 05
22 42 05  =1923+210    18 17 22  71.7 117.1 -1.2     -55.2    60     6756   22 41 06
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

22 42 20 J191142+1952  18 17 37  73.6 127.5 -0.9     -46.5     0     6756   22 42 20
22 43 30  ---          18 18 47  73.8 128.2 -0.9     -46.0    70     6792   22 42 21

22 43 30  GRB221009A   18 18 47  73.5 127.7 -0.9     -46.4    -8     6792   22 43 38
22 48 05  ---          18 23 23  74.3 130.4 -0.8     -44.1   267     6930   22 43 31

22 48 25 J191142+1952  18 23 43  74.6 131.2 -0.8     -43.5    12     6930   22 48 25
22 49 30  ---          18 24 48  74.8 131.9 -0.8     -42.9    65     6963   22 48 26

22 49 30  J1905+1943   18 24 48  75.6 136.6 -0.7     -38.9   -11     6963   22 49 41
22 51 15  ---          18 26 33  75.9 137.9 -0.7     -37.8    94     7012   22 49 31

22 51 15 J191142+1952  18 26 33  75.0 133.1 -0.8     -41.9   -11     7012   22 51 26
22 52 40  ---          18 27 59  75.3 134.1 -0.7     -41.1    74     7050   22 51 16

22 52 55  J1925+2106   18 28 14  73.8 122.2 -1.0     -51.3    -1     7050   22 52 56
22 53 55  =1923+210    18 29 14  73.9 122.7 -1.0     -50.9    59     7080   22 52 56

22 54 05  GRB221009A   18 29 24  75.2 134.4 -0.7     -40.8    -6     7080   22 54 11
22 58 30  ---          18 33 49  75.9 137.6 -0.7     -38.1   259     7214   22 54 06

22 58 50 J191142+1952  18 34 10  76.2 138.7 -0.6     -37.2    12     7214   22 58 50
23 00 15  ---          18 35 35  76.4 139.8 -0.6     -36.2    85     7258   22 58 51

23 00 15  GRB221009A   18 35 35  76.1 139.0 -0.6     -36.9    -8     7258   23 00 23
23 04 50  ---          18 40 11  76.7 142.7 -0.6     -33.6   267     7395   23 00 16

23 05 05  J1925+2106   18 40 26  75.9 129.4 -0.8     -45.5    -2     7395   23 05 07
23 06 05  =1923+210    18 41 26  76.0 130.1 -0.8     -44.9    58     7425   23 05 06

23 06 20 J191142+1952  18 41 41  77.2 145.0 -0.5     -31.7    -3     7425   23 06 23
23 07 45  ---          18 43 06  77.4 146.3 -0.5     -30.5    82     7467   23 06 21

23 07 45  J1923+2010   18 43 06  76.1 135.9 -0.7     -39.7   -15     7467   23 08 00
23 09 20  ---          18 44 41  76.3 137.1 -0.7     -38.6    80     7509   23 07 46

23 09 40 J191142+1952  18 45 01  77.6 148.1 -0.5     -28.9     4     7509   23 09 40
23 11 10  ---          18 46 32  77.7 149.6 -0.4     -27.6    90     7555   23 09 41

23 11 10  GRB221009A   18 46 32  77.5 148.5 -0.5     -28.6    -8     7555   23 11 18
23 15 45  ---          18 51 07  78.0 153.0 -0.4     -24.5   267     7693   23 11 11

23 16 00  J1925+2106   18 51 22  77.6 137.7 -0.6     -38.4    -4     7693   23 16 04
23 17 00  =1923+210    18 52 23  77.7 138.6 -0.6     -37.6    56     7721   23 16 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

23 17 10 J191142+1952  18 52 33  78.3 155.8 -0.3     -22.1   -10     7721   23 17 20
23 18 25  ---          18 53 48  78.5 157.1 -0.3     -20.8    65     7755   23 17 11

23 18 25  GRB221009A   18 53 48  78.3 155.8 -0.3     -22.0    -9     7755   23 18 34
23 23 00  ---          18 58 24  78.6 160.9 -0.3     -17.4   266     7892   23 18 26

23 23 20 J191142+1952  18 58 44  78.8 162.7 -0.2     -15.8    11     7892   23 23 20
23 24 25  ---          18 59 49  78.9 164.0 -0.2     -14.6    65     7925   23 23 21

23 24 40  J1925+2106   19 00 04  78.8 145.8 -0.4     -31.2    -6     7925   23 24 46
23 25 40  =1923+210    19 01 04  78.9 146.8 -0.4     -30.3    54     7953   23 24 41

23 26 00 J191249+1940  19 01 24  78.7 164.8 -0.2     -13.9    -1     7953   23 26 01
23 27 30  ---          19 02 54  78.8 166.6 -0.2     -12.3    89     7999   23 26 01

23 27 30 J191142+1952  19 02 54  79.0 167.7 -0.2     -11.2    -9     7999   23 27 39
23 28 55  ---          19 04 19  79.1 169.4 -0.1      -9.7    76     8038   23 27 31

23 28 55  GRB221009A   19 04 19  79.0 167.9 -0.2     -11.1    -9     8038   23 29 04
23 33 30  ---          19 08 55  79.1 173.5 -0.1      -5.9   266     8175   23 28 56

23 33 50 J191142+1952  19 09 15  79.2 175.6 -0.1      -4.1    11     8175   23 33 50
23 34 55  ---          19 10 20  79.3 176.9 -0.0      -2.8    65     8209   23 33 51

23 34 55  J1905+1943   19 10 20  79.1 184.6  0.1       4.2   -13     8209   23 35 08
23 36 40  ---          19 12 06  79.1 186.7  0.1       6.1    92     8256   23 34 56

23 36 40 J191142+1952  19 12 06  79.3 179.1 -0.0      -0.8   -13     8256   23 36 53
23 38 05  ---          19 13 31  79.3 180.9  0.0       0.9    72     8293   23 36 41

23 38 20  J1925+2106   19 13 46  80.1 161.7 -0.2     -16.8    -7     8293   23 38 27
23 39 20  =1923+210    19 14 46  80.1 163.0 -0.2     -15.6    53     8321   23 38 21

23 39 35  GRB221009A   19 15 01  79.2 181.1  0.0       1.0    -6     8321   23 39 41
23 44 10  ---          19 19 37  79.1 186.8  0.1       6.3   269     8459   23 39 36

23 44 30 J191142+1952  19 19 57  79.2 189.0  0.1       8.2    11     8459   23 44 30
23 45 55  ---          19 21 22  79.1 190.7  0.1       9.8    85     8503   23 44 31

23 45 55  GRB221009A   19 21 22  79.1 189.0  0.1       8.2    -9     8503   23 46 04
23 50 30  ---          19 25 58  78.9 194.6  0.2      13.3   266     8640   23 45 56

23 50 45  J1925+2106   19 26 13  80.5 178.8 -0.0      -1.1    -4     8640   23 50 49
23 51 45  =1923+210    19 27 13  80.5 180.2  0.0       0.2    56     8669   23 50 46
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  28 Oct 2024   Day 302 ---

23 51 45 J191142+1952  19 27 13  78.8 197.7  0.2      16.2   -21     8669   23 52 06
23 53 10  ---          19 28 38  78.7 199.4  0.3      17.7    64     8702   23 51 46

23 53 10  J1923+2010   19 28 38  79.5 185.6  0.1       5.2   -17     8702   23 53 27
23 54 45  ---          19 30 14  79.5 187.7  0.1       7.0    78     8742   23 53 11

23 55 05 J191142+1952  19 30 34  78.6 201.5  0.3      19.6     2     8742   23 55 05
23 56 35  ---          19 32 04  78.4 203.2  0.3      21.1    90     8789   23 55 06

 --- Start: Mon  28 Oct 2024   Day 302 -- Stop: Tue  29 Oct 2024   Day 303 ---

23 56 35  GRB221009A   19 32 04  78.5 201.6  0.3      19.6    -9     8789   23 56 44
00 01 10  ---          19 36 40  78.0 206.5  0.4      24.1   266     8926   23 56 36

00 01 25  J1925+2106   19 36 55  80.3 193.7  0.2      12.6    -2     8926   00 01 27
00 02 25  =1923+210    19 37 55  80.2 195.1  0.2      13.9    58     8956   00 01 26

00 02 40 J191142+1952  19 38 10  77.8 209.6  0.4      26.9    -3     8956   00 02 43
00 04 05  ---          19 39 35  77.7 211.0  0.4      28.1    82     8998   00 02 41

00 04 05  GRB221009A   19 39 35  77.8 209.4  0.4      26.7    -9     8998   00 04 14
00 08 40  ---          19 44 11  77.2 213.8  0.5      30.6   266     9135   00 04 06

00 09 00 J191142+1952  19 44 31  77.1 215.6  0.5      32.2    11     9135   00 09 00
00 10 05  ---          19 45 36  77.0 216.5  0.5      33.0    65     9168   00 09 01

00 10 20  J1925+2106   19 45 51  79.6 205.1  0.3      23.1    -1     9168   00 10 21
00 11 20  =1923+210    19 46 51  79.5 206.3  0.3      24.1    59     9199   00 10 21

00 11 20 J191249+1940  19 46 51  76.8 216.2  0.5      32.6   -15     9199   00 11 35
00 12 50  ---          19 48 22  76.6 217.5  0.6      33.8    75     9237   00 11 21

00 12 50 J191142+1952  19 48 22  76.6 218.9  0.6      35.1    -9     9237   00 12 59
00 14 20  ---          19 49 52  76.4 220.1  0.6      36.1    81     9279   00 12 51

00 14 20  GRB221009A   19 49 52  76.5 218.8  0.6      34.9    -9     9279   00 14 29
00 18 55  ---          19 54 28  75.9 222.4  0.7      38.1   266     9416   00 14 21

00 19 10  J1925+2106   19 54 43  78.7 214.9  0.5      31.8     1     9416   00 19 10
00 20 10  =1923+210    19 55 43  78.5 215.9  0.5      32.7    60     9447   00 19 11

00 20 10 J191142+1952  19 55 43  75.6 224.6  0.7      40.0   -14     9447   00 20 24
00 21 35  ---          19 57 08  75.3 225.6  0.7      40.8    71     9484   00 20 11
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

00 21 35  GRB221009A   19 57 08  75.5 224.4  0.7      39.8    -8     9484   00 21 43
00 26 10  ---          20 01 44  74.8 227.6  0.8      42.5   267     9621   00 21 36

00 26 30 J191142+1952  20 02 04  74.6 228.9  0.8      43.6    12     9621   00 26 30
00 27 35  ---          20 03 09  74.4 229.6  0.8      44.2    65     9655   00 26 31

00 27 35  J1905+1943   20 03 09  73.3 232.8  0.9      46.7   -10     9655   00 27 45
00 29 20  ---          20 04 54  72.9 233.8  1.0      47.5    95     9704   00 27 36

00 29 20 J191142+1952  20 04 54  74.1 230.7  0.9      45.1   -10     9704   00 29 30
00 30 45  ---          20 06 20  73.9 231.5  0.9      45.8    75     9742   00 29 21

00 31 00  J1925+2106   20 06 35  77.0 225.4  0.7      41.1     1     9742   00 31 00
00 32 00  =1923+210    20 07 35  76.9 226.2  0.7      41.8    60     9773   00 31 01

00 32 15  GRB221009A   20 07 50  73.8 231.4  0.9      45.6     1     9773   00 32 15
00 36 50  ---          20 12 26  73.0 234.0  1.0      47.7   275     9915   00 32 16

00 37 10 J191142+1952  20 12 46  72.7 235.1  1.0      48.6    12     9915   00 37 10
00 38 35  ---          20 14 11  72.5 235.8  1.0      49.2    85     9959   00 37 11

00 38 35  GRB221009A   20 14 11  72.7 234.9  1.0      48.4    -8     9959   00 38 43
00 43 10  ---          20 18 47  71.8 237.2  1.1      50.2   267    10096   00 38 36

00 43 25  J1925+2106   20 19 02  75.0 234.0  0.9      48.3     1    10096   00 43 25
00 44 25  =1923+210    20 20 02  74.8 234.6  0.9      48.7    60    10127   00 43 26

00 44 25 J191142+1952  20 20 02  71.4 238.7  1.1      51.4   -15    10127   00 44 40
00 45 50  ---          20 21 27  71.2 239.3  1.1      51.9    70    10163   00 44 26

00 45 50  J1923+2010   20 21 27  73.4 234.4  1.0      48.2   -12    10163   00 46 02
00 47 25  ---          20 23 02  73.2 235.3  1.0      48.9    83    10206   00 45 51

00 47 45 J191142+1952  20 23 22  70.8 240.2  1.2      52.5     7    10206   00 47 45
00 49 15  ---          20 24 53  70.5 240.8  1.2      53.0    90    10252   00 47 46

00 49 15  GRB221009A   20 24 53  70.7 240.0  1.2      52.4    -8    10252   00 49 23
00 53 50  ---          20 29 28  69.9 241.9  1.3      53.8   267    10390   00 49 16

00 54 05  J1925+2106   20 29 43  73.0 239.7  1.0      52.8     1    10390   00 54 05
00 55 05  =1923+210    20 30 44  72.9 240.2  1.1      53.2    60    10421   00 54 06

00 55 20 J191142+1952  20 30 59  69.4 243.3  1.3      54.8     0    10421   00 55 20
00 56 45  ---          20 32 24  69.1 243.8  1.3      55.2    85    10465   00 55 21
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

00 56 45  GRB221009A   20 32 24  69.3 243.1  1.3      54.6    -8    10465   00 56 53
01 01 20  ---          20 37 00  68.4 244.8  1.4      55.8   267    10602   00 56 46

01 01 40 J191142+1952  20 37 20  68.1 245.6  1.4      56.4    12    10602   01 01 40
01 02 45  ---          20 38 25  67.9 246.0  1.4      56.7    65    10636   01 01 41

01 03 00  J1925+2106   20 38 40  71.4 243.7  1.2      55.8     0    10636   01 03 00
01 04 00  =1923+210    20 39 40  71.2 244.1  1.2      56.1    60    10667   01 03 01

01 04 00 J191249+1940  20 39 40  67.8 245.6  1.4      56.3   -15    10667   01 04 15
01 05 30  ---          20 41 10  67.5 246.1  1.5      56.7    75    10705   01 04 01

01 05 30 J191142+1952  20 41 10  67.4 246.9  1.5      57.3    -8    10705   01 05 38
01 07 00  ---          20 42 41  67.1 247.4  1.5      57.6    82    10748   01 05 31

01 07 00  GRB221009A   20 42 41  67.3 246.7  1.5      57.2    -8    10748   01 07 08
01 11 35  ---          20 47 16  66.4 248.2  1.6      58.1   267    10885   01 07 01

01 11 50  J1925+2106   20 47 31  69.6 247.1  1.3      58.2     1    10885   01 11 50
01 12 50  =1923+210    20 48 32  69.4 247.4  1.4      58.4    60    10916   01 11 51

01 12 50 J191142+1952  20 48 32  65.9 249.2  1.6      58.8   -15    10916   01 13 05
01 14 15  ---          20 49 57  65.6 249.6  1.6      59.1    70    10952   01 12 51

01 14 15  GRB221009A   20 49 57  65.9 249.0  1.6      58.7    -8    10952   01 14 23
01 18 50  ---          20 54 33  64.9 250.4  1.7      59.5   267    11090   01 14 16

01 19 10 J191142+1952  20 54 53  64.6 251.0  1.7      59.9    12    11090   01 19 10
01 20 15  ---          20 55 58  64.4 251.3  1.7      60.1    65    11123   01 19 11

01 20 15  J1905+1943   20 55 58  63.1 252.6  1.8      60.8   -11    11123   01 20 26
01 22 00  ---          20 57 43  62.7 253.1  1.9      61.0    94    11172   01 20 16

01 22 00 J191142+1952  20 57 43  64.1 251.8  1.7      60.4   -11    11172   01 22 11
01 23 25  ---          20 59 08  63.8 252.2  1.8      60.6    74    11210   01 22 01

01 23 40  J1925+2106   20 59 23  67.2 250.9  1.5      60.7     0    11210   01 23 40
01 24 40  =1923+210    21 00 24  67.0 251.2  1.6      60.9    60    11241   01 23 41

01 24 55  GRB221009A   21 00 39  63.7 252.0  1.8      60.5     0    11241   01 24 55
01 29 30  ---          21 05 14  62.7 253.2  1.9      61.1   275    11382   01 24 56

01 29 50 J191142+1952  21 05 34  62.4 253.8  1.9      61.5    12    11382   01 29 50
01 31 15  ---          21 07 00  62.1 254.1  1.9      61.7    85    11426   01 29 51
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

01 31 15  GRB221009A   21 07 00  62.4 253.6  1.9      61.3    -8    11426   01 31 23
01 35 50  ---          21 11 35  61.4 254.7  2.0      61.9   267    11564   01 31 16

01 36 05  J1925+2106   21 11 50  64.7 254.3  1.7      62.6     1    11564   01 36 05
01 37 05  =1923+210    21 12 51  64.5 254.5  1.8      62.8    60    11595   01 36 06

01 37 05 J191142+1952  21 12 51  60.9 255.5  2.0      62.4   -15    11595   01 37 20
01 38 30  ---          21 14 16  60.6 255.8  2.0      62.5    70    11631   01 37 06

01 38 30  J1923+2010   21 14 16  63.2 253.7  1.8      61.7   -13    11631   01 38 43
01 40 05  ---          21 15 51  62.8 254.1  1.9      61.9    82    11673   01 38 31

01 40 25 J191142+1952  21 16 11  60.2 256.2  2.1      62.7     7    11673   01 40 25
01 41 55  ---          21 17 41  59.9 256.5  2.1      62.9    90    11719   01 40 26

01 41 55  GRB221009A   21 17 41  60.2 256.1  2.1      62.6    -8    11719   01 42 03
01 46 30  ---          21 22 17  59.2 257.1  2.1      63.0   267    11857   01 41 56

01 46 45  J1925+2106   21 22 32  62.5 256.8  1.9      63.9     1    11857   01 46 45
01 47 45  =1923+210    21 23 32  62.2 257.0  1.9      64.0    60    11888   01 46 46

01 48 00 J191142+1952  21 23 47  58.6 257.8  2.2      63.4     0    11888   01 48 00
01 49 25  ---          21 25 13  58.3 258.1  2.2      63.6    85    11932   01 48 01

01 49 25  GRB221009A   21 25 13  58.6 257.7  2.2      63.3    -8    11932   01 49 33
01 54 00  ---          21 29 48  57.6 258.6  2.3      63.7   267    12069   01 49 26

01 54 20 J191142+1952  21 30 08  57.3 259.1  2.3      64.0    12    12069   01 54 20
01 55 25  ---          21 31 14  57.1 259.3  2.3      64.0    65    12103   01 54 21

01 55 40  J1925+2106   21 31 29  60.6 258.7  2.1      64.8     0    12103   01 55 40
01 56 40  =1923+210    21 32 29  60.4 258.9  2.1      64.9    60    12134   01 55 41

01 56 40 J191249+1940  21 32 29  57.0 259.0  2.3      63.8   -15    12134   01 56 55
01 58 10  ---          21 33 59  56.6 259.2  2.3      63.9    75    12172   01 56 41

01 58 10 J191142+1952  21 33 59  56.5 259.8  2.4      64.2    -8    12172   01 58 18
01 59 40  ---          21 35 29  56.2 260.1  2.4      64.3    82    12215   01 58 11

01 59 40  GRB221009A   21 35 29  56.4 259.7  2.4      64.1    -8    12215   01 59 48
02 04 15  ---          21 40 05  55.4 260.5  2.4      64.4   267    12352   01 59 41

02 04 30  J1925+2106   21 40 20  58.7 260.4  2.2      65.5     1    12352   02 04 30
02 05 30  =1923+210    21 41 20  58.5 260.6  2.2      65.5    60    12383   02 04 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

02 05 30  J1925+2106   21 41 20  58.5 260.6  2.2      65.5    -6    12383   02 05 36
02 07 25  =1923+210    21 43 16  58.1 261.0  2.3      65.7   109    12439   02 05 31

02 07 25 J191142+1952  21 43 16  54.5 261.4  2.5      64.8   -15    12439   02 07 40
02 08 50  ---          21 44 41  54.2 261.7  2.5      64.9    70    12475   02 07 26

02 08 50  GRB221009A   21 44 41  54.5 261.3  2.5      64.7    -8    12475   02 08 58
02 13 25  ---          21 49 17  53.5 262.1  2.6      64.9   267    12613   02 08 51

02 13 45 J191142+1952  21 49 37  53.2 262.5  2.6      65.1    12    12613   02 13 45
02 14 50  ---          21 50 42  52.9 262.7  2.6      65.2    65    12646   02 13 46

02 14 50  J1905+1943   21 50 42  51.6 263.4  2.7      65.3   -11    12646   02 15 01
02 16 35  ---          21 52 27  51.2 263.7  2.8      65.3    94    12695   02 14 51

02 16 35 J191142+1952  21 52 27  52.6 263.0  2.7      65.3   -11    12695   02 16 46
02 18 00  ---          21 53 52  52.3 263.2  2.7      65.3    74    12733   02 16 36

02 18 15  J1925+2106   21 54 07  55.8 262.8  2.5      66.3     0    12733   02 18 15
02 19 15  =1923+210    21 55 07  55.6 263.0  2.5      66.3    60    12764   02 18 16

02 19 30  GRB221009A   21 55 23  52.2 263.1  2.7      65.2     0    12764   02 19 30
02 24 05  ---          21 59 58  51.2 263.8  2.8      65.4   275    12906   02 19 31

02 24 25 J191142+1952  22 00 18  50.9 264.2  2.8      65.6    12    12906   02 24 25
02 25 50  ---          22 01 44  50.6 264.4  2.8      65.6    85    12949   02 24 26

02 25 50  GRB221009A   22 01 44  50.8 264.1  2.8      65.5    -8    12949   02 25 58
02 30 25  ---          22 06 19  49.8 264.8  2.9      65.6   267    13087   02 25 51

02 30 40  J1925+2106   22 06 34  53.1 264.8  2.7      66.8     1    13087   02 30 40
02 31 40  =1923+210    22 07 35  52.9 265.0  2.7      66.8    60    13118   02 30 41

02 31 40 J191142+1952  22 07 35  49.3 265.3  2.9      65.8   -15    13118   02 31 55
02 33 05  ---          22 09 00  49.0 265.5  2.9      65.8    70    13154   02 31 41

02 33 05  J1923+2010   22 09 00  51.6 264.2  2.7      65.8   -13    13154   02 33 18
02 34 40  ---          22 10 35  51.3 264.5  2.8      65.9    82    13196   02 33 06

02 35 00 J191142+1952  22 10 55  48.6 265.8  3.0      65.9     7    13196   02 35 00
02 36 30  ---          22 12 25  48.3 266.0  3.0      65.9    90    13243   02 35 01

02 36 30  GRB221009A   22 12 25  48.5 265.7  3.0      65.8    -8    13243   02 36 38
02 41 05  ---          22 17 01  47.6 266.3  3.0      65.9   267    13380   02 36 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

02 41 20  J1925+2106   22 17 16  50.8 266.4  2.8      67.0     1    13380   02 41 20
02 42 20  =1923+210    22 18 16  50.6 266.6  2.9      67.1    60    13411   02 41 21

02 42 35 J191142+1952  22 18 31  47.0 266.9  3.1      66.0     0    13411   02 42 35
02 44 00  ---          22 19 57  46.7 267.1  3.1      66.1    85    13455   02 42 36

02 44 00  GRB221009A   22 19 57  46.9 266.8  3.1      65.9    -8    13455   02 44 08
02 48 35  ---          22 24 32  45.9 267.4  3.2      66.0   267    13592   02 44 01

02 48 55 J191142+1952  22 24 52  45.6 267.8  3.2      66.1    12    13592   02 48 55
02 50 00  ---          22 25 58  45.4 267.9  3.2      66.1    65    13626   02 48 56

02 50 15  J1925+2106   22 26 13  48.9 267.7  3.0      67.2     0    13626   02 50 15
02 51 15  =1923+210    22 27 13  48.7 267.8  3.0      67.2    60    13657   02 50 16

02 51 15 J191249+1940  22 27 13  45.3 267.7  3.2      66.0   -15    13657   02 51 30
02 52 45  ---          22 28 43  44.9 267.9  3.2      66.0    75    13696   02 51 16

02 52 45 J191142+1952  22 28 43  44.8 268.3  3.3      66.2    -8    13696   02 52 53
02 54 15  ---          22 30 13  44.5 268.5  3.3      66.2    82    13738   02 52 46

02 54 15  GRB221009A   22 30 13  44.7 268.2  3.3      66.1    -8    13738   02 54 23
02 58 50  ---          22 34 49  43.7 268.8  3.3      66.1   267    13875   02 54 16

02 59 05  J1925+2106   22 35 04  47.0 268.9  3.1      67.3     1    13875   02 59 05
03 00 05  =1923+210    22 36 04  46.8 269.0  3.2      67.3    60    13906   02 59 06

03 00 05 J191142+1952  22 36 04  43.2 269.2  3.4      66.2   -15    13906   03 00 20
03 01 30  ---          22 37 29  42.9 269.4  3.4      66.2    70    13942   03 00 06

03 01 30  GRB221009A   22 37 29  43.2 269.1  3.4      66.1    -8    13942   03 01 38
03 06 05  ---          22 42 05  42.2 269.7  3.5      66.1   267    14080   03 01 31

03 06 25 J191142+1952  22 42 25  41.8 270.1  3.5      66.2    12    14080   03 06 25
03 07 30  ---          22 43 30  41.6 270.2  3.5      66.2    65    14113   03 06 26

03 07 30  J1905+1943   22 43 30  40.2 270.8  3.6      66.1   -11    14113   03 07 41
03 09 15  ---          22 45 16  39.9 271.0  3.6      66.1    94    14162   03 07 31

03 09 15 J191142+1952  22 45 16  41.2 270.4  3.5      66.2   -11    14162   03 09 26
03 10 40  ---          22 46 41  40.9 270.6  3.6      66.2    74    14200   03 09 16

03 10 55  J1925+2106   22 46 56  44.4 270.4  3.3      67.3     0    14200   03 10 55
03 11 55  =1923+210    22 47 56  44.2 270.5  3.3      67.3    60    14231   03 10 56
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

03 12 10  GRB221009A   22 48 11  40.9 270.5  3.6      66.1     0    14231   03 12 10
03 16 45  ---          22 52 47  39.9 271.1  3.6      66.1   275    14373   03 12 11

03 17 05 J191142+1952  22 53 07  39.5 271.4  3.7      66.2    12    14373   03 17 05
03 18 30  ---          22 54 32  39.2 271.6  3.7      66.2    85    14416   03 17 06

03 18 30  GRB221009A   22 54 32  39.5 271.3  3.7      66.1    -8    14416   03 18 38
03 23 05  ---          22 59 08  38.5 271.9  3.8      66.1   267    14554   03 18 31

03 23 20  J1925+2106   22 59 23  41.8 271.9  3.5      67.2     1    14554   03 23 20
03 24 20  =1923+210    23 00 23  41.5 272.1  3.6      67.2    60    14585   03 23 21

03 24 20 J191142+1952  23 00 23  38.0 272.3  3.8      66.1   -15    14585   03 24 35
03 25 45  ---          23 01 48  37.7 272.5  3.8      66.1    70    14621   03 24 21

03 25 45  J1923+2010   23 01 48  40.3 271.4  3.6      66.4   -13    14621   03 25 58
03 27 20  ---          23 03 24  39.9 271.6  3.7      66.4    82    14663   03 25 46

03 27 40 J191142+1952  23 03 44  37.3 272.7  3.8      66.1     7    14663   03 27 40
03 29 10  ---          23 05 14  36.9 272.9  3.9      66.1    90    14710   03 27 41

03 29 10  GRB221009A   23 05 14  37.2 272.6  3.9      66.0    -8    14710   03 29 18
03 33 45  ---          23 09 50  36.2 273.1  3.9      66.0   267    14847   03 29 11

03 34 00  J1925+2106   23 10 05  39.5 273.2  3.7      67.1     1    14847   03 34 00
03 35 00  =1923+210    23 11 05  39.2 273.3  3.7      67.1    60    14878   03 34 01

03 35 15 J191142+1952  23 11 20  35.6 273.6  4.0      66.0     0    14878   03 35 15
03 36 40  ---          23 12 45  35.3 273.8  4.0      65.9    85    14922   03 35 16

03 36 40  GRB221009A   23 12 45  35.6 273.5  4.0      65.9    -8    14922   03 36 48
03 41 15  ---          23 17 21  34.6 274.0  4.1      65.8   267    15059   03 36 41

03 41 35 J191142+1952  23 17 41  34.3 274.3  4.1      65.9    12    15059   03 41 35
03 42 40  ---          23 18 46  34.0 274.5  4.1      65.8    65    15093   03 41 36

03 42 55  J1925+2106   23 19 01  37.5 274.2  3.9      66.9     0    15093   03 42 55
03 43 55  =1923+210    23 20 01  37.3 274.4  3.9      66.9    60    15124   03 42 56

03 43 55 J191249+1940  23 20 01  33.9 274.3  4.1      65.7   -15    15124   03 44 10
03 45 25  ---          23 21 32  33.6 274.4  4.1      65.7    75    15163   03 43 56

03 45 25 J191142+1952  23 21 32  33.4 274.8  4.1      65.8    -8    15163   03 45 33
03 46 55  ---          23 23 02  33.1 274.9  4.2      65.7    82    15205   03 45 26
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

03 46 55  GRB221009A   23 23 02  33.4 274.7  4.1      65.7    -8    15205   03 47 03
03 51 30  ---          23 27 38  32.4 275.2  4.2      65.6   267    15342   03 46 56

03 51 45  J1925+2106   23 27 53  35.6 275.3  4.0      66.7     1    15342   03 51 45
03 52 45  =1923+210    23 28 53  35.4 275.4  4.0      66.7    60    15373   03 51 46

03 52 45 J191142+1952  23 28 53  31.9 275.6  4.3      65.6   -15    15373   03 53 00
03 54 10  ---          23 30 18  31.6 275.8  4.3      65.6    70    15409   03 52 46

03 54 10  GRB221009A   23 30 18  31.8 275.5  4.3      65.6    -8    15409   03 54 18
03 58 45  ---          23 34 54  30.8 276.1  4.3      65.4   267    15547   03 54 11

03 59 05 J191142+1952  23 35 14  30.5 276.3  4.4      65.4    12    15547   03 59 05
04 00 10  ---          23 36 19  30.3 276.5  4.4      65.4    65    15580   03 59 06

04 00 10  J1905+1943   23 36 19  28.9 277.0  4.5      65.2   -11    15580   04 00 21
04 01 55  ---          23 38 04  28.5 277.2  4.5      65.1    94    15629   04 00 11

04 01 55 J191142+1952  23 38 04  29.9 276.7  4.4      65.4   -11    15629   04 02 06
04 03 20  ---          23 39 30  29.6 276.8  4.4      65.3    74    15667   04 01 56

04 03 35  J1925+2106   23 39 45  33.1 276.6  4.2      66.4     0    15667   04 03 35
04 04 35  =1923+210    23 40 45  32.9 276.7  4.2      66.4    60    15698   04 03 36

04 04 50  GRB221009A   23 41 00  29.5 276.7  4.4      65.3     0    15698   04 04 50
04 09 25  ---          23 45 36  28.5 277.3  4.5      65.1   275    15840   04 04 51

04 09 45 J191142+1952  23 45 56  28.2 277.5  4.6      65.1    12    15840   04 09 45
04 11 10  ---          23 47 21  27.9 277.7  4.6      65.1    85    15883   04 09 46

04 11 10  GRB221009A   23 47 21  28.2 277.5  4.6      65.1    -8    15883   04 11 18
04 15 45  ---          23 51 57  27.2 278.0  4.6      64.9   267    16021   04 11 11

04 16 00  J1925+2106   23 52 12  30.4 278.0  4.4      66.0     1    16021   04 16 00
04 17 00  =1923+210    23 53 12  30.2 278.1  4.4      66.0    60    16052   04 16 01

04 17 00 J191142+1952  23 53 12  26.7 278.4  4.7      64.9   -15    16052   04 17 15
04 18 25  ---          23 54 37  26.4 278.5  4.7      64.8    70    16088   04 17 01

04 18 25  J1923+2010   23 54 37  29.0 277.6  4.5      65.4   -13    16088   04 18 38
04 20 00  ---          23 56 12  28.6 277.7  4.5      65.3    82    16130   04 18 26

04 20 20 J191142+1952  23 56 32  26.0 278.7  4.7      64.8     7    16130   04 20 20
04 21 50  ---          23 58 03  25.6 278.9  4.8      64.7    90    16177   04 20 21
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

04 21 50  GRB221009A   23 58 03  25.9 278.7  4.7      64.7    -8    16177   04 21 58
04 26 25  ---          00 02 38  24.9 279.2  4.8      64.5   267    16314   04 21 51

04 26 40  J1925+2106   00 02 53  28.2 279.1  4.6      65.6     1    16314   04 26 40
04 27 40  =1923+210    00 03 54  28.0 279.2  4.6      65.6    60    16345   04 26 41

04 27 55 J191142+1952  00 04 09  24.3 279.6  4.9      64.5     0    16345   04 27 55
04 29 20  ---          00 05 34  24.0 279.7  4.9      64.4    85    16389   04 27 56

04 29 20  GRB221009A   00 05 34  24.3 279.5  4.9      64.4    -8    16389   04 29 28
04 33 55  ---          00 10 10  23.3 280.0  4.9      64.2   267    16526   04 29 21

04 34 15 J191142+1952  00 10 30  23.0 280.3  5.0      64.2    12    16526   04 34 15
04 35 20  ---          00 11 35  22.8 280.4  5.0      64.2    65    16560   04 34 16

04 35 35  J1925+2106   00 11 50  26.3 280.1  4.7      65.3     0    16560   04 35 35
04 36 35  =1923+210    00 12 50  26.1 280.2  4.8      65.2    60    16591   04 35 36

04 36 35 J191249+1940  00 12 50  22.7 280.2  5.0      64.1   -15    16591   04 36 50
04 38 05  ---          00 14 20  22.3 280.4  5.0      64.0    75    16630   04 36 36

04 38 05 J191142+1952  00 14 20  22.2 280.7  5.0      64.0    -8    16630   04 38 13
04 39 35  ---          00 15 51  21.9 280.9  5.1      64.0    82    16672   04 38 06

04 39 35  GRB221009A   00 15 51  22.1 280.6  5.0      64.0    -8    16672   04 39 43
04 44 10  ---          00 20 26  21.1 281.2  5.1      63.8   267    16809   04 39 36

04 44 25  J1925+2106   00 20 41  24.4 281.1  4.9      64.9     1    16809   04 44 25
04 45 25  =1923+210    00 21 41  24.2 281.2  4.9      64.8    60    16840   04 44 26

04 45 25 J191142+1952  00 21 41  20.6 281.5  5.1      63.7   -15    16840   04 45 40
04 46 50  ---          00 23 07  20.3 281.7  5.2      63.7    70    16876   04 45 26

04 46 50  GRB221009A   00 23 07  20.6 281.5  5.1      63.7    -8    16876   04 46 58
04 51 25  ---          00 27 42  19.6 282.0  5.2      63.5   267    17014   04 46 51

04 51 45 J191142+1952  00 28 03  19.3 282.2  5.3      63.4    12    17014   04 51 45
04 52 50  ---          00 29 08  19.1 282.4  5.3      63.4    65    17047   04 51 46

04 52 50  J1905+1943   00 29 08  17.7 282.9  5.4      63.0   -11    17047   04 53 01
04 54 35  ---          00 30 53  17.4 283.1  5.4      62.9    94    17096   04 52 51

04 54 35 J191142+1952  00 30 53  18.7 282.6  5.3      63.3   -11    17096   04 54 46
04 56 00  ---          00 32 18  18.4 282.7  5.3      63.2    74    17134   04 54 36
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

04 56 15  J1925+2106   00 32 33  21.9 282.4  5.1      64.3     0    17134   04 56 15
04 57 15  =1923+210    00 33 33  21.7 282.5  5.1      64.3    60    17165   04 56 16

04 57 30  GRB221009A   00 33 48  18.3 282.6  5.3      63.2     0    17165   04 57 30
05 02 05  ---          00 38 24  17.4 283.2  5.4      62.9   275    17307   04 57 31

05 02 25 J191142+1952  00 38 44  17.1 283.4  5.4      62.9    12    17307   05 02 25
05 03 50  ---          00 40 10  16.8 283.6  5.5      62.8    85    17350   05 02 26

05 03 50  GRB221009A   00 40 10  17.0 283.4  5.4      62.9    -8    17350   05 03 58
05 08 25  ---          00 44 45  16.0 283.9  5.5      62.6   267    17488   05 03 51

05 08 40  J1925+2106   00 45 00  19.3 283.7  5.3      63.7     1    17488   05 08 40
05 09 40  =1923+210    00 46 00  19.1 283.8  5.3      63.6    60    17519   05 08 41

05 09 40 J191142+1952  00 46 00  15.5 284.3  5.6      62.5   -15    17519   05 09 55
05 11 05  ---          00 47 26  15.2 284.4  5.6      62.4    70    17555   05 09 41

05 11 05  J1923+2010   00 47 26  17.8 283.4  5.4      63.1   -13    17555   05 11 18
05 12 40  ---          00 49 01  17.5 283.6  5.4      63.0    82    17597   05 11 06

05 13 00 J191142+1952  00 49 21  14.8 284.6  5.6      62.3     7    17597   05 13 00
05 14 30  ---          00 50 51  14.5 284.8  5.6      62.2    90    17644   05 13 01

05 14 30  GRB221009A   00 50 51  14.8 284.6  5.6      62.3    -8    17644   05 14 38
05 19 05  ---          00 55 27  13.8 285.1  5.7      62.0   267    17781   05 14 31

05 19 20  J1925+2106   00 55 42  17.1 284.9  5.5      63.1     1    17781   05 19 20
05 20 20  =1923+210    00 56 42  16.9 285.0  5.5      63.0    60    17812   05 19 21

05 20 35 J191142+1952  00 56 57  13.3 285.5  5.7      61.9     0    17812   05 20 35
05 22 00  ---          00 58 22  13.0 285.7  5.8      61.8    85    17856   05 20 36

05 22 00  GRB221009A   00 58 22  13.2 285.4  5.7      61.8    -8    17856   05 22 08
05 26 35  ---          01 02 58  12.2 285.9  5.8      61.6   267    17993   05 22 01

05 26 55 J191142+1952  01 03 18  11.9 286.2  5.8      61.5    12    17993   05 26 55
05 28 00  ---          01 04 23  11.7 286.3  5.9      61.4    65    18027   05 26 56

05 28 15  J1925+2106   01 04 39  15.2 285.9  5.6      62.5     0    18027   05 28 15
05 29 15  =1923+210    01 05 39  15.0 286.0  5.6      62.5    60    18058   05 28 16

05 29 15 J191249+1940  01 05 39  11.6 286.2  5.9      61.4   -15    18058   05 29 30
05 30 45  ---          01 07 09  11.3 286.4  5.9      61.3    75    18097   05 29 16
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GG088
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  29 Oct 2024   Day 303 ---

05 30 45 J191142+1952  01 07 09  11.2 286.7  5.9      61.2    -7    18097   05 30 52
05 32 15  ---          01 08 39  10.8 286.8  5.9      61.2    83    18139   05 30 46

05 32 15  GRB221009A   01 08 39  11.1 286.6  5.9      61.2    -8    18139   05 32 23
05 36 50  ---          01 13 15  10.1 287.1  6.0      60.9   267    18277   05 32 16

05 37 05  J1925+2106   01 13 30  13.4 286.9  5.8      62.0     1    18277   05 37 05
05 38 05  =1923+210    01 14 30  13.2 287.0  5.8      61.9    60    18308   05 37 06

05 38 05 J191142+1952  01 14 30   9.6 287.5  6.0      60.8   -15    18308   05 38 20
05 39 30  ---          01 15 55   9.3 287.7  6.1      60.7    70    18344   05 38 06

05 48 55  J1925+2106   01 25 22  10.9 288.2  6.0      61.2   550    18344   05 48 55
05 49 55  =1923+210    01 26 22  10.7 288.3  6.0      61.1    60    18375   05 48 56


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess324.C4096glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    7         Station: VLBA_FD           Total bit rate:  4096
   Format: VDIF              Bits per sample: 2         Sample rate:256.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  23  Setup file default.  Used with PCAL = off
   LO sum=   4612.00  4612.00  4740.00  4740.00  4868.00  4868.00  4996.00  4996.00
   BBC fr=    512.00   512.00   640.00   640.00   768.00   768.00   896.00   896.00
   Bandwd=    128.00   128.00   128.00   128.00   128.00   128.00   128.00   128.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     696.00    696.00    824.00    824.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  23  24  25  26  27  28  29  30  31  33

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * GRB221009A        19 10 52.500472   * 19 13 03.500400     19 14 07.827738       0.00
                     19 41 14.67648    * 19 46 24.22800      19 49 04.53286        0.00
                     From catalog imbedded in main SCHED input file.

 * J1905+1943        19 03 25.637172   * 19 05 36.472100     19 06 40.683873       0.00
                     19 38 29.62717    * 19 43 08.04500      19 45 32.77332        0.00
                     From catalog imbedded in main SCHED input file.

 * J1923+2010        19 21 02.282278   * 19 23 13.140228     19 24 17.442454       0.00
                     20 04 48.26646    * 20 10 39.75566      20 13 41.12286        0.00
                     From catalog imbedded in main SCHED input file.

 * J191142+1952      19 09 31.670884   * 19 11 42.509697     19 12 46.750398       0.00
                     19 46 56.00561    * 19 51 59.94423      19 54 37.46441        0.00
                     From catalog imbedded in main SCHED input file.

 * J191249+1940      19 10 38.054579   * 19 12 49.180000     19 13 53.569060       0.00
                     19 34 51.84540    * 19 40 00.40000      19 42 40.18189        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C286             13 28 49.657692   * 13 31 08.287984     13 32 15.756080       0.00
                     30 45 58.64021    * 30 30 32.95885      30 22 55.28743        0.00
                     From catalog imbedded in main SCHED input file.

   0834-201          08 34 24.601692   * 08 36 39.215252     08 37 45.716071       0.01
 * J0836-2016       -20 06 30.40853    *-20 16 59.50422     -20 21 53.67310        0.01
   J0836-20          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  16505 observations.

 * 3C279             12 53 35.831310   * 12 56 11.166577     12 57 26.904041       0.34
   J1256-0547       -05 31 07.99627    *-05 47 21.52513     -05 55 17.62310        0.56
   1253-055          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J1256-05          GSFC 2016a X/S astro solution,  13160 observations.

   1923+210          19 23 49.792392   * 19 25 59.605356     19 27 03.397150       0.01
 * J1925+2106        21 00 23.30493    * 21 06 26.16201      21 09 33.43088        0.00
   J1925+21          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  38704 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  GRB221009A sess324.C4096glob     1 2 3 7 8 9 10 11 12 13 15  +    15.078  1182.453
  J1905+1943 sess324.C4096glob     1 2 3 7 8 9 10 11 12 13 15  +     0.963    69.264
  J1923+2010 sess324.C4096glob     1 2 3 7 8 10 11 12 13 15 16 +     0.844    51.471
  J191142+195sess324.C4096glob     1 2 3 7 8 9 10 11 12 13 15  +     6.397   501.683
  J191249+194sess324.C4096glob     1 2 3 7 8 9 10 11 12 13 15  +     0.750    53.420
  3C286      sess324.C4096glob     9 16 23 32                        0.458     5.193
  J0836-2016 sess324.C4096glob     1 2 3                             1.333    20.000
  3C279      sess324.C4096glob     1 2 3                             2.591    38.871
  J1925+2106 sess324.C4096glob     1 2 3 7 8 9 10 11 12 13 15  +     1.351   141.157


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   GRB221009A          81.1
   J1905+1943          79.4
   J1923+2010          83.5
   J191142+1952        80.8
   J191249+1940        81.0
   3C286               44.9
   J0836-2016          79.8
   3C279               20.1
   J1925+2106          84.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

